(module USBA_Plug_UP2-AH-1-TH (layer F.Cu) (tedit 5A50BFBC)
  (fp_text reference REF** (at 0 8.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USBA_Plug_UP2-AH-1-TH (at 0 6.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6 -5.05) (end -6 -5.05) (layer F.Fab) (width 0.127))
  (fp_line (start -6 -5.05) (end -6 -2) (layer F.Fab) (width 0.127))
  (fp_line (start 6 -5.05) (end 6 -2) (layer F.Fab) (width 0.127))
  (fp_line (start 6 -2) (end 6 15.8) (layer F.Fab) (width 0.127))
  (fp_line (start 6 15.8) (end -6 15.8) (layer F.Fab) (width 0.127))
  (fp_line (start -6 15.8) (end -6 -2) (layer F.Fab) (width 0.127))
  (fp_line (start 5.85 15.8) (end -6.15 15.8) (layer F.Fab) (width 0.127))
  (fp_line (start -6 0.75) (end 6 0.75) (layer F.CrtYd) (width 0.127))
  (pad "" np_thru_hole circle (at -2.3 -2.9) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at 5.85 -2.9) (size 1.7 3.2) (drill oval 1 2.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1 -5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1 -5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 3.5 -5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -3.5 -5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -5.85 -2.9) (size 1.7 3.2) (drill oval 1 2.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.3 -2.9) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
)
