(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 51)
    (no_connects 17)
    (area 154.872999 87.372999 169.627001 102.127001)
    (thickness 1.6)
    (drawings 21)
    (tracks 288)
    (zones 0)
    (modules 10)
    (nets 21)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.155)
    (trace_clearance 0.155)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.155)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.55)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.901 0.901)
    (pad_drill 0)
    (pad_to_mask_clearance 0.03)
    (aux_axis_origin 0 0)
    (grid_origin 155 87.5)
    (visible_elements FFFFFF9F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 +5V)
  (net 6 "Net-(U1-Pad13)")
  (net 7 "Net-(U1-Pad14)")
  (net 8 /D+)
  (net 9 /D-)
  (net 10 /C2D)
  (net 11 /C2CK)
  (net 12 /P0.3)
  (net 13 /P0.2)
  (net 14 /P0.1)
  (net 15 /P0.0)
  (net 16 /P0.7)
  (net 17 /P0.6)
  (net 18 /P0.5)
  (net 19 /P0.4)
  (net 20 "Net-(SW1-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.155)
    (trace_width 0.155)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /C2CK)
    (add_net /C2D)
    (add_net /D+)
    (add_net /D-)
    (add_net /P0.0)
    (add_net /P0.1)
    (add_net /P0.2)
    (add_net /P0.3)
    (add_net /P0.4)
    (add_net /P0.5)
    (add_net /P0.6)
    (add_net /P0.7)
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
  )

  (net_class gnd ""
    (clearance 0.155)
    (trace_width 0.2)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222F7) (tstamp 59BC5FF5)
    (at 159 94.1)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6727)
    (attr smd)
    (fp_text reference C1 (at 5.6 0 90) (layer Cmts.User)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222FB) (tstamp 59BC5FFB)
    (at 158.6 93.1)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6754)
    (attr smd)
    (fp_text reference C2 (at 1.7 0 90) (layer Cmts.User)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 0 -1.27) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D22319) (tstamp 59BC6001)
    (at 160.2 92.3 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6871)
    (attr smd)
    (fp_text reference C3 (at -0.3 0.6 270) (layer Cmts.User)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (fp_text value 0.1uF (at 0 -1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222EE) (tstamp 59BC6007)
    (at 161.1 91.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC686B)
    (attr smd)
    (fp_text reference C4 (at 1.7 -0.7 360) (layer Cmts.User)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 0 -1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module qfn:QFN20_silabs (layer B.Cu) (tedit 59D2336D) (tstamp 59D1A41A)
    (at 157.5 90.25 180)
    (path /59D1CD41)
    (fp_text reference U1 (at 0 3.2 180) (layer Cmts.User)
      (effects (font (size 1.2 1.2) (thickness 0.15)))
    )
    (fp_text value EFM8UB1_QFN20 (at 0 -3.2 180) (layer B.Fab)
      (effects (font (size 1.2 1.2) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start -1.6 1.6) (end -1.6 1.325) (angle -270) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.6 1.1) (end 1.6 1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.6 1.6) (end 1.1 1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.1 -1.6) (end 1.6 -1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.6 -1.6) (end 1.6 -1.1) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.6 -1.1) (end -1.6 -1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.6 -1.6) (end -1.1 -1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.1 1.6) (end -1.6 1.6) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.6 1.6) (end -1.6 1.1) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.6 1.6) (end 1.6 1.6) (layer B.CrtYd) (width 0.15))
    (fp_line (start 1.6 1.6) (end 1.6 -1.6) (layer B.CrtYd) (width 0.15))
    (fp_line (start 1.6 -1.6) (end -1.6 -1.6) (layer B.CrtYd) (width 0.15))
    (fp_line (start -1.6 -1.6) (end -1.6 1.6) (layer B.CrtYd) (width 0.15))
    (pad 16 smd rect (at 1.25 1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /P0.6))
    (pad 11 smd rect (at 1.25 -1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (pad 6 smd rect (at -1.25 -1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 21 smd rect (at -0.45 -0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.45 -0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.45 0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.55 0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /P0.0))
    (pad 3 smd rect (at -1.55 0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.55 -0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /D+))
    (pad 5 smd rect (at -1.55 -0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /D-))
    (pad 7 smd rect (at -0.75 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 8 smd rect (at -0.25 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 9 smd rect (at 0.25 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 /C2CK))
    (pad 10 smd rect (at 0.75 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /C2D))
    (pad 12 smd rect (at 1.55 -0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.55 -0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 1.55 0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.55 0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 /P0.7))
    (pad 17 smd rect (at 0.75 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 /P0.5))
    (pad 18 smd rect (at 0.25 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 /P0.4))
    (pad 19 smd rect (at -0.25 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 /P0.3))
    (pad 20 smd rect (at -0.75 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 /P0.2))
    (pad 1 smd rect (at -1.25 1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /P0.1))
    (pad 21 smd rect (at -0.45 0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module conn_usb:USB_Micro_NoSlots_NoSilk (layer B.Cu) (tedit 59BC85A0) (tstamp 5A1C999A)
    (at 165.75 90.5)
    (path /59BC971A)
    (fp_text reference J1 (at -3.175 2.921 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value USB_OTG (at -0.07 -4.18) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 6 smd rect (at -3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at -1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad 6 smd rect (at -1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 8 /D+))
    (pad 2 smd rect (at -0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 9 /D-))
    (pad 1 smd rect (at -1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 6 thru_hole circle (at 2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at 1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
  )

  (module conn:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6) (tstamp 5A1C99AA)
    (at 156.225 96.85 180)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (path /59BC8422)
    (fp_text reference J2 (at 2.4325 1.635 180) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 2.4325 -5.445 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.5 0.635) (end 1.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -4.445) (end 0.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -4.445) (end 0.5 0.385) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.385) (end 0.75 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end 0.5 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end -0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end 0.5 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end 0.5 -1.07) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end -0.2 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.47) (end 0.5 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end 0.5 -2.34) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end -0.2 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.74) (end 0.5 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end 0.5 -3.61) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end -0.2 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -4.01) (end 0.5 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -1.15 1.15) (end -1.15 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.15 -4.95) (end 6 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 -4.95) (end 6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 1.15) (end -1.15 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole rect (at 0 -1.27 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 10 /C2D))
    (pad 3 thru_hole rect (at 0 -2.54 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 11 /C2CK))
    (pad 4 thru_hole rect (at 0 -3.81 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /C2D))
    (pad 3 thru_hole circle (at 1.27 -2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /C2CK))
    (pad 4 thru_hole circle (at 1.27 -3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
  )

  (module conn:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6) (tstamp 5A1C99B5)
    (at 168.25 100.65)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (path /59D1D839)
    (fp_text reference J3 (at 2.4325 1.635) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 2.4325 -5.445) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.5 0.635) (end 1.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -4.445) (end 0.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -4.445) (end 0.5 0.385) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.385) (end 0.75 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end 0.5 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end -0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end 0.5 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end 0.5 -1.07) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end -0.2 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.47) (end 0.5 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end 0.5 -2.34) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end -0.2 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.74) (end 0.5 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end 0.5 -3.61) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end -0.2 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -4.01) (end 0.5 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -1.15 1.15) (end -1.15 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.15 -4.95) (end 6 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 -4.95) (end 6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 1.15) (end -1.15 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /P0.3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 12 /P0.3))
    (pad 2 thru_hole rect (at 0 -1.27) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 13 /P0.2))
    (pad 3 thru_hole rect (at 0 -2.54) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 14 /P0.1))
    (pad 4 thru_hole rect (at 0 -3.81) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 15 /P0.0))
    (pad 2 thru_hole circle (at 1.27 -1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /P0.2))
    (pad 3 thru_hole circle (at 1.27 -2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /P0.1))
    (pad 4 thru_hole circle (at 1.27 -3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /P0.0))
  )

  (module conn:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6) (tstamp 5A1C99C0)
    (at 161.75 100.65 270)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (path /59D1DF9A)
    (fp_text reference J4 (at 2.4325 1.635 270) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 2.4325 -5.445 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.5 0.635) (end 1.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -4.445) (end 0.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -4.445) (end 0.5 0.385) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.385) (end 0.75 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end 0.5 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end -0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end 0.5 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end 0.5 -1.07) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end -0.2 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.47) (end 0.5 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end 0.5 -2.34) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end -0.2 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.74) (end 0.5 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end 0.5 -3.61) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end -0.2 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -4.01) (end 0.5 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -1.15 1.15) (end -1.15 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.15 -4.95) (end 6 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 -4.95) (end 6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 1.15) (end -1.15 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /P0.7))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 16 /P0.7))
    (pad 2 thru_hole rect (at 0 -1.27 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 17 /P0.6))
    (pad 3 thru_hole rect (at 0 -2.54 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 18 /P0.5))
    (pad 4 thru_hole rect (at 0 -3.81 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 19 /P0.4))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /P0.6))
    (pad 3 thru_hole circle (at 1.27 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /P0.5))
    (pad 4 thru_hole circle (at 1.27 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /P0.4))
  )

  (module switch_mx:Cherry_MX_Matias_No_Silk_Border (layer B.Cu) (tedit 5A1BC55D) (tstamp 5A1C99CB)
    (at 162.25 94.75)
    (tags switch)
    (path /5A1C99D7)
    (fp_text reference SW1 (at 0 -6) (layer Cmts.User)
      (effects (font (thickness 0.3048)))
    )
    (fp_text value SW_Push (at 1 -3.5) (layer F.Fab) hide
      (effects (font (thickness 0.3048)))
    )
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at 2.5 3.683) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (pad 1 thru_hole circle (at -2.5 4) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (model cherry_mx1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 156.25 100.65) (end 156.25 101.2) (angle 90) (layer Cmts.User) (width 0.254))
  (gr_line (start 161.75 100.65) (end 156.25 100.65) (angle 90) (layer Cmts.User) (width 0.254))
  (gr_text 2 (at 167.15 99.35) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text 5V (at 157.575 96.85) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text D (at 157.375 98.125) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text K (at 157.4 99.4) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text G (at 157.475 100.65) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text "7\n" (at 161.75 99.45) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text "6\n" (at 163 99.45) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 3 (at 167.2 100.65) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.13)) (justify mirror))
  )
  (gr_text 0 (at 168.7 95.6) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_line (start 169.5 87.5) (end 169.5 102) (layer Cmts.User) (width 0.2))
  (gr_line (start 155 102) (end 155 87.5) (layer Cmts.User) (width 0.2))
  (gr_line (start 169.5 102) (end 155 102) (layer Cmts.User) (width 0.2))
  (gr_line (start 155 87.5) (end 169.5 102) (layer Cmts.User) (width 0.2))
  (gr_line (start 169.5 87.5) (end 155 87.5) (layer Cmts.User) (width 0.2))
  (gr_line (start 155 102) (end 169.5 87.5) (layer Cmts.User) (width 0.2))
  (gr_line (start 155 102) (end 155 87.5) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 169.5 102) (end 155 102) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 169.5 87.5) (end 169.5 102) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 155 87.5) (end 169.5 87.5) (angle 90) (layer Edge.Cuts) (width 0.254))

  (segment (start 157.05 90.7) (end 157.95 89.8) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 157.95 90.7) (end 157.05 89.8) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 157.95 90.7) (end 157.95 89.8) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 164.75 98.433) (end 164.917 98.433) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 164.917 98.433) (end 166.06 97.29) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22F2C) (status 30))
  (segment (start 156.225 100.66) (end 156.965 100.66) (width 0.2) (layer B.Cu) (net 1) (status 10))
  (segment (start 156.965 100.66) (end 157.55 100.075) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22EEC))
  (segment (start 161.625 89.9) (end 161.625 91.725) (width 0.2) (layer B.Cu) (net 1))
  (segment (start 161.625 91.725) (end 161.1 92.25) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22C19) (status 20))
  (segment (start 166.06 97.29) (end 166.06 94.39) (width 0.2) (layer B.Cu) (net 1) (status 10))
  (segment (start 167.05 93.4) (end 167.05 91.55) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22C04) (status 20))
  (segment (start 166.06 94.39) (end 167.05 93.4) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22C02))
  (segment (start 159.55 94.1) (end 159.55 94.95) (width 0.2) (layer B.Cu) (net 1) (status 10))
  (segment (start 159.55 94.95) (end 157.55 96.95) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22B95))
  (segment (start 167.05 92.4) (end 167.05 91.55) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1B499) (status 30))
  (segment (start 161 89.6) (end 160.1 89.6) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D1ABEE))
  (segment (start 161.3 89.9) (end 161 89.6) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D1ABEC))
  (segment (start 166.7 89.9) (end 161.625 89.9) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D1ABEB))
  (segment (start 161.625 89.9) (end 161.3 89.9) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22C17))
  (segment (start 167.05 90.25) (end 166.7 89.9) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D1ABEA))
  (segment (start 167.05 91.55) (end 167.05 90.25) (width 0.2) (layer B.Cu) (net 1) (status 10))
  (segment (start 159.7 90) (end 160.1 89.6) (width 0.2) (layer B.Cu) (net 1))
  (segment (start 159.05 90) (end 159.7 90) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D1ABF5) (status 10))
  (segment (start 157.05 89.8) (end 157.95 89.8) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 157.05 90.7) (end 157.05 89.8) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 157.95 90.7) (end 157.05 90.7) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 159.05 90) (end 158.15 90) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 158.15 90) (end 157.95 89.8) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1ABCC) (status 30))
  (segment (start 155.95 91) (end 156.75 91) (width 0.2) (layer B.Cu) (net 1) (status 30))
  (segment (start 156.75 91) (end 157.05 90.7) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1ABC8) (status 30))
  (segment (start 160.2 92.85) (end 160.5 92.85) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 160.5 92.85) (end 161.1 92.25) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1A939) (status 20))
  (segment (start 159.15 93.1) (end 159.15 93.45) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 159.15 93.45) (end 159.55 93.85) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1A900) (status 20))
  (segment (start 159.55 93.85) (end 159.55 94.1) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1A901) (status 30))
  (segment (start 160.2 92.85) (end 159.95 92.85) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 159.95 92.85) (end 159.7 93.1) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1A8FC) (status 10))
  (segment (start 159.7 93.1) (end 159.15 93.1) (width 0.155) (layer B.Cu) (net 1) (tstamp 59D1A8FD) (status 20))
  (segment (start 157.55 96.95) (end 157.55 100.075) (width 0.2) (layer B.Cu) (net 1) (tstamp 59D22B97))
  (segment (start 160.2 91.75) (end 159 91.75) (width 0.155) (layer B.Cu) (net 2) (status 10))
  (segment (start 159 91.75) (end 158.75 91.5) (width 0.155) (layer B.Cu) (net 2) (tstamp 59D1A93F) (status 20))
  (segment (start 160.2 91.75) (end 160.5 91.75) (width 0.155) (layer B.Cu) (net 2) (status 10))
  (segment (start 160.5 91.75) (end 161.1 91.15) (width 0.155) (layer B.Cu) (net 2) (tstamp 59D1A93C) (status 20))
  (segment (start 164.45 91.55) (end 164.45 93.6) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 158.45 95.3) (end 158.45 94.1) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22CA9) (status 20))
  (segment (start 157.65 96.1) (end 158.45 95.3) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22CA8))
  (via (at 157.65 96.1) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 5))
  (segment (start 157.65 97) (end 157.65 96.1) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D22CA6))
  (segment (start 158.2 97.55) (end 157.65 97) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D22CA5))
  (via (at 158.2 97.55) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 5))
  (segment (start 158.65 97.1) (end 158.2 97.55) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22CA2))
  (segment (start 163.2 97.1) (end 158.65 97.1) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22CA0))
  (segment (start 164.7 95.6) (end 163.2 97.1) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22C9E))
  (segment (start 164.7 93.85) (end 164.7 95.6) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22C9D))
  (segment (start 164.45 93.6) (end 164.7 93.85) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22C9C))
  (segment (start 157.25 93.4) (end 157.25 93.3) (width 0.155) (layer F.Cu) (net 5))
  (segment (start 157.55 93.1) (end 157.25 93.4) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D22500))
  (via (at 157.25 93.4) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 5))
  (segment (start 158.05 93.1) (end 157.55 93.1) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 155.6 95.9) (end 156.27 96.57) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D2254B) (status 20))
  (segment (start 155.6 93.15) (end 155.6 95.9) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D2254A))
  (segment (start 155.9 92.85) (end 155.6 93.15) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D22549))
  (segment (start 156.8 92.85) (end 155.9 92.85) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D22548))
  (segment (start 157.25 93.3) (end 156.8 92.85) (width 0.155) (layer F.Cu) (net 5) (tstamp 59D22547))
  (segment (start 157.75 92.35) (end 158.05 92.65) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D1A8F5))
  (segment (start 157.75 91.8) (end 157.75 92.35) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 158.25 91.8) (end 158.25 92.45) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 158.05 92.65) (end 158.05 93.1) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D1A8F2) (status 20))
  (segment (start 158.25 92.45) (end 158.05 92.65) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D1A8F1))
  (segment (start 158.45 94.1) (end 158.45 93.5) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 158.45 93.5) (end 158.05 93.1) (width 0.155) (layer B.Cu) (net 5) (tstamp 59D1A8E0) (status 20))
  (segment (start 160.6 90.2) (end 161.75 90.2) (width 0.155) (layer F.Cu) (net 8))
  (segment (start 159.05 90.5) (end 159.7 90.5) (width 0.155) (layer B.Cu) (net 8) (status 10))
  (via (at 160.6 90.2) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 8))
  (segment (start 160 90.2) (end 160.6 90.2) (width 0.155) (layer B.Cu) (net 8) (tstamp 59D1AAC3))
  (segment (start 159.7 90.5) (end 160 90.2) (width 0.155) (layer B.Cu) (net 8) (tstamp 59D1AABE))
  (segment (start 166.4 93.2) (end 165.75 92.55) (width 0.155) (layer B.Cu) (net 8) (tstamp 59D1B33D) (status 20))
  (via (at 166.4 93.2) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 8))
  (segment (start 166.4 91.5) (end 166.4 93.2) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B33A))
  (segment (start 166.1 91.2) (end 166.4 91.5) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B337))
  (segment (start 163.55 91.2) (end 166.1 91.2) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B335))
  (segment (start 162.8 90.45) (end 163.55 91.2) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B334))
  (segment (start 162 90.45) (end 162.8 90.45) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B331))
  (segment (start 161.75 90.2) (end 162 90.45) (width 0.155) (layer F.Cu) (net 8) (tstamp 59D1B32F))
  (segment (start 165.75 92.55) (end 165.75 91.55) (width 0.155) (layer B.Cu) (net 8) (tstamp 59D1B33E) (status 30))
  (segment (start 160.2 90.8) (end 162.65 90.8) (width 0.155) (layer F.Cu) (net 9))
  (segment (start 160 91) (end 160.2 90.8) (width 0.155) (layer B.Cu) (net 9) (tstamp 59D1AAAB))
  (via (at 160.2 90.8) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 9))
  (segment (start 159.05 91) (end 160 91) (width 0.155) (layer B.Cu) (net 9) (status 10))
  (segment (start 165.1 92.7) (end 165.1 91.55) (width 0.155) (layer B.Cu) (net 9) (tstamp 59D1B355) (status 20))
  (segment (start 165.6 93.2) (end 165.1 92.7) (width 0.155) (layer B.Cu) (net 9) (tstamp 59D1B354))
  (via (at 165.6 93.2) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 9))
  (segment (start 165.9 92.9) (end 165.6 93.2) (width 0.155) (layer F.Cu) (net 9) (tstamp 59D1B350))
  (segment (start 165.9 91.75) (end 165.9 92.9) (width 0.155) (layer F.Cu) (net 9) (tstamp 59D1B34E))
  (segment (start 165.7 91.55) (end 165.9 91.75) (width 0.155) (layer F.Cu) (net 9) (tstamp 59D1B34A))
  (segment (start 163.4 91.55) (end 165.7 91.55) (width 0.155) (layer F.Cu) (net 9) (tstamp 59D1B347))
  (segment (start 162.65 90.8) (end 163.4 91.55) (width 0.155) (layer F.Cu) (net 9) (tstamp 59D1B343))
  (segment (start 156.225 98.12) (end 156.43 98.12) (width 0.155) (layer F.Cu) (net 10) (status 30))
  (segment (start 156.43 98.12) (end 157.05 97.5) (width 0.155) (layer F.Cu) (net 10) (tstamp 59D22F25) (status 10))
  (segment (start 157.05 96.275) (end 157.05 97.5) (width 0.155) (layer F.Cu) (net 10) (tstamp 59D2251C))
  (segment (start 156 95.225) (end 157.05 96.275) (width 0.155) (layer F.Cu) (net 10) (tstamp 59D2251A))
  (segment (start 156 93.55) (end 156 95.225) (width 0.155) (layer F.Cu) (net 10) (tstamp 59D22519))
  (segment (start 156.15 93.4) (end 156 93.55) (width 0.155) (layer F.Cu) (net 10) (tstamp 59D22518))
  (segment (start 156.75 91.8) (end 156.75 92.35) (width 0.155) (layer B.Cu) (net 10) (status 10))
  (via (at 156.15 93.4) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 10))
  (segment (start 156.15 92.95) (end 156.15 93.4) (width 0.155) (layer B.Cu) (net 10) (tstamp 59D22515))
  (segment (start 156.75 92.35) (end 156.15 92.95) (width 0.155) (layer B.Cu) (net 10) (tstamp 59D22514))
  (segment (start 156.225 99.39) (end 156.585 99.39) (width 0.155) (layer B.Cu) (net 11) (status 30))
  (segment (start 156.585 99.39) (end 157.05 98.925) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D22F1D) (status 10))
  (segment (start 157.05 98.925) (end 157.05 96.275) (width 0.155) (layer B.Cu) (net 11))
  (segment (start 156 95.225) (end 156 94.3) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D22F11))
  (segment (start 157.05 96.275) (end 156 95.225) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D22F10))
  (segment (start 156.7 93.6) (end 156 94.3) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D224EE))
  (segment (start 156.7 92.9) (end 156.7 93.6) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D22507))
  (segment (start 157.25 91.8) (end 157.25 92.35) (width 0.155) (layer B.Cu) (net 11) (status 10))
  (segment (start 157.25 92.35) (end 156.7 92.9) (width 0.155) (layer B.Cu) (net 11) (tstamp 59D22506))
  (segment (start 163.85 99.95) (end 166.6 99.95) (width 0.155) (layer B.Cu) (net 12))
  (segment (start 163.85 99.95) (end 163.1 99.2) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22BF5))
  (segment (start 163.1 99.2) (end 163.1 97.75) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22BF7))
  (segment (start 163.1 97.75) (end 165.05 95.8) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22BF9))
  (segment (start 165.05 95.8) (end 165.45 95.8) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22BFB))
  (via (at 165.45 95.8) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 12))
  (segment (start 165.45 95.8) (end 165.35 95.7) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D22BFE))
  (segment (start 165.35 94.25) (end 165.35 95.7) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D22BFF))
  (segment (start 167.3 100.65) (end 168.25 100.65) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22D59) (status 20))
  (segment (start 166.6 99.95) (end 167.3 100.65) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D22D58))
  (segment (start 161.35 91.75) (end 162.4 91.75) (width 0.155) (layer F.Cu) (net 12))
  (segment (start 159.9 92.45) (end 160.65 92.45) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B3E7))
  (segment (start 160.65 92.45) (end 161.35 91.75) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B3EC))
  (segment (start 164.65 93.55) (end 165.35 94.25) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B42E))
  (segment (start 164.65 92.65) (end 164.65 93.55) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B42D))
  (segment (start 164.3 92.3) (end 164.65 92.65) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B42C))
  (segment (start 162.95 92.3) (end 164.3 92.3) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B42B))
  (segment (start 162.4 91.75) (end 162.95 92.3) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B42A))
  (segment (start 157.6 89.3) (end 157.6 90.15) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B3E1))
  (segment (start 157.6 90.15) (end 159.9 92.45) (width 0.155) (layer F.Cu) (net 12) (tstamp 59D1B3E6))
  (segment (start 158.9 88) (end 157.6 89.3) (width 0.155) (layer F.Cu) (net 12))
  (segment (start 157.75 88.7) (end 157.75 88.05) (width 0.155) (layer B.Cu) (net 12) (status 10))
  (via (at 158.9 88) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 12))
  (segment (start 158.7 87.8) (end 158.9 88) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D1ACB9))
  (segment (start 158 87.8) (end 158.7 87.8) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D1ACB7))
  (segment (start 157.75 88.05) (end 158 87.8) (width 0.155) (layer B.Cu) (net 12) (tstamp 59D1ACB6))
  (segment (start 167.5 96.2) (end 167.9 95.8) (width 0.155) (layer B.Cu) (net 13))
  (segment (start 167.5 98.9) (end 167.5 96.2) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D22D67))
  (segment (start 167.98 99.38) (end 167.5 98.9) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D22D66) (status 10))
  (segment (start 168.1 95.8) (end 168.8 95.1) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D22D82))
  (via (at 168.1 95.8) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 13))
  (segment (start 167.9 95.8) (end 168.1 95.8) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D22D6E))
  (segment (start 168.8 95.1) (end 168.8 94.85) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D22D83))
  (segment (start 168.25 99.38) (end 167.98 99.38) (width 0.155) (layer B.Cu) (net 13) (status 30))
  (segment (start 168.8 90.1) (end 168.8 94.85) (width 0.155) (layer F.Cu) (net 13))
  (segment (start 168.8 94.85) (end 168.8 95.1) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D22D86))
  (segment (start 168.8 90.1) (end 168.45 89.75) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D1B2F0))
  (segment (start 161.5 88.7) (end 161.5 89) (width 0.155) (layer F.Cu) (net 13))
  (segment (start 161.5 89) (end 162.25 89.75) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D1B2E7))
  (segment (start 162.25 89.75) (end 168.45 89.75) (width 0.155) (layer F.Cu) (net 13) (tstamp 59D1B2E9))
  (segment (start 161.1 88.3) (end 161.5 88.7) (width 0.155) (layer F.Cu) (net 13))
  (via (at 161.1 88.3) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 13))
  (segment (start 160.8 88) (end 161.1 88.3) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D1ACAE))
  (segment (start 159.7 88) (end 160.8 88) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D1ACAC))
  (segment (start 159.1 88.6) (end 159.7 88) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D1ACA6))
  (segment (start 158.3 88.6) (end 159.1 88.6) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D1AC9C) (status 10))
  (segment (start 158.25 88.7) (end 158.25 88.55) (width 0.155) (layer B.Cu) (net 13) (status 30))
  (segment (start 158.25 88.55) (end 158.3 88.6) (width 0.155) (layer B.Cu) (net 13) (tstamp 59D1AC9A) (status 30))
  (segment (start 168.25 98.11) (end 167.81 98.11) (width 0.155) (layer F.Cu) (net 14) (status 30))
  (segment (start 167.81 98.11) (end 167.5 97.8) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22D8D) (status 10))
  (segment (start 167.5 97.8) (end 167.5 96.5) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22D8E))
  (segment (start 167.5 96.5) (end 166.95 95.95) (width 0.155) (layer F.Cu) (net 14))
  (segment (start 160.3 88.4) (end 160.9 89) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C8F))
  (segment (start 159.75 88.4) (end 160.3 88.4) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C8E))
  (segment (start 159.45 88.7) (end 159.75 88.4) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C8B))
  (segment (start 159.45 91.05) (end 159.45 88.7) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C8A))
  (segment (start 159.8 91.4) (end 159.45 91.05) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C89))
  (segment (start 160.75 91.4) (end 159.8 91.4) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C88))
  (segment (start 160.85 91.3) (end 160.75 91.4) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C87))
  (segment (start 162.5 91.3) (end 160.85 91.3) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C85))
  (segment (start 163.189998 91.989998) (end 162.5 91.3) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C83))
  (segment (start 164.539998 91.989998) (end 163.189998 91.989998) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C82))
  (segment (start 165 92.45) (end 164.539998 91.989998) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C81))
  (segment (start 165 93.4) (end 165 92.45) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C7F))
  (segment (start 165.9 94.3) (end 165 93.4) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C7E))
  (segment (start 165.9 95.1) (end 165.9 94.3) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C7C))
  (segment (start 166.75 95.95) (end 165.9 95.1) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C7B))
  (segment (start 166.95 95.95) (end 166.75 95.95) (width 0.155) (layer F.Cu) (net 14) (tstamp 59D22C7A))
  (segment (start 158.75 89) (end 159.2 89) (width 0.155) (layer B.Cu) (net 14) (status 10))
  (segment (start 159.2 89) (end 159.8 88.4) (width 0.155) (layer B.Cu) (net 14) (tstamp 59D1AC83))
  (segment (start 159.8 88.4) (end 160.3 88.4) (width 0.155) (layer B.Cu) (net 14) (tstamp 59D1AC8A))
  (segment (start 160.3 88.4) (end 160.9 89) (width 0.155) (layer B.Cu) (net 14) (tstamp 59D1AC90))
  (via (at 160.9 89) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 14))
  (segment (start 168.45 90.3) (end 168.45 93.25) (width 0.155) (layer F.Cu) (net 15))
  (segment (start 160.1 89) (end 160.1 89.1) (width 0.155) (layer F.Cu) (net 15))
  (segment (start 160.1 89.1) (end 160.65 89.65) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C4D))
  (segment (start 168.25 90.1) (end 168.45 90.3) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C51))
  (segment (start 162.1 90.1) (end 168.25 90.1) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C50))
  (segment (start 161.65 89.65) (end 162.1 90.1) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C4F))
  (segment (start 160.65 89.65) (end 161.65 89.65) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C4E))
  (segment (start 168.65 93.95) (end 168.65 96.74) (width 0.155) (layer B.Cu) (net 15) (tstamp 59D22C6F) (status 20))
  (segment (start 168.2 93.5) (end 168.65 93.95) (width 0.155) (layer B.Cu) (net 15) (tstamp 59D22C6E))
  (via (at 168.2 93.5) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 15))
  (segment (start 168.45 93.25) (end 168.2 93.5) (width 0.155) (layer F.Cu) (net 15) (tstamp 59D22C6C))
  (segment (start 168.65 96.74) (end 168.25 97.14) (width 0.155) (layer B.Cu) (net 15) (tstamp 59D22C70) (status 30))
  (segment (start 168.25 97.14) (end 168.25 96.7) (width 0.155) (layer B.Cu) (net 15) (status 30))
  (via (at 160.1 89) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 15))
  (segment (start 159.6 89.5) (end 160.1 89) (width 0.155) (layer B.Cu) (net 15) (tstamp 59D1AC71))
  (segment (start 159.05 89.5) (end 159.6 89.5) (width 0.155) (layer B.Cu) (net 15) (status 10))
  (segment (start 158.7 93.4) (end 158.7 96.75) (width 0.155) (layer F.Cu) (net 16))
  (segment (start 155.8 89.5) (end 155.5 89.2) (width 0.155) (layer B.Cu) (net 16) (tstamp 59D1AD37) (status 10))
  (via (at 155.5 88.9) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 16))
  (segment (start 155.5 89.2) (end 155.5 88.9) (width 0.155) (layer B.Cu) (net 16) (tstamp 59D1AD38))
  (segment (start 155.5 88.9) (end 156 89.4) (width 0.155) (layer F.Cu) (net 16))
  (segment (start 156 89.4) (end 156 90.7) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D1AD59))
  (segment (start 156 90.7) (end 158.7 93.4) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D1AD5A))
  (segment (start 161.75 98.6) (end 161.75 100.65) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D22B56) (status 20))
  (segment (start 160.35 97.2) (end 161.75 98.6) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D22B55))
  (segment (start 159.15 97.2) (end 160.35 97.2) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D22B54))
  (segment (start 158.7 96.75) (end 159.15 97.2) (width 0.155) (layer F.Cu) (net 16) (tstamp 59D22B53))
  (segment (start 155.95 89.5) (end 155.8 89.5) (width 0.155) (layer B.Cu) (net 16) (status 30))
  (segment (start 155.95 89.5) (end 155.95 89.45) (width 0.155) (layer B.Cu) (net 16) (status 30))
  (segment (start 162.65 99.85) (end 162.65 99.839998) (width 0.155) (layer F.Cu) (net 17))
  (segment (start 163.02 100.22) (end 162.65 99.85) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B6E) (status 10))
  (segment (start 159.1 96.65) (end 159.3 96.85) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B66))
  (segment (start 159.3 96.85) (end 160.55 96.85) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B67))
  (segment (start 160.55 96.85) (end 162.1 98.4) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B68))
  (segment (start 156.1 88.8) (end 156.4 89.1) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D1AD64))
  (segment (start 156.4 89.1) (end 156.4 90.6) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D1AD65))
  (segment (start 156.25 88.65) (end 156.25 89) (width 0.155) (layer B.Cu) (net 17) (status 20))
  (via (at 156.1 88.5) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 17))
  (segment (start 156.25 88.65) (end 156.1 88.5) (width 0.155) (layer B.Cu) (net 17) (tstamp 59D1AD3D))
  (segment (start 156.1 88.5) (end 156.1 88.8) (width 0.155) (layer F.Cu) (net 17))
  (segment (start 156.4 90.6) (end 159.1 93.3) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D1AD66))
  (segment (start 159.1 93.3) (end 159.1 96.65) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D1AD67))
  (segment (start 162.1 99.289998) (end 162.1 98.4) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B80))
  (segment (start 162.65 99.839998) (end 162.1 99.289998) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22B7F))
  (segment (start 163.02 100.22) (end 163.02 100.65) (width 0.155) (layer F.Cu) (net 17) (tstamp 59D22A72) (status 30))
  (segment (start 162.45 98.2) (end 159.7 95.45) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D22B85))
  (segment (start 163.6 99.95) (end 163.3 99.95) (width 0.155) (layer F.Cu) (net 18))
  (segment (start 164.29 100.64) (end 163.6 99.95) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D22A75) (status 10))
  (segment (start 159.7 95.45) (end 159.7 94.9) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D22B87))
  (segment (start 162.45 99.1) (end 162.45 98.2) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D22B84))
  (segment (start 163.3 99.95) (end 162.45 99.1) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D22B83))
  (segment (start 164.29 100.65) (end 164.29 100.64) (width 0.155) (layer F.Cu) (net 18) (status 30))
  (segment (start 155.7 87.9) (end 156.4 87.9) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D1AD9A))
  (segment (start 159.5 93.1) (end 159.5 94.7) (width 0.155) (layer F.Cu) (net 18))
  (segment (start 156.8 90.4) (end 159.5 93.1) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D1ADA5))
  (segment (start 156.8 88.3) (end 156.8 90.4) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D1AD9F))
  (segment (start 159.5 94.7) (end 159.7 94.9) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D1B16E))
  (segment (start 155.5 88.1) (end 155.7 87.9) (width 0.155) (layer F.Cu) (net 18))
  (via (at 155.5 88.1) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 18))
  (segment (start 155.7 87.9) (end 155.5 88.1) (width 0.155) (layer B.Cu) (net 18) (tstamp 59D1AD50))
  (segment (start 156.4 87.9) (end 155.7 87.9) (width 0.155) (layer B.Cu) (net 18) (tstamp 59D1AD4F))
  (segment (start 156.75 88.25) (end 156.4 87.9) (width 0.155) (layer B.Cu) (net 18) (tstamp 59D1AD4E) (status 10))
  (segment (start 156.4 87.9) (end 156.8 88.3) (width 0.155) (layer F.Cu) (net 18) (tstamp 59D1AD9B))
  (segment (start 156.75 88.7) (end 156.75 88.25) (width 0.155) (layer B.Cu) (net 18) (status 30))
  (segment (start 165.56 100.41) (end 165.56 100.65) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A82) (status 30))
  (segment (start 165.1 99.95) (end 165.56 100.41) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A81) (status 20))
  (segment (start 164.15 99.95) (end 165.1 99.95) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A80))
  (segment (start 163.8 99.6) (end 164.15 99.95) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A7F))
  (segment (start 163.5 99.6) (end 163.8 99.6) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A7E))
  (segment (start 163.1 99.2) (end 163.5 99.6) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A7D))
  (segment (start 163.1 97.6) (end 163.1 99.2) (width 0.155) (layer F.Cu) (net 19))
  (segment (start 163.1 97.6) (end 164.9 95.8) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D22A2A))
  (segment (start 164.9 94.3) (end 164.9 95.8) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D211C7))
  (via (at 161.95 92.3) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 19))
  (segment (start 157.2 87.9) (end 157.2 90.3) (width 0.155) (layer F.Cu) (net 19))
  (segment (start 157.25 87.95) (end 157.2 87.9) (width 0.155) (layer B.Cu) (net 19) (tstamp 59D1AD55))
  (via (at 157.2 87.9) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 19))
  (segment (start 157.25 88.7) (end 157.25 87.95) (width 0.155) (layer B.Cu) (net 19) (status 10))
  (segment (start 161.35 92.3) (end 161.95 92.3) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B312))
  (segment (start 160.7 92.95) (end 161.35 92.3) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B311))
  (segment (start 159.85 92.95) (end 160.7 92.95) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B30F))
  (segment (start 157.2 90.3) (end 159.85 92.95) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B308))
  (segment (start 164.3 93.7) (end 164.9 94.3) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B449))
  (segment (start 164.3 93.35) (end 164.3 93.7) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B446))
  (segment (start 163.8 92.85) (end 164.3 93.35) (width 0.155) (layer F.Cu) (net 19) (tstamp 59D1B445))
  (via (at 163.8 92.85) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 19))
  (segment (start 163.8 92.55) (end 163.8 92.85) (width 0.155) (layer B.Cu) (net 19) (tstamp 59D1B442))
  (segment (start 163.55 92.3) (end 163.8 92.55) (width 0.155) (layer B.Cu) (net 19) (tstamp 59D1B441))
  (segment (start 161.95 92.3) (end 163.55 92.3) (width 0.155) (layer B.Cu) (net 19) (tstamp 59D1B440))
  (segment (start 159.71 99.83) (end 159.71 98.31) (width 0.155) (layer F.Cu) (net 20) (status 30))
  (segment (start 159.71 98.31) (end 158.35 96.95) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22BCE) (status 10))
  (segment (start 158.35 96.95) (end 158.35 93.55) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22BD0))
  (segment (start 156.25 91.8) (end 156.6 91.8) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22545))
  (segment (start 156.6 91.8) (end 158.35 93.55) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22533))
  (segment (start 159.75 98.75) (end 159.71 99.83) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22939) (status 30))
  (segment (start 156.25 91.5) (end 156.25 91.8) (width 0.155) (layer B.Cu) (net 20) (status 10))
  (segment (start 155.85 92.2) (end 156.25 91.8) (width 0.155) (layer F.Cu) (net 20) (tstamp 59D22541))
  (via (at 155.85 92.2) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 20))
  (segment (start 156.25 91.8) (end 155.85 92.2) (width 0.155) (layer B.Cu) (net 20) (tstamp 59D2253F))

)
