(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 26)
    (no_connects 5)
    (area 156.224999 88.974999 170.775001 103.525001)
    (thickness 1.6)
    (drawings 4)
    (tracks 129)
    (zones 0)
    (modules 8)
    (nets 34)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.155)
    (trace_clearance 0.155)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.155)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.55)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.35)
    (pad_to_mask_clearance 0.03)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J2-Pad3)")
  (net 9 "Net-(U1-Pad2)")
  (net 10 "Net-(U1-Pad27)")
  (net 11 "Net-(U1-Pad28)")
  (net 12 "Net-(U1-Pad29)")
  (net 13 "Net-(U1-Pad30)")
  (net 14 "Net-(U1-Pad31)")
  (net 15 "Net-(U1-Pad32)")
  (net 16 +5V)
  (net 17 "Net-(U1-Pad11)")
  (net 18 "Net-(U1-Pad12)")
  (net 19 "Net-(U1-Pad13)")
  (net 20 "Net-(U1-Pad14)")
  (net 21 "Net-(U1-Pad15)")
  (net 22 "Net-(U1-Pad16)")
  (net 23 "Net-(U1-Pad17)")
  (net 24 "Net-(U1-Pad18)")
  (net 25 "Net-(U1-Pad19)")
  (net 26 "Net-(U1-Pad20)")
  (net 27 "Net-(U1-Pad21)")
  (net 28 "Net-(U1-Pad22)")
  (net 29 "Net-(U1-Pad23)")
  (net 30 "Net-(U1-Pad24)")
  (net 31 "Net-(U1-Pad25)")
  (net 32 "Net-(U1-Pad26)")
  (net 33 "Net-(SW1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.155)
    (trace_width 0.155)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
  )

  (module connectors:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk (layer B.Cu) (tedit 59BC8733) (tstamp 59BC6020)
    (at 158 98.5 180)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (path /59BC8422)
    (fp_text reference J2 (at 2.4325 1.635 180) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 2.4325 -5.445 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.5 0.635) (end 1.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -4.445) (end 0.5 -4.445) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -4.445) (end 0.5 0.385) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.385) (end 0.75 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end 0.5 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 0.2) (end -0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end 0.5 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end 0.5 -1.07) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.07) (end -0.2 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -1.47) (end 0.5 -1.47) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end 0.5 -2.34) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.34) (end -0.2 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -2.74) (end 0.5 -2.74) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end 0.5 -3.61) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -3.61) (end -0.2 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -0.2 -4.01) (end 0.5 -4.01) (layer B.Fab) (width 0.1))
    (fp_line (start -1.15 1.15) (end -1.15 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.15 -4.95) (end 6 -4.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 -4.95) (end 6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6 1.15) (end -1.15 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 2 thru_hole oval (at 0 -1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59BC87AF) (tstamp 59BC5FF5)
    (at 169.1 96.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6727)
    (attr smd)
    (fp_text reference C1 (at 5.6 0 360) (layer B.SilkS)
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0.1uF (at 0 -1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 16 +5V))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59BC87A4) (tstamp 59BC5FFB)
    (at 163 100.8 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6754)
    (attr smd)
    (fp_text reference C2 (at 1.7 0 360) (layer B.SilkS)
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1uF (at 0 -1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 16 +5V))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59BC87AC) (tstamp 59BC6001)
    (at 167.5 96.8)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC6871)
    (attr smd)
    (fp_text reference C3 (at -0.05 5.7) (layer B.SilkS)
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59BC878A) (tstamp 59BC6007)
    (at 164 100.8 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (path /59BC686B)
    (attr smd)
    (fp_text reference C4 (at 1.7 -0.7 360) (layer B.SilkS)
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1uF (at 0 -1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 1.27 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1 0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end 1 0.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1 -0.4) (end -1 -0.4) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module key_switch:Cherry_MX_Matias_No_Silk_Border (layer B.Cu) (tedit 59BC8171) (tstamp 59BC8094)
    (at 163.5 96.25)
    (tags switch)
    (path /59BC89F2)
    (fp_text reference SW1 (at 0 -6) (layer Cmts.User)
      (effects (font (thickness 0.3048)))
    )
    (fp_text value SW_Push (at 1 -3.5) (layer F.Fab) hide
      (effects (font (thickness 0.3048)))
    )
    (pad 2 thru_hole circle (at 2.5 3.683) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.5 4) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (model cherry_mx1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module usb_connector:micro_usb_no_silk (layer B.Cu) (tedit 59BC86E6) (tstamp 59BC6018)
    (at 160.5 92.2)
    (path /59BC971A)
    (fp_text reference J1 (at -3.9 -4.05) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_OTG (at -0.07 -4.18) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 6 smd rect (at -3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at -1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad 6 smd rect (at -1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 16 +5V))
    (pad 6 thru_hole circle (at 2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at 1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
  )

  (module qfn:QFN-32-1EP_5x5mm_Pitch0.5mm (layer B.Cu) (tedit 59BC8661) (tstamp 59BC6051)
    (at 167.6 92.2 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (path /59BC66D6)
    (attr smd)
    (fp_text reference U1 (at 0 3.75 90) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C8051F38x_32 (at 0 -3.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.625 2.625) (end -2.625 2.125) (layer B.SilkS) (width 0.15))
    (fp_circle (center -2.625 2.625) (end -2.825 2.775) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.5 2.5) (end 2.5 2.5) (layer B.Fab) (width 0.15))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer B.Fab) (width 0.15))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer B.Fab) (width 0.15))
    (fp_line (start -2.5 -2.5) (end -2.5 1.5) (layer B.Fab) (width 0.15))
    (fp_line (start -2.5 1.5) (end -1.5 2.5) (layer B.Fab) (width 0.15))
    (fp_line (start -3 3) (end -3 -3) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3 3) (end 3 -3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3 3) (end 3 3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3 -3) (end 3 -3) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.625 2.625) (end 2.625 2.1) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.625) (end -2.625 -2.1) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.625) (end 2.625 -2.1) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.625 2.625) (end -2.1 2.625) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.625) (end -2.1 -2.625) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.625) (end 2.1 -2.625) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.625 2.625) (end 2.1 2.625) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.4 1.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at -2.4 1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.4 0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.4 0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -2.4 -0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 6 smd rect (at -2.4 -0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -2.4 -1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 16 +5V))
    (pad 8 smd rect (at -2.4 -1.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 16 +5V))
    (pad 9 smd rect (at -1.75 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 10 smd rect (at -1.25 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 11 smd rect (at -0.75 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -0.25 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 0.25 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 0.75 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.25 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 1.75 -2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 2.4 -1.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 2.4 -1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 2.4 -0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 -0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 2.4 0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.4 0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.4 1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 2.4 1.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 1.75 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 1.25 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 0.75 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 0.25 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at -0.25 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at -0.75 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at -1.25 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at -1.75 2.4) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 0.8625 -0.8625 90) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 0.8625 90) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 90) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 90) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 156.3 103.45) (end 156.3 89.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.7 103.45) (end 156.3 103.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.7 89.05) (end 170.7 103.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.3 89.05) (end 170.7 89.05) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 158 102.31) (end 157.71 102.31) (width 0.155) (layer F.Cu) (net 1) (status 30))
  (segment (start 157.71 102.31) (end 157.1 101.7) (width 0.155) (layer F.Cu) (net 1) (tstamp 59BC6C61) (status 10))
  (segment (start 161.8 91.7) (end 161.8 93.25) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6C70) (status 20))
  (via (at 161.8 91.7) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 1))
  (segment (start 160.1 93.4) (end 161.8 91.7) (width 0.155) (layer F.Cu) (net 1) (tstamp 59BC6C6C))
  (segment (start 158.1 93.4) (end 160.1 93.4) (width 0.155) (layer F.Cu) (net 1) (tstamp 59BC6C6A))
  (segment (start 157.1 94.4) (end 158.1 93.4) (width 0.155) (layer F.Cu) (net 1) (tstamp 59BC6C65))
  (segment (start 157.1 101.7) (end 157.1 94.4) (width 0.155) (layer F.Cu) (net 1) (tstamp 59BC6C62))
  (segment (start 158 102.31) (end 159.71 102.31) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 164.25 101.3) (end 164.8 101.3) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 169.1 100.4) (end 169.1 97.45) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6AF7) (status 20))
  (segment (start 167.5 102) (end 169.1 100.4) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6AF5))
  (segment (start 165.5 102) (end 167.5 102) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6AF3))
  (segment (start 164.8 101.3) (end 165.5 102) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6AF1))
  (segment (start 168.35 94.6) (end 168.35 95.05) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 168.05 96.35) (end 168.05 96.8) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6A8E) (status 20))
  (segment (start 168.6 95.8) (end 168.05 96.35) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6A8D))
  (segment (start 168.6 95.3) (end 168.6 95.8) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6A8C))
  (segment (start 168.35 95.05) (end 168.6 95.3) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6A8B))
  (segment (start 169.1 97.45) (end 168.7 97.45) (width 0.155) (layer B.Cu) (net 1) (status 10))
  (segment (start 168.7 97.45) (end 168.05 96.8) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6A83) (status 20))
  (segment (start 163.25 101.3) (end 164.25 101.3) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 159.71 102.31) (end 160.98 101.04) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6B03) (status 20))
  (segment (start 163.25 101.3) (end 161.24 101.3) (width 0.155) (layer B.Cu) (net 1) (status 30))
  (segment (start 161.24 101.3) (end 160.98 101.04) (width 0.155) (layer B.Cu) (net 1) (tstamp 59BC6AFE) (status 30))
  (segment (start 164 100.25) (end 164 99.6) (width 0.155) (layer B.Cu) (net 2))
  (segment (start 164 99.6) (end 166.8 96.8) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC90BD))
  (segment (start 166.8 96.8) (end 166.95 96.8) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC90BF))
  (segment (start 166.85 94.6) (end 166.85 95.05) (width 0.155) (layer B.Cu) (net 2) (status 10))
  (segment (start 166.95 96.35) (end 166.95 96.8) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC69EE) (status 20))
  (segment (start 166.6 96) (end 166.95 96.35) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC69EC))
  (segment (start 166.6 95.3) (end 166.6 96) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC69EB))
  (segment (start 166.85 95.05) (end 166.6 95.3) (width 0.155) (layer B.Cu) (net 2) (tstamp 59BC69EA))
  (segment (start 164.6 99) (end 162.3 99) (width 0.155) (layer F.Cu) (net 5))
  (segment (start 167.85 94.6) (end 167.85 95.45) (width 0.155) (layer B.Cu) (net 5) (status 10))
  (segment (start 168 95.6) (end 164.6 99) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC69CD))
  (via (at 168 95.6) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 5))
  (segment (start 167.85 95.45) (end 168 95.6) (width 0.155) (layer B.Cu) (net 5) (tstamp 59BC69C9))
  (segment (start 161 97.3) (end 161 96.7) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC917A))
  (segment (start 160.8 97.5) (end 161 97.3) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC9179))
  (segment (start 160.8 98.2) (end 160.8 97.5) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC9178))
  (segment (start 161.2 98.6) (end 160.8 98.2) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC9177))
  (segment (start 161.9 98.6) (end 161.2 98.6) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC9176))
  (segment (start 162.3 99) (end 161.9 98.6) (width 0.155) (layer F.Cu) (net 5) (tstamp 59BC9175))
  (segment (start 160.5 96.2) (end 160.5 93.25) (width 0.155) (layer B.Cu) (net 5) (tstamp 59BC6BF2) (status 20))
  (segment (start 161 96.7) (end 160.5 96.2) (width 0.155) (layer B.Cu) (net 5) (tstamp 59BC6BF1))
  (via (at 161 96.7) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 5))
  (segment (start 164.4 98.6) (end 162.4 98.6) (width 0.155) (layer F.Cu) (net 6))
  (via (at 161.4 98) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 6))
  (segment (start 161.4 98) (end 159.85 96.45) (width 0.155) (layer B.Cu) (net 6) (tstamp 59BC6BE6))
  (segment (start 159.85 93.25) (end 159.85 96.45) (width 0.155) (layer B.Cu) (net 6) (tstamp 59BC6BE7) (status 20))
  (segment (start 167.2 95.6) (end 167.2 95.8) (width 0.155) (layer F.Cu) (net 6))
  (segment (start 167.2 95.8) (end 164.4 98.6) (width 0.155) (layer F.Cu) (net 6) (tstamp 59BC69BA))
  (segment (start 167.35 95.45) (end 167.35 94.6) (width 0.155) (layer B.Cu) (net 6) (status 10))
  (via (at 167.2 95.6) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 6))
  (segment (start 167.35 95.45) (end 167.2 95.6) (width 0.155) (layer B.Cu) (net 6) (tstamp 59BC6994))
  (segment (start 161.8 98) (end 161.4 98) (width 0.155) (layer F.Cu) (net 6) (tstamp 59BC9172))
  (segment (start 162.4 98.6) (end 161.8 98) (width 0.155) (layer F.Cu) (net 6) (tstamp 59BC9171))
  (segment (start 162.95 93.45) (end 162.9 93.45) (width 0.155) (layer B.Cu) (net 7))
  (segment (start 165.2 93.45) (end 163 93.45) (width 0.155) (layer B.Cu) (net 7))
  (via (at 162.55 93.1) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 7))
  (segment (start 162.55 93.1) (end 161.4 93.1) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC91C5))
  (segment (start 161.4 93.1) (end 161.3 93.2) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC91C6))
  (segment (start 159.7 94.8) (end 159.7 95) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC91A9))
  (segment (start 161.3 93.2) (end 159.7 94.8) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC91A8))
  (segment (start 163 93.45) (end 162.95 93.45) (width 0.155) (layer B.Cu) (net 7))
  (segment (start 162.9 93.45) (end 162.55 93.1) (width 0.155) (layer B.Cu) (net 7) (tstamp 59BC91D0))
  (segment (start 159.7 98.5) (end 158.43 99.77) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC6BFE) (status 20))
  (segment (start 159.7 94.9) (end 159.7 95) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC6BFA))
  (segment (start 159.7 95) (end 159.7 98.5) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC91AC))
  (segment (start 158.43 99.77) (end 158 99.77) (width 0.155) (layer F.Cu) (net 7) (tstamp 59BC6C01) (status 30))
  (segment (start 165.2 93.95) (end 164.45 93.95) (width 0.155) (layer B.Cu) (net 8))
  (segment (start 161.5 93.9) (end 161.3 94.1) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC91B8))
  (segment (start 161.6 93.9) (end 161.5 93.9) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC91B7))
  (segment (start 162.6 93.9) (end 161.6 93.9) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC91B6))
  (via (at 162.6 93.9) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 8))
  (segment (start 164.4 93.9) (end 162.6 93.9) (width 0.155) (layer B.Cu) (net 8) (tstamp 59BC91B4))
  (segment (start 164.45 93.95) (end 164.4 93.9) (width 0.155) (layer B.Cu) (net 8) (tstamp 59BC91B3))
  (segment (start 158 101.04) (end 158 100.9) (width 0.155) (layer F.Cu) (net 8))
  (segment (start 158 100.9) (end 158.4 100.5) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC9192))
  (segment (start 159.3 99.6) (end 160.2 98.7) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC9184))
  (segment (start 160.2 95.2) (end 160.2 98.7) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC6C1C))
  (segment (start 161.4 94) (end 161.3 94.1) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC6C18))
  (segment (start 161.3 94.1) (end 160.2 95.2) (width 0.155) (layer F.Cu) (net 8) (tstamp 59BC91BB))
  (segment (start 159.3 99.6) (end 158.4 100.5) (width 0.155) (layer F.Cu) (net 8))
  (segment (start 158 101.04) (end 158 101) (width 0.155) (layer F.Cu) (net 8))
  (segment (start 158 101.04) (end 158.06 101.04) (width 0.155) (layer B.Cu) (net 8) (status 30))
  (segment (start 165.85 94.6) (end 165.85 95.45) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 165.85 95.45) (end 166 95.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BCCF0C))
  (segment (start 166 95.6) (end 166 95.46159) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 166.35 95.11159) (end 166.35 94.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC9168))
  (segment (start 166 95.46159) (end 166.35 95.11159) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC9167))
  (segment (start 163 100.25) (end 163 100) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 163 100) (end 166 97) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC90B3))
  (segment (start 166 97) (end 166 96.5) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC90B4))
  (segment (start 166 96.5) (end 166 95.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC90B7))
  (segment (start 163 100.25) (end 163 100.2) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 162.9 100.15) (end 162.9 99.7) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 161.8 98.6) (end 158.5 98.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC80C3))
  (segment (start 161.8 98.6) (end 162.7 99.5) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC80C4))
  (segment (start 162.7 99.5) (end 162.9 99.7) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 162.9 100.15) (end 163 100.25) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC8102))
  (segment (start 163 100.1) (end 163 100.25) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC80FE))
  (segment (start 162.9 100.15) (end 163 100.25) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC80F1))
  (segment (start 158 98.5) (end 158.4 98.5) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 158.4 98.5) (end 158.5 98.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC80C2))
  (segment (start 169.1 96.35) (end 169.1 95.7) (width 0.155) (layer B.Cu) (net 16) (status 10))
  (segment (start 168.6 95) (end 166.8 95) (width 0.155) (layer F.Cu) (net 16) (tstamp 59BC6A95))
  (segment (start 169.2 95.6) (end 168.6 95) (width 0.155) (layer F.Cu) (net 16) (tstamp 59BC6A94))
  (via (at 169.2 95.6) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 16))
  (segment (start 169.1 95.7) (end 169.2 95.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC6A91))
  (segment (start 166 95.6) (end 166.2 95.6) (width 0.155) (layer F.Cu) (net 16))
  (segment (start 166.1 95.7) (end 166 95.6) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC6A16))
  (via (at 166 95.6) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 16))
  (segment (start 166.2 95.6) (end 166.8 95) (width 0.155) (layer F.Cu) (net 16) (tstamp 59BC6A69))
  (segment (start 157.2 97.1) (end 157.2 95.2) (width 0.155) (layer B.Cu) (net 16))
  (segment (start 158 98.5) (end 158 97.9) (width 0.155) (layer B.Cu) (net 16) (status 10))
  (segment (start 158 97.9) (end 157.2 97.1) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC6616))
  (segment (start 158.65 93.75) (end 159.2 93.75) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC6886) (status 20))
  (segment (start 157.2 95.2) (end 158.65 93.75) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC6885))
  (segment (start 159.2 93.4) (end 159.2 92.8) (width 0.155) (layer B.Cu) (net 16) (tstamp 59BC661C) (status 30))
  (segment (start 158 98.44) (end 158.06 98.44) (width 0.155) (layer B.Cu) (net 16) (status 30))
  (segment (start 169.1 101.5) (end 167.12 99.52) (width 0.155) (layer F.Cu) (net 33) (tstamp 59BC6B60) (status 20))
  (via (at 169.1 101.5) (size 0.55) (drill 0.3) (layers F.Cu B.Cu) (net 33))
  (segment (start 169.8 100.8) (end 169.1 101.5) (width 0.155) (layer B.Cu) (net 33) (tstamp 59BC6B5C))
  (segment (start 169.8 94.8) (end 169.8 100.8) (width 0.155) (layer B.Cu) (net 33) (tstamp 59BC6B59))
  (segment (start 167.12 99.52) (end 166.905 99.52) (width 0.155) (layer F.Cu) (net 33) (tstamp 59BC6B61) (status 30))
  (segment (start 169.6 94.6) (end 169.8 94.8) (width 0.155) (layer B.Cu) (net 33) (tstamp 59BC6B58))
  (segment (start 169.35 94.6) (end 169.6 94.6) (width 0.155) (layer B.Cu) (net 33) (status 10))

)
