EESchema-DOCLIB  Version 2.0
#
$CMP Audio-Jack-2
D 2-pin audio jack receptable (mono/TS connector)
K audio jack receptable mono phone headphone TS connector
F ~
$ENDCMP
#
$CMP Audio-Jack-2_Switch
D 2-pin audio jack receptable (mono/TS connector) with switching contact
K audio jack receptable mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP Audio-Jack-3
D 3-pin audio jack receptable (stereo/TRS connector)
K audio jack receptable stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP Audio-Jack-3_2Switches
D 3-pin audio jack receptable (stereo/TRS connector) with 2 switching contacts
K audio jack receptable stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP Audio-Jack-3_3Switches
D 3-pin (audio) jack receptable (stereo/TRS connector) with 3 switching contacts
K audio jack receptable stereo headphones connector
F ~
$ENDCMP
#
$CMP Audio-Jack-4
D 4-pin (audio) jack receptable (stereo + 4th pin/TRRS connector)
K audio jack receptable stereo headphones TRRS connector
F ~
$ENDCMP
#
$CMP Audio-Jack-5
D 5-pin (audio) jack receptable (TRRRS connector)
K audio jack receptable stereo headphones TRRRS connector
F ~
$ENDCMP
#
$CMP Barrel_Jack
D DC Barrel Jack
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Bus_ISA_16bit
D 16-bit ISA-AT bus connector
K ISA
F https://en.wikipedia.org/wiki/Industry_Standard_Architecture
$ENDCMP
#
$CMP Bus_ISA_8bit
D 8-bit ISA-PC bus connector
K ISA
F https://en.wikipedia.org/wiki/Industry_Standard_Architecture
$ENDCMP
#
$CMP Bus_PCI_32bit_5V
D PCI bus connector for 5V cards
K PCI 5V
F http://pinouts.ru/Slots/PCI_pinout.shtml
$ENDCMP
#
$CMP Bus_PCI_32bit_Universal
D PCI bus connector for universal 5V/3.3V cards
K PCI 5V 3.3V 3V3
F http://pinouts.ru/Slots/PCI_pinout.shtml
$ENDCMP
#
$CMP C64AB
D Connector Europe 64 contacts ranges A,B
K connector DIN
$ENDCMP
#
$CMP C64AC
D Connector Europe 64 contacts, ranges A,B,C
K connector DIN
$ENDCMP
#
$CMP C96ABC
D Connector Europe, 96 contacts, ranges A,B,C
K connector
$ENDCMP
#
$CMP CUI_PD-30
D 3 pin connector, PD-30
K connector 3-pin PD-30 power DIN
F http://www.cui.com/product/resource/pd-30.pdf
$ENDCMP
#
$CMP Conn_01x01
D Generic connector, single row, 01x01
K connector
F ~
$ENDCMP
#
$CMP Conn_01x01_Female
D Generic connector, single row, 01x01
K connector
F ~
$ENDCMP
#
$CMP Conn_01x01_Male
D Generic connector, single row, 01x01
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02
D Generic connector, single row, 01x02
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02_Female
D Generic connector, single row, 01x02
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02_Male
D Generic connector, single row, 01x02
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03
D Generic connector, single row, 01x03
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03_Female
D Generic connector, single row, 01x03
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03_Male
D Generic connector, single row, 01x03
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04
D Generic connector, single row, 01x04
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04_Female
D Generic connector, single row, 01x04
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04_Male
D Generic connector, single row, 01x04
K connector
F ~
$ENDCMP
#
$CMP Conn_01x05
D Generic connector, single row, 01x05
K connector
F ~
$ENDCMP
#
$CMP Conn_01x05_Female
D Generic connector, single row, 01x05
K connector
F ~
$ENDCMP
#
$CMP Conn_01x05_Male
D Generic connector, single row, 01x05
K connector
F ~
$ENDCMP
#
$CMP Conn_01x06
D Generic connector, single row, 01x06
K connector
F ~
$ENDCMP
#
$CMP Conn_01x06_Female
D Generic connector, single row, 01x06
K connector
F ~
$ENDCMP
#
$CMP Conn_01x06_Male
D Generic connector, single row, 01x06
K connector
F ~
$ENDCMP
#
$CMP Conn_01x07
D Generic connector, single row, 01x07
K connector
F ~
$ENDCMP
#
$CMP Conn_01x07_Female
D Generic connector, single row, 01x07
K connector
F ~
$ENDCMP
#
$CMP Conn_01x07_Male
D Generic connector, single row, 01x07
K connector
F ~
$ENDCMP
#
$CMP Conn_01x08
D Generic connector, single row, 01x08
K connector
F ~
$ENDCMP
#
$CMP Conn_01x08_Female
D Generic connector, single row, 01x08
K connector
F ~
$ENDCMP
#
$CMP Conn_01x08_Male
D Generic connector, single row, 01x08
K connector
F ~
$ENDCMP
#
$CMP Conn_01x09
D Generic connector, single row, 01x09
K connector
F ~
$ENDCMP
#
$CMP Conn_01x09_Female
D Generic connector, single row, 01x09
K connector
F ~
$ENDCMP
#
$CMP Conn_01x09_Male
D Generic connector, single row, 01x09
K connector
F ~
$ENDCMP
#
$CMP Conn_01x10
D Generic connector, single row, 01x10
K connector
F ~
$ENDCMP
#
$CMP Conn_01x10_Female
D Generic connector, single row, 01x10
K connector
F ~
$ENDCMP
#
$CMP Conn_01x10_Male
D Generic connector, single row, 01x10
K connector
F ~
$ENDCMP
#
$CMP Conn_01x11
D Generic connector, single row, 01x11
K connector
F ~
$ENDCMP
#
$CMP Conn_01x11_Female
D Generic connector, single row, 01x11
K connector
F ~
$ENDCMP
#
$CMP Conn_01x11_Male
D Generic connector, single row, 01x11
K connector
F ~
$ENDCMP
#
$CMP Conn_01x12
D Generic connector, single row, 01x12
K connector
F ~
$ENDCMP
#
$CMP Conn_01x12_Female
D Generic connector, single row, 01x12
K connector
F ~
$ENDCMP
#
$CMP Conn_01x12_Male
D Generic connector, single row, 01x12
K connector
F ~
$ENDCMP
#
$CMP Conn_01x13
D Generic connector, single row, 01x13
K connector
F ~
$ENDCMP
#
$CMP Conn_01x13_Female
D Generic connector, single row, 01x13
K connector
F ~
$ENDCMP
#
$CMP Conn_01x13_Male
D Generic connector, single row, 01x13
K connector
F ~
$ENDCMP
#
$CMP Conn_01x14
D Generic connector, single row, 01x14
K connector
F ~
$ENDCMP
#
$CMP Conn_01x14_Female
D Generic connector, single row, 01x14
K connector
F ~
$ENDCMP
#
$CMP Conn_01x14_Male
D Generic connector, single row, 01x14
K connector
F ~
$ENDCMP
#
$CMP Conn_01x15
D Generic connector, single row, 01x15
K connector
F ~
$ENDCMP
#
$CMP Conn_01x15_Female
D Generic connector, single row, 01x15
K connector
F ~
$ENDCMP
#
$CMP Conn_01x15_Male
D Generic connector, single row, 01x15
K connector
F ~
$ENDCMP
#
$CMP Conn_01x16
D Generic connector, single row, 01x16
K connector
F ~
$ENDCMP
#
$CMP Conn_01x16_Female
D Generic connector, single row, 01x16
K connector
F ~
$ENDCMP
#
$CMP Conn_01x16_Male
D Generic connector, single row, 01x16
K connector
F ~
$ENDCMP
#
$CMP Conn_01x17
D Generic connector, single row, 01x17
K connector
F ~
$ENDCMP
#
$CMP Conn_01x17_Female
D Generic connector, single row, 01x17
K connector
F ~
$ENDCMP
#
$CMP Conn_01x17_Male
D Generic connector, single row, 01x17
K connector
F ~
$ENDCMP
#
$CMP Conn_01x18
D Generic connector, single row, 01x18
K connector
F ~
$ENDCMP
#
$CMP Conn_01x18_Female
D Generic connector, single row, 01x18
K connector
F ~
$ENDCMP
#
$CMP Conn_01x18_Male
D Generic connector, single row, 01x18
K connector
F ~
$ENDCMP
#
$CMP Conn_01x19
D Generic connector, single row, 01x19
K connector
F ~
$ENDCMP
#
$CMP Conn_01x19_Female
D Generic connector, single row, 01x19
K connector
F ~
$ENDCMP
#
$CMP Conn_01x19_Male
D Generic connector, single row, 01x19
K connector
F ~
$ENDCMP
#
$CMP Conn_01x20
D Generic connector, single row, 01x20
K connector
F ~
$ENDCMP
#
$CMP Conn_01x20_Female
D Generic connector, single row, 01x20
K connector
F ~
$ENDCMP
#
$CMP Conn_01x20_Male
D Generic connector, single row, 01x20
K connector
F ~
$ENDCMP
#
$CMP Conn_01x21
D Generic connector, single row, 01x21
K connector
F ~
$ENDCMP
#
$CMP Conn_01x21_Female
D Generic connector, single row, 01x21
K connector
F ~
$ENDCMP
#
$CMP Conn_01x21_Male
D Generic connector, single row, 01x21
K connector
F ~
$ENDCMP
#
$CMP Conn_01x22
D Generic connector, single row, 01x22
K connector
F ~
$ENDCMP
#
$CMP Conn_01x22_Female
D Generic connector, single row, 01x22
K connector
F ~
$ENDCMP
#
$CMP Conn_01x22_Male
D Generic connector, single row, 01x22
K connector
F ~
$ENDCMP
#
$CMP Conn_01x23
D Generic connector, single row, 01x23
K connector
F ~
$ENDCMP
#
$CMP Conn_01x23_Female
D Generic connector, single row, 01x23
K connector
F ~
$ENDCMP
#
$CMP Conn_01x23_Male
D Generic connector, single row, 01x23
K connector
F ~
$ENDCMP
#
$CMP Conn_01x24
D Generic connector, single row, 01x24
K connector
F ~
$ENDCMP
#
$CMP Conn_01x24_Female
D Generic connector, single row, 01x24
K connector
F ~
$ENDCMP
#
$CMP Conn_01x24_Male
D Generic connector, single row, 01x24
K connector
F ~
$ENDCMP
#
$CMP Conn_01x25
D Generic connector, single row, 01x25
K connector
F ~
$ENDCMP
#
$CMP Conn_01x25_Female
D Generic connector, single row, 01x25
K connector
F ~
$ENDCMP
#
$CMP Conn_01x25_Male
D Generic connector, single row, 01x25
K connector
F ~
$ENDCMP
#
$CMP Conn_01x26
D Generic connector, single row, 01x26
K connector
F ~
$ENDCMP
#
$CMP Conn_01x26_Female
D Generic connector, single row, 01x26
K connector
F ~
$ENDCMP
#
$CMP Conn_01x26_Male
D Generic connector, single row, 01x26
K connector
F ~
$ENDCMP
#
$CMP Conn_01x27
D Generic connector, single row, 01x27
K connector
F ~
$ENDCMP
#
$CMP Conn_01x27_Female
D Generic connector, single row, 01x27
K connector
F ~
$ENDCMP
#
$CMP Conn_01x27_Male
D Generic connector, single row, 01x27
K connector
F ~
$ENDCMP
#
$CMP Conn_01x28
D Generic connector, single row, 01x28
K connector
F ~
$ENDCMP
#
$CMP Conn_01x28_Female
D Generic connector, single row, 01x28
K connector
F ~
$ENDCMP
#
$CMP Conn_01x28_Male
D Generic connector, single row, 01x28
K connector
F ~
$ENDCMP
#
$CMP Conn_01x29
D Generic connector, single row, 01x29
K connector
F ~
$ENDCMP
#
$CMP Conn_01x29_Female
D Generic connector, single row, 01x29
K connector
F ~
$ENDCMP
#
$CMP Conn_01x29_Male
D Generic connector, single row, 01x29
K connector
F ~
$ENDCMP
#
$CMP Conn_01x30
D Generic connector, single row, 01x30
K connector
F ~
$ENDCMP
#
$CMP Conn_01x30_Female
D Generic connector, single row, 01x30
K connector
F ~
$ENDCMP
#
$CMP Conn_01x30_Male
D Generic connector, single row, 01x30
K connector
F ~
$ENDCMP
#
$CMP Conn_01x31
D Generic connector, single row, 01x31
K connector
F ~
$ENDCMP
#
$CMP Conn_01x31_Female
D Generic connector, single row, 01x31
K connector
F ~
$ENDCMP
#
$CMP Conn_01x31_Male
D Generic connector, single row, 01x31
K connector
F ~
$ENDCMP
#
$CMP Conn_01x32
D Generic connector, single row, 01x32
K connector
F ~
$ENDCMP
#
$CMP Conn_01x32_Female
D Generic connector, single row, 01x32
K connector
F ~
$ENDCMP
#
$CMP Conn_01x32_Male
D Generic connector, single row, 01x32
K connector
F ~
$ENDCMP
#
$CMP Conn_01x33
D Generic connector, single row, 01x33
K connector
F ~
$ENDCMP
#
$CMP Conn_01x33_Female
D Generic connector, single row, 01x33
K connector
F ~
$ENDCMP
#
$CMP Conn_01x33_Male
D Generic connector, single row, 01x33
K connector
F ~
$ENDCMP
#
$CMP Conn_01x34
D Generic connector, single row, 01x34
K connector
F ~
$ENDCMP
#
$CMP Conn_01x34_Female
D Generic connector, single row, 01x34
K connector
F ~
$ENDCMP
#
$CMP Conn_01x34_Male
D Generic connector, single row, 01x34
K connector
F ~
$ENDCMP
#
$CMP Conn_01x35
D Generic connector, single row, 01x35
K connector
F ~
$ENDCMP
#
$CMP Conn_01x35_Female
D Generic connector, single row, 01x35
K connector
F ~
$ENDCMP
#
$CMP Conn_01x35_Male
D Generic connector, single row, 01x35
K connector
F ~
$ENDCMP
#
$CMP Conn_01x36
D Generic connector, single row, 01x36
K connector
F ~
$ENDCMP
#
$CMP Conn_01x36_Female
D Generic connector, single row, 01x36
K connector
F ~
$ENDCMP
#
$CMP Conn_01x36_Male
D Generic connector, single row, 01x36
K connector
F ~
$ENDCMP
#
$CMP Conn_01x37
D Generic connector, single row, 01x37
K connector
F ~
$ENDCMP
#
$CMP Conn_01x37_Female
D Generic connector, single row, 01x37
K connector
F ~
$ENDCMP
#
$CMP Conn_01x37_Male
D Generic connector, single row, 01x37
K connector
F ~
$ENDCMP
#
$CMP Conn_01x38
D Generic connector, single row, 01x38
K connector
F ~
$ENDCMP
#
$CMP Conn_01x38_Female
D Generic connector, single row, 01x38
K connector
F ~
$ENDCMP
#
$CMP Conn_01x38_Male
D Generic connector, single row, 01x38
K connector
F ~
$ENDCMP
#
$CMP Conn_01x39
D Generic connector, single row, 01x39
K connector
F ~
$ENDCMP
#
$CMP Conn_01x39_Female
D Generic connector, single row, 01x39
K connector
F ~
$ENDCMP
#
$CMP Conn_01x39_Male
D Generic connector, single row, 01x39
K connector
F ~
$ENDCMP
#
$CMP Conn_01x40
D Generic connector, single row, 01x40
K connector
F ~
$ENDCMP
#
$CMP Conn_01x40_Female
D Generic connector, single row, 01x40
K connector
F ~
$ENDCMP
#
$CMP Conn_01x40_Male
D Generic connector, single row, 01x40
K connector
F ~
$ENDCMP
#
$CMP Conn_02x01
D Generic connector, double row, 02x01, this symbol is compatible with counter-clockwise, top-bottom and odd-even numbering schemes.
K connector
F ~
$ENDCMP
#
$CMP Conn_02x01_Row_Letter_First
D Generic connector, double row, 02x01, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x01_Row_Letter_Last
D Generic connector, double row, 02x01, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x02_Counter_Clockwise
D Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x02_Odd_Even
D Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x02_Row_Letter_First
D Generic connector, double row, 02x02, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x02_Row_Letter_Last
D Generic connector, double row, 02x02, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x02_Top_Bottom
D Generic connector, double row, 02x02, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x03_Counter_Clockwise
D Generic connector, double row, 02x03, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x03_Odd_Even
D Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x03_Row_Letter_First
D Generic connector, double row, 02x03, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x03_Row_Letter_Last
D Generic connector, double row, 02x03, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x03_Top_Bottom
D Generic connector, double row, 02x03, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x04_Counter_Clockwise
D Generic connector, double row, 02x04, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x04_Odd_Even
D Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x04_Row_Letter_First
D Generic connector, double row, 02x04, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x04_Row_Letter_Last
D Generic connector, double row, 02x04, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x04_Top_Bottom
D Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Counter_Clockwise
D Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Odd_Even
D Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Row_Letter_First
D Generic connector, double row, 02x05, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Row_Letter_Last
D Generic connector, double row, 02x05, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Top_Bottom
D Generic connector, double row, 02x05, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x06_Counter_Clockwise
D Generic connector, double row, 02x06, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x06_Odd_Even
D Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x06_Row_Letter_First
D Generic connector, double row, 02x06, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x06_Row_Letter_Last
D Generic connector, double row, 02x06, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x06_Top_Bottom
D Generic connector, double row, 02x06, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x07_Counter_Clockwise
D Generic connector, double row, 02x07, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x07_Odd_Even
D Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x07_Row_Letter_First
D Generic connector, double row, 02x07, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x07_Row_Letter_Last
D Generic connector, double row, 02x07, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x07_Top_Bottom
D Generic connector, double row, 02x07, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x08_Counter_Clockwise
D Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x08_Odd_Even
D Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x08_Row_Letter_First
D Generic connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x08_Row_Letter_Last
D Generic connector, double row, 02x08, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x08_Top_Bottom
D Generic connector, double row, 02x08, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x09_Counter_Clockwise
D Generic connector, double row, 02x09, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x09_Odd_Even
D Generic connector, double row, 02x09, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x09_Row_Letter_First
D Generic connector, double row, 02x09, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x09_Row_Letter_Last
D Generic connector, double row, 02x09, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x09_Top_Bottom
D Generic connector, double row, 02x09, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x10_Counter_Clockwise
D Generic connector, double row, 02x10, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x10_Odd_Even
D Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x10_Row_Letter_First
D Generic connector, double row, 02x10, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x10_Row_Letter_Last
D Generic connector, double row, 02x10, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x10_Top_Bottom
D Generic connector, double row, 02x10, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x11_Counter_Clockwise
D Generic connector, double row, 02x11, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x11_Odd_Even
D Generic connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x11_Row_Letter_First
D Generic connector, double row, 02x11, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x11_Row_Letter_Last
D Generic connector, double row, 02x11, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x11_Top_Bottom
D Generic connector, double row, 02x11, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x12_Counter_Clockwise
D Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x12_Odd_Even
D Generic connector, double row, 02x12, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x12_Row_Letter_First
D Generic connector, double row, 02x12, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x12_Row_Letter_Last
D Generic connector, double row, 02x12, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x12_Top_Bottom
D Generic connector, double row, 02x12, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x13_Counter_Clockwise
D Generic connector, double row, 02x13, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x13_Odd_Even
D Generic connector, double row, 02x13, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x13_Row_Letter_First
D Generic connector, double row, 02x13, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x13_Row_Letter_Last
D Generic connector, double row, 02x13, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x13_Top_Bottom
D Generic connector, double row, 02x13, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x14_Counter_Clockwise
D Generic connector, double row, 02x14, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x14_Odd_Even
D Generic connector, double row, 02x14, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x14_Row_Letter_First
D Generic connector, double row, 02x14, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x14_Row_Letter_Last
D Generic connector, double row, 02x14, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x14_Top_Bottom
D Generic connector, double row, 02x14, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x15_Counter_Clockwise
D Generic connector, double row, 02x15, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x15_Odd_Even
D Generic connector, double row, 02x15, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x15_Row_Letter_First
D Generic connector, double row, 02x15, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x15_Row_Letter_Last
D Generic connector, double row, 02x15, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x15_Top_Bottom
D Generic connector, double row, 02x15, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x16_Counter_Clockwise
D Generic connector, double row, 02x16, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x16_Odd_Even
D Generic connector, double row, 02x16, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x16_Row_Letter_First
D Generic connector, double row, 02x16, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x16_Row_Letter_Last
D Generic connector, double row, 02x16, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x16_Top_Bottom
D Generic connector, double row, 02x16, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x17_Counter_Clockwise
D Generic connector, double row, 02x17, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x17_Odd_Even
D Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x17_Row_Letter_First
D Generic connector, double row, 02x17, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x17_Row_Letter_Last
D Generic connector, double row, 02x17, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x17_Top_Bottom
D Generic connector, double row, 02x17, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x18_Counter_Clockwise
D Generic connector, double row, 02x18, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x18_Odd_Even
D Generic connector, double row, 02x18, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x18_Row_Letter_First
D Generic connector, double row, 02x18, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x18_Row_Letter_Last
D Generic connector, double row, 02x18, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x18_Top_Bottom
D Generic connector, double row, 02x18, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x19_Counter_Clockwise
D Generic connector, double row, 02x19, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x19_Odd_Even
D Generic connector, double row, 02x19, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x19_Row_Letter_First
D Generic connector, double row, 02x19, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x19_Row_Letter_Last
D Generic connector, double row, 02x19, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x19_Top_Bottom
D Generic connector, double row, 02x19, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x20_Counter_Clockwise
D Generic connector, double row, 02x20, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x20_Odd_Even
D Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x20_Row_Letter_First
D Generic connector, double row, 02x20, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x20_Row_Letter_Last
D Generic connector, double row, 02x20, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x20_Top_Bottom
D Generic connector, double row, 02x20, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x21_Counter_Clockwise
D Generic connector, double row, 02x21, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x21_Odd_Even
D Generic connector, double row, 02x21, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x21_Row_Letter_First
D Generic connector, double row, 02x21, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x21_Row_Letter_Last
D Generic connector, double row, 02x21, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x21_Top_Bottom
D Generic connector, double row, 02x21, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x22_Counter_Clockwise
D Generic connector, double row, 02x22, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x22_Odd_Even
D Generic connector, double row, 02x22, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x22_Row_Letter_First
D Generic connector, double row, 02x22, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x22_Row_Letter_Last
D Generic connector, double row, 02x22, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x22_Top_Bottom
D Generic connector, double row, 02x22, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x23_Counter_Clockwise
D Generic connector, double row, 02x23, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x23_Odd_Even
D Generic connector, double row, 02x23, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x23_Row_Letter_First
D Generic connector, double row, 02x23, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x23_Row_Letter_Last
D Generic connector, double row, 02x23, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x23_Top_Bottom
D Generic connector, double row, 02x23, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x24_Counter_Clockwise
D Generic connector, double row, 02x24, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x24_Odd_Even
D Generic connector, double row, 02x24, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x24_Row_Letter_First
D Generic connector, double row, 02x24, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x24_Row_Letter_Last
D Generic connector, double row, 02x24, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x24_Top_Bottom
D Generic connector, double row, 02x24, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x25_Counter_Clockwise
D Generic connector, double row, 02x25, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x25_Odd_Even
D Generic connector, double row, 02x25, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x25_Row_Letter_First
D Generic connector, double row, 02x25, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x25_Row_Letter_Last
D Generic connector, double row, 02x25, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x25_Top_Bottom
D Generic connector, double row, 02x25, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x26_Counter_Clockwise
D Generic connector, double row, 02x26, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x26_Odd_Even
D Generic connector, double row, 02x26, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x26_Row_Letter_First
D Generic connector, double row, 02x26, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x26_Row_Letter_Last
D Generic connector, double row, 02x26, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x26_Top_Bottom
D Generic connector, double row, 02x26, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x27_Counter_Clockwise
D Generic connector, double row, 02x27, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x27_Odd_Even
D Generic connector, double row, 02x27, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x27_Row_Letter_First
D Generic connector, double row, 02x27, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x27_Row_Letter_Last
D Generic connector, double row, 02x27, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x27_Top_Bottom
D Generic connector, double row, 02x27, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x28_Counter_Clockwise
D Generic connector, double row, 02x28, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x28_Odd_Even
D Generic connector, double row, 02x28, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x28_Row_Letter_First
D Generic connector, double row, 02x28, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x28_Row_Letter_Last
D Generic connector, double row, 02x28, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x28_Top_Bottom
D Generic connector, double row, 02x28, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x29_Counter_Clockwise
D Generic connector, double row, 02x29, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x29_Odd_Even
D Generic connector, double row, 02x29, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x29_Row_Letter_First
D Generic connector, double row, 02x29, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x29_Row_Letter_Last
D Generic connector, double row, 02x29, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x29_Top_Bottom
D Generic connector, double row, 02x29, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x30_Counter_Clockwise
D Generic connector, double row, 02x30, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x30_Odd_Even
D Generic connector, double row, 02x30, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x30_Row_Letter_First
D Generic connector, double row, 02x30, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x30_Row_Letter_Last
D Generic connector, double row, 02x30, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x30_Top_Bottom
D Generic connector, double row, 02x30, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x31_Counter_Clockwise
D Generic connector, double row, 02x31, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x31_Odd_Even
D Generic connector, double row, 02x31, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x31_Row_Letter_First
D Generic connector, double row, 02x31, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x31_Row_Letter_Last
D Generic connector, double row, 02x31, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x31_Top_Bottom
D Generic connector, double row, 02x31, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x32_Counter_Clockwise
D Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x32_Odd_Even
D Generic connector, double row, 02x32, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x32_Row_Letter_First
D Generic connector, double row, 02x32, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x32_Row_Letter_Last
D Generic connector, double row, 02x32, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x32_Top_Bottom
D Generic connector, double row, 02x32, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x33_Counter_Clockwise
D Generic connector, double row, 02x33, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x33_Odd_Even
D Generic connector, double row, 02x33, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x33_Row_Letter_First
D Generic connector, double row, 02x33, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x33_Row_Letter_Last
D Generic connector, double row, 02x33, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x33_Top_Bottom
D Generic connector, double row, 02x33, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x34_Counter_Clockwise
D Generic connector, double row, 02x34, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x34_Odd_Even
D Generic connector, double row, 02x34, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x34_Row_Letter_First
D Generic connector, double row, 02x34, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x34_Row_Letter_Last
D Generic connector, double row, 02x34, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x34_Top_Bottom
D Generic connector, double row, 02x34, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x35_Counter_Clockwise
D Generic connector, double row, 02x35, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x35_Odd_Even
D Generic connector, double row, 02x35, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x35_Row_Letter_First
D Generic connector, double row, 02x35, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x35_Row_Letter_Last
D Generic connector, double row, 02x35, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x35_Top_Bottom
D Generic connector, double row, 02x35, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x36_Counter_Clockwise
D Generic connector, double row, 02x36, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x36_Odd_Even
D Generic connector, double row, 02x36, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x36_Row_Letter_First
D Generic connector, double row, 02x36, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x36_Row_Letter_Last
D Generic connector, double row, 02x36, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x36_Top_Bottom
D Generic connector, double row, 02x36, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x37_Counter_Clockwise
D Generic connector, double row, 02x37, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x37_Odd_Even
D Generic connector, double row, 02x37, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x37_Row_Letter_First
D Generic connector, double row, 02x37, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x37_Row_Letter_Last
D Generic connector, double row, 02x37, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x37_Top_Bottom
D Generic connector, double row, 02x37, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x38_Counter_Clockwise
D Generic connector, double row, 02x38, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x38_Odd_Even
D Generic connector, double row, 02x38, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x38_Row_Letter_First
D Generic connector, double row, 02x38, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x38_Row_Letter_Last
D Generic connector, double row, 02x38, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x38_Top_Bottom
D Generic connector, double row, 02x38, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x39_Counter_Clockwise
D Generic connector, double row, 02x39, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x39_Odd_Even
D Generic connector, double row, 02x39, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x39_Row_Letter_First
D Generic connector, double row, 02x39, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x39_Row_Letter_Last
D Generic connector, double row, 02x39, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x39_Top_Bottom
D Generic connector, double row, 02x39, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x40_Counter_Clockwise
D Generic connector, double row, 02x40, counter clockwise pin numbering scheme (similar to DIP packge numbering)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x40_Odd_Even
D Generic connector, double row, 02x40, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x40_Row_Letter_First
D Generic connector, double row, 02x40, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x40_Row_Letter_Last
D Generic connector, double row, 02x40, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb))
K connector
F ~
$ENDCMP
#
$CMP Conn_02x40_Top_Bottom
D Generic connector, double row, 02x40, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins)
K connector
F ~
$ENDCMP
#
$CMP Conn_15X4
D Connector Europe, 60 contacts, ranges A,B,C,D
K connector
$ENDCMP
#
$CMP Conn_ARM_JTAG_SWD_20
D Standard IDC20 Male Connector, ARM legacy JTAG and SWD interface
K IDC20 Male Connector ARM JTAG SWD
F http://infocenter.arm.com/help/topic/com.arm.doc.dui0499b/DUI0499B_system_design_reference.pdf
$ENDCMP
#
$CMP Conn_Coaxial
D coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
$ENDCMP
#
$CMP Conn_Coaxial_Power
D coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
F ~
$ENDCMP
#
$CMP Conn_Coaxial_x2
D double coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
$ENDCMP
#
$CMP Conn_WallPlug
D 3-pin general wall plug, no Earth wire (110VAC, 220VAC)
K wall plug 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallPlug_Earth
D 3-pin general wall plug, with Earth wire (110VAC, 220VAC)
K wall plug 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallSocket
D 3-pin german wall socket, no Earth wire (110VAC, 220VAC)
K wall socket 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallSocket_Earth
D 3-pin german wall socket, with Earth wire (110VAC, 220VAC)
K wall socket 110VAC 220VAC
F ~
$ENDCMP
#
$CMP DB15_Female
D 15-pin female D-SUB connector (low-density/2 columns)
K female D-SUB connector
$ENDCMP
#
$CMP DB15_Female_HighDensity
D 15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector
K connector db15 VGA female D-SUB
$ENDCMP
#
$CMP DB15_Female_HighDensity_MountingHoles
D 15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole
K connector db15 female D-SUB VGA
$ENDCMP
#
$CMP DB15_Female_MountingHoles
D 15-pin female D-SUB connector (low-density/2 columns), Mounting Hole
K female D-SUB connector
$ENDCMP
#
$CMP DB15_Male
D 15-pin male D-SUB connector (low-density/2 columns)
K male D-SUB connector
$ENDCMP
#
$CMP DB15_Male_HighDensity
D 15-pin male D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector
K connector male VGA D-SUB
$ENDCMP
#
$CMP DB15_Male_HighDensity_MountingHoles
D 15-pin male D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole
K connector male D-SUB VGA
$ENDCMP
#
$CMP DB15_Male_MountingHoles
D 15-pin male D-SUB connector (low-density/2 columns), Mounting Hole
K male D-SUB connector
$ENDCMP
#
$CMP DB25_Female
D 25-pin female D-SUB connector
K female D-SUB connector
$ENDCMP
#
$CMP DB25_Female_MountingHoles
D 25-pin female D-SUB connector, Mounting Hole
K female D-SUB connector
$ENDCMP
#
$CMP DB25_Male
D 25-pin male D-SUB connector
K male D-SUB connector
$ENDCMP
#
$CMP DB25_Male_MountingHoles
D 25-pin male D-SUB connector, Mounting Hole
K male D-SUB connector
$ENDCMP
#
$CMP DB37_Female
D 37-pin female D-SUB connector
K female D-SUB connector
$ENDCMP
#
$CMP DB37_Female_MountingHoles
D 37-pin female D-SUB connector, Mounting Hole
K female D-SUB connector
$ENDCMP
#
$CMP DB37_Male
D 37-pin male D-SUB connector
K male D-SUB connector
$ENDCMP
#
$CMP DB37_Male_MountingHoles
D 37-pin male D-SUB connector, Mounting Hole
K male D-SUB connector
$ENDCMP
#
$CMP DB9_Female
D 9-pin female D-SUB connector
K connector female D-SUB
$ENDCMP
#
$CMP DB9_Female_MountingHoles
D 9-pin female D-SUB connector, Mounting Hole
K connector female D-SUB
$ENDCMP
#
$CMP DB9_Male
D 9-pin male D-SUB connector
K connector male D-SUB
$ENDCMP
#
$CMP DB9_Male_MountingHoles
D 9-pin male D-SUB connector, Mounting Hole
K connector male D-SUB
$ENDCMP
#
$CMP DIN-3
D 3-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-4
D 4-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-5
D 5-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-5_180degree
D 5-pin DIN connector (5-pin DIN-5 stereo)
K circular DIN connector stereo audio
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-6
D 6-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-7
D 7-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-7_CenterPin7
D 7-pin DIN connector with pin 7 in center
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-8
D 8-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP GS2
D 2-pin jumper/solder bridge
K jumper solder bridge
$ENDCMP
#
$CMP GS3
D 3-pin jumper/solder bridge
K jumper solder bridge
$ENDCMP
#
$CMP HE10-16
K connector
$ENDCMP
#
$CMP HE10-20
K connector
$ENDCMP
#
$CMP HE10-26
K connector
$ENDCMP
#
$CMP HE10-32
K connector
$ENDCMP
#
$CMP HE10-34
K connector
$ENDCMP
#
$CMP IEEE1394a
D FireWire/IEEE1394a 6-pin connector
K connector IEEE1394a FireWire
F ~
$ENDCMP
#
$CMP Jack-DC
D DC Barrel Jack
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP LEMO2
D 2-pin LEMO connector
K LEMO connector
$ENDCMP
#
$CMP LEMO4
D 4-pin LEMO connector
K LEMO connector
$ENDCMP
#
$CMP LEMO5
D 5-pin LEMO connector
K LEMO connector
$ENDCMP
#
$CMP LEMO6
D 6-pin LEMO connector
K LEMO connector
$ENDCMP
#
$CMP Micro_SD_Card
D Micro SD Card Socket
K connector SD microsd
F http://katalog.we-online.de/em/datasheet/693072010801.pdf
$ENDCMP
#
$CMP Micro_SD_Card_Det
D Micro SD Card Socket with card detection pins
K connector SD microsd
F https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1
$ENDCMP
#
$CMP Micro_SD_Card_Det_Hirose_DM3AT
D Micro SD Card Socket with card detection pins
K connector SD microsd
F https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1
$ENDCMP
#
$CMP Mini-DIN-3
D 3-pin Mini-DIN connector
K Mini-DIN
F http://www.assmann-wsw.com/fileadmin/catalogue/10_MiniDIN_rev4-0.pdf
$ENDCMP
#
$CMP Mini-DIN-4
D 4-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-5
D 5-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-6
D 6-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-7
D 7-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-8
D 8-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP RJ12
D RJ12 connector with 2 shield pins
K RJ12 connector
$ENDCMP
#
$CMP RJ45
D RJ45 connector with shield
K RJ45
$ENDCMP
#
$CMP RJ45-TRANSFO
D RJ45 with transformer + leds WURTH
K RJ45
$ENDCMP
#
$CMP RJ45_LEDS
D RJ45, status leds
K RJ45 RJ45_LEDS
$ENDCMP
#
$CMP Raspberry_Pi_2_3
D expansion header for Raspberry Pi 2 & 3
K raspberrypi gpio
F https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/RPI-3B-V1_2-SCHEMATIC-REDUCED.pdf
$ENDCMP
#
$CMP SCART-F
D Prise Peritel
K connector
$ENDCMP
#
$CMP SD_Card
D SD Card Reader
K connector SD
F http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf
$ENDCMP
#
$CMP SIM_Card
D SIM Card
K SIM card UICC
$ENDCMP
#
$CMP Screw_Terminal_01x01
D Generic screw terminal, single row, 01x01
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x02
D Generic screw terminal, single row, 01x02
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x03
D Generic screw terminal, single row, 01x03
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x04
D Generic screw terminal, single row, 01x04
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x05
D Generic screw terminal, single row, 01x05
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x06
D Generic screw terminal, single row, 01x06
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x07
D Generic screw terminal, single row, 01x07
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x08
D Generic screw terminal, single row, 01x08
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x09
D Generic screw terminal, single row, 01x09
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x10
D Generic screw terminal, single row, 01x10
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x11
D Generic screw terminal, single row, 01x11
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x12
D Generic screw terminal, single row, 01x12
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x13
D Generic screw terminal, single row, 01x13
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x14
D Generic screw terminal, single row, 01x14
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x15
D Generic screw terminal, single row, 01x15
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x16
D Generic screw terminal, single row, 01x16
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x17
D Generic screw terminal, single row, 01x17
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x18
D Generic screw terminal, single row, 01x18
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x19
D Generic screw terminal, single row, 01x19
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x20
D Generic screw terminal, single row, 01x20
K screw terminal
F ~
$ENDCMP
#
$CMP TEST_1P
D point
K point tp
$ENDCMP
#
$CMP TEST_2P
D point
K point tp
$ENDCMP
#
$CMP USB3_A
D USB 3.0 A connector
K usb universal serial bus
F ~
$ENDCMP
#
$CMP USB3_B
D USB 3.0 B connector
K usb universal serial bus
F ~
$ENDCMP
#
$CMP USB_A
D USB Type A connector
K connector USB
$ENDCMP
#
$CMP USB_B
D USB Type B connector
K connector USB
$ENDCMP
#
$CMP USB_C_Plug
D USB Type-C Plug connector
K usb universal serial bus
F http://www.usb.org/developers/docs/usb_31_033017.zip
$ENDCMP
#
$CMP USB_C_Receptacle
D USB Type-C Receptacle connector
K usb universal serial bus
F http://www.usb.org/developers/docs/usb_31_033017.zip
$ENDCMP
#
$CMP USB_OTG
D USB mini/micro connector
K connector USB
$ENDCMP
#
$CMP XLR3
D 3 pins
K connector
$ENDCMP
#
$CMP XLR4
D 4 pins
K connector
$ENDCMP
#
$CMP XLR5
D 5 pins
K connector
$ENDCMP
#
#End Doc Library
