(module TC2050-NL_SMALL (layer F.Cu) (tedit 4FBDD038)
  (descr "Tag-Connect TC2050-NL footprint by carloscuev@gmail.com")
  (tags "Tag-Connect TC2050-NL")
  (clearance 0.127)
  (attr virtual)
  (fp_text reference TC2050-NL (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_text value VAL (at 0 2.667) (layer F.SilkS) hide
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_line (start 3.8735 1.905) (end -3.3528 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.8735 -1.905) (end -3.3528 -1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start -4.5339 0.7239) (end -3.3528 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start -4.5339 -0.7239) (end -3.3528 -1.905) (layer F.SilkS) (width 0.127))
  (fp_arc (start -3.81 0) (end -4.5339 0.7239) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_line (start 4.826 -0.9525) (end 4.826 0.9525) (layer F.SilkS) (width 0.127))
  (fp_arc (start 3.8735 0.9525) (end 4.826 0.9525) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_arc (start 3.8735 -0.9525) (end 3.8735 -1.905) (angle 90) (layer F.SilkS) (width 0.127))
  (pad 6 connect circle (at 2.54 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 5 connect circle (at 2.54 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 7 connect circle (at 1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 4 connect circle (at 1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 1 connect circle (at -2.54 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 10 connect circle (at -2.54 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 2 connect circle (at -1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 9 connect circle (at -1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 3 connect circle (at 0 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 8 connect circle (at 0 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad "" np_thru_hole circle (at -3.81 0) (size 0.98806 0.98806) (drill 0.98806) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 3.81 -1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 3.81 1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
)
