(module SwitchPush_C&K_MultiFoot_RS-187R05A2-DS_And_PTS645_SMT (layer F.Cu) (tedit 5A3859B9)
  (descr https://media.digikey.com/pdf/Data%20Sheets/C&K/RS-187R05-DS%20MT_RT.pdf)
  (tags "switch, push button")
  (fp_text reference REF** (at 0 4.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SwitchPush_C&K_RS-187R05A2-DS (at 0 -4.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.3 -2.9) (end 3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.3 2.9) (end 3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.3 -2.9) (end -3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.3 -2.9) (end -3.3 -2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.6 1.2) (end -2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start -1.2 -2.6) (end -2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start 1.2 -2.6) (end -1.2 -2.6) (layer F.Fab) (width 0.15))
  (fp_line (start 2.6 -1.2) (end 1.2 -2.6) (layer F.Fab) (width 0.15))
  (fp_line (start 2.6 1.2) (end 2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start 1.2 2.6) (end 2.6 1.2) (layer F.Fab) (width 0.15))
  (fp_line (start -1.2 2.6) (end 1.2 2.6) (layer F.Fab) (width 0.15))
  (fp_line (start -2.6 1.2) (end -1.2 2.6) (layer F.Fab) (width 0.15))
  (fp_line (start -3 3) (end 3 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 1) (end 3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 -3) (end -3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -1) (end -3 1) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 1.75 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -3.25) (end -4.5 3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.5 3.25) (end 4.5 3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 -3.25) (end -4.5 -3.25) (layer F.CrtYd) (width 0.15))
  (fp_circle (center 0 0) (end 1.75 0) (layer F.Fab) (width 0.15))
  (fp_line (start -3 -3) (end 3 -3) (layer F.Fab) (width 0.15))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.15))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.15))
  (fp_line (start -3 3) (end -3 -3) (layer F.Fab) (width 0.15))
  (pad 2 smd rect (at -3.1 1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.1 1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.1 -1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.1 -1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
)
