(module USB_TypeC_Hirose_CX70M-24P1 (layer F.Cu) (tedit 5A2BC3BC)
  (descr "https://www.hirose.com/product/en/download_file/key_name/CX70M-24P1/category/Drawing%20(2D)/doc_file_id/141189/?file_category_id=6&item_id=04800304000&is_series=")
  (tags "USB, Type-C")
  (fp_text reference J1 (at 0 -3.6) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_C_Receptacle (at -0.1 1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.67 -6.65) (end 4.67 -6.65) (layer F.CrtYd) (width 0.1))
  (fp_line (start 6.2 0) (end 4.67 0) (layer F.CrtYd) (width 0.1))
  (fp_line (start 4.67 0) (end 4.67 -6.65) (layer F.CrtYd) (width 0.1))
  (fp_line (start -4.67 0) (end -4.67 -6.65) (layer F.CrtYd) (width 0.1))
  (fp_line (start -6.2 0) (end -4.67 0) (layer F.CrtYd) (width 0.1))
  (pad "" np_thru_hole circle (at 4.67 -6.15) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  (pad S1 smd rect (at 3.915 -8.325) (size 0.46 0.9) (layers F.Cu F.Paste F.Mask))
  (pad S1 smd rect (at -3.915 -8.325) (size 0.46 0.9) (layers F.Cu F.Paste F.Mask))
  (pad S1 smd rect (at -5.2 -2.6) (size 0.7 2.3) (layers B.Cu B.Mask))
  (pad S1 smd rect (at 5.2 -2.6) (size 0.7 2.3) (layers B.Cu B.Mask))
  (pad S1 thru_hole oval (at 5.55 -2.6) (size 1.3 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 smd rect (at 5.2 -2.6) (size 0.7 2.3) (layers F.Cu F.Mask))
  (pad S1 thru_hole oval (at -5.55 -2.6) (size 1.3 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -5.55 -7.65) (size 1.2 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at 5.55 -7.65) (size 1.2 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 smd rect (at -5.2 -2.6) (size 0.7 2.3) (layers F.Cu F.Mask))
  (pad B12 smd rect (at -3.4 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B11 smd rect (at -3 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B10 smd rect (at -2.6 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A1 smd rect (at -2.2 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd rect (at -1.8 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd rect (at -1.4 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A4 smd rect (at -1 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A5 smd rect (at -0.6 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A6 smd rect (at -0.2 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A7 smd rect (at 0.2 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A8 smd rect (at 0.6 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A9 smd rect (at 1 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A10 smd rect (at 1.4 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A11 smd rect (at 1.8 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A12 smd rect (at 2.2 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd rect (at 2.6 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd rect (at 3 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd rect (at 3.4 -8.325) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B9 thru_hole circle (at -2 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B8 thru_hole circle (at -1.2 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B7 thru_hole circle (at -0.4 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B6 thru_hole circle (at 0.4 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B5 thru_hole circle (at 1.2 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B4 thru_hole circle (at 2 -7.2) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -4.67 -6.15) (size 1 1) (drill 1) (layers *.Cu *.Mask))
)
