(module split-planck:Switch-smd-slide-6pin (layer F.Cu) (tedit 57528C8F)
  (fp_text reference REF** (at 0 4.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Switch-smd-slide-6pin (at 0 -4.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.5 3.6) (end 3.5 -3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 3.6) (end 3.5 3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 -3.6) (end -3.5 3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 -3.6) (end 3.5 -3.6) (layer F.SilkS) (width 0.15))
  (pad 4 smd rect (at -2.5 -2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 -2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.5 -2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.5 2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.5 2.5) (size 0.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 1.5 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -1.5 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
)
