(module Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer F.Cu) (tedit 59D21DD6)
  (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
  (tags "Through hole angled pin header THT 1x04 1.27mm single row")
  (fp_text reference J3 (at 2.4325 -1.635) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Conn_01x04 (at 2.4325 5.445) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5 -0.635) (end 1.5 4.445) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 4.445) (end 0.5 4.445) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 4.445) (end 0.5 -0.385) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -0.385) (end 0.75 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 -0.2) (end 0.5 -0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 0.2) (end 0.5 0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 1.07) (end 0.5 1.07) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 1.07) (end -0.2 1.47) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 1.47) (end 0.5 1.47) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 2.34) (end 0.5 2.34) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 2.34) (end -0.2 2.74) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 2.74) (end 0.5 2.74) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 3.61) (end 0.5 3.61) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 3.61) (end -0.2 4.01) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 4.01) (end 0.5 4.01) (layer F.Fab) (width 0.1))
  (fp_line (start -1.15 -1.15) (end -1.15 4.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.15 4.95) (end 6 4.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6 4.95) (end 6 -1.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6 -1.15) (end -1.15 -1.15) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 0 1.27) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at 0 2.54) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at 0 3.81) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
)
