(module NRF24L01-Module-SMD (layer F.Cu) (tedit 5A78B6DD)
  (descr "Through hole pin header, pitch 1.27mm")
  (tags "pin header")
  (fp_text reference REF** (at -9.5 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value nRF24L01_module (at -8 -5.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user IRQ (at -2.1 -4.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MISO (at -2.6 -3.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MOSI (at -2.6 -1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SCK (at -2.3 -0.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user CSN (at -2.3 0.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user CE (at -2.05 1.95) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -2.3 3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at -2.3 4.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -17 6) (end 1 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -17 -6) (end -17 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -6) (end -17 -6) (layer F.SilkS) (width 0.15))
  (pad 8 smd rect (at 0.3 -4.445) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.3 -3.175) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.3 -1.905) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.3 -0.635) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.3 0.635) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.3 1.905) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.3 3.175) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0.3 4.445) (size 2.5 0.95) (drill (offset 0.45 0)) (layers F.Cu F.Paste F.Mask))
)
