(module SwitchPush_C&K_RS-187R05A2-DS (layer F.Cu) (tedit 5A3859E4)
  (descr https://media.digikey.com/pdf/Data%20Sheets/C&K/RS-187R05-DS%20MT_RT.pdf)
  (tags "switch, push button")
  (fp_text reference REF** (at 0 3.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SwitchPush_C&K_RS-187R05A2-DS (at 0 -3.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.3 -2.9) (end 3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.3 2.9) (end 3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.3 -2.9) (end -3.3 2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.3 -2.9) (end -3.3 -2.9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.6 1.2) (end -2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start -1.2 -2.6) (end -2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start 1.2 -2.6) (end -1.2 -2.6) (layer F.Fab) (width 0.15))
  (fp_line (start 2.6 -1.2) (end 1.2 -2.6) (layer F.Fab) (width 0.15))
  (fp_line (start 2.6 1.2) (end 2.6 -1.2) (layer F.Fab) (width 0.15))
  (fp_line (start 1.2 2.6) (end 2.6 1.2) (layer F.Fab) (width 0.15))
  (fp_line (start -1.2 2.6) (end 1.2 2.6) (layer F.Fab) (width 0.15))
  (fp_line (start -2.6 1.2) (end -1.2 2.6) (layer F.Fab) (width 0.15))
  (fp_line (start -2.6 -1.05) (end -2.6 1.05) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.6 2.65) (end 2.6 2.65) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.6 1.05) (end 2.6 -1.05) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.6 -2.65) (end -2.6 -2.65) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 0 -1) (layer F.SilkS) (width 0.15))
  (pad 2 smd rect (at -3.1 1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.1 1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.1 -1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.1 -1.85) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask))
)
