(module TC2030-NL_SMALL_AND_IDC_PDI (layer F.Cu) (tedit 5A4D5A09)
  (descr "Tag-Connect TC2030-NL footprint by carloscuev@gmail.com")
  (tags "Tag-Connect TC2030-NL")
  (clearance 0.127)
  (attr virtual)
  (fp_text reference J3 (at -3 2 90) (layer F.SilkS)
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_text value TC2030-IDC (at -1.933 0 90) (layer F.SilkS) hide
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_line (start 2.6035 1.905) (end 2.3035 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.4 -1.9) (end -0.4 -1.9) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.3 1.9) (end -0.4 1.9) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.2639 0.7239) (end -2.0828 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.2639 -0.7239) (end -2.0828 -1.905) (layer F.SilkS) (width 0.127))
  (fp_arc (start -2.54 0) (end -3.2639 0.7239) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.556 -0.9525) (end 3.556 0.9525) (layer F.SilkS) (width 0.127))
  (fp_arc (start 2.6035 0.9525) (end 3.556 0.9525) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_arc (start 2.6035 -0.9525) (end 2.6035 -1.905) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.6035 -1.905) (end 2.3035 -1.905) (layer F.SilkS) (width 0.127))
  (pad 1 connect circle (at -1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 2 connect circle (at -1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 5 connect circle (at 1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 6 connect circle (at 1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad "" np_thru_hole circle (at -2.54 0) (size 0.98806 0.98806) (drill 0.98806) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 2.54 -1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 2.54 1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
