(module NRF24L01-Module-SMD-TH (layer F.Cu) (tedit 5A1BF4A9)
  (descr "Through hole pin header, pitch 1.27mm")
  (tags "pin header")
  (fp_text reference U3 (at 2.5 0 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NRF24L01_module (at -8 -7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user IRQ (at -2.4 -4.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MISO (at -2.5 -3.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MOSI (at -2.5 -1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SCK (at -2.3 -0.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user CSN (at -2.3 0.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user CE (at -2.35 1.95) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -2.3 3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at -2.3 4.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -17 6) (end 1 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -17 -6) (end -17 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -6) (end -17 -6) (layer F.SilkS) (width 0.15))
  (pad 8 thru_hole rect (at 0 -4.445) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole rect (at 0 -3.175) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole rect (at 0 -1.905) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole rect (at 0 -0.635) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole rect (at 0 0.635) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole rect (at 0 1.905) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole rect (at 0 3.175) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole rect (at 0 4.445) (size 2 0.95) (drill 0.65 (offset 0.45 0)) (layers *.Cu *.Mask F.SilkS))
)
