(module PG1350 (layer F.Cu) (tedit 5A0E6266)
  (descr "Kailh LP switch")
  (fp_text reference SW1 (at 0 4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_PUSH (at 0 -8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 2 (at -0.5 -5.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 1 (at -5 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 7.5 0) (end 7.5 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.5 -7.5) (end -7.5 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.5 -7.5) (end -7.5 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.5 7.5) (end 7.5 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.5 7.5) (end 7.5 0) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 5 -3.8) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -5 -3.8) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 -5.9) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
)
