(module SwitchPush_C&K_PTS645_SMT (layer F.Cu) (tedit 5A385A0F)
  (fp_text reference REF** (at 0 -3.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SwitchPush_C&K_PTS645_SMT (at 0 4.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 3) (end 3 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 3) (end 3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 -3) (end -3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -3) (end -3 3) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 1.75 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -3.25) (end -4.5 3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.5 3.25) (end 4.5 3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 -3.25) (end -4.5 -3.25) (layer F.CrtYd) (width 0.15))
  (fp_circle (center 0 0) (end 1.75 0) (layer F.Fab) (width 0.15))
  (fp_line (start -3 -3) (end 3 -3) (layer F.Fab) (width 0.15))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.15))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.15))
  (fp_line (start -3 3) (end -3 -3) (layer F.Fab) (width 0.15))
  (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
)
