(module USB_TypeC_Hirose_CX70M-24P1 (layer F.Cu) (tedit 5A77C92D)
  (descr "https://www.hirose.com/product/en/download_file/key_name/CX70M-24P1/category/Drawing%20(2D)/doc_file_id/141189/?file_category_id=6&item_id=04800304000&is_series=")
  (tags "USB, Type-C")
  (attr smd)
  (fp_text reference J1 (at 0.57 0 90) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_C_Receptacle (at 0 -0.01) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.48 4.67) (end -2.48 -4.67) (layer F.CrtYd) (width 0.1))
  (fp_line (start 4.17 -6.2) (end 4.17 -4.67) (layer F.CrtYd) (width 0.1))
  (fp_line (start 4.17 -4.67) (end -2.48 -4.67) (layer F.CrtYd) (width 0.1))
  (fp_line (start 4.17 4.67) (end -2.48 4.67) (layer F.CrtYd) (width 0.1))
  (fp_line (start 4.17 6.2) (end 4.17 4.67) (layer F.CrtYd) (width 0.1))
  (pad "" np_thru_hole circle (at -2.25 -4.5 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  (pad S1 smd oval (at -4.155 -3.915 90) (size 0.46 0.9) (layers F.Cu F.Paste F.Mask))
  (pad S1 smd oval (at -4.155 3.915 90) (size 0.46 0.9) (layers F.Cu F.Paste F.Mask))
  (pad S1 smd rect (at 1.57 5.2 90) (size 0.7 2.3) (layers B.Cu B.Mask))
  (pad S1 smd rect (at 1.57 -5.2 90) (size 0.7 2.3) (layers B.Cu B.Mask))
  (pad S1 thru_hole oval (at 1.57 -5.55 90) (size 1.3 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 smd rect (at 1.57 -5.2 90) (size 0.7 2.3) (layers F.Cu F.Mask))
  (pad S1 thru_hole oval (at 1.57 5.55 90) (size 1.3 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -3.48 5.55 90) (size 1.2 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -3.48 -5.55 90) (size 1.2 2.3) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad S1 smd rect (at 1.57 5.2 90) (size 0.7 2.3) (layers F.Cu F.Mask))
  (pad B12 smd oval (at -4.155 3.4 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B11 smd oval (at -4.155 3 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B10 smd oval (at -4.155 2.6 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A1 smd oval (at -4.155 2.2 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd oval (at -4.155 1.8 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd oval (at -4.155 1.4 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A4 smd oval (at -4.155 1 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A5 smd oval (at -4.155 0.6 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A6 smd oval (at -4.155 0.2 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A7 smd oval (at -4.155 -0.2 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A8 smd oval (at -4.155 -0.6 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A9 smd oval (at -4.155 -1 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A10 smd oval (at -4.155 -1.4 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A11 smd oval (at -4.155 -1.8 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad A12 smd oval (at -4.155 -2.2 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd oval (at -4.155 -2.6 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd oval (at -4.155 -3 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd oval (at -4.155 -3.4 90) (size 0.23 0.9) (layers F.Cu F.Paste F.Mask))
  (pad B9 thru_hole circle (at -3.03 2 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B8 thru_hole circle (at -3.03 1.2 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B7 thru_hole circle (at -3.03 0.4 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B6 thru_hole circle (at -3.03 -0.4 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B5 thru_hole circle (at -3.03 -1.2 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad B4 thru_hole circle (at -3.03 -2 90) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.25 4.5 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
)
