VERSION 5.8 ;
ALIAS alias1 aliasValue1 1 ;
ALIAS alias2 aliasValue2 0 ;
DIVIDERCHAR "/" ;
BUSBITCHARS "[]" ;
DESIGN design ;
TECHNOLOGY technology ;
UNITS DISTANCE MICRONS 1000 ;

PROPERTYDEFINITIONS
DESIGN strprop STRING "aString" ;
DESIGN intprop INTEGER 1 ;
DESIGN realprop REAL 1.1 ;
DESIGN intrangeprop INTEGER RANGE 1 100 25 ;
DESIGN realrangeprop REAL RANGE 1.1 100.1 25.25 ;
REGION strprop STRING ;
REGION intprop INTEGER ;
REGION realprop REAL ;
REGION intrangeprop INTEGER RANGE 1 100 ;
REGION realrangeprop REAL RANGE 1.1 100.1 ;
GROUP strprop STRING ;
GROUP intprop INTEGER ;
GROUP realprop REAL ;
GROUP intrangeprop INTEGER RANGE 1 100 ;
GROUP realrangeprop REAL RANGE 1.1 100.1 ;
COMPONENT strprop STRING ;
COMPONENT intprop INTEGER ;
COMPONENT realprop REAL ;
COMPONENT intrangeprop INTEGER RANGE 1 100 ;
COMPONENT realrangeprop REAL RANGE 1.1 100.1 ;
NET strprop STRING ;
NET intprop INTEGER ;
NET realprop REAL ;
NET intrangeprop INTEGER RANGE 1 100 ;
NET realrangeprop REAL RANGE 1.1 100.1 ;
SPECIALNET strprop STRING ;
SPECIALNET intprop INTEGER ;
SPECIALNET realprop REAL ;
SPECIALNET intrangeprop INTEGER RANGE 1 100 ;
SPECIALNET realrangeprop REAL RANGE 1.1 100.1 ;
Parsed 50 number of lines!!
ROW strprop STRING ;
ROW intprop INTEGER ;
ROW realprop REAL ;
ROW intrangeprop INTEGER RANGE 1 100 ;
ROW realrangeprop REAL RANGE 1.1 100.1 ;
COMPONENTPIN strprop STRING ;
COMPONENTPIN intprop INTEGER ;
COMPONENTPIN realprop REAL ;
COMPONENTPIN intrangeprop INTEGER RANGE 1 100 ;
COMPONENTPIN realrangeprop REAL RANGE 1.1 100.1 ;
NONDEFAULTRULE strprop STRING ;
NONDEFAULTRULE intprop INTEGER ;
NONDEFAULTRULE realprop REAL ;
NONDEFAULTRULE intrangeprop INTEGER RANGE 1 100 ;
NONDEFAULTRULE realrangeprop REAL RANGE 1.1 100.1 ;
END PROPERTYDEFINITIONS

DIEAREA -190000 -120000 -190000 350000 ;
DIEAREA -190000 -120000 -190000 350000 190000 350000 190000 190000 190360 190000 190360 -120000 ;
ROW ROW_1 CORE 1000 1000 N DO 100 BY 1 STEP 700 0 ;
  + PROPERTY strprop aString STRING   + PROPERTY intprop 1 INTEGER   + PROPERTY realprop 1.1 REAL   + PROPERTY intrangeprop 25 INTEGER   + PROPERTY realrangeprop 25.25 REAL ;
ROW ROW_2 CORE 1000 2000 S DO 100 BY 1 STEP 700 0 ;
ROW ROW_3 CORE 1000 3000 E DO 100 BY 1 STEP 8400 0 ;
ROW ROW_4 CORE 1000 4000 W DO 100 BY 1 STEP 8400 0 ;
ROW ROW_5 CORE 1000 5000 FN DO 100 BY 1 STEP 700 0 ;
ROW ROW_6 CORE 1000 6000 FS DO 100 BY 1 STEP 700 0 ;
ROW ROW_7 CORE 1000 7000 FE DO 100 BY 1 STEP 8400 0 ;
ROW ROW_8 CORE 1000 8000 FW DO 100 BY 1 STEP 8400 0 ;
ROW ROW_VERT_1 CORE -10000 -10000 N DO 1 BY 10 STEP 0 8400 ;
ROW ROW_VERT_2 CORE -9000 -10000 S DO 1 BY 10 STEP 0 8400 ;
ROW ROW_VERT_3 CORE -8000 -10000 E DO 1 BY 10 STEP 0 700 ;
Parsed 100 number of lines!!
ROW ROW_VERT_4 CORE -7000 -10000 W DO 1 BY 10 STEP 0 700 ;
ROW ROW_VERT_5 CORE -6000 -10000 FN DO 1 BY 10 STEP 0 8400 ;
ROW ROW_VERT_6 CORE -5000 -10000 FS DO 1 BY 10 STEP 0 8400 ;
ROW ROW_VERT_7 CORE -4000 -10000 FE DO 1 BY 10 STEP 0 700 ;
ROW ROW_VERT_8 CORE -3000 -10000 FW DO 1 BY 1 STEP 0 700 ;
ROW ROW_array0 ARRAYSITE 10000 10000 N DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array1 ARRAYSITE 10000 17000 W DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array2 ARRAYSITE 10000 17000 S DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array3 ARRAYSITE 10000 17000 E DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array4 ARRAYSITE 10000 17000 FN DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array5 ARRAYSITE 10000 17000 FE DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array6 ARRAYSITE 10000 17000 FS DO 100 BY 1 STEP 16000 0 ;
ROW ROW_array7 ARRAYSITE 10000 17000 FW DO 100 BY 1 STEP 16000 0 ;
TRACKS Y 52 DO 857 STEP 104 MASK 1 LAYER ;
TRACKS Y 52 DO 857 STEP 104 MASK 1 SAMEMASK LAYER M1 M2 ;
TRACKS X 52 DO 1720 STEP 104 MASK 2 LAYER M2 ;
TRACKS X 52 DO 1720 STEP 104 LAYER ;
GCELLGRID X 0 DO 100 STEP 600 ;
GCELLGRID Y 10 DO 120 STEP 400 ;

VIAS 6 ;
Parsed 150 number of lines!!
- VIAGEN12_0 + RECT METAL1 -4400 -3800 4400 3800 
+ RECT M2 + MASK 3 -4500 -3800 4500 3800 
+ RECT V1 + MASK 2 -3600 -3800 -2000 -2200 
+ RECT V1 + MASK 1 -3600 2200 -2000 3800 
+ RECT V1 + MASK 2 2000 -3800 3600 -2200 
+ RECT V1 + MASK 3 2000 2200 3600 3800 
 ;
- VIAGEN12_2 + RECT METAL1 -2500 -1500 2500 1500 
+ RECT M2 -2500 -1500 2500 1500 
+ RECT V1 -2360 -960 -760 640 
+ RECT V1 -1320 -960 280 640 
+ RECT V1 760 -960 2360 640 
 ;
- VIAGEN12_3 + RECT METAL1 -1600 -1600 1600 1600 
+ RECT M2 -1600 -1600 1600 1600 
+ RECT V1 -800 -800 800 800 
 ;
- VIAGEN12_4  ;
+ VIARULE 'VIAGEN12'
  + CUTSIZE 1600 1600
  + LAYERS M1 V1 M2
  + CUTSPACING 5600 6100
  + ENCLOSURE 100 100 150 150
  + ROWCOL 5 14
  + ORIGIN 10 -10
  + OFFSET 0 0 20 -20
  + PATTERN '2_FFE0_3_FFFF'
- M2_M1rct_0 + RECT V1 -25 -65 25 65 
+ RECT M1 -35 -95 35 95 
+ RECT M2 -65 -65 65 65 
 ;
- VIAGEN12_1 + RECT M2 -2500 -1500 2500 1500 
+ RECT V1 -2400 -960 -700 640 

  + POLYGON METAL1 + MASK 2 -2500 -1500 -2500 2500 1500 2500 1500 1500 2500 1500 2500 -1500  ;
END VIAS
- CUSTOMVIA 
  + POLYGON METAL1 + MASK 3 -2500 -1500 -2500 2500 1500 2500 1500 1500 2500 1500 2500 -1500  ;
END VIAS
- TURNM1_1 + RECT METAL1 -100 -60 100 60 
 ;
END VIAS
- TURNM2_1 + RECT M2 -100 -60 100 60 
 ;
END VIAS
Parsed 200 number of lines!!
- TURNM3_1 + RECT M3 -100 -60 100 60 
 ;
END VIAS
- myvia1 + RECT METAL1 + MASK 2 0 0 40000 40000 
+ RECT V1 + MASK 3 0 0 40000 40000 
+ RECT M2 0 0 40000 40000 
 ;
END VIAS

STYLES 10 ;
- STYLE 0 30 10 10 30 -10 30 -30 10 -30 -10 -10 -30 10 -30 30 -10 ;
- STYLE 1 25 25 -25 25 -25 -25 25 -25 ;
- STYLE 2 50 50 -50 50 -50 -50 50 -50 ;
- STYLE 3 50 21 21 50 -21 50 -50 21 -50 -21 -21 -50 21 -50 50 -21 ;
- STYLE 4 -30 -20 10 -60 50 -20 50 40 0 40 -30 10 ;
- STYLE 5 0 2000 0 -2000 0 2000 0 -2000 ;
- STYLE 6 -2000 2000 2000 -2000 2000 -2000 ;
- STYLE 7 0 0 0 1000 1000 0 ;
- STYLE 8 -7500 -3110 -3110 -7500 3110 -7500 7500 -3110 7500 7500 -7500 7500 ;
- STYLE 9 0 -10610 7500 -3110 7500 3110 3110 7500 -3110 7500 -10610 0 ;
END STYLES

NONDEFAULTRULES 1 ;
Parsed 250 number of lines!!
- DEFAULT
   + LAYER METAL1 WIDTH 10 DIAGWIDTH 8 SPACING 2 WIREEXT 1
   + LAYER M2 WIDTH 10 SPACING 2
   + LAYER M3 WIDTH 11 SPACING 3
   + VIA M1_M2
   + VIA M2_M3
   + VIARULE VIAGEN12
   + MINCUTS V1 2
   + PROPERTY strprop aString STRING
   + PROPERTY intprop 1 INTEGER
   + PROPERTY realprop 1.1 REAL
   + PROPERTY intrangeprop 25 INTEGER
   + PROPERTY realrangeprop 25.25 REAL
END NONDEFAULTRULES
- RULE2
   + HARDSPACING
   + LAYER METAL1 WIDTH 10 DIAGWIDTH 8 SPACING 2 WIREEXT 1
   + LAYER M2 WIDTH 10 SPACING 2
   + LAYER M3 WIDTH 11 SPACING 3
   + VIA M1_M2
   + VIA M2_M3
   + VIARULE VIAGEN12
   + MINCUTS V1 2
   + PROPERTY strprop aString STRING
   + PROPERTY intprop 1 INTEGER
   + PROPERTY realprop 1.1 REAL
   + PROPERTY intrangeprop 25 INTEGER
   + PROPERTY realrangeprop 25.25 REAL
END NONDEFAULTRULES

REGIONS 2 ;
- region1 -500 -500 300 100 
500 500 1000 1000 
+ TYPE FENCE
+ PROPERTY strprop aString STRING + PROPERTY intprop 1 INTEGER + PROPERTY realprop 1.1 REAL + PROPERTY intrangeprop 25 INTEGER + PROPERTY realrangeprop 25.25 REAL ;
- region2 4000 0 5000 1000 
+ TYPE GUIDE
;
END REGIONS
Parsed 300 number of lines!!

COMPONENTMASKSHIFT M3 M2 V1 M1 ;

COMPONENTS 13 ;
- I1 B + PLACED 100 100 N + SOURCE NETLIST + GENERATE generator + WEIGHT 100 + EEQMASTER A + REGION region1 + MASKSHIFT 1102
+ HALO SOFT 5 6 7 8
+ ROUTEHALO 100 METAL1 M3
+ PROPERTY strprop aString STRING + PROPERTY intprop 1 INTEGER + PROPERTY realprop 1.1 REAL + PROPERTY intrangeprop 25 INTEGER + PROPERTY realrangeprop 25.25 REAL ;
- I2 A + PLACED 200 200 S + SOURCE DIST + ROUTEHALO 100 M2 M3
;
- I3 A + PLACED 300 300 E + SOURCE USER ;
- I4 A + PLACED 400 400 W + SOURCE TIMING ;
- I5 A + PLACED 500 500 FN ;
Parsed 350 number of lines!!
- I6 A + PLACED 600 600 FS ;
- I7 A + PLACED 700 700 FE ;
- I8 A + PLACED 800 800 FW ;
- I9 A + FIXED 900 900 N ;
- I10 A + COVER 1000 1000 N ;
- I11 A + UNPLACED ;
- I12[0] A ;
- I12[1] A ;
END COMPONENTS
- I13[0][10] A ;
END COMPONENTS
- I14\[1\] A ;
END COMPONENTS
- vectormodule[1]/scalarname A ;
END COMPONENTS
- vectormodule[1]/vectorname[1] A ;
END COMPONENTS
- scancell1 CHK3A ;
END COMPONENTS
- scancell2 CHK3A ;
END COMPONENTS
- scancell3 CHK3A ;
END COMPONENTS
- scancell4 CHK3A ;
END COMPONENTS
- scancell5 CHK3A ;
END COMPONENTS
- scancell6 CHK3A ;
END COMPONENTS
- scancell7 CHK3A ;
END COMPONENTS
- scancell8 CHK3A ;
END COMPONENTS
- scancell9 CHK3A ;
END COMPONENTS
- scancell10 CHK3A ;
END COMPONENTS
- scancell11 CHK3A ;
END COMPONENTS
- scancell12 CHK3A ;
END COMPONENTS
- nobrackets A ;
END COMPONENTS
- somethingwith[1] A ;
END COMPONENTS
- more[]brackets A ;
END COMPONENTS
- more[1]brackets A ;
END COMPONENTS
- more\[1\]brackets A ;
END COMPONENTS
- more[1][2] A ;
END COMPONENTS
- more\[1\]\[2\] A ;
END COMPONENTS
- more\[2\] A ;
END COMPONENTS
- foo\[1\]\[2\]/haha\[3\]\[4\] A ;
END COMPONENTS
- foo[2][3]/haha[4][5] A ;
END COMPONENTS
- foo\[3\]\[4\]/haha[5][6] A ;
END COMPONENTS
- foo[4][5]/haha\[6\]\[7\] A ;
END COMPONENTS
- foo[5][6]bar/haha\[7\]\[8\] A ;
END COMPONENTS
- foo[6][7]bar/haha[8][9] A ;
END COMPONENTS
Parsed 400 number of lines!!

PINS 11 ;
Parsed 450 number of lines!!
- P0 + NET N0 + DIRECTION INPUT + USE SIGNAL + NETEXPR "power1 VDD" + SUPPLYSENSITIVITY P1 + GROUNDSENSITIVITY P2 
  + PORT
     + LAYER M2 MASK 2 0 0 30 135 
     + VIA VIAGEN12_0 ( 0 100 ) 
     + FIXED ( 45 -2160 ) N 
  + PORT
     + LAYER M1 0 0 30 135 
     + VIA M1_M2 MASK 023 ( 100 0 ) 
     + COVER ( 0 -1000 ) N 
  + PORT
     + LAYER M3 0 0 30 135 
     + PLACED ( 1000 -1000 ) N + SPECIAL ANTENNAPINPARTIALMETALAREA 5 LAYER METAL1
ANTENNAPINPARTIALMETALAREA 5 LAYER M2
ANTENNAPINPARTIALMETALSIDEAREA 10 LAYER METAL1
ANTENNAPINPARTIALMETALSIDEAREA 10 LAYER M2
ANTENNAPINDIFFAREA 20 LAYER M1
ANTENNAPINDIFFAREA 20 LAYER M2
ANTENNAPINPARTIALCUTAREA 35 LAYER V1
ANTENNAPINPARTIALCUTAREA 35 LAYER V2
ANTENNAMODEL OXIDE1
ANTENNAPINGATEAREA 15 LAYER M1
ANTENNAPINGATEAREA 15 LAYER M2
ANTENNAPINMAXAREACAR 25 LAYER M1
ANTENNAPINMAXSIDEAREACAR 30 LAYER M1
ANTENNAPINMAXCUTCAR 40 LAYER M1
ANTENNAMODEL OXIDE2
ANTENNAPINGATEAREA 115 LAYER M1
ANTENNAPINGATEAREA 115 LAYER M2
ANTENNAPINMAXAREACAR 125 LAYER M1
ANTENNAPINMAXSIDEAREACAR 130 LAYER M1
ANTENNAPINMAXCUTCAR 140 LAYER M1
ANTENNAMODEL OXIDE3
ANTENNAPINGATEAREA 115 LAYER M1
ANTENNAPINGATEAREA 115 LAYER M2
ANTENNAPINMAXAREACAR 125 LAYER M1
ANTENNAPINMAXSIDEAREACAR 130 LAYER M1
ANTENNAPINMAXCUTCAR 140 LAYER M1
ANTENNAMODEL OXIDE4
ANTENNAPINGATEAREA 115 LAYER M1
ANTENNAPINGATEAREA 115 LAYER M2
ANTENNAPINMAXAREACAR 125 LAYER M1
ANTENNAPINMAXSIDEAREACAR 130 LAYER M1
ANTENNAPINMAXCUTCAR 140 LAYER M1
;
- P1 + NET N1 + DIRECTION OUTPUT + USE POWER + NETEXPR "power1 VDD[1]" 
  + POLYGON M2 MASK 3 0 0 0 100 50 100 50 50 100 50 100 0 + PLACED ( 45 -2160 ) N ANTENNAPINPARTIALMETALAREA 5
ANTENNAPINPARTIALMETALSIDEAREA 10
ANTENNAPINDIFFAREA 20
ANTENNAPINPARTIALCUTAREA 35
ANTENNAMODEL OXIDE1
ANTENNAPINGATEAREA 15
;
- P2 + NET N2 + DIRECTION INOUT + USE GROUND 
  + LAYER M2 MASK 2 0 0 30 135 + COVER ( 45 -2160 ) N ;
- P2.extra1 + NET N2 + DIRECTION INOUT + USE GROUND 
  + LAYER METAL1 0 0 10 10 + COVER ( 0 0 ) N ;
- P3 + NET N3 + DIRECTION FEEDTHRU + USE CLOCK ;
- P4 + NET N4 + USE SIGNAL ;
- P5 + NET N5 + USE ANALOG ;
- P6 + NET N6 + USE SCAN ;
Parsed 500 number of lines!!
- P7 + NET N7 + USE RESET ;
- ARRAYPIN[0][10] + NET ARRAYNET[0][10] 
  + LAYER M2 0 0 30 135 ;
- ARRAYPIN.extra2[0][10] + NET ARRAYNET[0][10] 
  + LAYER M2 0 0 10 10 ;
END PINS
- scanpin + NET SCAN + USE SCAN ;
END PINS
- scanpin2 + NET SCAN + USE SCAN ;
END PINS
- INBUS[1] + NET INBUS<1> 
  + LAYER METAL1 0 0 10 10 ;
END PINS
- OUTBUS<1> + NET OUTBUS<1> ;
END PINS
- INBUS.extra1[1] + NET INBUS<1> 
  + LAYER M1 10 10 100 100 ;
END PINS
- vectorpin[0] + NET vectormodule[1]/vectornet[0] ;
END PINS
- scalarpin + NET vectormodule[1]/scalarnet ;
END PINS
- RE_RDY_2 + NET RE_RDY_2 + DIRECTION OUTPUT + USE SIGNAL 
  + PORT
     + VIA myvia1 MASK 123 ( 500 500 ) 
     + FIXED ( -390000 0 ) N 
  + PORT
     + POLYGON METAL1 MASK 22 ( 40000 40000 ) ( 80000 40000 ) ( 80000 -40000 ) ( 40000 -40000 ) ( 40000 -80000 ) ( -40000 -80000 ) ( -40000 -40000 ) ( -80000 -40000 ) ( -80000 40000 ) ( -40000 40000 ) ( -40000 80000 ) ( 40000 80000 ) 
     + FIXED ( -190000 0 ) N 
  + PORT
     + VIA myvia1 ( 100 100 ) 
     + FIXED ( 290000 0 ) N ;
END PINS

PINPROPERTIES 2 ;
- PIN P0 ;
  + PROPERTY strprop aString STRING   + PROPERTY intprop 1 INTEGER   + PROPERTY realprop 1.1 REAL   + PROPERTY intrangeprop 25 INTEGER   + PROPERTY realrangeprop 25.25 REAL ;
Parsed 550 number of lines!!
- I1 A ;
  + PROPERTY strprop aString STRING   + PROPERTY intprop 1 INTEGER   + PROPERTY realprop 1.1 REAL   + PROPERTY intrangeprop 25 INTEGER   + PROPERTY realrangeprop 25.25 REAL ;
END PINPROPERTIES

BLOCKAGES 8 ;
- LAYER METAL1
   + MASK 1
   RECT 60 70 80 90
;
- LAYER M2
   + COMPONENT I1
   + SLOTS
   + PUSHDOWN
   + EXCEPTPGNET
   + MASK 3
   POLYGON 100 100 100 200 150 200 150 150 200 150 200 100 
;
- LAYER M2
   + SLOTS
   + MASK 2
   RECT 10 20 40 50
;
- LAYER METAL1
   + FILLS
   + MASK 1
   RECT -10 20 30 40
;
- LAYER M1
   + PUSHDOWN
   + MASK 1
   + SPACING 3
   RECT 50 30 55 40
;
- LAYER M1
   + EXCEPTPGNET
   + MASK 1
   + DESIGNRULEWIDTH 45
   RECT 50 30 55 40
;
- PLACEMENT
   RECT -15 0 0 20
   RECT -15 20 30 40
   RECT 30 5 50 40
   RECT -10 -15 50 0
;
- PLACEMENT
   + PARTIAL 0.4
   + COMPONENT I1
   + PUSHDOWN
   RECT -10 0 0 20
   RECT -10 20 30 40
   RECT 30 0 50 40
   RECT -10 -5 50 0
;
END BLOCKAGES
- PLACEMENT
   + PUSHDOWN
   RECT -5 0 0 20
   RECT -5 20 30 40
   RECT 30 0 25 40
   RECT -5 0 50 10
;
END BLOCKAGES
Parsed 600 number of lines!!
- PLACEMENT
   + SOFT
   RECT 50 30 55 40
;
END BLOCKAGES
- PLACEMENT
   + PARTIAL 0.4
   RECT 50 30 55 40
;
END BLOCKAGES

SPECIALNETS 5 ;
- SN1 Parsed 650 number of lines!!
( I1 Z.extra1 ) ( I2 Z ) ( I3 Z ) ( * Z ) 
  + ROUTED 
M1 120 + SHAPE RING ( 14000 341440 ) ( 9600 341440 ) 
( 9600 282400 ) M1_M2 DO 2 BY 2 STEP 200 200 ( 2400 282400 ) NEW METAL1 
120 + SHAPE STRIPE ( 2400 282400 ) ( 240 282400 ) M1_M2 
NEW M1 120 + SHAPE FOLLOWPIN ( 2500 282400 ) ( 250 282400 ) 
VIAGEN12_0 N NEW M1 120 + SHAPE IOWIRE 
( 2600 282400 ) ( 260 282400 ) VIAGEN12_2 NEW METAL1 120 
+ SHAPE COREWIRE ( 2700 282400 ) ( 270 282400 ) VIAGEN12_3 NEW M1 
120 + SHAPE BLOCKWIRE ( 2800 282400 ) ( 280 282400 ) CUSTOMVIA 
VIAGEN12_1 NEW M1 120 + SHAPE FILLWIRE ( 2900 282400 ) 
( 290 282400 ) VIAGEN12_4 NEW M1 120 + SHAPE FILLWIREOPC 
( 2900 282400 ) VIAGEN12_4 NEW M1 120 + SHAPE BLOCKAGEWIRE 
( 2000 282400 ) ( 200 282400 ) VIAGEN12 NEW M1 120 
+ SHAPE BLOCKRING ( 2100 282400 ) ( 210 282400 ) NEW M1 120 
+ SHAPE PADRING ( 2200 282400 ) ( 220 282400 ) NEW M1 200 
( 3000 3000 ) TURNM1_1 NEW M2 200 ( 3100 3100 ) 
( 3200 3100 ) TURNM2_1 NEW M2 200 ( 3300 3300 ) 
( 3400 3300 ) TURNM2_1 ( 3400 3600 ) NEW M2 200 
( 400 400 ) M1_M2 ( 400 400 ) NEW M2 200 
( 500 500 ) M1_M2 ( 500 500 ) M1_M2 NEW M2 
200 ( 700 700 ) M1_M2 ( 700 700 ) ( 700 800 ) 
NEW M2 15000 + STYLE 9 ( 105000 105000 ) ( 50000 50000 ) 
NEW M2 15000 + STYLE 8 ( 105000 155000 ) ( 105000 105000 ) 

  + COVER METAL1 100 ( 100 100 ) ( 100 200 ) 

  + FIXED M1 100 ( 200 200 ) ( 300 200 ) 

  + ROUTED M1 120 + SHAPE DRCFILL ( 8000 8000 ) 
( 8000 8200 ) ( 8400 8200 ) 

  + SHIELD N1 M2 90 ( 14100 340440 ) ( 8160 340440 ) 
M1_M2 ( 8160 301600 ) M1_M2 FN DO 2 BY 2 STEP 200 200 
( 2400 301600 ) 
  + PROPERTY strprop aString STRING 
  + PROPERTY intprop 1 INTEGER 
  + PROPERTY realprop 1.1 REAL 
  + PROPERTY intrangeprop 25 INTEGER 
  + PROPERTY realrangeprop 25.25 REAL 

  + FIXEDBUMP 
  + VOLTAGE 3200 
  + WEIGHT 30 
  + SOURCE NETLIST 
  + PATTERN STEINER 
  + ORIGINAL VDD 
  + USE SIGNAL ;
- VDD Parsed 700 number of lines!!

  + ROUTED M1 20 ( 10 0 ) MASK 3 
( 10 20 ) VIAGEN12_4 NEW M2 100 ( 10 10 ) 
( 20 10 ) MASK 1 ( 20 20 ) MASK 031 VIAGEN12_3 

  + ROUTED M1 100 ( 0 0 100 ) ( 0 0 50 ) 
( 100 0 50 ) M1_M2 ( 100 100 50 ) 

  + ROUTED M1 50 + STYLE 0 ( 0 0 ) 
( 150 150 ) 

  + ROUTED M1 50 + STYLE 0 ( 150 150 ) 
( 0 0 ) 

  + ROUTED M1 50 + STYLE 0 ( 150 0 ) 
( 0 150 ) 

  + ROUTED M1 50 + STYLE 0 ( 0 150 ) 
( 150 0 ) 

  + ROUTED M1 50 + STYLE 1 ( 150 150 ) 
( 300 0 ) ( 400 0 ) 

  + ROUTED M2 100 + SHAPE RING + STYLE 0 
( 0 0 ) ( 100 100 ) ( 200 100 ) 

  + ROUTED M1 100 + STYLE 2 ( 0 0 ) 
M1_M2 ( 600 0 ) M1_M2 

  + ROUTED M1 50 ( 150 150 ) ( 300 300 ) 

  + FIXED 
  + SHAPE RING 
  + MASK 2 + POLYGON METAL1 0 0 0 100 100 100 200 200 200 0 
  + COVER 
  + SHAPE RING 
  + MASK 3 + POLYGON M2 100 100 100 200 200 200 300 300 300 100 
  + FIXED 
  + SHAPE RING 
  + RECT M3 0 0 10 10
  + SHIELD 
  + N1 
  + SHAPE BLOCKRING 
  + RECT M3 0 0 10 10
  + ROUTED 
  + VIA M1_M2  N 2400 0 10 10;

  + ROUTED 
  + SHAPE STRIPE 
  + VIA VIA12_2  N 30 30 40 40;

  + VOLTAGE 5000 ;
- SN2 
  + ROUTED M2 100 + STYLE 3 ( 0 0 ) 
( 150 150 ) ( 300 0 ) NEW M2 100 ( 300 0 ) 
( 400 0 ) 

  + ROUTED M1 100 ( 0 0 ) ( 150 150 ) 
( 300 0 ) ( 400 0 ) 

  + ROUTED M1 4000 + STYLE 5 ( 0 0 ) 
( 1000 0 ) 

  + ROUTED M1 4000 + STYLE 6 ( 0 0 ) 
( 1000 1000 ) 

  + ROUTED M1 1000 + STYLE 7 ( 0 0 ) 
( 0 0 ) 
;
- SN3 
  + ROUTED M2 100 ( 100 0 ) ( 100 3000 ) 
NEW M3 100 ( 0 1000 ) ( 3000 1000 ) 

  + SHIELD N1 M2 40 + SHAPE FILLWIRE ( 300 80 ) 
( 300 1920 ) NEW M2 40 + SHAPE FILLWIRE ( 500 80 ) 
( 500 1920 ) 

  + USE GROUND ;
- DUMMY 
  + ROUTED M1 100 + SHAPE FILLWIRE ( 0 0 ) 
( 100 0 ) 
;
END SPECIALNETS
- DUMMY2 
  + ROUTED M2 100 + SHAPE FILLWIREOPC ( 0 0 ) 
( 100 0 ) 
;
END SPECIALNETS
Parsed 750 number of lines!!

NETS 6 ;
- SCAN ( scancell1 PA10 ) + SYNTHESIZED ( scancell2 PA2 ) + SYNTHESIZED + SOURCE TEST ;
- N1    + SUBNET CBK N1_SUB0 Parsed 800 number of lines!!
   + NONDEFAULTRULE CBK RULE1 ( I1 A ) ( PIN P0 ) + NONDEFAULTRULE RULE1
  + N1_VP0 M3 -333 -333 333 333 P 189560 27300 N
  + N1_VP1 M3 -333 -333 333 333 P 189560 27300 S
  + N1_VP2 M3 -333 -333 333 333 P 189560 27300 E
  + N1_VP3 M3 -333 -333 333 333 P 189560 27300 W
  + N1_VP4 M3 -333 -333 333 333 P 189560 27300 FN
  + N1_VP5 M3 -333 -333 333 333 P 189560 27300 FS
  + N1_VP6 M3 -333 -333 333 333 P 189560 27300 FE
  + N1_VP7 M3 -333 -333 333 333 P 189560 27300 FW
  + N1_VP8 -333 -333 333 333

  + FIXED M3 ( 10 0 ) MASK 3 ( 10 20 ) 
MASK 031 M1_M2 

  + ROUTED M1 ( 0 0 ) ( 5 0 ) VIRTUAL ( 2 3 ) 
MASK 1 ( 7 7 ) 

  + ROUTED M1 ( 0 0 ) ( 5 0 ) VIRTUAL ( 2 3 ) 
RECT ( 1 2 3 4 ) ( 7 7 ) 

  + FIXED M1 ( 0 0 ) ( 5 0 ) ( 7 7 ) 

  + FIXED M1 ( 0 0 ) ( 5 0 ) MASK 3 
RECT ( 1 2 3 4 ) ( 7 7 ) 

  + NOSHIELD M2 ( 14100 341440 ) ( 14000 341440 ) M1_M2 

  + ROUTED M2 ( 14000 341440 ) ( 9600 341440 ) ( 9600 282400 ) 
nd1VIA12 ( 2400 282400 ) TURNM1_1 NEW M1 TAPER 
( 2400 282400 ) ( 240 282400 ) 

  + SHIELDNET SN1
  + SHIELDNET VDD
  + SUBNET N1_SUB0  ( I2 A )
 ( PIN P1 )
 ( VPIN N1_VP9 )
  ROUTED M1 ( 168280 63300 700 ) ( 168280 64500 ) M1_M2 
( 169400 64500 800 ) M2_M3   + PROPERTY strprop aString STRING 
  + PROPERTY intprop 1 INTEGER 
  + PROPERTY realprop 1.1 REAL 
  + PROPERTY intrangeprop 25 INTEGER 
  + PROPERTY realrangeprop 25.25 REAL 
+ WEIGHT 100 + ESTCAP 1.5e+06 + SOURCE NETLIST + FIXEDBUMP + FREQUENCY 100 + PATTERN STEINER + ORIGINAL N2 + USE SIGNAL ;
- N2 ( I3 A ) ( PIN P2 ) 
  + FIXED M2 ( 14000 341440 ) ( 9600 341440 ) ( 9600 282400 ) 
M1_M2 ( 2400 282400 ) NEW M1 TAPERRULE RULE1 ( 2400 282400 ) 
( 240 282400 ) 
+ WEIGHT 500 + SOURCE DIST + PATTERN BALANCED ;
- N3 ( I4 A ) ( PIN P3 ) 
  + COVER M2 ( 14000 341440 ) ( 9600 341440 ) ( 9600 282400 ) 
M1_M2 ( 2400 282400 ) VIAGEN12_0 N NEW M1 
( 2400 282400 ) ( 240 282400 ) NEW M2 ( 400 400 ) M1_M2 
N ( 400 400 ) NEW M2 ( 500 500 ) M1_M2 
( 500 500 ) M1_M2 NEW M2 ( 600 600 10 ) M1_M2 
S ( 600 600 30 ) ( 600 800 ) NEW M2 ( 700 700 ) 
M1_M2 ( 700 700 ) ( 700 800 ) NEW M1 ( 0 0 ) 
M1_M2 FS M2_M3 NEW M3 ( 0 0 ) 
M2_M3 W M1_M2 NEW M1 ( 10 10 ) 
( 20 10 ) MASK 1 ( 20 20 ) MASK 031 VIA1_2 
+ SOURCE USER + PATTERN TRUNK ;
- N4 ( I5 A ) ( PIN P4 ) 
  + ROUTED M2 STYLE 1 ( 0 0 ) ( 150 150 ) 
( 300 0 ) ( 400 0 ) 

  + ROUTED M1 ( 150 150 ) MASK 3 ( 300 300 ) 
MASK 032 VIAGEN12 

  + NOSHIELD M1 ( 150 150 30 ) ( 150 300 30 ) 

  + ROUTED M1 STYLE 0 ( 0 0 ) ( 150 150 ) 
NEW M1 STYLE 1 ( 150 150 ) MASK 2 ( 300 0 ) 
( 400 0 ) 
+ SOURCE TEST + USE GROUND ;
- N5 ( I6 A ) ( PIN P5 ) 
  + ROUTED M2 STYLE 3 ( 0 1000 ) ( 150 1150 ) 
( 300 1000 ) ( 400 1000 ) 

  + ROUTED M1 ( 0 1000 ) ( 150 1150 ) ( 300 1000 ) 
( 400 1000 ) 
+ SOURCE TIMING ;
END NETS
Parsed 850 number of lines!!
- N6    + NONDEFAULTRULE CBK RULE2 + NONDEFAULTRULE RULE2

  + ROUTED M1 STYLE 4 ( 1000 0 ) ( 1100 100 ) 

  + ROUTED M1 STYLE 4 ( 1200 100 ) ( 1300 0 ) 

  + ROUTED M1 STYLE 4 ( 1000 -100 ) ( 1300 -100 ) 
;
END NETS
- SCAN ( scancell1 PA10 ) + SYNTHESIZED ( scancell2 PA2 ) + SYNTHESIZED + SOURCE TEST ;
END NETS
- MUSTJOIN_1 ( I7 A ) ;
END NETS
- ARRAYNET[0][10] ;
END NETS
- vectormodule[1]/vectornet[0] ;
END NETS
- vectormodule[1]/scalarnet ;
END NETS

SCANCHAINS 2 ;
- chain1
  + START I1 B
  + STOP I4 B
  + COMMONSCANPINS  ( IN PA1 )  ( OUT PA2 ) 
  + FLOATING
    scancell3 ( IN PA2 ) 
    scancell4 ( OUT PA10 ) ( BITS 4 ) 
  + ORDERED
    scancell1 ( IN PA2 ) 
    scancell2 ( OUT PA10 ) ( BITS 4 ) 
  + PARTITION clock1 MAXBITS 256 ;
Parsed 900 number of lines!!
- chain2
  + START PIN scanpin
  + STOP PIN scanpin2
  + COMMONSCANPINS  ( IN PA1 )  ( OUT PA2 ) 
  + FLOATING
    scancell7 ( IN PA2 ) 
    scancell8 ( OUT PA10 ) ( BITS 4 ) 
  + ORDERED
    scancell5 ( IN PA2 ) 
    scancell6 ( OUT PA10 ) ( BITS 4 ) 
  + PARTITION clock1 MAXBITS 256 ;
END SCANCHAINS
- chain3
  + START I5 B
  + STOP I6 B
  + COMMONSCANPINS  ( IN PA1 )  ( OUT PA2 ) 
  + FLOATING
    scancell11 ( IN PA2 ) 
    scancell12 ( OUT PA10 ) ( BITS 4 ) 
  + ORDERED
    scancell9 ( IN PA2 ) 
    scancell10 ( OUT PA10 ) ( BITS 4 ) 
  + PARTITION clock1 MAXBITS 256 ;
END SCANCHAINS

GROUPS 3 ;
- group1 I3 I2
  + REGION region1 
  + PROPERTY strprop aString STRING 
  + PROPERTY intprop 1 INTEGER 
  + PROPERTY realprop 1.1 REAL 
  + PROPERTY intrangeprop 25 INTEGER 
  + PROPERTY realrangeprop 25.25 REAL  ;
- group2 I4 ;
- region2 I7 I8
  + REGION region2  ;
END GROUPS
Parsed 950 number of lines!!

SLOTS 3 ;
- LAYER M1
   RECT 3 3 6 8
;
- LAYER M2
   RECT 3 3 6 8
   POLYGON 0 0 0 10 10 10 10 20 20 20 20 0 ;
;
- LAYER M3
   RECT 3 3 6 8
;
END SLOTS

FILLS 5 ;
- VIA myvia1 + MASK 002 + OPC
 5000 5000 800 800;
;
- LAYER M1 + MASK 2
   RECT 0 2 1 10
;
- LAYER M2 + OPC
   RECT 0 2 1 10
   POLYGON 0 0 0 10 10 10 10 20 20 20 20 0 ;
;
- LAYER M3
   RECT 0 2 1 10
;
- VIA M1_M2 + MASK 202 + OPC
 2400 0 10 10;
;
END FILLS
- VIA VIAGEN12_0 + OPC
 100 100 200 100;
;
END FILLS
Parsed 1000 number of lines!!
BEGINEXT  "tag"
- CREATOR "Cadence" ;
- OTTER furry
  + PROPERTY arrg later
  ;
- SEAL cousin to WALRUS ;
ENDEXT
END DESIGN
