cell : grmx4_c
One out of four pass transistor output multiplexer.
This cell is placed just below the rom precharged bit lines.
One of the four lines is selected, depending on the data given as input.
The line bl_p[i] is selected when the s[i] line is high.
