ENTITY rf_inmux_mem IS
PORT (
  datain0   : in  BIT;
  datain1   : in  BIT;
  sel0      : in  BIT;
  sel1      : in  BIT;
  dinx      : out BIT;
  vdd	    : in  BIT;
  vss	    : in  BIT
);
END rf_inmux_mem;

ARCHITECTURE VBE OF rf_inmux_mem IS

BEGIN
  ASSERT (vdd and not (vss))
  REPORT "power supply is missing on sff1_x4"
  SEVERITY WARNING;

  dinx <= (sel0 and datain0) or (sel1 and datain1);

END;
