ENTITY dp_sff_scan_x4 IS
PORT (
  ckx		: in  BIT;
  nckx		: in  BIT;
  wenx		: in  BIT;
  nwenx		: in  BIT;
  scanx		: in  BIT;
  nscanx	: in  BIT;
  i   		: in  BIT;
  scin		: in  BIT;
  q		: out BIT;
  vdd		: in  BIT;
  vss		: in  BIT
);
END dp_sff_scan_x4;

ARCHITECTURE vbe OF dp_sff_scan_x4 IS
  SIGNAL ff : REG_BIT REGISTER;

BEGIN
  ASSERT (vdd and not (vss))
  REPORT "power supply is missing on dp_sff_scan_x4"
  SEVERITY WARNING;

  ASSERT (ckx xor nckx)
  REPORT "wrong values for ckx and nckx in dp_sff_scan_x4"
  SEVERITY WARNING;

  ASSERT (wenx xor nwenx)
  REPORT "wrong values for wenx and nwenx in dp_sff_scan_x4"
  SEVERITY WARNING;

  ASSERT (scanx xor nscanx)
  REPORT "wrong values for scanx and nscanx in dp_sff_scan_x4"
  SEVERITY WARNING;

  label0 : BLOCK ((ckx and not (ckx'STABLE)) = '1')
  BEGIN
    ff <= GUARDED ((scanx and scin) or (nscanx and ((wenx and i) or (nwenx and ff))));
  END BLOCK label0;

  q <= ff;
END;
