DP_BUFF(3)

NAME
DP_BUFF - inverter

SYNOPSYS
#include  <fpgen.h>
void  DP_BUFF(
    char *InstName,  /*         Instance name         */
    long  Width   ,  /*        Number of slices       */
    long  Slice   ,  /*   Index of the bottom slice   */
    long  Drive   ,  /*  Fanout : among 1, 2 or 3     */
    char *BusI0   ,  /* IN     Input Operand     DATA */
    char *BusO    ,  /* OUT    Result output     DATA */
               EOL);

DESCRIPTION
    DP_BUFF creates a buffer of Width bits and then instanciates it with the name InstName. The maximal authorized value for Width is the full width of the current data-path, set by the previous call to the function DP_DEFLOFIG. In the layout the leaf cells are placed on the slices numbered from Slice to Slice+Width-1 (the bottom slice is 0).

CHARACTERISTICS
Operator wide	:	drive = 1	-->	18 lambdas.
		drive = 2	-->	24 lambdas.
		drive = 3	-->	36 lambdas.

EXAMPLE
    DP_BUFF( "inv_instance0", 32,
                               0, 1, "input_i0[3:0]",
                                     "output_o[3:0]", EOL);

SEE ALSO
fpgen(1), dpr(1), genlib(1), mbk(1), DP_DEFLOFIG(3), DP_SAVLOFIG(3), DP_LOCON(3), DP_IMPORT(3), DP_INV(3), DP_BUSE(3), DP_AND2(3), DP_NAND2(3), DP_AND3(3), DP_NAND3(3), DP_OR2(3), DP_NOR2(3), DP_OR3(3), DP_NOR3(3), DP_XOR2(3), DP_XNOR2(3), DP_NAND2MASK(3), DP_NOR2MASK(3), DP_XNOR2MASK(3), DP_CONST(3), DP_NMUX2CS(3), DP_MUX2CS(3), DP_MUX3CS(3), DP_MUX4CS(3), DP_MUX5CS(3), DP_BUSE(3), DP_NBUSE(3), DP_ADD2F(3), DP_ADSB2F(3), DP_SHIFT(3), DP_MULT(3), DP_MULTP(3), DP_NUL(3), DP_PDFF(3), DP_PDFFR(3), DP_PDFFT(3), DP_PDFFRT(3), DP_RFG1C0(3), DP_RFG1CC(3), DP_RFG2C0(3), DP_RFG2CC(3) ,