VERSION 5.7 ;
   NAMESCASESENSITIVE ON ;
   DIVIDERCHAR "/" ;
   BUSBITCHARS "()" ;
   DESIGN chip_io_alt ;
   TECHNOLOGY sky130A ;
   UNITS DISTANCE MICRONS 1000 ;
   DIEAREA ( 0 0 ) ( 3588000 5188000 ) ;

VIAS 29 ;
   - via4_11630_22770
      + RECT met4 ( -5815 -11385 ) ( 5815 11385 )
      + RECT met5 ( -5935 -11505 ) ( 5935 11505 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via3_11890_22760_hx
      + RECT met3 ( -5975 -11380 ) ( 5975 11380 )
      + RECT met4 ( -5950 -11385 ) ( 5950 11385 )
      + RECT via3 ( -5700 -11300 ) ( -5500 -11100 )
      + RECT via3 ( -5300 -11300 ) ( -5100 -11100 )
      + RECT via3 ( -4900 -11300 ) ( -4700 -11100 )
      + RECT via3 ( -4500 -11300 ) ( -4300 -11100 )
      + RECT via3 ( -4100 -11300 ) ( -3900 -11100 )
      + RECT via3 ( -3700 -11300 ) ( -3500 -11100 )
      + RECT via3 ( -3300 -11300 ) ( -3100 -11100 )
      + RECT via3 ( -2900 -11300 ) ( -2700 -11100 )
      + RECT via3 ( -2500 -11300 ) ( -2300 -11100 )
      + RECT via3 ( -2100 -11300 ) ( -1900 -11100 )
      + RECT via3 ( -1700 -11300 ) ( -1500 -11100 )
      + RECT via3 ( -1300 -11300 ) ( -1100 -11100 )
      + RECT via3 ( -900 -11300 ) ( -700 -11100 )
      + RECT via3 ( -500 -11300 ) ( -300 -11100 )
      + RECT via3 ( -100 -11300 ) ( 100 -11100 )
      + RECT via3 ( 300 -11300 ) ( 500 -11100 )
      + RECT via3 ( 700 -11300 ) ( 900 -11100 )
      + RECT via3 ( 1100 -11300 ) ( 1300 -11100 )
      + RECT via3 ( 1500 -11300 ) ( 1700 -11100 )
      + RECT via3 ( 1900 -11300 ) ( 2100 -11100 )
      + RECT via3 ( 2300 -11300 ) ( 2500 -11100 )
      + RECT via3 ( 2700 -11300 ) ( 2900 -11100 )
      + RECT via3 ( 3100 -11300 ) ( 3300 -11100 )
      + RECT via3 ( 3500 -11300 ) ( 3700 -11100 )
      + RECT via3 ( 3900 -11300 ) ( 4100 -11100 )
      + RECT via3 ( 4300 -11300 ) ( 4500 -11100 )
      + RECT via3 ( 4700 -11300 ) ( 4900 -11100 )
      + RECT via3 ( 5100 -11300 ) ( 5300 -11100 )
      + RECT via3 ( 5500 -11300 ) ( 5700 -11100 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 )
      + RECT via3 ( -5700 11100 ) ( -5500 11300 )
      + RECT via3 ( -5300 11100 ) ( -5100 11300 )
      + RECT via3 ( -4900 11100 ) ( -4700 11300 )
      + RECT via3 ( -4500 11100 ) ( -4300 11300 )
      + RECT via3 ( -4100 11100 ) ( -3900 11300 )
      + RECT via3 ( -3700 11100 ) ( -3500 11300 )
      + RECT via3 ( -3300 11100 ) ( -3100 11300 )
      + RECT via3 ( -2900 11100 ) ( -2700 11300 )
      + RECT via3 ( -2500 11100 ) ( -2300 11300 )
      + RECT via3 ( -2100 11100 ) ( -1900 11300 )
      + RECT via3 ( -1700 11100 ) ( -1500 11300 )
      + RECT via3 ( -1300 11100 ) ( -1100 11300 )
      + RECT via3 ( -900 11100 ) ( -700 11300 )
      + RECT via3 ( -500 11100 ) ( -300 11300 )
      + RECT via3 ( -100 11100 ) ( 100 11300 )
      + RECT via3 ( 300 11100 ) ( 500 11300 )
      + RECT via3 ( 700 11100 ) ( 900 11300 )
      + RECT via3 ( 1100 11100 ) ( 1300 11300 )
      + RECT via3 ( 1500 11100 ) ( 1700 11300 )
      + RECT via3 ( 1900 11100 ) ( 2100 11300 )
      + RECT via3 ( 2300 11100 ) ( 2500 11300 )
      + RECT via3 ( 2700 11100 ) ( 2900 11300 )
      + RECT via3 ( 3100 11100 ) ( 3300 11300 )
      + RECT via3 ( 3500 11100 ) ( 3700 11300 )
      + RECT via3 ( 3900 11100 ) ( 4100 11300 )
      + RECT via3 ( 4300 11100 ) ( 4500 11300 )
      + RECT via3 ( 4700 11100 ) ( 4900 11300 )
      + RECT via3 ( 5100 11100 ) ( 5300 11300 )
      + RECT via3 ( 5500 11100 ) ( 5700 11300 ) ;
   - via4_11790_23020
      + RECT met4 ( -5895 -11510 ) ( 5895 11510 )
      + RECT met5 ( -6015 -11630 ) ( 6015 11630 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via3_1825_3785_hx
      + RECT met3 ( -942.5 -1892.5 ) ( 942.5 1892.5 )
      + RECT met4 ( -917.5 -1897.5 ) ( 917.5 1897.5 )
      + RECT via3 ( -700 -1700 ) ( -500 -1500 )
      + RECT via3 ( -300 -1700 ) ( -100 -1500 )
      + RECT via3 ( 100 -1700 ) ( 300 -1500 )
      + RECT via3 ( 500 -1700 ) ( 700 -1500 )
      + RECT via3 ( -700 -1300 ) ( -500 -1100 )
      + RECT via3 ( -300 -1300 ) ( -100 -1100 )
      + RECT via3 ( 100 -1300 ) ( 300 -1100 )
      + RECT via3 ( 500 -1300 ) ( 700 -1100 )
      + RECT via3 ( -700 -900 ) ( -500 -700 )
      + RECT via3 ( -300 -900 ) ( -100 -700 )
      + RECT via3 ( 100 -900 ) ( 300 -700 )
      + RECT via3 ( 500 -900 ) ( 700 -700 )
      + RECT via3 ( -700 -500 ) ( -500 -300 )
      + RECT via3 ( -300 -500 ) ( -100 -300 )
      + RECT via3 ( 100 -500 ) ( 300 -300 )
      + RECT via3 ( 500 -500 ) ( 700 -300 )
      + RECT via3 ( -700 -100 ) ( -500 100 )
      + RECT via3 ( -300 -100 ) ( -100 100 )
      + RECT via3 ( 100 -100 ) ( 300 100 )
      + RECT via3 ( 500 -100 ) ( 700 100 )
      + RECT via3 ( -700 300 ) ( -500 500 )
      + RECT via3 ( -300 300 ) ( -100 500 )
      + RECT via3 ( 100 300 ) ( 300 500 )
      + RECT via3 ( 500 300 ) ( 700 500 )
      + RECT via3 ( -700 700 ) ( -500 900 )
      + RECT via3 ( -300 700 ) ( -100 900 )
      + RECT via3 ( 100 700 ) ( 300 900 )
      + RECT via3 ( 500 700 ) ( 700 900 )
      + RECT via3 ( -700 1100 ) ( -500 1300 )
      + RECT via3 ( -300 1100 ) ( -100 1300 )
      + RECT via3 ( 100 1100 ) ( 300 1300 )
      + RECT via3 ( 500 1100 ) ( 700 1300 )
      + RECT via3 ( -700 1500 ) ( -500 1700 )
      + RECT via3 ( -300 1500 ) ( -100 1700 )
      + RECT via3 ( 100 1500 ) ( 300 1700 )
      + RECT via3 ( 500 1500 ) ( 700 1700 ) ;
   - via3_1640_3905_hx
      + RECT met3 ( -850 -1952.5 ) ( 850 1952.5 )
      + RECT met4 ( -825 -1957.5 ) ( 825 1957.5 )
      + RECT via3 ( -700 -1700 ) ( -500 -1500 )
      + RECT via3 ( -300 -1700 ) ( -100 -1500 )
      + RECT via3 ( 100 -1700 ) ( 300 -1500 )
      + RECT via3 ( 500 -1700 ) ( 700 -1500 )
      + RECT via3 ( -700 -1300 ) ( -500 -1100 )
      + RECT via3 ( -300 -1300 ) ( -100 -1100 )
      + RECT via3 ( 100 -1300 ) ( 300 -1100 )
      + RECT via3 ( 500 -1300 ) ( 700 -1100 )
      + RECT via3 ( -700 -900 ) ( -500 -700 )
      + RECT via3 ( -300 -900 ) ( -100 -700 )
      + RECT via3 ( 100 -900 ) ( 300 -700 )
      + RECT via3 ( 500 -900 ) ( 700 -700 )
      + RECT via3 ( -700 -500 ) ( -500 -300 )
      + RECT via3 ( -300 -500 ) ( -100 -300 )
      + RECT via3 ( 100 -500 ) ( 300 -300 )
      + RECT via3 ( 500 -500 ) ( 700 -300 )
      + RECT via3 ( -700 -100 ) ( -500 100 )
      + RECT via3 ( -300 -100 ) ( -100 100 )
      + RECT via3 ( 100 -100 ) ( 300 100 )
      + RECT via3 ( 500 -100 ) ( 700 100 )
      + RECT via3 ( -700 300 ) ( -500 500 )
      + RECT via3 ( -300 300 ) ( -100 500 )
      + RECT via3 ( 100 300 ) ( 300 500 )
      + RECT via3 ( 500 300 ) ( 700 500 )
      + RECT via3 ( -700 700 ) ( -500 900 )
      + RECT via3 ( -300 700 ) ( -100 900 )
      + RECT via3 ( 100 700 ) ( 300 900 )
      + RECT via3 ( 500 700 ) ( 700 900 )
      + RECT via3 ( -700 1100 ) ( -500 1300 )
      + RECT via3 ( -300 1100 ) ( -100 1300 )
      + RECT via3 ( 100 1100 ) ( 300 1300 )
      + RECT via3 ( 500 1100 ) ( 700 1300 )
      + RECT via3 ( -700 1500 ) ( -500 1700 )
      + RECT via3 ( -300 1500 ) ( -100 1700 )
      + RECT via3 ( 100 1500 ) ( 300 1700 )
      + RECT via3 ( 500 1500 ) ( 700 1700 ) ;
   - via_260_260_hv
      + RECT met1 ( -160 -130 ) ( 160 130 )
      + RECT met2 ( -130 -160 ) ( 130 160 )
      + RECT via ( -75 -75 ) ( 75 75 ) ;
   - via2_300_300_hx
      + RECT met2 ( -195 -150 ) ( 195 150 )
      + RECT met3 ( -175 -175 ) ( 175 175 )
      + RECT via2 ( -100 -100 ) ( 100 100 ) ;
   - via4_11820_22030
      + RECT met4 ( -5910 -11015 ) ( 5910 11015 )
      + RECT met5 ( -6030 -11135 ) ( 6030 11135 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via_560_260_hv
      + RECT met1 ( -310 -130 ) ( 310 130 )
      + RECT met2 ( -280 -160 ) ( 280 160 )
      + RECT via ( -75 -75 ) ( 75 75 ) ;
   - via4_11850_22100
      + RECT met4 ( -5925 -11050 ) ( 5925 11050 )
      + RECT met5 ( -6045 -11170 ) ( 6045 11170 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via_860_260_hv
      + RECT met1 ( -460 -130 ) ( 460 130 )
      + RECT met2 ( -430 -160 ) ( 430 160 )
      + RECT via ( -235 -75 ) ( -85 75 )
      + RECT via ( 85 -75 ) ( 235 75 ) ;
   - via3_11630_22770_hx
      + RECT met3 ( -5845 -11385 ) ( 5845 11385 )
      + RECT met4 ( -5820 -11390 ) ( 5820 11390 )
      + RECT via3 ( -5700 -11300 ) ( -5500 -11100 )
      + RECT via3 ( -5300 -11300 ) ( -5100 -11100 )
      + RECT via3 ( -4900 -11300 ) ( -4700 -11100 )
      + RECT via3 ( -4500 -11300 ) ( -4300 -11100 )
      + RECT via3 ( -4100 -11300 ) ( -3900 -11100 )
      + RECT via3 ( -3700 -11300 ) ( -3500 -11100 )
      + RECT via3 ( -3300 -11300 ) ( -3100 -11100 )
      + RECT via3 ( -2900 -11300 ) ( -2700 -11100 )
      + RECT via3 ( -2500 -11300 ) ( -2300 -11100 )
      + RECT via3 ( -2100 -11300 ) ( -1900 -11100 )
      + RECT via3 ( -1700 -11300 ) ( -1500 -11100 )
      + RECT via3 ( -1300 -11300 ) ( -1100 -11100 )
      + RECT via3 ( -900 -11300 ) ( -700 -11100 )
      + RECT via3 ( -500 -11300 ) ( -300 -11100 )
      + RECT via3 ( -100 -11300 ) ( 100 -11100 )
      + RECT via3 ( 300 -11300 ) ( 500 -11100 )
      + RECT via3 ( 700 -11300 ) ( 900 -11100 )
      + RECT via3 ( 1100 -11300 ) ( 1300 -11100 )
      + RECT via3 ( 1500 -11300 ) ( 1700 -11100 )
      + RECT via3 ( 1900 -11300 ) ( 2100 -11100 )
      + RECT via3 ( 2300 -11300 ) ( 2500 -11100 )
      + RECT via3 ( 2700 -11300 ) ( 2900 -11100 )
      + RECT via3 ( 3100 -11300 ) ( 3300 -11100 )
      + RECT via3 ( 3500 -11300 ) ( 3700 -11100 )
      + RECT via3 ( 3900 -11300 ) ( 4100 -11100 )
      + RECT via3 ( 4300 -11300 ) ( 4500 -11100 )
      + RECT via3 ( 4700 -11300 ) ( 4900 -11100 )
      + RECT via3 ( 5100 -11300 ) ( 5300 -11100 )
      + RECT via3 ( 5500 -11300 ) ( 5700 -11100 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 )
      + RECT via3 ( -5700 11100 ) ( -5500 11300 )
      + RECT via3 ( -5300 11100 ) ( -5100 11300 )
      + RECT via3 ( -4900 11100 ) ( -4700 11300 )
      + RECT via3 ( -4500 11100 ) ( -4300 11300 )
      + RECT via3 ( -4100 11100 ) ( -3900 11300 )
      + RECT via3 ( -3700 11100 ) ( -3500 11300 )
      + RECT via3 ( -3300 11100 ) ( -3100 11300 )
      + RECT via3 ( -2900 11100 ) ( -2700 11300 )
      + RECT via3 ( -2500 11100 ) ( -2300 11300 )
      + RECT via3 ( -2100 11100 ) ( -1900 11300 )
      + RECT via3 ( -1700 11100 ) ( -1500 11300 )
      + RECT via3 ( -1300 11100 ) ( -1100 11300 )
      + RECT via3 ( -900 11100 ) ( -700 11300 )
      + RECT via3 ( -500 11100 ) ( -300 11300 )
      + RECT via3 ( -100 11100 ) ( 100 11300 )
      + RECT via3 ( 300 11100 ) ( 500 11300 )
      + RECT via3 ( 700 11100 ) ( 900 11300 )
      + RECT via3 ( 1100 11100 ) ( 1300 11300 )
      + RECT via3 ( 1500 11100 ) ( 1700 11300 )
      + RECT via3 ( 1900 11100 ) ( 2100 11300 )
      + RECT via3 ( 2300 11100 ) ( 2500 11300 )
      + RECT via3 ( 2700 11100 ) ( 2900 11300 )
      + RECT via3 ( 3100 11100 ) ( 3300 11300 )
      + RECT via3 ( 3500 11100 ) ( 3700 11300 )
      + RECT via3 ( 3900 11100 ) ( 4100 11300 )
      + RECT via3 ( 4300 11100 ) ( 4500 11300 )
      + RECT via3 ( 4700 11100 ) ( 4900 11300 )
      + RECT via3 ( 5100 11100 ) ( 5300 11300 )
      + RECT via3 ( 5500 11100 ) ( 5700 11300 ) ;
   - via_260_260_vh
      + RECT met1 ( -130 -160 ) ( 130 160 )
      + RECT met2 ( -160 -130 ) ( 160 130 )
      + RECT via ( -75 -75 ) ( 75 75 ) ;
   - via3_11790_23020_hx
      + RECT met3 ( -5925 -11510 ) ( 5925 11510 )
      + RECT met4 ( -5900 -11515 ) ( 5900 11515 )
      + RECT via3 ( -5700 -11300 ) ( -5500 -11100 )
      + RECT via3 ( -5300 -11300 ) ( -5100 -11100 )
      + RECT via3 ( -4900 -11300 ) ( -4700 -11100 )
      + RECT via3 ( -4500 -11300 ) ( -4300 -11100 )
      + RECT via3 ( -4100 -11300 ) ( -3900 -11100 )
      + RECT via3 ( -3700 -11300 ) ( -3500 -11100 )
      + RECT via3 ( -3300 -11300 ) ( -3100 -11100 )
      + RECT via3 ( -2900 -11300 ) ( -2700 -11100 )
      + RECT via3 ( -2500 -11300 ) ( -2300 -11100 )
      + RECT via3 ( -2100 -11300 ) ( -1900 -11100 )
      + RECT via3 ( -1700 -11300 ) ( -1500 -11100 )
      + RECT via3 ( -1300 -11300 ) ( -1100 -11100 )
      + RECT via3 ( -900 -11300 ) ( -700 -11100 )
      + RECT via3 ( -500 -11300 ) ( -300 -11100 )
      + RECT via3 ( -100 -11300 ) ( 100 -11100 )
      + RECT via3 ( 300 -11300 ) ( 500 -11100 )
      + RECT via3 ( 700 -11300 ) ( 900 -11100 )
      + RECT via3 ( 1100 -11300 ) ( 1300 -11100 )
      + RECT via3 ( 1500 -11300 ) ( 1700 -11100 )
      + RECT via3 ( 1900 -11300 ) ( 2100 -11100 )
      + RECT via3 ( 2300 -11300 ) ( 2500 -11100 )
      + RECT via3 ( 2700 -11300 ) ( 2900 -11100 )
      + RECT via3 ( 3100 -11300 ) ( 3300 -11100 )
      + RECT via3 ( 3500 -11300 ) ( 3700 -11100 )
      + RECT via3 ( 3900 -11300 ) ( 4100 -11100 )
      + RECT via3 ( 4300 -11300 ) ( 4500 -11100 )
      + RECT via3 ( 4700 -11300 ) ( 4900 -11100 )
      + RECT via3 ( 5100 -11300 ) ( 5300 -11100 )
      + RECT via3 ( 5500 -11300 ) ( 5700 -11100 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 )
      + RECT via3 ( -5700 11100 ) ( -5500 11300 )
      + RECT via3 ( -5300 11100 ) ( -5100 11300 )
      + RECT via3 ( -4900 11100 ) ( -4700 11300 )
      + RECT via3 ( -4500 11100 ) ( -4300 11300 )
      + RECT via3 ( -4100 11100 ) ( -3900 11300 )
      + RECT via3 ( -3700 11100 ) ( -3500 11300 )
      + RECT via3 ( -3300 11100 ) ( -3100 11300 )
      + RECT via3 ( -2900 11100 ) ( -2700 11300 )
      + RECT via3 ( -2500 11100 ) ( -2300 11300 )
      + RECT via3 ( -2100 11100 ) ( -1900 11300 )
      + RECT via3 ( -1700 11100 ) ( -1500 11300 )
      + RECT via3 ( -1300 11100 ) ( -1100 11300 )
      + RECT via3 ( -900 11100 ) ( -700 11300 )
      + RECT via3 ( -500 11100 ) ( -300 11300 )
      + RECT via3 ( -100 11100 ) ( 100 11300 )
      + RECT via3 ( 300 11100 ) ( 500 11300 )
      + RECT via3 ( 700 11100 ) ( 900 11300 )
      + RECT via3 ( 1100 11100 ) ( 1300 11300 )
      + RECT via3 ( 1500 11100 ) ( 1700 11300 )
      + RECT via3 ( 1900 11100 ) ( 2100 11300 )
      + RECT via3 ( 2300 11100 ) ( 2500 11300 )
      + RECT via3 ( 2700 11100 ) ( 2900 11300 )
      + RECT via3 ( 3100 11100 ) ( 3300 11300 )
      + RECT via3 ( 3500 11100 ) ( 3700 11300 )
      + RECT via3 ( 3900 11100 ) ( 4100 11300 )
      + RECT via3 ( 4300 11100 ) ( 4500 11300 )
      + RECT via3 ( 4700 11100 ) ( 4900 11300 )
      + RECT via3 ( 5100 11100 ) ( 5300 11300 )
      + RECT via3 ( 5500 11100 ) ( 5700 11300 ) ;
   - via4_11890_22760
      + RECT met4 ( -5945 -11380 ) ( 5945 11380 )
      + RECT met5 ( -6065 -11500 ) ( 6065 11500 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via3_11830_22150_hx
      + RECT met3 ( -5945 -11075 ) ( 5945 11075 )
      + RECT met4 ( -5920 -11080 ) ( 5920 11080 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 ) ;
   - via4_11690_21950
      + RECT met4 ( -5845 -10975 ) ( 5845 10975 )
      + RECT met5 ( -5965 -11095 ) ( 5965 11095 )
      + RECT via4 ( -5200 -10000 ) ( -4400 -9200 )
      + RECT via4 ( -3600 -10000 ) ( -2800 -9200 )
      + RECT via4 ( -2000 -10000 ) ( -1200 -9200 )
      + RECT via4 ( -400 -10000 ) ( 400 -9200 )
      + RECT via4 ( 1200 -10000 ) ( 2000 -9200 )
      + RECT via4 ( 2800 -10000 ) ( 3600 -9200 )
      + RECT via4 ( 4400 -10000 ) ( 5200 -9200 )
      + RECT via4 ( -5200 -8400 ) ( -4400 -7600 )
      + RECT via4 ( -3600 -8400 ) ( -2800 -7600 )
      + RECT via4 ( -2000 -8400 ) ( -1200 -7600 )
      + RECT via4 ( -400 -8400 ) ( 400 -7600 )
      + RECT via4 ( 1200 -8400 ) ( 2000 -7600 )
      + RECT via4 ( 2800 -8400 ) ( 3600 -7600 )
      + RECT via4 ( 4400 -8400 ) ( 5200 -7600 )
      + RECT via4 ( -5200 -6800 ) ( -4400 -6000 )
      + RECT via4 ( -3600 -6800 ) ( -2800 -6000 )
      + RECT via4 ( -2000 -6800 ) ( -1200 -6000 )
      + RECT via4 ( -400 -6800 ) ( 400 -6000 )
      + RECT via4 ( 1200 -6800 ) ( 2000 -6000 )
      + RECT via4 ( 2800 -6800 ) ( 3600 -6000 )
      + RECT via4 ( 4400 -6800 ) ( 5200 -6000 )
      + RECT via4 ( -5200 -5200 ) ( -4400 -4400 )
      + RECT via4 ( -3600 -5200 ) ( -2800 -4400 )
      + RECT via4 ( -2000 -5200 ) ( -1200 -4400 )
      + RECT via4 ( -400 -5200 ) ( 400 -4400 )
      + RECT via4 ( 1200 -5200 ) ( 2000 -4400 )
      + RECT via4 ( 2800 -5200 ) ( 3600 -4400 )
      + RECT via4 ( 4400 -5200 ) ( 5200 -4400 )
      + RECT via4 ( -5200 -3600 ) ( -4400 -2800 )
      + RECT via4 ( -3600 -3600 ) ( -2800 -2800 )
      + RECT via4 ( -2000 -3600 ) ( -1200 -2800 )
      + RECT via4 ( -400 -3600 ) ( 400 -2800 )
      + RECT via4 ( 1200 -3600 ) ( 2000 -2800 )
      + RECT via4 ( 2800 -3600 ) ( 3600 -2800 )
      + RECT via4 ( 4400 -3600 ) ( 5200 -2800 )
      + RECT via4 ( -5200 -2000 ) ( -4400 -1200 )
      + RECT via4 ( -3600 -2000 ) ( -2800 -1200 )
      + RECT via4 ( -2000 -2000 ) ( -1200 -1200 )
      + RECT via4 ( -400 -2000 ) ( 400 -1200 )
      + RECT via4 ( 1200 -2000 ) ( 2000 -1200 )
      + RECT via4 ( 2800 -2000 ) ( 3600 -1200 )
      + RECT via4 ( 4400 -2000 ) ( 5200 -1200 )
      + RECT via4 ( -5200 -400 ) ( -4400 400 )
      + RECT via4 ( -3600 -400 ) ( -2800 400 )
      + RECT via4 ( -2000 -400 ) ( -1200 400 )
      + RECT via4 ( -400 -400 ) ( 400 400 )
      + RECT via4 ( 1200 -400 ) ( 2000 400 )
      + RECT via4 ( 2800 -400 ) ( 3600 400 )
      + RECT via4 ( 4400 -400 ) ( 5200 400 )
      + RECT via4 ( -5200 1200 ) ( -4400 2000 )
      + RECT via4 ( -3600 1200 ) ( -2800 2000 )
      + RECT via4 ( -2000 1200 ) ( -1200 2000 )
      + RECT via4 ( -400 1200 ) ( 400 2000 )
      + RECT via4 ( 1200 1200 ) ( 2000 2000 )
      + RECT via4 ( 2800 1200 ) ( 3600 2000 )
      + RECT via4 ( 4400 1200 ) ( 5200 2000 )
      + RECT via4 ( -5200 2800 ) ( -4400 3600 )
      + RECT via4 ( -3600 2800 ) ( -2800 3600 )
      + RECT via4 ( -2000 2800 ) ( -1200 3600 )
      + RECT via4 ( -400 2800 ) ( 400 3600 )
      + RECT via4 ( 1200 2800 ) ( 2000 3600 )
      + RECT via4 ( 2800 2800 ) ( 3600 3600 )
      + RECT via4 ( 4400 2800 ) ( 5200 3600 )
      + RECT via4 ( -5200 4400 ) ( -4400 5200 )
      + RECT via4 ( -3600 4400 ) ( -2800 5200 )
      + RECT via4 ( -2000 4400 ) ( -1200 5200 )
      + RECT via4 ( -400 4400 ) ( 400 5200 )
      + RECT via4 ( 1200 4400 ) ( 2000 5200 )
      + RECT via4 ( 2800 4400 ) ( 3600 5200 )
      + RECT via4 ( 4400 4400 ) ( 5200 5200 )
      + RECT via4 ( -5200 6000 ) ( -4400 6800 )
      + RECT via4 ( -3600 6000 ) ( -2800 6800 )
      + RECT via4 ( -2000 6000 ) ( -1200 6800 )
      + RECT via4 ( -400 6000 ) ( 400 6800 )
      + RECT via4 ( 1200 6000 ) ( 2000 6800 )
      + RECT via4 ( 2800 6000 ) ( 3600 6800 )
      + RECT via4 ( 4400 6000 ) ( 5200 6800 )
      + RECT via4 ( -5200 7600 ) ( -4400 8400 )
      + RECT via4 ( -3600 7600 ) ( -2800 8400 )
      + RECT via4 ( -2000 7600 ) ( -1200 8400 )
      + RECT via4 ( -400 7600 ) ( 400 8400 )
      + RECT via4 ( 1200 7600 ) ( 2000 8400 )
      + RECT via4 ( 2800 7600 ) ( 3600 8400 )
      + RECT via4 ( 4400 7600 ) ( 5200 8400 )
      + RECT via4 ( -5200 9200 ) ( -4400 10000 )
      + RECT via4 ( -3600 9200 ) ( -2800 10000 )
      + RECT via4 ( -2000 9200 ) ( -1200 10000 )
      + RECT via4 ( -400 9200 ) ( 400 10000 )
      + RECT via4 ( 1200 9200 ) ( 2000 10000 )
      + RECT via4 ( 2800 9200 ) ( 3600 10000 )
      + RECT via4 ( 4400 9200 ) ( 5200 10000 ) ;
   - via3_11850_22100_hx
      + RECT met3 ( -5955 -11050 ) ( 5955 11050 )
      + RECT met4 ( -5930 -11055 ) ( 5930 11055 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 ) ;
   - via2_300_300_vx
      + RECT met2 ( -150 -195 ) ( 150 195 )
      + RECT met3 ( -175 -175 ) ( 175 175 )
      + RECT via2 ( -100 -100 ) ( 100 100 ) ;
   - via4_11830_22150
      + RECT met4 ( -5915 -11075 ) ( 5915 11075 )
      + RECT met5 ( -6035 -11195 ) ( 6035 11195 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via3_11820_22030_hx
      + RECT met3 ( -5940 -11015 ) ( 5940 11015 )
      + RECT met4 ( -5915 -11020 ) ( 5915 11020 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 ) ;
   - via3_11700_22620_hx
      + RECT met3 ( -5880 -11310 ) ( 5880 11310 )
      + RECT met4 ( -5855 -11315 ) ( 5855 11315 )
      + RECT via3 ( -5700 -11100 ) ( -5500 -10900 )
      + RECT via3 ( -5300 -11100 ) ( -5100 -10900 )
      + RECT via3 ( -4900 -11100 ) ( -4700 -10900 )
      + RECT via3 ( -4500 -11100 ) ( -4300 -10900 )
      + RECT via3 ( -4100 -11100 ) ( -3900 -10900 )
      + RECT via3 ( -3700 -11100 ) ( -3500 -10900 )
      + RECT via3 ( -3300 -11100 ) ( -3100 -10900 )
      + RECT via3 ( -2900 -11100 ) ( -2700 -10900 )
      + RECT via3 ( -2500 -11100 ) ( -2300 -10900 )
      + RECT via3 ( -2100 -11100 ) ( -1900 -10900 )
      + RECT via3 ( -1700 -11100 ) ( -1500 -10900 )
      + RECT via3 ( -1300 -11100 ) ( -1100 -10900 )
      + RECT via3 ( -900 -11100 ) ( -700 -10900 )
      + RECT via3 ( -500 -11100 ) ( -300 -10900 )
      + RECT via3 ( -100 -11100 ) ( 100 -10900 )
      + RECT via3 ( 300 -11100 ) ( 500 -10900 )
      + RECT via3 ( 700 -11100 ) ( 900 -10900 )
      + RECT via3 ( 1100 -11100 ) ( 1300 -10900 )
      + RECT via3 ( 1500 -11100 ) ( 1700 -10900 )
      + RECT via3 ( 1900 -11100 ) ( 2100 -10900 )
      + RECT via3 ( 2300 -11100 ) ( 2500 -10900 )
      + RECT via3 ( 2700 -11100 ) ( 2900 -10900 )
      + RECT via3 ( 3100 -11100 ) ( 3300 -10900 )
      + RECT via3 ( 3500 -11100 ) ( 3700 -10900 )
      + RECT via3 ( 3900 -11100 ) ( 4100 -10900 )
      + RECT via3 ( 4300 -11100 ) ( 4500 -10900 )
      + RECT via3 ( 4700 -11100 ) ( 4900 -10900 )
      + RECT via3 ( 5100 -11100 ) ( 5300 -10900 )
      + RECT via3 ( 5500 -11100 ) ( 5700 -10900 )
      + RECT via3 ( -5700 -10700 ) ( -5500 -10500 )
      + RECT via3 ( -5300 -10700 ) ( -5100 -10500 )
      + RECT via3 ( -4900 -10700 ) ( -4700 -10500 )
      + RECT via3 ( -4500 -10700 ) ( -4300 -10500 )
      + RECT via3 ( -4100 -10700 ) ( -3900 -10500 )
      + RECT via3 ( -3700 -10700 ) ( -3500 -10500 )
      + RECT via3 ( -3300 -10700 ) ( -3100 -10500 )
      + RECT via3 ( -2900 -10700 ) ( -2700 -10500 )
      + RECT via3 ( -2500 -10700 ) ( -2300 -10500 )
      + RECT via3 ( -2100 -10700 ) ( -1900 -10500 )
      + RECT via3 ( -1700 -10700 ) ( -1500 -10500 )
      + RECT via3 ( -1300 -10700 ) ( -1100 -10500 )
      + RECT via3 ( -900 -10700 ) ( -700 -10500 )
      + RECT via3 ( -500 -10700 ) ( -300 -10500 )
      + RECT via3 ( -100 -10700 ) ( 100 -10500 )
      + RECT via3 ( 300 -10700 ) ( 500 -10500 )
      + RECT via3 ( 700 -10700 ) ( 900 -10500 )
      + RECT via3 ( 1100 -10700 ) ( 1300 -10500 )
      + RECT via3 ( 1500 -10700 ) ( 1700 -10500 )
      + RECT via3 ( 1900 -10700 ) ( 2100 -10500 )
      + RECT via3 ( 2300 -10700 ) ( 2500 -10500 )
      + RECT via3 ( 2700 -10700 ) ( 2900 -10500 )
      + RECT via3 ( 3100 -10700 ) ( 3300 -10500 )
      + RECT via3 ( 3500 -10700 ) ( 3700 -10500 )
      + RECT via3 ( 3900 -10700 ) ( 4100 -10500 )
      + RECT via3 ( 4300 -10700 ) ( 4500 -10500 )
      + RECT via3 ( 4700 -10700 ) ( 4900 -10500 )
      + RECT via3 ( 5100 -10700 ) ( 5300 -10500 )
      + RECT via3 ( 5500 -10700 ) ( 5700 -10500 )
      + RECT via3 ( -5700 -10300 ) ( -5500 -10100 )
      + RECT via3 ( -5300 -10300 ) ( -5100 -10100 )
      + RECT via3 ( -4900 -10300 ) ( -4700 -10100 )
      + RECT via3 ( -4500 -10300 ) ( -4300 -10100 )
      + RECT via3 ( -4100 -10300 ) ( -3900 -10100 )
      + RECT via3 ( -3700 -10300 ) ( -3500 -10100 )
      + RECT via3 ( -3300 -10300 ) ( -3100 -10100 )
      + RECT via3 ( -2900 -10300 ) ( -2700 -10100 )
      + RECT via3 ( -2500 -10300 ) ( -2300 -10100 )
      + RECT via3 ( -2100 -10300 ) ( -1900 -10100 )
      + RECT via3 ( -1700 -10300 ) ( -1500 -10100 )
      + RECT via3 ( -1300 -10300 ) ( -1100 -10100 )
      + RECT via3 ( -900 -10300 ) ( -700 -10100 )
      + RECT via3 ( -500 -10300 ) ( -300 -10100 )
      + RECT via3 ( -100 -10300 ) ( 100 -10100 )
      + RECT via3 ( 300 -10300 ) ( 500 -10100 )
      + RECT via3 ( 700 -10300 ) ( 900 -10100 )
      + RECT via3 ( 1100 -10300 ) ( 1300 -10100 )
      + RECT via3 ( 1500 -10300 ) ( 1700 -10100 )
      + RECT via3 ( 1900 -10300 ) ( 2100 -10100 )
      + RECT via3 ( 2300 -10300 ) ( 2500 -10100 )
      + RECT via3 ( 2700 -10300 ) ( 2900 -10100 )
      + RECT via3 ( 3100 -10300 ) ( 3300 -10100 )
      + RECT via3 ( 3500 -10300 ) ( 3700 -10100 )
      + RECT via3 ( 3900 -10300 ) ( 4100 -10100 )
      + RECT via3 ( 4300 -10300 ) ( 4500 -10100 )
      + RECT via3 ( 4700 -10300 ) ( 4900 -10100 )
      + RECT via3 ( 5100 -10300 ) ( 5300 -10100 )
      + RECT via3 ( 5500 -10300 ) ( 5700 -10100 )
      + RECT via3 ( -5700 -9900 ) ( -5500 -9700 )
      + RECT via3 ( -5300 -9900 ) ( -5100 -9700 )
      + RECT via3 ( -4900 -9900 ) ( -4700 -9700 )
      + RECT via3 ( -4500 -9900 ) ( -4300 -9700 )
      + RECT via3 ( -4100 -9900 ) ( -3900 -9700 )
      + RECT via3 ( -3700 -9900 ) ( -3500 -9700 )
      + RECT via3 ( -3300 -9900 ) ( -3100 -9700 )
      + RECT via3 ( -2900 -9900 ) ( -2700 -9700 )
      + RECT via3 ( -2500 -9900 ) ( -2300 -9700 )
      + RECT via3 ( -2100 -9900 ) ( -1900 -9700 )
      + RECT via3 ( -1700 -9900 ) ( -1500 -9700 )
      + RECT via3 ( -1300 -9900 ) ( -1100 -9700 )
      + RECT via3 ( -900 -9900 ) ( -700 -9700 )
      + RECT via3 ( -500 -9900 ) ( -300 -9700 )
      + RECT via3 ( -100 -9900 ) ( 100 -9700 )
      + RECT via3 ( 300 -9900 ) ( 500 -9700 )
      + RECT via3 ( 700 -9900 ) ( 900 -9700 )
      + RECT via3 ( 1100 -9900 ) ( 1300 -9700 )
      + RECT via3 ( 1500 -9900 ) ( 1700 -9700 )
      + RECT via3 ( 1900 -9900 ) ( 2100 -9700 )
      + RECT via3 ( 2300 -9900 ) ( 2500 -9700 )
      + RECT via3 ( 2700 -9900 ) ( 2900 -9700 )
      + RECT via3 ( 3100 -9900 ) ( 3300 -9700 )
      + RECT via3 ( 3500 -9900 ) ( 3700 -9700 )
      + RECT via3 ( 3900 -9900 ) ( 4100 -9700 )
      + RECT via3 ( 4300 -9900 ) ( 4500 -9700 )
      + RECT via3 ( 4700 -9900 ) ( 4900 -9700 )
      + RECT via3 ( 5100 -9900 ) ( 5300 -9700 )
      + RECT via3 ( 5500 -9900 ) ( 5700 -9700 )
      + RECT via3 ( -5700 -9500 ) ( -5500 -9300 )
      + RECT via3 ( -5300 -9500 ) ( -5100 -9300 )
      + RECT via3 ( -4900 -9500 ) ( -4700 -9300 )
      + RECT via3 ( -4500 -9500 ) ( -4300 -9300 )
      + RECT via3 ( -4100 -9500 ) ( -3900 -9300 )
      + RECT via3 ( -3700 -9500 ) ( -3500 -9300 )
      + RECT via3 ( -3300 -9500 ) ( -3100 -9300 )
      + RECT via3 ( -2900 -9500 ) ( -2700 -9300 )
      + RECT via3 ( -2500 -9500 ) ( -2300 -9300 )
      + RECT via3 ( -2100 -9500 ) ( -1900 -9300 )
      + RECT via3 ( -1700 -9500 ) ( -1500 -9300 )
      + RECT via3 ( -1300 -9500 ) ( -1100 -9300 )
      + RECT via3 ( -900 -9500 ) ( -700 -9300 )
      + RECT via3 ( -500 -9500 ) ( -300 -9300 )
      + RECT via3 ( -100 -9500 ) ( 100 -9300 )
      + RECT via3 ( 300 -9500 ) ( 500 -9300 )
      + RECT via3 ( 700 -9500 ) ( 900 -9300 )
      + RECT via3 ( 1100 -9500 ) ( 1300 -9300 )
      + RECT via3 ( 1500 -9500 ) ( 1700 -9300 )
      + RECT via3 ( 1900 -9500 ) ( 2100 -9300 )
      + RECT via3 ( 2300 -9500 ) ( 2500 -9300 )
      + RECT via3 ( 2700 -9500 ) ( 2900 -9300 )
      + RECT via3 ( 3100 -9500 ) ( 3300 -9300 )
      + RECT via3 ( 3500 -9500 ) ( 3700 -9300 )
      + RECT via3 ( 3900 -9500 ) ( 4100 -9300 )
      + RECT via3 ( 4300 -9500 ) ( 4500 -9300 )
      + RECT via3 ( 4700 -9500 ) ( 4900 -9300 )
      + RECT via3 ( 5100 -9500 ) ( 5300 -9300 )
      + RECT via3 ( 5500 -9500 ) ( 5700 -9300 )
      + RECT via3 ( -5700 -9100 ) ( -5500 -8900 )
      + RECT via3 ( -5300 -9100 ) ( -5100 -8900 )
      + RECT via3 ( -4900 -9100 ) ( -4700 -8900 )
      + RECT via3 ( -4500 -9100 ) ( -4300 -8900 )
      + RECT via3 ( -4100 -9100 ) ( -3900 -8900 )
      + RECT via3 ( -3700 -9100 ) ( -3500 -8900 )
      + RECT via3 ( -3300 -9100 ) ( -3100 -8900 )
      + RECT via3 ( -2900 -9100 ) ( -2700 -8900 )
      + RECT via3 ( -2500 -9100 ) ( -2300 -8900 )
      + RECT via3 ( -2100 -9100 ) ( -1900 -8900 )
      + RECT via3 ( -1700 -9100 ) ( -1500 -8900 )
      + RECT via3 ( -1300 -9100 ) ( -1100 -8900 )
      + RECT via3 ( -900 -9100 ) ( -700 -8900 )
      + RECT via3 ( -500 -9100 ) ( -300 -8900 )
      + RECT via3 ( -100 -9100 ) ( 100 -8900 )
      + RECT via3 ( 300 -9100 ) ( 500 -8900 )
      + RECT via3 ( 700 -9100 ) ( 900 -8900 )
      + RECT via3 ( 1100 -9100 ) ( 1300 -8900 )
      + RECT via3 ( 1500 -9100 ) ( 1700 -8900 )
      + RECT via3 ( 1900 -9100 ) ( 2100 -8900 )
      + RECT via3 ( 2300 -9100 ) ( 2500 -8900 )
      + RECT via3 ( 2700 -9100 ) ( 2900 -8900 )
      + RECT via3 ( 3100 -9100 ) ( 3300 -8900 )
      + RECT via3 ( 3500 -9100 ) ( 3700 -8900 )
      + RECT via3 ( 3900 -9100 ) ( 4100 -8900 )
      + RECT via3 ( 4300 -9100 ) ( 4500 -8900 )
      + RECT via3 ( 4700 -9100 ) ( 4900 -8900 )
      + RECT via3 ( 5100 -9100 ) ( 5300 -8900 )
      + RECT via3 ( 5500 -9100 ) ( 5700 -8900 )
      + RECT via3 ( -5700 -8700 ) ( -5500 -8500 )
      + RECT via3 ( -5300 -8700 ) ( -5100 -8500 )
      + RECT via3 ( -4900 -8700 ) ( -4700 -8500 )
      + RECT via3 ( -4500 -8700 ) ( -4300 -8500 )
      + RECT via3 ( -4100 -8700 ) ( -3900 -8500 )
      + RECT via3 ( -3700 -8700 ) ( -3500 -8500 )
      + RECT via3 ( -3300 -8700 ) ( -3100 -8500 )
      + RECT via3 ( -2900 -8700 ) ( -2700 -8500 )
      + RECT via3 ( -2500 -8700 ) ( -2300 -8500 )
      + RECT via3 ( -2100 -8700 ) ( -1900 -8500 )
      + RECT via3 ( -1700 -8700 ) ( -1500 -8500 )
      + RECT via3 ( -1300 -8700 ) ( -1100 -8500 )
      + RECT via3 ( -900 -8700 ) ( -700 -8500 )
      + RECT via3 ( -500 -8700 ) ( -300 -8500 )
      + RECT via3 ( -100 -8700 ) ( 100 -8500 )
      + RECT via3 ( 300 -8700 ) ( 500 -8500 )
      + RECT via3 ( 700 -8700 ) ( 900 -8500 )
      + RECT via3 ( 1100 -8700 ) ( 1300 -8500 )
      + RECT via3 ( 1500 -8700 ) ( 1700 -8500 )
      + RECT via3 ( 1900 -8700 ) ( 2100 -8500 )
      + RECT via3 ( 2300 -8700 ) ( 2500 -8500 )
      + RECT via3 ( 2700 -8700 ) ( 2900 -8500 )
      + RECT via3 ( 3100 -8700 ) ( 3300 -8500 )
      + RECT via3 ( 3500 -8700 ) ( 3700 -8500 )
      + RECT via3 ( 3900 -8700 ) ( 4100 -8500 )
      + RECT via3 ( 4300 -8700 ) ( 4500 -8500 )
      + RECT via3 ( 4700 -8700 ) ( 4900 -8500 )
      + RECT via3 ( 5100 -8700 ) ( 5300 -8500 )
      + RECT via3 ( 5500 -8700 ) ( 5700 -8500 )
      + RECT via3 ( -5700 -8300 ) ( -5500 -8100 )
      + RECT via3 ( -5300 -8300 ) ( -5100 -8100 )
      + RECT via3 ( -4900 -8300 ) ( -4700 -8100 )
      + RECT via3 ( -4500 -8300 ) ( -4300 -8100 )
      + RECT via3 ( -4100 -8300 ) ( -3900 -8100 )
      + RECT via3 ( -3700 -8300 ) ( -3500 -8100 )
      + RECT via3 ( -3300 -8300 ) ( -3100 -8100 )
      + RECT via3 ( -2900 -8300 ) ( -2700 -8100 )
      + RECT via3 ( -2500 -8300 ) ( -2300 -8100 )
      + RECT via3 ( -2100 -8300 ) ( -1900 -8100 )
      + RECT via3 ( -1700 -8300 ) ( -1500 -8100 )
      + RECT via3 ( -1300 -8300 ) ( -1100 -8100 )
      + RECT via3 ( -900 -8300 ) ( -700 -8100 )
      + RECT via3 ( -500 -8300 ) ( -300 -8100 )
      + RECT via3 ( -100 -8300 ) ( 100 -8100 )
      + RECT via3 ( 300 -8300 ) ( 500 -8100 )
      + RECT via3 ( 700 -8300 ) ( 900 -8100 )
      + RECT via3 ( 1100 -8300 ) ( 1300 -8100 )
      + RECT via3 ( 1500 -8300 ) ( 1700 -8100 )
      + RECT via3 ( 1900 -8300 ) ( 2100 -8100 )
      + RECT via3 ( 2300 -8300 ) ( 2500 -8100 )
      + RECT via3 ( 2700 -8300 ) ( 2900 -8100 )
      + RECT via3 ( 3100 -8300 ) ( 3300 -8100 )
      + RECT via3 ( 3500 -8300 ) ( 3700 -8100 )
      + RECT via3 ( 3900 -8300 ) ( 4100 -8100 )
      + RECT via3 ( 4300 -8300 ) ( 4500 -8100 )
      + RECT via3 ( 4700 -8300 ) ( 4900 -8100 )
      + RECT via3 ( 5100 -8300 ) ( 5300 -8100 )
      + RECT via3 ( 5500 -8300 ) ( 5700 -8100 )
      + RECT via3 ( -5700 -7900 ) ( -5500 -7700 )
      + RECT via3 ( -5300 -7900 ) ( -5100 -7700 )
      + RECT via3 ( -4900 -7900 ) ( -4700 -7700 )
      + RECT via3 ( -4500 -7900 ) ( -4300 -7700 )
      + RECT via3 ( -4100 -7900 ) ( -3900 -7700 )
      + RECT via3 ( -3700 -7900 ) ( -3500 -7700 )
      + RECT via3 ( -3300 -7900 ) ( -3100 -7700 )
      + RECT via3 ( -2900 -7900 ) ( -2700 -7700 )
      + RECT via3 ( -2500 -7900 ) ( -2300 -7700 )
      + RECT via3 ( -2100 -7900 ) ( -1900 -7700 )
      + RECT via3 ( -1700 -7900 ) ( -1500 -7700 )
      + RECT via3 ( -1300 -7900 ) ( -1100 -7700 )
      + RECT via3 ( -900 -7900 ) ( -700 -7700 )
      + RECT via3 ( -500 -7900 ) ( -300 -7700 )
      + RECT via3 ( -100 -7900 ) ( 100 -7700 )
      + RECT via3 ( 300 -7900 ) ( 500 -7700 )
      + RECT via3 ( 700 -7900 ) ( 900 -7700 )
      + RECT via3 ( 1100 -7900 ) ( 1300 -7700 )
      + RECT via3 ( 1500 -7900 ) ( 1700 -7700 )
      + RECT via3 ( 1900 -7900 ) ( 2100 -7700 )
      + RECT via3 ( 2300 -7900 ) ( 2500 -7700 )
      + RECT via3 ( 2700 -7900 ) ( 2900 -7700 )
      + RECT via3 ( 3100 -7900 ) ( 3300 -7700 )
      + RECT via3 ( 3500 -7900 ) ( 3700 -7700 )
      + RECT via3 ( 3900 -7900 ) ( 4100 -7700 )
      + RECT via3 ( 4300 -7900 ) ( 4500 -7700 )
      + RECT via3 ( 4700 -7900 ) ( 4900 -7700 )
      + RECT via3 ( 5100 -7900 ) ( 5300 -7700 )
      + RECT via3 ( 5500 -7900 ) ( 5700 -7700 )
      + RECT via3 ( -5700 -7500 ) ( -5500 -7300 )
      + RECT via3 ( -5300 -7500 ) ( -5100 -7300 )
      + RECT via3 ( -4900 -7500 ) ( -4700 -7300 )
      + RECT via3 ( -4500 -7500 ) ( -4300 -7300 )
      + RECT via3 ( -4100 -7500 ) ( -3900 -7300 )
      + RECT via3 ( -3700 -7500 ) ( -3500 -7300 )
      + RECT via3 ( -3300 -7500 ) ( -3100 -7300 )
      + RECT via3 ( -2900 -7500 ) ( -2700 -7300 )
      + RECT via3 ( -2500 -7500 ) ( -2300 -7300 )
      + RECT via3 ( -2100 -7500 ) ( -1900 -7300 )
      + RECT via3 ( -1700 -7500 ) ( -1500 -7300 )
      + RECT via3 ( -1300 -7500 ) ( -1100 -7300 )
      + RECT via3 ( -900 -7500 ) ( -700 -7300 )
      + RECT via3 ( -500 -7500 ) ( -300 -7300 )
      + RECT via3 ( -100 -7500 ) ( 100 -7300 )
      + RECT via3 ( 300 -7500 ) ( 500 -7300 )
      + RECT via3 ( 700 -7500 ) ( 900 -7300 )
      + RECT via3 ( 1100 -7500 ) ( 1300 -7300 )
      + RECT via3 ( 1500 -7500 ) ( 1700 -7300 )
      + RECT via3 ( 1900 -7500 ) ( 2100 -7300 )
      + RECT via3 ( 2300 -7500 ) ( 2500 -7300 )
      + RECT via3 ( 2700 -7500 ) ( 2900 -7300 )
      + RECT via3 ( 3100 -7500 ) ( 3300 -7300 )
      + RECT via3 ( 3500 -7500 ) ( 3700 -7300 )
      + RECT via3 ( 3900 -7500 ) ( 4100 -7300 )
      + RECT via3 ( 4300 -7500 ) ( 4500 -7300 )
      + RECT via3 ( 4700 -7500 ) ( 4900 -7300 )
      + RECT via3 ( 5100 -7500 ) ( 5300 -7300 )
      + RECT via3 ( 5500 -7500 ) ( 5700 -7300 )
      + RECT via3 ( -5700 -7100 ) ( -5500 -6900 )
      + RECT via3 ( -5300 -7100 ) ( -5100 -6900 )
      + RECT via3 ( -4900 -7100 ) ( -4700 -6900 )
      + RECT via3 ( -4500 -7100 ) ( -4300 -6900 )
      + RECT via3 ( -4100 -7100 ) ( -3900 -6900 )
      + RECT via3 ( -3700 -7100 ) ( -3500 -6900 )
      + RECT via3 ( -3300 -7100 ) ( -3100 -6900 )
      + RECT via3 ( -2900 -7100 ) ( -2700 -6900 )
      + RECT via3 ( -2500 -7100 ) ( -2300 -6900 )
      + RECT via3 ( -2100 -7100 ) ( -1900 -6900 )
      + RECT via3 ( -1700 -7100 ) ( -1500 -6900 )
      + RECT via3 ( -1300 -7100 ) ( -1100 -6900 )
      + RECT via3 ( -900 -7100 ) ( -700 -6900 )
      + RECT via3 ( -500 -7100 ) ( -300 -6900 )
      + RECT via3 ( -100 -7100 ) ( 100 -6900 )
      + RECT via3 ( 300 -7100 ) ( 500 -6900 )
      + RECT via3 ( 700 -7100 ) ( 900 -6900 )
      + RECT via3 ( 1100 -7100 ) ( 1300 -6900 )
      + RECT via3 ( 1500 -7100 ) ( 1700 -6900 )
      + RECT via3 ( 1900 -7100 ) ( 2100 -6900 )
      + RECT via3 ( 2300 -7100 ) ( 2500 -6900 )
      + RECT via3 ( 2700 -7100 ) ( 2900 -6900 )
      + RECT via3 ( 3100 -7100 ) ( 3300 -6900 )
      + RECT via3 ( 3500 -7100 ) ( 3700 -6900 )
      + RECT via3 ( 3900 -7100 ) ( 4100 -6900 )
      + RECT via3 ( 4300 -7100 ) ( 4500 -6900 )
      + RECT via3 ( 4700 -7100 ) ( 4900 -6900 )
      + RECT via3 ( 5100 -7100 ) ( 5300 -6900 )
      + RECT via3 ( 5500 -7100 ) ( 5700 -6900 )
      + RECT via3 ( -5700 -6700 ) ( -5500 -6500 )
      + RECT via3 ( -5300 -6700 ) ( -5100 -6500 )
      + RECT via3 ( -4900 -6700 ) ( -4700 -6500 )
      + RECT via3 ( -4500 -6700 ) ( -4300 -6500 )
      + RECT via3 ( -4100 -6700 ) ( -3900 -6500 )
      + RECT via3 ( -3700 -6700 ) ( -3500 -6500 )
      + RECT via3 ( -3300 -6700 ) ( -3100 -6500 )
      + RECT via3 ( -2900 -6700 ) ( -2700 -6500 )
      + RECT via3 ( -2500 -6700 ) ( -2300 -6500 )
      + RECT via3 ( -2100 -6700 ) ( -1900 -6500 )
      + RECT via3 ( -1700 -6700 ) ( -1500 -6500 )
      + RECT via3 ( -1300 -6700 ) ( -1100 -6500 )
      + RECT via3 ( -900 -6700 ) ( -700 -6500 )
      + RECT via3 ( -500 -6700 ) ( -300 -6500 )
      + RECT via3 ( -100 -6700 ) ( 100 -6500 )
      + RECT via3 ( 300 -6700 ) ( 500 -6500 )
      + RECT via3 ( 700 -6700 ) ( 900 -6500 )
      + RECT via3 ( 1100 -6700 ) ( 1300 -6500 )
      + RECT via3 ( 1500 -6700 ) ( 1700 -6500 )
      + RECT via3 ( 1900 -6700 ) ( 2100 -6500 )
      + RECT via3 ( 2300 -6700 ) ( 2500 -6500 )
      + RECT via3 ( 2700 -6700 ) ( 2900 -6500 )
      + RECT via3 ( 3100 -6700 ) ( 3300 -6500 )
      + RECT via3 ( 3500 -6700 ) ( 3700 -6500 )
      + RECT via3 ( 3900 -6700 ) ( 4100 -6500 )
      + RECT via3 ( 4300 -6700 ) ( 4500 -6500 )
      + RECT via3 ( 4700 -6700 ) ( 4900 -6500 )
      + RECT via3 ( 5100 -6700 ) ( 5300 -6500 )
      + RECT via3 ( 5500 -6700 ) ( 5700 -6500 )
      + RECT via3 ( -5700 -6300 ) ( -5500 -6100 )
      + RECT via3 ( -5300 -6300 ) ( -5100 -6100 )
      + RECT via3 ( -4900 -6300 ) ( -4700 -6100 )
      + RECT via3 ( -4500 -6300 ) ( -4300 -6100 )
      + RECT via3 ( -4100 -6300 ) ( -3900 -6100 )
      + RECT via3 ( -3700 -6300 ) ( -3500 -6100 )
      + RECT via3 ( -3300 -6300 ) ( -3100 -6100 )
      + RECT via3 ( -2900 -6300 ) ( -2700 -6100 )
      + RECT via3 ( -2500 -6300 ) ( -2300 -6100 )
      + RECT via3 ( -2100 -6300 ) ( -1900 -6100 )
      + RECT via3 ( -1700 -6300 ) ( -1500 -6100 )
      + RECT via3 ( -1300 -6300 ) ( -1100 -6100 )
      + RECT via3 ( -900 -6300 ) ( -700 -6100 )
      + RECT via3 ( -500 -6300 ) ( -300 -6100 )
      + RECT via3 ( -100 -6300 ) ( 100 -6100 )
      + RECT via3 ( 300 -6300 ) ( 500 -6100 )
      + RECT via3 ( 700 -6300 ) ( 900 -6100 )
      + RECT via3 ( 1100 -6300 ) ( 1300 -6100 )
      + RECT via3 ( 1500 -6300 ) ( 1700 -6100 )
      + RECT via3 ( 1900 -6300 ) ( 2100 -6100 )
      + RECT via3 ( 2300 -6300 ) ( 2500 -6100 )
      + RECT via3 ( 2700 -6300 ) ( 2900 -6100 )
      + RECT via3 ( 3100 -6300 ) ( 3300 -6100 )
      + RECT via3 ( 3500 -6300 ) ( 3700 -6100 )
      + RECT via3 ( 3900 -6300 ) ( 4100 -6100 )
      + RECT via3 ( 4300 -6300 ) ( 4500 -6100 )
      + RECT via3 ( 4700 -6300 ) ( 4900 -6100 )
      + RECT via3 ( 5100 -6300 ) ( 5300 -6100 )
      + RECT via3 ( 5500 -6300 ) ( 5700 -6100 )
      + RECT via3 ( -5700 -5900 ) ( -5500 -5700 )
      + RECT via3 ( -5300 -5900 ) ( -5100 -5700 )
      + RECT via3 ( -4900 -5900 ) ( -4700 -5700 )
      + RECT via3 ( -4500 -5900 ) ( -4300 -5700 )
      + RECT via3 ( -4100 -5900 ) ( -3900 -5700 )
      + RECT via3 ( -3700 -5900 ) ( -3500 -5700 )
      + RECT via3 ( -3300 -5900 ) ( -3100 -5700 )
      + RECT via3 ( -2900 -5900 ) ( -2700 -5700 )
      + RECT via3 ( -2500 -5900 ) ( -2300 -5700 )
      + RECT via3 ( -2100 -5900 ) ( -1900 -5700 )
      + RECT via3 ( -1700 -5900 ) ( -1500 -5700 )
      + RECT via3 ( -1300 -5900 ) ( -1100 -5700 )
      + RECT via3 ( -900 -5900 ) ( -700 -5700 )
      + RECT via3 ( -500 -5900 ) ( -300 -5700 )
      + RECT via3 ( -100 -5900 ) ( 100 -5700 )
      + RECT via3 ( 300 -5900 ) ( 500 -5700 )
      + RECT via3 ( 700 -5900 ) ( 900 -5700 )
      + RECT via3 ( 1100 -5900 ) ( 1300 -5700 )
      + RECT via3 ( 1500 -5900 ) ( 1700 -5700 )
      + RECT via3 ( 1900 -5900 ) ( 2100 -5700 )
      + RECT via3 ( 2300 -5900 ) ( 2500 -5700 )
      + RECT via3 ( 2700 -5900 ) ( 2900 -5700 )
      + RECT via3 ( 3100 -5900 ) ( 3300 -5700 )
      + RECT via3 ( 3500 -5900 ) ( 3700 -5700 )
      + RECT via3 ( 3900 -5900 ) ( 4100 -5700 )
      + RECT via3 ( 4300 -5900 ) ( 4500 -5700 )
      + RECT via3 ( 4700 -5900 ) ( 4900 -5700 )
      + RECT via3 ( 5100 -5900 ) ( 5300 -5700 )
      + RECT via3 ( 5500 -5900 ) ( 5700 -5700 )
      + RECT via3 ( -5700 -5500 ) ( -5500 -5300 )
      + RECT via3 ( -5300 -5500 ) ( -5100 -5300 )
      + RECT via3 ( -4900 -5500 ) ( -4700 -5300 )
      + RECT via3 ( -4500 -5500 ) ( -4300 -5300 )
      + RECT via3 ( -4100 -5500 ) ( -3900 -5300 )
      + RECT via3 ( -3700 -5500 ) ( -3500 -5300 )
      + RECT via3 ( -3300 -5500 ) ( -3100 -5300 )
      + RECT via3 ( -2900 -5500 ) ( -2700 -5300 )
      + RECT via3 ( -2500 -5500 ) ( -2300 -5300 )
      + RECT via3 ( -2100 -5500 ) ( -1900 -5300 )
      + RECT via3 ( -1700 -5500 ) ( -1500 -5300 )
      + RECT via3 ( -1300 -5500 ) ( -1100 -5300 )
      + RECT via3 ( -900 -5500 ) ( -700 -5300 )
      + RECT via3 ( -500 -5500 ) ( -300 -5300 )
      + RECT via3 ( -100 -5500 ) ( 100 -5300 )
      + RECT via3 ( 300 -5500 ) ( 500 -5300 )
      + RECT via3 ( 700 -5500 ) ( 900 -5300 )
      + RECT via3 ( 1100 -5500 ) ( 1300 -5300 )
      + RECT via3 ( 1500 -5500 ) ( 1700 -5300 )
      + RECT via3 ( 1900 -5500 ) ( 2100 -5300 )
      + RECT via3 ( 2300 -5500 ) ( 2500 -5300 )
      + RECT via3 ( 2700 -5500 ) ( 2900 -5300 )
      + RECT via3 ( 3100 -5500 ) ( 3300 -5300 )
      + RECT via3 ( 3500 -5500 ) ( 3700 -5300 )
      + RECT via3 ( 3900 -5500 ) ( 4100 -5300 )
      + RECT via3 ( 4300 -5500 ) ( 4500 -5300 )
      + RECT via3 ( 4700 -5500 ) ( 4900 -5300 )
      + RECT via3 ( 5100 -5500 ) ( 5300 -5300 )
      + RECT via3 ( 5500 -5500 ) ( 5700 -5300 )
      + RECT via3 ( -5700 -5100 ) ( -5500 -4900 )
      + RECT via3 ( -5300 -5100 ) ( -5100 -4900 )
      + RECT via3 ( -4900 -5100 ) ( -4700 -4900 )
      + RECT via3 ( -4500 -5100 ) ( -4300 -4900 )
      + RECT via3 ( -4100 -5100 ) ( -3900 -4900 )
      + RECT via3 ( -3700 -5100 ) ( -3500 -4900 )
      + RECT via3 ( -3300 -5100 ) ( -3100 -4900 )
      + RECT via3 ( -2900 -5100 ) ( -2700 -4900 )
      + RECT via3 ( -2500 -5100 ) ( -2300 -4900 )
      + RECT via3 ( -2100 -5100 ) ( -1900 -4900 )
      + RECT via3 ( -1700 -5100 ) ( -1500 -4900 )
      + RECT via3 ( -1300 -5100 ) ( -1100 -4900 )
      + RECT via3 ( -900 -5100 ) ( -700 -4900 )
      + RECT via3 ( -500 -5100 ) ( -300 -4900 )
      + RECT via3 ( -100 -5100 ) ( 100 -4900 )
      + RECT via3 ( 300 -5100 ) ( 500 -4900 )
      + RECT via3 ( 700 -5100 ) ( 900 -4900 )
      + RECT via3 ( 1100 -5100 ) ( 1300 -4900 )
      + RECT via3 ( 1500 -5100 ) ( 1700 -4900 )
      + RECT via3 ( 1900 -5100 ) ( 2100 -4900 )
      + RECT via3 ( 2300 -5100 ) ( 2500 -4900 )
      + RECT via3 ( 2700 -5100 ) ( 2900 -4900 )
      + RECT via3 ( 3100 -5100 ) ( 3300 -4900 )
      + RECT via3 ( 3500 -5100 ) ( 3700 -4900 )
      + RECT via3 ( 3900 -5100 ) ( 4100 -4900 )
      + RECT via3 ( 4300 -5100 ) ( 4500 -4900 )
      + RECT via3 ( 4700 -5100 ) ( 4900 -4900 )
      + RECT via3 ( 5100 -5100 ) ( 5300 -4900 )
      + RECT via3 ( 5500 -5100 ) ( 5700 -4900 )
      + RECT via3 ( -5700 -4700 ) ( -5500 -4500 )
      + RECT via3 ( -5300 -4700 ) ( -5100 -4500 )
      + RECT via3 ( -4900 -4700 ) ( -4700 -4500 )
      + RECT via3 ( -4500 -4700 ) ( -4300 -4500 )
      + RECT via3 ( -4100 -4700 ) ( -3900 -4500 )
      + RECT via3 ( -3700 -4700 ) ( -3500 -4500 )
      + RECT via3 ( -3300 -4700 ) ( -3100 -4500 )
      + RECT via3 ( -2900 -4700 ) ( -2700 -4500 )
      + RECT via3 ( -2500 -4700 ) ( -2300 -4500 )
      + RECT via3 ( -2100 -4700 ) ( -1900 -4500 )
      + RECT via3 ( -1700 -4700 ) ( -1500 -4500 )
      + RECT via3 ( -1300 -4700 ) ( -1100 -4500 )
      + RECT via3 ( -900 -4700 ) ( -700 -4500 )
      + RECT via3 ( -500 -4700 ) ( -300 -4500 )
      + RECT via3 ( -100 -4700 ) ( 100 -4500 )
      + RECT via3 ( 300 -4700 ) ( 500 -4500 )
      + RECT via3 ( 700 -4700 ) ( 900 -4500 )
      + RECT via3 ( 1100 -4700 ) ( 1300 -4500 )
      + RECT via3 ( 1500 -4700 ) ( 1700 -4500 )
      + RECT via3 ( 1900 -4700 ) ( 2100 -4500 )
      + RECT via3 ( 2300 -4700 ) ( 2500 -4500 )
      + RECT via3 ( 2700 -4700 ) ( 2900 -4500 )
      + RECT via3 ( 3100 -4700 ) ( 3300 -4500 )
      + RECT via3 ( 3500 -4700 ) ( 3700 -4500 )
      + RECT via3 ( 3900 -4700 ) ( 4100 -4500 )
      + RECT via3 ( 4300 -4700 ) ( 4500 -4500 )
      + RECT via3 ( 4700 -4700 ) ( 4900 -4500 )
      + RECT via3 ( 5100 -4700 ) ( 5300 -4500 )
      + RECT via3 ( 5500 -4700 ) ( 5700 -4500 )
      + RECT via3 ( -5700 -4300 ) ( -5500 -4100 )
      + RECT via3 ( -5300 -4300 ) ( -5100 -4100 )
      + RECT via3 ( -4900 -4300 ) ( -4700 -4100 )
      + RECT via3 ( -4500 -4300 ) ( -4300 -4100 )
      + RECT via3 ( -4100 -4300 ) ( -3900 -4100 )
      + RECT via3 ( -3700 -4300 ) ( -3500 -4100 )
      + RECT via3 ( -3300 -4300 ) ( -3100 -4100 )
      + RECT via3 ( -2900 -4300 ) ( -2700 -4100 )
      + RECT via3 ( -2500 -4300 ) ( -2300 -4100 )
      + RECT via3 ( -2100 -4300 ) ( -1900 -4100 )
      + RECT via3 ( -1700 -4300 ) ( -1500 -4100 )
      + RECT via3 ( -1300 -4300 ) ( -1100 -4100 )
      + RECT via3 ( -900 -4300 ) ( -700 -4100 )
      + RECT via3 ( -500 -4300 ) ( -300 -4100 )
      + RECT via3 ( -100 -4300 ) ( 100 -4100 )
      + RECT via3 ( 300 -4300 ) ( 500 -4100 )
      + RECT via3 ( 700 -4300 ) ( 900 -4100 )
      + RECT via3 ( 1100 -4300 ) ( 1300 -4100 )
      + RECT via3 ( 1500 -4300 ) ( 1700 -4100 )
      + RECT via3 ( 1900 -4300 ) ( 2100 -4100 )
      + RECT via3 ( 2300 -4300 ) ( 2500 -4100 )
      + RECT via3 ( 2700 -4300 ) ( 2900 -4100 )
      + RECT via3 ( 3100 -4300 ) ( 3300 -4100 )
      + RECT via3 ( 3500 -4300 ) ( 3700 -4100 )
      + RECT via3 ( 3900 -4300 ) ( 4100 -4100 )
      + RECT via3 ( 4300 -4300 ) ( 4500 -4100 )
      + RECT via3 ( 4700 -4300 ) ( 4900 -4100 )
      + RECT via3 ( 5100 -4300 ) ( 5300 -4100 )
      + RECT via3 ( 5500 -4300 ) ( 5700 -4100 )
      + RECT via3 ( -5700 -3900 ) ( -5500 -3700 )
      + RECT via3 ( -5300 -3900 ) ( -5100 -3700 )
      + RECT via3 ( -4900 -3900 ) ( -4700 -3700 )
      + RECT via3 ( -4500 -3900 ) ( -4300 -3700 )
      + RECT via3 ( -4100 -3900 ) ( -3900 -3700 )
      + RECT via3 ( -3700 -3900 ) ( -3500 -3700 )
      + RECT via3 ( -3300 -3900 ) ( -3100 -3700 )
      + RECT via3 ( -2900 -3900 ) ( -2700 -3700 )
      + RECT via3 ( -2500 -3900 ) ( -2300 -3700 )
      + RECT via3 ( -2100 -3900 ) ( -1900 -3700 )
      + RECT via3 ( -1700 -3900 ) ( -1500 -3700 )
      + RECT via3 ( -1300 -3900 ) ( -1100 -3700 )
      + RECT via3 ( -900 -3900 ) ( -700 -3700 )
      + RECT via3 ( -500 -3900 ) ( -300 -3700 )
      + RECT via3 ( -100 -3900 ) ( 100 -3700 )
      + RECT via3 ( 300 -3900 ) ( 500 -3700 )
      + RECT via3 ( 700 -3900 ) ( 900 -3700 )
      + RECT via3 ( 1100 -3900 ) ( 1300 -3700 )
      + RECT via3 ( 1500 -3900 ) ( 1700 -3700 )
      + RECT via3 ( 1900 -3900 ) ( 2100 -3700 )
      + RECT via3 ( 2300 -3900 ) ( 2500 -3700 )
      + RECT via3 ( 2700 -3900 ) ( 2900 -3700 )
      + RECT via3 ( 3100 -3900 ) ( 3300 -3700 )
      + RECT via3 ( 3500 -3900 ) ( 3700 -3700 )
      + RECT via3 ( 3900 -3900 ) ( 4100 -3700 )
      + RECT via3 ( 4300 -3900 ) ( 4500 -3700 )
      + RECT via3 ( 4700 -3900 ) ( 4900 -3700 )
      + RECT via3 ( 5100 -3900 ) ( 5300 -3700 )
      + RECT via3 ( 5500 -3900 ) ( 5700 -3700 )
      + RECT via3 ( -5700 -3500 ) ( -5500 -3300 )
      + RECT via3 ( -5300 -3500 ) ( -5100 -3300 )
      + RECT via3 ( -4900 -3500 ) ( -4700 -3300 )
      + RECT via3 ( -4500 -3500 ) ( -4300 -3300 )
      + RECT via3 ( -4100 -3500 ) ( -3900 -3300 )
      + RECT via3 ( -3700 -3500 ) ( -3500 -3300 )
      + RECT via3 ( -3300 -3500 ) ( -3100 -3300 )
      + RECT via3 ( -2900 -3500 ) ( -2700 -3300 )
      + RECT via3 ( -2500 -3500 ) ( -2300 -3300 )
      + RECT via3 ( -2100 -3500 ) ( -1900 -3300 )
      + RECT via3 ( -1700 -3500 ) ( -1500 -3300 )
      + RECT via3 ( -1300 -3500 ) ( -1100 -3300 )
      + RECT via3 ( -900 -3500 ) ( -700 -3300 )
      + RECT via3 ( -500 -3500 ) ( -300 -3300 )
      + RECT via3 ( -100 -3500 ) ( 100 -3300 )
      + RECT via3 ( 300 -3500 ) ( 500 -3300 )
      + RECT via3 ( 700 -3500 ) ( 900 -3300 )
      + RECT via3 ( 1100 -3500 ) ( 1300 -3300 )
      + RECT via3 ( 1500 -3500 ) ( 1700 -3300 )
      + RECT via3 ( 1900 -3500 ) ( 2100 -3300 )
      + RECT via3 ( 2300 -3500 ) ( 2500 -3300 )
      + RECT via3 ( 2700 -3500 ) ( 2900 -3300 )
      + RECT via3 ( 3100 -3500 ) ( 3300 -3300 )
      + RECT via3 ( 3500 -3500 ) ( 3700 -3300 )
      + RECT via3 ( 3900 -3500 ) ( 4100 -3300 )
      + RECT via3 ( 4300 -3500 ) ( 4500 -3300 )
      + RECT via3 ( 4700 -3500 ) ( 4900 -3300 )
      + RECT via3 ( 5100 -3500 ) ( 5300 -3300 )
      + RECT via3 ( 5500 -3500 ) ( 5700 -3300 )
      + RECT via3 ( -5700 -3100 ) ( -5500 -2900 )
      + RECT via3 ( -5300 -3100 ) ( -5100 -2900 )
      + RECT via3 ( -4900 -3100 ) ( -4700 -2900 )
      + RECT via3 ( -4500 -3100 ) ( -4300 -2900 )
      + RECT via3 ( -4100 -3100 ) ( -3900 -2900 )
      + RECT via3 ( -3700 -3100 ) ( -3500 -2900 )
      + RECT via3 ( -3300 -3100 ) ( -3100 -2900 )
      + RECT via3 ( -2900 -3100 ) ( -2700 -2900 )
      + RECT via3 ( -2500 -3100 ) ( -2300 -2900 )
      + RECT via3 ( -2100 -3100 ) ( -1900 -2900 )
      + RECT via3 ( -1700 -3100 ) ( -1500 -2900 )
      + RECT via3 ( -1300 -3100 ) ( -1100 -2900 )
      + RECT via3 ( -900 -3100 ) ( -700 -2900 )
      + RECT via3 ( -500 -3100 ) ( -300 -2900 )
      + RECT via3 ( -100 -3100 ) ( 100 -2900 )
      + RECT via3 ( 300 -3100 ) ( 500 -2900 )
      + RECT via3 ( 700 -3100 ) ( 900 -2900 )
      + RECT via3 ( 1100 -3100 ) ( 1300 -2900 )
      + RECT via3 ( 1500 -3100 ) ( 1700 -2900 )
      + RECT via3 ( 1900 -3100 ) ( 2100 -2900 )
      + RECT via3 ( 2300 -3100 ) ( 2500 -2900 )
      + RECT via3 ( 2700 -3100 ) ( 2900 -2900 )
      + RECT via3 ( 3100 -3100 ) ( 3300 -2900 )
      + RECT via3 ( 3500 -3100 ) ( 3700 -2900 )
      + RECT via3 ( 3900 -3100 ) ( 4100 -2900 )
      + RECT via3 ( 4300 -3100 ) ( 4500 -2900 )
      + RECT via3 ( 4700 -3100 ) ( 4900 -2900 )
      + RECT via3 ( 5100 -3100 ) ( 5300 -2900 )
      + RECT via3 ( 5500 -3100 ) ( 5700 -2900 )
      + RECT via3 ( -5700 -2700 ) ( -5500 -2500 )
      + RECT via3 ( -5300 -2700 ) ( -5100 -2500 )
      + RECT via3 ( -4900 -2700 ) ( -4700 -2500 )
      + RECT via3 ( -4500 -2700 ) ( -4300 -2500 )
      + RECT via3 ( -4100 -2700 ) ( -3900 -2500 )
      + RECT via3 ( -3700 -2700 ) ( -3500 -2500 )
      + RECT via3 ( -3300 -2700 ) ( -3100 -2500 )
      + RECT via3 ( -2900 -2700 ) ( -2700 -2500 )
      + RECT via3 ( -2500 -2700 ) ( -2300 -2500 )
      + RECT via3 ( -2100 -2700 ) ( -1900 -2500 )
      + RECT via3 ( -1700 -2700 ) ( -1500 -2500 )
      + RECT via3 ( -1300 -2700 ) ( -1100 -2500 )
      + RECT via3 ( -900 -2700 ) ( -700 -2500 )
      + RECT via3 ( -500 -2700 ) ( -300 -2500 )
      + RECT via3 ( -100 -2700 ) ( 100 -2500 )
      + RECT via3 ( 300 -2700 ) ( 500 -2500 )
      + RECT via3 ( 700 -2700 ) ( 900 -2500 )
      + RECT via3 ( 1100 -2700 ) ( 1300 -2500 )
      + RECT via3 ( 1500 -2700 ) ( 1700 -2500 )
      + RECT via3 ( 1900 -2700 ) ( 2100 -2500 )
      + RECT via3 ( 2300 -2700 ) ( 2500 -2500 )
      + RECT via3 ( 2700 -2700 ) ( 2900 -2500 )
      + RECT via3 ( 3100 -2700 ) ( 3300 -2500 )
      + RECT via3 ( 3500 -2700 ) ( 3700 -2500 )
      + RECT via3 ( 3900 -2700 ) ( 4100 -2500 )
      + RECT via3 ( 4300 -2700 ) ( 4500 -2500 )
      + RECT via3 ( 4700 -2700 ) ( 4900 -2500 )
      + RECT via3 ( 5100 -2700 ) ( 5300 -2500 )
      + RECT via3 ( 5500 -2700 ) ( 5700 -2500 )
      + RECT via3 ( -5700 -2300 ) ( -5500 -2100 )
      + RECT via3 ( -5300 -2300 ) ( -5100 -2100 )
      + RECT via3 ( -4900 -2300 ) ( -4700 -2100 )
      + RECT via3 ( -4500 -2300 ) ( -4300 -2100 )
      + RECT via3 ( -4100 -2300 ) ( -3900 -2100 )
      + RECT via3 ( -3700 -2300 ) ( -3500 -2100 )
      + RECT via3 ( -3300 -2300 ) ( -3100 -2100 )
      + RECT via3 ( -2900 -2300 ) ( -2700 -2100 )
      + RECT via3 ( -2500 -2300 ) ( -2300 -2100 )
      + RECT via3 ( -2100 -2300 ) ( -1900 -2100 )
      + RECT via3 ( -1700 -2300 ) ( -1500 -2100 )
      + RECT via3 ( -1300 -2300 ) ( -1100 -2100 )
      + RECT via3 ( -900 -2300 ) ( -700 -2100 )
      + RECT via3 ( -500 -2300 ) ( -300 -2100 )
      + RECT via3 ( -100 -2300 ) ( 100 -2100 )
      + RECT via3 ( 300 -2300 ) ( 500 -2100 )
      + RECT via3 ( 700 -2300 ) ( 900 -2100 )
      + RECT via3 ( 1100 -2300 ) ( 1300 -2100 )
      + RECT via3 ( 1500 -2300 ) ( 1700 -2100 )
      + RECT via3 ( 1900 -2300 ) ( 2100 -2100 )
      + RECT via3 ( 2300 -2300 ) ( 2500 -2100 )
      + RECT via3 ( 2700 -2300 ) ( 2900 -2100 )
      + RECT via3 ( 3100 -2300 ) ( 3300 -2100 )
      + RECT via3 ( 3500 -2300 ) ( 3700 -2100 )
      + RECT via3 ( 3900 -2300 ) ( 4100 -2100 )
      + RECT via3 ( 4300 -2300 ) ( 4500 -2100 )
      + RECT via3 ( 4700 -2300 ) ( 4900 -2100 )
      + RECT via3 ( 5100 -2300 ) ( 5300 -2100 )
      + RECT via3 ( 5500 -2300 ) ( 5700 -2100 )
      + RECT via3 ( -5700 -1900 ) ( -5500 -1700 )
      + RECT via3 ( -5300 -1900 ) ( -5100 -1700 )
      + RECT via3 ( -4900 -1900 ) ( -4700 -1700 )
      + RECT via3 ( -4500 -1900 ) ( -4300 -1700 )
      + RECT via3 ( -4100 -1900 ) ( -3900 -1700 )
      + RECT via3 ( -3700 -1900 ) ( -3500 -1700 )
      + RECT via3 ( -3300 -1900 ) ( -3100 -1700 )
      + RECT via3 ( -2900 -1900 ) ( -2700 -1700 )
      + RECT via3 ( -2500 -1900 ) ( -2300 -1700 )
      + RECT via3 ( -2100 -1900 ) ( -1900 -1700 )
      + RECT via3 ( -1700 -1900 ) ( -1500 -1700 )
      + RECT via3 ( -1300 -1900 ) ( -1100 -1700 )
      + RECT via3 ( -900 -1900 ) ( -700 -1700 )
      + RECT via3 ( -500 -1900 ) ( -300 -1700 )
      + RECT via3 ( -100 -1900 ) ( 100 -1700 )
      + RECT via3 ( 300 -1900 ) ( 500 -1700 )
      + RECT via3 ( 700 -1900 ) ( 900 -1700 )
      + RECT via3 ( 1100 -1900 ) ( 1300 -1700 )
      + RECT via3 ( 1500 -1900 ) ( 1700 -1700 )
      + RECT via3 ( 1900 -1900 ) ( 2100 -1700 )
      + RECT via3 ( 2300 -1900 ) ( 2500 -1700 )
      + RECT via3 ( 2700 -1900 ) ( 2900 -1700 )
      + RECT via3 ( 3100 -1900 ) ( 3300 -1700 )
      + RECT via3 ( 3500 -1900 ) ( 3700 -1700 )
      + RECT via3 ( 3900 -1900 ) ( 4100 -1700 )
      + RECT via3 ( 4300 -1900 ) ( 4500 -1700 )
      + RECT via3 ( 4700 -1900 ) ( 4900 -1700 )
      + RECT via3 ( 5100 -1900 ) ( 5300 -1700 )
      + RECT via3 ( 5500 -1900 ) ( 5700 -1700 )
      + RECT via3 ( -5700 -1500 ) ( -5500 -1300 )
      + RECT via3 ( -5300 -1500 ) ( -5100 -1300 )
      + RECT via3 ( -4900 -1500 ) ( -4700 -1300 )
      + RECT via3 ( -4500 -1500 ) ( -4300 -1300 )
      + RECT via3 ( -4100 -1500 ) ( -3900 -1300 )
      + RECT via3 ( -3700 -1500 ) ( -3500 -1300 )
      + RECT via3 ( -3300 -1500 ) ( -3100 -1300 )
      + RECT via3 ( -2900 -1500 ) ( -2700 -1300 )
      + RECT via3 ( -2500 -1500 ) ( -2300 -1300 )
      + RECT via3 ( -2100 -1500 ) ( -1900 -1300 )
      + RECT via3 ( -1700 -1500 ) ( -1500 -1300 )
      + RECT via3 ( -1300 -1500 ) ( -1100 -1300 )
      + RECT via3 ( -900 -1500 ) ( -700 -1300 )
      + RECT via3 ( -500 -1500 ) ( -300 -1300 )
      + RECT via3 ( -100 -1500 ) ( 100 -1300 )
      + RECT via3 ( 300 -1500 ) ( 500 -1300 )
      + RECT via3 ( 700 -1500 ) ( 900 -1300 )
      + RECT via3 ( 1100 -1500 ) ( 1300 -1300 )
      + RECT via3 ( 1500 -1500 ) ( 1700 -1300 )
      + RECT via3 ( 1900 -1500 ) ( 2100 -1300 )
      + RECT via3 ( 2300 -1500 ) ( 2500 -1300 )
      + RECT via3 ( 2700 -1500 ) ( 2900 -1300 )
      + RECT via3 ( 3100 -1500 ) ( 3300 -1300 )
      + RECT via3 ( 3500 -1500 ) ( 3700 -1300 )
      + RECT via3 ( 3900 -1500 ) ( 4100 -1300 )
      + RECT via3 ( 4300 -1500 ) ( 4500 -1300 )
      + RECT via3 ( 4700 -1500 ) ( 4900 -1300 )
      + RECT via3 ( 5100 -1500 ) ( 5300 -1300 )
      + RECT via3 ( 5500 -1500 ) ( 5700 -1300 )
      + RECT via3 ( -5700 -1100 ) ( -5500 -900 )
      + RECT via3 ( -5300 -1100 ) ( -5100 -900 )
      + RECT via3 ( -4900 -1100 ) ( -4700 -900 )
      + RECT via3 ( -4500 -1100 ) ( -4300 -900 )
      + RECT via3 ( -4100 -1100 ) ( -3900 -900 )
      + RECT via3 ( -3700 -1100 ) ( -3500 -900 )
      + RECT via3 ( -3300 -1100 ) ( -3100 -900 )
      + RECT via3 ( -2900 -1100 ) ( -2700 -900 )
      + RECT via3 ( -2500 -1100 ) ( -2300 -900 )
      + RECT via3 ( -2100 -1100 ) ( -1900 -900 )
      + RECT via3 ( -1700 -1100 ) ( -1500 -900 )
      + RECT via3 ( -1300 -1100 ) ( -1100 -900 )
      + RECT via3 ( -900 -1100 ) ( -700 -900 )
      + RECT via3 ( -500 -1100 ) ( -300 -900 )
      + RECT via3 ( -100 -1100 ) ( 100 -900 )
      + RECT via3 ( 300 -1100 ) ( 500 -900 )
      + RECT via3 ( 700 -1100 ) ( 900 -900 )
      + RECT via3 ( 1100 -1100 ) ( 1300 -900 )
      + RECT via3 ( 1500 -1100 ) ( 1700 -900 )
      + RECT via3 ( 1900 -1100 ) ( 2100 -900 )
      + RECT via3 ( 2300 -1100 ) ( 2500 -900 )
      + RECT via3 ( 2700 -1100 ) ( 2900 -900 )
      + RECT via3 ( 3100 -1100 ) ( 3300 -900 )
      + RECT via3 ( 3500 -1100 ) ( 3700 -900 )
      + RECT via3 ( 3900 -1100 ) ( 4100 -900 )
      + RECT via3 ( 4300 -1100 ) ( 4500 -900 )
      + RECT via3 ( 4700 -1100 ) ( 4900 -900 )
      + RECT via3 ( 5100 -1100 ) ( 5300 -900 )
      + RECT via3 ( 5500 -1100 ) ( 5700 -900 )
      + RECT via3 ( -5700 -700 ) ( -5500 -500 )
      + RECT via3 ( -5300 -700 ) ( -5100 -500 )
      + RECT via3 ( -4900 -700 ) ( -4700 -500 )
      + RECT via3 ( -4500 -700 ) ( -4300 -500 )
      + RECT via3 ( -4100 -700 ) ( -3900 -500 )
      + RECT via3 ( -3700 -700 ) ( -3500 -500 )
      + RECT via3 ( -3300 -700 ) ( -3100 -500 )
      + RECT via3 ( -2900 -700 ) ( -2700 -500 )
      + RECT via3 ( -2500 -700 ) ( -2300 -500 )
      + RECT via3 ( -2100 -700 ) ( -1900 -500 )
      + RECT via3 ( -1700 -700 ) ( -1500 -500 )
      + RECT via3 ( -1300 -700 ) ( -1100 -500 )
      + RECT via3 ( -900 -700 ) ( -700 -500 )
      + RECT via3 ( -500 -700 ) ( -300 -500 )
      + RECT via3 ( -100 -700 ) ( 100 -500 )
      + RECT via3 ( 300 -700 ) ( 500 -500 )
      + RECT via3 ( 700 -700 ) ( 900 -500 )
      + RECT via3 ( 1100 -700 ) ( 1300 -500 )
      + RECT via3 ( 1500 -700 ) ( 1700 -500 )
      + RECT via3 ( 1900 -700 ) ( 2100 -500 )
      + RECT via3 ( 2300 -700 ) ( 2500 -500 )
      + RECT via3 ( 2700 -700 ) ( 2900 -500 )
      + RECT via3 ( 3100 -700 ) ( 3300 -500 )
      + RECT via3 ( 3500 -700 ) ( 3700 -500 )
      + RECT via3 ( 3900 -700 ) ( 4100 -500 )
      + RECT via3 ( 4300 -700 ) ( 4500 -500 )
      + RECT via3 ( 4700 -700 ) ( 4900 -500 )
      + RECT via3 ( 5100 -700 ) ( 5300 -500 )
      + RECT via3 ( 5500 -700 ) ( 5700 -500 )
      + RECT via3 ( -5700 -300 ) ( -5500 -100 )
      + RECT via3 ( -5300 -300 ) ( -5100 -100 )
      + RECT via3 ( -4900 -300 ) ( -4700 -100 )
      + RECT via3 ( -4500 -300 ) ( -4300 -100 )
      + RECT via3 ( -4100 -300 ) ( -3900 -100 )
      + RECT via3 ( -3700 -300 ) ( -3500 -100 )
      + RECT via3 ( -3300 -300 ) ( -3100 -100 )
      + RECT via3 ( -2900 -300 ) ( -2700 -100 )
      + RECT via3 ( -2500 -300 ) ( -2300 -100 )
      + RECT via3 ( -2100 -300 ) ( -1900 -100 )
      + RECT via3 ( -1700 -300 ) ( -1500 -100 )
      + RECT via3 ( -1300 -300 ) ( -1100 -100 )
      + RECT via3 ( -900 -300 ) ( -700 -100 )
      + RECT via3 ( -500 -300 ) ( -300 -100 )
      + RECT via3 ( -100 -300 ) ( 100 -100 )
      + RECT via3 ( 300 -300 ) ( 500 -100 )
      + RECT via3 ( 700 -300 ) ( 900 -100 )
      + RECT via3 ( 1100 -300 ) ( 1300 -100 )
      + RECT via3 ( 1500 -300 ) ( 1700 -100 )
      + RECT via3 ( 1900 -300 ) ( 2100 -100 )
      + RECT via3 ( 2300 -300 ) ( 2500 -100 )
      + RECT via3 ( 2700 -300 ) ( 2900 -100 )
      + RECT via3 ( 3100 -300 ) ( 3300 -100 )
      + RECT via3 ( 3500 -300 ) ( 3700 -100 )
      + RECT via3 ( 3900 -300 ) ( 4100 -100 )
      + RECT via3 ( 4300 -300 ) ( 4500 -100 )
      + RECT via3 ( 4700 -300 ) ( 4900 -100 )
      + RECT via3 ( 5100 -300 ) ( 5300 -100 )
      + RECT via3 ( 5500 -300 ) ( 5700 -100 )
      + RECT via3 ( -5700 100 ) ( -5500 300 )
      + RECT via3 ( -5300 100 ) ( -5100 300 )
      + RECT via3 ( -4900 100 ) ( -4700 300 )
      + RECT via3 ( -4500 100 ) ( -4300 300 )
      + RECT via3 ( -4100 100 ) ( -3900 300 )
      + RECT via3 ( -3700 100 ) ( -3500 300 )
      + RECT via3 ( -3300 100 ) ( -3100 300 )
      + RECT via3 ( -2900 100 ) ( -2700 300 )
      + RECT via3 ( -2500 100 ) ( -2300 300 )
      + RECT via3 ( -2100 100 ) ( -1900 300 )
      + RECT via3 ( -1700 100 ) ( -1500 300 )
      + RECT via3 ( -1300 100 ) ( -1100 300 )
      + RECT via3 ( -900 100 ) ( -700 300 )
      + RECT via3 ( -500 100 ) ( -300 300 )
      + RECT via3 ( -100 100 ) ( 100 300 )
      + RECT via3 ( 300 100 ) ( 500 300 )
      + RECT via3 ( 700 100 ) ( 900 300 )
      + RECT via3 ( 1100 100 ) ( 1300 300 )
      + RECT via3 ( 1500 100 ) ( 1700 300 )
      + RECT via3 ( 1900 100 ) ( 2100 300 )
      + RECT via3 ( 2300 100 ) ( 2500 300 )
      + RECT via3 ( 2700 100 ) ( 2900 300 )
      + RECT via3 ( 3100 100 ) ( 3300 300 )
      + RECT via3 ( 3500 100 ) ( 3700 300 )
      + RECT via3 ( 3900 100 ) ( 4100 300 )
      + RECT via3 ( 4300 100 ) ( 4500 300 )
      + RECT via3 ( 4700 100 ) ( 4900 300 )
      + RECT via3 ( 5100 100 ) ( 5300 300 )
      + RECT via3 ( 5500 100 ) ( 5700 300 )
      + RECT via3 ( -5700 500 ) ( -5500 700 )
      + RECT via3 ( -5300 500 ) ( -5100 700 )
      + RECT via3 ( -4900 500 ) ( -4700 700 )
      + RECT via3 ( -4500 500 ) ( -4300 700 )
      + RECT via3 ( -4100 500 ) ( -3900 700 )
      + RECT via3 ( -3700 500 ) ( -3500 700 )
      + RECT via3 ( -3300 500 ) ( -3100 700 )
      + RECT via3 ( -2900 500 ) ( -2700 700 )
      + RECT via3 ( -2500 500 ) ( -2300 700 )
      + RECT via3 ( -2100 500 ) ( -1900 700 )
      + RECT via3 ( -1700 500 ) ( -1500 700 )
      + RECT via3 ( -1300 500 ) ( -1100 700 )
      + RECT via3 ( -900 500 ) ( -700 700 )
      + RECT via3 ( -500 500 ) ( -300 700 )
      + RECT via3 ( -100 500 ) ( 100 700 )
      + RECT via3 ( 300 500 ) ( 500 700 )
      + RECT via3 ( 700 500 ) ( 900 700 )
      + RECT via3 ( 1100 500 ) ( 1300 700 )
      + RECT via3 ( 1500 500 ) ( 1700 700 )
      + RECT via3 ( 1900 500 ) ( 2100 700 )
      + RECT via3 ( 2300 500 ) ( 2500 700 )
      + RECT via3 ( 2700 500 ) ( 2900 700 )
      + RECT via3 ( 3100 500 ) ( 3300 700 )
      + RECT via3 ( 3500 500 ) ( 3700 700 )
      + RECT via3 ( 3900 500 ) ( 4100 700 )
      + RECT via3 ( 4300 500 ) ( 4500 700 )
      + RECT via3 ( 4700 500 ) ( 4900 700 )
      + RECT via3 ( 5100 500 ) ( 5300 700 )
      + RECT via3 ( 5500 500 ) ( 5700 700 )
      + RECT via3 ( -5700 900 ) ( -5500 1100 )
      + RECT via3 ( -5300 900 ) ( -5100 1100 )
      + RECT via3 ( -4900 900 ) ( -4700 1100 )
      + RECT via3 ( -4500 900 ) ( -4300 1100 )
      + RECT via3 ( -4100 900 ) ( -3900 1100 )
      + RECT via3 ( -3700 900 ) ( -3500 1100 )
      + RECT via3 ( -3300 900 ) ( -3100 1100 )
      + RECT via3 ( -2900 900 ) ( -2700 1100 )
      + RECT via3 ( -2500 900 ) ( -2300 1100 )
      + RECT via3 ( -2100 900 ) ( -1900 1100 )
      + RECT via3 ( -1700 900 ) ( -1500 1100 )
      + RECT via3 ( -1300 900 ) ( -1100 1100 )
      + RECT via3 ( -900 900 ) ( -700 1100 )
      + RECT via3 ( -500 900 ) ( -300 1100 )
      + RECT via3 ( -100 900 ) ( 100 1100 )
      + RECT via3 ( 300 900 ) ( 500 1100 )
      + RECT via3 ( 700 900 ) ( 900 1100 )
      + RECT via3 ( 1100 900 ) ( 1300 1100 )
      + RECT via3 ( 1500 900 ) ( 1700 1100 )
      + RECT via3 ( 1900 900 ) ( 2100 1100 )
      + RECT via3 ( 2300 900 ) ( 2500 1100 )
      + RECT via3 ( 2700 900 ) ( 2900 1100 )
      + RECT via3 ( 3100 900 ) ( 3300 1100 )
      + RECT via3 ( 3500 900 ) ( 3700 1100 )
      + RECT via3 ( 3900 900 ) ( 4100 1100 )
      + RECT via3 ( 4300 900 ) ( 4500 1100 )
      + RECT via3 ( 4700 900 ) ( 4900 1100 )
      + RECT via3 ( 5100 900 ) ( 5300 1100 )
      + RECT via3 ( 5500 900 ) ( 5700 1100 )
      + RECT via3 ( -5700 1300 ) ( -5500 1500 )
      + RECT via3 ( -5300 1300 ) ( -5100 1500 )
      + RECT via3 ( -4900 1300 ) ( -4700 1500 )
      + RECT via3 ( -4500 1300 ) ( -4300 1500 )
      + RECT via3 ( -4100 1300 ) ( -3900 1500 )
      + RECT via3 ( -3700 1300 ) ( -3500 1500 )
      + RECT via3 ( -3300 1300 ) ( -3100 1500 )
      + RECT via3 ( -2900 1300 ) ( -2700 1500 )
      + RECT via3 ( -2500 1300 ) ( -2300 1500 )
      + RECT via3 ( -2100 1300 ) ( -1900 1500 )
      + RECT via3 ( -1700 1300 ) ( -1500 1500 )
      + RECT via3 ( -1300 1300 ) ( -1100 1500 )
      + RECT via3 ( -900 1300 ) ( -700 1500 )
      + RECT via3 ( -500 1300 ) ( -300 1500 )
      + RECT via3 ( -100 1300 ) ( 100 1500 )
      + RECT via3 ( 300 1300 ) ( 500 1500 )
      + RECT via3 ( 700 1300 ) ( 900 1500 )
      + RECT via3 ( 1100 1300 ) ( 1300 1500 )
      + RECT via3 ( 1500 1300 ) ( 1700 1500 )
      + RECT via3 ( 1900 1300 ) ( 2100 1500 )
      + RECT via3 ( 2300 1300 ) ( 2500 1500 )
      + RECT via3 ( 2700 1300 ) ( 2900 1500 )
      + RECT via3 ( 3100 1300 ) ( 3300 1500 )
      + RECT via3 ( 3500 1300 ) ( 3700 1500 )
      + RECT via3 ( 3900 1300 ) ( 4100 1500 )
      + RECT via3 ( 4300 1300 ) ( 4500 1500 )
      + RECT via3 ( 4700 1300 ) ( 4900 1500 )
      + RECT via3 ( 5100 1300 ) ( 5300 1500 )
      + RECT via3 ( 5500 1300 ) ( 5700 1500 )
      + RECT via3 ( -5700 1700 ) ( -5500 1900 )
      + RECT via3 ( -5300 1700 ) ( -5100 1900 )
      + RECT via3 ( -4900 1700 ) ( -4700 1900 )
      + RECT via3 ( -4500 1700 ) ( -4300 1900 )
      + RECT via3 ( -4100 1700 ) ( -3900 1900 )
      + RECT via3 ( -3700 1700 ) ( -3500 1900 )
      + RECT via3 ( -3300 1700 ) ( -3100 1900 )
      + RECT via3 ( -2900 1700 ) ( -2700 1900 )
      + RECT via3 ( -2500 1700 ) ( -2300 1900 )
      + RECT via3 ( -2100 1700 ) ( -1900 1900 )
      + RECT via3 ( -1700 1700 ) ( -1500 1900 )
      + RECT via3 ( -1300 1700 ) ( -1100 1900 )
      + RECT via3 ( -900 1700 ) ( -700 1900 )
      + RECT via3 ( -500 1700 ) ( -300 1900 )
      + RECT via3 ( -100 1700 ) ( 100 1900 )
      + RECT via3 ( 300 1700 ) ( 500 1900 )
      + RECT via3 ( 700 1700 ) ( 900 1900 )
      + RECT via3 ( 1100 1700 ) ( 1300 1900 )
      + RECT via3 ( 1500 1700 ) ( 1700 1900 )
      + RECT via3 ( 1900 1700 ) ( 2100 1900 )
      + RECT via3 ( 2300 1700 ) ( 2500 1900 )
      + RECT via3 ( 2700 1700 ) ( 2900 1900 )
      + RECT via3 ( 3100 1700 ) ( 3300 1900 )
      + RECT via3 ( 3500 1700 ) ( 3700 1900 )
      + RECT via3 ( 3900 1700 ) ( 4100 1900 )
      + RECT via3 ( 4300 1700 ) ( 4500 1900 )
      + RECT via3 ( 4700 1700 ) ( 4900 1900 )
      + RECT via3 ( 5100 1700 ) ( 5300 1900 )
      + RECT via3 ( 5500 1700 ) ( 5700 1900 )
      + RECT via3 ( -5700 2100 ) ( -5500 2300 )
      + RECT via3 ( -5300 2100 ) ( -5100 2300 )
      + RECT via3 ( -4900 2100 ) ( -4700 2300 )
      + RECT via3 ( -4500 2100 ) ( -4300 2300 )
      + RECT via3 ( -4100 2100 ) ( -3900 2300 )
      + RECT via3 ( -3700 2100 ) ( -3500 2300 )
      + RECT via3 ( -3300 2100 ) ( -3100 2300 )
      + RECT via3 ( -2900 2100 ) ( -2700 2300 )
      + RECT via3 ( -2500 2100 ) ( -2300 2300 )
      + RECT via3 ( -2100 2100 ) ( -1900 2300 )
      + RECT via3 ( -1700 2100 ) ( -1500 2300 )
      + RECT via3 ( -1300 2100 ) ( -1100 2300 )
      + RECT via3 ( -900 2100 ) ( -700 2300 )
      + RECT via3 ( -500 2100 ) ( -300 2300 )
      + RECT via3 ( -100 2100 ) ( 100 2300 )
      + RECT via3 ( 300 2100 ) ( 500 2300 )
      + RECT via3 ( 700 2100 ) ( 900 2300 )
      + RECT via3 ( 1100 2100 ) ( 1300 2300 )
      + RECT via3 ( 1500 2100 ) ( 1700 2300 )
      + RECT via3 ( 1900 2100 ) ( 2100 2300 )
      + RECT via3 ( 2300 2100 ) ( 2500 2300 )
      + RECT via3 ( 2700 2100 ) ( 2900 2300 )
      + RECT via3 ( 3100 2100 ) ( 3300 2300 )
      + RECT via3 ( 3500 2100 ) ( 3700 2300 )
      + RECT via3 ( 3900 2100 ) ( 4100 2300 )
      + RECT via3 ( 4300 2100 ) ( 4500 2300 )
      + RECT via3 ( 4700 2100 ) ( 4900 2300 )
      + RECT via3 ( 5100 2100 ) ( 5300 2300 )
      + RECT via3 ( 5500 2100 ) ( 5700 2300 )
      + RECT via3 ( -5700 2500 ) ( -5500 2700 )
      + RECT via3 ( -5300 2500 ) ( -5100 2700 )
      + RECT via3 ( -4900 2500 ) ( -4700 2700 )
      + RECT via3 ( -4500 2500 ) ( -4300 2700 )
      + RECT via3 ( -4100 2500 ) ( -3900 2700 )
      + RECT via3 ( -3700 2500 ) ( -3500 2700 )
      + RECT via3 ( -3300 2500 ) ( -3100 2700 )
      + RECT via3 ( -2900 2500 ) ( -2700 2700 )
      + RECT via3 ( -2500 2500 ) ( -2300 2700 )
      + RECT via3 ( -2100 2500 ) ( -1900 2700 )
      + RECT via3 ( -1700 2500 ) ( -1500 2700 )
      + RECT via3 ( -1300 2500 ) ( -1100 2700 )
      + RECT via3 ( -900 2500 ) ( -700 2700 )
      + RECT via3 ( -500 2500 ) ( -300 2700 )
      + RECT via3 ( -100 2500 ) ( 100 2700 )
      + RECT via3 ( 300 2500 ) ( 500 2700 )
      + RECT via3 ( 700 2500 ) ( 900 2700 )
      + RECT via3 ( 1100 2500 ) ( 1300 2700 )
      + RECT via3 ( 1500 2500 ) ( 1700 2700 )
      + RECT via3 ( 1900 2500 ) ( 2100 2700 )
      + RECT via3 ( 2300 2500 ) ( 2500 2700 )
      + RECT via3 ( 2700 2500 ) ( 2900 2700 )
      + RECT via3 ( 3100 2500 ) ( 3300 2700 )
      + RECT via3 ( 3500 2500 ) ( 3700 2700 )
      + RECT via3 ( 3900 2500 ) ( 4100 2700 )
      + RECT via3 ( 4300 2500 ) ( 4500 2700 )
      + RECT via3 ( 4700 2500 ) ( 4900 2700 )
      + RECT via3 ( 5100 2500 ) ( 5300 2700 )
      + RECT via3 ( 5500 2500 ) ( 5700 2700 )
      + RECT via3 ( -5700 2900 ) ( -5500 3100 )
      + RECT via3 ( -5300 2900 ) ( -5100 3100 )
      + RECT via3 ( -4900 2900 ) ( -4700 3100 )
      + RECT via3 ( -4500 2900 ) ( -4300 3100 )
      + RECT via3 ( -4100 2900 ) ( -3900 3100 )
      + RECT via3 ( -3700 2900 ) ( -3500 3100 )
      + RECT via3 ( -3300 2900 ) ( -3100 3100 )
      + RECT via3 ( -2900 2900 ) ( -2700 3100 )
      + RECT via3 ( -2500 2900 ) ( -2300 3100 )
      + RECT via3 ( -2100 2900 ) ( -1900 3100 )
      + RECT via3 ( -1700 2900 ) ( -1500 3100 )
      + RECT via3 ( -1300 2900 ) ( -1100 3100 )
      + RECT via3 ( -900 2900 ) ( -700 3100 )
      + RECT via3 ( -500 2900 ) ( -300 3100 )
      + RECT via3 ( -100 2900 ) ( 100 3100 )
      + RECT via3 ( 300 2900 ) ( 500 3100 )
      + RECT via3 ( 700 2900 ) ( 900 3100 )
      + RECT via3 ( 1100 2900 ) ( 1300 3100 )
      + RECT via3 ( 1500 2900 ) ( 1700 3100 )
      + RECT via3 ( 1900 2900 ) ( 2100 3100 )
      + RECT via3 ( 2300 2900 ) ( 2500 3100 )
      + RECT via3 ( 2700 2900 ) ( 2900 3100 )
      + RECT via3 ( 3100 2900 ) ( 3300 3100 )
      + RECT via3 ( 3500 2900 ) ( 3700 3100 )
      + RECT via3 ( 3900 2900 ) ( 4100 3100 )
      + RECT via3 ( 4300 2900 ) ( 4500 3100 )
      + RECT via3 ( 4700 2900 ) ( 4900 3100 )
      + RECT via3 ( 5100 2900 ) ( 5300 3100 )
      + RECT via3 ( 5500 2900 ) ( 5700 3100 )
      + RECT via3 ( -5700 3300 ) ( -5500 3500 )
      + RECT via3 ( -5300 3300 ) ( -5100 3500 )
      + RECT via3 ( -4900 3300 ) ( -4700 3500 )
      + RECT via3 ( -4500 3300 ) ( -4300 3500 )
      + RECT via3 ( -4100 3300 ) ( -3900 3500 )
      + RECT via3 ( -3700 3300 ) ( -3500 3500 )
      + RECT via3 ( -3300 3300 ) ( -3100 3500 )
      + RECT via3 ( -2900 3300 ) ( -2700 3500 )
      + RECT via3 ( -2500 3300 ) ( -2300 3500 )
      + RECT via3 ( -2100 3300 ) ( -1900 3500 )
      + RECT via3 ( -1700 3300 ) ( -1500 3500 )
      + RECT via3 ( -1300 3300 ) ( -1100 3500 )
      + RECT via3 ( -900 3300 ) ( -700 3500 )
      + RECT via3 ( -500 3300 ) ( -300 3500 )
      + RECT via3 ( -100 3300 ) ( 100 3500 )
      + RECT via3 ( 300 3300 ) ( 500 3500 )
      + RECT via3 ( 700 3300 ) ( 900 3500 )
      + RECT via3 ( 1100 3300 ) ( 1300 3500 )
      + RECT via3 ( 1500 3300 ) ( 1700 3500 )
      + RECT via3 ( 1900 3300 ) ( 2100 3500 )
      + RECT via3 ( 2300 3300 ) ( 2500 3500 )
      + RECT via3 ( 2700 3300 ) ( 2900 3500 )
      + RECT via3 ( 3100 3300 ) ( 3300 3500 )
      + RECT via3 ( 3500 3300 ) ( 3700 3500 )
      + RECT via3 ( 3900 3300 ) ( 4100 3500 )
      + RECT via3 ( 4300 3300 ) ( 4500 3500 )
      + RECT via3 ( 4700 3300 ) ( 4900 3500 )
      + RECT via3 ( 5100 3300 ) ( 5300 3500 )
      + RECT via3 ( 5500 3300 ) ( 5700 3500 )
      + RECT via3 ( -5700 3700 ) ( -5500 3900 )
      + RECT via3 ( -5300 3700 ) ( -5100 3900 )
      + RECT via3 ( -4900 3700 ) ( -4700 3900 )
      + RECT via3 ( -4500 3700 ) ( -4300 3900 )
      + RECT via3 ( -4100 3700 ) ( -3900 3900 )
      + RECT via3 ( -3700 3700 ) ( -3500 3900 )
      + RECT via3 ( -3300 3700 ) ( -3100 3900 )
      + RECT via3 ( -2900 3700 ) ( -2700 3900 )
      + RECT via3 ( -2500 3700 ) ( -2300 3900 )
      + RECT via3 ( -2100 3700 ) ( -1900 3900 )
      + RECT via3 ( -1700 3700 ) ( -1500 3900 )
      + RECT via3 ( -1300 3700 ) ( -1100 3900 )
      + RECT via3 ( -900 3700 ) ( -700 3900 )
      + RECT via3 ( -500 3700 ) ( -300 3900 )
      + RECT via3 ( -100 3700 ) ( 100 3900 )
      + RECT via3 ( 300 3700 ) ( 500 3900 )
      + RECT via3 ( 700 3700 ) ( 900 3900 )
      + RECT via3 ( 1100 3700 ) ( 1300 3900 )
      + RECT via3 ( 1500 3700 ) ( 1700 3900 )
      + RECT via3 ( 1900 3700 ) ( 2100 3900 )
      + RECT via3 ( 2300 3700 ) ( 2500 3900 )
      + RECT via3 ( 2700 3700 ) ( 2900 3900 )
      + RECT via3 ( 3100 3700 ) ( 3300 3900 )
      + RECT via3 ( 3500 3700 ) ( 3700 3900 )
      + RECT via3 ( 3900 3700 ) ( 4100 3900 )
      + RECT via3 ( 4300 3700 ) ( 4500 3900 )
      + RECT via3 ( 4700 3700 ) ( 4900 3900 )
      + RECT via3 ( 5100 3700 ) ( 5300 3900 )
      + RECT via3 ( 5500 3700 ) ( 5700 3900 )
      + RECT via3 ( -5700 4100 ) ( -5500 4300 )
      + RECT via3 ( -5300 4100 ) ( -5100 4300 )
      + RECT via3 ( -4900 4100 ) ( -4700 4300 )
      + RECT via3 ( -4500 4100 ) ( -4300 4300 )
      + RECT via3 ( -4100 4100 ) ( -3900 4300 )
      + RECT via3 ( -3700 4100 ) ( -3500 4300 )
      + RECT via3 ( -3300 4100 ) ( -3100 4300 )
      + RECT via3 ( -2900 4100 ) ( -2700 4300 )
      + RECT via3 ( -2500 4100 ) ( -2300 4300 )
      + RECT via3 ( -2100 4100 ) ( -1900 4300 )
      + RECT via3 ( -1700 4100 ) ( -1500 4300 )
      + RECT via3 ( -1300 4100 ) ( -1100 4300 )
      + RECT via3 ( -900 4100 ) ( -700 4300 )
      + RECT via3 ( -500 4100 ) ( -300 4300 )
      + RECT via3 ( -100 4100 ) ( 100 4300 )
      + RECT via3 ( 300 4100 ) ( 500 4300 )
      + RECT via3 ( 700 4100 ) ( 900 4300 )
      + RECT via3 ( 1100 4100 ) ( 1300 4300 )
      + RECT via3 ( 1500 4100 ) ( 1700 4300 )
      + RECT via3 ( 1900 4100 ) ( 2100 4300 )
      + RECT via3 ( 2300 4100 ) ( 2500 4300 )
      + RECT via3 ( 2700 4100 ) ( 2900 4300 )
      + RECT via3 ( 3100 4100 ) ( 3300 4300 )
      + RECT via3 ( 3500 4100 ) ( 3700 4300 )
      + RECT via3 ( 3900 4100 ) ( 4100 4300 )
      + RECT via3 ( 4300 4100 ) ( 4500 4300 )
      + RECT via3 ( 4700 4100 ) ( 4900 4300 )
      + RECT via3 ( 5100 4100 ) ( 5300 4300 )
      + RECT via3 ( 5500 4100 ) ( 5700 4300 )
      + RECT via3 ( -5700 4500 ) ( -5500 4700 )
      + RECT via3 ( -5300 4500 ) ( -5100 4700 )
      + RECT via3 ( -4900 4500 ) ( -4700 4700 )
      + RECT via3 ( -4500 4500 ) ( -4300 4700 )
      + RECT via3 ( -4100 4500 ) ( -3900 4700 )
      + RECT via3 ( -3700 4500 ) ( -3500 4700 )
      + RECT via3 ( -3300 4500 ) ( -3100 4700 )
      + RECT via3 ( -2900 4500 ) ( -2700 4700 )
      + RECT via3 ( -2500 4500 ) ( -2300 4700 )
      + RECT via3 ( -2100 4500 ) ( -1900 4700 )
      + RECT via3 ( -1700 4500 ) ( -1500 4700 )
      + RECT via3 ( -1300 4500 ) ( -1100 4700 )
      + RECT via3 ( -900 4500 ) ( -700 4700 )
      + RECT via3 ( -500 4500 ) ( -300 4700 )
      + RECT via3 ( -100 4500 ) ( 100 4700 )
      + RECT via3 ( 300 4500 ) ( 500 4700 )
      + RECT via3 ( 700 4500 ) ( 900 4700 )
      + RECT via3 ( 1100 4500 ) ( 1300 4700 )
      + RECT via3 ( 1500 4500 ) ( 1700 4700 )
      + RECT via3 ( 1900 4500 ) ( 2100 4700 )
      + RECT via3 ( 2300 4500 ) ( 2500 4700 )
      + RECT via3 ( 2700 4500 ) ( 2900 4700 )
      + RECT via3 ( 3100 4500 ) ( 3300 4700 )
      + RECT via3 ( 3500 4500 ) ( 3700 4700 )
      + RECT via3 ( 3900 4500 ) ( 4100 4700 )
      + RECT via3 ( 4300 4500 ) ( 4500 4700 )
      + RECT via3 ( 4700 4500 ) ( 4900 4700 )
      + RECT via3 ( 5100 4500 ) ( 5300 4700 )
      + RECT via3 ( 5500 4500 ) ( 5700 4700 )
      + RECT via3 ( -5700 4900 ) ( -5500 5100 )
      + RECT via3 ( -5300 4900 ) ( -5100 5100 )
      + RECT via3 ( -4900 4900 ) ( -4700 5100 )
      + RECT via3 ( -4500 4900 ) ( -4300 5100 )
      + RECT via3 ( -4100 4900 ) ( -3900 5100 )
      + RECT via3 ( -3700 4900 ) ( -3500 5100 )
      + RECT via3 ( -3300 4900 ) ( -3100 5100 )
      + RECT via3 ( -2900 4900 ) ( -2700 5100 )
      + RECT via3 ( -2500 4900 ) ( -2300 5100 )
      + RECT via3 ( -2100 4900 ) ( -1900 5100 )
      + RECT via3 ( -1700 4900 ) ( -1500 5100 )
      + RECT via3 ( -1300 4900 ) ( -1100 5100 )
      + RECT via3 ( -900 4900 ) ( -700 5100 )
      + RECT via3 ( -500 4900 ) ( -300 5100 )
      + RECT via3 ( -100 4900 ) ( 100 5100 )
      + RECT via3 ( 300 4900 ) ( 500 5100 )
      + RECT via3 ( 700 4900 ) ( 900 5100 )
      + RECT via3 ( 1100 4900 ) ( 1300 5100 )
      + RECT via3 ( 1500 4900 ) ( 1700 5100 )
      + RECT via3 ( 1900 4900 ) ( 2100 5100 )
      + RECT via3 ( 2300 4900 ) ( 2500 5100 )
      + RECT via3 ( 2700 4900 ) ( 2900 5100 )
      + RECT via3 ( 3100 4900 ) ( 3300 5100 )
      + RECT via3 ( 3500 4900 ) ( 3700 5100 )
      + RECT via3 ( 3900 4900 ) ( 4100 5100 )
      + RECT via3 ( 4300 4900 ) ( 4500 5100 )
      + RECT via3 ( 4700 4900 ) ( 4900 5100 )
      + RECT via3 ( 5100 4900 ) ( 5300 5100 )
      + RECT via3 ( 5500 4900 ) ( 5700 5100 )
      + RECT via3 ( -5700 5300 ) ( -5500 5500 )
      + RECT via3 ( -5300 5300 ) ( -5100 5500 )
      + RECT via3 ( -4900 5300 ) ( -4700 5500 )
      + RECT via3 ( -4500 5300 ) ( -4300 5500 )
      + RECT via3 ( -4100 5300 ) ( -3900 5500 )
      + RECT via3 ( -3700 5300 ) ( -3500 5500 )
      + RECT via3 ( -3300 5300 ) ( -3100 5500 )
      + RECT via3 ( -2900 5300 ) ( -2700 5500 )
      + RECT via3 ( -2500 5300 ) ( -2300 5500 )
      + RECT via3 ( -2100 5300 ) ( -1900 5500 )
      + RECT via3 ( -1700 5300 ) ( -1500 5500 )
      + RECT via3 ( -1300 5300 ) ( -1100 5500 )
      + RECT via3 ( -900 5300 ) ( -700 5500 )
      + RECT via3 ( -500 5300 ) ( -300 5500 )
      + RECT via3 ( -100 5300 ) ( 100 5500 )
      + RECT via3 ( 300 5300 ) ( 500 5500 )
      + RECT via3 ( 700 5300 ) ( 900 5500 )
      + RECT via3 ( 1100 5300 ) ( 1300 5500 )
      + RECT via3 ( 1500 5300 ) ( 1700 5500 )
      + RECT via3 ( 1900 5300 ) ( 2100 5500 )
      + RECT via3 ( 2300 5300 ) ( 2500 5500 )
      + RECT via3 ( 2700 5300 ) ( 2900 5500 )
      + RECT via3 ( 3100 5300 ) ( 3300 5500 )
      + RECT via3 ( 3500 5300 ) ( 3700 5500 )
      + RECT via3 ( 3900 5300 ) ( 4100 5500 )
      + RECT via3 ( 4300 5300 ) ( 4500 5500 )
      + RECT via3 ( 4700 5300 ) ( 4900 5500 )
      + RECT via3 ( 5100 5300 ) ( 5300 5500 )
      + RECT via3 ( 5500 5300 ) ( 5700 5500 )
      + RECT via3 ( -5700 5700 ) ( -5500 5900 )
      + RECT via3 ( -5300 5700 ) ( -5100 5900 )
      + RECT via3 ( -4900 5700 ) ( -4700 5900 )
      + RECT via3 ( -4500 5700 ) ( -4300 5900 )
      + RECT via3 ( -4100 5700 ) ( -3900 5900 )
      + RECT via3 ( -3700 5700 ) ( -3500 5900 )
      + RECT via3 ( -3300 5700 ) ( -3100 5900 )
      + RECT via3 ( -2900 5700 ) ( -2700 5900 )
      + RECT via3 ( -2500 5700 ) ( -2300 5900 )
      + RECT via3 ( -2100 5700 ) ( -1900 5900 )
      + RECT via3 ( -1700 5700 ) ( -1500 5900 )
      + RECT via3 ( -1300 5700 ) ( -1100 5900 )
      + RECT via3 ( -900 5700 ) ( -700 5900 )
      + RECT via3 ( -500 5700 ) ( -300 5900 )
      + RECT via3 ( -100 5700 ) ( 100 5900 )
      + RECT via3 ( 300 5700 ) ( 500 5900 )
      + RECT via3 ( 700 5700 ) ( 900 5900 )
      + RECT via3 ( 1100 5700 ) ( 1300 5900 )
      + RECT via3 ( 1500 5700 ) ( 1700 5900 )
      + RECT via3 ( 1900 5700 ) ( 2100 5900 )
      + RECT via3 ( 2300 5700 ) ( 2500 5900 )
      + RECT via3 ( 2700 5700 ) ( 2900 5900 )
      + RECT via3 ( 3100 5700 ) ( 3300 5900 )
      + RECT via3 ( 3500 5700 ) ( 3700 5900 )
      + RECT via3 ( 3900 5700 ) ( 4100 5900 )
      + RECT via3 ( 4300 5700 ) ( 4500 5900 )
      + RECT via3 ( 4700 5700 ) ( 4900 5900 )
      + RECT via3 ( 5100 5700 ) ( 5300 5900 )
      + RECT via3 ( 5500 5700 ) ( 5700 5900 )
      + RECT via3 ( -5700 6100 ) ( -5500 6300 )
      + RECT via3 ( -5300 6100 ) ( -5100 6300 )
      + RECT via3 ( -4900 6100 ) ( -4700 6300 )
      + RECT via3 ( -4500 6100 ) ( -4300 6300 )
      + RECT via3 ( -4100 6100 ) ( -3900 6300 )
      + RECT via3 ( -3700 6100 ) ( -3500 6300 )
      + RECT via3 ( -3300 6100 ) ( -3100 6300 )
      + RECT via3 ( -2900 6100 ) ( -2700 6300 )
      + RECT via3 ( -2500 6100 ) ( -2300 6300 )
      + RECT via3 ( -2100 6100 ) ( -1900 6300 )
      + RECT via3 ( -1700 6100 ) ( -1500 6300 )
      + RECT via3 ( -1300 6100 ) ( -1100 6300 )
      + RECT via3 ( -900 6100 ) ( -700 6300 )
      + RECT via3 ( -500 6100 ) ( -300 6300 )
      + RECT via3 ( -100 6100 ) ( 100 6300 )
      + RECT via3 ( 300 6100 ) ( 500 6300 )
      + RECT via3 ( 700 6100 ) ( 900 6300 )
      + RECT via3 ( 1100 6100 ) ( 1300 6300 )
      + RECT via3 ( 1500 6100 ) ( 1700 6300 )
      + RECT via3 ( 1900 6100 ) ( 2100 6300 )
      + RECT via3 ( 2300 6100 ) ( 2500 6300 )
      + RECT via3 ( 2700 6100 ) ( 2900 6300 )
      + RECT via3 ( 3100 6100 ) ( 3300 6300 )
      + RECT via3 ( 3500 6100 ) ( 3700 6300 )
      + RECT via3 ( 3900 6100 ) ( 4100 6300 )
      + RECT via3 ( 4300 6100 ) ( 4500 6300 )
      + RECT via3 ( 4700 6100 ) ( 4900 6300 )
      + RECT via3 ( 5100 6100 ) ( 5300 6300 )
      + RECT via3 ( 5500 6100 ) ( 5700 6300 )
      + RECT via3 ( -5700 6500 ) ( -5500 6700 )
      + RECT via3 ( -5300 6500 ) ( -5100 6700 )
      + RECT via3 ( -4900 6500 ) ( -4700 6700 )
      + RECT via3 ( -4500 6500 ) ( -4300 6700 )
      + RECT via3 ( -4100 6500 ) ( -3900 6700 )
      + RECT via3 ( -3700 6500 ) ( -3500 6700 )
      + RECT via3 ( -3300 6500 ) ( -3100 6700 )
      + RECT via3 ( -2900 6500 ) ( -2700 6700 )
      + RECT via3 ( -2500 6500 ) ( -2300 6700 )
      + RECT via3 ( -2100 6500 ) ( -1900 6700 )
      + RECT via3 ( -1700 6500 ) ( -1500 6700 )
      + RECT via3 ( -1300 6500 ) ( -1100 6700 )
      + RECT via3 ( -900 6500 ) ( -700 6700 )
      + RECT via3 ( -500 6500 ) ( -300 6700 )
      + RECT via3 ( -100 6500 ) ( 100 6700 )
      + RECT via3 ( 300 6500 ) ( 500 6700 )
      + RECT via3 ( 700 6500 ) ( 900 6700 )
      + RECT via3 ( 1100 6500 ) ( 1300 6700 )
      + RECT via3 ( 1500 6500 ) ( 1700 6700 )
      + RECT via3 ( 1900 6500 ) ( 2100 6700 )
      + RECT via3 ( 2300 6500 ) ( 2500 6700 )
      + RECT via3 ( 2700 6500 ) ( 2900 6700 )
      + RECT via3 ( 3100 6500 ) ( 3300 6700 )
      + RECT via3 ( 3500 6500 ) ( 3700 6700 )
      + RECT via3 ( 3900 6500 ) ( 4100 6700 )
      + RECT via3 ( 4300 6500 ) ( 4500 6700 )
      + RECT via3 ( 4700 6500 ) ( 4900 6700 )
      + RECT via3 ( 5100 6500 ) ( 5300 6700 )
      + RECT via3 ( 5500 6500 ) ( 5700 6700 )
      + RECT via3 ( -5700 6900 ) ( -5500 7100 )
      + RECT via3 ( -5300 6900 ) ( -5100 7100 )
      + RECT via3 ( -4900 6900 ) ( -4700 7100 )
      + RECT via3 ( -4500 6900 ) ( -4300 7100 )
      + RECT via3 ( -4100 6900 ) ( -3900 7100 )
      + RECT via3 ( -3700 6900 ) ( -3500 7100 )
      + RECT via3 ( -3300 6900 ) ( -3100 7100 )
      + RECT via3 ( -2900 6900 ) ( -2700 7100 )
      + RECT via3 ( -2500 6900 ) ( -2300 7100 )
      + RECT via3 ( -2100 6900 ) ( -1900 7100 )
      + RECT via3 ( -1700 6900 ) ( -1500 7100 )
      + RECT via3 ( -1300 6900 ) ( -1100 7100 )
      + RECT via3 ( -900 6900 ) ( -700 7100 )
      + RECT via3 ( -500 6900 ) ( -300 7100 )
      + RECT via3 ( -100 6900 ) ( 100 7100 )
      + RECT via3 ( 300 6900 ) ( 500 7100 )
      + RECT via3 ( 700 6900 ) ( 900 7100 )
      + RECT via3 ( 1100 6900 ) ( 1300 7100 )
      + RECT via3 ( 1500 6900 ) ( 1700 7100 )
      + RECT via3 ( 1900 6900 ) ( 2100 7100 )
      + RECT via3 ( 2300 6900 ) ( 2500 7100 )
      + RECT via3 ( 2700 6900 ) ( 2900 7100 )
      + RECT via3 ( 3100 6900 ) ( 3300 7100 )
      + RECT via3 ( 3500 6900 ) ( 3700 7100 )
      + RECT via3 ( 3900 6900 ) ( 4100 7100 )
      + RECT via3 ( 4300 6900 ) ( 4500 7100 )
      + RECT via3 ( 4700 6900 ) ( 4900 7100 )
      + RECT via3 ( 5100 6900 ) ( 5300 7100 )
      + RECT via3 ( 5500 6900 ) ( 5700 7100 )
      + RECT via3 ( -5700 7300 ) ( -5500 7500 )
      + RECT via3 ( -5300 7300 ) ( -5100 7500 )
      + RECT via3 ( -4900 7300 ) ( -4700 7500 )
      + RECT via3 ( -4500 7300 ) ( -4300 7500 )
      + RECT via3 ( -4100 7300 ) ( -3900 7500 )
      + RECT via3 ( -3700 7300 ) ( -3500 7500 )
      + RECT via3 ( -3300 7300 ) ( -3100 7500 )
      + RECT via3 ( -2900 7300 ) ( -2700 7500 )
      + RECT via3 ( -2500 7300 ) ( -2300 7500 )
      + RECT via3 ( -2100 7300 ) ( -1900 7500 )
      + RECT via3 ( -1700 7300 ) ( -1500 7500 )
      + RECT via3 ( -1300 7300 ) ( -1100 7500 )
      + RECT via3 ( -900 7300 ) ( -700 7500 )
      + RECT via3 ( -500 7300 ) ( -300 7500 )
      + RECT via3 ( -100 7300 ) ( 100 7500 )
      + RECT via3 ( 300 7300 ) ( 500 7500 )
      + RECT via3 ( 700 7300 ) ( 900 7500 )
      + RECT via3 ( 1100 7300 ) ( 1300 7500 )
      + RECT via3 ( 1500 7300 ) ( 1700 7500 )
      + RECT via3 ( 1900 7300 ) ( 2100 7500 )
      + RECT via3 ( 2300 7300 ) ( 2500 7500 )
      + RECT via3 ( 2700 7300 ) ( 2900 7500 )
      + RECT via3 ( 3100 7300 ) ( 3300 7500 )
      + RECT via3 ( 3500 7300 ) ( 3700 7500 )
      + RECT via3 ( 3900 7300 ) ( 4100 7500 )
      + RECT via3 ( 4300 7300 ) ( 4500 7500 )
      + RECT via3 ( 4700 7300 ) ( 4900 7500 )
      + RECT via3 ( 5100 7300 ) ( 5300 7500 )
      + RECT via3 ( 5500 7300 ) ( 5700 7500 )
      + RECT via3 ( -5700 7700 ) ( -5500 7900 )
      + RECT via3 ( -5300 7700 ) ( -5100 7900 )
      + RECT via3 ( -4900 7700 ) ( -4700 7900 )
      + RECT via3 ( -4500 7700 ) ( -4300 7900 )
      + RECT via3 ( -4100 7700 ) ( -3900 7900 )
      + RECT via3 ( -3700 7700 ) ( -3500 7900 )
      + RECT via3 ( -3300 7700 ) ( -3100 7900 )
      + RECT via3 ( -2900 7700 ) ( -2700 7900 )
      + RECT via3 ( -2500 7700 ) ( -2300 7900 )
      + RECT via3 ( -2100 7700 ) ( -1900 7900 )
      + RECT via3 ( -1700 7700 ) ( -1500 7900 )
      + RECT via3 ( -1300 7700 ) ( -1100 7900 )
      + RECT via3 ( -900 7700 ) ( -700 7900 )
      + RECT via3 ( -500 7700 ) ( -300 7900 )
      + RECT via3 ( -100 7700 ) ( 100 7900 )
      + RECT via3 ( 300 7700 ) ( 500 7900 )
      + RECT via3 ( 700 7700 ) ( 900 7900 )
      + RECT via3 ( 1100 7700 ) ( 1300 7900 )
      + RECT via3 ( 1500 7700 ) ( 1700 7900 )
      + RECT via3 ( 1900 7700 ) ( 2100 7900 )
      + RECT via3 ( 2300 7700 ) ( 2500 7900 )
      + RECT via3 ( 2700 7700 ) ( 2900 7900 )
      + RECT via3 ( 3100 7700 ) ( 3300 7900 )
      + RECT via3 ( 3500 7700 ) ( 3700 7900 )
      + RECT via3 ( 3900 7700 ) ( 4100 7900 )
      + RECT via3 ( 4300 7700 ) ( 4500 7900 )
      + RECT via3 ( 4700 7700 ) ( 4900 7900 )
      + RECT via3 ( 5100 7700 ) ( 5300 7900 )
      + RECT via3 ( 5500 7700 ) ( 5700 7900 )
      + RECT via3 ( -5700 8100 ) ( -5500 8300 )
      + RECT via3 ( -5300 8100 ) ( -5100 8300 )
      + RECT via3 ( -4900 8100 ) ( -4700 8300 )
      + RECT via3 ( -4500 8100 ) ( -4300 8300 )
      + RECT via3 ( -4100 8100 ) ( -3900 8300 )
      + RECT via3 ( -3700 8100 ) ( -3500 8300 )
      + RECT via3 ( -3300 8100 ) ( -3100 8300 )
      + RECT via3 ( -2900 8100 ) ( -2700 8300 )
      + RECT via3 ( -2500 8100 ) ( -2300 8300 )
      + RECT via3 ( -2100 8100 ) ( -1900 8300 )
      + RECT via3 ( -1700 8100 ) ( -1500 8300 )
      + RECT via3 ( -1300 8100 ) ( -1100 8300 )
      + RECT via3 ( -900 8100 ) ( -700 8300 )
      + RECT via3 ( -500 8100 ) ( -300 8300 )
      + RECT via3 ( -100 8100 ) ( 100 8300 )
      + RECT via3 ( 300 8100 ) ( 500 8300 )
      + RECT via3 ( 700 8100 ) ( 900 8300 )
      + RECT via3 ( 1100 8100 ) ( 1300 8300 )
      + RECT via3 ( 1500 8100 ) ( 1700 8300 )
      + RECT via3 ( 1900 8100 ) ( 2100 8300 )
      + RECT via3 ( 2300 8100 ) ( 2500 8300 )
      + RECT via3 ( 2700 8100 ) ( 2900 8300 )
      + RECT via3 ( 3100 8100 ) ( 3300 8300 )
      + RECT via3 ( 3500 8100 ) ( 3700 8300 )
      + RECT via3 ( 3900 8100 ) ( 4100 8300 )
      + RECT via3 ( 4300 8100 ) ( 4500 8300 )
      + RECT via3 ( 4700 8100 ) ( 4900 8300 )
      + RECT via3 ( 5100 8100 ) ( 5300 8300 )
      + RECT via3 ( 5500 8100 ) ( 5700 8300 )
      + RECT via3 ( -5700 8500 ) ( -5500 8700 )
      + RECT via3 ( -5300 8500 ) ( -5100 8700 )
      + RECT via3 ( -4900 8500 ) ( -4700 8700 )
      + RECT via3 ( -4500 8500 ) ( -4300 8700 )
      + RECT via3 ( -4100 8500 ) ( -3900 8700 )
      + RECT via3 ( -3700 8500 ) ( -3500 8700 )
      + RECT via3 ( -3300 8500 ) ( -3100 8700 )
      + RECT via3 ( -2900 8500 ) ( -2700 8700 )
      + RECT via3 ( -2500 8500 ) ( -2300 8700 )
      + RECT via3 ( -2100 8500 ) ( -1900 8700 )
      + RECT via3 ( -1700 8500 ) ( -1500 8700 )
      + RECT via3 ( -1300 8500 ) ( -1100 8700 )
      + RECT via3 ( -900 8500 ) ( -700 8700 )
      + RECT via3 ( -500 8500 ) ( -300 8700 )
      + RECT via3 ( -100 8500 ) ( 100 8700 )
      + RECT via3 ( 300 8500 ) ( 500 8700 )
      + RECT via3 ( 700 8500 ) ( 900 8700 )
      + RECT via3 ( 1100 8500 ) ( 1300 8700 )
      + RECT via3 ( 1500 8500 ) ( 1700 8700 )
      + RECT via3 ( 1900 8500 ) ( 2100 8700 )
      + RECT via3 ( 2300 8500 ) ( 2500 8700 )
      + RECT via3 ( 2700 8500 ) ( 2900 8700 )
      + RECT via3 ( 3100 8500 ) ( 3300 8700 )
      + RECT via3 ( 3500 8500 ) ( 3700 8700 )
      + RECT via3 ( 3900 8500 ) ( 4100 8700 )
      + RECT via3 ( 4300 8500 ) ( 4500 8700 )
      + RECT via3 ( 4700 8500 ) ( 4900 8700 )
      + RECT via3 ( 5100 8500 ) ( 5300 8700 )
      + RECT via3 ( 5500 8500 ) ( 5700 8700 )
      + RECT via3 ( -5700 8900 ) ( -5500 9100 )
      + RECT via3 ( -5300 8900 ) ( -5100 9100 )
      + RECT via3 ( -4900 8900 ) ( -4700 9100 )
      + RECT via3 ( -4500 8900 ) ( -4300 9100 )
      + RECT via3 ( -4100 8900 ) ( -3900 9100 )
      + RECT via3 ( -3700 8900 ) ( -3500 9100 )
      + RECT via3 ( -3300 8900 ) ( -3100 9100 )
      + RECT via3 ( -2900 8900 ) ( -2700 9100 )
      + RECT via3 ( -2500 8900 ) ( -2300 9100 )
      + RECT via3 ( -2100 8900 ) ( -1900 9100 )
      + RECT via3 ( -1700 8900 ) ( -1500 9100 )
      + RECT via3 ( -1300 8900 ) ( -1100 9100 )
      + RECT via3 ( -900 8900 ) ( -700 9100 )
      + RECT via3 ( -500 8900 ) ( -300 9100 )
      + RECT via3 ( -100 8900 ) ( 100 9100 )
      + RECT via3 ( 300 8900 ) ( 500 9100 )
      + RECT via3 ( 700 8900 ) ( 900 9100 )
      + RECT via3 ( 1100 8900 ) ( 1300 9100 )
      + RECT via3 ( 1500 8900 ) ( 1700 9100 )
      + RECT via3 ( 1900 8900 ) ( 2100 9100 )
      + RECT via3 ( 2300 8900 ) ( 2500 9100 )
      + RECT via3 ( 2700 8900 ) ( 2900 9100 )
      + RECT via3 ( 3100 8900 ) ( 3300 9100 )
      + RECT via3 ( 3500 8900 ) ( 3700 9100 )
      + RECT via3 ( 3900 8900 ) ( 4100 9100 )
      + RECT via3 ( 4300 8900 ) ( 4500 9100 )
      + RECT via3 ( 4700 8900 ) ( 4900 9100 )
      + RECT via3 ( 5100 8900 ) ( 5300 9100 )
      + RECT via3 ( 5500 8900 ) ( 5700 9100 )
      + RECT via3 ( -5700 9300 ) ( -5500 9500 )
      + RECT via3 ( -5300 9300 ) ( -5100 9500 )
      + RECT via3 ( -4900 9300 ) ( -4700 9500 )
      + RECT via3 ( -4500 9300 ) ( -4300 9500 )
      + RECT via3 ( -4100 9300 ) ( -3900 9500 )
      + RECT via3 ( -3700 9300 ) ( -3500 9500 )
      + RECT via3 ( -3300 9300 ) ( -3100 9500 )
      + RECT via3 ( -2900 9300 ) ( -2700 9500 )
      + RECT via3 ( -2500 9300 ) ( -2300 9500 )
      + RECT via3 ( -2100 9300 ) ( -1900 9500 )
      + RECT via3 ( -1700 9300 ) ( -1500 9500 )
      + RECT via3 ( -1300 9300 ) ( -1100 9500 )
      + RECT via3 ( -900 9300 ) ( -700 9500 )
      + RECT via3 ( -500 9300 ) ( -300 9500 )
      + RECT via3 ( -100 9300 ) ( 100 9500 )
      + RECT via3 ( 300 9300 ) ( 500 9500 )
      + RECT via3 ( 700 9300 ) ( 900 9500 )
      + RECT via3 ( 1100 9300 ) ( 1300 9500 )
      + RECT via3 ( 1500 9300 ) ( 1700 9500 )
      + RECT via3 ( 1900 9300 ) ( 2100 9500 )
      + RECT via3 ( 2300 9300 ) ( 2500 9500 )
      + RECT via3 ( 2700 9300 ) ( 2900 9500 )
      + RECT via3 ( 3100 9300 ) ( 3300 9500 )
      + RECT via3 ( 3500 9300 ) ( 3700 9500 )
      + RECT via3 ( 3900 9300 ) ( 4100 9500 )
      + RECT via3 ( 4300 9300 ) ( 4500 9500 )
      + RECT via3 ( 4700 9300 ) ( 4900 9500 )
      + RECT via3 ( 5100 9300 ) ( 5300 9500 )
      + RECT via3 ( 5500 9300 ) ( 5700 9500 )
      + RECT via3 ( -5700 9700 ) ( -5500 9900 )
      + RECT via3 ( -5300 9700 ) ( -5100 9900 )
      + RECT via3 ( -4900 9700 ) ( -4700 9900 )
      + RECT via3 ( -4500 9700 ) ( -4300 9900 )
      + RECT via3 ( -4100 9700 ) ( -3900 9900 )
      + RECT via3 ( -3700 9700 ) ( -3500 9900 )
      + RECT via3 ( -3300 9700 ) ( -3100 9900 )
      + RECT via3 ( -2900 9700 ) ( -2700 9900 )
      + RECT via3 ( -2500 9700 ) ( -2300 9900 )
      + RECT via3 ( -2100 9700 ) ( -1900 9900 )
      + RECT via3 ( -1700 9700 ) ( -1500 9900 )
      + RECT via3 ( -1300 9700 ) ( -1100 9900 )
      + RECT via3 ( -900 9700 ) ( -700 9900 )
      + RECT via3 ( -500 9700 ) ( -300 9900 )
      + RECT via3 ( -100 9700 ) ( 100 9900 )
      + RECT via3 ( 300 9700 ) ( 500 9900 )
      + RECT via3 ( 700 9700 ) ( 900 9900 )
      + RECT via3 ( 1100 9700 ) ( 1300 9900 )
      + RECT via3 ( 1500 9700 ) ( 1700 9900 )
      + RECT via3 ( 1900 9700 ) ( 2100 9900 )
      + RECT via3 ( 2300 9700 ) ( 2500 9900 )
      + RECT via3 ( 2700 9700 ) ( 2900 9900 )
      + RECT via3 ( 3100 9700 ) ( 3300 9900 )
      + RECT via3 ( 3500 9700 ) ( 3700 9900 )
      + RECT via3 ( 3900 9700 ) ( 4100 9900 )
      + RECT via3 ( 4300 9700 ) ( 4500 9900 )
      + RECT via3 ( 4700 9700 ) ( 4900 9900 )
      + RECT via3 ( 5100 9700 ) ( 5300 9900 )
      + RECT via3 ( 5500 9700 ) ( 5700 9900 )
      + RECT via3 ( -5700 10100 ) ( -5500 10300 )
      + RECT via3 ( -5300 10100 ) ( -5100 10300 )
      + RECT via3 ( -4900 10100 ) ( -4700 10300 )
      + RECT via3 ( -4500 10100 ) ( -4300 10300 )
      + RECT via3 ( -4100 10100 ) ( -3900 10300 )
      + RECT via3 ( -3700 10100 ) ( -3500 10300 )
      + RECT via3 ( -3300 10100 ) ( -3100 10300 )
      + RECT via3 ( -2900 10100 ) ( -2700 10300 )
      + RECT via3 ( -2500 10100 ) ( -2300 10300 )
      + RECT via3 ( -2100 10100 ) ( -1900 10300 )
      + RECT via3 ( -1700 10100 ) ( -1500 10300 )
      + RECT via3 ( -1300 10100 ) ( -1100 10300 )
      + RECT via3 ( -900 10100 ) ( -700 10300 )
      + RECT via3 ( -500 10100 ) ( -300 10300 )
      + RECT via3 ( -100 10100 ) ( 100 10300 )
      + RECT via3 ( 300 10100 ) ( 500 10300 )
      + RECT via3 ( 700 10100 ) ( 900 10300 )
      + RECT via3 ( 1100 10100 ) ( 1300 10300 )
      + RECT via3 ( 1500 10100 ) ( 1700 10300 )
      + RECT via3 ( 1900 10100 ) ( 2100 10300 )
      + RECT via3 ( 2300 10100 ) ( 2500 10300 )
      + RECT via3 ( 2700 10100 ) ( 2900 10300 )
      + RECT via3 ( 3100 10100 ) ( 3300 10300 )
      + RECT via3 ( 3500 10100 ) ( 3700 10300 )
      + RECT via3 ( 3900 10100 ) ( 4100 10300 )
      + RECT via3 ( 4300 10100 ) ( 4500 10300 )
      + RECT via3 ( 4700 10100 ) ( 4900 10300 )
      + RECT via3 ( 5100 10100 ) ( 5300 10300 )
      + RECT via3 ( 5500 10100 ) ( 5700 10300 )
      + RECT via3 ( -5700 10500 ) ( -5500 10700 )
      + RECT via3 ( -5300 10500 ) ( -5100 10700 )
      + RECT via3 ( -4900 10500 ) ( -4700 10700 )
      + RECT via3 ( -4500 10500 ) ( -4300 10700 )
      + RECT via3 ( -4100 10500 ) ( -3900 10700 )
      + RECT via3 ( -3700 10500 ) ( -3500 10700 )
      + RECT via3 ( -3300 10500 ) ( -3100 10700 )
      + RECT via3 ( -2900 10500 ) ( -2700 10700 )
      + RECT via3 ( -2500 10500 ) ( -2300 10700 )
      + RECT via3 ( -2100 10500 ) ( -1900 10700 )
      + RECT via3 ( -1700 10500 ) ( -1500 10700 )
      + RECT via3 ( -1300 10500 ) ( -1100 10700 )
      + RECT via3 ( -900 10500 ) ( -700 10700 )
      + RECT via3 ( -500 10500 ) ( -300 10700 )
      + RECT via3 ( -100 10500 ) ( 100 10700 )
      + RECT via3 ( 300 10500 ) ( 500 10700 )
      + RECT via3 ( 700 10500 ) ( 900 10700 )
      + RECT via3 ( 1100 10500 ) ( 1300 10700 )
      + RECT via3 ( 1500 10500 ) ( 1700 10700 )
      + RECT via3 ( 1900 10500 ) ( 2100 10700 )
      + RECT via3 ( 2300 10500 ) ( 2500 10700 )
      + RECT via3 ( 2700 10500 ) ( 2900 10700 )
      + RECT via3 ( 3100 10500 ) ( 3300 10700 )
      + RECT via3 ( 3500 10500 ) ( 3700 10700 )
      + RECT via3 ( 3900 10500 ) ( 4100 10700 )
      + RECT via3 ( 4300 10500 ) ( 4500 10700 )
      + RECT via3 ( 4700 10500 ) ( 4900 10700 )
      + RECT via3 ( 5100 10500 ) ( 5300 10700 )
      + RECT via3 ( 5500 10500 ) ( 5700 10700 )
      + RECT via3 ( -5700 10900 ) ( -5500 11100 )
      + RECT via3 ( -5300 10900 ) ( -5100 11100 )
      + RECT via3 ( -4900 10900 ) ( -4700 11100 )
      + RECT via3 ( -4500 10900 ) ( -4300 11100 )
      + RECT via3 ( -4100 10900 ) ( -3900 11100 )
      + RECT via3 ( -3700 10900 ) ( -3500 11100 )
      + RECT via3 ( -3300 10900 ) ( -3100 11100 )
      + RECT via3 ( -2900 10900 ) ( -2700 11100 )
      + RECT via3 ( -2500 10900 ) ( -2300 11100 )
      + RECT via3 ( -2100 10900 ) ( -1900 11100 )
      + RECT via3 ( -1700 10900 ) ( -1500 11100 )
      + RECT via3 ( -1300 10900 ) ( -1100 11100 )
      + RECT via3 ( -900 10900 ) ( -700 11100 )
      + RECT via3 ( -500 10900 ) ( -300 11100 )
      + RECT via3 ( -100 10900 ) ( 100 11100 )
      + RECT via3 ( 300 10900 ) ( 500 11100 )
      + RECT via3 ( 700 10900 ) ( 900 11100 )
      + RECT via3 ( 1100 10900 ) ( 1300 11100 )
      + RECT via3 ( 1500 10900 ) ( 1700 11100 )
      + RECT via3 ( 1900 10900 ) ( 2100 11100 )
      + RECT via3 ( 2300 10900 ) ( 2500 11100 )
      + RECT via3 ( 2700 10900 ) ( 2900 11100 )
      + RECT via3 ( 3100 10900 ) ( 3300 11100 )
      + RECT via3 ( 3500 10900 ) ( 3700 11100 )
      + RECT via3 ( 3900 10900 ) ( 4100 11100 )
      + RECT via3 ( 4300 10900 ) ( 4500 11100 )
      + RECT via3 ( 4700 10900 ) ( 4900 11100 )
      + RECT via3 ( 5100 10900 ) ( 5300 11100 )
      + RECT via3 ( 5500 10900 ) ( 5700 11100 ) ;
   - via4_11930_22800
      + RECT met4 ( -5965 -11400 ) ( 5965 11400 )
      + RECT met5 ( -6085 -11520 ) ( 6085 11520 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via2_280_280_vx
      + RECT met2 ( -140 -185 ) ( 140 185 )
      + RECT met3 ( -165 -165 ) ( 165 165 )
      + RECT via2 ( -100 -100 ) ( 100 100 ) ;
   - via2_560_280_hx
      + RECT met2 ( -325 -140 ) ( 325 140 )
      + RECT met3 ( -305 -165 ) ( 305 165 )
      + RECT via2 ( -100 -100 ) ( 100 100 ) ;
   - via4_11700_22620
      + RECT met4 ( -5850 -11310 ) ( 5850 11310 )
      + RECT met5 ( -5970 -11430 ) ( 5970 11430 )
      + RECT via4 ( -5200 -10800 ) ( -4400 -10000 )
      + RECT via4 ( -3600 -10800 ) ( -2800 -10000 )
      + RECT via4 ( -2000 -10800 ) ( -1200 -10000 )
      + RECT via4 ( -400 -10800 ) ( 400 -10000 )
      + RECT via4 ( 1200 -10800 ) ( 2000 -10000 )
      + RECT via4 ( 2800 -10800 ) ( 3600 -10000 )
      + RECT via4 ( 4400 -10800 ) ( 5200 -10000 )
      + RECT via4 ( -5200 -9200 ) ( -4400 -8400 )
      + RECT via4 ( -3600 -9200 ) ( -2800 -8400 )
      + RECT via4 ( -2000 -9200 ) ( -1200 -8400 )
      + RECT via4 ( -400 -9200 ) ( 400 -8400 )
      + RECT via4 ( 1200 -9200 ) ( 2000 -8400 )
      + RECT via4 ( 2800 -9200 ) ( 3600 -8400 )
      + RECT via4 ( 4400 -9200 ) ( 5200 -8400 )
      + RECT via4 ( -5200 -7600 ) ( -4400 -6800 )
      + RECT via4 ( -3600 -7600 ) ( -2800 -6800 )
      + RECT via4 ( -2000 -7600 ) ( -1200 -6800 )
      + RECT via4 ( -400 -7600 ) ( 400 -6800 )
      + RECT via4 ( 1200 -7600 ) ( 2000 -6800 )
      + RECT via4 ( 2800 -7600 ) ( 3600 -6800 )
      + RECT via4 ( 4400 -7600 ) ( 5200 -6800 )
      + RECT via4 ( -5200 -6000 ) ( -4400 -5200 )
      + RECT via4 ( -3600 -6000 ) ( -2800 -5200 )
      + RECT via4 ( -2000 -6000 ) ( -1200 -5200 )
      + RECT via4 ( -400 -6000 ) ( 400 -5200 )
      + RECT via4 ( 1200 -6000 ) ( 2000 -5200 )
      + RECT via4 ( 2800 -6000 ) ( 3600 -5200 )
      + RECT via4 ( 4400 -6000 ) ( 5200 -5200 )
      + RECT via4 ( -5200 -4400 ) ( -4400 -3600 )
      + RECT via4 ( -3600 -4400 ) ( -2800 -3600 )
      + RECT via4 ( -2000 -4400 ) ( -1200 -3600 )
      + RECT via4 ( -400 -4400 ) ( 400 -3600 )
      + RECT via4 ( 1200 -4400 ) ( 2000 -3600 )
      + RECT via4 ( 2800 -4400 ) ( 3600 -3600 )
      + RECT via4 ( 4400 -4400 ) ( 5200 -3600 )
      + RECT via4 ( -5200 -2800 ) ( -4400 -2000 )
      + RECT via4 ( -3600 -2800 ) ( -2800 -2000 )
      + RECT via4 ( -2000 -2800 ) ( -1200 -2000 )
      + RECT via4 ( -400 -2800 ) ( 400 -2000 )
      + RECT via4 ( 1200 -2800 ) ( 2000 -2000 )
      + RECT via4 ( 2800 -2800 ) ( 3600 -2000 )
      + RECT via4 ( 4400 -2800 ) ( 5200 -2000 )
      + RECT via4 ( -5200 -1200 ) ( -4400 -400 )
      + RECT via4 ( -3600 -1200 ) ( -2800 -400 )
      + RECT via4 ( -2000 -1200 ) ( -1200 -400 )
      + RECT via4 ( -400 -1200 ) ( 400 -400 )
      + RECT via4 ( 1200 -1200 ) ( 2000 -400 )
      + RECT via4 ( 2800 -1200 ) ( 3600 -400 )
      + RECT via4 ( 4400 -1200 ) ( 5200 -400 )
      + RECT via4 ( -5200 400 ) ( -4400 1200 )
      + RECT via4 ( -3600 400 ) ( -2800 1200 )
      + RECT via4 ( -2000 400 ) ( -1200 1200 )
      + RECT via4 ( -400 400 ) ( 400 1200 )
      + RECT via4 ( 1200 400 ) ( 2000 1200 )
      + RECT via4 ( 2800 400 ) ( 3600 1200 )
      + RECT via4 ( 4400 400 ) ( 5200 1200 )
      + RECT via4 ( -5200 2000 ) ( -4400 2800 )
      + RECT via4 ( -3600 2000 ) ( -2800 2800 )
      + RECT via4 ( -2000 2000 ) ( -1200 2800 )
      + RECT via4 ( -400 2000 ) ( 400 2800 )
      + RECT via4 ( 1200 2000 ) ( 2000 2800 )
      + RECT via4 ( 2800 2000 ) ( 3600 2800 )
      + RECT via4 ( 4400 2000 ) ( 5200 2800 )
      + RECT via4 ( -5200 3600 ) ( -4400 4400 )
      + RECT via4 ( -3600 3600 ) ( -2800 4400 )
      + RECT via4 ( -2000 3600 ) ( -1200 4400 )
      + RECT via4 ( -400 3600 ) ( 400 4400 )
      + RECT via4 ( 1200 3600 ) ( 2000 4400 )
      + RECT via4 ( 2800 3600 ) ( 3600 4400 )
      + RECT via4 ( 4400 3600 ) ( 5200 4400 )
      + RECT via4 ( -5200 5200 ) ( -4400 6000 )
      + RECT via4 ( -3600 5200 ) ( -2800 6000 )
      + RECT via4 ( -2000 5200 ) ( -1200 6000 )
      + RECT via4 ( -400 5200 ) ( 400 6000 )
      + RECT via4 ( 1200 5200 ) ( 2000 6000 )
      + RECT via4 ( 2800 5200 ) ( 3600 6000 )
      + RECT via4 ( 4400 5200 ) ( 5200 6000 )
      + RECT via4 ( -5200 6800 ) ( -4400 7600 )
      + RECT via4 ( -3600 6800 ) ( -2800 7600 )
      + RECT via4 ( -2000 6800 ) ( -1200 7600 )
      + RECT via4 ( -400 6800 ) ( 400 7600 )
      + RECT via4 ( 1200 6800 ) ( 2000 7600 )
      + RECT via4 ( 2800 6800 ) ( 3600 7600 )
      + RECT via4 ( 4400 6800 ) ( 5200 7600 )
      + RECT via4 ( -5200 8400 ) ( -4400 9200 )
      + RECT via4 ( -3600 8400 ) ( -2800 9200 )
      + RECT via4 ( -2000 8400 ) ( -1200 9200 )
      + RECT via4 ( -400 8400 ) ( 400 9200 )
      + RECT via4 ( 1200 8400 ) ( 2000 9200 )
      + RECT via4 ( 2800 8400 ) ( 3600 9200 )
      + RECT via4 ( 4400 8400 ) ( 5200 9200 )
      + RECT via4 ( -5200 10000 ) ( -4400 10800 )
      + RECT via4 ( -3600 10000 ) ( -2800 10800 )
      + RECT via4 ( -2000 10000 ) ( -1200 10800 )
      + RECT via4 ( -400 10000 ) ( 400 10800 )
      + RECT via4 ( 1200 10000 ) ( 2000 10800 )
      + RECT via4 ( 2800 10000 ) ( 3600 10800 )
      + RECT via4 ( 4400 10000 ) ( 5200 10800 ) ;
   - via3_11930_22800_hx
      + RECT met3 ( -5995 -11400 ) ( 5995 11400 )
      + RECT met4 ( -5970 -11405 ) ( 5970 11405 )
      + RECT via3 ( -5900 -11300 ) ( -5700 -11100 )
      + RECT via3 ( -5500 -11300 ) ( -5300 -11100 )
      + RECT via3 ( -5100 -11300 ) ( -4900 -11100 )
      + RECT via3 ( -4700 -11300 ) ( -4500 -11100 )
      + RECT via3 ( -4300 -11300 ) ( -4100 -11100 )
      + RECT via3 ( -3900 -11300 ) ( -3700 -11100 )
      + RECT via3 ( -3500 -11300 ) ( -3300 -11100 )
      + RECT via3 ( -3100 -11300 ) ( -2900 -11100 )
      + RECT via3 ( -2700 -11300 ) ( -2500 -11100 )
      + RECT via3 ( -2300 -11300 ) ( -2100 -11100 )
      + RECT via3 ( -1900 -11300 ) ( -1700 -11100 )
      + RECT via3 ( -1500 -11300 ) ( -1300 -11100 )
      + RECT via3 ( -1100 -11300 ) ( -900 -11100 )
      + RECT via3 ( -700 -11300 ) ( -500 -11100 )
      + RECT via3 ( -300 -11300 ) ( -100 -11100 )
      + RECT via3 ( 100 -11300 ) ( 300 -11100 )
      + RECT via3 ( 500 -11300 ) ( 700 -11100 )
      + RECT via3 ( 900 -11300 ) ( 1100 -11100 )
      + RECT via3 ( 1300 -11300 ) ( 1500 -11100 )
      + RECT via3 ( 1700 -11300 ) ( 1900 -11100 )
      + RECT via3 ( 2100 -11300 ) ( 2300 -11100 )
      + RECT via3 ( 2500 -11300 ) ( 2700 -11100 )
      + RECT via3 ( 2900 -11300 ) ( 3100 -11100 )
      + RECT via3 ( 3300 -11300 ) ( 3500 -11100 )
      + RECT via3 ( 3700 -11300 ) ( 3900 -11100 )
      + RECT via3 ( 4100 -11300 ) ( 4300 -11100 )
      + RECT via3 ( 4500 -11300 ) ( 4700 -11100 )
      + RECT via3 ( 4900 -11300 ) ( 5100 -11100 )
      + RECT via3 ( 5300 -11300 ) ( 5500 -11100 )
      + RECT via3 ( 5700 -11300 ) ( 5900 -11100 )
      + RECT via3 ( -5900 -10900 ) ( -5700 -10700 )
      + RECT via3 ( -5500 -10900 ) ( -5300 -10700 )
      + RECT via3 ( -5100 -10900 ) ( -4900 -10700 )
      + RECT via3 ( -4700 -10900 ) ( -4500 -10700 )
      + RECT via3 ( -4300 -10900 ) ( -4100 -10700 )
      + RECT via3 ( -3900 -10900 ) ( -3700 -10700 )
      + RECT via3 ( -3500 -10900 ) ( -3300 -10700 )
      + RECT via3 ( -3100 -10900 ) ( -2900 -10700 )
      + RECT via3 ( -2700 -10900 ) ( -2500 -10700 )
      + RECT via3 ( -2300 -10900 ) ( -2100 -10700 )
      + RECT via3 ( -1900 -10900 ) ( -1700 -10700 )
      + RECT via3 ( -1500 -10900 ) ( -1300 -10700 )
      + RECT via3 ( -1100 -10900 ) ( -900 -10700 )
      + RECT via3 ( -700 -10900 ) ( -500 -10700 )
      + RECT via3 ( -300 -10900 ) ( -100 -10700 )
      + RECT via3 ( 100 -10900 ) ( 300 -10700 )
      + RECT via3 ( 500 -10900 ) ( 700 -10700 )
      + RECT via3 ( 900 -10900 ) ( 1100 -10700 )
      + RECT via3 ( 1300 -10900 ) ( 1500 -10700 )
      + RECT via3 ( 1700 -10900 ) ( 1900 -10700 )
      + RECT via3 ( 2100 -10900 ) ( 2300 -10700 )
      + RECT via3 ( 2500 -10900 ) ( 2700 -10700 )
      + RECT via3 ( 2900 -10900 ) ( 3100 -10700 )
      + RECT via3 ( 3300 -10900 ) ( 3500 -10700 )
      + RECT via3 ( 3700 -10900 ) ( 3900 -10700 )
      + RECT via3 ( 4100 -10900 ) ( 4300 -10700 )
      + RECT via3 ( 4500 -10900 ) ( 4700 -10700 )
      + RECT via3 ( 4900 -10900 ) ( 5100 -10700 )
      + RECT via3 ( 5300 -10900 ) ( 5500 -10700 )
      + RECT via3 ( 5700 -10900 ) ( 5900 -10700 )
      + RECT via3 ( -5900 -10500 ) ( -5700 -10300 )
      + RECT via3 ( -5500 -10500 ) ( -5300 -10300 )
      + RECT via3 ( -5100 -10500 ) ( -4900 -10300 )
      + RECT via3 ( -4700 -10500 ) ( -4500 -10300 )
      + RECT via3 ( -4300 -10500 ) ( -4100 -10300 )
      + RECT via3 ( -3900 -10500 ) ( -3700 -10300 )
      + RECT via3 ( -3500 -10500 ) ( -3300 -10300 )
      + RECT via3 ( -3100 -10500 ) ( -2900 -10300 )
      + RECT via3 ( -2700 -10500 ) ( -2500 -10300 )
      + RECT via3 ( -2300 -10500 ) ( -2100 -10300 )
      + RECT via3 ( -1900 -10500 ) ( -1700 -10300 )
      + RECT via3 ( -1500 -10500 ) ( -1300 -10300 )
      + RECT via3 ( -1100 -10500 ) ( -900 -10300 )
      + RECT via3 ( -700 -10500 ) ( -500 -10300 )
      + RECT via3 ( -300 -10500 ) ( -100 -10300 )
      + RECT via3 ( 100 -10500 ) ( 300 -10300 )
      + RECT via3 ( 500 -10500 ) ( 700 -10300 )
      + RECT via3 ( 900 -10500 ) ( 1100 -10300 )
      + RECT via3 ( 1300 -10500 ) ( 1500 -10300 )
      + RECT via3 ( 1700 -10500 ) ( 1900 -10300 )
      + RECT via3 ( 2100 -10500 ) ( 2300 -10300 )
      + RECT via3 ( 2500 -10500 ) ( 2700 -10300 )
      + RECT via3 ( 2900 -10500 ) ( 3100 -10300 )
      + RECT via3 ( 3300 -10500 ) ( 3500 -10300 )
      + RECT via3 ( 3700 -10500 ) ( 3900 -10300 )
      + RECT via3 ( 4100 -10500 ) ( 4300 -10300 )
      + RECT via3 ( 4500 -10500 ) ( 4700 -10300 )
      + RECT via3 ( 4900 -10500 ) ( 5100 -10300 )
      + RECT via3 ( 5300 -10500 ) ( 5500 -10300 )
      + RECT via3 ( 5700 -10500 ) ( 5900 -10300 )
      + RECT via3 ( -5900 -10100 ) ( -5700 -9900 )
      + RECT via3 ( -5500 -10100 ) ( -5300 -9900 )
      + RECT via3 ( -5100 -10100 ) ( -4900 -9900 )
      + RECT via3 ( -4700 -10100 ) ( -4500 -9900 )
      + RECT via3 ( -4300 -10100 ) ( -4100 -9900 )
      + RECT via3 ( -3900 -10100 ) ( -3700 -9900 )
      + RECT via3 ( -3500 -10100 ) ( -3300 -9900 )
      + RECT via3 ( -3100 -10100 ) ( -2900 -9900 )
      + RECT via3 ( -2700 -10100 ) ( -2500 -9900 )
      + RECT via3 ( -2300 -10100 ) ( -2100 -9900 )
      + RECT via3 ( -1900 -10100 ) ( -1700 -9900 )
      + RECT via3 ( -1500 -10100 ) ( -1300 -9900 )
      + RECT via3 ( -1100 -10100 ) ( -900 -9900 )
      + RECT via3 ( -700 -10100 ) ( -500 -9900 )
      + RECT via3 ( -300 -10100 ) ( -100 -9900 )
      + RECT via3 ( 100 -10100 ) ( 300 -9900 )
      + RECT via3 ( 500 -10100 ) ( 700 -9900 )
      + RECT via3 ( 900 -10100 ) ( 1100 -9900 )
      + RECT via3 ( 1300 -10100 ) ( 1500 -9900 )
      + RECT via3 ( 1700 -10100 ) ( 1900 -9900 )
      + RECT via3 ( 2100 -10100 ) ( 2300 -9900 )
      + RECT via3 ( 2500 -10100 ) ( 2700 -9900 )
      + RECT via3 ( 2900 -10100 ) ( 3100 -9900 )
      + RECT via3 ( 3300 -10100 ) ( 3500 -9900 )
      + RECT via3 ( 3700 -10100 ) ( 3900 -9900 )
      + RECT via3 ( 4100 -10100 ) ( 4300 -9900 )
      + RECT via3 ( 4500 -10100 ) ( 4700 -9900 )
      + RECT via3 ( 4900 -10100 ) ( 5100 -9900 )
      + RECT via3 ( 5300 -10100 ) ( 5500 -9900 )
      + RECT via3 ( 5700 -10100 ) ( 5900 -9900 )
      + RECT via3 ( -5900 -9700 ) ( -5700 -9500 )
      + RECT via3 ( -5500 -9700 ) ( -5300 -9500 )
      + RECT via3 ( -5100 -9700 ) ( -4900 -9500 )
      + RECT via3 ( -4700 -9700 ) ( -4500 -9500 )
      + RECT via3 ( -4300 -9700 ) ( -4100 -9500 )
      + RECT via3 ( -3900 -9700 ) ( -3700 -9500 )
      + RECT via3 ( -3500 -9700 ) ( -3300 -9500 )
      + RECT via3 ( -3100 -9700 ) ( -2900 -9500 )
      + RECT via3 ( -2700 -9700 ) ( -2500 -9500 )
      + RECT via3 ( -2300 -9700 ) ( -2100 -9500 )
      + RECT via3 ( -1900 -9700 ) ( -1700 -9500 )
      + RECT via3 ( -1500 -9700 ) ( -1300 -9500 )
      + RECT via3 ( -1100 -9700 ) ( -900 -9500 )
      + RECT via3 ( -700 -9700 ) ( -500 -9500 )
      + RECT via3 ( -300 -9700 ) ( -100 -9500 )
      + RECT via3 ( 100 -9700 ) ( 300 -9500 )
      + RECT via3 ( 500 -9700 ) ( 700 -9500 )
      + RECT via3 ( 900 -9700 ) ( 1100 -9500 )
      + RECT via3 ( 1300 -9700 ) ( 1500 -9500 )
      + RECT via3 ( 1700 -9700 ) ( 1900 -9500 )
      + RECT via3 ( 2100 -9700 ) ( 2300 -9500 )
      + RECT via3 ( 2500 -9700 ) ( 2700 -9500 )
      + RECT via3 ( 2900 -9700 ) ( 3100 -9500 )
      + RECT via3 ( 3300 -9700 ) ( 3500 -9500 )
      + RECT via3 ( 3700 -9700 ) ( 3900 -9500 )
      + RECT via3 ( 4100 -9700 ) ( 4300 -9500 )
      + RECT via3 ( 4500 -9700 ) ( 4700 -9500 )
      + RECT via3 ( 4900 -9700 ) ( 5100 -9500 )
      + RECT via3 ( 5300 -9700 ) ( 5500 -9500 )
      + RECT via3 ( 5700 -9700 ) ( 5900 -9500 )
      + RECT via3 ( -5900 -9300 ) ( -5700 -9100 )
      + RECT via3 ( -5500 -9300 ) ( -5300 -9100 )
      + RECT via3 ( -5100 -9300 ) ( -4900 -9100 )
      + RECT via3 ( -4700 -9300 ) ( -4500 -9100 )
      + RECT via3 ( -4300 -9300 ) ( -4100 -9100 )
      + RECT via3 ( -3900 -9300 ) ( -3700 -9100 )
      + RECT via3 ( -3500 -9300 ) ( -3300 -9100 )
      + RECT via3 ( -3100 -9300 ) ( -2900 -9100 )
      + RECT via3 ( -2700 -9300 ) ( -2500 -9100 )
      + RECT via3 ( -2300 -9300 ) ( -2100 -9100 )
      + RECT via3 ( -1900 -9300 ) ( -1700 -9100 )
      + RECT via3 ( -1500 -9300 ) ( -1300 -9100 )
      + RECT via3 ( -1100 -9300 ) ( -900 -9100 )
      + RECT via3 ( -700 -9300 ) ( -500 -9100 )
      + RECT via3 ( -300 -9300 ) ( -100 -9100 )
      + RECT via3 ( 100 -9300 ) ( 300 -9100 )
      + RECT via3 ( 500 -9300 ) ( 700 -9100 )
      + RECT via3 ( 900 -9300 ) ( 1100 -9100 )
      + RECT via3 ( 1300 -9300 ) ( 1500 -9100 )
      + RECT via3 ( 1700 -9300 ) ( 1900 -9100 )
      + RECT via3 ( 2100 -9300 ) ( 2300 -9100 )
      + RECT via3 ( 2500 -9300 ) ( 2700 -9100 )
      + RECT via3 ( 2900 -9300 ) ( 3100 -9100 )
      + RECT via3 ( 3300 -9300 ) ( 3500 -9100 )
      + RECT via3 ( 3700 -9300 ) ( 3900 -9100 )
      + RECT via3 ( 4100 -9300 ) ( 4300 -9100 )
      + RECT via3 ( 4500 -9300 ) ( 4700 -9100 )
      + RECT via3 ( 4900 -9300 ) ( 5100 -9100 )
      + RECT via3 ( 5300 -9300 ) ( 5500 -9100 )
      + RECT via3 ( 5700 -9300 ) ( 5900 -9100 )
      + RECT via3 ( -5900 -8900 ) ( -5700 -8700 )
      + RECT via3 ( -5500 -8900 ) ( -5300 -8700 )
      + RECT via3 ( -5100 -8900 ) ( -4900 -8700 )
      + RECT via3 ( -4700 -8900 ) ( -4500 -8700 )
      + RECT via3 ( -4300 -8900 ) ( -4100 -8700 )
      + RECT via3 ( -3900 -8900 ) ( -3700 -8700 )
      + RECT via3 ( -3500 -8900 ) ( -3300 -8700 )
      + RECT via3 ( -3100 -8900 ) ( -2900 -8700 )
      + RECT via3 ( -2700 -8900 ) ( -2500 -8700 )
      + RECT via3 ( -2300 -8900 ) ( -2100 -8700 )
      + RECT via3 ( -1900 -8900 ) ( -1700 -8700 )
      + RECT via3 ( -1500 -8900 ) ( -1300 -8700 )
      + RECT via3 ( -1100 -8900 ) ( -900 -8700 )
      + RECT via3 ( -700 -8900 ) ( -500 -8700 )
      + RECT via3 ( -300 -8900 ) ( -100 -8700 )
      + RECT via3 ( 100 -8900 ) ( 300 -8700 )
      + RECT via3 ( 500 -8900 ) ( 700 -8700 )
      + RECT via3 ( 900 -8900 ) ( 1100 -8700 )
      + RECT via3 ( 1300 -8900 ) ( 1500 -8700 )
      + RECT via3 ( 1700 -8900 ) ( 1900 -8700 )
      + RECT via3 ( 2100 -8900 ) ( 2300 -8700 )
      + RECT via3 ( 2500 -8900 ) ( 2700 -8700 )
      + RECT via3 ( 2900 -8900 ) ( 3100 -8700 )
      + RECT via3 ( 3300 -8900 ) ( 3500 -8700 )
      + RECT via3 ( 3700 -8900 ) ( 3900 -8700 )
      + RECT via3 ( 4100 -8900 ) ( 4300 -8700 )
      + RECT via3 ( 4500 -8900 ) ( 4700 -8700 )
      + RECT via3 ( 4900 -8900 ) ( 5100 -8700 )
      + RECT via3 ( 5300 -8900 ) ( 5500 -8700 )
      + RECT via3 ( 5700 -8900 ) ( 5900 -8700 )
      + RECT via3 ( -5900 -8500 ) ( -5700 -8300 )
      + RECT via3 ( -5500 -8500 ) ( -5300 -8300 )
      + RECT via3 ( -5100 -8500 ) ( -4900 -8300 )
      + RECT via3 ( -4700 -8500 ) ( -4500 -8300 )
      + RECT via3 ( -4300 -8500 ) ( -4100 -8300 )
      + RECT via3 ( -3900 -8500 ) ( -3700 -8300 )
      + RECT via3 ( -3500 -8500 ) ( -3300 -8300 )
      + RECT via3 ( -3100 -8500 ) ( -2900 -8300 )
      + RECT via3 ( -2700 -8500 ) ( -2500 -8300 )
      + RECT via3 ( -2300 -8500 ) ( -2100 -8300 )
      + RECT via3 ( -1900 -8500 ) ( -1700 -8300 )
      + RECT via3 ( -1500 -8500 ) ( -1300 -8300 )
      + RECT via3 ( -1100 -8500 ) ( -900 -8300 )
      + RECT via3 ( -700 -8500 ) ( -500 -8300 )
      + RECT via3 ( -300 -8500 ) ( -100 -8300 )
      + RECT via3 ( 100 -8500 ) ( 300 -8300 )
      + RECT via3 ( 500 -8500 ) ( 700 -8300 )
      + RECT via3 ( 900 -8500 ) ( 1100 -8300 )
      + RECT via3 ( 1300 -8500 ) ( 1500 -8300 )
      + RECT via3 ( 1700 -8500 ) ( 1900 -8300 )
      + RECT via3 ( 2100 -8500 ) ( 2300 -8300 )
      + RECT via3 ( 2500 -8500 ) ( 2700 -8300 )
      + RECT via3 ( 2900 -8500 ) ( 3100 -8300 )
      + RECT via3 ( 3300 -8500 ) ( 3500 -8300 )
      + RECT via3 ( 3700 -8500 ) ( 3900 -8300 )
      + RECT via3 ( 4100 -8500 ) ( 4300 -8300 )
      + RECT via3 ( 4500 -8500 ) ( 4700 -8300 )
      + RECT via3 ( 4900 -8500 ) ( 5100 -8300 )
      + RECT via3 ( 5300 -8500 ) ( 5500 -8300 )
      + RECT via3 ( 5700 -8500 ) ( 5900 -8300 )
      + RECT via3 ( -5900 -8100 ) ( -5700 -7900 )
      + RECT via3 ( -5500 -8100 ) ( -5300 -7900 )
      + RECT via3 ( -5100 -8100 ) ( -4900 -7900 )
      + RECT via3 ( -4700 -8100 ) ( -4500 -7900 )
      + RECT via3 ( -4300 -8100 ) ( -4100 -7900 )
      + RECT via3 ( -3900 -8100 ) ( -3700 -7900 )
      + RECT via3 ( -3500 -8100 ) ( -3300 -7900 )
      + RECT via3 ( -3100 -8100 ) ( -2900 -7900 )
      + RECT via3 ( -2700 -8100 ) ( -2500 -7900 )
      + RECT via3 ( -2300 -8100 ) ( -2100 -7900 )
      + RECT via3 ( -1900 -8100 ) ( -1700 -7900 )
      + RECT via3 ( -1500 -8100 ) ( -1300 -7900 )
      + RECT via3 ( -1100 -8100 ) ( -900 -7900 )
      + RECT via3 ( -700 -8100 ) ( -500 -7900 )
      + RECT via3 ( -300 -8100 ) ( -100 -7900 )
      + RECT via3 ( 100 -8100 ) ( 300 -7900 )
      + RECT via3 ( 500 -8100 ) ( 700 -7900 )
      + RECT via3 ( 900 -8100 ) ( 1100 -7900 )
      + RECT via3 ( 1300 -8100 ) ( 1500 -7900 )
      + RECT via3 ( 1700 -8100 ) ( 1900 -7900 )
      + RECT via3 ( 2100 -8100 ) ( 2300 -7900 )
      + RECT via3 ( 2500 -8100 ) ( 2700 -7900 )
      + RECT via3 ( 2900 -8100 ) ( 3100 -7900 )
      + RECT via3 ( 3300 -8100 ) ( 3500 -7900 )
      + RECT via3 ( 3700 -8100 ) ( 3900 -7900 )
      + RECT via3 ( 4100 -8100 ) ( 4300 -7900 )
      + RECT via3 ( 4500 -8100 ) ( 4700 -7900 )
      + RECT via3 ( 4900 -8100 ) ( 5100 -7900 )
      + RECT via3 ( 5300 -8100 ) ( 5500 -7900 )
      + RECT via3 ( 5700 -8100 ) ( 5900 -7900 )
      + RECT via3 ( -5900 -7700 ) ( -5700 -7500 )
      + RECT via3 ( -5500 -7700 ) ( -5300 -7500 )
      + RECT via3 ( -5100 -7700 ) ( -4900 -7500 )
      + RECT via3 ( -4700 -7700 ) ( -4500 -7500 )
      + RECT via3 ( -4300 -7700 ) ( -4100 -7500 )
      + RECT via3 ( -3900 -7700 ) ( -3700 -7500 )
      + RECT via3 ( -3500 -7700 ) ( -3300 -7500 )
      + RECT via3 ( -3100 -7700 ) ( -2900 -7500 )
      + RECT via3 ( -2700 -7700 ) ( -2500 -7500 )
      + RECT via3 ( -2300 -7700 ) ( -2100 -7500 )
      + RECT via3 ( -1900 -7700 ) ( -1700 -7500 )
      + RECT via3 ( -1500 -7700 ) ( -1300 -7500 )
      + RECT via3 ( -1100 -7700 ) ( -900 -7500 )
      + RECT via3 ( -700 -7700 ) ( -500 -7500 )
      + RECT via3 ( -300 -7700 ) ( -100 -7500 )
      + RECT via3 ( 100 -7700 ) ( 300 -7500 )
      + RECT via3 ( 500 -7700 ) ( 700 -7500 )
      + RECT via3 ( 900 -7700 ) ( 1100 -7500 )
      + RECT via3 ( 1300 -7700 ) ( 1500 -7500 )
      + RECT via3 ( 1700 -7700 ) ( 1900 -7500 )
      + RECT via3 ( 2100 -7700 ) ( 2300 -7500 )
      + RECT via3 ( 2500 -7700 ) ( 2700 -7500 )
      + RECT via3 ( 2900 -7700 ) ( 3100 -7500 )
      + RECT via3 ( 3300 -7700 ) ( 3500 -7500 )
      + RECT via3 ( 3700 -7700 ) ( 3900 -7500 )
      + RECT via3 ( 4100 -7700 ) ( 4300 -7500 )
      + RECT via3 ( 4500 -7700 ) ( 4700 -7500 )
      + RECT via3 ( 4900 -7700 ) ( 5100 -7500 )
      + RECT via3 ( 5300 -7700 ) ( 5500 -7500 )
      + RECT via3 ( 5700 -7700 ) ( 5900 -7500 )
      + RECT via3 ( -5900 -7300 ) ( -5700 -7100 )
      + RECT via3 ( -5500 -7300 ) ( -5300 -7100 )
      + RECT via3 ( -5100 -7300 ) ( -4900 -7100 )
      + RECT via3 ( -4700 -7300 ) ( -4500 -7100 )
      + RECT via3 ( -4300 -7300 ) ( -4100 -7100 )
      + RECT via3 ( -3900 -7300 ) ( -3700 -7100 )
      + RECT via3 ( -3500 -7300 ) ( -3300 -7100 )
      + RECT via3 ( -3100 -7300 ) ( -2900 -7100 )
      + RECT via3 ( -2700 -7300 ) ( -2500 -7100 )
      + RECT via3 ( -2300 -7300 ) ( -2100 -7100 )
      + RECT via3 ( -1900 -7300 ) ( -1700 -7100 )
      + RECT via3 ( -1500 -7300 ) ( -1300 -7100 )
      + RECT via3 ( -1100 -7300 ) ( -900 -7100 )
      + RECT via3 ( -700 -7300 ) ( -500 -7100 )
      + RECT via3 ( -300 -7300 ) ( -100 -7100 )
      + RECT via3 ( 100 -7300 ) ( 300 -7100 )
      + RECT via3 ( 500 -7300 ) ( 700 -7100 )
      + RECT via3 ( 900 -7300 ) ( 1100 -7100 )
      + RECT via3 ( 1300 -7300 ) ( 1500 -7100 )
      + RECT via3 ( 1700 -7300 ) ( 1900 -7100 )
      + RECT via3 ( 2100 -7300 ) ( 2300 -7100 )
      + RECT via3 ( 2500 -7300 ) ( 2700 -7100 )
      + RECT via3 ( 2900 -7300 ) ( 3100 -7100 )
      + RECT via3 ( 3300 -7300 ) ( 3500 -7100 )
      + RECT via3 ( 3700 -7300 ) ( 3900 -7100 )
      + RECT via3 ( 4100 -7300 ) ( 4300 -7100 )
      + RECT via3 ( 4500 -7300 ) ( 4700 -7100 )
      + RECT via3 ( 4900 -7300 ) ( 5100 -7100 )
      + RECT via3 ( 5300 -7300 ) ( 5500 -7100 )
      + RECT via3 ( 5700 -7300 ) ( 5900 -7100 )
      + RECT via3 ( -5900 -6900 ) ( -5700 -6700 )
      + RECT via3 ( -5500 -6900 ) ( -5300 -6700 )
      + RECT via3 ( -5100 -6900 ) ( -4900 -6700 )
      + RECT via3 ( -4700 -6900 ) ( -4500 -6700 )
      + RECT via3 ( -4300 -6900 ) ( -4100 -6700 )
      + RECT via3 ( -3900 -6900 ) ( -3700 -6700 )
      + RECT via3 ( -3500 -6900 ) ( -3300 -6700 )
      + RECT via3 ( -3100 -6900 ) ( -2900 -6700 )
      + RECT via3 ( -2700 -6900 ) ( -2500 -6700 )
      + RECT via3 ( -2300 -6900 ) ( -2100 -6700 )
      + RECT via3 ( -1900 -6900 ) ( -1700 -6700 )
      + RECT via3 ( -1500 -6900 ) ( -1300 -6700 )
      + RECT via3 ( -1100 -6900 ) ( -900 -6700 )
      + RECT via3 ( -700 -6900 ) ( -500 -6700 )
      + RECT via3 ( -300 -6900 ) ( -100 -6700 )
      + RECT via3 ( 100 -6900 ) ( 300 -6700 )
      + RECT via3 ( 500 -6900 ) ( 700 -6700 )
      + RECT via3 ( 900 -6900 ) ( 1100 -6700 )
      + RECT via3 ( 1300 -6900 ) ( 1500 -6700 )
      + RECT via3 ( 1700 -6900 ) ( 1900 -6700 )
      + RECT via3 ( 2100 -6900 ) ( 2300 -6700 )
      + RECT via3 ( 2500 -6900 ) ( 2700 -6700 )
      + RECT via3 ( 2900 -6900 ) ( 3100 -6700 )
      + RECT via3 ( 3300 -6900 ) ( 3500 -6700 )
      + RECT via3 ( 3700 -6900 ) ( 3900 -6700 )
      + RECT via3 ( 4100 -6900 ) ( 4300 -6700 )
      + RECT via3 ( 4500 -6900 ) ( 4700 -6700 )
      + RECT via3 ( 4900 -6900 ) ( 5100 -6700 )
      + RECT via3 ( 5300 -6900 ) ( 5500 -6700 )
      + RECT via3 ( 5700 -6900 ) ( 5900 -6700 )
      + RECT via3 ( -5900 -6500 ) ( -5700 -6300 )
      + RECT via3 ( -5500 -6500 ) ( -5300 -6300 )
      + RECT via3 ( -5100 -6500 ) ( -4900 -6300 )
      + RECT via3 ( -4700 -6500 ) ( -4500 -6300 )
      + RECT via3 ( -4300 -6500 ) ( -4100 -6300 )
      + RECT via3 ( -3900 -6500 ) ( -3700 -6300 )
      + RECT via3 ( -3500 -6500 ) ( -3300 -6300 )
      + RECT via3 ( -3100 -6500 ) ( -2900 -6300 )
      + RECT via3 ( -2700 -6500 ) ( -2500 -6300 )
      + RECT via3 ( -2300 -6500 ) ( -2100 -6300 )
      + RECT via3 ( -1900 -6500 ) ( -1700 -6300 )
      + RECT via3 ( -1500 -6500 ) ( -1300 -6300 )
      + RECT via3 ( -1100 -6500 ) ( -900 -6300 )
      + RECT via3 ( -700 -6500 ) ( -500 -6300 )
      + RECT via3 ( -300 -6500 ) ( -100 -6300 )
      + RECT via3 ( 100 -6500 ) ( 300 -6300 )
      + RECT via3 ( 500 -6500 ) ( 700 -6300 )
      + RECT via3 ( 900 -6500 ) ( 1100 -6300 )
      + RECT via3 ( 1300 -6500 ) ( 1500 -6300 )
      + RECT via3 ( 1700 -6500 ) ( 1900 -6300 )
      + RECT via3 ( 2100 -6500 ) ( 2300 -6300 )
      + RECT via3 ( 2500 -6500 ) ( 2700 -6300 )
      + RECT via3 ( 2900 -6500 ) ( 3100 -6300 )
      + RECT via3 ( 3300 -6500 ) ( 3500 -6300 )
      + RECT via3 ( 3700 -6500 ) ( 3900 -6300 )
      + RECT via3 ( 4100 -6500 ) ( 4300 -6300 )
      + RECT via3 ( 4500 -6500 ) ( 4700 -6300 )
      + RECT via3 ( 4900 -6500 ) ( 5100 -6300 )
      + RECT via3 ( 5300 -6500 ) ( 5500 -6300 )
      + RECT via3 ( 5700 -6500 ) ( 5900 -6300 )
      + RECT via3 ( -5900 -6100 ) ( -5700 -5900 )
      + RECT via3 ( -5500 -6100 ) ( -5300 -5900 )
      + RECT via3 ( -5100 -6100 ) ( -4900 -5900 )
      + RECT via3 ( -4700 -6100 ) ( -4500 -5900 )
      + RECT via3 ( -4300 -6100 ) ( -4100 -5900 )
      + RECT via3 ( -3900 -6100 ) ( -3700 -5900 )
      + RECT via3 ( -3500 -6100 ) ( -3300 -5900 )
      + RECT via3 ( -3100 -6100 ) ( -2900 -5900 )
      + RECT via3 ( -2700 -6100 ) ( -2500 -5900 )
      + RECT via3 ( -2300 -6100 ) ( -2100 -5900 )
      + RECT via3 ( -1900 -6100 ) ( -1700 -5900 )
      + RECT via3 ( -1500 -6100 ) ( -1300 -5900 )
      + RECT via3 ( -1100 -6100 ) ( -900 -5900 )
      + RECT via3 ( -700 -6100 ) ( -500 -5900 )
      + RECT via3 ( -300 -6100 ) ( -100 -5900 )
      + RECT via3 ( 100 -6100 ) ( 300 -5900 )
      + RECT via3 ( 500 -6100 ) ( 700 -5900 )
      + RECT via3 ( 900 -6100 ) ( 1100 -5900 )
      + RECT via3 ( 1300 -6100 ) ( 1500 -5900 )
      + RECT via3 ( 1700 -6100 ) ( 1900 -5900 )
      + RECT via3 ( 2100 -6100 ) ( 2300 -5900 )
      + RECT via3 ( 2500 -6100 ) ( 2700 -5900 )
      + RECT via3 ( 2900 -6100 ) ( 3100 -5900 )
      + RECT via3 ( 3300 -6100 ) ( 3500 -5900 )
      + RECT via3 ( 3700 -6100 ) ( 3900 -5900 )
      + RECT via3 ( 4100 -6100 ) ( 4300 -5900 )
      + RECT via3 ( 4500 -6100 ) ( 4700 -5900 )
      + RECT via3 ( 4900 -6100 ) ( 5100 -5900 )
      + RECT via3 ( 5300 -6100 ) ( 5500 -5900 )
      + RECT via3 ( 5700 -6100 ) ( 5900 -5900 )
      + RECT via3 ( -5900 -5700 ) ( -5700 -5500 )
      + RECT via3 ( -5500 -5700 ) ( -5300 -5500 )
      + RECT via3 ( -5100 -5700 ) ( -4900 -5500 )
      + RECT via3 ( -4700 -5700 ) ( -4500 -5500 )
      + RECT via3 ( -4300 -5700 ) ( -4100 -5500 )
      + RECT via3 ( -3900 -5700 ) ( -3700 -5500 )
      + RECT via3 ( -3500 -5700 ) ( -3300 -5500 )
      + RECT via3 ( -3100 -5700 ) ( -2900 -5500 )
      + RECT via3 ( -2700 -5700 ) ( -2500 -5500 )
      + RECT via3 ( -2300 -5700 ) ( -2100 -5500 )
      + RECT via3 ( -1900 -5700 ) ( -1700 -5500 )
      + RECT via3 ( -1500 -5700 ) ( -1300 -5500 )
      + RECT via3 ( -1100 -5700 ) ( -900 -5500 )
      + RECT via3 ( -700 -5700 ) ( -500 -5500 )
      + RECT via3 ( -300 -5700 ) ( -100 -5500 )
      + RECT via3 ( 100 -5700 ) ( 300 -5500 )
      + RECT via3 ( 500 -5700 ) ( 700 -5500 )
      + RECT via3 ( 900 -5700 ) ( 1100 -5500 )
      + RECT via3 ( 1300 -5700 ) ( 1500 -5500 )
      + RECT via3 ( 1700 -5700 ) ( 1900 -5500 )
      + RECT via3 ( 2100 -5700 ) ( 2300 -5500 )
      + RECT via3 ( 2500 -5700 ) ( 2700 -5500 )
      + RECT via3 ( 2900 -5700 ) ( 3100 -5500 )
      + RECT via3 ( 3300 -5700 ) ( 3500 -5500 )
      + RECT via3 ( 3700 -5700 ) ( 3900 -5500 )
      + RECT via3 ( 4100 -5700 ) ( 4300 -5500 )
      + RECT via3 ( 4500 -5700 ) ( 4700 -5500 )
      + RECT via3 ( 4900 -5700 ) ( 5100 -5500 )
      + RECT via3 ( 5300 -5700 ) ( 5500 -5500 )
      + RECT via3 ( 5700 -5700 ) ( 5900 -5500 )
      + RECT via3 ( -5900 -5300 ) ( -5700 -5100 )
      + RECT via3 ( -5500 -5300 ) ( -5300 -5100 )
      + RECT via3 ( -5100 -5300 ) ( -4900 -5100 )
      + RECT via3 ( -4700 -5300 ) ( -4500 -5100 )
      + RECT via3 ( -4300 -5300 ) ( -4100 -5100 )
      + RECT via3 ( -3900 -5300 ) ( -3700 -5100 )
      + RECT via3 ( -3500 -5300 ) ( -3300 -5100 )
      + RECT via3 ( -3100 -5300 ) ( -2900 -5100 )
      + RECT via3 ( -2700 -5300 ) ( -2500 -5100 )
      + RECT via3 ( -2300 -5300 ) ( -2100 -5100 )
      + RECT via3 ( -1900 -5300 ) ( -1700 -5100 )
      + RECT via3 ( -1500 -5300 ) ( -1300 -5100 )
      + RECT via3 ( -1100 -5300 ) ( -900 -5100 )
      + RECT via3 ( -700 -5300 ) ( -500 -5100 )
      + RECT via3 ( -300 -5300 ) ( -100 -5100 )
      + RECT via3 ( 100 -5300 ) ( 300 -5100 )
      + RECT via3 ( 500 -5300 ) ( 700 -5100 )
      + RECT via3 ( 900 -5300 ) ( 1100 -5100 )
      + RECT via3 ( 1300 -5300 ) ( 1500 -5100 )
      + RECT via3 ( 1700 -5300 ) ( 1900 -5100 )
      + RECT via3 ( 2100 -5300 ) ( 2300 -5100 )
      + RECT via3 ( 2500 -5300 ) ( 2700 -5100 )
      + RECT via3 ( 2900 -5300 ) ( 3100 -5100 )
      + RECT via3 ( 3300 -5300 ) ( 3500 -5100 )
      + RECT via3 ( 3700 -5300 ) ( 3900 -5100 )
      + RECT via3 ( 4100 -5300 ) ( 4300 -5100 )
      + RECT via3 ( 4500 -5300 ) ( 4700 -5100 )
      + RECT via3 ( 4900 -5300 ) ( 5100 -5100 )
      + RECT via3 ( 5300 -5300 ) ( 5500 -5100 )
      + RECT via3 ( 5700 -5300 ) ( 5900 -5100 )
      + RECT via3 ( -5900 -4900 ) ( -5700 -4700 )
      + RECT via3 ( -5500 -4900 ) ( -5300 -4700 )
      + RECT via3 ( -5100 -4900 ) ( -4900 -4700 )
      + RECT via3 ( -4700 -4900 ) ( -4500 -4700 )
      + RECT via3 ( -4300 -4900 ) ( -4100 -4700 )
      + RECT via3 ( -3900 -4900 ) ( -3700 -4700 )
      + RECT via3 ( -3500 -4900 ) ( -3300 -4700 )
      + RECT via3 ( -3100 -4900 ) ( -2900 -4700 )
      + RECT via3 ( -2700 -4900 ) ( -2500 -4700 )
      + RECT via3 ( -2300 -4900 ) ( -2100 -4700 )
      + RECT via3 ( -1900 -4900 ) ( -1700 -4700 )
      + RECT via3 ( -1500 -4900 ) ( -1300 -4700 )
      + RECT via3 ( -1100 -4900 ) ( -900 -4700 )
      + RECT via3 ( -700 -4900 ) ( -500 -4700 )
      + RECT via3 ( -300 -4900 ) ( -100 -4700 )
      + RECT via3 ( 100 -4900 ) ( 300 -4700 )
      + RECT via3 ( 500 -4900 ) ( 700 -4700 )
      + RECT via3 ( 900 -4900 ) ( 1100 -4700 )
      + RECT via3 ( 1300 -4900 ) ( 1500 -4700 )
      + RECT via3 ( 1700 -4900 ) ( 1900 -4700 )
      + RECT via3 ( 2100 -4900 ) ( 2300 -4700 )
      + RECT via3 ( 2500 -4900 ) ( 2700 -4700 )
      + RECT via3 ( 2900 -4900 ) ( 3100 -4700 )
      + RECT via3 ( 3300 -4900 ) ( 3500 -4700 )
      + RECT via3 ( 3700 -4900 ) ( 3900 -4700 )
      + RECT via3 ( 4100 -4900 ) ( 4300 -4700 )
      + RECT via3 ( 4500 -4900 ) ( 4700 -4700 )
      + RECT via3 ( 4900 -4900 ) ( 5100 -4700 )
      + RECT via3 ( 5300 -4900 ) ( 5500 -4700 )
      + RECT via3 ( 5700 -4900 ) ( 5900 -4700 )
      + RECT via3 ( -5900 -4500 ) ( -5700 -4300 )
      + RECT via3 ( -5500 -4500 ) ( -5300 -4300 )
      + RECT via3 ( -5100 -4500 ) ( -4900 -4300 )
      + RECT via3 ( -4700 -4500 ) ( -4500 -4300 )
      + RECT via3 ( -4300 -4500 ) ( -4100 -4300 )
      + RECT via3 ( -3900 -4500 ) ( -3700 -4300 )
      + RECT via3 ( -3500 -4500 ) ( -3300 -4300 )
      + RECT via3 ( -3100 -4500 ) ( -2900 -4300 )
      + RECT via3 ( -2700 -4500 ) ( -2500 -4300 )
      + RECT via3 ( -2300 -4500 ) ( -2100 -4300 )
      + RECT via3 ( -1900 -4500 ) ( -1700 -4300 )
      + RECT via3 ( -1500 -4500 ) ( -1300 -4300 )
      + RECT via3 ( -1100 -4500 ) ( -900 -4300 )
      + RECT via3 ( -700 -4500 ) ( -500 -4300 )
      + RECT via3 ( -300 -4500 ) ( -100 -4300 )
      + RECT via3 ( 100 -4500 ) ( 300 -4300 )
      + RECT via3 ( 500 -4500 ) ( 700 -4300 )
      + RECT via3 ( 900 -4500 ) ( 1100 -4300 )
      + RECT via3 ( 1300 -4500 ) ( 1500 -4300 )
      + RECT via3 ( 1700 -4500 ) ( 1900 -4300 )
      + RECT via3 ( 2100 -4500 ) ( 2300 -4300 )
      + RECT via3 ( 2500 -4500 ) ( 2700 -4300 )
      + RECT via3 ( 2900 -4500 ) ( 3100 -4300 )
      + RECT via3 ( 3300 -4500 ) ( 3500 -4300 )
      + RECT via3 ( 3700 -4500 ) ( 3900 -4300 )
      + RECT via3 ( 4100 -4500 ) ( 4300 -4300 )
      + RECT via3 ( 4500 -4500 ) ( 4700 -4300 )
      + RECT via3 ( 4900 -4500 ) ( 5100 -4300 )
      + RECT via3 ( 5300 -4500 ) ( 5500 -4300 )
      + RECT via3 ( 5700 -4500 ) ( 5900 -4300 )
      + RECT via3 ( -5900 -4100 ) ( -5700 -3900 )
      + RECT via3 ( -5500 -4100 ) ( -5300 -3900 )
      + RECT via3 ( -5100 -4100 ) ( -4900 -3900 )
      + RECT via3 ( -4700 -4100 ) ( -4500 -3900 )
      + RECT via3 ( -4300 -4100 ) ( -4100 -3900 )
      + RECT via3 ( -3900 -4100 ) ( -3700 -3900 )
      + RECT via3 ( -3500 -4100 ) ( -3300 -3900 )
      + RECT via3 ( -3100 -4100 ) ( -2900 -3900 )
      + RECT via3 ( -2700 -4100 ) ( -2500 -3900 )
      + RECT via3 ( -2300 -4100 ) ( -2100 -3900 )
      + RECT via3 ( -1900 -4100 ) ( -1700 -3900 )
      + RECT via3 ( -1500 -4100 ) ( -1300 -3900 )
      + RECT via3 ( -1100 -4100 ) ( -900 -3900 )
      + RECT via3 ( -700 -4100 ) ( -500 -3900 )
      + RECT via3 ( -300 -4100 ) ( -100 -3900 )
      + RECT via3 ( 100 -4100 ) ( 300 -3900 )
      + RECT via3 ( 500 -4100 ) ( 700 -3900 )
      + RECT via3 ( 900 -4100 ) ( 1100 -3900 )
      + RECT via3 ( 1300 -4100 ) ( 1500 -3900 )
      + RECT via3 ( 1700 -4100 ) ( 1900 -3900 )
      + RECT via3 ( 2100 -4100 ) ( 2300 -3900 )
      + RECT via3 ( 2500 -4100 ) ( 2700 -3900 )
      + RECT via3 ( 2900 -4100 ) ( 3100 -3900 )
      + RECT via3 ( 3300 -4100 ) ( 3500 -3900 )
      + RECT via3 ( 3700 -4100 ) ( 3900 -3900 )
      + RECT via3 ( 4100 -4100 ) ( 4300 -3900 )
      + RECT via3 ( 4500 -4100 ) ( 4700 -3900 )
      + RECT via3 ( 4900 -4100 ) ( 5100 -3900 )
      + RECT via3 ( 5300 -4100 ) ( 5500 -3900 )
      + RECT via3 ( 5700 -4100 ) ( 5900 -3900 )
      + RECT via3 ( -5900 -3700 ) ( -5700 -3500 )
      + RECT via3 ( -5500 -3700 ) ( -5300 -3500 )
      + RECT via3 ( -5100 -3700 ) ( -4900 -3500 )
      + RECT via3 ( -4700 -3700 ) ( -4500 -3500 )
      + RECT via3 ( -4300 -3700 ) ( -4100 -3500 )
      + RECT via3 ( -3900 -3700 ) ( -3700 -3500 )
      + RECT via3 ( -3500 -3700 ) ( -3300 -3500 )
      + RECT via3 ( -3100 -3700 ) ( -2900 -3500 )
      + RECT via3 ( -2700 -3700 ) ( -2500 -3500 )
      + RECT via3 ( -2300 -3700 ) ( -2100 -3500 )
      + RECT via3 ( -1900 -3700 ) ( -1700 -3500 )
      + RECT via3 ( -1500 -3700 ) ( -1300 -3500 )
      + RECT via3 ( -1100 -3700 ) ( -900 -3500 )
      + RECT via3 ( -700 -3700 ) ( -500 -3500 )
      + RECT via3 ( -300 -3700 ) ( -100 -3500 )
      + RECT via3 ( 100 -3700 ) ( 300 -3500 )
      + RECT via3 ( 500 -3700 ) ( 700 -3500 )
      + RECT via3 ( 900 -3700 ) ( 1100 -3500 )
      + RECT via3 ( 1300 -3700 ) ( 1500 -3500 )
      + RECT via3 ( 1700 -3700 ) ( 1900 -3500 )
      + RECT via3 ( 2100 -3700 ) ( 2300 -3500 )
      + RECT via3 ( 2500 -3700 ) ( 2700 -3500 )
      + RECT via3 ( 2900 -3700 ) ( 3100 -3500 )
      + RECT via3 ( 3300 -3700 ) ( 3500 -3500 )
      + RECT via3 ( 3700 -3700 ) ( 3900 -3500 )
      + RECT via3 ( 4100 -3700 ) ( 4300 -3500 )
      + RECT via3 ( 4500 -3700 ) ( 4700 -3500 )
      + RECT via3 ( 4900 -3700 ) ( 5100 -3500 )
      + RECT via3 ( 5300 -3700 ) ( 5500 -3500 )
      + RECT via3 ( 5700 -3700 ) ( 5900 -3500 )
      + RECT via3 ( -5900 -3300 ) ( -5700 -3100 )
      + RECT via3 ( -5500 -3300 ) ( -5300 -3100 )
      + RECT via3 ( -5100 -3300 ) ( -4900 -3100 )
      + RECT via3 ( -4700 -3300 ) ( -4500 -3100 )
      + RECT via3 ( -4300 -3300 ) ( -4100 -3100 )
      + RECT via3 ( -3900 -3300 ) ( -3700 -3100 )
      + RECT via3 ( -3500 -3300 ) ( -3300 -3100 )
      + RECT via3 ( -3100 -3300 ) ( -2900 -3100 )
      + RECT via3 ( -2700 -3300 ) ( -2500 -3100 )
      + RECT via3 ( -2300 -3300 ) ( -2100 -3100 )
      + RECT via3 ( -1900 -3300 ) ( -1700 -3100 )
      + RECT via3 ( -1500 -3300 ) ( -1300 -3100 )
      + RECT via3 ( -1100 -3300 ) ( -900 -3100 )
      + RECT via3 ( -700 -3300 ) ( -500 -3100 )
      + RECT via3 ( -300 -3300 ) ( -100 -3100 )
      + RECT via3 ( 100 -3300 ) ( 300 -3100 )
      + RECT via3 ( 500 -3300 ) ( 700 -3100 )
      + RECT via3 ( 900 -3300 ) ( 1100 -3100 )
      + RECT via3 ( 1300 -3300 ) ( 1500 -3100 )
      + RECT via3 ( 1700 -3300 ) ( 1900 -3100 )
      + RECT via3 ( 2100 -3300 ) ( 2300 -3100 )
      + RECT via3 ( 2500 -3300 ) ( 2700 -3100 )
      + RECT via3 ( 2900 -3300 ) ( 3100 -3100 )
      + RECT via3 ( 3300 -3300 ) ( 3500 -3100 )
      + RECT via3 ( 3700 -3300 ) ( 3900 -3100 )
      + RECT via3 ( 4100 -3300 ) ( 4300 -3100 )
      + RECT via3 ( 4500 -3300 ) ( 4700 -3100 )
      + RECT via3 ( 4900 -3300 ) ( 5100 -3100 )
      + RECT via3 ( 5300 -3300 ) ( 5500 -3100 )
      + RECT via3 ( 5700 -3300 ) ( 5900 -3100 )
      + RECT via3 ( -5900 -2900 ) ( -5700 -2700 )
      + RECT via3 ( -5500 -2900 ) ( -5300 -2700 )
      + RECT via3 ( -5100 -2900 ) ( -4900 -2700 )
      + RECT via3 ( -4700 -2900 ) ( -4500 -2700 )
      + RECT via3 ( -4300 -2900 ) ( -4100 -2700 )
      + RECT via3 ( -3900 -2900 ) ( -3700 -2700 )
      + RECT via3 ( -3500 -2900 ) ( -3300 -2700 )
      + RECT via3 ( -3100 -2900 ) ( -2900 -2700 )
      + RECT via3 ( -2700 -2900 ) ( -2500 -2700 )
      + RECT via3 ( -2300 -2900 ) ( -2100 -2700 )
      + RECT via3 ( -1900 -2900 ) ( -1700 -2700 )
      + RECT via3 ( -1500 -2900 ) ( -1300 -2700 )
      + RECT via3 ( -1100 -2900 ) ( -900 -2700 )
      + RECT via3 ( -700 -2900 ) ( -500 -2700 )
      + RECT via3 ( -300 -2900 ) ( -100 -2700 )
      + RECT via3 ( 100 -2900 ) ( 300 -2700 )
      + RECT via3 ( 500 -2900 ) ( 700 -2700 )
      + RECT via3 ( 900 -2900 ) ( 1100 -2700 )
      + RECT via3 ( 1300 -2900 ) ( 1500 -2700 )
      + RECT via3 ( 1700 -2900 ) ( 1900 -2700 )
      + RECT via3 ( 2100 -2900 ) ( 2300 -2700 )
      + RECT via3 ( 2500 -2900 ) ( 2700 -2700 )
      + RECT via3 ( 2900 -2900 ) ( 3100 -2700 )
      + RECT via3 ( 3300 -2900 ) ( 3500 -2700 )
      + RECT via3 ( 3700 -2900 ) ( 3900 -2700 )
      + RECT via3 ( 4100 -2900 ) ( 4300 -2700 )
      + RECT via3 ( 4500 -2900 ) ( 4700 -2700 )
      + RECT via3 ( 4900 -2900 ) ( 5100 -2700 )
      + RECT via3 ( 5300 -2900 ) ( 5500 -2700 )
      + RECT via3 ( 5700 -2900 ) ( 5900 -2700 )
      + RECT via3 ( -5900 -2500 ) ( -5700 -2300 )
      + RECT via3 ( -5500 -2500 ) ( -5300 -2300 )
      + RECT via3 ( -5100 -2500 ) ( -4900 -2300 )
      + RECT via3 ( -4700 -2500 ) ( -4500 -2300 )
      + RECT via3 ( -4300 -2500 ) ( -4100 -2300 )
      + RECT via3 ( -3900 -2500 ) ( -3700 -2300 )
      + RECT via3 ( -3500 -2500 ) ( -3300 -2300 )
      + RECT via3 ( -3100 -2500 ) ( -2900 -2300 )
      + RECT via3 ( -2700 -2500 ) ( -2500 -2300 )
      + RECT via3 ( -2300 -2500 ) ( -2100 -2300 )
      + RECT via3 ( -1900 -2500 ) ( -1700 -2300 )
      + RECT via3 ( -1500 -2500 ) ( -1300 -2300 )
      + RECT via3 ( -1100 -2500 ) ( -900 -2300 )
      + RECT via3 ( -700 -2500 ) ( -500 -2300 )
      + RECT via3 ( -300 -2500 ) ( -100 -2300 )
      + RECT via3 ( 100 -2500 ) ( 300 -2300 )
      + RECT via3 ( 500 -2500 ) ( 700 -2300 )
      + RECT via3 ( 900 -2500 ) ( 1100 -2300 )
      + RECT via3 ( 1300 -2500 ) ( 1500 -2300 )
      + RECT via3 ( 1700 -2500 ) ( 1900 -2300 )
      + RECT via3 ( 2100 -2500 ) ( 2300 -2300 )
      + RECT via3 ( 2500 -2500 ) ( 2700 -2300 )
      + RECT via3 ( 2900 -2500 ) ( 3100 -2300 )
      + RECT via3 ( 3300 -2500 ) ( 3500 -2300 )
      + RECT via3 ( 3700 -2500 ) ( 3900 -2300 )
      + RECT via3 ( 4100 -2500 ) ( 4300 -2300 )
      + RECT via3 ( 4500 -2500 ) ( 4700 -2300 )
      + RECT via3 ( 4900 -2500 ) ( 5100 -2300 )
      + RECT via3 ( 5300 -2500 ) ( 5500 -2300 )
      + RECT via3 ( 5700 -2500 ) ( 5900 -2300 )
      + RECT via3 ( -5900 -2100 ) ( -5700 -1900 )
      + RECT via3 ( -5500 -2100 ) ( -5300 -1900 )
      + RECT via3 ( -5100 -2100 ) ( -4900 -1900 )
      + RECT via3 ( -4700 -2100 ) ( -4500 -1900 )
      + RECT via3 ( -4300 -2100 ) ( -4100 -1900 )
      + RECT via3 ( -3900 -2100 ) ( -3700 -1900 )
      + RECT via3 ( -3500 -2100 ) ( -3300 -1900 )
      + RECT via3 ( -3100 -2100 ) ( -2900 -1900 )
      + RECT via3 ( -2700 -2100 ) ( -2500 -1900 )
      + RECT via3 ( -2300 -2100 ) ( -2100 -1900 )
      + RECT via3 ( -1900 -2100 ) ( -1700 -1900 )
      + RECT via3 ( -1500 -2100 ) ( -1300 -1900 )
      + RECT via3 ( -1100 -2100 ) ( -900 -1900 )
      + RECT via3 ( -700 -2100 ) ( -500 -1900 )
      + RECT via3 ( -300 -2100 ) ( -100 -1900 )
      + RECT via3 ( 100 -2100 ) ( 300 -1900 )
      + RECT via3 ( 500 -2100 ) ( 700 -1900 )
      + RECT via3 ( 900 -2100 ) ( 1100 -1900 )
      + RECT via3 ( 1300 -2100 ) ( 1500 -1900 )
      + RECT via3 ( 1700 -2100 ) ( 1900 -1900 )
      + RECT via3 ( 2100 -2100 ) ( 2300 -1900 )
      + RECT via3 ( 2500 -2100 ) ( 2700 -1900 )
      + RECT via3 ( 2900 -2100 ) ( 3100 -1900 )
      + RECT via3 ( 3300 -2100 ) ( 3500 -1900 )
      + RECT via3 ( 3700 -2100 ) ( 3900 -1900 )
      + RECT via3 ( 4100 -2100 ) ( 4300 -1900 )
      + RECT via3 ( 4500 -2100 ) ( 4700 -1900 )
      + RECT via3 ( 4900 -2100 ) ( 5100 -1900 )
      + RECT via3 ( 5300 -2100 ) ( 5500 -1900 )
      + RECT via3 ( 5700 -2100 ) ( 5900 -1900 )
      + RECT via3 ( -5900 -1700 ) ( -5700 -1500 )
      + RECT via3 ( -5500 -1700 ) ( -5300 -1500 )
      + RECT via3 ( -5100 -1700 ) ( -4900 -1500 )
      + RECT via3 ( -4700 -1700 ) ( -4500 -1500 )
      + RECT via3 ( -4300 -1700 ) ( -4100 -1500 )
      + RECT via3 ( -3900 -1700 ) ( -3700 -1500 )
      + RECT via3 ( -3500 -1700 ) ( -3300 -1500 )
      + RECT via3 ( -3100 -1700 ) ( -2900 -1500 )
      + RECT via3 ( -2700 -1700 ) ( -2500 -1500 )
      + RECT via3 ( -2300 -1700 ) ( -2100 -1500 )
      + RECT via3 ( -1900 -1700 ) ( -1700 -1500 )
      + RECT via3 ( -1500 -1700 ) ( -1300 -1500 )
      + RECT via3 ( -1100 -1700 ) ( -900 -1500 )
      + RECT via3 ( -700 -1700 ) ( -500 -1500 )
      + RECT via3 ( -300 -1700 ) ( -100 -1500 )
      + RECT via3 ( 100 -1700 ) ( 300 -1500 )
      + RECT via3 ( 500 -1700 ) ( 700 -1500 )
      + RECT via3 ( 900 -1700 ) ( 1100 -1500 )
      + RECT via3 ( 1300 -1700 ) ( 1500 -1500 )
      + RECT via3 ( 1700 -1700 ) ( 1900 -1500 )
      + RECT via3 ( 2100 -1700 ) ( 2300 -1500 )
      + RECT via3 ( 2500 -1700 ) ( 2700 -1500 )
      + RECT via3 ( 2900 -1700 ) ( 3100 -1500 )
      + RECT via3 ( 3300 -1700 ) ( 3500 -1500 )
      + RECT via3 ( 3700 -1700 ) ( 3900 -1500 )
      + RECT via3 ( 4100 -1700 ) ( 4300 -1500 )
      + RECT via3 ( 4500 -1700 ) ( 4700 -1500 )
      + RECT via3 ( 4900 -1700 ) ( 5100 -1500 )
      + RECT via3 ( 5300 -1700 ) ( 5500 -1500 )
      + RECT via3 ( 5700 -1700 ) ( 5900 -1500 )
      + RECT via3 ( -5900 -1300 ) ( -5700 -1100 )
      + RECT via3 ( -5500 -1300 ) ( -5300 -1100 )
      + RECT via3 ( -5100 -1300 ) ( -4900 -1100 )
      + RECT via3 ( -4700 -1300 ) ( -4500 -1100 )
      + RECT via3 ( -4300 -1300 ) ( -4100 -1100 )
      + RECT via3 ( -3900 -1300 ) ( -3700 -1100 )
      + RECT via3 ( -3500 -1300 ) ( -3300 -1100 )
      + RECT via3 ( -3100 -1300 ) ( -2900 -1100 )
      + RECT via3 ( -2700 -1300 ) ( -2500 -1100 )
      + RECT via3 ( -2300 -1300 ) ( -2100 -1100 )
      + RECT via3 ( -1900 -1300 ) ( -1700 -1100 )
      + RECT via3 ( -1500 -1300 ) ( -1300 -1100 )
      + RECT via3 ( -1100 -1300 ) ( -900 -1100 )
      + RECT via3 ( -700 -1300 ) ( -500 -1100 )
      + RECT via3 ( -300 -1300 ) ( -100 -1100 )
      + RECT via3 ( 100 -1300 ) ( 300 -1100 )
      + RECT via3 ( 500 -1300 ) ( 700 -1100 )
      + RECT via3 ( 900 -1300 ) ( 1100 -1100 )
      + RECT via3 ( 1300 -1300 ) ( 1500 -1100 )
      + RECT via3 ( 1700 -1300 ) ( 1900 -1100 )
      + RECT via3 ( 2100 -1300 ) ( 2300 -1100 )
      + RECT via3 ( 2500 -1300 ) ( 2700 -1100 )
      + RECT via3 ( 2900 -1300 ) ( 3100 -1100 )
      + RECT via3 ( 3300 -1300 ) ( 3500 -1100 )
      + RECT via3 ( 3700 -1300 ) ( 3900 -1100 )
      + RECT via3 ( 4100 -1300 ) ( 4300 -1100 )
      + RECT via3 ( 4500 -1300 ) ( 4700 -1100 )
      + RECT via3 ( 4900 -1300 ) ( 5100 -1100 )
      + RECT via3 ( 5300 -1300 ) ( 5500 -1100 )
      + RECT via3 ( 5700 -1300 ) ( 5900 -1100 )
      + RECT via3 ( -5900 -900 ) ( -5700 -700 )
      + RECT via3 ( -5500 -900 ) ( -5300 -700 )
      + RECT via3 ( -5100 -900 ) ( -4900 -700 )
      + RECT via3 ( -4700 -900 ) ( -4500 -700 )
      + RECT via3 ( -4300 -900 ) ( -4100 -700 )
      + RECT via3 ( -3900 -900 ) ( -3700 -700 )
      + RECT via3 ( -3500 -900 ) ( -3300 -700 )
      + RECT via3 ( -3100 -900 ) ( -2900 -700 )
      + RECT via3 ( -2700 -900 ) ( -2500 -700 )
      + RECT via3 ( -2300 -900 ) ( -2100 -700 )
      + RECT via3 ( -1900 -900 ) ( -1700 -700 )
      + RECT via3 ( -1500 -900 ) ( -1300 -700 )
      + RECT via3 ( -1100 -900 ) ( -900 -700 )
      + RECT via3 ( -700 -900 ) ( -500 -700 )
      + RECT via3 ( -300 -900 ) ( -100 -700 )
      + RECT via3 ( 100 -900 ) ( 300 -700 )
      + RECT via3 ( 500 -900 ) ( 700 -700 )
      + RECT via3 ( 900 -900 ) ( 1100 -700 )
      + RECT via3 ( 1300 -900 ) ( 1500 -700 )
      + RECT via3 ( 1700 -900 ) ( 1900 -700 )
      + RECT via3 ( 2100 -900 ) ( 2300 -700 )
      + RECT via3 ( 2500 -900 ) ( 2700 -700 )
      + RECT via3 ( 2900 -900 ) ( 3100 -700 )
      + RECT via3 ( 3300 -900 ) ( 3500 -700 )
      + RECT via3 ( 3700 -900 ) ( 3900 -700 )
      + RECT via3 ( 4100 -900 ) ( 4300 -700 )
      + RECT via3 ( 4500 -900 ) ( 4700 -700 )
      + RECT via3 ( 4900 -900 ) ( 5100 -700 )
      + RECT via3 ( 5300 -900 ) ( 5500 -700 )
      + RECT via3 ( 5700 -900 ) ( 5900 -700 )
      + RECT via3 ( -5900 -500 ) ( -5700 -300 )
      + RECT via3 ( -5500 -500 ) ( -5300 -300 )
      + RECT via3 ( -5100 -500 ) ( -4900 -300 )
      + RECT via3 ( -4700 -500 ) ( -4500 -300 )
      + RECT via3 ( -4300 -500 ) ( -4100 -300 )
      + RECT via3 ( -3900 -500 ) ( -3700 -300 )
      + RECT via3 ( -3500 -500 ) ( -3300 -300 )
      + RECT via3 ( -3100 -500 ) ( -2900 -300 )
      + RECT via3 ( -2700 -500 ) ( -2500 -300 )
      + RECT via3 ( -2300 -500 ) ( -2100 -300 )
      + RECT via3 ( -1900 -500 ) ( -1700 -300 )
      + RECT via3 ( -1500 -500 ) ( -1300 -300 )
      + RECT via3 ( -1100 -500 ) ( -900 -300 )
      + RECT via3 ( -700 -500 ) ( -500 -300 )
      + RECT via3 ( -300 -500 ) ( -100 -300 )
      + RECT via3 ( 100 -500 ) ( 300 -300 )
      + RECT via3 ( 500 -500 ) ( 700 -300 )
      + RECT via3 ( 900 -500 ) ( 1100 -300 )
      + RECT via3 ( 1300 -500 ) ( 1500 -300 )
      + RECT via3 ( 1700 -500 ) ( 1900 -300 )
      + RECT via3 ( 2100 -500 ) ( 2300 -300 )
      + RECT via3 ( 2500 -500 ) ( 2700 -300 )
      + RECT via3 ( 2900 -500 ) ( 3100 -300 )
      + RECT via3 ( 3300 -500 ) ( 3500 -300 )
      + RECT via3 ( 3700 -500 ) ( 3900 -300 )
      + RECT via3 ( 4100 -500 ) ( 4300 -300 )
      + RECT via3 ( 4500 -500 ) ( 4700 -300 )
      + RECT via3 ( 4900 -500 ) ( 5100 -300 )
      + RECT via3 ( 5300 -500 ) ( 5500 -300 )
      + RECT via3 ( 5700 -500 ) ( 5900 -300 )
      + RECT via3 ( -5900 -100 ) ( -5700 100 )
      + RECT via3 ( -5500 -100 ) ( -5300 100 )
      + RECT via3 ( -5100 -100 ) ( -4900 100 )
      + RECT via3 ( -4700 -100 ) ( -4500 100 )
      + RECT via3 ( -4300 -100 ) ( -4100 100 )
      + RECT via3 ( -3900 -100 ) ( -3700 100 )
      + RECT via3 ( -3500 -100 ) ( -3300 100 )
      + RECT via3 ( -3100 -100 ) ( -2900 100 )
      + RECT via3 ( -2700 -100 ) ( -2500 100 )
      + RECT via3 ( -2300 -100 ) ( -2100 100 )
      + RECT via3 ( -1900 -100 ) ( -1700 100 )
      + RECT via3 ( -1500 -100 ) ( -1300 100 )
      + RECT via3 ( -1100 -100 ) ( -900 100 )
      + RECT via3 ( -700 -100 ) ( -500 100 )
      + RECT via3 ( -300 -100 ) ( -100 100 )
      + RECT via3 ( 100 -100 ) ( 300 100 )
      + RECT via3 ( 500 -100 ) ( 700 100 )
      + RECT via3 ( 900 -100 ) ( 1100 100 )
      + RECT via3 ( 1300 -100 ) ( 1500 100 )
      + RECT via3 ( 1700 -100 ) ( 1900 100 )
      + RECT via3 ( 2100 -100 ) ( 2300 100 )
      + RECT via3 ( 2500 -100 ) ( 2700 100 )
      + RECT via3 ( 2900 -100 ) ( 3100 100 )
      + RECT via3 ( 3300 -100 ) ( 3500 100 )
      + RECT via3 ( 3700 -100 ) ( 3900 100 )
      + RECT via3 ( 4100 -100 ) ( 4300 100 )
      + RECT via3 ( 4500 -100 ) ( 4700 100 )
      + RECT via3 ( 4900 -100 ) ( 5100 100 )
      + RECT via3 ( 5300 -100 ) ( 5500 100 )
      + RECT via3 ( 5700 -100 ) ( 5900 100 )
      + RECT via3 ( -5900 300 ) ( -5700 500 )
      + RECT via3 ( -5500 300 ) ( -5300 500 )
      + RECT via3 ( -5100 300 ) ( -4900 500 )
      + RECT via3 ( -4700 300 ) ( -4500 500 )
      + RECT via3 ( -4300 300 ) ( -4100 500 )
      + RECT via3 ( -3900 300 ) ( -3700 500 )
      + RECT via3 ( -3500 300 ) ( -3300 500 )
      + RECT via3 ( -3100 300 ) ( -2900 500 )
      + RECT via3 ( -2700 300 ) ( -2500 500 )
      + RECT via3 ( -2300 300 ) ( -2100 500 )
      + RECT via3 ( -1900 300 ) ( -1700 500 )
      + RECT via3 ( -1500 300 ) ( -1300 500 )
      + RECT via3 ( -1100 300 ) ( -900 500 )
      + RECT via3 ( -700 300 ) ( -500 500 )
      + RECT via3 ( -300 300 ) ( -100 500 )
      + RECT via3 ( 100 300 ) ( 300 500 )
      + RECT via3 ( 500 300 ) ( 700 500 )
      + RECT via3 ( 900 300 ) ( 1100 500 )
      + RECT via3 ( 1300 300 ) ( 1500 500 )
      + RECT via3 ( 1700 300 ) ( 1900 500 )
      + RECT via3 ( 2100 300 ) ( 2300 500 )
      + RECT via3 ( 2500 300 ) ( 2700 500 )
      + RECT via3 ( 2900 300 ) ( 3100 500 )
      + RECT via3 ( 3300 300 ) ( 3500 500 )
      + RECT via3 ( 3700 300 ) ( 3900 500 )
      + RECT via3 ( 4100 300 ) ( 4300 500 )
      + RECT via3 ( 4500 300 ) ( 4700 500 )
      + RECT via3 ( 4900 300 ) ( 5100 500 )
      + RECT via3 ( 5300 300 ) ( 5500 500 )
      + RECT via3 ( 5700 300 ) ( 5900 500 )
      + RECT via3 ( -5900 700 ) ( -5700 900 )
      + RECT via3 ( -5500 700 ) ( -5300 900 )
      + RECT via3 ( -5100 700 ) ( -4900 900 )
      + RECT via3 ( -4700 700 ) ( -4500 900 )
      + RECT via3 ( -4300 700 ) ( -4100 900 )
      + RECT via3 ( -3900 700 ) ( -3700 900 )
      + RECT via3 ( -3500 700 ) ( -3300 900 )
      + RECT via3 ( -3100 700 ) ( -2900 900 )
      + RECT via3 ( -2700 700 ) ( -2500 900 )
      + RECT via3 ( -2300 700 ) ( -2100 900 )
      + RECT via3 ( -1900 700 ) ( -1700 900 )
      + RECT via3 ( -1500 700 ) ( -1300 900 )
      + RECT via3 ( -1100 700 ) ( -900 900 )
      + RECT via3 ( -700 700 ) ( -500 900 )
      + RECT via3 ( -300 700 ) ( -100 900 )
      + RECT via3 ( 100 700 ) ( 300 900 )
      + RECT via3 ( 500 700 ) ( 700 900 )
      + RECT via3 ( 900 700 ) ( 1100 900 )
      + RECT via3 ( 1300 700 ) ( 1500 900 )
      + RECT via3 ( 1700 700 ) ( 1900 900 )
      + RECT via3 ( 2100 700 ) ( 2300 900 )
      + RECT via3 ( 2500 700 ) ( 2700 900 )
      + RECT via3 ( 2900 700 ) ( 3100 900 )
      + RECT via3 ( 3300 700 ) ( 3500 900 )
      + RECT via3 ( 3700 700 ) ( 3900 900 )
      + RECT via3 ( 4100 700 ) ( 4300 900 )
      + RECT via3 ( 4500 700 ) ( 4700 900 )
      + RECT via3 ( 4900 700 ) ( 5100 900 )
      + RECT via3 ( 5300 700 ) ( 5500 900 )
      + RECT via3 ( 5700 700 ) ( 5900 900 )
      + RECT via3 ( -5900 1100 ) ( -5700 1300 )
      + RECT via3 ( -5500 1100 ) ( -5300 1300 )
      + RECT via3 ( -5100 1100 ) ( -4900 1300 )
      + RECT via3 ( -4700 1100 ) ( -4500 1300 )
      + RECT via3 ( -4300 1100 ) ( -4100 1300 )
      + RECT via3 ( -3900 1100 ) ( -3700 1300 )
      + RECT via3 ( -3500 1100 ) ( -3300 1300 )
      + RECT via3 ( -3100 1100 ) ( -2900 1300 )
      + RECT via3 ( -2700 1100 ) ( -2500 1300 )
      + RECT via3 ( -2300 1100 ) ( -2100 1300 )
      + RECT via3 ( -1900 1100 ) ( -1700 1300 )
      + RECT via3 ( -1500 1100 ) ( -1300 1300 )
      + RECT via3 ( -1100 1100 ) ( -900 1300 )
      + RECT via3 ( -700 1100 ) ( -500 1300 )
      + RECT via3 ( -300 1100 ) ( -100 1300 )
      + RECT via3 ( 100 1100 ) ( 300 1300 )
      + RECT via3 ( 500 1100 ) ( 700 1300 )
      + RECT via3 ( 900 1100 ) ( 1100 1300 )
      + RECT via3 ( 1300 1100 ) ( 1500 1300 )
      + RECT via3 ( 1700 1100 ) ( 1900 1300 )
      + RECT via3 ( 2100 1100 ) ( 2300 1300 )
      + RECT via3 ( 2500 1100 ) ( 2700 1300 )
      + RECT via3 ( 2900 1100 ) ( 3100 1300 )
      + RECT via3 ( 3300 1100 ) ( 3500 1300 )
      + RECT via3 ( 3700 1100 ) ( 3900 1300 )
      + RECT via3 ( 4100 1100 ) ( 4300 1300 )
      + RECT via3 ( 4500 1100 ) ( 4700 1300 )
      + RECT via3 ( 4900 1100 ) ( 5100 1300 )
      + RECT via3 ( 5300 1100 ) ( 5500 1300 )
      + RECT via3 ( 5700 1100 ) ( 5900 1300 )
      + RECT via3 ( -5900 1500 ) ( -5700 1700 )
      + RECT via3 ( -5500 1500 ) ( -5300 1700 )
      + RECT via3 ( -5100 1500 ) ( -4900 1700 )
      + RECT via3 ( -4700 1500 ) ( -4500 1700 )
      + RECT via3 ( -4300 1500 ) ( -4100 1700 )
      + RECT via3 ( -3900 1500 ) ( -3700 1700 )
      + RECT via3 ( -3500 1500 ) ( -3300 1700 )
      + RECT via3 ( -3100 1500 ) ( -2900 1700 )
      + RECT via3 ( -2700 1500 ) ( -2500 1700 )
      + RECT via3 ( -2300 1500 ) ( -2100 1700 )
      + RECT via3 ( -1900 1500 ) ( -1700 1700 )
      + RECT via3 ( -1500 1500 ) ( -1300 1700 )
      + RECT via3 ( -1100 1500 ) ( -900 1700 )
      + RECT via3 ( -700 1500 ) ( -500 1700 )
      + RECT via3 ( -300 1500 ) ( -100 1700 )
      + RECT via3 ( 100 1500 ) ( 300 1700 )
      + RECT via3 ( 500 1500 ) ( 700 1700 )
      + RECT via3 ( 900 1500 ) ( 1100 1700 )
      + RECT via3 ( 1300 1500 ) ( 1500 1700 )
      + RECT via3 ( 1700 1500 ) ( 1900 1700 )
      + RECT via3 ( 2100 1500 ) ( 2300 1700 )
      + RECT via3 ( 2500 1500 ) ( 2700 1700 )
      + RECT via3 ( 2900 1500 ) ( 3100 1700 )
      + RECT via3 ( 3300 1500 ) ( 3500 1700 )
      + RECT via3 ( 3700 1500 ) ( 3900 1700 )
      + RECT via3 ( 4100 1500 ) ( 4300 1700 )
      + RECT via3 ( 4500 1500 ) ( 4700 1700 )
      + RECT via3 ( 4900 1500 ) ( 5100 1700 )
      + RECT via3 ( 5300 1500 ) ( 5500 1700 )
      + RECT via3 ( 5700 1500 ) ( 5900 1700 )
      + RECT via3 ( -5900 1900 ) ( -5700 2100 )
      + RECT via3 ( -5500 1900 ) ( -5300 2100 )
      + RECT via3 ( -5100 1900 ) ( -4900 2100 )
      + RECT via3 ( -4700 1900 ) ( -4500 2100 )
      + RECT via3 ( -4300 1900 ) ( -4100 2100 )
      + RECT via3 ( -3900 1900 ) ( -3700 2100 )
      + RECT via3 ( -3500 1900 ) ( -3300 2100 )
      + RECT via3 ( -3100 1900 ) ( -2900 2100 )
      + RECT via3 ( -2700 1900 ) ( -2500 2100 )
      + RECT via3 ( -2300 1900 ) ( -2100 2100 )
      + RECT via3 ( -1900 1900 ) ( -1700 2100 )
      + RECT via3 ( -1500 1900 ) ( -1300 2100 )
      + RECT via3 ( -1100 1900 ) ( -900 2100 )
      + RECT via3 ( -700 1900 ) ( -500 2100 )
      + RECT via3 ( -300 1900 ) ( -100 2100 )
      + RECT via3 ( 100 1900 ) ( 300 2100 )
      + RECT via3 ( 500 1900 ) ( 700 2100 )
      + RECT via3 ( 900 1900 ) ( 1100 2100 )
      + RECT via3 ( 1300 1900 ) ( 1500 2100 )
      + RECT via3 ( 1700 1900 ) ( 1900 2100 )
      + RECT via3 ( 2100 1900 ) ( 2300 2100 )
      + RECT via3 ( 2500 1900 ) ( 2700 2100 )
      + RECT via3 ( 2900 1900 ) ( 3100 2100 )
      + RECT via3 ( 3300 1900 ) ( 3500 2100 )
      + RECT via3 ( 3700 1900 ) ( 3900 2100 )
      + RECT via3 ( 4100 1900 ) ( 4300 2100 )
      + RECT via3 ( 4500 1900 ) ( 4700 2100 )
      + RECT via3 ( 4900 1900 ) ( 5100 2100 )
      + RECT via3 ( 5300 1900 ) ( 5500 2100 )
      + RECT via3 ( 5700 1900 ) ( 5900 2100 )
      + RECT via3 ( -5900 2300 ) ( -5700 2500 )
      + RECT via3 ( -5500 2300 ) ( -5300 2500 )
      + RECT via3 ( -5100 2300 ) ( -4900 2500 )
      + RECT via3 ( -4700 2300 ) ( -4500 2500 )
      + RECT via3 ( -4300 2300 ) ( -4100 2500 )
      + RECT via3 ( -3900 2300 ) ( -3700 2500 )
      + RECT via3 ( -3500 2300 ) ( -3300 2500 )
      + RECT via3 ( -3100 2300 ) ( -2900 2500 )
      + RECT via3 ( -2700 2300 ) ( -2500 2500 )
      + RECT via3 ( -2300 2300 ) ( -2100 2500 )
      + RECT via3 ( -1900 2300 ) ( -1700 2500 )
      + RECT via3 ( -1500 2300 ) ( -1300 2500 )
      + RECT via3 ( -1100 2300 ) ( -900 2500 )
      + RECT via3 ( -700 2300 ) ( -500 2500 )
      + RECT via3 ( -300 2300 ) ( -100 2500 )
      + RECT via3 ( 100 2300 ) ( 300 2500 )
      + RECT via3 ( 500 2300 ) ( 700 2500 )
      + RECT via3 ( 900 2300 ) ( 1100 2500 )
      + RECT via3 ( 1300 2300 ) ( 1500 2500 )
      + RECT via3 ( 1700 2300 ) ( 1900 2500 )
      + RECT via3 ( 2100 2300 ) ( 2300 2500 )
      + RECT via3 ( 2500 2300 ) ( 2700 2500 )
      + RECT via3 ( 2900 2300 ) ( 3100 2500 )
      + RECT via3 ( 3300 2300 ) ( 3500 2500 )
      + RECT via3 ( 3700 2300 ) ( 3900 2500 )
      + RECT via3 ( 4100 2300 ) ( 4300 2500 )
      + RECT via3 ( 4500 2300 ) ( 4700 2500 )
      + RECT via3 ( 4900 2300 ) ( 5100 2500 )
      + RECT via3 ( 5300 2300 ) ( 5500 2500 )
      + RECT via3 ( 5700 2300 ) ( 5900 2500 )
      + RECT via3 ( -5900 2700 ) ( -5700 2900 )
      + RECT via3 ( -5500 2700 ) ( -5300 2900 )
      + RECT via3 ( -5100 2700 ) ( -4900 2900 )
      + RECT via3 ( -4700 2700 ) ( -4500 2900 )
      + RECT via3 ( -4300 2700 ) ( -4100 2900 )
      + RECT via3 ( -3900 2700 ) ( -3700 2900 )
      + RECT via3 ( -3500 2700 ) ( -3300 2900 )
      + RECT via3 ( -3100 2700 ) ( -2900 2900 )
      + RECT via3 ( -2700 2700 ) ( -2500 2900 )
      + RECT via3 ( -2300 2700 ) ( -2100 2900 )
      + RECT via3 ( -1900 2700 ) ( -1700 2900 )
      + RECT via3 ( -1500 2700 ) ( -1300 2900 )
      + RECT via3 ( -1100 2700 ) ( -900 2900 )
      + RECT via3 ( -700 2700 ) ( -500 2900 )
      + RECT via3 ( -300 2700 ) ( -100 2900 )
      + RECT via3 ( 100 2700 ) ( 300 2900 )
      + RECT via3 ( 500 2700 ) ( 700 2900 )
      + RECT via3 ( 900 2700 ) ( 1100 2900 )
      + RECT via3 ( 1300 2700 ) ( 1500 2900 )
      + RECT via3 ( 1700 2700 ) ( 1900 2900 )
      + RECT via3 ( 2100 2700 ) ( 2300 2900 )
      + RECT via3 ( 2500 2700 ) ( 2700 2900 )
      + RECT via3 ( 2900 2700 ) ( 3100 2900 )
      + RECT via3 ( 3300 2700 ) ( 3500 2900 )
      + RECT via3 ( 3700 2700 ) ( 3900 2900 )
      + RECT via3 ( 4100 2700 ) ( 4300 2900 )
      + RECT via3 ( 4500 2700 ) ( 4700 2900 )
      + RECT via3 ( 4900 2700 ) ( 5100 2900 )
      + RECT via3 ( 5300 2700 ) ( 5500 2900 )
      + RECT via3 ( 5700 2700 ) ( 5900 2900 )
      + RECT via3 ( -5900 3100 ) ( -5700 3300 )
      + RECT via3 ( -5500 3100 ) ( -5300 3300 )
      + RECT via3 ( -5100 3100 ) ( -4900 3300 )
      + RECT via3 ( -4700 3100 ) ( -4500 3300 )
      + RECT via3 ( -4300 3100 ) ( -4100 3300 )
      + RECT via3 ( -3900 3100 ) ( -3700 3300 )
      + RECT via3 ( -3500 3100 ) ( -3300 3300 )
      + RECT via3 ( -3100 3100 ) ( -2900 3300 )
      + RECT via3 ( -2700 3100 ) ( -2500 3300 )
      + RECT via3 ( -2300 3100 ) ( -2100 3300 )
      + RECT via3 ( -1900 3100 ) ( -1700 3300 )
      + RECT via3 ( -1500 3100 ) ( -1300 3300 )
      + RECT via3 ( -1100 3100 ) ( -900 3300 )
      + RECT via3 ( -700 3100 ) ( -500 3300 )
      + RECT via3 ( -300 3100 ) ( -100 3300 )
      + RECT via3 ( 100 3100 ) ( 300 3300 )
      + RECT via3 ( 500 3100 ) ( 700 3300 )
      + RECT via3 ( 900 3100 ) ( 1100 3300 )
      + RECT via3 ( 1300 3100 ) ( 1500 3300 )
      + RECT via3 ( 1700 3100 ) ( 1900 3300 )
      + RECT via3 ( 2100 3100 ) ( 2300 3300 )
      + RECT via3 ( 2500 3100 ) ( 2700 3300 )
      + RECT via3 ( 2900 3100 ) ( 3100 3300 )
      + RECT via3 ( 3300 3100 ) ( 3500 3300 )
      + RECT via3 ( 3700 3100 ) ( 3900 3300 )
      + RECT via3 ( 4100 3100 ) ( 4300 3300 )
      + RECT via3 ( 4500 3100 ) ( 4700 3300 )
      + RECT via3 ( 4900 3100 ) ( 5100 3300 )
      + RECT via3 ( 5300 3100 ) ( 5500 3300 )
      + RECT via3 ( 5700 3100 ) ( 5900 3300 )
      + RECT via3 ( -5900 3500 ) ( -5700 3700 )
      + RECT via3 ( -5500 3500 ) ( -5300 3700 )
      + RECT via3 ( -5100 3500 ) ( -4900 3700 )
      + RECT via3 ( -4700 3500 ) ( -4500 3700 )
      + RECT via3 ( -4300 3500 ) ( -4100 3700 )
      + RECT via3 ( -3900 3500 ) ( -3700 3700 )
      + RECT via3 ( -3500 3500 ) ( -3300 3700 )
      + RECT via3 ( -3100 3500 ) ( -2900 3700 )
      + RECT via3 ( -2700 3500 ) ( -2500 3700 )
      + RECT via3 ( -2300 3500 ) ( -2100 3700 )
      + RECT via3 ( -1900 3500 ) ( -1700 3700 )
      + RECT via3 ( -1500 3500 ) ( -1300 3700 )
      + RECT via3 ( -1100 3500 ) ( -900 3700 )
      + RECT via3 ( -700 3500 ) ( -500 3700 )
      + RECT via3 ( -300 3500 ) ( -100 3700 )
      + RECT via3 ( 100 3500 ) ( 300 3700 )
      + RECT via3 ( 500 3500 ) ( 700 3700 )
      + RECT via3 ( 900 3500 ) ( 1100 3700 )
      + RECT via3 ( 1300 3500 ) ( 1500 3700 )
      + RECT via3 ( 1700 3500 ) ( 1900 3700 )
      + RECT via3 ( 2100 3500 ) ( 2300 3700 )
      + RECT via3 ( 2500 3500 ) ( 2700 3700 )
      + RECT via3 ( 2900 3500 ) ( 3100 3700 )
      + RECT via3 ( 3300 3500 ) ( 3500 3700 )
      + RECT via3 ( 3700 3500 ) ( 3900 3700 )
      + RECT via3 ( 4100 3500 ) ( 4300 3700 )
      + RECT via3 ( 4500 3500 ) ( 4700 3700 )
      + RECT via3 ( 4900 3500 ) ( 5100 3700 )
      + RECT via3 ( 5300 3500 ) ( 5500 3700 )
      + RECT via3 ( 5700 3500 ) ( 5900 3700 )
      + RECT via3 ( -5900 3900 ) ( -5700 4100 )
      + RECT via3 ( -5500 3900 ) ( -5300 4100 )
      + RECT via3 ( -5100 3900 ) ( -4900 4100 )
      + RECT via3 ( -4700 3900 ) ( -4500 4100 )
      + RECT via3 ( -4300 3900 ) ( -4100 4100 )
      + RECT via3 ( -3900 3900 ) ( -3700 4100 )
      + RECT via3 ( -3500 3900 ) ( -3300 4100 )
      + RECT via3 ( -3100 3900 ) ( -2900 4100 )
      + RECT via3 ( -2700 3900 ) ( -2500 4100 )
      + RECT via3 ( -2300 3900 ) ( -2100 4100 )
      + RECT via3 ( -1900 3900 ) ( -1700 4100 )
      + RECT via3 ( -1500 3900 ) ( -1300 4100 )
      + RECT via3 ( -1100 3900 ) ( -900 4100 )
      + RECT via3 ( -700 3900 ) ( -500 4100 )
      + RECT via3 ( -300 3900 ) ( -100 4100 )
      + RECT via3 ( 100 3900 ) ( 300 4100 )
      + RECT via3 ( 500 3900 ) ( 700 4100 )
      + RECT via3 ( 900 3900 ) ( 1100 4100 )
      + RECT via3 ( 1300 3900 ) ( 1500 4100 )
      + RECT via3 ( 1700 3900 ) ( 1900 4100 )
      + RECT via3 ( 2100 3900 ) ( 2300 4100 )
      + RECT via3 ( 2500 3900 ) ( 2700 4100 )
      + RECT via3 ( 2900 3900 ) ( 3100 4100 )
      + RECT via3 ( 3300 3900 ) ( 3500 4100 )
      + RECT via3 ( 3700 3900 ) ( 3900 4100 )
      + RECT via3 ( 4100 3900 ) ( 4300 4100 )
      + RECT via3 ( 4500 3900 ) ( 4700 4100 )
      + RECT via3 ( 4900 3900 ) ( 5100 4100 )
      + RECT via3 ( 5300 3900 ) ( 5500 4100 )
      + RECT via3 ( 5700 3900 ) ( 5900 4100 )
      + RECT via3 ( -5900 4300 ) ( -5700 4500 )
      + RECT via3 ( -5500 4300 ) ( -5300 4500 )
      + RECT via3 ( -5100 4300 ) ( -4900 4500 )
      + RECT via3 ( -4700 4300 ) ( -4500 4500 )
      + RECT via3 ( -4300 4300 ) ( -4100 4500 )
      + RECT via3 ( -3900 4300 ) ( -3700 4500 )
      + RECT via3 ( -3500 4300 ) ( -3300 4500 )
      + RECT via3 ( -3100 4300 ) ( -2900 4500 )
      + RECT via3 ( -2700 4300 ) ( -2500 4500 )
      + RECT via3 ( -2300 4300 ) ( -2100 4500 )
      + RECT via3 ( -1900 4300 ) ( -1700 4500 )
      + RECT via3 ( -1500 4300 ) ( -1300 4500 )
      + RECT via3 ( -1100 4300 ) ( -900 4500 )
      + RECT via3 ( -700 4300 ) ( -500 4500 )
      + RECT via3 ( -300 4300 ) ( -100 4500 )
      + RECT via3 ( 100 4300 ) ( 300 4500 )
      + RECT via3 ( 500 4300 ) ( 700 4500 )
      + RECT via3 ( 900 4300 ) ( 1100 4500 )
      + RECT via3 ( 1300 4300 ) ( 1500 4500 )
      + RECT via3 ( 1700 4300 ) ( 1900 4500 )
      + RECT via3 ( 2100 4300 ) ( 2300 4500 )
      + RECT via3 ( 2500 4300 ) ( 2700 4500 )
      + RECT via3 ( 2900 4300 ) ( 3100 4500 )
      + RECT via3 ( 3300 4300 ) ( 3500 4500 )
      + RECT via3 ( 3700 4300 ) ( 3900 4500 )
      + RECT via3 ( 4100 4300 ) ( 4300 4500 )
      + RECT via3 ( 4500 4300 ) ( 4700 4500 )
      + RECT via3 ( 4900 4300 ) ( 5100 4500 )
      + RECT via3 ( 5300 4300 ) ( 5500 4500 )
      + RECT via3 ( 5700 4300 ) ( 5900 4500 )
      + RECT via3 ( -5900 4700 ) ( -5700 4900 )
      + RECT via3 ( -5500 4700 ) ( -5300 4900 )
      + RECT via3 ( -5100 4700 ) ( -4900 4900 )
      + RECT via3 ( -4700 4700 ) ( -4500 4900 )
      + RECT via3 ( -4300 4700 ) ( -4100 4900 )
      + RECT via3 ( -3900 4700 ) ( -3700 4900 )
      + RECT via3 ( -3500 4700 ) ( -3300 4900 )
      + RECT via3 ( -3100 4700 ) ( -2900 4900 )
      + RECT via3 ( -2700 4700 ) ( -2500 4900 )
      + RECT via3 ( -2300 4700 ) ( -2100 4900 )
      + RECT via3 ( -1900 4700 ) ( -1700 4900 )
      + RECT via3 ( -1500 4700 ) ( -1300 4900 )
      + RECT via3 ( -1100 4700 ) ( -900 4900 )
      + RECT via3 ( -700 4700 ) ( -500 4900 )
      + RECT via3 ( -300 4700 ) ( -100 4900 )
      + RECT via3 ( 100 4700 ) ( 300 4900 )
      + RECT via3 ( 500 4700 ) ( 700 4900 )
      + RECT via3 ( 900 4700 ) ( 1100 4900 )
      + RECT via3 ( 1300 4700 ) ( 1500 4900 )
      + RECT via3 ( 1700 4700 ) ( 1900 4900 )
      + RECT via3 ( 2100 4700 ) ( 2300 4900 )
      + RECT via3 ( 2500 4700 ) ( 2700 4900 )
      + RECT via3 ( 2900 4700 ) ( 3100 4900 )
      + RECT via3 ( 3300 4700 ) ( 3500 4900 )
      + RECT via3 ( 3700 4700 ) ( 3900 4900 )
      + RECT via3 ( 4100 4700 ) ( 4300 4900 )
      + RECT via3 ( 4500 4700 ) ( 4700 4900 )
      + RECT via3 ( 4900 4700 ) ( 5100 4900 )
      + RECT via3 ( 5300 4700 ) ( 5500 4900 )
      + RECT via3 ( 5700 4700 ) ( 5900 4900 )
      + RECT via3 ( -5900 5100 ) ( -5700 5300 )
      + RECT via3 ( -5500 5100 ) ( -5300 5300 )
      + RECT via3 ( -5100 5100 ) ( -4900 5300 )
      + RECT via3 ( -4700 5100 ) ( -4500 5300 )
      + RECT via3 ( -4300 5100 ) ( -4100 5300 )
      + RECT via3 ( -3900 5100 ) ( -3700 5300 )
      + RECT via3 ( -3500 5100 ) ( -3300 5300 )
      + RECT via3 ( -3100 5100 ) ( -2900 5300 )
      + RECT via3 ( -2700 5100 ) ( -2500 5300 )
      + RECT via3 ( -2300 5100 ) ( -2100 5300 )
      + RECT via3 ( -1900 5100 ) ( -1700 5300 )
      + RECT via3 ( -1500 5100 ) ( -1300 5300 )
      + RECT via3 ( -1100 5100 ) ( -900 5300 )
      + RECT via3 ( -700 5100 ) ( -500 5300 )
      + RECT via3 ( -300 5100 ) ( -100 5300 )
      + RECT via3 ( 100 5100 ) ( 300 5300 )
      + RECT via3 ( 500 5100 ) ( 700 5300 )
      + RECT via3 ( 900 5100 ) ( 1100 5300 )
      + RECT via3 ( 1300 5100 ) ( 1500 5300 )
      + RECT via3 ( 1700 5100 ) ( 1900 5300 )
      + RECT via3 ( 2100 5100 ) ( 2300 5300 )
      + RECT via3 ( 2500 5100 ) ( 2700 5300 )
      + RECT via3 ( 2900 5100 ) ( 3100 5300 )
      + RECT via3 ( 3300 5100 ) ( 3500 5300 )
      + RECT via3 ( 3700 5100 ) ( 3900 5300 )
      + RECT via3 ( 4100 5100 ) ( 4300 5300 )
      + RECT via3 ( 4500 5100 ) ( 4700 5300 )
      + RECT via3 ( 4900 5100 ) ( 5100 5300 )
      + RECT via3 ( 5300 5100 ) ( 5500 5300 )
      + RECT via3 ( 5700 5100 ) ( 5900 5300 )
      + RECT via3 ( -5900 5500 ) ( -5700 5700 )
      + RECT via3 ( -5500 5500 ) ( -5300 5700 )
      + RECT via3 ( -5100 5500 ) ( -4900 5700 )
      + RECT via3 ( -4700 5500 ) ( -4500 5700 )
      + RECT via3 ( -4300 5500 ) ( -4100 5700 )
      + RECT via3 ( -3900 5500 ) ( -3700 5700 )
      + RECT via3 ( -3500 5500 ) ( -3300 5700 )
      + RECT via3 ( -3100 5500 ) ( -2900 5700 )
      + RECT via3 ( -2700 5500 ) ( -2500 5700 )
      + RECT via3 ( -2300 5500 ) ( -2100 5700 )
      + RECT via3 ( -1900 5500 ) ( -1700 5700 )
      + RECT via3 ( -1500 5500 ) ( -1300 5700 )
      + RECT via3 ( -1100 5500 ) ( -900 5700 )
      + RECT via3 ( -700 5500 ) ( -500 5700 )
      + RECT via3 ( -300 5500 ) ( -100 5700 )
      + RECT via3 ( 100 5500 ) ( 300 5700 )
      + RECT via3 ( 500 5500 ) ( 700 5700 )
      + RECT via3 ( 900 5500 ) ( 1100 5700 )
      + RECT via3 ( 1300 5500 ) ( 1500 5700 )
      + RECT via3 ( 1700 5500 ) ( 1900 5700 )
      + RECT via3 ( 2100 5500 ) ( 2300 5700 )
      + RECT via3 ( 2500 5500 ) ( 2700 5700 )
      + RECT via3 ( 2900 5500 ) ( 3100 5700 )
      + RECT via3 ( 3300 5500 ) ( 3500 5700 )
      + RECT via3 ( 3700 5500 ) ( 3900 5700 )
      + RECT via3 ( 4100 5500 ) ( 4300 5700 )
      + RECT via3 ( 4500 5500 ) ( 4700 5700 )
      + RECT via3 ( 4900 5500 ) ( 5100 5700 )
      + RECT via3 ( 5300 5500 ) ( 5500 5700 )
      + RECT via3 ( 5700 5500 ) ( 5900 5700 )
      + RECT via3 ( -5900 5900 ) ( -5700 6100 )
      + RECT via3 ( -5500 5900 ) ( -5300 6100 )
      + RECT via3 ( -5100 5900 ) ( -4900 6100 )
      + RECT via3 ( -4700 5900 ) ( -4500 6100 )
      + RECT via3 ( -4300 5900 ) ( -4100 6100 )
      + RECT via3 ( -3900 5900 ) ( -3700 6100 )
      + RECT via3 ( -3500 5900 ) ( -3300 6100 )
      + RECT via3 ( -3100 5900 ) ( -2900 6100 )
      + RECT via3 ( -2700 5900 ) ( -2500 6100 )
      + RECT via3 ( -2300 5900 ) ( -2100 6100 )
      + RECT via3 ( -1900 5900 ) ( -1700 6100 )
      + RECT via3 ( -1500 5900 ) ( -1300 6100 )
      + RECT via3 ( -1100 5900 ) ( -900 6100 )
      + RECT via3 ( -700 5900 ) ( -500 6100 )
      + RECT via3 ( -300 5900 ) ( -100 6100 )
      + RECT via3 ( 100 5900 ) ( 300 6100 )
      + RECT via3 ( 500 5900 ) ( 700 6100 )
      + RECT via3 ( 900 5900 ) ( 1100 6100 )
      + RECT via3 ( 1300 5900 ) ( 1500 6100 )
      + RECT via3 ( 1700 5900 ) ( 1900 6100 )
      + RECT via3 ( 2100 5900 ) ( 2300 6100 )
      + RECT via3 ( 2500 5900 ) ( 2700 6100 )
      + RECT via3 ( 2900 5900 ) ( 3100 6100 )
      + RECT via3 ( 3300 5900 ) ( 3500 6100 )
      + RECT via3 ( 3700 5900 ) ( 3900 6100 )
      + RECT via3 ( 4100 5900 ) ( 4300 6100 )
      + RECT via3 ( 4500 5900 ) ( 4700 6100 )
      + RECT via3 ( 4900 5900 ) ( 5100 6100 )
      + RECT via3 ( 5300 5900 ) ( 5500 6100 )
      + RECT via3 ( 5700 5900 ) ( 5900 6100 )
      + RECT via3 ( -5900 6300 ) ( -5700 6500 )
      + RECT via3 ( -5500 6300 ) ( -5300 6500 )
      + RECT via3 ( -5100 6300 ) ( -4900 6500 )
      + RECT via3 ( -4700 6300 ) ( -4500 6500 )
      + RECT via3 ( -4300 6300 ) ( -4100 6500 )
      + RECT via3 ( -3900 6300 ) ( -3700 6500 )
      + RECT via3 ( -3500 6300 ) ( -3300 6500 )
      + RECT via3 ( -3100 6300 ) ( -2900 6500 )
      + RECT via3 ( -2700 6300 ) ( -2500 6500 )
      + RECT via3 ( -2300 6300 ) ( -2100 6500 )
      + RECT via3 ( -1900 6300 ) ( -1700 6500 )
      + RECT via3 ( -1500 6300 ) ( -1300 6500 )
      + RECT via3 ( -1100 6300 ) ( -900 6500 )
      + RECT via3 ( -700 6300 ) ( -500 6500 )
      + RECT via3 ( -300 6300 ) ( -100 6500 )
      + RECT via3 ( 100 6300 ) ( 300 6500 )
      + RECT via3 ( 500 6300 ) ( 700 6500 )
      + RECT via3 ( 900 6300 ) ( 1100 6500 )
      + RECT via3 ( 1300 6300 ) ( 1500 6500 )
      + RECT via3 ( 1700 6300 ) ( 1900 6500 )
      + RECT via3 ( 2100 6300 ) ( 2300 6500 )
      + RECT via3 ( 2500 6300 ) ( 2700 6500 )
      + RECT via3 ( 2900 6300 ) ( 3100 6500 )
      + RECT via3 ( 3300 6300 ) ( 3500 6500 )
      + RECT via3 ( 3700 6300 ) ( 3900 6500 )
      + RECT via3 ( 4100 6300 ) ( 4300 6500 )
      + RECT via3 ( 4500 6300 ) ( 4700 6500 )
      + RECT via3 ( 4900 6300 ) ( 5100 6500 )
      + RECT via3 ( 5300 6300 ) ( 5500 6500 )
      + RECT via3 ( 5700 6300 ) ( 5900 6500 )
      + RECT via3 ( -5900 6700 ) ( -5700 6900 )
      + RECT via3 ( -5500 6700 ) ( -5300 6900 )
      + RECT via3 ( -5100 6700 ) ( -4900 6900 )
      + RECT via3 ( -4700 6700 ) ( -4500 6900 )
      + RECT via3 ( -4300 6700 ) ( -4100 6900 )
      + RECT via3 ( -3900 6700 ) ( -3700 6900 )
      + RECT via3 ( -3500 6700 ) ( -3300 6900 )
      + RECT via3 ( -3100 6700 ) ( -2900 6900 )
      + RECT via3 ( -2700 6700 ) ( -2500 6900 )
      + RECT via3 ( -2300 6700 ) ( -2100 6900 )
      + RECT via3 ( -1900 6700 ) ( -1700 6900 )
      + RECT via3 ( -1500 6700 ) ( -1300 6900 )
      + RECT via3 ( -1100 6700 ) ( -900 6900 )
      + RECT via3 ( -700 6700 ) ( -500 6900 )
      + RECT via3 ( -300 6700 ) ( -100 6900 )
      + RECT via3 ( 100 6700 ) ( 300 6900 )
      + RECT via3 ( 500 6700 ) ( 700 6900 )
      + RECT via3 ( 900 6700 ) ( 1100 6900 )
      + RECT via3 ( 1300 6700 ) ( 1500 6900 )
      + RECT via3 ( 1700 6700 ) ( 1900 6900 )
      + RECT via3 ( 2100 6700 ) ( 2300 6900 )
      + RECT via3 ( 2500 6700 ) ( 2700 6900 )
      + RECT via3 ( 2900 6700 ) ( 3100 6900 )
      + RECT via3 ( 3300 6700 ) ( 3500 6900 )
      + RECT via3 ( 3700 6700 ) ( 3900 6900 )
      + RECT via3 ( 4100 6700 ) ( 4300 6900 )
      + RECT via3 ( 4500 6700 ) ( 4700 6900 )
      + RECT via3 ( 4900 6700 ) ( 5100 6900 )
      + RECT via3 ( 5300 6700 ) ( 5500 6900 )
      + RECT via3 ( 5700 6700 ) ( 5900 6900 )
      + RECT via3 ( -5900 7100 ) ( -5700 7300 )
      + RECT via3 ( -5500 7100 ) ( -5300 7300 )
      + RECT via3 ( -5100 7100 ) ( -4900 7300 )
      + RECT via3 ( -4700 7100 ) ( -4500 7300 )
      + RECT via3 ( -4300 7100 ) ( -4100 7300 )
      + RECT via3 ( -3900 7100 ) ( -3700 7300 )
      + RECT via3 ( -3500 7100 ) ( -3300 7300 )
      + RECT via3 ( -3100 7100 ) ( -2900 7300 )
      + RECT via3 ( -2700 7100 ) ( -2500 7300 )
      + RECT via3 ( -2300 7100 ) ( -2100 7300 )
      + RECT via3 ( -1900 7100 ) ( -1700 7300 )
      + RECT via3 ( -1500 7100 ) ( -1300 7300 )
      + RECT via3 ( -1100 7100 ) ( -900 7300 )
      + RECT via3 ( -700 7100 ) ( -500 7300 )
      + RECT via3 ( -300 7100 ) ( -100 7300 )
      + RECT via3 ( 100 7100 ) ( 300 7300 )
      + RECT via3 ( 500 7100 ) ( 700 7300 )
      + RECT via3 ( 900 7100 ) ( 1100 7300 )
      + RECT via3 ( 1300 7100 ) ( 1500 7300 )
      + RECT via3 ( 1700 7100 ) ( 1900 7300 )
      + RECT via3 ( 2100 7100 ) ( 2300 7300 )
      + RECT via3 ( 2500 7100 ) ( 2700 7300 )
      + RECT via3 ( 2900 7100 ) ( 3100 7300 )
      + RECT via3 ( 3300 7100 ) ( 3500 7300 )
      + RECT via3 ( 3700 7100 ) ( 3900 7300 )
      + RECT via3 ( 4100 7100 ) ( 4300 7300 )
      + RECT via3 ( 4500 7100 ) ( 4700 7300 )
      + RECT via3 ( 4900 7100 ) ( 5100 7300 )
      + RECT via3 ( 5300 7100 ) ( 5500 7300 )
      + RECT via3 ( 5700 7100 ) ( 5900 7300 )
      + RECT via3 ( -5900 7500 ) ( -5700 7700 )
      + RECT via3 ( -5500 7500 ) ( -5300 7700 )
      + RECT via3 ( -5100 7500 ) ( -4900 7700 )
      + RECT via3 ( -4700 7500 ) ( -4500 7700 )
      + RECT via3 ( -4300 7500 ) ( -4100 7700 )
      + RECT via3 ( -3900 7500 ) ( -3700 7700 )
      + RECT via3 ( -3500 7500 ) ( -3300 7700 )
      + RECT via3 ( -3100 7500 ) ( -2900 7700 )
      + RECT via3 ( -2700 7500 ) ( -2500 7700 )
      + RECT via3 ( -2300 7500 ) ( -2100 7700 )
      + RECT via3 ( -1900 7500 ) ( -1700 7700 )
      + RECT via3 ( -1500 7500 ) ( -1300 7700 )
      + RECT via3 ( -1100 7500 ) ( -900 7700 )
      + RECT via3 ( -700 7500 ) ( -500 7700 )
      + RECT via3 ( -300 7500 ) ( -100 7700 )
      + RECT via3 ( 100 7500 ) ( 300 7700 )
      + RECT via3 ( 500 7500 ) ( 700 7700 )
      + RECT via3 ( 900 7500 ) ( 1100 7700 )
      + RECT via3 ( 1300 7500 ) ( 1500 7700 )
      + RECT via3 ( 1700 7500 ) ( 1900 7700 )
      + RECT via3 ( 2100 7500 ) ( 2300 7700 )
      + RECT via3 ( 2500 7500 ) ( 2700 7700 )
      + RECT via3 ( 2900 7500 ) ( 3100 7700 )
      + RECT via3 ( 3300 7500 ) ( 3500 7700 )
      + RECT via3 ( 3700 7500 ) ( 3900 7700 )
      + RECT via3 ( 4100 7500 ) ( 4300 7700 )
      + RECT via3 ( 4500 7500 ) ( 4700 7700 )
      + RECT via3 ( 4900 7500 ) ( 5100 7700 )
      + RECT via3 ( 5300 7500 ) ( 5500 7700 )
      + RECT via3 ( 5700 7500 ) ( 5900 7700 )
      + RECT via3 ( -5900 7900 ) ( -5700 8100 )
      + RECT via3 ( -5500 7900 ) ( -5300 8100 )
      + RECT via3 ( -5100 7900 ) ( -4900 8100 )
      + RECT via3 ( -4700 7900 ) ( -4500 8100 )
      + RECT via3 ( -4300 7900 ) ( -4100 8100 )
      + RECT via3 ( -3900 7900 ) ( -3700 8100 )
      + RECT via3 ( -3500 7900 ) ( -3300 8100 )
      + RECT via3 ( -3100 7900 ) ( -2900 8100 )
      + RECT via3 ( -2700 7900 ) ( -2500 8100 )
      + RECT via3 ( -2300 7900 ) ( -2100 8100 )
      + RECT via3 ( -1900 7900 ) ( -1700 8100 )
      + RECT via3 ( -1500 7900 ) ( -1300 8100 )
      + RECT via3 ( -1100 7900 ) ( -900 8100 )
      + RECT via3 ( -700 7900 ) ( -500 8100 )
      + RECT via3 ( -300 7900 ) ( -100 8100 )
      + RECT via3 ( 100 7900 ) ( 300 8100 )
      + RECT via3 ( 500 7900 ) ( 700 8100 )
      + RECT via3 ( 900 7900 ) ( 1100 8100 )
      + RECT via3 ( 1300 7900 ) ( 1500 8100 )
      + RECT via3 ( 1700 7900 ) ( 1900 8100 )
      + RECT via3 ( 2100 7900 ) ( 2300 8100 )
      + RECT via3 ( 2500 7900 ) ( 2700 8100 )
      + RECT via3 ( 2900 7900 ) ( 3100 8100 )
      + RECT via3 ( 3300 7900 ) ( 3500 8100 )
      + RECT via3 ( 3700 7900 ) ( 3900 8100 )
      + RECT via3 ( 4100 7900 ) ( 4300 8100 )
      + RECT via3 ( 4500 7900 ) ( 4700 8100 )
      + RECT via3 ( 4900 7900 ) ( 5100 8100 )
      + RECT via3 ( 5300 7900 ) ( 5500 8100 )
      + RECT via3 ( 5700 7900 ) ( 5900 8100 )
      + RECT via3 ( -5900 8300 ) ( -5700 8500 )
      + RECT via3 ( -5500 8300 ) ( -5300 8500 )
      + RECT via3 ( -5100 8300 ) ( -4900 8500 )
      + RECT via3 ( -4700 8300 ) ( -4500 8500 )
      + RECT via3 ( -4300 8300 ) ( -4100 8500 )
      + RECT via3 ( -3900 8300 ) ( -3700 8500 )
      + RECT via3 ( -3500 8300 ) ( -3300 8500 )
      + RECT via3 ( -3100 8300 ) ( -2900 8500 )
      + RECT via3 ( -2700 8300 ) ( -2500 8500 )
      + RECT via3 ( -2300 8300 ) ( -2100 8500 )
      + RECT via3 ( -1900 8300 ) ( -1700 8500 )
      + RECT via3 ( -1500 8300 ) ( -1300 8500 )
      + RECT via3 ( -1100 8300 ) ( -900 8500 )
      + RECT via3 ( -700 8300 ) ( -500 8500 )
      + RECT via3 ( -300 8300 ) ( -100 8500 )
      + RECT via3 ( 100 8300 ) ( 300 8500 )
      + RECT via3 ( 500 8300 ) ( 700 8500 )
      + RECT via3 ( 900 8300 ) ( 1100 8500 )
      + RECT via3 ( 1300 8300 ) ( 1500 8500 )
      + RECT via3 ( 1700 8300 ) ( 1900 8500 )
      + RECT via3 ( 2100 8300 ) ( 2300 8500 )
      + RECT via3 ( 2500 8300 ) ( 2700 8500 )
      + RECT via3 ( 2900 8300 ) ( 3100 8500 )
      + RECT via3 ( 3300 8300 ) ( 3500 8500 )
      + RECT via3 ( 3700 8300 ) ( 3900 8500 )
      + RECT via3 ( 4100 8300 ) ( 4300 8500 )
      + RECT via3 ( 4500 8300 ) ( 4700 8500 )
      + RECT via3 ( 4900 8300 ) ( 5100 8500 )
      + RECT via3 ( 5300 8300 ) ( 5500 8500 )
      + RECT via3 ( 5700 8300 ) ( 5900 8500 )
      + RECT via3 ( -5900 8700 ) ( -5700 8900 )
      + RECT via3 ( -5500 8700 ) ( -5300 8900 )
      + RECT via3 ( -5100 8700 ) ( -4900 8900 )
      + RECT via3 ( -4700 8700 ) ( -4500 8900 )
      + RECT via3 ( -4300 8700 ) ( -4100 8900 )
      + RECT via3 ( -3900 8700 ) ( -3700 8900 )
      + RECT via3 ( -3500 8700 ) ( -3300 8900 )
      + RECT via3 ( -3100 8700 ) ( -2900 8900 )
      + RECT via3 ( -2700 8700 ) ( -2500 8900 )
      + RECT via3 ( -2300 8700 ) ( -2100 8900 )
      + RECT via3 ( -1900 8700 ) ( -1700 8900 )
      + RECT via3 ( -1500 8700 ) ( -1300 8900 )
      + RECT via3 ( -1100 8700 ) ( -900 8900 )
      + RECT via3 ( -700 8700 ) ( -500 8900 )
      + RECT via3 ( -300 8700 ) ( -100 8900 )
      + RECT via3 ( 100 8700 ) ( 300 8900 )
      + RECT via3 ( 500 8700 ) ( 700 8900 )
      + RECT via3 ( 900 8700 ) ( 1100 8900 )
      + RECT via3 ( 1300 8700 ) ( 1500 8900 )
      + RECT via3 ( 1700 8700 ) ( 1900 8900 )
      + RECT via3 ( 2100 8700 ) ( 2300 8900 )
      + RECT via3 ( 2500 8700 ) ( 2700 8900 )
      + RECT via3 ( 2900 8700 ) ( 3100 8900 )
      + RECT via3 ( 3300 8700 ) ( 3500 8900 )
      + RECT via3 ( 3700 8700 ) ( 3900 8900 )
      + RECT via3 ( 4100 8700 ) ( 4300 8900 )
      + RECT via3 ( 4500 8700 ) ( 4700 8900 )
      + RECT via3 ( 4900 8700 ) ( 5100 8900 )
      + RECT via3 ( 5300 8700 ) ( 5500 8900 )
      + RECT via3 ( 5700 8700 ) ( 5900 8900 )
      + RECT via3 ( -5900 9100 ) ( -5700 9300 )
      + RECT via3 ( -5500 9100 ) ( -5300 9300 )
      + RECT via3 ( -5100 9100 ) ( -4900 9300 )
      + RECT via3 ( -4700 9100 ) ( -4500 9300 )
      + RECT via3 ( -4300 9100 ) ( -4100 9300 )
      + RECT via3 ( -3900 9100 ) ( -3700 9300 )
      + RECT via3 ( -3500 9100 ) ( -3300 9300 )
      + RECT via3 ( -3100 9100 ) ( -2900 9300 )
      + RECT via3 ( -2700 9100 ) ( -2500 9300 )
      + RECT via3 ( -2300 9100 ) ( -2100 9300 )
      + RECT via3 ( -1900 9100 ) ( -1700 9300 )
      + RECT via3 ( -1500 9100 ) ( -1300 9300 )
      + RECT via3 ( -1100 9100 ) ( -900 9300 )
      + RECT via3 ( -700 9100 ) ( -500 9300 )
      + RECT via3 ( -300 9100 ) ( -100 9300 )
      + RECT via3 ( 100 9100 ) ( 300 9300 )
      + RECT via3 ( 500 9100 ) ( 700 9300 )
      + RECT via3 ( 900 9100 ) ( 1100 9300 )
      + RECT via3 ( 1300 9100 ) ( 1500 9300 )
      + RECT via3 ( 1700 9100 ) ( 1900 9300 )
      + RECT via3 ( 2100 9100 ) ( 2300 9300 )
      + RECT via3 ( 2500 9100 ) ( 2700 9300 )
      + RECT via3 ( 2900 9100 ) ( 3100 9300 )
      + RECT via3 ( 3300 9100 ) ( 3500 9300 )
      + RECT via3 ( 3700 9100 ) ( 3900 9300 )
      + RECT via3 ( 4100 9100 ) ( 4300 9300 )
      + RECT via3 ( 4500 9100 ) ( 4700 9300 )
      + RECT via3 ( 4900 9100 ) ( 5100 9300 )
      + RECT via3 ( 5300 9100 ) ( 5500 9300 )
      + RECT via3 ( 5700 9100 ) ( 5900 9300 )
      + RECT via3 ( -5900 9500 ) ( -5700 9700 )
      + RECT via3 ( -5500 9500 ) ( -5300 9700 )
      + RECT via3 ( -5100 9500 ) ( -4900 9700 )
      + RECT via3 ( -4700 9500 ) ( -4500 9700 )
      + RECT via3 ( -4300 9500 ) ( -4100 9700 )
      + RECT via3 ( -3900 9500 ) ( -3700 9700 )
      + RECT via3 ( -3500 9500 ) ( -3300 9700 )
      + RECT via3 ( -3100 9500 ) ( -2900 9700 )
      + RECT via3 ( -2700 9500 ) ( -2500 9700 )
      + RECT via3 ( -2300 9500 ) ( -2100 9700 )
      + RECT via3 ( -1900 9500 ) ( -1700 9700 )
      + RECT via3 ( -1500 9500 ) ( -1300 9700 )
      + RECT via3 ( -1100 9500 ) ( -900 9700 )
      + RECT via3 ( -700 9500 ) ( -500 9700 )
      + RECT via3 ( -300 9500 ) ( -100 9700 )
      + RECT via3 ( 100 9500 ) ( 300 9700 )
      + RECT via3 ( 500 9500 ) ( 700 9700 )
      + RECT via3 ( 900 9500 ) ( 1100 9700 )
      + RECT via3 ( 1300 9500 ) ( 1500 9700 )
      + RECT via3 ( 1700 9500 ) ( 1900 9700 )
      + RECT via3 ( 2100 9500 ) ( 2300 9700 )
      + RECT via3 ( 2500 9500 ) ( 2700 9700 )
      + RECT via3 ( 2900 9500 ) ( 3100 9700 )
      + RECT via3 ( 3300 9500 ) ( 3500 9700 )
      + RECT via3 ( 3700 9500 ) ( 3900 9700 )
      + RECT via3 ( 4100 9500 ) ( 4300 9700 )
      + RECT via3 ( 4500 9500 ) ( 4700 9700 )
      + RECT via3 ( 4900 9500 ) ( 5100 9700 )
      + RECT via3 ( 5300 9500 ) ( 5500 9700 )
      + RECT via3 ( 5700 9500 ) ( 5900 9700 )
      + RECT via3 ( -5900 9900 ) ( -5700 10100 )
      + RECT via3 ( -5500 9900 ) ( -5300 10100 )
      + RECT via3 ( -5100 9900 ) ( -4900 10100 )
      + RECT via3 ( -4700 9900 ) ( -4500 10100 )
      + RECT via3 ( -4300 9900 ) ( -4100 10100 )
      + RECT via3 ( -3900 9900 ) ( -3700 10100 )
      + RECT via3 ( -3500 9900 ) ( -3300 10100 )
      + RECT via3 ( -3100 9900 ) ( -2900 10100 )
      + RECT via3 ( -2700 9900 ) ( -2500 10100 )
      + RECT via3 ( -2300 9900 ) ( -2100 10100 )
      + RECT via3 ( -1900 9900 ) ( -1700 10100 )
      + RECT via3 ( -1500 9900 ) ( -1300 10100 )
      + RECT via3 ( -1100 9900 ) ( -900 10100 )
      + RECT via3 ( -700 9900 ) ( -500 10100 )
      + RECT via3 ( -300 9900 ) ( -100 10100 )
      + RECT via3 ( 100 9900 ) ( 300 10100 )
      + RECT via3 ( 500 9900 ) ( 700 10100 )
      + RECT via3 ( 900 9900 ) ( 1100 10100 )
      + RECT via3 ( 1300 9900 ) ( 1500 10100 )
      + RECT via3 ( 1700 9900 ) ( 1900 10100 )
      + RECT via3 ( 2100 9900 ) ( 2300 10100 )
      + RECT via3 ( 2500 9900 ) ( 2700 10100 )
      + RECT via3 ( 2900 9900 ) ( 3100 10100 )
      + RECT via3 ( 3300 9900 ) ( 3500 10100 )
      + RECT via3 ( 3700 9900 ) ( 3900 10100 )
      + RECT via3 ( 4100 9900 ) ( 4300 10100 )
      + RECT via3 ( 4500 9900 ) ( 4700 10100 )
      + RECT via3 ( 4900 9900 ) ( 5100 10100 )
      + RECT via3 ( 5300 9900 ) ( 5500 10100 )
      + RECT via3 ( 5700 9900 ) ( 5900 10100 )
      + RECT via3 ( -5900 10300 ) ( -5700 10500 )
      + RECT via3 ( -5500 10300 ) ( -5300 10500 )
      + RECT via3 ( -5100 10300 ) ( -4900 10500 )
      + RECT via3 ( -4700 10300 ) ( -4500 10500 )
      + RECT via3 ( -4300 10300 ) ( -4100 10500 )
      + RECT via3 ( -3900 10300 ) ( -3700 10500 )
      + RECT via3 ( -3500 10300 ) ( -3300 10500 )
      + RECT via3 ( -3100 10300 ) ( -2900 10500 )
      + RECT via3 ( -2700 10300 ) ( -2500 10500 )
      + RECT via3 ( -2300 10300 ) ( -2100 10500 )
      + RECT via3 ( -1900 10300 ) ( -1700 10500 )
      + RECT via3 ( -1500 10300 ) ( -1300 10500 )
      + RECT via3 ( -1100 10300 ) ( -900 10500 )
      + RECT via3 ( -700 10300 ) ( -500 10500 )
      + RECT via3 ( -300 10300 ) ( -100 10500 )
      + RECT via3 ( 100 10300 ) ( 300 10500 )
      + RECT via3 ( 500 10300 ) ( 700 10500 )
      + RECT via3 ( 900 10300 ) ( 1100 10500 )
      + RECT via3 ( 1300 10300 ) ( 1500 10500 )
      + RECT via3 ( 1700 10300 ) ( 1900 10500 )
      + RECT via3 ( 2100 10300 ) ( 2300 10500 )
      + RECT via3 ( 2500 10300 ) ( 2700 10500 )
      + RECT via3 ( 2900 10300 ) ( 3100 10500 )
      + RECT via3 ( 3300 10300 ) ( 3500 10500 )
      + RECT via3 ( 3700 10300 ) ( 3900 10500 )
      + RECT via3 ( 4100 10300 ) ( 4300 10500 )
      + RECT via3 ( 4500 10300 ) ( 4700 10500 )
      + RECT via3 ( 4900 10300 ) ( 5100 10500 )
      + RECT via3 ( 5300 10300 ) ( 5500 10500 )
      + RECT via3 ( 5700 10300 ) ( 5900 10500 )
      + RECT via3 ( -5900 10700 ) ( -5700 10900 )
      + RECT via3 ( -5500 10700 ) ( -5300 10900 )
      + RECT via3 ( -5100 10700 ) ( -4900 10900 )
      + RECT via3 ( -4700 10700 ) ( -4500 10900 )
      + RECT via3 ( -4300 10700 ) ( -4100 10900 )
      + RECT via3 ( -3900 10700 ) ( -3700 10900 )
      + RECT via3 ( -3500 10700 ) ( -3300 10900 )
      + RECT via3 ( -3100 10700 ) ( -2900 10900 )
      + RECT via3 ( -2700 10700 ) ( -2500 10900 )
      + RECT via3 ( -2300 10700 ) ( -2100 10900 )
      + RECT via3 ( -1900 10700 ) ( -1700 10900 )
      + RECT via3 ( -1500 10700 ) ( -1300 10900 )
      + RECT via3 ( -1100 10700 ) ( -900 10900 )
      + RECT via3 ( -700 10700 ) ( -500 10900 )
      + RECT via3 ( -300 10700 ) ( -100 10900 )
      + RECT via3 ( 100 10700 ) ( 300 10900 )
      + RECT via3 ( 500 10700 ) ( 700 10900 )
      + RECT via3 ( 900 10700 ) ( 1100 10900 )
      + RECT via3 ( 1300 10700 ) ( 1500 10900 )
      + RECT via3 ( 1700 10700 ) ( 1900 10900 )
      + RECT via3 ( 2100 10700 ) ( 2300 10900 )
      + RECT via3 ( 2500 10700 ) ( 2700 10900 )
      + RECT via3 ( 2900 10700 ) ( 3100 10900 )
      + RECT via3 ( 3300 10700 ) ( 3500 10900 )
      + RECT via3 ( 3700 10700 ) ( 3900 10900 )
      + RECT via3 ( 4100 10700 ) ( 4300 10900 )
      + RECT via3 ( 4500 10700 ) ( 4700 10900 )
      + RECT via3 ( 4900 10700 ) ( 5100 10900 )
      + RECT via3 ( 5300 10700 ) ( 5500 10900 )
      + RECT via3 ( 5700 10700 ) ( 5900 10900 )
      + RECT via3 ( -5900 11100 ) ( -5700 11300 )
      + RECT via3 ( -5500 11100 ) ( -5300 11300 )
      + RECT via3 ( -5100 11100 ) ( -4900 11300 )
      + RECT via3 ( -4700 11100 ) ( -4500 11300 )
      + RECT via3 ( -4300 11100 ) ( -4100 11300 )
      + RECT via3 ( -3900 11100 ) ( -3700 11300 )
      + RECT via3 ( -3500 11100 ) ( -3300 11300 )
      + RECT via3 ( -3100 11100 ) ( -2900 11300 )
      + RECT via3 ( -2700 11100 ) ( -2500 11300 )
      + RECT via3 ( -2300 11100 ) ( -2100 11300 )
      + RECT via3 ( -1900 11100 ) ( -1700 11300 )
      + RECT via3 ( -1500 11100 ) ( -1300 11300 )
      + RECT via3 ( -1100 11100 ) ( -900 11300 )
      + RECT via3 ( -700 11100 ) ( -500 11300 )
      + RECT via3 ( -300 11100 ) ( -100 11300 )
      + RECT via3 ( 100 11100 ) ( 300 11300 )
      + RECT via3 ( 500 11100 ) ( 700 11300 )
      + RECT via3 ( 900 11100 ) ( 1100 11300 )
      + RECT via3 ( 1300 11100 ) ( 1500 11300 )
      + RECT via3 ( 1700 11100 ) ( 1900 11300 )
      + RECT via3 ( 2100 11100 ) ( 2300 11300 )
      + RECT via3 ( 2500 11100 ) ( 2700 11300 )
      + RECT via3 ( 2900 11100 ) ( 3100 11300 )
      + RECT via3 ( 3300 11100 ) ( 3500 11300 )
      + RECT via3 ( 3700 11100 ) ( 3900 11300 )
      + RECT via3 ( 4100 11100 ) ( 4300 11300 )
      + RECT via3 ( 4500 11100 ) ( 4700 11300 )
      + RECT via3 ( 4900 11100 ) ( 5100 11300 )
      + RECT via3 ( 5300 11100 ) ( 5500 11300 )
      + RECT via3 ( 5700 11100 ) ( 5900 11300 ) ;
   - via3_11690_21950_hx
      + RECT met3 ( -5875 -10975 ) ( 5875 10975 )
      + RECT met4 ( -5850 -10980 ) ( 5850 10980 )
      + RECT via3 ( -5700 -10900 ) ( -5500 -10700 )
      + RECT via3 ( -5300 -10900 ) ( -5100 -10700 )
      + RECT via3 ( -4900 -10900 ) ( -4700 -10700 )
      + RECT via3 ( -4500 -10900 ) ( -4300 -10700 )
      + RECT via3 ( -4100 -10900 ) ( -3900 -10700 )
      + RECT via3 ( -3700 -10900 ) ( -3500 -10700 )
      + RECT via3 ( -3300 -10900 ) ( -3100 -10700 )
      + RECT via3 ( -2900 -10900 ) ( -2700 -10700 )
      + RECT via3 ( -2500 -10900 ) ( -2300 -10700 )
      + RECT via3 ( -2100 -10900 ) ( -1900 -10700 )
      + RECT via3 ( -1700 -10900 ) ( -1500 -10700 )
      + RECT via3 ( -1300 -10900 ) ( -1100 -10700 )
      + RECT via3 ( -900 -10900 ) ( -700 -10700 )
      + RECT via3 ( -500 -10900 ) ( -300 -10700 )
      + RECT via3 ( -100 -10900 ) ( 100 -10700 )
      + RECT via3 ( 300 -10900 ) ( 500 -10700 )
      + RECT via3 ( 700 -10900 ) ( 900 -10700 )
      + RECT via3 ( 1100 -10900 ) ( 1300 -10700 )
      + RECT via3 ( 1500 -10900 ) ( 1700 -10700 )
      + RECT via3 ( 1900 -10900 ) ( 2100 -10700 )
      + RECT via3 ( 2300 -10900 ) ( 2500 -10700 )
      + RECT via3 ( 2700 -10900 ) ( 2900 -10700 )
      + RECT via3 ( 3100 -10900 ) ( 3300 -10700 )
      + RECT via3 ( 3500 -10900 ) ( 3700 -10700 )
      + RECT via3 ( 3900 -10900 ) ( 4100 -10700 )
      + RECT via3 ( 4300 -10900 ) ( 4500 -10700 )
      + RECT via3 ( 4700 -10900 ) ( 4900 -10700 )
      + RECT via3 ( 5100 -10900 ) ( 5300 -10700 )
      + RECT via3 ( 5500 -10900 ) ( 5700 -10700 )
      + RECT via3 ( -5700 -10500 ) ( -5500 -10300 )
      + RECT via3 ( -5300 -10500 ) ( -5100 -10300 )
      + RECT via3 ( -4900 -10500 ) ( -4700 -10300 )
      + RECT via3 ( -4500 -10500 ) ( -4300 -10300 )
      + RECT via3 ( -4100 -10500 ) ( -3900 -10300 )
      + RECT via3 ( -3700 -10500 ) ( -3500 -10300 )
      + RECT via3 ( -3300 -10500 ) ( -3100 -10300 )
      + RECT via3 ( -2900 -10500 ) ( -2700 -10300 )
      + RECT via3 ( -2500 -10500 ) ( -2300 -10300 )
      + RECT via3 ( -2100 -10500 ) ( -1900 -10300 )
      + RECT via3 ( -1700 -10500 ) ( -1500 -10300 )
      + RECT via3 ( -1300 -10500 ) ( -1100 -10300 )
      + RECT via3 ( -900 -10500 ) ( -700 -10300 )
      + RECT via3 ( -500 -10500 ) ( -300 -10300 )
      + RECT via3 ( -100 -10500 ) ( 100 -10300 )
      + RECT via3 ( 300 -10500 ) ( 500 -10300 )
      + RECT via3 ( 700 -10500 ) ( 900 -10300 )
      + RECT via3 ( 1100 -10500 ) ( 1300 -10300 )
      + RECT via3 ( 1500 -10500 ) ( 1700 -10300 )
      + RECT via3 ( 1900 -10500 ) ( 2100 -10300 )
      + RECT via3 ( 2300 -10500 ) ( 2500 -10300 )
      + RECT via3 ( 2700 -10500 ) ( 2900 -10300 )
      + RECT via3 ( 3100 -10500 ) ( 3300 -10300 )
      + RECT via3 ( 3500 -10500 ) ( 3700 -10300 )
      + RECT via3 ( 3900 -10500 ) ( 4100 -10300 )
      + RECT via3 ( 4300 -10500 ) ( 4500 -10300 )
      + RECT via3 ( 4700 -10500 ) ( 4900 -10300 )
      + RECT via3 ( 5100 -10500 ) ( 5300 -10300 )
      + RECT via3 ( 5500 -10500 ) ( 5700 -10300 )
      + RECT via3 ( -5700 -10100 ) ( -5500 -9900 )
      + RECT via3 ( -5300 -10100 ) ( -5100 -9900 )
      + RECT via3 ( -4900 -10100 ) ( -4700 -9900 )
      + RECT via3 ( -4500 -10100 ) ( -4300 -9900 )
      + RECT via3 ( -4100 -10100 ) ( -3900 -9900 )
      + RECT via3 ( -3700 -10100 ) ( -3500 -9900 )
      + RECT via3 ( -3300 -10100 ) ( -3100 -9900 )
      + RECT via3 ( -2900 -10100 ) ( -2700 -9900 )
      + RECT via3 ( -2500 -10100 ) ( -2300 -9900 )
      + RECT via3 ( -2100 -10100 ) ( -1900 -9900 )
      + RECT via3 ( -1700 -10100 ) ( -1500 -9900 )
      + RECT via3 ( -1300 -10100 ) ( -1100 -9900 )
      + RECT via3 ( -900 -10100 ) ( -700 -9900 )
      + RECT via3 ( -500 -10100 ) ( -300 -9900 )
      + RECT via3 ( -100 -10100 ) ( 100 -9900 )
      + RECT via3 ( 300 -10100 ) ( 500 -9900 )
      + RECT via3 ( 700 -10100 ) ( 900 -9900 )
      + RECT via3 ( 1100 -10100 ) ( 1300 -9900 )
      + RECT via3 ( 1500 -10100 ) ( 1700 -9900 )
      + RECT via3 ( 1900 -10100 ) ( 2100 -9900 )
      + RECT via3 ( 2300 -10100 ) ( 2500 -9900 )
      + RECT via3 ( 2700 -10100 ) ( 2900 -9900 )
      + RECT via3 ( 3100 -10100 ) ( 3300 -9900 )
      + RECT via3 ( 3500 -10100 ) ( 3700 -9900 )
      + RECT via3 ( 3900 -10100 ) ( 4100 -9900 )
      + RECT via3 ( 4300 -10100 ) ( 4500 -9900 )
      + RECT via3 ( 4700 -10100 ) ( 4900 -9900 )
      + RECT via3 ( 5100 -10100 ) ( 5300 -9900 )
      + RECT via3 ( 5500 -10100 ) ( 5700 -9900 )
      + RECT via3 ( -5700 -9700 ) ( -5500 -9500 )
      + RECT via3 ( -5300 -9700 ) ( -5100 -9500 )
      + RECT via3 ( -4900 -9700 ) ( -4700 -9500 )
      + RECT via3 ( -4500 -9700 ) ( -4300 -9500 )
      + RECT via3 ( -4100 -9700 ) ( -3900 -9500 )
      + RECT via3 ( -3700 -9700 ) ( -3500 -9500 )
      + RECT via3 ( -3300 -9700 ) ( -3100 -9500 )
      + RECT via3 ( -2900 -9700 ) ( -2700 -9500 )
      + RECT via3 ( -2500 -9700 ) ( -2300 -9500 )
      + RECT via3 ( -2100 -9700 ) ( -1900 -9500 )
      + RECT via3 ( -1700 -9700 ) ( -1500 -9500 )
      + RECT via3 ( -1300 -9700 ) ( -1100 -9500 )
      + RECT via3 ( -900 -9700 ) ( -700 -9500 )
      + RECT via3 ( -500 -9700 ) ( -300 -9500 )
      + RECT via3 ( -100 -9700 ) ( 100 -9500 )
      + RECT via3 ( 300 -9700 ) ( 500 -9500 )
      + RECT via3 ( 700 -9700 ) ( 900 -9500 )
      + RECT via3 ( 1100 -9700 ) ( 1300 -9500 )
      + RECT via3 ( 1500 -9700 ) ( 1700 -9500 )
      + RECT via3 ( 1900 -9700 ) ( 2100 -9500 )
      + RECT via3 ( 2300 -9700 ) ( 2500 -9500 )
      + RECT via3 ( 2700 -9700 ) ( 2900 -9500 )
      + RECT via3 ( 3100 -9700 ) ( 3300 -9500 )
      + RECT via3 ( 3500 -9700 ) ( 3700 -9500 )
      + RECT via3 ( 3900 -9700 ) ( 4100 -9500 )
      + RECT via3 ( 4300 -9700 ) ( 4500 -9500 )
      + RECT via3 ( 4700 -9700 ) ( 4900 -9500 )
      + RECT via3 ( 5100 -9700 ) ( 5300 -9500 )
      + RECT via3 ( 5500 -9700 ) ( 5700 -9500 )
      + RECT via3 ( -5700 -9300 ) ( -5500 -9100 )
      + RECT via3 ( -5300 -9300 ) ( -5100 -9100 )
      + RECT via3 ( -4900 -9300 ) ( -4700 -9100 )
      + RECT via3 ( -4500 -9300 ) ( -4300 -9100 )
      + RECT via3 ( -4100 -9300 ) ( -3900 -9100 )
      + RECT via3 ( -3700 -9300 ) ( -3500 -9100 )
      + RECT via3 ( -3300 -9300 ) ( -3100 -9100 )
      + RECT via3 ( -2900 -9300 ) ( -2700 -9100 )
      + RECT via3 ( -2500 -9300 ) ( -2300 -9100 )
      + RECT via3 ( -2100 -9300 ) ( -1900 -9100 )
      + RECT via3 ( -1700 -9300 ) ( -1500 -9100 )
      + RECT via3 ( -1300 -9300 ) ( -1100 -9100 )
      + RECT via3 ( -900 -9300 ) ( -700 -9100 )
      + RECT via3 ( -500 -9300 ) ( -300 -9100 )
      + RECT via3 ( -100 -9300 ) ( 100 -9100 )
      + RECT via3 ( 300 -9300 ) ( 500 -9100 )
      + RECT via3 ( 700 -9300 ) ( 900 -9100 )
      + RECT via3 ( 1100 -9300 ) ( 1300 -9100 )
      + RECT via3 ( 1500 -9300 ) ( 1700 -9100 )
      + RECT via3 ( 1900 -9300 ) ( 2100 -9100 )
      + RECT via3 ( 2300 -9300 ) ( 2500 -9100 )
      + RECT via3 ( 2700 -9300 ) ( 2900 -9100 )
      + RECT via3 ( 3100 -9300 ) ( 3300 -9100 )
      + RECT via3 ( 3500 -9300 ) ( 3700 -9100 )
      + RECT via3 ( 3900 -9300 ) ( 4100 -9100 )
      + RECT via3 ( 4300 -9300 ) ( 4500 -9100 )
      + RECT via3 ( 4700 -9300 ) ( 4900 -9100 )
      + RECT via3 ( 5100 -9300 ) ( 5300 -9100 )
      + RECT via3 ( 5500 -9300 ) ( 5700 -9100 )
      + RECT via3 ( -5700 -8900 ) ( -5500 -8700 )
      + RECT via3 ( -5300 -8900 ) ( -5100 -8700 )
      + RECT via3 ( -4900 -8900 ) ( -4700 -8700 )
      + RECT via3 ( -4500 -8900 ) ( -4300 -8700 )
      + RECT via3 ( -4100 -8900 ) ( -3900 -8700 )
      + RECT via3 ( -3700 -8900 ) ( -3500 -8700 )
      + RECT via3 ( -3300 -8900 ) ( -3100 -8700 )
      + RECT via3 ( -2900 -8900 ) ( -2700 -8700 )
      + RECT via3 ( -2500 -8900 ) ( -2300 -8700 )
      + RECT via3 ( -2100 -8900 ) ( -1900 -8700 )
      + RECT via3 ( -1700 -8900 ) ( -1500 -8700 )
      + RECT via3 ( -1300 -8900 ) ( -1100 -8700 )
      + RECT via3 ( -900 -8900 ) ( -700 -8700 )
      + RECT via3 ( -500 -8900 ) ( -300 -8700 )
      + RECT via3 ( -100 -8900 ) ( 100 -8700 )
      + RECT via3 ( 300 -8900 ) ( 500 -8700 )
      + RECT via3 ( 700 -8900 ) ( 900 -8700 )
      + RECT via3 ( 1100 -8900 ) ( 1300 -8700 )
      + RECT via3 ( 1500 -8900 ) ( 1700 -8700 )
      + RECT via3 ( 1900 -8900 ) ( 2100 -8700 )
      + RECT via3 ( 2300 -8900 ) ( 2500 -8700 )
      + RECT via3 ( 2700 -8900 ) ( 2900 -8700 )
      + RECT via3 ( 3100 -8900 ) ( 3300 -8700 )
      + RECT via3 ( 3500 -8900 ) ( 3700 -8700 )
      + RECT via3 ( 3900 -8900 ) ( 4100 -8700 )
      + RECT via3 ( 4300 -8900 ) ( 4500 -8700 )
      + RECT via3 ( 4700 -8900 ) ( 4900 -8700 )
      + RECT via3 ( 5100 -8900 ) ( 5300 -8700 )
      + RECT via3 ( 5500 -8900 ) ( 5700 -8700 )
      + RECT via3 ( -5700 -8500 ) ( -5500 -8300 )
      + RECT via3 ( -5300 -8500 ) ( -5100 -8300 )
      + RECT via3 ( -4900 -8500 ) ( -4700 -8300 )
      + RECT via3 ( -4500 -8500 ) ( -4300 -8300 )
      + RECT via3 ( -4100 -8500 ) ( -3900 -8300 )
      + RECT via3 ( -3700 -8500 ) ( -3500 -8300 )
      + RECT via3 ( -3300 -8500 ) ( -3100 -8300 )
      + RECT via3 ( -2900 -8500 ) ( -2700 -8300 )
      + RECT via3 ( -2500 -8500 ) ( -2300 -8300 )
      + RECT via3 ( -2100 -8500 ) ( -1900 -8300 )
      + RECT via3 ( -1700 -8500 ) ( -1500 -8300 )
      + RECT via3 ( -1300 -8500 ) ( -1100 -8300 )
      + RECT via3 ( -900 -8500 ) ( -700 -8300 )
      + RECT via3 ( -500 -8500 ) ( -300 -8300 )
      + RECT via3 ( -100 -8500 ) ( 100 -8300 )
      + RECT via3 ( 300 -8500 ) ( 500 -8300 )
      + RECT via3 ( 700 -8500 ) ( 900 -8300 )
      + RECT via3 ( 1100 -8500 ) ( 1300 -8300 )
      + RECT via3 ( 1500 -8500 ) ( 1700 -8300 )
      + RECT via3 ( 1900 -8500 ) ( 2100 -8300 )
      + RECT via3 ( 2300 -8500 ) ( 2500 -8300 )
      + RECT via3 ( 2700 -8500 ) ( 2900 -8300 )
      + RECT via3 ( 3100 -8500 ) ( 3300 -8300 )
      + RECT via3 ( 3500 -8500 ) ( 3700 -8300 )
      + RECT via3 ( 3900 -8500 ) ( 4100 -8300 )
      + RECT via3 ( 4300 -8500 ) ( 4500 -8300 )
      + RECT via3 ( 4700 -8500 ) ( 4900 -8300 )
      + RECT via3 ( 5100 -8500 ) ( 5300 -8300 )
      + RECT via3 ( 5500 -8500 ) ( 5700 -8300 )
      + RECT via3 ( -5700 -8100 ) ( -5500 -7900 )
      + RECT via3 ( -5300 -8100 ) ( -5100 -7900 )
      + RECT via3 ( -4900 -8100 ) ( -4700 -7900 )
      + RECT via3 ( -4500 -8100 ) ( -4300 -7900 )
      + RECT via3 ( -4100 -8100 ) ( -3900 -7900 )
      + RECT via3 ( -3700 -8100 ) ( -3500 -7900 )
      + RECT via3 ( -3300 -8100 ) ( -3100 -7900 )
      + RECT via3 ( -2900 -8100 ) ( -2700 -7900 )
      + RECT via3 ( -2500 -8100 ) ( -2300 -7900 )
      + RECT via3 ( -2100 -8100 ) ( -1900 -7900 )
      + RECT via3 ( -1700 -8100 ) ( -1500 -7900 )
      + RECT via3 ( -1300 -8100 ) ( -1100 -7900 )
      + RECT via3 ( -900 -8100 ) ( -700 -7900 )
      + RECT via3 ( -500 -8100 ) ( -300 -7900 )
      + RECT via3 ( -100 -8100 ) ( 100 -7900 )
      + RECT via3 ( 300 -8100 ) ( 500 -7900 )
      + RECT via3 ( 700 -8100 ) ( 900 -7900 )
      + RECT via3 ( 1100 -8100 ) ( 1300 -7900 )
      + RECT via3 ( 1500 -8100 ) ( 1700 -7900 )
      + RECT via3 ( 1900 -8100 ) ( 2100 -7900 )
      + RECT via3 ( 2300 -8100 ) ( 2500 -7900 )
      + RECT via3 ( 2700 -8100 ) ( 2900 -7900 )
      + RECT via3 ( 3100 -8100 ) ( 3300 -7900 )
      + RECT via3 ( 3500 -8100 ) ( 3700 -7900 )
      + RECT via3 ( 3900 -8100 ) ( 4100 -7900 )
      + RECT via3 ( 4300 -8100 ) ( 4500 -7900 )
      + RECT via3 ( 4700 -8100 ) ( 4900 -7900 )
      + RECT via3 ( 5100 -8100 ) ( 5300 -7900 )
      + RECT via3 ( 5500 -8100 ) ( 5700 -7900 )
      + RECT via3 ( -5700 -7700 ) ( -5500 -7500 )
      + RECT via3 ( -5300 -7700 ) ( -5100 -7500 )
      + RECT via3 ( -4900 -7700 ) ( -4700 -7500 )
      + RECT via3 ( -4500 -7700 ) ( -4300 -7500 )
      + RECT via3 ( -4100 -7700 ) ( -3900 -7500 )
      + RECT via3 ( -3700 -7700 ) ( -3500 -7500 )
      + RECT via3 ( -3300 -7700 ) ( -3100 -7500 )
      + RECT via3 ( -2900 -7700 ) ( -2700 -7500 )
      + RECT via3 ( -2500 -7700 ) ( -2300 -7500 )
      + RECT via3 ( -2100 -7700 ) ( -1900 -7500 )
      + RECT via3 ( -1700 -7700 ) ( -1500 -7500 )
      + RECT via3 ( -1300 -7700 ) ( -1100 -7500 )
      + RECT via3 ( -900 -7700 ) ( -700 -7500 )
      + RECT via3 ( -500 -7700 ) ( -300 -7500 )
      + RECT via3 ( -100 -7700 ) ( 100 -7500 )
      + RECT via3 ( 300 -7700 ) ( 500 -7500 )
      + RECT via3 ( 700 -7700 ) ( 900 -7500 )
      + RECT via3 ( 1100 -7700 ) ( 1300 -7500 )
      + RECT via3 ( 1500 -7700 ) ( 1700 -7500 )
      + RECT via3 ( 1900 -7700 ) ( 2100 -7500 )
      + RECT via3 ( 2300 -7700 ) ( 2500 -7500 )
      + RECT via3 ( 2700 -7700 ) ( 2900 -7500 )
      + RECT via3 ( 3100 -7700 ) ( 3300 -7500 )
      + RECT via3 ( 3500 -7700 ) ( 3700 -7500 )
      + RECT via3 ( 3900 -7700 ) ( 4100 -7500 )
      + RECT via3 ( 4300 -7700 ) ( 4500 -7500 )
      + RECT via3 ( 4700 -7700 ) ( 4900 -7500 )
      + RECT via3 ( 5100 -7700 ) ( 5300 -7500 )
      + RECT via3 ( 5500 -7700 ) ( 5700 -7500 )
      + RECT via3 ( -5700 -7300 ) ( -5500 -7100 )
      + RECT via3 ( -5300 -7300 ) ( -5100 -7100 )
      + RECT via3 ( -4900 -7300 ) ( -4700 -7100 )
      + RECT via3 ( -4500 -7300 ) ( -4300 -7100 )
      + RECT via3 ( -4100 -7300 ) ( -3900 -7100 )
      + RECT via3 ( -3700 -7300 ) ( -3500 -7100 )
      + RECT via3 ( -3300 -7300 ) ( -3100 -7100 )
      + RECT via3 ( -2900 -7300 ) ( -2700 -7100 )
      + RECT via3 ( -2500 -7300 ) ( -2300 -7100 )
      + RECT via3 ( -2100 -7300 ) ( -1900 -7100 )
      + RECT via3 ( -1700 -7300 ) ( -1500 -7100 )
      + RECT via3 ( -1300 -7300 ) ( -1100 -7100 )
      + RECT via3 ( -900 -7300 ) ( -700 -7100 )
      + RECT via3 ( -500 -7300 ) ( -300 -7100 )
      + RECT via3 ( -100 -7300 ) ( 100 -7100 )
      + RECT via3 ( 300 -7300 ) ( 500 -7100 )
      + RECT via3 ( 700 -7300 ) ( 900 -7100 )
      + RECT via3 ( 1100 -7300 ) ( 1300 -7100 )
      + RECT via3 ( 1500 -7300 ) ( 1700 -7100 )
      + RECT via3 ( 1900 -7300 ) ( 2100 -7100 )
      + RECT via3 ( 2300 -7300 ) ( 2500 -7100 )
      + RECT via3 ( 2700 -7300 ) ( 2900 -7100 )
      + RECT via3 ( 3100 -7300 ) ( 3300 -7100 )
      + RECT via3 ( 3500 -7300 ) ( 3700 -7100 )
      + RECT via3 ( 3900 -7300 ) ( 4100 -7100 )
      + RECT via3 ( 4300 -7300 ) ( 4500 -7100 )
      + RECT via3 ( 4700 -7300 ) ( 4900 -7100 )
      + RECT via3 ( 5100 -7300 ) ( 5300 -7100 )
      + RECT via3 ( 5500 -7300 ) ( 5700 -7100 )
      + RECT via3 ( -5700 -6900 ) ( -5500 -6700 )
      + RECT via3 ( -5300 -6900 ) ( -5100 -6700 )
      + RECT via3 ( -4900 -6900 ) ( -4700 -6700 )
      + RECT via3 ( -4500 -6900 ) ( -4300 -6700 )
      + RECT via3 ( -4100 -6900 ) ( -3900 -6700 )
      + RECT via3 ( -3700 -6900 ) ( -3500 -6700 )
      + RECT via3 ( -3300 -6900 ) ( -3100 -6700 )
      + RECT via3 ( -2900 -6900 ) ( -2700 -6700 )
      + RECT via3 ( -2500 -6900 ) ( -2300 -6700 )
      + RECT via3 ( -2100 -6900 ) ( -1900 -6700 )
      + RECT via3 ( -1700 -6900 ) ( -1500 -6700 )
      + RECT via3 ( -1300 -6900 ) ( -1100 -6700 )
      + RECT via3 ( -900 -6900 ) ( -700 -6700 )
      + RECT via3 ( -500 -6900 ) ( -300 -6700 )
      + RECT via3 ( -100 -6900 ) ( 100 -6700 )
      + RECT via3 ( 300 -6900 ) ( 500 -6700 )
      + RECT via3 ( 700 -6900 ) ( 900 -6700 )
      + RECT via3 ( 1100 -6900 ) ( 1300 -6700 )
      + RECT via3 ( 1500 -6900 ) ( 1700 -6700 )
      + RECT via3 ( 1900 -6900 ) ( 2100 -6700 )
      + RECT via3 ( 2300 -6900 ) ( 2500 -6700 )
      + RECT via3 ( 2700 -6900 ) ( 2900 -6700 )
      + RECT via3 ( 3100 -6900 ) ( 3300 -6700 )
      + RECT via3 ( 3500 -6900 ) ( 3700 -6700 )
      + RECT via3 ( 3900 -6900 ) ( 4100 -6700 )
      + RECT via3 ( 4300 -6900 ) ( 4500 -6700 )
      + RECT via3 ( 4700 -6900 ) ( 4900 -6700 )
      + RECT via3 ( 5100 -6900 ) ( 5300 -6700 )
      + RECT via3 ( 5500 -6900 ) ( 5700 -6700 )
      + RECT via3 ( -5700 -6500 ) ( -5500 -6300 )
      + RECT via3 ( -5300 -6500 ) ( -5100 -6300 )
      + RECT via3 ( -4900 -6500 ) ( -4700 -6300 )
      + RECT via3 ( -4500 -6500 ) ( -4300 -6300 )
      + RECT via3 ( -4100 -6500 ) ( -3900 -6300 )
      + RECT via3 ( -3700 -6500 ) ( -3500 -6300 )
      + RECT via3 ( -3300 -6500 ) ( -3100 -6300 )
      + RECT via3 ( -2900 -6500 ) ( -2700 -6300 )
      + RECT via3 ( -2500 -6500 ) ( -2300 -6300 )
      + RECT via3 ( -2100 -6500 ) ( -1900 -6300 )
      + RECT via3 ( -1700 -6500 ) ( -1500 -6300 )
      + RECT via3 ( -1300 -6500 ) ( -1100 -6300 )
      + RECT via3 ( -900 -6500 ) ( -700 -6300 )
      + RECT via3 ( -500 -6500 ) ( -300 -6300 )
      + RECT via3 ( -100 -6500 ) ( 100 -6300 )
      + RECT via3 ( 300 -6500 ) ( 500 -6300 )
      + RECT via3 ( 700 -6500 ) ( 900 -6300 )
      + RECT via3 ( 1100 -6500 ) ( 1300 -6300 )
      + RECT via3 ( 1500 -6500 ) ( 1700 -6300 )
      + RECT via3 ( 1900 -6500 ) ( 2100 -6300 )
      + RECT via3 ( 2300 -6500 ) ( 2500 -6300 )
      + RECT via3 ( 2700 -6500 ) ( 2900 -6300 )
      + RECT via3 ( 3100 -6500 ) ( 3300 -6300 )
      + RECT via3 ( 3500 -6500 ) ( 3700 -6300 )
      + RECT via3 ( 3900 -6500 ) ( 4100 -6300 )
      + RECT via3 ( 4300 -6500 ) ( 4500 -6300 )
      + RECT via3 ( 4700 -6500 ) ( 4900 -6300 )
      + RECT via3 ( 5100 -6500 ) ( 5300 -6300 )
      + RECT via3 ( 5500 -6500 ) ( 5700 -6300 )
      + RECT via3 ( -5700 -6100 ) ( -5500 -5900 )
      + RECT via3 ( -5300 -6100 ) ( -5100 -5900 )
      + RECT via3 ( -4900 -6100 ) ( -4700 -5900 )
      + RECT via3 ( -4500 -6100 ) ( -4300 -5900 )
      + RECT via3 ( -4100 -6100 ) ( -3900 -5900 )
      + RECT via3 ( -3700 -6100 ) ( -3500 -5900 )
      + RECT via3 ( -3300 -6100 ) ( -3100 -5900 )
      + RECT via3 ( -2900 -6100 ) ( -2700 -5900 )
      + RECT via3 ( -2500 -6100 ) ( -2300 -5900 )
      + RECT via3 ( -2100 -6100 ) ( -1900 -5900 )
      + RECT via3 ( -1700 -6100 ) ( -1500 -5900 )
      + RECT via3 ( -1300 -6100 ) ( -1100 -5900 )
      + RECT via3 ( -900 -6100 ) ( -700 -5900 )
      + RECT via3 ( -500 -6100 ) ( -300 -5900 )
      + RECT via3 ( -100 -6100 ) ( 100 -5900 )
      + RECT via3 ( 300 -6100 ) ( 500 -5900 )
      + RECT via3 ( 700 -6100 ) ( 900 -5900 )
      + RECT via3 ( 1100 -6100 ) ( 1300 -5900 )
      + RECT via3 ( 1500 -6100 ) ( 1700 -5900 )
      + RECT via3 ( 1900 -6100 ) ( 2100 -5900 )
      + RECT via3 ( 2300 -6100 ) ( 2500 -5900 )
      + RECT via3 ( 2700 -6100 ) ( 2900 -5900 )
      + RECT via3 ( 3100 -6100 ) ( 3300 -5900 )
      + RECT via3 ( 3500 -6100 ) ( 3700 -5900 )
      + RECT via3 ( 3900 -6100 ) ( 4100 -5900 )
      + RECT via3 ( 4300 -6100 ) ( 4500 -5900 )
      + RECT via3 ( 4700 -6100 ) ( 4900 -5900 )
      + RECT via3 ( 5100 -6100 ) ( 5300 -5900 )
      + RECT via3 ( 5500 -6100 ) ( 5700 -5900 )
      + RECT via3 ( -5700 -5700 ) ( -5500 -5500 )
      + RECT via3 ( -5300 -5700 ) ( -5100 -5500 )
      + RECT via3 ( -4900 -5700 ) ( -4700 -5500 )
      + RECT via3 ( -4500 -5700 ) ( -4300 -5500 )
      + RECT via3 ( -4100 -5700 ) ( -3900 -5500 )
      + RECT via3 ( -3700 -5700 ) ( -3500 -5500 )
      + RECT via3 ( -3300 -5700 ) ( -3100 -5500 )
      + RECT via3 ( -2900 -5700 ) ( -2700 -5500 )
      + RECT via3 ( -2500 -5700 ) ( -2300 -5500 )
      + RECT via3 ( -2100 -5700 ) ( -1900 -5500 )
      + RECT via3 ( -1700 -5700 ) ( -1500 -5500 )
      + RECT via3 ( -1300 -5700 ) ( -1100 -5500 )
      + RECT via3 ( -900 -5700 ) ( -700 -5500 )
      + RECT via3 ( -500 -5700 ) ( -300 -5500 )
      + RECT via3 ( -100 -5700 ) ( 100 -5500 )
      + RECT via3 ( 300 -5700 ) ( 500 -5500 )
      + RECT via3 ( 700 -5700 ) ( 900 -5500 )
      + RECT via3 ( 1100 -5700 ) ( 1300 -5500 )
      + RECT via3 ( 1500 -5700 ) ( 1700 -5500 )
      + RECT via3 ( 1900 -5700 ) ( 2100 -5500 )
      + RECT via3 ( 2300 -5700 ) ( 2500 -5500 )
      + RECT via3 ( 2700 -5700 ) ( 2900 -5500 )
      + RECT via3 ( 3100 -5700 ) ( 3300 -5500 )
      + RECT via3 ( 3500 -5700 ) ( 3700 -5500 )
      + RECT via3 ( 3900 -5700 ) ( 4100 -5500 )
      + RECT via3 ( 4300 -5700 ) ( 4500 -5500 )
      + RECT via3 ( 4700 -5700 ) ( 4900 -5500 )
      + RECT via3 ( 5100 -5700 ) ( 5300 -5500 )
      + RECT via3 ( 5500 -5700 ) ( 5700 -5500 )
      + RECT via3 ( -5700 -5300 ) ( -5500 -5100 )
      + RECT via3 ( -5300 -5300 ) ( -5100 -5100 )
      + RECT via3 ( -4900 -5300 ) ( -4700 -5100 )
      + RECT via3 ( -4500 -5300 ) ( -4300 -5100 )
      + RECT via3 ( -4100 -5300 ) ( -3900 -5100 )
      + RECT via3 ( -3700 -5300 ) ( -3500 -5100 )
      + RECT via3 ( -3300 -5300 ) ( -3100 -5100 )
      + RECT via3 ( -2900 -5300 ) ( -2700 -5100 )
      + RECT via3 ( -2500 -5300 ) ( -2300 -5100 )
      + RECT via3 ( -2100 -5300 ) ( -1900 -5100 )
      + RECT via3 ( -1700 -5300 ) ( -1500 -5100 )
      + RECT via3 ( -1300 -5300 ) ( -1100 -5100 )
      + RECT via3 ( -900 -5300 ) ( -700 -5100 )
      + RECT via3 ( -500 -5300 ) ( -300 -5100 )
      + RECT via3 ( -100 -5300 ) ( 100 -5100 )
      + RECT via3 ( 300 -5300 ) ( 500 -5100 )
      + RECT via3 ( 700 -5300 ) ( 900 -5100 )
      + RECT via3 ( 1100 -5300 ) ( 1300 -5100 )
      + RECT via3 ( 1500 -5300 ) ( 1700 -5100 )
      + RECT via3 ( 1900 -5300 ) ( 2100 -5100 )
      + RECT via3 ( 2300 -5300 ) ( 2500 -5100 )
      + RECT via3 ( 2700 -5300 ) ( 2900 -5100 )
      + RECT via3 ( 3100 -5300 ) ( 3300 -5100 )
      + RECT via3 ( 3500 -5300 ) ( 3700 -5100 )
      + RECT via3 ( 3900 -5300 ) ( 4100 -5100 )
      + RECT via3 ( 4300 -5300 ) ( 4500 -5100 )
      + RECT via3 ( 4700 -5300 ) ( 4900 -5100 )
      + RECT via3 ( 5100 -5300 ) ( 5300 -5100 )
      + RECT via3 ( 5500 -5300 ) ( 5700 -5100 )
      + RECT via3 ( -5700 -4900 ) ( -5500 -4700 )
      + RECT via3 ( -5300 -4900 ) ( -5100 -4700 )
      + RECT via3 ( -4900 -4900 ) ( -4700 -4700 )
      + RECT via3 ( -4500 -4900 ) ( -4300 -4700 )
      + RECT via3 ( -4100 -4900 ) ( -3900 -4700 )
      + RECT via3 ( -3700 -4900 ) ( -3500 -4700 )
      + RECT via3 ( -3300 -4900 ) ( -3100 -4700 )
      + RECT via3 ( -2900 -4900 ) ( -2700 -4700 )
      + RECT via3 ( -2500 -4900 ) ( -2300 -4700 )
      + RECT via3 ( -2100 -4900 ) ( -1900 -4700 )
      + RECT via3 ( -1700 -4900 ) ( -1500 -4700 )
      + RECT via3 ( -1300 -4900 ) ( -1100 -4700 )
      + RECT via3 ( -900 -4900 ) ( -700 -4700 )
      + RECT via3 ( -500 -4900 ) ( -300 -4700 )
      + RECT via3 ( -100 -4900 ) ( 100 -4700 )
      + RECT via3 ( 300 -4900 ) ( 500 -4700 )
      + RECT via3 ( 700 -4900 ) ( 900 -4700 )
      + RECT via3 ( 1100 -4900 ) ( 1300 -4700 )
      + RECT via3 ( 1500 -4900 ) ( 1700 -4700 )
      + RECT via3 ( 1900 -4900 ) ( 2100 -4700 )
      + RECT via3 ( 2300 -4900 ) ( 2500 -4700 )
      + RECT via3 ( 2700 -4900 ) ( 2900 -4700 )
      + RECT via3 ( 3100 -4900 ) ( 3300 -4700 )
      + RECT via3 ( 3500 -4900 ) ( 3700 -4700 )
      + RECT via3 ( 3900 -4900 ) ( 4100 -4700 )
      + RECT via3 ( 4300 -4900 ) ( 4500 -4700 )
      + RECT via3 ( 4700 -4900 ) ( 4900 -4700 )
      + RECT via3 ( 5100 -4900 ) ( 5300 -4700 )
      + RECT via3 ( 5500 -4900 ) ( 5700 -4700 )
      + RECT via3 ( -5700 -4500 ) ( -5500 -4300 )
      + RECT via3 ( -5300 -4500 ) ( -5100 -4300 )
      + RECT via3 ( -4900 -4500 ) ( -4700 -4300 )
      + RECT via3 ( -4500 -4500 ) ( -4300 -4300 )
      + RECT via3 ( -4100 -4500 ) ( -3900 -4300 )
      + RECT via3 ( -3700 -4500 ) ( -3500 -4300 )
      + RECT via3 ( -3300 -4500 ) ( -3100 -4300 )
      + RECT via3 ( -2900 -4500 ) ( -2700 -4300 )
      + RECT via3 ( -2500 -4500 ) ( -2300 -4300 )
      + RECT via3 ( -2100 -4500 ) ( -1900 -4300 )
      + RECT via3 ( -1700 -4500 ) ( -1500 -4300 )
      + RECT via3 ( -1300 -4500 ) ( -1100 -4300 )
      + RECT via3 ( -900 -4500 ) ( -700 -4300 )
      + RECT via3 ( -500 -4500 ) ( -300 -4300 )
      + RECT via3 ( -100 -4500 ) ( 100 -4300 )
      + RECT via3 ( 300 -4500 ) ( 500 -4300 )
      + RECT via3 ( 700 -4500 ) ( 900 -4300 )
      + RECT via3 ( 1100 -4500 ) ( 1300 -4300 )
      + RECT via3 ( 1500 -4500 ) ( 1700 -4300 )
      + RECT via3 ( 1900 -4500 ) ( 2100 -4300 )
      + RECT via3 ( 2300 -4500 ) ( 2500 -4300 )
      + RECT via3 ( 2700 -4500 ) ( 2900 -4300 )
      + RECT via3 ( 3100 -4500 ) ( 3300 -4300 )
      + RECT via3 ( 3500 -4500 ) ( 3700 -4300 )
      + RECT via3 ( 3900 -4500 ) ( 4100 -4300 )
      + RECT via3 ( 4300 -4500 ) ( 4500 -4300 )
      + RECT via3 ( 4700 -4500 ) ( 4900 -4300 )
      + RECT via3 ( 5100 -4500 ) ( 5300 -4300 )
      + RECT via3 ( 5500 -4500 ) ( 5700 -4300 )
      + RECT via3 ( -5700 -4100 ) ( -5500 -3900 )
      + RECT via3 ( -5300 -4100 ) ( -5100 -3900 )
      + RECT via3 ( -4900 -4100 ) ( -4700 -3900 )
      + RECT via3 ( -4500 -4100 ) ( -4300 -3900 )
      + RECT via3 ( -4100 -4100 ) ( -3900 -3900 )
      + RECT via3 ( -3700 -4100 ) ( -3500 -3900 )
      + RECT via3 ( -3300 -4100 ) ( -3100 -3900 )
      + RECT via3 ( -2900 -4100 ) ( -2700 -3900 )
      + RECT via3 ( -2500 -4100 ) ( -2300 -3900 )
      + RECT via3 ( -2100 -4100 ) ( -1900 -3900 )
      + RECT via3 ( -1700 -4100 ) ( -1500 -3900 )
      + RECT via3 ( -1300 -4100 ) ( -1100 -3900 )
      + RECT via3 ( -900 -4100 ) ( -700 -3900 )
      + RECT via3 ( -500 -4100 ) ( -300 -3900 )
      + RECT via3 ( -100 -4100 ) ( 100 -3900 )
      + RECT via3 ( 300 -4100 ) ( 500 -3900 )
      + RECT via3 ( 700 -4100 ) ( 900 -3900 )
      + RECT via3 ( 1100 -4100 ) ( 1300 -3900 )
      + RECT via3 ( 1500 -4100 ) ( 1700 -3900 )
      + RECT via3 ( 1900 -4100 ) ( 2100 -3900 )
      + RECT via3 ( 2300 -4100 ) ( 2500 -3900 )
      + RECT via3 ( 2700 -4100 ) ( 2900 -3900 )
      + RECT via3 ( 3100 -4100 ) ( 3300 -3900 )
      + RECT via3 ( 3500 -4100 ) ( 3700 -3900 )
      + RECT via3 ( 3900 -4100 ) ( 4100 -3900 )
      + RECT via3 ( 4300 -4100 ) ( 4500 -3900 )
      + RECT via3 ( 4700 -4100 ) ( 4900 -3900 )
      + RECT via3 ( 5100 -4100 ) ( 5300 -3900 )
      + RECT via3 ( 5500 -4100 ) ( 5700 -3900 )
      + RECT via3 ( -5700 -3700 ) ( -5500 -3500 )
      + RECT via3 ( -5300 -3700 ) ( -5100 -3500 )
      + RECT via3 ( -4900 -3700 ) ( -4700 -3500 )
      + RECT via3 ( -4500 -3700 ) ( -4300 -3500 )
      + RECT via3 ( -4100 -3700 ) ( -3900 -3500 )
      + RECT via3 ( -3700 -3700 ) ( -3500 -3500 )
      + RECT via3 ( -3300 -3700 ) ( -3100 -3500 )
      + RECT via3 ( -2900 -3700 ) ( -2700 -3500 )
      + RECT via3 ( -2500 -3700 ) ( -2300 -3500 )
      + RECT via3 ( -2100 -3700 ) ( -1900 -3500 )
      + RECT via3 ( -1700 -3700 ) ( -1500 -3500 )
      + RECT via3 ( -1300 -3700 ) ( -1100 -3500 )
      + RECT via3 ( -900 -3700 ) ( -700 -3500 )
      + RECT via3 ( -500 -3700 ) ( -300 -3500 )
      + RECT via3 ( -100 -3700 ) ( 100 -3500 )
      + RECT via3 ( 300 -3700 ) ( 500 -3500 )
      + RECT via3 ( 700 -3700 ) ( 900 -3500 )
      + RECT via3 ( 1100 -3700 ) ( 1300 -3500 )
      + RECT via3 ( 1500 -3700 ) ( 1700 -3500 )
      + RECT via3 ( 1900 -3700 ) ( 2100 -3500 )
      + RECT via3 ( 2300 -3700 ) ( 2500 -3500 )
      + RECT via3 ( 2700 -3700 ) ( 2900 -3500 )
      + RECT via3 ( 3100 -3700 ) ( 3300 -3500 )
      + RECT via3 ( 3500 -3700 ) ( 3700 -3500 )
      + RECT via3 ( 3900 -3700 ) ( 4100 -3500 )
      + RECT via3 ( 4300 -3700 ) ( 4500 -3500 )
      + RECT via3 ( 4700 -3700 ) ( 4900 -3500 )
      + RECT via3 ( 5100 -3700 ) ( 5300 -3500 )
      + RECT via3 ( 5500 -3700 ) ( 5700 -3500 )
      + RECT via3 ( -5700 -3300 ) ( -5500 -3100 )
      + RECT via3 ( -5300 -3300 ) ( -5100 -3100 )
      + RECT via3 ( -4900 -3300 ) ( -4700 -3100 )
      + RECT via3 ( -4500 -3300 ) ( -4300 -3100 )
      + RECT via3 ( -4100 -3300 ) ( -3900 -3100 )
      + RECT via3 ( -3700 -3300 ) ( -3500 -3100 )
      + RECT via3 ( -3300 -3300 ) ( -3100 -3100 )
      + RECT via3 ( -2900 -3300 ) ( -2700 -3100 )
      + RECT via3 ( -2500 -3300 ) ( -2300 -3100 )
      + RECT via3 ( -2100 -3300 ) ( -1900 -3100 )
      + RECT via3 ( -1700 -3300 ) ( -1500 -3100 )
      + RECT via3 ( -1300 -3300 ) ( -1100 -3100 )
      + RECT via3 ( -900 -3300 ) ( -700 -3100 )
      + RECT via3 ( -500 -3300 ) ( -300 -3100 )
      + RECT via3 ( -100 -3300 ) ( 100 -3100 )
      + RECT via3 ( 300 -3300 ) ( 500 -3100 )
      + RECT via3 ( 700 -3300 ) ( 900 -3100 )
      + RECT via3 ( 1100 -3300 ) ( 1300 -3100 )
      + RECT via3 ( 1500 -3300 ) ( 1700 -3100 )
      + RECT via3 ( 1900 -3300 ) ( 2100 -3100 )
      + RECT via3 ( 2300 -3300 ) ( 2500 -3100 )
      + RECT via3 ( 2700 -3300 ) ( 2900 -3100 )
      + RECT via3 ( 3100 -3300 ) ( 3300 -3100 )
      + RECT via3 ( 3500 -3300 ) ( 3700 -3100 )
      + RECT via3 ( 3900 -3300 ) ( 4100 -3100 )
      + RECT via3 ( 4300 -3300 ) ( 4500 -3100 )
      + RECT via3 ( 4700 -3300 ) ( 4900 -3100 )
      + RECT via3 ( 5100 -3300 ) ( 5300 -3100 )
      + RECT via3 ( 5500 -3300 ) ( 5700 -3100 )
      + RECT via3 ( -5700 -2900 ) ( -5500 -2700 )
      + RECT via3 ( -5300 -2900 ) ( -5100 -2700 )
      + RECT via3 ( -4900 -2900 ) ( -4700 -2700 )
      + RECT via3 ( -4500 -2900 ) ( -4300 -2700 )
      + RECT via3 ( -4100 -2900 ) ( -3900 -2700 )
      + RECT via3 ( -3700 -2900 ) ( -3500 -2700 )
      + RECT via3 ( -3300 -2900 ) ( -3100 -2700 )
      + RECT via3 ( -2900 -2900 ) ( -2700 -2700 )
      + RECT via3 ( -2500 -2900 ) ( -2300 -2700 )
      + RECT via3 ( -2100 -2900 ) ( -1900 -2700 )
      + RECT via3 ( -1700 -2900 ) ( -1500 -2700 )
      + RECT via3 ( -1300 -2900 ) ( -1100 -2700 )
      + RECT via3 ( -900 -2900 ) ( -700 -2700 )
      + RECT via3 ( -500 -2900 ) ( -300 -2700 )
      + RECT via3 ( -100 -2900 ) ( 100 -2700 )
      + RECT via3 ( 300 -2900 ) ( 500 -2700 )
      + RECT via3 ( 700 -2900 ) ( 900 -2700 )
      + RECT via3 ( 1100 -2900 ) ( 1300 -2700 )
      + RECT via3 ( 1500 -2900 ) ( 1700 -2700 )
      + RECT via3 ( 1900 -2900 ) ( 2100 -2700 )
      + RECT via3 ( 2300 -2900 ) ( 2500 -2700 )
      + RECT via3 ( 2700 -2900 ) ( 2900 -2700 )
      + RECT via3 ( 3100 -2900 ) ( 3300 -2700 )
      + RECT via3 ( 3500 -2900 ) ( 3700 -2700 )
      + RECT via3 ( 3900 -2900 ) ( 4100 -2700 )
      + RECT via3 ( 4300 -2900 ) ( 4500 -2700 )
      + RECT via3 ( 4700 -2900 ) ( 4900 -2700 )
      + RECT via3 ( 5100 -2900 ) ( 5300 -2700 )
      + RECT via3 ( 5500 -2900 ) ( 5700 -2700 )
      + RECT via3 ( -5700 -2500 ) ( -5500 -2300 )
      + RECT via3 ( -5300 -2500 ) ( -5100 -2300 )
      + RECT via3 ( -4900 -2500 ) ( -4700 -2300 )
      + RECT via3 ( -4500 -2500 ) ( -4300 -2300 )
      + RECT via3 ( -4100 -2500 ) ( -3900 -2300 )
      + RECT via3 ( -3700 -2500 ) ( -3500 -2300 )
      + RECT via3 ( -3300 -2500 ) ( -3100 -2300 )
      + RECT via3 ( -2900 -2500 ) ( -2700 -2300 )
      + RECT via3 ( -2500 -2500 ) ( -2300 -2300 )
      + RECT via3 ( -2100 -2500 ) ( -1900 -2300 )
      + RECT via3 ( -1700 -2500 ) ( -1500 -2300 )
      + RECT via3 ( -1300 -2500 ) ( -1100 -2300 )
      + RECT via3 ( -900 -2500 ) ( -700 -2300 )
      + RECT via3 ( -500 -2500 ) ( -300 -2300 )
      + RECT via3 ( -100 -2500 ) ( 100 -2300 )
      + RECT via3 ( 300 -2500 ) ( 500 -2300 )
      + RECT via3 ( 700 -2500 ) ( 900 -2300 )
      + RECT via3 ( 1100 -2500 ) ( 1300 -2300 )
      + RECT via3 ( 1500 -2500 ) ( 1700 -2300 )
      + RECT via3 ( 1900 -2500 ) ( 2100 -2300 )
      + RECT via3 ( 2300 -2500 ) ( 2500 -2300 )
      + RECT via3 ( 2700 -2500 ) ( 2900 -2300 )
      + RECT via3 ( 3100 -2500 ) ( 3300 -2300 )
      + RECT via3 ( 3500 -2500 ) ( 3700 -2300 )
      + RECT via3 ( 3900 -2500 ) ( 4100 -2300 )
      + RECT via3 ( 4300 -2500 ) ( 4500 -2300 )
      + RECT via3 ( 4700 -2500 ) ( 4900 -2300 )
      + RECT via3 ( 5100 -2500 ) ( 5300 -2300 )
      + RECT via3 ( 5500 -2500 ) ( 5700 -2300 )
      + RECT via3 ( -5700 -2100 ) ( -5500 -1900 )
      + RECT via3 ( -5300 -2100 ) ( -5100 -1900 )
      + RECT via3 ( -4900 -2100 ) ( -4700 -1900 )
      + RECT via3 ( -4500 -2100 ) ( -4300 -1900 )
      + RECT via3 ( -4100 -2100 ) ( -3900 -1900 )
      + RECT via3 ( -3700 -2100 ) ( -3500 -1900 )
      + RECT via3 ( -3300 -2100 ) ( -3100 -1900 )
      + RECT via3 ( -2900 -2100 ) ( -2700 -1900 )
      + RECT via3 ( -2500 -2100 ) ( -2300 -1900 )
      + RECT via3 ( -2100 -2100 ) ( -1900 -1900 )
      + RECT via3 ( -1700 -2100 ) ( -1500 -1900 )
      + RECT via3 ( -1300 -2100 ) ( -1100 -1900 )
      + RECT via3 ( -900 -2100 ) ( -700 -1900 )
      + RECT via3 ( -500 -2100 ) ( -300 -1900 )
      + RECT via3 ( -100 -2100 ) ( 100 -1900 )
      + RECT via3 ( 300 -2100 ) ( 500 -1900 )
      + RECT via3 ( 700 -2100 ) ( 900 -1900 )
      + RECT via3 ( 1100 -2100 ) ( 1300 -1900 )
      + RECT via3 ( 1500 -2100 ) ( 1700 -1900 )
      + RECT via3 ( 1900 -2100 ) ( 2100 -1900 )
      + RECT via3 ( 2300 -2100 ) ( 2500 -1900 )
      + RECT via3 ( 2700 -2100 ) ( 2900 -1900 )
      + RECT via3 ( 3100 -2100 ) ( 3300 -1900 )
      + RECT via3 ( 3500 -2100 ) ( 3700 -1900 )
      + RECT via3 ( 3900 -2100 ) ( 4100 -1900 )
      + RECT via3 ( 4300 -2100 ) ( 4500 -1900 )
      + RECT via3 ( 4700 -2100 ) ( 4900 -1900 )
      + RECT via3 ( 5100 -2100 ) ( 5300 -1900 )
      + RECT via3 ( 5500 -2100 ) ( 5700 -1900 )
      + RECT via3 ( -5700 -1700 ) ( -5500 -1500 )
      + RECT via3 ( -5300 -1700 ) ( -5100 -1500 )
      + RECT via3 ( -4900 -1700 ) ( -4700 -1500 )
      + RECT via3 ( -4500 -1700 ) ( -4300 -1500 )
      + RECT via3 ( -4100 -1700 ) ( -3900 -1500 )
      + RECT via3 ( -3700 -1700 ) ( -3500 -1500 )
      + RECT via3 ( -3300 -1700 ) ( -3100 -1500 )
      + RECT via3 ( -2900 -1700 ) ( -2700 -1500 )
      + RECT via3 ( -2500 -1700 ) ( -2300 -1500 )
      + RECT via3 ( -2100 -1700 ) ( -1900 -1500 )
      + RECT via3 ( -1700 -1700 ) ( -1500 -1500 )
      + RECT via3 ( -1300 -1700 ) ( -1100 -1500 )
      + RECT via3 ( -900 -1700 ) ( -700 -1500 )
      + RECT via3 ( -500 -1700 ) ( -300 -1500 )
      + RECT via3 ( -100 -1700 ) ( 100 -1500 )
      + RECT via3 ( 300 -1700 ) ( 500 -1500 )
      + RECT via3 ( 700 -1700 ) ( 900 -1500 )
      + RECT via3 ( 1100 -1700 ) ( 1300 -1500 )
      + RECT via3 ( 1500 -1700 ) ( 1700 -1500 )
      + RECT via3 ( 1900 -1700 ) ( 2100 -1500 )
      + RECT via3 ( 2300 -1700 ) ( 2500 -1500 )
      + RECT via3 ( 2700 -1700 ) ( 2900 -1500 )
      + RECT via3 ( 3100 -1700 ) ( 3300 -1500 )
      + RECT via3 ( 3500 -1700 ) ( 3700 -1500 )
      + RECT via3 ( 3900 -1700 ) ( 4100 -1500 )
      + RECT via3 ( 4300 -1700 ) ( 4500 -1500 )
      + RECT via3 ( 4700 -1700 ) ( 4900 -1500 )
      + RECT via3 ( 5100 -1700 ) ( 5300 -1500 )
      + RECT via3 ( 5500 -1700 ) ( 5700 -1500 )
      + RECT via3 ( -5700 -1300 ) ( -5500 -1100 )
      + RECT via3 ( -5300 -1300 ) ( -5100 -1100 )
      + RECT via3 ( -4900 -1300 ) ( -4700 -1100 )
      + RECT via3 ( -4500 -1300 ) ( -4300 -1100 )
      + RECT via3 ( -4100 -1300 ) ( -3900 -1100 )
      + RECT via3 ( -3700 -1300 ) ( -3500 -1100 )
      + RECT via3 ( -3300 -1300 ) ( -3100 -1100 )
      + RECT via3 ( -2900 -1300 ) ( -2700 -1100 )
      + RECT via3 ( -2500 -1300 ) ( -2300 -1100 )
      + RECT via3 ( -2100 -1300 ) ( -1900 -1100 )
      + RECT via3 ( -1700 -1300 ) ( -1500 -1100 )
      + RECT via3 ( -1300 -1300 ) ( -1100 -1100 )
      + RECT via3 ( -900 -1300 ) ( -700 -1100 )
      + RECT via3 ( -500 -1300 ) ( -300 -1100 )
      + RECT via3 ( -100 -1300 ) ( 100 -1100 )
      + RECT via3 ( 300 -1300 ) ( 500 -1100 )
      + RECT via3 ( 700 -1300 ) ( 900 -1100 )
      + RECT via3 ( 1100 -1300 ) ( 1300 -1100 )
      + RECT via3 ( 1500 -1300 ) ( 1700 -1100 )
      + RECT via3 ( 1900 -1300 ) ( 2100 -1100 )
      + RECT via3 ( 2300 -1300 ) ( 2500 -1100 )
      + RECT via3 ( 2700 -1300 ) ( 2900 -1100 )
      + RECT via3 ( 3100 -1300 ) ( 3300 -1100 )
      + RECT via3 ( 3500 -1300 ) ( 3700 -1100 )
      + RECT via3 ( 3900 -1300 ) ( 4100 -1100 )
      + RECT via3 ( 4300 -1300 ) ( 4500 -1100 )
      + RECT via3 ( 4700 -1300 ) ( 4900 -1100 )
      + RECT via3 ( 5100 -1300 ) ( 5300 -1100 )
      + RECT via3 ( 5500 -1300 ) ( 5700 -1100 )
      + RECT via3 ( -5700 -900 ) ( -5500 -700 )
      + RECT via3 ( -5300 -900 ) ( -5100 -700 )
      + RECT via3 ( -4900 -900 ) ( -4700 -700 )
      + RECT via3 ( -4500 -900 ) ( -4300 -700 )
      + RECT via3 ( -4100 -900 ) ( -3900 -700 )
      + RECT via3 ( -3700 -900 ) ( -3500 -700 )
      + RECT via3 ( -3300 -900 ) ( -3100 -700 )
      + RECT via3 ( -2900 -900 ) ( -2700 -700 )
      + RECT via3 ( -2500 -900 ) ( -2300 -700 )
      + RECT via3 ( -2100 -900 ) ( -1900 -700 )
      + RECT via3 ( -1700 -900 ) ( -1500 -700 )
      + RECT via3 ( -1300 -900 ) ( -1100 -700 )
      + RECT via3 ( -900 -900 ) ( -700 -700 )
      + RECT via3 ( -500 -900 ) ( -300 -700 )
      + RECT via3 ( -100 -900 ) ( 100 -700 )
      + RECT via3 ( 300 -900 ) ( 500 -700 )
      + RECT via3 ( 700 -900 ) ( 900 -700 )
      + RECT via3 ( 1100 -900 ) ( 1300 -700 )
      + RECT via3 ( 1500 -900 ) ( 1700 -700 )
      + RECT via3 ( 1900 -900 ) ( 2100 -700 )
      + RECT via3 ( 2300 -900 ) ( 2500 -700 )
      + RECT via3 ( 2700 -900 ) ( 2900 -700 )
      + RECT via3 ( 3100 -900 ) ( 3300 -700 )
      + RECT via3 ( 3500 -900 ) ( 3700 -700 )
      + RECT via3 ( 3900 -900 ) ( 4100 -700 )
      + RECT via3 ( 4300 -900 ) ( 4500 -700 )
      + RECT via3 ( 4700 -900 ) ( 4900 -700 )
      + RECT via3 ( 5100 -900 ) ( 5300 -700 )
      + RECT via3 ( 5500 -900 ) ( 5700 -700 )
      + RECT via3 ( -5700 -500 ) ( -5500 -300 )
      + RECT via3 ( -5300 -500 ) ( -5100 -300 )
      + RECT via3 ( -4900 -500 ) ( -4700 -300 )
      + RECT via3 ( -4500 -500 ) ( -4300 -300 )
      + RECT via3 ( -4100 -500 ) ( -3900 -300 )
      + RECT via3 ( -3700 -500 ) ( -3500 -300 )
      + RECT via3 ( -3300 -500 ) ( -3100 -300 )
      + RECT via3 ( -2900 -500 ) ( -2700 -300 )
      + RECT via3 ( -2500 -500 ) ( -2300 -300 )
      + RECT via3 ( -2100 -500 ) ( -1900 -300 )
      + RECT via3 ( -1700 -500 ) ( -1500 -300 )
      + RECT via3 ( -1300 -500 ) ( -1100 -300 )
      + RECT via3 ( -900 -500 ) ( -700 -300 )
      + RECT via3 ( -500 -500 ) ( -300 -300 )
      + RECT via3 ( -100 -500 ) ( 100 -300 )
      + RECT via3 ( 300 -500 ) ( 500 -300 )
      + RECT via3 ( 700 -500 ) ( 900 -300 )
      + RECT via3 ( 1100 -500 ) ( 1300 -300 )
      + RECT via3 ( 1500 -500 ) ( 1700 -300 )
      + RECT via3 ( 1900 -500 ) ( 2100 -300 )
      + RECT via3 ( 2300 -500 ) ( 2500 -300 )
      + RECT via3 ( 2700 -500 ) ( 2900 -300 )
      + RECT via3 ( 3100 -500 ) ( 3300 -300 )
      + RECT via3 ( 3500 -500 ) ( 3700 -300 )
      + RECT via3 ( 3900 -500 ) ( 4100 -300 )
      + RECT via3 ( 4300 -500 ) ( 4500 -300 )
      + RECT via3 ( 4700 -500 ) ( 4900 -300 )
      + RECT via3 ( 5100 -500 ) ( 5300 -300 )
      + RECT via3 ( 5500 -500 ) ( 5700 -300 )
      + RECT via3 ( -5700 -100 ) ( -5500 100 )
      + RECT via3 ( -5300 -100 ) ( -5100 100 )
      + RECT via3 ( -4900 -100 ) ( -4700 100 )
      + RECT via3 ( -4500 -100 ) ( -4300 100 )
      + RECT via3 ( -4100 -100 ) ( -3900 100 )
      + RECT via3 ( -3700 -100 ) ( -3500 100 )
      + RECT via3 ( -3300 -100 ) ( -3100 100 )
      + RECT via3 ( -2900 -100 ) ( -2700 100 )
      + RECT via3 ( -2500 -100 ) ( -2300 100 )
      + RECT via3 ( -2100 -100 ) ( -1900 100 )
      + RECT via3 ( -1700 -100 ) ( -1500 100 )
      + RECT via3 ( -1300 -100 ) ( -1100 100 )
      + RECT via3 ( -900 -100 ) ( -700 100 )
      + RECT via3 ( -500 -100 ) ( -300 100 )
      + RECT via3 ( -100 -100 ) ( 100 100 )
      + RECT via3 ( 300 -100 ) ( 500 100 )
      + RECT via3 ( 700 -100 ) ( 900 100 )
      + RECT via3 ( 1100 -100 ) ( 1300 100 )
      + RECT via3 ( 1500 -100 ) ( 1700 100 )
      + RECT via3 ( 1900 -100 ) ( 2100 100 )
      + RECT via3 ( 2300 -100 ) ( 2500 100 )
      + RECT via3 ( 2700 -100 ) ( 2900 100 )
      + RECT via3 ( 3100 -100 ) ( 3300 100 )
      + RECT via3 ( 3500 -100 ) ( 3700 100 )
      + RECT via3 ( 3900 -100 ) ( 4100 100 )
      + RECT via3 ( 4300 -100 ) ( 4500 100 )
      + RECT via3 ( 4700 -100 ) ( 4900 100 )
      + RECT via3 ( 5100 -100 ) ( 5300 100 )
      + RECT via3 ( 5500 -100 ) ( 5700 100 )
      + RECT via3 ( -5700 300 ) ( -5500 500 )
      + RECT via3 ( -5300 300 ) ( -5100 500 )
      + RECT via3 ( -4900 300 ) ( -4700 500 )
      + RECT via3 ( -4500 300 ) ( -4300 500 )
      + RECT via3 ( -4100 300 ) ( -3900 500 )
      + RECT via3 ( -3700 300 ) ( -3500 500 )
      + RECT via3 ( -3300 300 ) ( -3100 500 )
      + RECT via3 ( -2900 300 ) ( -2700 500 )
      + RECT via3 ( -2500 300 ) ( -2300 500 )
      + RECT via3 ( -2100 300 ) ( -1900 500 )
      + RECT via3 ( -1700 300 ) ( -1500 500 )
      + RECT via3 ( -1300 300 ) ( -1100 500 )
      + RECT via3 ( -900 300 ) ( -700 500 )
      + RECT via3 ( -500 300 ) ( -300 500 )
      + RECT via3 ( -100 300 ) ( 100 500 )
      + RECT via3 ( 300 300 ) ( 500 500 )
      + RECT via3 ( 700 300 ) ( 900 500 )
      + RECT via3 ( 1100 300 ) ( 1300 500 )
      + RECT via3 ( 1500 300 ) ( 1700 500 )
      + RECT via3 ( 1900 300 ) ( 2100 500 )
      + RECT via3 ( 2300 300 ) ( 2500 500 )
      + RECT via3 ( 2700 300 ) ( 2900 500 )
      + RECT via3 ( 3100 300 ) ( 3300 500 )
      + RECT via3 ( 3500 300 ) ( 3700 500 )
      + RECT via3 ( 3900 300 ) ( 4100 500 )
      + RECT via3 ( 4300 300 ) ( 4500 500 )
      + RECT via3 ( 4700 300 ) ( 4900 500 )
      + RECT via3 ( 5100 300 ) ( 5300 500 )
      + RECT via3 ( 5500 300 ) ( 5700 500 )
      + RECT via3 ( -5700 700 ) ( -5500 900 )
      + RECT via3 ( -5300 700 ) ( -5100 900 )
      + RECT via3 ( -4900 700 ) ( -4700 900 )
      + RECT via3 ( -4500 700 ) ( -4300 900 )
      + RECT via3 ( -4100 700 ) ( -3900 900 )
      + RECT via3 ( -3700 700 ) ( -3500 900 )
      + RECT via3 ( -3300 700 ) ( -3100 900 )
      + RECT via3 ( -2900 700 ) ( -2700 900 )
      + RECT via3 ( -2500 700 ) ( -2300 900 )
      + RECT via3 ( -2100 700 ) ( -1900 900 )
      + RECT via3 ( -1700 700 ) ( -1500 900 )
      + RECT via3 ( -1300 700 ) ( -1100 900 )
      + RECT via3 ( -900 700 ) ( -700 900 )
      + RECT via3 ( -500 700 ) ( -300 900 )
      + RECT via3 ( -100 700 ) ( 100 900 )
      + RECT via3 ( 300 700 ) ( 500 900 )
      + RECT via3 ( 700 700 ) ( 900 900 )
      + RECT via3 ( 1100 700 ) ( 1300 900 )
      + RECT via3 ( 1500 700 ) ( 1700 900 )
      + RECT via3 ( 1900 700 ) ( 2100 900 )
      + RECT via3 ( 2300 700 ) ( 2500 900 )
      + RECT via3 ( 2700 700 ) ( 2900 900 )
      + RECT via3 ( 3100 700 ) ( 3300 900 )
      + RECT via3 ( 3500 700 ) ( 3700 900 )
      + RECT via3 ( 3900 700 ) ( 4100 900 )
      + RECT via3 ( 4300 700 ) ( 4500 900 )
      + RECT via3 ( 4700 700 ) ( 4900 900 )
      + RECT via3 ( 5100 700 ) ( 5300 900 )
      + RECT via3 ( 5500 700 ) ( 5700 900 )
      + RECT via3 ( -5700 1100 ) ( -5500 1300 )
      + RECT via3 ( -5300 1100 ) ( -5100 1300 )
      + RECT via3 ( -4900 1100 ) ( -4700 1300 )
      + RECT via3 ( -4500 1100 ) ( -4300 1300 )
      + RECT via3 ( -4100 1100 ) ( -3900 1300 )
      + RECT via3 ( -3700 1100 ) ( -3500 1300 )
      + RECT via3 ( -3300 1100 ) ( -3100 1300 )
      + RECT via3 ( -2900 1100 ) ( -2700 1300 )
      + RECT via3 ( -2500 1100 ) ( -2300 1300 )
      + RECT via3 ( -2100 1100 ) ( -1900 1300 )
      + RECT via3 ( -1700 1100 ) ( -1500 1300 )
      + RECT via3 ( -1300 1100 ) ( -1100 1300 )
      + RECT via3 ( -900 1100 ) ( -700 1300 )
      + RECT via3 ( -500 1100 ) ( -300 1300 )
      + RECT via3 ( -100 1100 ) ( 100 1300 )
      + RECT via3 ( 300 1100 ) ( 500 1300 )
      + RECT via3 ( 700 1100 ) ( 900 1300 )
      + RECT via3 ( 1100 1100 ) ( 1300 1300 )
      + RECT via3 ( 1500 1100 ) ( 1700 1300 )
      + RECT via3 ( 1900 1100 ) ( 2100 1300 )
      + RECT via3 ( 2300 1100 ) ( 2500 1300 )
      + RECT via3 ( 2700 1100 ) ( 2900 1300 )
      + RECT via3 ( 3100 1100 ) ( 3300 1300 )
      + RECT via3 ( 3500 1100 ) ( 3700 1300 )
      + RECT via3 ( 3900 1100 ) ( 4100 1300 )
      + RECT via3 ( 4300 1100 ) ( 4500 1300 )
      + RECT via3 ( 4700 1100 ) ( 4900 1300 )
      + RECT via3 ( 5100 1100 ) ( 5300 1300 )
      + RECT via3 ( 5500 1100 ) ( 5700 1300 )
      + RECT via3 ( -5700 1500 ) ( -5500 1700 )
      + RECT via3 ( -5300 1500 ) ( -5100 1700 )
      + RECT via3 ( -4900 1500 ) ( -4700 1700 )
      + RECT via3 ( -4500 1500 ) ( -4300 1700 )
      + RECT via3 ( -4100 1500 ) ( -3900 1700 )
      + RECT via3 ( -3700 1500 ) ( -3500 1700 )
      + RECT via3 ( -3300 1500 ) ( -3100 1700 )
      + RECT via3 ( -2900 1500 ) ( -2700 1700 )
      + RECT via3 ( -2500 1500 ) ( -2300 1700 )
      + RECT via3 ( -2100 1500 ) ( -1900 1700 )
      + RECT via3 ( -1700 1500 ) ( -1500 1700 )
      + RECT via3 ( -1300 1500 ) ( -1100 1700 )
      + RECT via3 ( -900 1500 ) ( -700 1700 )
      + RECT via3 ( -500 1500 ) ( -300 1700 )
      + RECT via3 ( -100 1500 ) ( 100 1700 )
      + RECT via3 ( 300 1500 ) ( 500 1700 )
      + RECT via3 ( 700 1500 ) ( 900 1700 )
      + RECT via3 ( 1100 1500 ) ( 1300 1700 )
      + RECT via3 ( 1500 1500 ) ( 1700 1700 )
      + RECT via3 ( 1900 1500 ) ( 2100 1700 )
      + RECT via3 ( 2300 1500 ) ( 2500 1700 )
      + RECT via3 ( 2700 1500 ) ( 2900 1700 )
      + RECT via3 ( 3100 1500 ) ( 3300 1700 )
      + RECT via3 ( 3500 1500 ) ( 3700 1700 )
      + RECT via3 ( 3900 1500 ) ( 4100 1700 )
      + RECT via3 ( 4300 1500 ) ( 4500 1700 )
      + RECT via3 ( 4700 1500 ) ( 4900 1700 )
      + RECT via3 ( 5100 1500 ) ( 5300 1700 )
      + RECT via3 ( 5500 1500 ) ( 5700 1700 )
      + RECT via3 ( -5700 1900 ) ( -5500 2100 )
      + RECT via3 ( -5300 1900 ) ( -5100 2100 )
      + RECT via3 ( -4900 1900 ) ( -4700 2100 )
      + RECT via3 ( -4500 1900 ) ( -4300 2100 )
      + RECT via3 ( -4100 1900 ) ( -3900 2100 )
      + RECT via3 ( -3700 1900 ) ( -3500 2100 )
      + RECT via3 ( -3300 1900 ) ( -3100 2100 )
      + RECT via3 ( -2900 1900 ) ( -2700 2100 )
      + RECT via3 ( -2500 1900 ) ( -2300 2100 )
      + RECT via3 ( -2100 1900 ) ( -1900 2100 )
      + RECT via3 ( -1700 1900 ) ( -1500 2100 )
      + RECT via3 ( -1300 1900 ) ( -1100 2100 )
      + RECT via3 ( -900 1900 ) ( -700 2100 )
      + RECT via3 ( -500 1900 ) ( -300 2100 )
      + RECT via3 ( -100 1900 ) ( 100 2100 )
      + RECT via3 ( 300 1900 ) ( 500 2100 )
      + RECT via3 ( 700 1900 ) ( 900 2100 )
      + RECT via3 ( 1100 1900 ) ( 1300 2100 )
      + RECT via3 ( 1500 1900 ) ( 1700 2100 )
      + RECT via3 ( 1900 1900 ) ( 2100 2100 )
      + RECT via3 ( 2300 1900 ) ( 2500 2100 )
      + RECT via3 ( 2700 1900 ) ( 2900 2100 )
      + RECT via3 ( 3100 1900 ) ( 3300 2100 )
      + RECT via3 ( 3500 1900 ) ( 3700 2100 )
      + RECT via3 ( 3900 1900 ) ( 4100 2100 )
      + RECT via3 ( 4300 1900 ) ( 4500 2100 )
      + RECT via3 ( 4700 1900 ) ( 4900 2100 )
      + RECT via3 ( 5100 1900 ) ( 5300 2100 )
      + RECT via3 ( 5500 1900 ) ( 5700 2100 )
      + RECT via3 ( -5700 2300 ) ( -5500 2500 )
      + RECT via3 ( -5300 2300 ) ( -5100 2500 )
      + RECT via3 ( -4900 2300 ) ( -4700 2500 )
      + RECT via3 ( -4500 2300 ) ( -4300 2500 )
      + RECT via3 ( -4100 2300 ) ( -3900 2500 )
      + RECT via3 ( -3700 2300 ) ( -3500 2500 )
      + RECT via3 ( -3300 2300 ) ( -3100 2500 )
      + RECT via3 ( -2900 2300 ) ( -2700 2500 )
      + RECT via3 ( -2500 2300 ) ( -2300 2500 )
      + RECT via3 ( -2100 2300 ) ( -1900 2500 )
      + RECT via3 ( -1700 2300 ) ( -1500 2500 )
      + RECT via3 ( -1300 2300 ) ( -1100 2500 )
      + RECT via3 ( -900 2300 ) ( -700 2500 )
      + RECT via3 ( -500 2300 ) ( -300 2500 )
      + RECT via3 ( -100 2300 ) ( 100 2500 )
      + RECT via3 ( 300 2300 ) ( 500 2500 )
      + RECT via3 ( 700 2300 ) ( 900 2500 )
      + RECT via3 ( 1100 2300 ) ( 1300 2500 )
      + RECT via3 ( 1500 2300 ) ( 1700 2500 )
      + RECT via3 ( 1900 2300 ) ( 2100 2500 )
      + RECT via3 ( 2300 2300 ) ( 2500 2500 )
      + RECT via3 ( 2700 2300 ) ( 2900 2500 )
      + RECT via3 ( 3100 2300 ) ( 3300 2500 )
      + RECT via3 ( 3500 2300 ) ( 3700 2500 )
      + RECT via3 ( 3900 2300 ) ( 4100 2500 )
      + RECT via3 ( 4300 2300 ) ( 4500 2500 )
      + RECT via3 ( 4700 2300 ) ( 4900 2500 )
      + RECT via3 ( 5100 2300 ) ( 5300 2500 )
      + RECT via3 ( 5500 2300 ) ( 5700 2500 )
      + RECT via3 ( -5700 2700 ) ( -5500 2900 )
      + RECT via3 ( -5300 2700 ) ( -5100 2900 )
      + RECT via3 ( -4900 2700 ) ( -4700 2900 )
      + RECT via3 ( -4500 2700 ) ( -4300 2900 )
      + RECT via3 ( -4100 2700 ) ( -3900 2900 )
      + RECT via3 ( -3700 2700 ) ( -3500 2900 )
      + RECT via3 ( -3300 2700 ) ( -3100 2900 )
      + RECT via3 ( -2900 2700 ) ( -2700 2900 )
      + RECT via3 ( -2500 2700 ) ( -2300 2900 )
      + RECT via3 ( -2100 2700 ) ( -1900 2900 )
      + RECT via3 ( -1700 2700 ) ( -1500 2900 )
      + RECT via3 ( -1300 2700 ) ( -1100 2900 )
      + RECT via3 ( -900 2700 ) ( -700 2900 )
      + RECT via3 ( -500 2700 ) ( -300 2900 )
      + RECT via3 ( -100 2700 ) ( 100 2900 )
      + RECT via3 ( 300 2700 ) ( 500 2900 )
      + RECT via3 ( 700 2700 ) ( 900 2900 )
      + RECT via3 ( 1100 2700 ) ( 1300 2900 )
      + RECT via3 ( 1500 2700 ) ( 1700 2900 )
      + RECT via3 ( 1900 2700 ) ( 2100 2900 )
      + RECT via3 ( 2300 2700 ) ( 2500 2900 )
      + RECT via3 ( 2700 2700 ) ( 2900 2900 )
      + RECT via3 ( 3100 2700 ) ( 3300 2900 )
      + RECT via3 ( 3500 2700 ) ( 3700 2900 )
      + RECT via3 ( 3900 2700 ) ( 4100 2900 )
      + RECT via3 ( 4300 2700 ) ( 4500 2900 )
      + RECT via3 ( 4700 2700 ) ( 4900 2900 )
      + RECT via3 ( 5100 2700 ) ( 5300 2900 )
      + RECT via3 ( 5500 2700 ) ( 5700 2900 )
      + RECT via3 ( -5700 3100 ) ( -5500 3300 )
      + RECT via3 ( -5300 3100 ) ( -5100 3300 )
      + RECT via3 ( -4900 3100 ) ( -4700 3300 )
      + RECT via3 ( -4500 3100 ) ( -4300 3300 )
      + RECT via3 ( -4100 3100 ) ( -3900 3300 )
      + RECT via3 ( -3700 3100 ) ( -3500 3300 )
      + RECT via3 ( -3300 3100 ) ( -3100 3300 )
      + RECT via3 ( -2900 3100 ) ( -2700 3300 )
      + RECT via3 ( -2500 3100 ) ( -2300 3300 )
      + RECT via3 ( -2100 3100 ) ( -1900 3300 )
      + RECT via3 ( -1700 3100 ) ( -1500 3300 )
      + RECT via3 ( -1300 3100 ) ( -1100 3300 )
      + RECT via3 ( -900 3100 ) ( -700 3300 )
      + RECT via3 ( -500 3100 ) ( -300 3300 )
      + RECT via3 ( -100 3100 ) ( 100 3300 )
      + RECT via3 ( 300 3100 ) ( 500 3300 )
      + RECT via3 ( 700 3100 ) ( 900 3300 )
      + RECT via3 ( 1100 3100 ) ( 1300 3300 )
      + RECT via3 ( 1500 3100 ) ( 1700 3300 )
      + RECT via3 ( 1900 3100 ) ( 2100 3300 )
      + RECT via3 ( 2300 3100 ) ( 2500 3300 )
      + RECT via3 ( 2700 3100 ) ( 2900 3300 )
      + RECT via3 ( 3100 3100 ) ( 3300 3300 )
      + RECT via3 ( 3500 3100 ) ( 3700 3300 )
      + RECT via3 ( 3900 3100 ) ( 4100 3300 )
      + RECT via3 ( 4300 3100 ) ( 4500 3300 )
      + RECT via3 ( 4700 3100 ) ( 4900 3300 )
      + RECT via3 ( 5100 3100 ) ( 5300 3300 )
      + RECT via3 ( 5500 3100 ) ( 5700 3300 )
      + RECT via3 ( -5700 3500 ) ( -5500 3700 )
      + RECT via3 ( -5300 3500 ) ( -5100 3700 )
      + RECT via3 ( -4900 3500 ) ( -4700 3700 )
      + RECT via3 ( -4500 3500 ) ( -4300 3700 )
      + RECT via3 ( -4100 3500 ) ( -3900 3700 )
      + RECT via3 ( -3700 3500 ) ( -3500 3700 )
      + RECT via3 ( -3300 3500 ) ( -3100 3700 )
      + RECT via3 ( -2900 3500 ) ( -2700 3700 )
      + RECT via3 ( -2500 3500 ) ( -2300 3700 )
      + RECT via3 ( -2100 3500 ) ( -1900 3700 )
      + RECT via3 ( -1700 3500 ) ( -1500 3700 )
      + RECT via3 ( -1300 3500 ) ( -1100 3700 )
      + RECT via3 ( -900 3500 ) ( -700 3700 )
      + RECT via3 ( -500 3500 ) ( -300 3700 )
      + RECT via3 ( -100 3500 ) ( 100 3700 )
      + RECT via3 ( 300 3500 ) ( 500 3700 )
      + RECT via3 ( 700 3500 ) ( 900 3700 )
      + RECT via3 ( 1100 3500 ) ( 1300 3700 )
      + RECT via3 ( 1500 3500 ) ( 1700 3700 )
      + RECT via3 ( 1900 3500 ) ( 2100 3700 )
      + RECT via3 ( 2300 3500 ) ( 2500 3700 )
      + RECT via3 ( 2700 3500 ) ( 2900 3700 )
      + RECT via3 ( 3100 3500 ) ( 3300 3700 )
      + RECT via3 ( 3500 3500 ) ( 3700 3700 )
      + RECT via3 ( 3900 3500 ) ( 4100 3700 )
      + RECT via3 ( 4300 3500 ) ( 4500 3700 )
      + RECT via3 ( 4700 3500 ) ( 4900 3700 )
      + RECT via3 ( 5100 3500 ) ( 5300 3700 )
      + RECT via3 ( 5500 3500 ) ( 5700 3700 )
      + RECT via3 ( -5700 3900 ) ( -5500 4100 )
      + RECT via3 ( -5300 3900 ) ( -5100 4100 )
      + RECT via3 ( -4900 3900 ) ( -4700 4100 )
      + RECT via3 ( -4500 3900 ) ( -4300 4100 )
      + RECT via3 ( -4100 3900 ) ( -3900 4100 )
      + RECT via3 ( -3700 3900 ) ( -3500 4100 )
      + RECT via3 ( -3300 3900 ) ( -3100 4100 )
      + RECT via3 ( -2900 3900 ) ( -2700 4100 )
      + RECT via3 ( -2500 3900 ) ( -2300 4100 )
      + RECT via3 ( -2100 3900 ) ( -1900 4100 )
      + RECT via3 ( -1700 3900 ) ( -1500 4100 )
      + RECT via3 ( -1300 3900 ) ( -1100 4100 )
      + RECT via3 ( -900 3900 ) ( -700 4100 )
      + RECT via3 ( -500 3900 ) ( -300 4100 )
      + RECT via3 ( -100 3900 ) ( 100 4100 )
      + RECT via3 ( 300 3900 ) ( 500 4100 )
      + RECT via3 ( 700 3900 ) ( 900 4100 )
      + RECT via3 ( 1100 3900 ) ( 1300 4100 )
      + RECT via3 ( 1500 3900 ) ( 1700 4100 )
      + RECT via3 ( 1900 3900 ) ( 2100 4100 )
      + RECT via3 ( 2300 3900 ) ( 2500 4100 )
      + RECT via3 ( 2700 3900 ) ( 2900 4100 )
      + RECT via3 ( 3100 3900 ) ( 3300 4100 )
      + RECT via3 ( 3500 3900 ) ( 3700 4100 )
      + RECT via3 ( 3900 3900 ) ( 4100 4100 )
      + RECT via3 ( 4300 3900 ) ( 4500 4100 )
      + RECT via3 ( 4700 3900 ) ( 4900 4100 )
      + RECT via3 ( 5100 3900 ) ( 5300 4100 )
      + RECT via3 ( 5500 3900 ) ( 5700 4100 )
      + RECT via3 ( -5700 4300 ) ( -5500 4500 )
      + RECT via3 ( -5300 4300 ) ( -5100 4500 )
      + RECT via3 ( -4900 4300 ) ( -4700 4500 )
      + RECT via3 ( -4500 4300 ) ( -4300 4500 )
      + RECT via3 ( -4100 4300 ) ( -3900 4500 )
      + RECT via3 ( -3700 4300 ) ( -3500 4500 )
      + RECT via3 ( -3300 4300 ) ( -3100 4500 )
      + RECT via3 ( -2900 4300 ) ( -2700 4500 )
      + RECT via3 ( -2500 4300 ) ( -2300 4500 )
      + RECT via3 ( -2100 4300 ) ( -1900 4500 )
      + RECT via3 ( -1700 4300 ) ( -1500 4500 )
      + RECT via3 ( -1300 4300 ) ( -1100 4500 )
      + RECT via3 ( -900 4300 ) ( -700 4500 )
      + RECT via3 ( -500 4300 ) ( -300 4500 )
      + RECT via3 ( -100 4300 ) ( 100 4500 )
      + RECT via3 ( 300 4300 ) ( 500 4500 )
      + RECT via3 ( 700 4300 ) ( 900 4500 )
      + RECT via3 ( 1100 4300 ) ( 1300 4500 )
      + RECT via3 ( 1500 4300 ) ( 1700 4500 )
      + RECT via3 ( 1900 4300 ) ( 2100 4500 )
      + RECT via3 ( 2300 4300 ) ( 2500 4500 )
      + RECT via3 ( 2700 4300 ) ( 2900 4500 )
      + RECT via3 ( 3100 4300 ) ( 3300 4500 )
      + RECT via3 ( 3500 4300 ) ( 3700 4500 )
      + RECT via3 ( 3900 4300 ) ( 4100 4500 )
      + RECT via3 ( 4300 4300 ) ( 4500 4500 )
      + RECT via3 ( 4700 4300 ) ( 4900 4500 )
      + RECT via3 ( 5100 4300 ) ( 5300 4500 )
      + RECT via3 ( 5500 4300 ) ( 5700 4500 )
      + RECT via3 ( -5700 4700 ) ( -5500 4900 )
      + RECT via3 ( -5300 4700 ) ( -5100 4900 )
      + RECT via3 ( -4900 4700 ) ( -4700 4900 )
      + RECT via3 ( -4500 4700 ) ( -4300 4900 )
      + RECT via3 ( -4100 4700 ) ( -3900 4900 )
      + RECT via3 ( -3700 4700 ) ( -3500 4900 )
      + RECT via3 ( -3300 4700 ) ( -3100 4900 )
      + RECT via3 ( -2900 4700 ) ( -2700 4900 )
      + RECT via3 ( -2500 4700 ) ( -2300 4900 )
      + RECT via3 ( -2100 4700 ) ( -1900 4900 )
      + RECT via3 ( -1700 4700 ) ( -1500 4900 )
      + RECT via3 ( -1300 4700 ) ( -1100 4900 )
      + RECT via3 ( -900 4700 ) ( -700 4900 )
      + RECT via3 ( -500 4700 ) ( -300 4900 )
      + RECT via3 ( -100 4700 ) ( 100 4900 )
      + RECT via3 ( 300 4700 ) ( 500 4900 )
      + RECT via3 ( 700 4700 ) ( 900 4900 )
      + RECT via3 ( 1100 4700 ) ( 1300 4900 )
      + RECT via3 ( 1500 4700 ) ( 1700 4900 )
      + RECT via3 ( 1900 4700 ) ( 2100 4900 )
      + RECT via3 ( 2300 4700 ) ( 2500 4900 )
      + RECT via3 ( 2700 4700 ) ( 2900 4900 )
      + RECT via3 ( 3100 4700 ) ( 3300 4900 )
      + RECT via3 ( 3500 4700 ) ( 3700 4900 )
      + RECT via3 ( 3900 4700 ) ( 4100 4900 )
      + RECT via3 ( 4300 4700 ) ( 4500 4900 )
      + RECT via3 ( 4700 4700 ) ( 4900 4900 )
      + RECT via3 ( 5100 4700 ) ( 5300 4900 )
      + RECT via3 ( 5500 4700 ) ( 5700 4900 )
      + RECT via3 ( -5700 5100 ) ( -5500 5300 )
      + RECT via3 ( -5300 5100 ) ( -5100 5300 )
      + RECT via3 ( -4900 5100 ) ( -4700 5300 )
      + RECT via3 ( -4500 5100 ) ( -4300 5300 )
      + RECT via3 ( -4100 5100 ) ( -3900 5300 )
      + RECT via3 ( -3700 5100 ) ( -3500 5300 )
      + RECT via3 ( -3300 5100 ) ( -3100 5300 )
      + RECT via3 ( -2900 5100 ) ( -2700 5300 )
      + RECT via3 ( -2500 5100 ) ( -2300 5300 )
      + RECT via3 ( -2100 5100 ) ( -1900 5300 )
      + RECT via3 ( -1700 5100 ) ( -1500 5300 )
      + RECT via3 ( -1300 5100 ) ( -1100 5300 )
      + RECT via3 ( -900 5100 ) ( -700 5300 )
      + RECT via3 ( -500 5100 ) ( -300 5300 )
      + RECT via3 ( -100 5100 ) ( 100 5300 )
      + RECT via3 ( 300 5100 ) ( 500 5300 )
      + RECT via3 ( 700 5100 ) ( 900 5300 )
      + RECT via3 ( 1100 5100 ) ( 1300 5300 )
      + RECT via3 ( 1500 5100 ) ( 1700 5300 )
      + RECT via3 ( 1900 5100 ) ( 2100 5300 )
      + RECT via3 ( 2300 5100 ) ( 2500 5300 )
      + RECT via3 ( 2700 5100 ) ( 2900 5300 )
      + RECT via3 ( 3100 5100 ) ( 3300 5300 )
      + RECT via3 ( 3500 5100 ) ( 3700 5300 )
      + RECT via3 ( 3900 5100 ) ( 4100 5300 )
      + RECT via3 ( 4300 5100 ) ( 4500 5300 )
      + RECT via3 ( 4700 5100 ) ( 4900 5300 )
      + RECT via3 ( 5100 5100 ) ( 5300 5300 )
      + RECT via3 ( 5500 5100 ) ( 5700 5300 )
      + RECT via3 ( -5700 5500 ) ( -5500 5700 )
      + RECT via3 ( -5300 5500 ) ( -5100 5700 )
      + RECT via3 ( -4900 5500 ) ( -4700 5700 )
      + RECT via3 ( -4500 5500 ) ( -4300 5700 )
      + RECT via3 ( -4100 5500 ) ( -3900 5700 )
      + RECT via3 ( -3700 5500 ) ( -3500 5700 )
      + RECT via3 ( -3300 5500 ) ( -3100 5700 )
      + RECT via3 ( -2900 5500 ) ( -2700 5700 )
      + RECT via3 ( -2500 5500 ) ( -2300 5700 )
      + RECT via3 ( -2100 5500 ) ( -1900 5700 )
      + RECT via3 ( -1700 5500 ) ( -1500 5700 )
      + RECT via3 ( -1300 5500 ) ( -1100 5700 )
      + RECT via3 ( -900 5500 ) ( -700 5700 )
      + RECT via3 ( -500 5500 ) ( -300 5700 )
      + RECT via3 ( -100 5500 ) ( 100 5700 )
      + RECT via3 ( 300 5500 ) ( 500 5700 )
      + RECT via3 ( 700 5500 ) ( 900 5700 )
      + RECT via3 ( 1100 5500 ) ( 1300 5700 )
      + RECT via3 ( 1500 5500 ) ( 1700 5700 )
      + RECT via3 ( 1900 5500 ) ( 2100 5700 )
      + RECT via3 ( 2300 5500 ) ( 2500 5700 )
      + RECT via3 ( 2700 5500 ) ( 2900 5700 )
      + RECT via3 ( 3100 5500 ) ( 3300 5700 )
      + RECT via3 ( 3500 5500 ) ( 3700 5700 )
      + RECT via3 ( 3900 5500 ) ( 4100 5700 )
      + RECT via3 ( 4300 5500 ) ( 4500 5700 )
      + RECT via3 ( 4700 5500 ) ( 4900 5700 )
      + RECT via3 ( 5100 5500 ) ( 5300 5700 )
      + RECT via3 ( 5500 5500 ) ( 5700 5700 )
      + RECT via3 ( -5700 5900 ) ( -5500 6100 )
      + RECT via3 ( -5300 5900 ) ( -5100 6100 )
      + RECT via3 ( -4900 5900 ) ( -4700 6100 )
      + RECT via3 ( -4500 5900 ) ( -4300 6100 )
      + RECT via3 ( -4100 5900 ) ( -3900 6100 )
      + RECT via3 ( -3700 5900 ) ( -3500 6100 )
      + RECT via3 ( -3300 5900 ) ( -3100 6100 )
      + RECT via3 ( -2900 5900 ) ( -2700 6100 )
      + RECT via3 ( -2500 5900 ) ( -2300 6100 )
      + RECT via3 ( -2100 5900 ) ( -1900 6100 )
      + RECT via3 ( -1700 5900 ) ( -1500 6100 )
      + RECT via3 ( -1300 5900 ) ( -1100 6100 )
      + RECT via3 ( -900 5900 ) ( -700 6100 )
      + RECT via3 ( -500 5900 ) ( -300 6100 )
      + RECT via3 ( -100 5900 ) ( 100 6100 )
      + RECT via3 ( 300 5900 ) ( 500 6100 )
      + RECT via3 ( 700 5900 ) ( 900 6100 )
      + RECT via3 ( 1100 5900 ) ( 1300 6100 )
      + RECT via3 ( 1500 5900 ) ( 1700 6100 )
      + RECT via3 ( 1900 5900 ) ( 2100 6100 )
      + RECT via3 ( 2300 5900 ) ( 2500 6100 )
      + RECT via3 ( 2700 5900 ) ( 2900 6100 )
      + RECT via3 ( 3100 5900 ) ( 3300 6100 )
      + RECT via3 ( 3500 5900 ) ( 3700 6100 )
      + RECT via3 ( 3900 5900 ) ( 4100 6100 )
      + RECT via3 ( 4300 5900 ) ( 4500 6100 )
      + RECT via3 ( 4700 5900 ) ( 4900 6100 )
      + RECT via3 ( 5100 5900 ) ( 5300 6100 )
      + RECT via3 ( 5500 5900 ) ( 5700 6100 )
      + RECT via3 ( -5700 6300 ) ( -5500 6500 )
      + RECT via3 ( -5300 6300 ) ( -5100 6500 )
      + RECT via3 ( -4900 6300 ) ( -4700 6500 )
      + RECT via3 ( -4500 6300 ) ( -4300 6500 )
      + RECT via3 ( -4100 6300 ) ( -3900 6500 )
      + RECT via3 ( -3700 6300 ) ( -3500 6500 )
      + RECT via3 ( -3300 6300 ) ( -3100 6500 )
      + RECT via3 ( -2900 6300 ) ( -2700 6500 )
      + RECT via3 ( -2500 6300 ) ( -2300 6500 )
      + RECT via3 ( -2100 6300 ) ( -1900 6500 )
      + RECT via3 ( -1700 6300 ) ( -1500 6500 )
      + RECT via3 ( -1300 6300 ) ( -1100 6500 )
      + RECT via3 ( -900 6300 ) ( -700 6500 )
      + RECT via3 ( -500 6300 ) ( -300 6500 )
      + RECT via3 ( -100 6300 ) ( 100 6500 )
      + RECT via3 ( 300 6300 ) ( 500 6500 )
      + RECT via3 ( 700 6300 ) ( 900 6500 )
      + RECT via3 ( 1100 6300 ) ( 1300 6500 )
      + RECT via3 ( 1500 6300 ) ( 1700 6500 )
      + RECT via3 ( 1900 6300 ) ( 2100 6500 )
      + RECT via3 ( 2300 6300 ) ( 2500 6500 )
      + RECT via3 ( 2700 6300 ) ( 2900 6500 )
      + RECT via3 ( 3100 6300 ) ( 3300 6500 )
      + RECT via3 ( 3500 6300 ) ( 3700 6500 )
      + RECT via3 ( 3900 6300 ) ( 4100 6500 )
      + RECT via3 ( 4300 6300 ) ( 4500 6500 )
      + RECT via3 ( 4700 6300 ) ( 4900 6500 )
      + RECT via3 ( 5100 6300 ) ( 5300 6500 )
      + RECT via3 ( 5500 6300 ) ( 5700 6500 )
      + RECT via3 ( -5700 6700 ) ( -5500 6900 )
      + RECT via3 ( -5300 6700 ) ( -5100 6900 )
      + RECT via3 ( -4900 6700 ) ( -4700 6900 )
      + RECT via3 ( -4500 6700 ) ( -4300 6900 )
      + RECT via3 ( -4100 6700 ) ( -3900 6900 )
      + RECT via3 ( -3700 6700 ) ( -3500 6900 )
      + RECT via3 ( -3300 6700 ) ( -3100 6900 )
      + RECT via3 ( -2900 6700 ) ( -2700 6900 )
      + RECT via3 ( -2500 6700 ) ( -2300 6900 )
      + RECT via3 ( -2100 6700 ) ( -1900 6900 )
      + RECT via3 ( -1700 6700 ) ( -1500 6900 )
      + RECT via3 ( -1300 6700 ) ( -1100 6900 )
      + RECT via3 ( -900 6700 ) ( -700 6900 )
      + RECT via3 ( -500 6700 ) ( -300 6900 )
      + RECT via3 ( -100 6700 ) ( 100 6900 )
      + RECT via3 ( 300 6700 ) ( 500 6900 )
      + RECT via3 ( 700 6700 ) ( 900 6900 )
      + RECT via3 ( 1100 6700 ) ( 1300 6900 )
      + RECT via3 ( 1500 6700 ) ( 1700 6900 )
      + RECT via3 ( 1900 6700 ) ( 2100 6900 )
      + RECT via3 ( 2300 6700 ) ( 2500 6900 )
      + RECT via3 ( 2700 6700 ) ( 2900 6900 )
      + RECT via3 ( 3100 6700 ) ( 3300 6900 )
      + RECT via3 ( 3500 6700 ) ( 3700 6900 )
      + RECT via3 ( 3900 6700 ) ( 4100 6900 )
      + RECT via3 ( 4300 6700 ) ( 4500 6900 )
      + RECT via3 ( 4700 6700 ) ( 4900 6900 )
      + RECT via3 ( 5100 6700 ) ( 5300 6900 )
      + RECT via3 ( 5500 6700 ) ( 5700 6900 )
      + RECT via3 ( -5700 7100 ) ( -5500 7300 )
      + RECT via3 ( -5300 7100 ) ( -5100 7300 )
      + RECT via3 ( -4900 7100 ) ( -4700 7300 )
      + RECT via3 ( -4500 7100 ) ( -4300 7300 )
      + RECT via3 ( -4100 7100 ) ( -3900 7300 )
      + RECT via3 ( -3700 7100 ) ( -3500 7300 )
      + RECT via3 ( -3300 7100 ) ( -3100 7300 )
      + RECT via3 ( -2900 7100 ) ( -2700 7300 )
      + RECT via3 ( -2500 7100 ) ( -2300 7300 )
      + RECT via3 ( -2100 7100 ) ( -1900 7300 )
      + RECT via3 ( -1700 7100 ) ( -1500 7300 )
      + RECT via3 ( -1300 7100 ) ( -1100 7300 )
      + RECT via3 ( -900 7100 ) ( -700 7300 )
      + RECT via3 ( -500 7100 ) ( -300 7300 )
      + RECT via3 ( -100 7100 ) ( 100 7300 )
      + RECT via3 ( 300 7100 ) ( 500 7300 )
      + RECT via3 ( 700 7100 ) ( 900 7300 )
      + RECT via3 ( 1100 7100 ) ( 1300 7300 )
      + RECT via3 ( 1500 7100 ) ( 1700 7300 )
      + RECT via3 ( 1900 7100 ) ( 2100 7300 )
      + RECT via3 ( 2300 7100 ) ( 2500 7300 )
      + RECT via3 ( 2700 7100 ) ( 2900 7300 )
      + RECT via3 ( 3100 7100 ) ( 3300 7300 )
      + RECT via3 ( 3500 7100 ) ( 3700 7300 )
      + RECT via3 ( 3900 7100 ) ( 4100 7300 )
      + RECT via3 ( 4300 7100 ) ( 4500 7300 )
      + RECT via3 ( 4700 7100 ) ( 4900 7300 )
      + RECT via3 ( 5100 7100 ) ( 5300 7300 )
      + RECT via3 ( 5500 7100 ) ( 5700 7300 )
      + RECT via3 ( -5700 7500 ) ( -5500 7700 )
      + RECT via3 ( -5300 7500 ) ( -5100 7700 )
      + RECT via3 ( -4900 7500 ) ( -4700 7700 )
      + RECT via3 ( -4500 7500 ) ( -4300 7700 )
      + RECT via3 ( -4100 7500 ) ( -3900 7700 )
      + RECT via3 ( -3700 7500 ) ( -3500 7700 )
      + RECT via3 ( -3300 7500 ) ( -3100 7700 )
      + RECT via3 ( -2900 7500 ) ( -2700 7700 )
      + RECT via3 ( -2500 7500 ) ( -2300 7700 )
      + RECT via3 ( -2100 7500 ) ( -1900 7700 )
      + RECT via3 ( -1700 7500 ) ( -1500 7700 )
      + RECT via3 ( -1300 7500 ) ( -1100 7700 )
      + RECT via3 ( -900 7500 ) ( -700 7700 )
      + RECT via3 ( -500 7500 ) ( -300 7700 )
      + RECT via3 ( -100 7500 ) ( 100 7700 )
      + RECT via3 ( 300 7500 ) ( 500 7700 )
      + RECT via3 ( 700 7500 ) ( 900 7700 )
      + RECT via3 ( 1100 7500 ) ( 1300 7700 )
      + RECT via3 ( 1500 7500 ) ( 1700 7700 )
      + RECT via3 ( 1900 7500 ) ( 2100 7700 )
      + RECT via3 ( 2300 7500 ) ( 2500 7700 )
      + RECT via3 ( 2700 7500 ) ( 2900 7700 )
      + RECT via3 ( 3100 7500 ) ( 3300 7700 )
      + RECT via3 ( 3500 7500 ) ( 3700 7700 )
      + RECT via3 ( 3900 7500 ) ( 4100 7700 )
      + RECT via3 ( 4300 7500 ) ( 4500 7700 )
      + RECT via3 ( 4700 7500 ) ( 4900 7700 )
      + RECT via3 ( 5100 7500 ) ( 5300 7700 )
      + RECT via3 ( 5500 7500 ) ( 5700 7700 )
      + RECT via3 ( -5700 7900 ) ( -5500 8100 )
      + RECT via3 ( -5300 7900 ) ( -5100 8100 )
      + RECT via3 ( -4900 7900 ) ( -4700 8100 )
      + RECT via3 ( -4500 7900 ) ( -4300 8100 )
      + RECT via3 ( -4100 7900 ) ( -3900 8100 )
      + RECT via3 ( -3700 7900 ) ( -3500 8100 )
      + RECT via3 ( -3300 7900 ) ( -3100 8100 )
      + RECT via3 ( -2900 7900 ) ( -2700 8100 )
      + RECT via3 ( -2500 7900 ) ( -2300 8100 )
      + RECT via3 ( -2100 7900 ) ( -1900 8100 )
      + RECT via3 ( -1700 7900 ) ( -1500 8100 )
      + RECT via3 ( -1300 7900 ) ( -1100 8100 )
      + RECT via3 ( -900 7900 ) ( -700 8100 )
      + RECT via3 ( -500 7900 ) ( -300 8100 )
      + RECT via3 ( -100 7900 ) ( 100 8100 )
      + RECT via3 ( 300 7900 ) ( 500 8100 )
      + RECT via3 ( 700 7900 ) ( 900 8100 )
      + RECT via3 ( 1100 7900 ) ( 1300 8100 )
      + RECT via3 ( 1500 7900 ) ( 1700 8100 )
      + RECT via3 ( 1900 7900 ) ( 2100 8100 )
      + RECT via3 ( 2300 7900 ) ( 2500 8100 )
      + RECT via3 ( 2700 7900 ) ( 2900 8100 )
      + RECT via3 ( 3100 7900 ) ( 3300 8100 )
      + RECT via3 ( 3500 7900 ) ( 3700 8100 )
      + RECT via3 ( 3900 7900 ) ( 4100 8100 )
      + RECT via3 ( 4300 7900 ) ( 4500 8100 )
      + RECT via3 ( 4700 7900 ) ( 4900 8100 )
      + RECT via3 ( 5100 7900 ) ( 5300 8100 )
      + RECT via3 ( 5500 7900 ) ( 5700 8100 )
      + RECT via3 ( -5700 8300 ) ( -5500 8500 )
      + RECT via3 ( -5300 8300 ) ( -5100 8500 )
      + RECT via3 ( -4900 8300 ) ( -4700 8500 )
      + RECT via3 ( -4500 8300 ) ( -4300 8500 )
      + RECT via3 ( -4100 8300 ) ( -3900 8500 )
      + RECT via3 ( -3700 8300 ) ( -3500 8500 )
      + RECT via3 ( -3300 8300 ) ( -3100 8500 )
      + RECT via3 ( -2900 8300 ) ( -2700 8500 )
      + RECT via3 ( -2500 8300 ) ( -2300 8500 )
      + RECT via3 ( -2100 8300 ) ( -1900 8500 )
      + RECT via3 ( -1700 8300 ) ( -1500 8500 )
      + RECT via3 ( -1300 8300 ) ( -1100 8500 )
      + RECT via3 ( -900 8300 ) ( -700 8500 )
      + RECT via3 ( -500 8300 ) ( -300 8500 )
      + RECT via3 ( -100 8300 ) ( 100 8500 )
      + RECT via3 ( 300 8300 ) ( 500 8500 )
      + RECT via3 ( 700 8300 ) ( 900 8500 )
      + RECT via3 ( 1100 8300 ) ( 1300 8500 )
      + RECT via3 ( 1500 8300 ) ( 1700 8500 )
      + RECT via3 ( 1900 8300 ) ( 2100 8500 )
      + RECT via3 ( 2300 8300 ) ( 2500 8500 )
      + RECT via3 ( 2700 8300 ) ( 2900 8500 )
      + RECT via3 ( 3100 8300 ) ( 3300 8500 )
      + RECT via3 ( 3500 8300 ) ( 3700 8500 )
      + RECT via3 ( 3900 8300 ) ( 4100 8500 )
      + RECT via3 ( 4300 8300 ) ( 4500 8500 )
      + RECT via3 ( 4700 8300 ) ( 4900 8500 )
      + RECT via3 ( 5100 8300 ) ( 5300 8500 )
      + RECT via3 ( 5500 8300 ) ( 5700 8500 )
      + RECT via3 ( -5700 8700 ) ( -5500 8900 )
      + RECT via3 ( -5300 8700 ) ( -5100 8900 )
      + RECT via3 ( -4900 8700 ) ( -4700 8900 )
      + RECT via3 ( -4500 8700 ) ( -4300 8900 )
      + RECT via3 ( -4100 8700 ) ( -3900 8900 )
      + RECT via3 ( -3700 8700 ) ( -3500 8900 )
      + RECT via3 ( -3300 8700 ) ( -3100 8900 )
      + RECT via3 ( -2900 8700 ) ( -2700 8900 )
      + RECT via3 ( -2500 8700 ) ( -2300 8900 )
      + RECT via3 ( -2100 8700 ) ( -1900 8900 )
      + RECT via3 ( -1700 8700 ) ( -1500 8900 )
      + RECT via3 ( -1300 8700 ) ( -1100 8900 )
      + RECT via3 ( -900 8700 ) ( -700 8900 )
      + RECT via3 ( -500 8700 ) ( -300 8900 )
      + RECT via3 ( -100 8700 ) ( 100 8900 )
      + RECT via3 ( 300 8700 ) ( 500 8900 )
      + RECT via3 ( 700 8700 ) ( 900 8900 )
      + RECT via3 ( 1100 8700 ) ( 1300 8900 )
      + RECT via3 ( 1500 8700 ) ( 1700 8900 )
      + RECT via3 ( 1900 8700 ) ( 2100 8900 )
      + RECT via3 ( 2300 8700 ) ( 2500 8900 )
      + RECT via3 ( 2700 8700 ) ( 2900 8900 )
      + RECT via3 ( 3100 8700 ) ( 3300 8900 )
      + RECT via3 ( 3500 8700 ) ( 3700 8900 )
      + RECT via3 ( 3900 8700 ) ( 4100 8900 )
      + RECT via3 ( 4300 8700 ) ( 4500 8900 )
      + RECT via3 ( 4700 8700 ) ( 4900 8900 )
      + RECT via3 ( 5100 8700 ) ( 5300 8900 )
      + RECT via3 ( 5500 8700 ) ( 5700 8900 )
      + RECT via3 ( -5700 9100 ) ( -5500 9300 )
      + RECT via3 ( -5300 9100 ) ( -5100 9300 )
      + RECT via3 ( -4900 9100 ) ( -4700 9300 )
      + RECT via3 ( -4500 9100 ) ( -4300 9300 )
      + RECT via3 ( -4100 9100 ) ( -3900 9300 )
      + RECT via3 ( -3700 9100 ) ( -3500 9300 )
      + RECT via3 ( -3300 9100 ) ( -3100 9300 )
      + RECT via3 ( -2900 9100 ) ( -2700 9300 )
      + RECT via3 ( -2500 9100 ) ( -2300 9300 )
      + RECT via3 ( -2100 9100 ) ( -1900 9300 )
      + RECT via3 ( -1700 9100 ) ( -1500 9300 )
      + RECT via3 ( -1300 9100 ) ( -1100 9300 )
      + RECT via3 ( -900 9100 ) ( -700 9300 )
      + RECT via3 ( -500 9100 ) ( -300 9300 )
      + RECT via3 ( -100 9100 ) ( 100 9300 )
      + RECT via3 ( 300 9100 ) ( 500 9300 )
      + RECT via3 ( 700 9100 ) ( 900 9300 )
      + RECT via3 ( 1100 9100 ) ( 1300 9300 )
      + RECT via3 ( 1500 9100 ) ( 1700 9300 )
      + RECT via3 ( 1900 9100 ) ( 2100 9300 )
      + RECT via3 ( 2300 9100 ) ( 2500 9300 )
      + RECT via3 ( 2700 9100 ) ( 2900 9300 )
      + RECT via3 ( 3100 9100 ) ( 3300 9300 )
      + RECT via3 ( 3500 9100 ) ( 3700 9300 )
      + RECT via3 ( 3900 9100 ) ( 4100 9300 )
      + RECT via3 ( 4300 9100 ) ( 4500 9300 )
      + RECT via3 ( 4700 9100 ) ( 4900 9300 )
      + RECT via3 ( 5100 9100 ) ( 5300 9300 )
      + RECT via3 ( 5500 9100 ) ( 5700 9300 )
      + RECT via3 ( -5700 9500 ) ( -5500 9700 )
      + RECT via3 ( -5300 9500 ) ( -5100 9700 )
      + RECT via3 ( -4900 9500 ) ( -4700 9700 )
      + RECT via3 ( -4500 9500 ) ( -4300 9700 )
      + RECT via3 ( -4100 9500 ) ( -3900 9700 )
      + RECT via3 ( -3700 9500 ) ( -3500 9700 )
      + RECT via3 ( -3300 9500 ) ( -3100 9700 )
      + RECT via3 ( -2900 9500 ) ( -2700 9700 )
      + RECT via3 ( -2500 9500 ) ( -2300 9700 )
      + RECT via3 ( -2100 9500 ) ( -1900 9700 )
      + RECT via3 ( -1700 9500 ) ( -1500 9700 )
      + RECT via3 ( -1300 9500 ) ( -1100 9700 )
      + RECT via3 ( -900 9500 ) ( -700 9700 )
      + RECT via3 ( -500 9500 ) ( -300 9700 )
      + RECT via3 ( -100 9500 ) ( 100 9700 )
      + RECT via3 ( 300 9500 ) ( 500 9700 )
      + RECT via3 ( 700 9500 ) ( 900 9700 )
      + RECT via3 ( 1100 9500 ) ( 1300 9700 )
      + RECT via3 ( 1500 9500 ) ( 1700 9700 )
      + RECT via3 ( 1900 9500 ) ( 2100 9700 )
      + RECT via3 ( 2300 9500 ) ( 2500 9700 )
      + RECT via3 ( 2700 9500 ) ( 2900 9700 )
      + RECT via3 ( 3100 9500 ) ( 3300 9700 )
      + RECT via3 ( 3500 9500 ) ( 3700 9700 )
      + RECT via3 ( 3900 9500 ) ( 4100 9700 )
      + RECT via3 ( 4300 9500 ) ( 4500 9700 )
      + RECT via3 ( 4700 9500 ) ( 4900 9700 )
      + RECT via3 ( 5100 9500 ) ( 5300 9700 )
      + RECT via3 ( 5500 9500 ) ( 5700 9700 )
      + RECT via3 ( -5700 9900 ) ( -5500 10100 )
      + RECT via3 ( -5300 9900 ) ( -5100 10100 )
      + RECT via3 ( -4900 9900 ) ( -4700 10100 )
      + RECT via3 ( -4500 9900 ) ( -4300 10100 )
      + RECT via3 ( -4100 9900 ) ( -3900 10100 )
      + RECT via3 ( -3700 9900 ) ( -3500 10100 )
      + RECT via3 ( -3300 9900 ) ( -3100 10100 )
      + RECT via3 ( -2900 9900 ) ( -2700 10100 )
      + RECT via3 ( -2500 9900 ) ( -2300 10100 )
      + RECT via3 ( -2100 9900 ) ( -1900 10100 )
      + RECT via3 ( -1700 9900 ) ( -1500 10100 )
      + RECT via3 ( -1300 9900 ) ( -1100 10100 )
      + RECT via3 ( -900 9900 ) ( -700 10100 )
      + RECT via3 ( -500 9900 ) ( -300 10100 )
      + RECT via3 ( -100 9900 ) ( 100 10100 )
      + RECT via3 ( 300 9900 ) ( 500 10100 )
      + RECT via3 ( 700 9900 ) ( 900 10100 )
      + RECT via3 ( 1100 9900 ) ( 1300 10100 )
      + RECT via3 ( 1500 9900 ) ( 1700 10100 )
      + RECT via3 ( 1900 9900 ) ( 2100 10100 )
      + RECT via3 ( 2300 9900 ) ( 2500 10100 )
      + RECT via3 ( 2700 9900 ) ( 2900 10100 )
      + RECT via3 ( 3100 9900 ) ( 3300 10100 )
      + RECT via3 ( 3500 9900 ) ( 3700 10100 )
      + RECT via3 ( 3900 9900 ) ( 4100 10100 )
      + RECT via3 ( 4300 9900 ) ( 4500 10100 )
      + RECT via3 ( 4700 9900 ) ( 4900 10100 )
      + RECT via3 ( 5100 9900 ) ( 5300 10100 )
      + RECT via3 ( 5500 9900 ) ( 5700 10100 )
      + RECT via3 ( -5700 10300 ) ( -5500 10500 )
      + RECT via3 ( -5300 10300 ) ( -5100 10500 )
      + RECT via3 ( -4900 10300 ) ( -4700 10500 )
      + RECT via3 ( -4500 10300 ) ( -4300 10500 )
      + RECT via3 ( -4100 10300 ) ( -3900 10500 )
      + RECT via3 ( -3700 10300 ) ( -3500 10500 )
      + RECT via3 ( -3300 10300 ) ( -3100 10500 )
      + RECT via3 ( -2900 10300 ) ( -2700 10500 )
      + RECT via3 ( -2500 10300 ) ( -2300 10500 )
      + RECT via3 ( -2100 10300 ) ( -1900 10500 )
      + RECT via3 ( -1700 10300 ) ( -1500 10500 )
      + RECT via3 ( -1300 10300 ) ( -1100 10500 )
      + RECT via3 ( -900 10300 ) ( -700 10500 )
      + RECT via3 ( -500 10300 ) ( -300 10500 )
      + RECT via3 ( -100 10300 ) ( 100 10500 )
      + RECT via3 ( 300 10300 ) ( 500 10500 )
      + RECT via3 ( 700 10300 ) ( 900 10500 )
      + RECT via3 ( 1100 10300 ) ( 1300 10500 )
      + RECT via3 ( 1500 10300 ) ( 1700 10500 )
      + RECT via3 ( 1900 10300 ) ( 2100 10500 )
      + RECT via3 ( 2300 10300 ) ( 2500 10500 )
      + RECT via3 ( 2700 10300 ) ( 2900 10500 )
      + RECT via3 ( 3100 10300 ) ( 3300 10500 )
      + RECT via3 ( 3500 10300 ) ( 3700 10500 )
      + RECT via3 ( 3900 10300 ) ( 4100 10500 )
      + RECT via3 ( 4300 10300 ) ( 4500 10500 )
      + RECT via3 ( 4700 10300 ) ( 4900 10500 )
      + RECT via3 ( 5100 10300 ) ( 5300 10500 )
      + RECT via3 ( 5500 10300 ) ( 5700 10500 )
      + RECT via3 ( -5700 10700 ) ( -5500 10900 )
      + RECT via3 ( -5300 10700 ) ( -5100 10900 )
      + RECT via3 ( -4900 10700 ) ( -4700 10900 )
      + RECT via3 ( -4500 10700 ) ( -4300 10900 )
      + RECT via3 ( -4100 10700 ) ( -3900 10900 )
      + RECT via3 ( -3700 10700 ) ( -3500 10900 )
      + RECT via3 ( -3300 10700 ) ( -3100 10900 )
      + RECT via3 ( -2900 10700 ) ( -2700 10900 )
      + RECT via3 ( -2500 10700 ) ( -2300 10900 )
      + RECT via3 ( -2100 10700 ) ( -1900 10900 )
      + RECT via3 ( -1700 10700 ) ( -1500 10900 )
      + RECT via3 ( -1300 10700 ) ( -1100 10900 )
      + RECT via3 ( -900 10700 ) ( -700 10900 )
      + RECT via3 ( -500 10700 ) ( -300 10900 )
      + RECT via3 ( -100 10700 ) ( 100 10900 )
      + RECT via3 ( 300 10700 ) ( 500 10900 )
      + RECT via3 ( 700 10700 ) ( 900 10900 )
      + RECT via3 ( 1100 10700 ) ( 1300 10900 )
      + RECT via3 ( 1500 10700 ) ( 1700 10900 )
      + RECT via3 ( 1900 10700 ) ( 2100 10900 )
      + RECT via3 ( 2300 10700 ) ( 2500 10900 )
      + RECT via3 ( 2700 10700 ) ( 2900 10900 )
      + RECT via3 ( 3100 10700 ) ( 3300 10900 )
      + RECT via3 ( 3500 10700 ) ( 3700 10900 )
      + RECT via3 ( 3900 10700 ) ( 4100 10900 )
      + RECT via3 ( 4300 10700 ) ( 4500 10900 )
      + RECT via3 ( 4700 10700 ) ( 4900 10900 )
      + RECT via3 ( 5100 10700 ) ( 5300 10900 )
      + RECT via3 ( 5500 10700 ) ( 5700 10900 ) ;
   - via3_800_1590_hx
      + RECT met3 ( -430 -795 ) ( 430 795 )
      + RECT met4 ( -405 -800 ) ( 405 800 )
      + RECT via3 ( -300 -700 ) ( -100 -500 )
      + RECT via3 ( 100 -700 ) ( 300 -500 )
      + RECT via3 ( -300 -300 ) ( -100 -100 )
      + RECT via3 ( 100 -300 ) ( 300 -100 )
      + RECT via3 ( -300 100 ) ( -100 300 )
      + RECT via3 ( 100 100 ) ( 300 300 )
      + RECT via3 ( -300 500 ) ( -100 700 )
      + RECT via3 ( 100 500 ) ( 300 700 ) ;
END VIAS

COMPONENTS 824 ;
   - FILLER_148 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 200000 0 ) S ;
   - FILLER_352 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 204000 ) W ;
   - mgmt_corner\[0\] sky130_ef_io__corner_pad
      + PLACED ( 0 0 ) S ;
   - FILLER_149 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 220000 0 ) S ;
   - FILLER_150 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 230000 0 ) S ;
   - FILLER_151 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 235000 0 ) S ;
   - FILLER_152 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 236000 0 ) S ;
   - bus_tie_1 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 237000 0 ) S ;
   - bus_tie_2 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 257000 0 ) S ;
   - bus_tie_3 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 277000 0 ) S ;
   - FILLER_159 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 357000 0 ) S ;
   - bus_tie_4 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 297000 0 ) S ;
   - bus_tie_5 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 317000 0 ) S ;
   - bus_tie_6 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 337000 0 ) S ;
   - FILLER_160 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 377000 0 ) S ;
   - FILLER_161 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 387000 0 ) S ;
   - FILLER_162 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 392000 0 ) S ;
   - FILLER_163 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 393000 0 ) S ;
   - mgmt_vssa_hvclamp_pad sky130_ef_io__vssa_hvc_clamped_pad
      + PLACED ( 394000 0 ) S ;
   - FILLER_165 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 469000 0 ) S ;
   - FILLER_166 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 489000 0 ) S ;
   - FILLER_167 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 499000 0 ) S ;
   - FILLER_168 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 504000 0 ) S ;
   - FILLER_169 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 505000 0 ) S ;
   - bus_tie_7 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 506000 0 ) S ;
   - bus_tie_8 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 526000 0 ) S ;
   - bus_tie_9 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 546000 0 ) S ;
   - bus_tie_10 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 566000 0 ) S ;
   - bus_tie_11 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 586000 0 ) S ;
   - bus_tie_12 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 606000 0 ) S ;
   - FILLER_176 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 626000 0 ) S ;
   - FILLER_177 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 646000 0 ) S ;
   - FILLER_178 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 656000 0 ) S ;
   - FILLER_179 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 661000 0 ) S ;
   - FILLER_180 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 662000 0 ) S ;
   - resetb_pad sky130_fd_io__top_xres4v2
      + PLACED ( 663000 0 ) S ;
   - FILLER_182 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 738000 0 ) S ;
   - FILLER_183 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 758000 0 ) S ;
   - FILLER_184 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 768000 0 ) S ;
   - FILLER_185 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 773000 0 ) S ;
   - FILLER_186 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 774000 0 ) S ;
   - bus_tie_13 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 775000 0 ) S ;
   - constant_block_0 constant_block
      + PLACED ( 741080 198040 ) FN ;
   - bus_tie_14 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 795000 0 ) S ;
   - bus_tie_15 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 815000 0 ) S ;
   - bus_tie_16 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 835000 0 ) S ;
   - FILLER_193 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 895000 0 ) S ;
   - FILLER_194 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 915000 0 ) S ;
   - bus_tie_17 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 855000 0 ) S ;
   - bus_tie_18 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 875000 0 ) S ;
   - FILLER_195 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 925000 0 ) S ;
   - FILLER_196 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 930000 0 ) S ;
   - FILLER_197 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 931000 0 ) S ;
   - clock_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 932000 0 ) S ;
   - FILLER_199 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1012000 0 ) S ;
   - FILLER_200 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1032000 0 ) S ;
   - FILLER_201 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1042000 0 ) S ;
   - FILLER_202 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1047000 0 ) S ;
   - FILLER_203 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1048000 0 ) S ;
   - bus_tie_19 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1049000 0 ) S ;
   - constant_block_1 constant_block
      + PLACED ( 1015080 198040 ) FN ;
   - bus_tie_20 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1069000 0 ) S ;
   - bus_tie_21 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1089000 0 ) S ;
   - bus_tie_22 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1109000 0 ) S ;
   - bus_tie_23 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1129000 0 ) S ;
   - FILLER_210 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1169000 0 ) S ;
   - FILLER_211 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1189000 0 ) S ;
   - FILLER_212 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1199000 0 ) S ;
   - FILLER_213 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1204000 0 ) S ;
   - FILLER_214 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1205000 0 ) S ;
   - bus_tie_24 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1149000 0 ) S ;
   - mgmt_vssd_lvclamp_pad sky130_ef_io__vssd_lvc_clamped_pad
      + PLACED ( 1206000 0 ) S ;
   - FILLER_216 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1281000 0 ) S ;
   - FILLER_217 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1301000 0 ) S ;
   - FILLER_218 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1311000 0 ) S ;
   - FILLER_219 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1316000 0 ) S ;
   - FILLER_220 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1317000 0 ) S ;
   - bus_tie_25 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1318000 0 ) S ;
   - bus_tie_26 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1338000 0 ) S ;
   - bus_tie_27 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1358000 0 ) S ;
   - bus_tie_28 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1378000 0 ) S ;
   - bus_tie_29 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1398000 0 ) S ;
   - bus_tie_30 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1418000 0 ) S ;
   - FILLER_227 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1438000 0 ) S ;
   - FILLER_228 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1458000 0 ) S ;
   - FILLER_229 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1468000 0 ) S ;
   - FILLER_230 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1473000 0 ) S ;
   - FILLER_231 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1474000 0 ) S ;
   - flash_csb_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 1475000 0 ) S ;
   - FILLER_233 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1555000 0 ) S ;
   - FILLER_234 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1575000 0 ) S ;
   - constant_block_2 constant_block
      + PLACED ( 1563080 198040 ) FN ;
   - FILLER_235 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1585000 0 ) S ;
   - FILLER_236 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1590000 0 ) S ;
   - FILLER_237 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1591000 0 ) S ;
   - bus_tie_31 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1592000 0 ) S ;
   - bus_tie_32 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1612000 0 ) S ;
   - bus_tie_33 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1632000 0 ) S ;
   - bus_tie_34 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1652000 0 ) S ;
   - bus_tie_35 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1672000 0 ) S ;
   - FILLER_244 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1712000 0 ) S ;
   - FILLER_245 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1732000 0 ) S ;
   - FILLER_246 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1742000 0 ) S ;
   - FILLER_247 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1747000 0 ) S ;
   - FILLER_248 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1748000 0 ) S ;
   - bus_tie_36 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1692000 0 ) S ;
   - flash_clk_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 1749000 0 ) S ;
   - FILLER_250 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1829000 0 ) S ;
   - constant_block_3 constant_block
      + PLACED ( 1837080 198040 ) FN ;
   - FILLER_251 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1849000 0 ) S ;
   - FILLER_252 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1859000 0 ) S ;
   - FILLER_253 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1864000 0 ) S ;
   - FILLER_254 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1865000 0 ) S ;
   - bus_tie_37 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1866000 0 ) S ;
   - bus_tie_38 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1886000 0 ) S ;
   - bus_tie_39 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1906000 0 ) S ;
   - bus_tie_40 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1926000 0 ) S ;
   - bus_tie_41 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1946000 0 ) S ;
   - bus_tie_42 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 1966000 0 ) S ;
   - FILLER_261 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1986000 0 ) S ;
   - FILLER_262 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2006000 0 ) S ;
   - FILLER_263 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2016000 0 ) S ;
   - FILLER_264 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2021000 0 ) S ;
   - FILLER_265 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2022000 0 ) S ;
   - flash_io0_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 2023000 0 ) S ;
   - FILLER_267 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2103000 0 ) S ;
   - FILLER_268 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2123000 0 ) S ;
   - FILLER_269 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2133000 0 ) S ;
   - FILLER_270 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2138000 0 ) S ;
   - FILLER_271 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2139000 0 ) S ;
   - bus_tie_43 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2140000 0 ) S ;
   - bus_tie_44 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2160000 0 ) S ;
   - bus_tie_45 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2180000 0 ) S ;
   - constant_block_4 constant_block
      + PLACED ( 2111080 198040 ) FN ;
   - FILLER_278 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2260000 0 ) S ;
   - bus_tie_46 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2200000 0 ) S ;
   - bus_tie_47 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2220000 0 ) S ;
   - bus_tie_48 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2240000 0 ) S ;
   - FILLER_279 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2280000 0 ) S ;
   - FILLER_280 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2290000 0 ) S ;
   - FILLER_281 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2295000 0 ) S ;
   - FILLER_282 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2296000 0 ) S ;
   - flash_io1_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 2297000 0 ) S ;
   - FILLER_284 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2377000 0 ) S ;
   - FILLER_285 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2397000 0 ) S ;
   - constant_block_5 constant_block
      + PLACED ( 2385080 198040 ) FN ;
   - FILLER_286 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2407000 0 ) S ;
   - FILLER_287 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2412000 0 ) S ;
   - FILLER_288 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2413000 0 ) S ;
   - bus_tie_49 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2414000 0 ) S ;
   - bus_tie_50 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2434000 0 ) S ;
   - bus_tie_51 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2454000 0 ) S ;
   - bus_tie_52 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2474000 0 ) S ;
   - bus_tie_53 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2494000 0 ) S ;
   - bus_tie_54 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2514000 0 ) S ;
   - FILLER_295 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2534000 0 ) S ;
   - FILLER_296 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2554000 0 ) S ;
   - FILLER_297 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2564000 0 ) S ;
   - FILLER_298 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2569000 0 ) S ;
   - FILLER_299 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2570000 0 ) S ;
   - gpio_pad sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 2571000 0 ) S ;
   - FILLER_301 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2651000 0 ) S ;
   - FILLER_302 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2671000 0 ) S ;
   - FILLER_303 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2681000 0 ) S ;
   - FILLER_304 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2686000 0 ) S ;
   - FILLER_305 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2687000 0 ) S ;
   - bus_tie_55 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2688000 0 ) S ;
   - constant_block_6 constant_block
      + PLACED ( 2659080 198040 ) FN ;
   - bus_tie_56 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2708000 0 ) S ;
   - bus_tie_57 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2728000 0 ) S ;
   - FILLER_312 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2808000 0 ) S ;
   - bus_tie_58 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2748000 0 ) S ;
   - bus_tie_59 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2768000 0 ) S ;
   - bus_tie_60 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2788000 0 ) S ;
   - FILLER_313 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2828000 0 ) S ;
   - FILLER_314 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2838000 0 ) S ;
   - FILLER_315 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2843000 0 ) S ;
   - FILLER_316 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2844000 0 ) S ;
   - mgmt_vssio_hvclamp_pad\[0\] sky130_ef_io__vssio_hvc_clamped_pad
      + PLACED ( 2845000 0 ) S ;
   - FILLER_318 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2920000 0 ) S ;
   - FILLER_319 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2940000 0 ) S ;
   - FILLER_320 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2950000 0 ) S ;
   - FILLER_321 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2955000 0 ) S ;
   - FILLER_322 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2956000 0 ) S ;
   - bus_tie_61 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2957000 0 ) S ;
   - bus_tie_62 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2977000 0 ) S ;
   - bus_tie_63 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 2997000 0 ) S ;
   - bus_tie_64 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3017000 0 ) S ;
   - FILLER_329 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3077000 0 ) S ;
   - FILLER_330 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 3097000 0 ) S ;
   - bus_tie_65 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3037000 0 ) S ;
   - bus_tie_66 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3057000 0 ) S ;
   - FILLER_331 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3107000 0 ) S ;
   - FILLER_332 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3112000 0 ) S ;
   - FILLER_333 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3113000 0 ) S ;
   - mgmt_vdda_hvclamp_pad sky130_ef_io__vdda_hvc_clamped_pad
      + PLACED ( 3114000 0 ) S ;
   - FILLER_335 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3189000 0 ) S ;
   - FILLER_336 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 3209000 0 ) S ;
   - FILLER_337 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3219000 0 ) S ;
   - FILLER_338 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3224000 0 ) S ;
   - FILLER_339 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3225000 0 ) S ;
   - bus_tie_67 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3226000 0 ) S ;
   - bus_tie_68 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3246000 0 ) S ;
   - bus_tie_69 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3266000 0 ) S ;
   - bus_tie_70 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3286000 0 ) S ;
   - bus_tie_71 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3306000 0 ) S ;
   - bus_tie_72 sky130_ef_io__connect_vcchib_vccd_and_vswitch_vddio_slice_20um
      + PLACED ( 3326000 0 ) S ;
   - FILLER_346 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3346000 0 ) S ;
   - FILLER_347 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 3366000 0 ) S ;
   - FILLER_348 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3376000 0 ) S ;
   - FILLER_349 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3381000 0 ) S ;
   - FILLER_350 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3382000 0 ) S ;
   - FILLER_351 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3383000 0 ) S ;
   - FILLER_580 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 200000 ) E ;
   - mgmt_corner\[1\] sky130_ef_io__corner_pad
      + PLACED ( 3384000 0 ) E ;
   - FILLER_353 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 224000 ) W ;
   - FILLER_354 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 244000 ) W ;
   - FILLER_355 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 264000 ) W ;
   - FILLER_356 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 284000 ) W ;
   - FILLER_357 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 304000 ) W ;
   - FILLER_358 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 324000 ) W ;
   - FILLER_359 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 334000 ) W ;
   - FILLER_360 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 339000 ) W ;
   - mgmt_vccd_lvclamp_pad sky130_ef_io__vccd_lvc_clamped_pad
      + PLACED ( 0 340000 ) W ;
   - FILLER_362 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 415000 ) W ;
   - FILLER_581 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 220000 ) E ;
   - FILLER_582 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 240000 ) E ;
   - FILLER_583 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 260000 ) E ;
   - FILLER_584 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 280000 ) E ;
   - FILLER_585 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 300000 ) E ;
   - FILLER_586 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 320000 ) E ;
   - FILLER_587 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 340000 ) E ;
   - FILLER_SB1 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 350000 ) E ;
   - disconnect_vdda_1 sky130_ef_io__disconnect_vdda_slice_5um
      + PLACED ( 3390035 345000 ) E ;
   - FILLER_590 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 355000 ) E ;
   - FILLER_591 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 375000 ) E ;
   - FILLER_592 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 395000 ) E ;
   - FILLER_593 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 415000 ) E ;
   - FILLER_363 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 435000 ) W ;
   - FILLER_364 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 455000 ) W ;
   - FILLER_365 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 475000 ) W ;
   - FILLER_366 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 495000 ) W ;
   - FILLER_367 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 515000 ) W ;
   - FILLER_368 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 535000 ) W ;
   - FILLER_369 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 545000 ) W ;
   - FILLER_370 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 550000 ) W ;
   - mgmt_vddio_hvclamp_pad\[0\] sky130_ef_io__vddio_hvc_clamped_pad
      + PLACED ( 0 551000 ) W ;
   - FILLER_SB2 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 631000 ) W ;
   - disconnect_vdda_2 sky130_ef_io__disconnect_vdda_slice_5um
      + PLACED ( 0 626000 ) W ;
   - FILLER_594 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 435000 ) E ;
   - FILLER_595 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 455000 ) E ;
   - FILLER_596 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 475000 ) E ;
   - FILLER_597 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 495000 ) E ;
   - FILLER_599 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 580000 ) E ;
   - FILLER_600 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 600000 ) E ;
   - FILLER_601 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 620000 ) E ;
   - chip_io_gpio_connects_0 chip_io_gpio_connects
      + PLACED ( 0 0 ) N ;
   - mprj_pads.area1_io_pad\[0\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 500000 ) E ;
   - FILLER_374 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 636000 ) W ;
   - FILLER_375 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 656000 ) W ;
   - FILLER_376 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 676000 ) W ;
   - FILLER_377 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 696000 ) W ;
   - FILLER_378 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 716000 ) W ;
   - FILLER_379 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 736000 ) W ;
   - FILLER_380 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 756000 ) W ;
   - FILLER_381 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 776000 ) W ;
   - FILLER_382 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 796000 ) W ;
   - FILLER_383 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 816000 ) W ;
   - FILLER_384 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 836000 ) W ;
   - FILLER_602 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 640000 ) E ;
   - FILLER_603 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 660000 ) E ;
   - FILLER_604 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 680000 ) E ;
   - FILLER_605 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 700000 ) E ;
   - FILLER_606 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 720000 ) E ;
   - FILLER_607 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 725000 ) E ;
   - chip_io_gpio_connects_1 chip_io_gpio_connects
      + PLACED ( 0 226000 ) N ;
   - mprj_pads.area1_io_pad\[1\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 726000 ) E ;
   - FILLER_609 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 806000 ) E ;
   - FILLER_610 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 826000 ) E ;
   - FILLER_385 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 856000 ) W ;
   - FILLER_386 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 876000 ) W ;
   - FILLER_387 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 896000 ) W ;
   - FILLER_388 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 906000 ) W ;
   - FILLER_389 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 907000 ) W ;
   - chip_io_gpio_connects_15 chip_io_gpio_connects
      + PLACED ( -3168470 409975 ) S ;
   - mprj_pads.area2_io_pad\[12\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 908000 ) W ;
   - FILLER_391 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 988000 ) W ;
   - FILLER_392 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1008000 ) W ;
   - FILLER_393 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1028000 ) W ;
   - FILLER_394 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1048000 ) W ;
   - FILLER_611 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 846000 ) E ;
   - FILLER_612 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 866000 ) E ;
   - FILLER_613 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 886000 ) E ;
   - FILLER_614 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 906000 ) E ;
   - FILLER_615 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 926000 ) E ;
   - FILLER_616 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 946000 ) E ;
   - chip_io_gpio_connects_2 chip_io_gpio_connects
      + PLACED ( 0 451000 ) N ;
   - mprj_pads.area1_io_pad\[2\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 951000 ) E ;
   - FILLER_618 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1031000 ) E ;
   - FILLER_619 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1051000 ) E ;
   - FILLER_395 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1068000 ) W ;
   - FILLER_396 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1088000 ) W ;
   - FILLER_397 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 1108000 ) W ;
   - FILLER_398 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 1118000 ) W ;
   - FILLER_399 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 1123000 ) W ;
   - chip_io_gpio_connects_38 chip_io_gpio_connects
      + PLACED ( -3168470 625975 ) S ;
   - mprj_pads.area2_io_pad\[11\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 1124000 ) W ;
   - FILLER_401 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1204000 ) W ;
   - FILLER_402 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1224000 ) W ;
   - FILLER_403 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1244000 ) W ;
   - FILLER_404 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1264000 ) W ;
   - FILLER_620 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1071000 ) E ;
   - FILLER_621 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1091000 ) E ;
   - FILLER_622 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1111000 ) E ;
   - FILLER_623 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1131000 ) E ;
   - FILLER_624 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1151000 ) E ;
   - FILLER_625 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 1171000 ) E ;
   - FILLER_626 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 1176000 ) E ;
   - chip_io_gpio_connects_3 chip_io_gpio_connects
      + PLACED ( 0 677000 ) N ;
   - mprj_pads.area1_io_pad\[3\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 1177000 ) E ;
   - FILLER_628 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1257000 ) E ;
   - FILLER_405 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1284000 ) W ;
   - FILLER_406 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1304000 ) W ;
   - FILLER_407 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 1324000 ) W ;
   - FILLER_408 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 1334000 ) W ;
   - FILLER_409 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 1339000 ) W ;
   - chip_io_gpio_connects_37 chip_io_gpio_connects
      + PLACED ( -3168470 841975 ) S ;
   - mprj_pads.area2_io_pad\[10\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 1340000 ) W ;
   - FILLER_411 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1420000 ) W ;
   - FILLER_412 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1440000 ) W ;
   - FILLER_413 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1460000 ) W ;
   - FILLER_629 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1277000 ) E ;
   - FILLER_630 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1297000 ) E ;
   - FILLER_631 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1317000 ) E ;
   - FILLER_632 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1337000 ) E ;
   - FILLER_633 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1357000 ) E ;
   - FILLER_634 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1377000 ) E ;
   - FILLER_635 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 1397000 ) E ;
   - chip_io_gpio_connects_4 chip_io_gpio_connects
      + PLACED ( 0 902000 ) N ;
   - mprj_pads.area1_io_pad\[4\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 1402000 ) E ;
   - FILLER_414 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1480000 ) W ;
   - FILLER_415 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1500000 ) W ;
   - FILLER_416 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1520000 ) W ;
   - FILLER_417 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 1540000 ) W ;
   - FILLER_418 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 1550000 ) W ;
   - FILLER_419 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 1555000 ) W ;
   - mprj_pads.area2_io_pad\[9\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 1556000 ) W ;
   - FILLER_421 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1636000 ) W ;
   - chip_io_gpio_connects_36 chip_io_gpio_connects
      + PLACED ( -3168470 1057975 ) S ;
   - FILLER_422 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1656000 ) W ;
   - FILLER_423 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1676000 ) W ;
   - FILLER_637 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1482000 ) E ;
   - FILLER_638 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1502000 ) E ;
   - FILLER_639 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1522000 ) E ;
   - FILLER_640 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1542000 ) E ;
   - FILLER_641 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1562000 ) E ;
   - FILLER_642 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1582000 ) E ;
   - FILLER_643 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1602000 ) E ;
   - FILLER_644 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 1622000 ) E ;
   - chip_io_gpio_connects_5 chip_io_gpio_connects
      + PLACED ( 0 1127000 ) N ;
   - mprj_pads.area1_io_pad\[5\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 1627000 ) E ;
   - FILLER_424 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1696000 ) W ;
   - FILLER_425 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1716000 ) W ;
   - FILLER_426 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1736000 ) W ;
   - FILLER_427 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 1756000 ) W ;
   - FILLER_428 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 1766000 ) W ;
   - FILLER_429 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 1771000 ) W ;
   - chip_io_gpio_connects_35 chip_io_gpio_connects
      + PLACED ( -3168470 1273975 ) S ;
   - mprj_pads.area2_io_pad\[8\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 1772000 ) W ;
   - FILLER_431 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1852000 ) W ;
   - FILLER_432 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1872000 ) W ;
   - FILLER_433 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1892000 ) W ;
   - FILLER_646 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1707000 ) E ;
   - FILLER_647 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1727000 ) E ;
   - FILLER_648 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1747000 ) E ;
   - FILLER_649 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1767000 ) E ;
   - FILLER_650 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1787000 ) E ;
   - FILLER_651 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1807000 ) E ;
   - FILLER_652 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1827000 ) E ;
   - FILLER_653 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 1847000 ) E ;
   - FILLER_654 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 1852000 ) E ;
   - chip_io_gpio_connects_6 chip_io_gpio_connects
      + PLACED ( 0 1353000 ) N ;
   - mprj_pads.area1_io_pad\[6\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 1853000 ) E ;
   - FILLER_434 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1912000 ) W ;
   - FILLER_435 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1932000 ) W ;
   - FILLER_436 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 1952000 ) W ;
   - FILLER_437 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 1972000 ) W ;
   - FILLER_438 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 1982000 ) W ;
   - FILLER_439 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 1987000 ) W ;
   - chip_io_gpio_connects_34 chip_io_gpio_connects
      + PLACED ( -3168470 1489975 ) S ;
   - mprj_pads.area2_io_pad\[7\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 1988000 ) W ;
   - FILLER_441 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2068000 ) W ;
   - FILLER_442 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2088000 ) W ;
   - FILLER_443 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2108000 ) W ;
   - FILLER_656 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1933000 ) E ;
   - FILLER_657 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1953000 ) E ;
   - FILLER_658 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1973000 ) E ;
   - FILLER_659 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 1993000 ) E ;
   - FILLER_660 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2013000 ) E ;
   - FILLER_661 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2033000 ) E ;
   - FILLER_662 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2053000 ) E ;
   - FILLER_663 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 2073000 ) E ;
   - user1_vssa_hvclamp_pad\[1\] sky130_ef_io__vssa_hvc_clamped_pad
      + PLACED ( 3390035 2078000 ) E ;
   - FILLER_444 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2128000 ) W ;
   - FILLER_445 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2148000 ) W ;
   - FILLER_446 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2168000 ) W ;
   - FILLER_447 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 2188000 ) W ;
   - FILLER_448 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 2198000 ) W ;
   - FILLER_449 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 2203000 ) W ;
   - FILLER_451 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2279000 ) W ;
   - user2_vssd_lvclamp_pad sky130_ef_io__vssd_lvc_clamped3_pad
      + PLACED ( 0 2204000 ) W ;
   - FILLER_452 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2299000 ) W ;
   - FILLER_453 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2319000 ) W ;
   - FILLER_665 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2153000 ) E ;
   - FILLER_666 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2173000 ) E ;
   - FILLER_667 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2193000 ) E ;
   - FILLER_668 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2213000 ) E ;
   - FILLER_669 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2233000 ) E ;
   - FILLER_670 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2253000 ) E ;
   - FILLER_671 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2273000 ) E ;
   - FILLER_672 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 2293000 ) E ;
   - FILLER_673 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 2298000 ) E ;
   - user1_vssd_lvclamp_pad sky130_ef_io__vssd_lvc_clamped3_pad
      + PLACED ( 3390035 2299000 ) E ;
   - FILLER_454 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2339000 ) W ;
   - FILLER_455 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2359000 ) W ;
   - FILLER_456 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2379000 ) W ;
   - FILLER_457 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 2399000 ) W ;
   - FILLER_458 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 2409000 ) W ;
   - FILLER_459 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 2414000 ) W ;
   - user2_vdda_hvclamp_pad sky130_ef_io__vdda_hvc_clamped_pad
      + PLACED ( 0 2415000 ) W ;
   - FILLER_461 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2490000 ) W ;
   - FILLER_462 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2510000 ) W ;
   - FILLER_463 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2530000 ) W ;
   - FILLER_675 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2374000 ) E ;
   - FILLER_676 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2394000 ) E ;
   - FILLER_677 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2414000 ) E ;
   - FILLER_678 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2434000 ) E ;
   - FILLER_679 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2454000 ) E ;
   - FILLER_680 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2474000 ) E ;
   - FILLER_681 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2494000 ) E ;
   - FILLER_682 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 2514000 ) E ;
   - user1_vdda_hvclamp_pad\[1\] sky130_ef_io__vdda_hvc_clamped_pad
      + PLACED ( 3390035 2519000 ) E ;
   - FILLER_464 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2550000 ) W ;
   - FILLER_465 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2570000 ) W ;
   - FILLER_466 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2590000 ) W ;
   - FILLER_467 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 2610000 ) W ;
   - FILLER_468 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 2620000 ) W ;
   - FILLER_469 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 2625000 ) W ;
   - chip_io_gpio_connects_33 chip_io_gpio_connects
      + PLACED ( -3168470 2127975 ) S ;
   - mprj_pads.area2_io_pad\[6\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 2626000 ) W ;
   - FILLER_471 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2706000 ) W ;
   - FILLER_472 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2726000 ) W ;
   - FILLER_684 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2594000 ) E ;
   - FILLER_685 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2614000 ) E ;
   - FILLER_686 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2634000 ) E ;
   - FILLER_687 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2654000 ) E ;
   - FILLER_688 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2674000 ) E ;
   - FILLER_689 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2694000 ) E ;
   - FILLER_690 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2714000 ) E ;
   - FILLER_691 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 2734000 ) E ;
   - chip_io_gpio_connects_7 chip_io_gpio_connects
      + PLACED ( 0 2239000 ) N ;
   - mprj_pads.area1_io_pad\[7\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 2739000 ) E ;
   - FILLER_473 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2746000 ) W ;
   - FILLER_474 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2766000 ) W ;
   - FILLER_475 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2786000 ) W ;
   - FILLER_476 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2806000 ) W ;
   - FILLER_477 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 2826000 ) W ;
   - FILLER_478 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 2836000 ) W ;
   - FILLER_479 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 2841000 ) W ;
   - chip_io_gpio_connects_32 chip_io_gpio_connects
      + PLACED ( -3168470 2343975 ) S ;
   - mprj_pads.area2_io_pad\[5\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 2842000 ) W ;
   - FILLER_481 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2922000 ) W ;
   - FILLER_482 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2942000 ) W ;
   - FILLER_693 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2819000 ) E ;
   - FILLER_694 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2839000 ) E ;
   - FILLER_695 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2859000 ) E ;
   - FILLER_696 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2879000 ) E ;
   - FILLER_697 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2899000 ) E ;
   - FILLER_698 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2919000 ) E ;
   - FILLER_699 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 2939000 ) E ;
   - FILLER_483 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2962000 ) W ;
   - FILLER_484 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 2982000 ) W ;
   - FILLER_485 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3002000 ) W ;
   - FILLER_486 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3022000 ) W ;
   - FILLER_487 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 3042000 ) W ;
   - FILLER_488 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 3052000 ) W ;
   - FILLER_489 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 3057000 ) W ;
   - chip_io_gpio_connects_31 chip_io_gpio_connects
      + PLACED ( -3168470 2559975 ) S ;
   - mprj_pads.area2_io_pad\[4\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 3058000 ) W ;
   - FILLER_491 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3138000 ) W ;
   - FILLER_492 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3158000 ) W ;
   - FILLER_700 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 2959000 ) E ;
   - FILLER_701 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 2964000 ) E ;
   - chip_io_gpio_connects_8 chip_io_gpio_connects
      + PLACED ( 0 2465000 ) N ;
   - mprj_pads.area1_io_pad\[8\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 2965000 ) E ;
   - FILLER_703 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3045000 ) E ;
   - FILLER_704 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3065000 ) E ;
   - FILLER_705 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3085000 ) E ;
   - FILLER_706 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3105000 ) E ;
   - FILLER_707 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3125000 ) E ;
   - FILLER_708 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3145000 ) E ;
   - FILLER_493 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3178000 ) W ;
   - FILLER_494 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3198000 ) W ;
   - FILLER_495 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3218000 ) W ;
   - FILLER_496 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3238000 ) W ;
   - FILLER_497 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 3258000 ) W ;
   - FILLER_498 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 3268000 ) W ;
   - FILLER_499 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 3273000 ) W ;
   - chip_io_gpio_connects_30 chip_io_gpio_connects
      + PLACED ( -3168470 2775975 ) S ;
   - mprj_pads.area2_io_pad\[3\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 3274000 ) W ;
   - FILLER_501 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3354000 ) W ;
   - FILLER_502 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3374000 ) W ;
   - FILLER_709 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3165000 ) E ;
   - FILLER_710 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 3185000 ) E ;
   - chip_io_gpio_connects_9 chip_io_gpio_connects
      + PLACED ( 0 2690000 ) N ;
   - mprj_pads.area1_io_pad\[9\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 3190000 ) E ;
   - FILLER_712 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3270000 ) E ;
   - FILLER_713 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3290000 ) E ;
   - FILLER_714 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3310000 ) E ;
   - FILLER_715 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3330000 ) E ;
   - FILLER_716 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3350000 ) E ;
   - FILLER_717 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3370000 ) E ;
   - FILLER_503 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3394000 ) W ;
   - FILLER_504 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3414000 ) W ;
   - FILLER_505 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3434000 ) W ;
   - FILLER_506 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3454000 ) W ;
   - FILLER_507 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 3474000 ) W ;
   - FILLER_508 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 3484000 ) W ;
   - FILLER_509 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 3489000 ) W ;
   - chip_io_gpio_connects_29 chip_io_gpio_connects
      + PLACED ( -3168470 2991975 ) S ;
   - mprj_pads.area2_io_pad\[2\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 3490000 ) W ;
   - FILLER_511 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3570000 ) W ;
   - FILLER_718 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3390000 ) E ;
   - FILLER_719 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 3410000 ) E ;
   - FILLER_720 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 3415000 ) E ;
   - chip_io_gpio_connects_10 chip_io_gpio_connects
      + PLACED ( 0 2916000 ) N ;
   - mprj_pads.area1_io_pad\[10\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 3416000 ) E ;
   - FILLER_722 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3496000 ) E ;
   - FILLER_723 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3516000 ) E ;
   - FILLER_724 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3536000 ) E ;
   - FILLER_725 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3556000 ) E ;
   - FILLER_726 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3576000 ) E ;
   - FILLER_512 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3590000 ) W ;
   - FILLER_513 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3610000 ) W ;
   - FILLER_514 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3630000 ) W ;
   - FILLER_515 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3650000 ) W ;
   - FILLER_516 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3670000 ) W ;
   - FILLER_517 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 3690000 ) W ;
   - FILLER_518 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 3700000 ) W ;
   - FILLER_519 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 3705000 ) W ;
   - chip_io_gpio_connects_28 chip_io_gpio_connects
      + PLACED ( -3168470 3207975 ) S ;
   - mprj_pads.area2_io_pad\[1\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 3706000 ) W ;
   - FILLER_521 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3786000 ) W ;
   - FILLER_727 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3596000 ) E ;
   - FILLER_728 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3616000 ) E ;
   - FILLER_729 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 3636000 ) E ;
   - FILLER_731 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3721000 ) E ;
   - FILLER_732 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3741000 ) E ;
   - FILLER_733 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3761000 ) E ;
   - FILLER_734 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3781000 ) E ;
   - chip_io_gpio_connects_11 chip_io_gpio_connects
      + PLACED ( 0 3141000 ) N ;
   - mprj_pads.area1_io_pad\[11\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 3641000 ) E ;
   - FILLER_522 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3806000 ) W ;
   - FILLER_523 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3826000 ) W ;
   - FILLER_524 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3846000 ) W ;
   - FILLER_525 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3866000 ) W ;
   - FILLER_526 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 3886000 ) W ;
   - FILLER_527 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 3906000 ) W ;
   - FILLER_528 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 3916000 ) W ;
   - FILLER_529 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 3921000 ) W ;
   - chip_io_gpio_connects_27 chip_io_gpio_connects
      + PLACED ( -3168470 3423975 ) S ;
   - mprj_pads.area2_io_pad\[0\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 0 3922000 ) W ;
   - FILLER_531 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4002000 ) W ;
   - FILLER_735 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3801000 ) E ;
   - FILLER_736 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3821000 ) E ;
   - FILLER_737 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3841000 ) E ;
   - FILLER_738 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 3861000 ) E ;
   - chip_io_gpio_connects_12 chip_io_gpio_connects
      + PLACED ( 0 3366000 ) N ;
   - mprj_pads.area1_io_pad\[12\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 3866000 ) E ;
   - FILLER_740 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3946000 ) E ;
   - FILLER_741 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3966000 ) E ;
   - FILLER_742 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 3986000 ) E ;
   - FILLER_743 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4006000 ) E ;
   - FILLER_532 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4022000 ) W ;
   - FILLER_533 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4042000 ) W ;
   - FILLER_534 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4062000 ) W ;
   - FILLER_535 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4082000 ) W ;
   - FILLER_536 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4102000 ) W ;
   - FILLER_537 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 4122000 ) W ;
   - FILLER_538 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 4132000 ) W ;
   - FILLER_539 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4137000 ) W ;
   - user2_vssa_hvclamp_pad sky130_ef_io__vssa_hvc_clamped_pad
      + PLACED ( 0 4138000 ) W ;
   - FILLER_541 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4213000 ) W ;
   - FILLER_744 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4026000 ) E ;
   - FILLER_745 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4046000 ) E ;
   - FILLER_746 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4066000 ) E ;
   - FILLER_747 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 4086000 ) E ;
   - FILLER_748 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 4091000 ) E ;
   - FILLER_750 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4167000 ) E ;
   - FILLER_751 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4187000 ) E ;
   - FILLER_752 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4207000 ) E ;
   - user1_vdda_hvclamp_pad\[0\] sky130_ef_io__vdda_hvc_clamped_pad
      + PLACED ( 3390035 4092000 ) E ;
   - FILLER_542 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4233000 ) W ;
   - FILLER_543 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4253000 ) W ;
   - FILLER_544 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4273000 ) W ;
   - FILLER_545 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4293000 ) W ;
   - FILLER_546 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4313000 ) W ;
   - FILLER_547 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 4333000 ) W ;
   - FILLER_548 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 4343000 ) W ;
   - FILLER_549 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4348000 ) W ;
   - mgmt_vddio_hvclamp_pad\[1\] sky130_ef_io__vddio_hvc_clamped_pad
      + PLACED ( 0 4349000 ) W ;
   - FILLER_551 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4424000 ) W ;
   - FILLER_753 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4227000 ) E ;
   - FILLER_754 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4247000 ) E ;
   - FILLER_755 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4267000 ) E ;
   - FILLER_756 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4287000 ) E ;
   - FILLER_757 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 4307000 ) E ;
   - FILLER_759 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4392000 ) E ;
   - FILLER_760 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4412000 ) E ;
   - chip_io_gpio_connects_13 chip_io_gpio_connects
      + PLACED ( 0 3812000 ) N ;
   - mprj_pads.area1_io_pad\[13\] sky130_ef_io__gpiov2_pad_wrapped
      + PLACED ( 3377035 4312000 ) E ;
   - FILLER_552 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4444000 ) W ;
   - FILLER_553 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4464000 ) W ;
   - FILLER_554 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4484000 ) W ;
   - FILLER_555 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4504000 ) W ;
   - FILLER_556 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4524000 ) W ;
   - FILLER_557 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 4544000 ) W ;
   - FILLER_558 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 4554000 ) W ;
   - FILLER_559 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4559000 ) W ;
   - user2_vccd_lvclamp_pad sky130_ef_io__vccd_lvc_clamped3_pad
      + PLACED ( 0 4560000 ) W ;
   - FILLER_561 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4635000 ) W ;
   - FILLER_761 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4432000 ) E ;
   - FILLER_762 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4452000 ) E ;
   - FILLER_763 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4472000 ) E ;
   - FILLER_764 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4492000 ) E ;
   - FILLER_765 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4512000 ) E ;
   - FILLER_766 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 4532000 ) E ;
   - FILLER_767 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 4537000 ) E ;
   - user1_vccd_lvclamp_pad sky130_ef_io__vccd_lvc_clamped3_pad
      + PLACED ( 3390035 4538000 ) E ;
   - FILLER_769 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4613000 ) E ;
   - FILLER_770 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4633000 ) E ;
   - FILLER_562 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4655000 ) W ;
   - FILLER_563 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4675000 ) W ;
   - FILLER_564 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4695000 ) W ;
   - FILLER_565 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4715000 ) W ;
   - FILLER_566 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4735000 ) W ;
   - FILLER_567 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4755000 ) W ;
   - FILLER_568 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4775000 ) W ;
   - FILLER_570 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4851000 ) W ;
   - user2_analog_pad\[3\] sky130_ef_io__analog_pad
      + PLACED ( 0 4776000 ) W ;
   - FILLER_771 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4653000 ) E ;
   - FILLER_772 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4673000 ) E ;
   - FILLER_773 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4693000 ) E ;
   - FILLER_774 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4713000 ) E ;
   - FILLER_775 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4733000 ) E ;
   - FILLER_776 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 3390035 4833000 ) E ;
   - FILLER_777 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3390035 4753000 ) E ;
   - FILLER_779 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4843000 ) E ;
   - user1_analog_pad\[3\] sky130_ef_io__analog_pad
      + PLACED ( 3388000 4758000 ) E ;
   - FILLER_571 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4871000 ) W ;
   - FILLER_572 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4891000 ) W ;
   - FILLER_573 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4911000 ) W ;
   - FILLER_574 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4931000 ) W ;
   - FILLER_575 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 0 4951000 ) W ;
   - FILLER_576 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 0 4971000 ) W ;
   - FILLER_577 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 0 4981000 ) W ;
   - FILLER_578 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4986000 ) W ;
   - FILLER_579 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 0 4987000 ) W ;
   - FILLER_5 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 204000 4990035 ) N ;
   - user2_corner sky130_ef_io__corner_pad
      + PLACED ( 0 4988000 ) W ;
   - FILLER_6 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 224000 4990035 ) N ;
   - FILLER_7 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 244000 4990035 ) N ;
   - FILLER_8 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 264000 4990035 ) N ;
   - FILLER_9 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 284000 4990035 ) N ;
   - FILLER_10 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 304000 4990035 ) N ;
   - FILLER_11 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 324000 4990035 ) N ;
   - FILLER_12 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 344000 4990035 ) N ;
   - FILLER_13 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 364000 4990035 ) N ;
   - FILLER_14 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 384000 4990035 ) N ;
   - FILLER_15 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 385000 4990035 ) N ;
   - user2_analog_pad\[2\] sky130_ef_io__analog_pad
      + PLACED ( 386000 4988000 ) N ;
   - FILLER_17 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 461000 4990035 ) N ;
   - FILLER_18 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 481000 4990035 ) N ;
   - FILLER_19 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 501000 4990035 ) N ;
   - FILLER_20 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 521000 4990035 ) N ;
   - FILLER_21 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 541000 4990035 ) N ;
   - FILLER_22 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 561000 4990035 ) N ;
   - FILLER_23 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 581000 4990035 ) N ;
   - FILLER_24 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 601000 4990035 ) N ;
   - FILLER_25 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 621000 4990035 ) N ;
   - FILLER_26 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 641000 4990035 ) N ;
   - FILLER_27 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 642000 4990035 ) N ;
   - user2_analog_pad\[1\] sky130_ef_io__analog_pad
      + PLACED ( 643000 4988000 ) N ;
   - FILLER_29 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 718000 4990035 ) N ;
   - FILLER_30 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 738000 4990035 ) N ;
   - FILLER_31 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 758000 4990035 ) N ;
   - FILLER_32 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 778000 4990035 ) N ;
   - FILLER_33 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 798000 4990035 ) N ;
   - FILLER_34 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 818000 4990035 ) N ;
   - FILLER_35 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 838000 4990035 ) N ;
   - FILLER_36 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 858000 4990035 ) N ;
   - FILLER_37 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 878000 4990035 ) N ;
   - FILLER_38 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 898000 4990035 ) N ;
   - FILLER_39 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 899000 4990035 ) N ;
   - FILLER_41 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 975000 4990035 ) N ;
   - FILLER_42 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 995000 4990035 ) N ;
   - FILLER_43 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1015000 4990035 ) N ;
   - FILLER_44 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1035000 4990035 ) N ;
   - user2_analog_pad\[0\] sky130_ef_io__analog_pad
      + PLACED ( 900000 4988000 ) N ;
   - FILLER_45 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1055000 4990035 ) N ;
   - FILLER_46 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1075000 4990035 ) N ;
   - FILLER_47 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1095000 4990035 ) N ;
   - user2_analog_pad_with_clamp\[1\] sky130_ef_io__top_power_hvc
      + PLACED ( 1105000 4990035 ) N ;
   - FILLER_49 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1274000 4990035 ) N ;
   - FILLER_50 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1294000 4990035 ) N ;
   - FILLER_51 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1314000 4990035 ) N ;
   - FILLER_52 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1334000 4990035 ) N ;
   - FILLER_53 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1354000 4990035 ) N ;
   - FILLER_54 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1359000 4990035 ) N ;
   - FILLER_55 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1360000 4990035 ) N ;
   - FILLER_56 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1361000 4990035 ) N ;
   - FILLER_57 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 1362000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_5um_2 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1363000 4990035 ) N ;
   - user2_analog_pad_with_clamp\[0\] sky130_ef_io__top_power_hvc
      + PLACED ( 1368000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_5um_3 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1537000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_10um_1 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1542000 4990035 ) N ;
   - FILLER_60 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1552000 4990035 ) N ;
   - FILLER_61 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1572000 4990035 ) N ;
   - FILLER_62 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1592000 4990035 ) N ;
   - FILLER_63 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1612000 4990035 ) N ;
   - FILLER_64 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1632000 4990035 ) N ;
   - FILLER_65 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 1652000 4990035 ) N ;
   - FILLER_66 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1662000 4990035 ) N ;
   - mgmt_vssio_hvclamp_pad\[1\] sky130_ef_io__vssio_hvc_clamped_pad
      + PLACED ( 1667000 4990035 ) N ;
   - FILLER_68 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1742000 4990035 ) N ;
   - FILLER_69 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1762000 4990035 ) N ;
   - FILLER_70 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1782000 4990035 ) N ;
   - FILLER_71 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1802000 4990035 ) N ;
   - FILLER_72 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1822000 4990035 ) N ;
   - FILLER_73 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 1842000 4990035 ) N ;
   - FILLER_SB3 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1867000 4990035 ) N ;
   - disconnect_vdda_0 sky130_ef_io__disconnect_vdda_slice_5um
      + PLACED ( 1862000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_5um_0 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 1872000 4990035 ) N ;
   - user1_analog_pad_with_clamp sky130_ef_io__top_power_hvc
      + PLACED ( 1877000 4990035 ) N ;
   - FILLER_78 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2061000 4990035 ) N ;
   - FILLER_79 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2081000 4990035 ) N ;
   - FILLER_80 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2101000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_5um_1 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2046000 4990035 ) N ;
   - sky130_ef_io__com_bus_slice_10um_0 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2051000 4990035 ) N ;
   - FILLER_81 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2121000 4990035 ) N ;
   - FILLER_82 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2141000 4990035 ) N ;
   - FILLER_83 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2161000 4990035 ) N ;
   - FILLER_84 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2181000 4990035 ) N ;
   - FILLER_85 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2201000 4990035 ) N ;
   - FILLER_86 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2221000 4990035 ) N ;
   - FILLER_87 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2241000 4990035 ) N ;
   - FILLER_88 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2261000 4990035 ) N ;
   - FILLER_89 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2281000 4990035 ) N ;
   - FILLER_90 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2301000 4990035 ) N ;
   - FILLER_91 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2321000 4990035 ) N ;
   - FILLER_92 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2341000 4990035 ) N ;
   - FILLER_93 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2361000 4990035 ) N ;
   - FILLER_94 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2366000 4990035 ) N ;
   - FILLER_95 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2367000 4990035 ) N ;
   - FILLER_96 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2368000 4990035 ) N ;
   - user1_analog_pad\[2\] sky130_ef_io__analog_pad
      + PLACED ( 2369000 4988000 ) N ;
   - FILLER_98 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2444000 4990035 ) N ;
   - FILLER_99 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2464000 4990035 ) N ;
   - FILLER_100 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2484000 4990035 ) N ;
   - FILLER_101 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2504000 4990035 ) N ;
   - FILLER_102 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2524000 4990035 ) N ;
   - FILLER_103 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2544000 4990035 ) N ;
   - FILLER_104 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2564000 4990035 ) N ;
   - FILLER_105 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2584000 4990035 ) N ;
   - FILLER_106 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2604000 4990035 ) N ;
   - FILLER_107 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2624000 4990035 ) N ;
   - FILLER_108 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2625000 4990035 ) N ;
   - user1_analog_pad\[1\] sky130_ef_io__analog_pad
      + PLACED ( 2626000 4988000 ) N ;
   - FILLER_110 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2701000 4990035 ) N ;
   - FILLER_111 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2721000 4990035 ) N ;
   - FILLER_112 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2741000 4990035 ) N ;
   - FILLER_113 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2761000 4990035 ) N ;
   - FILLER_114 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2781000 4990035 ) N ;
   - FILLER_115 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2801000 4990035 ) N ;
   - FILLER_116 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2821000 4990035 ) N ;
   - FILLER_117 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2841000 4990035 ) N ;
   - FILLER_118 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 2861000 4990035 ) N ;
   - FILLER_119 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 2871000 4990035 ) N ;
   - FILLER_120 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2876000 4990035 ) N ;
   - FILLER_121 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 2877000 4990035 ) N ;
   - user1_vssa_hvclamp_pad\[0\] sky130_ef_io__vssa_hvc_clamped_pad
      + PLACED ( 2878000 4990035 ) N ;
   - FILLER_123 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2953000 4990035 ) N ;
   - FILLER_124 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2973000 4990035 ) N ;
   - FILLER_125 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 2993000 4990035 ) N ;
   - FILLER_126 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3013000 4990035 ) N ;
   - FILLER_127 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3033000 4990035 ) N ;
   - FILLER_128 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3053000 4990035 ) N ;
   - FILLER_129 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3073000 4990035 ) N ;
   - FILLER_130 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3093000 4990035 ) N ;
   - FILLER_131 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3113000 4990035 ) N ;
   - FILLER_132 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3133000 4990035 ) N ;
   - FILLER_133 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3134000 4990035 ) N ;
   - user1_analog_pad\[0\] sky130_ef_io__analog_pad
      + PLACED ( 3135000 4988000 ) N ;
   - FILLER_135 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3210000 4990035 ) N ;
   - FILLER_136 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3230000 4990035 ) N ;
   - FILLER_137 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3250000 4990035 ) N ;
   - FILLER_138 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3270000 4990035 ) N ;
   - FILLER_139 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3290000 4990035 ) N ;
   - FILLER_140 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3310000 4990035 ) N ;
   - FILLER_141 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3330000 4990035 ) N ;
   - FILLER_142 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3350000 4990035 ) N ;
   - FILLER_143 sky130_ef_io__com_bus_slice_10um
      + PLACED ( 3370000 4990035 ) N ;
   - FILLER_780 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4863000 ) E ;
   - FILLER_781 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4883000 ) E ;
   - FILLER_782 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4903000 ) E ;
   - FILLER_783 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4923000 ) E ;
   - FILLER_784 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4943000 ) E ;
   - FILLER_785 sky130_ef_io__com_bus_slice_20um
      + PLACED ( 3390035 4963000 ) E ;
   - FILLER_786 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3390035 4983000 ) E ;
   - FILLER_144 sky130_ef_io__com_bus_slice_5um
      + PLACED ( 3380000 4990035 ) N ;
   - FILLER_145 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3385000 4990035 ) N ;
   - FILLER_146 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3386000 4990035 ) N ;
   - FILLER_147 sky130_ef_io__com_bus_slice_1um
      + PLACED ( 3387000 4990035 ) N ;
   - user1_corner sky130_ef_io__corner_pad
      + PLACED ( 3388000 4984000 ) N ;
END COMPONENTS

PINS 584 ;
   - clock + NET clock
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 969550 64215 ) N ;
   - flash_clk + NET flash_clk
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 1786550 64215 ) N ;
   - flash_csb + NET flash_csb
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 1512550 64215 ) N ;
   - flash_io0 + NET flash_io0
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 2060550 64215 ) N ;
   - flash_io1 + NET flash_io1
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 2334550 64215 ) N ;
   - gpio + NET gpio
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31350 -31225 ) ( 31350 31225 )        + PLACED ( 2608550 64215 ) N ;
   - vccd_pad + NET vccd_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -33630 -27200 ) ( 33630 27200 )        + PLACED ( 64465 377470 ) N ;
   - vdda_pad + NET vdda_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 3151530 64465 ) N ;
   - vddio_pad + NET vddio_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 64465 588470 ) N ;
   - vddio_pad2 + NET vddio_pad2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 64465 4386470 ) N ;
   - vssa_pad + NET vssa_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 431530 64465 ) N ;
   - vssd_pad + NET vssd_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -27200 -33630 ) ( 27200 33630 )        + PLACED ( 1243530 64465 ) N ;
   - vssio_pad + NET vssio_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 2882530 64465 ) N ;
   - vssio_pad2 + NET vssio_pad2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 1704470 5123530 ) N ;
   - mprj_io[0] + NET mprj_io[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 537550 ) N ;
   - mprj_io_analog_en[0] + NET mprj_io_analog_en[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 529155 ) N ;
   - mprj_io_analog_pol[0] + NET mprj_io_analog_pol[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 535595 ) N ;
   - mprj_io_analog_sel[0] + NET mprj_io_analog_sel[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 550775 ) N ;
   - mprj_io_dm[0] + NET mprj_io_dm[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 532375 ) N ;
   - mprj_io_dm[1] + NET mprj_io_dm[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 523175 ) N ;
   - mprj_io_dm[2] + NET mprj_io_dm[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 553995 ) N ;
   - mprj_io_holdover[0] + NET mprj_io_holdover[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 557215 ) N ;
   - mprj_io_ib_mode_sel[0] + NET mprj_io_ib_mode_sel[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 572395 ) N ;
   - mprj_io_inp_dis[0] + NET mprj_io_inp_dis[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 538355 ) N ;
   - mprj_io_oeb[0] + NET mprj_io_oeb[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 575615 ) N ;
   - mprj_io_out[0] + NET mprj_io_out[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 559975 ) N ;
   - mprj_io_slow_sel[0] + NET mprj_io_slow_sel[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 513975 ) N ;
   - mprj_io_vtrip_sel[0] + NET mprj_io_vtrip_sel[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 569175 ) N ;
   - mprj_io_in[0] + NET mprj_io_in[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 504775 ) N ;
   - mprj_io_in_3v3[0] + NET mprj_io_in_3v3[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 578375 ) N ;
   - mprj_gpio_analog[3] + NET mprj_gpio_analog[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3433195 ) N ;
   - mprj_gpio_noesd[3] + NET mprj_gpio_noesd[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3442395 ) N ;
   - mprj_io[10] + NET mprj_io[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 3453550 ) N ;
   - mprj_io_analog_en[10] + NET mprj_io_analog_en[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3445155 ) N ;
   - mprj_io_analog_pol[10] + NET mprj_io_analog_pol[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3451595 ) N ;
   - mprj_io_analog_sel[10] + NET mprj_io_analog_sel[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3466775 ) N ;
   - mprj_io_dm[30] + NET mprj_io_dm[30]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3448375 ) N ;
   - mprj_io_dm[31] + NET mprj_io_dm[31]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3439175 ) N ;
   - mprj_io_dm[32] + NET mprj_io_dm[32]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3469995 ) N ;
   - mprj_io_holdover[10] + NET mprj_io_holdover[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3473215 ) N ;
   - mprj_io_ib_mode_sel[10] + NET mprj_io_ib_mode_sel[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3488395 ) N ;
   - mprj_io_inp_dis[10] + NET mprj_io_inp_dis[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3454355 ) N ;
   - mprj_io_oeb[10] + NET mprj_io_oeb[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3491615 ) N ;
   - mprj_io_out[10] + NET mprj_io_out[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3475975 ) N ;
   - mprj_io_slow_sel[10] + NET mprj_io_slow_sel[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3429975 ) N ;
   - mprj_io_vtrip_sel[10] + NET mprj_io_vtrip_sel[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3485175 ) N ;
   - mprj_io_in[10] + NET mprj_io_in[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3420775 ) N ;
   - mprj_io_in_3v3[10] + NET mprj_io_in_3v3[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3494375 ) N ;
   - mprj_gpio_analog[4] + NET mprj_gpio_analog[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3658195 ) N ;
   - mprj_gpio_noesd[4] + NET mprj_gpio_noesd[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3667395 ) N ;
   - mprj_io[11] + NET mprj_io[11]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 3678550 ) N ;
   - mprj_io_analog_en[11] + NET mprj_io_analog_en[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3670155 ) N ;
   - mprj_io_analog_pol[11] + NET mprj_io_analog_pol[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3676595 ) N ;
   - mprj_io_analog_sel[11] + NET mprj_io_analog_sel[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3691775 ) N ;
   - mprj_io_dm[33] + NET mprj_io_dm[33]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3673375 ) N ;
   - mprj_io_dm[34] + NET mprj_io_dm[34]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3664175 ) N ;
   - mprj_io_dm[35] + NET mprj_io_dm[35]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3694995 ) N ;
   - mprj_io_holdover[11] + NET mprj_io_holdover[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3698215 ) N ;
   - mprj_io_ib_mode_sel[11] + NET mprj_io_ib_mode_sel[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3713395 ) N ;
   - mprj_io_inp_dis[11] + NET mprj_io_inp_dis[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3679355 ) N ;
   - mprj_io_oeb[11] + NET mprj_io_oeb[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3716615 ) N ;
   - mprj_io_out[11] + NET mprj_io_out[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3700975 ) N ;
   - mprj_io_slow_sel[11] + NET mprj_io_slow_sel[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3654975 ) N ;
   - mprj_io_vtrip_sel[11] + NET mprj_io_vtrip_sel[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3710175 ) N ;
   - mprj_io_in[11] + NET mprj_io_in[11]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3645775 ) N ;
   - mprj_io_in_3v3[11] + NET mprj_io_in_3v3[11]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3719375 ) N ;
   - mprj_gpio_analog[5] + NET mprj_gpio_analog[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3883195 ) N ;
   - mprj_gpio_noesd[5] + NET mprj_gpio_noesd[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3892395 ) N ;
   - mprj_io[12] + NET mprj_io[12]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 3903550 ) N ;
   - mprj_io_analog_en[12] + NET mprj_io_analog_en[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3895155 ) N ;
   - mprj_io_analog_pol[12] + NET mprj_io_analog_pol[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3901595 ) N ;
   - mprj_io_analog_sel[12] + NET mprj_io_analog_sel[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3916775 ) N ;
   - mprj_io_dm[36] + NET mprj_io_dm[36]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3898375 ) N ;
   - mprj_io_dm[37] + NET mprj_io_dm[37]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3889175 ) N ;
   - mprj_io_dm[38] + NET mprj_io_dm[38]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3919995 ) N ;
   - mprj_io_holdover[12] + NET mprj_io_holdover[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3923215 ) N ;
   - mprj_io_ib_mode_sel[12] + NET mprj_io_ib_mode_sel[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3938395 ) N ;
   - mprj_io_inp_dis[12] + NET mprj_io_inp_dis[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3904355 ) N ;
   - mprj_io_oeb[12] + NET mprj_io_oeb[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3941615 ) N ;
   - mprj_io_out[12] + NET mprj_io_out[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3925975 ) N ;
   - mprj_io_slow_sel[12] + NET mprj_io_slow_sel[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3879975 ) N ;
   - mprj_io_vtrip_sel[12] + NET mprj_io_vtrip_sel[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3935175 ) N ;
   - mprj_io_in[12] + NET mprj_io_in[12]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3870775 ) N ;
   - mprj_io_in_3v3[12] + NET mprj_io_in_3v3[12]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3944375 ) N ;
   - mprj_gpio_analog[6] + NET mprj_gpio_analog[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4329195 ) N ;
   - mprj_gpio_noesd[6] + NET mprj_gpio_noesd[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4338395 ) N ;
   - mprj_io[13] + NET mprj_io[13]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 4349550 ) N ;
   - mprj_io_analog_en[13] + NET mprj_io_analog_en[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4341155 ) N ;
   - mprj_io_analog_pol[13] + NET mprj_io_analog_pol[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4347595 ) N ;
   - mprj_io_analog_sel[13] + NET mprj_io_analog_sel[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4362775 ) N ;
   - mprj_io_dm[39] + NET mprj_io_dm[39]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4344375 ) N ;
   - mprj_io_dm[40] + NET mprj_io_dm[40]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4335175 ) N ;
   - mprj_io_dm[41] + NET mprj_io_dm[41]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4365995 ) N ;
   - mprj_io_holdover[13] + NET mprj_io_holdover[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4369215 ) N ;
   - mprj_io_ib_mode_sel[13] + NET mprj_io_ib_mode_sel[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4384395 ) N ;
   - mprj_io_inp_dis[13] + NET mprj_io_inp_dis[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4350355 ) N ;
   - mprj_io_oeb[13] + NET mprj_io_oeb[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4387615 ) N ;
   - mprj_io_out[13] + NET mprj_io_out[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4371975 ) N ;
   - mprj_io_slow_sel[13] + NET mprj_io_slow_sel[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4325975 ) N ;
   - mprj_io_vtrip_sel[13] + NET mprj_io_vtrip_sel[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4381175 ) N ;
   - mprj_io_in[13] + NET mprj_io_in[13]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4316775 ) N ;
   - mprj_io_in_3v3[13] + NET mprj_io_in_3v3[13]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4390375 ) N ;
   - mprj_io[1] + NET mprj_io[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 763550 ) N ;
   - mprj_io_analog_en[1] + NET mprj_io_analog_en[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 755155 ) N ;
   - mprj_io_analog_pol[1] + NET mprj_io_analog_pol[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 761595 ) N ;
   - mprj_io_analog_sel[1] + NET mprj_io_analog_sel[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 776775 ) N ;
   - mprj_io_dm[3] + NET mprj_io_dm[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 758375 ) N ;
   - mprj_io_dm[4] + NET mprj_io_dm[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 749175 ) N ;
   - mprj_io_dm[5] + NET mprj_io_dm[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 779995 ) N ;
   - mprj_io_holdover[1] + NET mprj_io_holdover[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 783215 ) N ;
   - mprj_io_ib_mode_sel[1] + NET mprj_io_ib_mode_sel[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 798395 ) N ;
   - mprj_io_inp_dis[1] + NET mprj_io_inp_dis[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 764355 ) N ;
   - mprj_io_oeb[1] + NET mprj_io_oeb[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 801615 ) N ;
   - mprj_io_out[1] + NET mprj_io_out[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 785975 ) N ;
   - mprj_io_slow_sel[1] + NET mprj_io_slow_sel[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 739975 ) N ;
   - mprj_io_vtrip_sel[1] + NET mprj_io_vtrip_sel[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 795175 ) N ;
   - mprj_io_in[1] + NET mprj_io_in[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 730775 ) N ;
   - mprj_io_in_3v3[1] + NET mprj_io_in_3v3[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 804375 ) N ;
   - mprj_io[2] + NET mprj_io[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 988550 ) N ;
   - mprj_io_analog_en[2] + NET mprj_io_analog_en[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 980155 ) N ;
   - mprj_io_analog_pol[2] + NET mprj_io_analog_pol[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 986595 ) N ;
   - mprj_io_analog_sel[2] + NET mprj_io_analog_sel[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1001775 ) N ;
   - mprj_io_dm[6] + NET mprj_io_dm[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 983375 ) N ;
   - mprj_io_dm[7] + NET mprj_io_dm[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 974175 ) N ;
   - mprj_io_dm[8] + NET mprj_io_dm[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1004995 ) N ;
   - mprj_io_holdover[2] + NET mprj_io_holdover[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1008215 ) N ;
   - mprj_io_ib_mode_sel[2] + NET mprj_io_ib_mode_sel[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1023395 ) N ;
   - mprj_io_inp_dis[2] + NET mprj_io_inp_dis[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 989355 ) N ;
   - mprj_io_oeb[2] + NET mprj_io_oeb[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1026615 ) N ;
   - mprj_io_out[2] + NET mprj_io_out[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1010975 ) N ;
   - mprj_io_slow_sel[2] + NET mprj_io_slow_sel[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 964975 ) N ;
   - mprj_io_vtrip_sel[2] + NET mprj_io_vtrip_sel[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1020175 ) N ;
   - mprj_io_in[2] + NET mprj_io_in[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 955775 ) N ;
   - mprj_io_in_3v3[2] + NET mprj_io_in_3v3[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1029375 ) N ;
   - mprj_io[3] + NET mprj_io[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 1214550 ) N ;
   - mprj_io_analog_en[3] + NET mprj_io_analog_en[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1206155 ) N ;
   - mprj_io_analog_pol[3] + NET mprj_io_analog_pol[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1212595 ) N ;
   - mprj_io_analog_sel[3] + NET mprj_io_analog_sel[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1227775 ) N ;
   - mprj_io_dm[10] + NET mprj_io_dm[10]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1200175 ) N ;
   - mprj_io_dm[11] + NET mprj_io_dm[11]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1230995 ) N ;
   - mprj_io_dm[9] + NET mprj_io_dm[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1209375 ) N ;
   - mprj_io_holdover[3] + NET mprj_io_holdover[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1234215 ) N ;
   - mprj_io_ib_mode_sel[3] + NET mprj_io_ib_mode_sel[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1249395 ) N ;
   - mprj_io_inp_dis[3] + NET mprj_io_inp_dis[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1215355 ) N ;
   - mprj_io_oeb[3] + NET mprj_io_oeb[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1252615 ) N ;
   - mprj_io_out[3] + NET mprj_io_out[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1236975 ) N ;
   - mprj_io_slow_sel[3] + NET mprj_io_slow_sel[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1190975 ) N ;
   - mprj_io_vtrip_sel[3] + NET mprj_io_vtrip_sel[3]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1246175 ) N ;
   - mprj_io_in[3] + NET mprj_io_in[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1181775 ) N ;
   - mprj_io_in_3v3[3] + NET mprj_io_in_3v3[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1255375 ) N ;
   - mprj_io[4] + NET mprj_io[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 1439550 ) N ;
   - mprj_io_analog_en[4] + NET mprj_io_analog_en[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1431155 ) N ;
   - mprj_io_analog_pol[4] + NET mprj_io_analog_pol[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1437595 ) N ;
   - mprj_io_analog_sel[4] + NET mprj_io_analog_sel[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1452775 ) N ;
   - mprj_io_dm[12] + NET mprj_io_dm[12]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1434375 ) N ;
   - mprj_io_dm[13] + NET mprj_io_dm[13]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1425175 ) N ;
   - mprj_io_dm[14] + NET mprj_io_dm[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1455995 ) N ;
   - mprj_io_holdover[4] + NET mprj_io_holdover[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1459215 ) N ;
   - mprj_io_ib_mode_sel[4] + NET mprj_io_ib_mode_sel[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1474395 ) N ;
   - mprj_io_inp_dis[4] + NET mprj_io_inp_dis[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1440355 ) N ;
   - mprj_io_oeb[4] + NET mprj_io_oeb[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1477615 ) N ;
   - mprj_io_out[4] + NET mprj_io_out[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1461975 ) N ;
   - mprj_io_slow_sel[4] + NET mprj_io_slow_sel[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1415975 ) N ;
   - mprj_io_vtrip_sel[4] + NET mprj_io_vtrip_sel[4]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1471175 ) N ;
   - mprj_io_in[4] + NET mprj_io_in[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1406775 ) N ;
   - mprj_io_in_3v3[4] + NET mprj_io_in_3v3[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1480375 ) N ;
   - mprj_io[5] + NET mprj_io[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 1664550 ) N ;
   - mprj_io_analog_en[5] + NET mprj_io_analog_en[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1656155 ) N ;
   - mprj_io_analog_pol[5] + NET mprj_io_analog_pol[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1662595 ) N ;
   - mprj_io_analog_sel[5] + NET mprj_io_analog_sel[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1677775 ) N ;
   - mprj_io_dm[15] + NET mprj_io_dm[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1659375 ) N ;
   - mprj_io_dm[16] + NET mprj_io_dm[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1650175 ) N ;
   - mprj_io_dm[17] + NET mprj_io_dm[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1680995 ) N ;
   - mprj_io_holdover[5] + NET mprj_io_holdover[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1684215 ) N ;
   - mprj_io_ib_mode_sel[5] + NET mprj_io_ib_mode_sel[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1699395 ) N ;
   - mprj_io_inp_dis[5] + NET mprj_io_inp_dis[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1665355 ) N ;
   - mprj_io_oeb[5] + NET mprj_io_oeb[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1702615 ) N ;
   - mprj_io_out[5] + NET mprj_io_out[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1686975 ) N ;
   - mprj_io_slow_sel[5] + NET mprj_io_slow_sel[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1640975 ) N ;
   - mprj_io_vtrip_sel[5] + NET mprj_io_vtrip_sel[5]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1696175 ) N ;
   - mprj_io_in[5] + NET mprj_io_in[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1631775 ) N ;
   - mprj_io_in_3v3[5] + NET mprj_io_in_3v3[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1705375 ) N ;
   - mprj_io[6] + NET mprj_io[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 1890550 ) N ;
   - mprj_io_analog_en[6] + NET mprj_io_analog_en[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1882155 ) N ;
   - mprj_io_analog_pol[6] + NET mprj_io_analog_pol[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1888595 ) N ;
   - mprj_io_analog_sel[6] + NET mprj_io_analog_sel[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1903775 ) N ;
   - mprj_io_dm[18] + NET mprj_io_dm[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1885375 ) N ;
   - mprj_io_dm[19] + NET mprj_io_dm[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1876175 ) N ;
   - mprj_io_dm[20] + NET mprj_io_dm[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1906995 ) N ;
   - mprj_io_holdover[6] + NET mprj_io_holdover[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1910215 ) N ;
   - mprj_io_ib_mode_sel[6] + NET mprj_io_ib_mode_sel[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1925395 ) N ;
   - mprj_io_inp_dis[6] + NET mprj_io_inp_dis[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1891355 ) N ;
   - mprj_io_oeb[6] + NET mprj_io_oeb[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1928615 ) N ;
   - mprj_io_out[6] + NET mprj_io_out[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1912975 ) N ;
   - mprj_io_slow_sel[6] + NET mprj_io_slow_sel[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1866975 ) N ;
   - mprj_io_vtrip_sel[6] + NET mprj_io_vtrip_sel[6]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1922175 ) N ;
   - mprj_io_in[6] + NET mprj_io_in[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1857775 ) N ;
   - mprj_io_in_3v3[6] + NET mprj_io_in_3v3[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1931375 ) N ;
   - mprj_gpio_analog[0] + NET mprj_gpio_analog[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2756195 ) N ;
   - mprj_gpio_noesd[0] + NET mprj_gpio_noesd[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2765395 ) N ;
   - mprj_io[7] + NET mprj_io[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 2776550 ) N ;
   - mprj_io_analog_en[7] + NET mprj_io_analog_en[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2768155 ) N ;
   - mprj_io_analog_pol[7] + NET mprj_io_analog_pol[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2774595 ) N ;
   - mprj_io_analog_sel[7] + NET mprj_io_analog_sel[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2789775 ) N ;
   - mprj_io_dm[21] + NET mprj_io_dm[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2771375 ) N ;
   - mprj_io_dm[22] + NET mprj_io_dm[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2762175 ) N ;
   - mprj_io_dm[23] + NET mprj_io_dm[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2792995 ) N ;
   - mprj_io_holdover[7] + NET mprj_io_holdover[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2796215 ) N ;
   - mprj_io_ib_mode_sel[7] + NET mprj_io_ib_mode_sel[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2811395 ) N ;
   - mprj_io_inp_dis[7] + NET mprj_io_inp_dis[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2777355 ) N ;
   - mprj_io_oeb[7] + NET mprj_io_oeb[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2814615 ) N ;
   - mprj_io_out[7] + NET mprj_io_out[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2798975 ) N ;
   - mprj_io_slow_sel[7] + NET mprj_io_slow_sel[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2752975 ) N ;
   - mprj_io_vtrip_sel[7] + NET mprj_io_vtrip_sel[7]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2808175 ) N ;
   - mprj_io_in[7] + NET mprj_io_in[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2743775 ) N ;
   - mprj_io_in_3v3[7] + NET mprj_io_in_3v3[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2817375 ) N ;
   - mprj_gpio_analog[1] + NET mprj_gpio_analog[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2982195 ) N ;
   - mprj_gpio_noesd[1] + NET mprj_gpio_noesd[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2991395 ) N ;
   - mprj_io[8] + NET mprj_io[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 3002550 ) N ;
   - mprj_io_analog_en[8] + NET mprj_io_analog_en[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2994155 ) N ;
   - mprj_io_analog_pol[8] + NET mprj_io_analog_pol[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3000595 ) N ;
   - mprj_io_analog_sel[8] + NET mprj_io_analog_sel[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3015775 ) N ;
   - mprj_io_dm[24] + NET mprj_io_dm[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2997375 ) N ;
   - mprj_io_dm[25] + NET mprj_io_dm[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2988175 ) N ;
   - mprj_io_dm[26] + NET mprj_io_dm[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3018995 ) N ;
   - mprj_io_holdover[8] + NET mprj_io_holdover[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3022215 ) N ;
   - mprj_io_ib_mode_sel[8] + NET mprj_io_ib_mode_sel[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3037395 ) N ;
   - mprj_io_inp_dis[8] + NET mprj_io_inp_dis[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3003355 ) N ;
   - mprj_io_oeb[8] + NET mprj_io_oeb[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3040615 ) N ;
   - mprj_io_out[8] + NET mprj_io_out[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3024975 ) N ;
   - mprj_io_slow_sel[8] + NET mprj_io_slow_sel[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2978975 ) N ;
   - mprj_io_vtrip_sel[8] + NET mprj_io_vtrip_sel[8]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3034175 ) N ;
   - mprj_io_in[8] + NET mprj_io_in[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2969775 ) N ;
   - mprj_io_in_3v3[8] + NET mprj_io_in_3v3[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3043375 ) N ;
   - mprj_gpio_analog[2] + NET mprj_gpio_analog[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3207195 ) N ;
   - mprj_gpio_noesd[2] + NET mprj_gpio_noesd[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3216395 ) N ;
   - mprj_io[9] + NET mprj_io[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 3523785 3227550 ) N ;
   - mprj_io_analog_en[9] + NET mprj_io_analog_en[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3219155 ) N ;
   - mprj_io_analog_pol[9] + NET mprj_io_analog_pol[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3225595 ) N ;
   - mprj_io_analog_sel[9] + NET mprj_io_analog_sel[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3240775 ) N ;
   - mprj_io_dm[27] + NET mprj_io_dm[27]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3222375 ) N ;
   - mprj_io_dm[28] + NET mprj_io_dm[28]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3213175 ) N ;
   - mprj_io_dm[29] + NET mprj_io_dm[29]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3243995 ) N ;
   - mprj_io_holdover[9] + NET mprj_io_holdover[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3247215 ) N ;
   - mprj_io_ib_mode_sel[9] + NET mprj_io_ib_mode_sel[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3262395 ) N ;
   - mprj_io_inp_dis[9] + NET mprj_io_inp_dis[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3228355 ) N ;
   - mprj_io_oeb[9] + NET mprj_io_oeb[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3265615 ) N ;
   - mprj_io_out[9] + NET mprj_io_out[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3249975 ) N ;
   - mprj_io_slow_sel[9] + NET mprj_io_slow_sel[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3203975 ) N ;
   - mprj_io_vtrip_sel[9] + NET mprj_io_vtrip_sel[9]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3259175 ) N ;
   - mprj_io_in[9] + NET mprj_io_in[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3194775 ) N ;
   - mprj_io_in_3v3[9] + NET mprj_io_in_3v3[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3268375 ) N ;
   - mprj_gpio_analog[7] + NET mprj_gpio_analog[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3984805 ) N ;
   - mprj_gpio_noesd[7] + NET mprj_gpio_noesd[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3975605 ) N ;
   - mprj_io[25] + NET mprj_io[25]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 3964450 ) N ;
   - mprj_io_analog_en[14] + NET mprj_io_analog_en[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3972845 ) N ;
   - mprj_io_analog_pol[14] + NET mprj_io_analog_pol[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3966405 ) N ;
   - mprj_io_analog_sel[14] + NET mprj_io_analog_sel[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3951225 ) N ;
   - mprj_io_dm[42] + NET mprj_io_dm[42]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3969625 ) N ;
   - mprj_io_dm[43] + NET mprj_io_dm[43]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3978825 ) N ;
   - mprj_io_dm[44] + NET mprj_io_dm[44]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3948005 ) N ;
   - mprj_io_holdover[14] + NET mprj_io_holdover[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3944785 ) N ;
   - mprj_io_ib_mode_sel[14] + NET mprj_io_ib_mode_sel[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3929605 ) N ;
   - mprj_io_inp_dis[14] + NET mprj_io_inp_dis[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3963645 ) N ;
   - mprj_io_oeb[14] + NET mprj_io_oeb[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3926385 ) N ;
   - mprj_io_out[14] + NET mprj_io_out[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3942025 ) N ;
   - mprj_io_slow_sel[14] + NET mprj_io_slow_sel[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3988025 ) N ;
   - mprj_io_vtrip_sel[14] + NET mprj_io_vtrip_sel[14]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3932825 ) N ;
   - mprj_io_in[14] + NET mprj_io_in[14]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3997225 ) N ;
   - mprj_io_in_3v3[14] + NET mprj_io_in_3v3[14]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3923625 ) N ;
   - mprj_gpio_analog[17] + NET mprj_gpio_analog[17]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1402805 ) N ;
   - mprj_gpio_noesd[17] + NET mprj_gpio_noesd[17]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1393605 ) N ;
   - mprj_io[35] + NET mprj_io[35]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 1382450 ) N ;
   - mprj_io_analog_en[24] + NET mprj_io_analog_en[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1390845 ) N ;
   - mprj_io_analog_pol[24] + NET mprj_io_analog_pol[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1384405 ) N ;
   - mprj_io_analog_sel[24] + NET mprj_io_analog_sel[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1369225 ) N ;
   - mprj_io_dm[72] + NET mprj_io_dm[72]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1387625 ) N ;
   - mprj_io_dm[73] + NET mprj_io_dm[73]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1396825 ) N ;
   - mprj_io_dm[74] + NET mprj_io_dm[74]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1366005 ) N ;
   - mprj_io_holdover[24] + NET mprj_io_holdover[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1362785 ) N ;
   - mprj_io_ib_mode_sel[24] + NET mprj_io_ib_mode_sel[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1347605 ) N ;
   - mprj_io_inp_dis[24] + NET mprj_io_inp_dis[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1381645 ) N ;
   - mprj_io_oeb[24] + NET mprj_io_oeb[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1344385 ) N ;
   - mprj_io_out[24] + NET mprj_io_out[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1360025 ) N ;
   - mprj_io_slow_sel[24] + NET mprj_io_slow_sel[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1406025 ) N ;
   - mprj_io_vtrip_sel[24] + NET mprj_io_vtrip_sel[24]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1350825 ) N ;
   - mprj_io_in[24] + NET mprj_io_in[24]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1415225 ) N ;
   - mprj_io_in_3v3[24] + NET mprj_io_in_3v3[24]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1341625 ) N ;
   - mprj_io[36] + NET mprj_io[36]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 1166450 ) N ;
   - mprj_io_analog_en[25] + NET mprj_io_analog_en[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1174845 ) N ;
   - mprj_io_analog_pol[25] + NET mprj_io_analog_pol[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1168405 ) N ;
   - mprj_io_analog_sel[25] + NET mprj_io_analog_sel[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1153225 ) N ;
   - mprj_io_dm[75] + NET mprj_io_dm[75]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1171625 ) N ;
   - mprj_io_dm[76] + NET mprj_io_dm[76]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1180825 ) N ;
   - mprj_io_dm[77] + NET mprj_io_dm[77]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1150005 ) N ;
   - mprj_io_holdover[25] + NET mprj_io_holdover[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1146785 ) N ;
   - mprj_io_ib_mode_sel[25] + NET mprj_io_ib_mode_sel[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1131605 ) N ;
   - mprj_io_inp_dis[25] + NET mprj_io_inp_dis[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1165645 ) N ;
   - mprj_io_oeb[25] + NET mprj_io_oeb[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1128385 ) N ;
   - mprj_io_out[25] + NET mprj_io_out[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1144025 ) N ;
   - mprj_io_slow_sel[25] + NET mprj_io_slow_sel[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1190025 ) N ;
   - mprj_io_vtrip_sel[25] + NET mprj_io_vtrip_sel[25]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1134825 ) N ;
   - mprj_io_in[25] + NET mprj_io_in[25]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1199225 ) N ;
   - mprj_io_in_3v3[25] + NET mprj_io_in_3v3[25]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1125625 ) N ;
   - mprj_io[37] + NET mprj_io[37]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 950450 ) N ;
   - mprj_io_analog_en[26] + NET mprj_io_analog_en[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 958845 ) N ;
   - mprj_io_analog_pol[26] + NET mprj_io_analog_pol[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 952405 ) N ;
   - mprj_io_analog_sel[26] + NET mprj_io_analog_sel[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 937225 ) N ;
   - mprj_io_dm[78] + NET mprj_io_dm[78]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 955625 ) N ;
   - mprj_io_dm[79] + NET mprj_io_dm[79]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 964825 ) N ;
   - mprj_io_dm[80] + NET mprj_io_dm[80]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 934005 ) N ;
   - mprj_io_holdover[26] + NET mprj_io_holdover[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 930785 ) N ;
   - mprj_io_ib_mode_sel[26] + NET mprj_io_ib_mode_sel[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 915605 ) N ;
   - mprj_io_inp_dis[26] + NET mprj_io_inp_dis[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 949645 ) N ;
   - mprj_io_oeb[26] + NET mprj_io_oeb[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 912385 ) N ;
   - mprj_io_out[26] + NET mprj_io_out[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 928025 ) N ;
   - mprj_io_slow_sel[26] + NET mprj_io_slow_sel[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 974025 ) N ;
   - mprj_io_vtrip_sel[26] + NET mprj_io_vtrip_sel[26]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 918825 ) N ;
   - mprj_io_in[26] + NET mprj_io_in[26]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 983225 ) N ;
   - mprj_io_in_3v3[26] + NET mprj_io_in_3v3[26]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 909625 ) N ;
   - mprj_gpio_analog[8] + NET mprj_gpio_analog[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3768805 ) N ;
   - mprj_gpio_noesd[8] + NET mprj_gpio_noesd[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3759605 ) N ;
   - mprj_io[26] + NET mprj_io[26]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 3748450 ) N ;
   - mprj_io_analog_en[15] + NET mprj_io_analog_en[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3756845 ) N ;
   - mprj_io_analog_pol[15] + NET mprj_io_analog_pol[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3750405 ) N ;
   - mprj_io_analog_sel[15] + NET mprj_io_analog_sel[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3735225 ) N ;
   - mprj_io_dm[45] + NET mprj_io_dm[45]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3753625 ) N ;
   - mprj_io_dm[46] + NET mprj_io_dm[46]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3762825 ) N ;
   - mprj_io_dm[47] + NET mprj_io_dm[47]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3732005 ) N ;
   - mprj_io_holdover[15] + NET mprj_io_holdover[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3728785 ) N ;
   - mprj_io_ib_mode_sel[15] + NET mprj_io_ib_mode_sel[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3713605 ) N ;
   - mprj_io_inp_dis[15] + NET mprj_io_inp_dis[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3747645 ) N ;
   - mprj_io_oeb[15] + NET mprj_io_oeb[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3710385 ) N ;
   - mprj_io_out[15] + NET mprj_io_out[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3726025 ) N ;
   - mprj_io_slow_sel[15] + NET mprj_io_slow_sel[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3772025 ) N ;
   - mprj_io_vtrip_sel[15] + NET mprj_io_vtrip_sel[15]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3716825 ) N ;
   - mprj_io_in[15] + NET mprj_io_in[15]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3781225 ) N ;
   - mprj_io_in_3v3[15] + NET mprj_io_in_3v3[15]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3707625 ) N ;
   - mprj_gpio_analog[9] + NET mprj_gpio_analog[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3552805 ) N ;
   - mprj_gpio_noesd[9] + NET mprj_gpio_noesd[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3543605 ) N ;
   - mprj_io[27] + NET mprj_io[27]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 3532450 ) N ;
   - mprj_io_analog_en[16] + NET mprj_io_analog_en[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3540845 ) N ;
   - mprj_io_analog_pol[16] + NET mprj_io_analog_pol[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3534405 ) N ;
   - mprj_io_analog_sel[16] + NET mprj_io_analog_sel[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3519225 ) N ;
   - mprj_io_dm[48] + NET mprj_io_dm[48]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3537625 ) N ;
   - mprj_io_dm[49] + NET mprj_io_dm[49]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3546825 ) N ;
   - mprj_io_dm[50] + NET mprj_io_dm[50]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3516005 ) N ;
   - mprj_io_holdover[16] + NET mprj_io_holdover[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3512785 ) N ;
   - mprj_io_ib_mode_sel[16] + NET mprj_io_ib_mode_sel[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3497605 ) N ;
   - mprj_io_inp_dis[16] + NET mprj_io_inp_dis[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3531645 ) N ;
   - mprj_io_oeb[16] + NET mprj_io_oeb[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3494385 ) N ;
   - mprj_io_out[16] + NET mprj_io_out[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3510025 ) N ;
   - mprj_io_slow_sel[16] + NET mprj_io_slow_sel[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3556025 ) N ;
   - mprj_io_vtrip_sel[16] + NET mprj_io_vtrip_sel[16]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3500825 ) N ;
   - mprj_io_in[16] + NET mprj_io_in[16]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3565225 ) N ;
   - mprj_io_in_3v3[16] + NET mprj_io_in_3v3[16]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3491625 ) N ;
   - mprj_gpio_analog[10] + NET mprj_gpio_analog[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3336805 ) N ;
   - mprj_gpio_noesd[10] + NET mprj_gpio_noesd[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3327605 ) N ;
   - mprj_io[28] + NET mprj_io[28]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 3316450 ) N ;
   - mprj_io_analog_en[17] + NET mprj_io_analog_en[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3324845 ) N ;
   - mprj_io_analog_pol[17] + NET mprj_io_analog_pol[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3318405 ) N ;
   - mprj_io_analog_sel[17] + NET mprj_io_analog_sel[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3303225 ) N ;
   - mprj_io_dm[51] + NET mprj_io_dm[51]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3321625 ) N ;
   - mprj_io_dm[52] + NET mprj_io_dm[52]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3330825 ) N ;
   - mprj_io_dm[53] + NET mprj_io_dm[53]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3300005 ) N ;
   - mprj_io_holdover[17] + NET mprj_io_holdover[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3296785 ) N ;
   - mprj_io_ib_mode_sel[17] + NET mprj_io_ib_mode_sel[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3281605 ) N ;
   - mprj_io_inp_dis[17] + NET mprj_io_inp_dis[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3315645 ) N ;
   - mprj_io_oeb[17] + NET mprj_io_oeb[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3278385 ) N ;
   - mprj_io_out[17] + NET mprj_io_out[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3294025 ) N ;
   - mprj_io_slow_sel[17] + NET mprj_io_slow_sel[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3340025 ) N ;
   - mprj_io_vtrip_sel[17] + NET mprj_io_vtrip_sel[17]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3284825 ) N ;
   - mprj_io_in[17] + NET mprj_io_in[17]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3349225 ) N ;
   - mprj_io_in_3v3[17] + NET mprj_io_in_3v3[17]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3275625 ) N ;
   - mprj_gpio_analog[11] + NET mprj_gpio_analog[11]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3120805 ) N ;
   - mprj_gpio_noesd[11] + NET mprj_gpio_noesd[11]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3111605 ) N ;
   - mprj_io[29] + NET mprj_io[29]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 3100450 ) N ;
   - mprj_io_analog_en[18] + NET mprj_io_analog_en[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3108845 ) N ;
   - mprj_io_analog_pol[18] + NET mprj_io_analog_pol[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3102405 ) N ;
   - mprj_io_analog_sel[18] + NET mprj_io_analog_sel[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3087225 ) N ;
   - mprj_io_dm[54] + NET mprj_io_dm[54]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3105625 ) N ;
   - mprj_io_dm[55] + NET mprj_io_dm[55]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3114825 ) N ;
   - mprj_io_dm[56] + NET mprj_io_dm[56]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3084005 ) N ;
   - mprj_io_holdover[18] + NET mprj_io_holdover[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3080785 ) N ;
   - mprj_io_ib_mode_sel[18] + NET mprj_io_ib_mode_sel[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3065605 ) N ;
   - mprj_io_inp_dis[18] + NET mprj_io_inp_dis[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3099645 ) N ;
   - mprj_io_oeb[18] + NET mprj_io_oeb[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3062385 ) N ;
   - mprj_io_out[18] + NET mprj_io_out[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3078025 ) N ;
   - mprj_io_slow_sel[18] + NET mprj_io_slow_sel[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3124025 ) N ;
   - mprj_io_vtrip_sel[18] + NET mprj_io_vtrip_sel[18]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3068825 ) N ;
   - mprj_io_in[18] + NET mprj_io_in[18]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3133225 ) N ;
   - mprj_io_in_3v3[18] + NET mprj_io_in_3v3[18]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3059625 ) N ;
   - mprj_gpio_analog[12] + NET mprj_gpio_analog[12]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2904805 ) N ;
   - mprj_gpio_noesd[12] + NET mprj_gpio_noesd[12]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2895605 ) N ;
   - mprj_io[30] + NET mprj_io[30]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 2884450 ) N ;
   - mprj_io_analog_en[19] + NET mprj_io_analog_en[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2892845 ) N ;
   - mprj_io_analog_pol[19] + NET mprj_io_analog_pol[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2886405 ) N ;
   - mprj_io_analog_sel[19] + NET mprj_io_analog_sel[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2871225 ) N ;
   - mprj_io_dm[57] + NET mprj_io_dm[57]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2889625 ) N ;
   - mprj_io_dm[58] + NET mprj_io_dm[58]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2898825 ) N ;
   - mprj_io_dm[59] + NET mprj_io_dm[59]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2868005 ) N ;
   - mprj_io_holdover[19] + NET mprj_io_holdover[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2864785 ) N ;
   - mprj_io_ib_mode_sel[19] + NET mprj_io_ib_mode_sel[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2849605 ) N ;
   - mprj_io_inp_dis[19] + NET mprj_io_inp_dis[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2883645 ) N ;
   - mprj_io_oeb[19] + NET mprj_io_oeb[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2846385 ) N ;
   - mprj_io_out[19] + NET mprj_io_out[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2862025 ) N ;
   - mprj_io_slow_sel[19] + NET mprj_io_slow_sel[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2908025 ) N ;
   - mprj_io_vtrip_sel[19] + NET mprj_io_vtrip_sel[19]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2852825 ) N ;
   - mprj_io_in[19] + NET mprj_io_in[19]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2917225 ) N ;
   - mprj_io_in_3v3[19] + NET mprj_io_in_3v3[19]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2843625 ) N ;
   - mprj_gpio_analog[13] + NET mprj_gpio_analog[13]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2688805 ) N ;
   - mprj_gpio_noesd[13] + NET mprj_gpio_noesd[13]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2679605 ) N ;
   - mprj_io[31] + NET mprj_io[31]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 2668450 ) N ;
   - mprj_io_analog_en[20] + NET mprj_io_analog_en[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2676845 ) N ;
   - mprj_io_analog_pol[20] + NET mprj_io_analog_pol[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2670405 ) N ;
   - mprj_io_analog_sel[20] + NET mprj_io_analog_sel[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2655225 ) N ;
   - mprj_io_dm[60] + NET mprj_io_dm[60]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2673625 ) N ;
   - mprj_io_dm[61] + NET mprj_io_dm[61]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2682825 ) N ;
   - mprj_io_dm[62] + NET mprj_io_dm[62]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2652005 ) N ;
   - mprj_io_holdover[20] + NET mprj_io_holdover[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2648785 ) N ;
   - mprj_io_ib_mode_sel[20] + NET mprj_io_ib_mode_sel[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2633605 ) N ;
   - mprj_io_inp_dis[20] + NET mprj_io_inp_dis[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2667645 ) N ;
   - mprj_io_oeb[20] + NET mprj_io_oeb[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2630385 ) N ;
   - mprj_io_out[20] + NET mprj_io_out[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2646025 ) N ;
   - mprj_io_slow_sel[20] + NET mprj_io_slow_sel[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2692025 ) N ;
   - mprj_io_vtrip_sel[20] + NET mprj_io_vtrip_sel[20]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2636825 ) N ;
   - mprj_io_in[20] + NET mprj_io_in[20]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2701225 ) N ;
   - mprj_io_in_3v3[20] + NET mprj_io_in_3v3[20]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2627625 ) N ;
   - mprj_gpio_analog[14] + NET mprj_gpio_analog[14]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2050805 ) N ;
   - mprj_gpio_noesd[14] + NET mprj_gpio_noesd[14]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2041605 ) N ;
   - mprj_io[32] + NET mprj_io[32]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 2030450 ) N ;
   - mprj_io_analog_en[21] + NET mprj_io_analog_en[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2038845 ) N ;
   - mprj_io_analog_pol[21] + NET mprj_io_analog_pol[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2032405 ) N ;
   - mprj_io_analog_sel[21] + NET mprj_io_analog_sel[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2017225 ) N ;
   - mprj_io_dm[63] + NET mprj_io_dm[63]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2035625 ) N ;
   - mprj_io_dm[64] + NET mprj_io_dm[64]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2044825 ) N ;
   - mprj_io_dm[65] + NET mprj_io_dm[65]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2014005 ) N ;
   - mprj_io_holdover[21] + NET mprj_io_holdover[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2010785 ) N ;
   - mprj_io_ib_mode_sel[21] + NET mprj_io_ib_mode_sel[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1995605 ) N ;
   - mprj_io_inp_dis[21] + NET mprj_io_inp_dis[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2029645 ) N ;
   - mprj_io_oeb[21] + NET mprj_io_oeb[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1992385 ) N ;
   - mprj_io_out[21] + NET mprj_io_out[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2008025 ) N ;
   - mprj_io_slow_sel[21] + NET mprj_io_slow_sel[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2054025 ) N ;
   - mprj_io_vtrip_sel[21] + NET mprj_io_vtrip_sel[21]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1998825 ) N ;
   - mprj_io_in[21] + NET mprj_io_in[21]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2063225 ) N ;
   - mprj_io_in_3v3[21] + NET mprj_io_in_3v3[21]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1989625 ) N ;
   - mprj_gpio_analog[15] + NET mprj_gpio_analog[15]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1834805 ) N ;
   - mprj_gpio_noesd[15] + NET mprj_gpio_noesd[15]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1825605 ) N ;
   - mprj_io[33] + NET mprj_io[33]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 1814450 ) N ;
   - mprj_io_analog_en[22] + NET mprj_io_analog_en[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1822845 ) N ;
   - mprj_io_analog_pol[22] + NET mprj_io_analog_pol[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1816405 ) N ;
   - mprj_io_analog_sel[22] + NET mprj_io_analog_sel[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1801225 ) N ;
   - mprj_io_dm[66] + NET mprj_io_dm[66]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1819625 ) N ;
   - mprj_io_dm[67] + NET mprj_io_dm[67]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1828825 ) N ;
   - mprj_io_dm[68] + NET mprj_io_dm[68]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1798005 ) N ;
   - mprj_io_holdover[22] + NET mprj_io_holdover[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1794785 ) N ;
   - mprj_io_ib_mode_sel[22] + NET mprj_io_ib_mode_sel[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1779605 ) N ;
   - mprj_io_inp_dis[22] + NET mprj_io_inp_dis[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1813645 ) N ;
   - mprj_io_oeb[22] + NET mprj_io_oeb[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1776385 ) N ;
   - mprj_io_out[22] + NET mprj_io_out[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1792025 ) N ;
   - mprj_io_slow_sel[22] + NET mprj_io_slow_sel[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1838025 ) N ;
   - mprj_io_vtrip_sel[22] + NET mprj_io_vtrip_sel[22]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1782825 ) N ;
   - mprj_io_in[22] + NET mprj_io_in[22]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1847225 ) N ;
   - mprj_io_in_3v3[22] + NET mprj_io_in_3v3[22]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1773625 ) N ;
   - mprj_gpio_analog[16] + NET mprj_gpio_analog[16]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1618805 ) N ;
   - mprj_gpio_noesd[16] + NET mprj_gpio_noesd[16]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1609605 ) N ;
   - mprj_io[34] + NET mprj_io[34]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -31225 -31350 ) ( 31225 31350 )        + PLACED ( 64215 1598450 ) N ;
   - mprj_io_analog_en[23] + NET mprj_io_analog_en[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1606845 ) N ;
   - mprj_io_analog_pol[23] + NET mprj_io_analog_pol[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1600405 ) N ;
   - mprj_io_analog_sel[23] + NET mprj_io_analog_sel[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1585225 ) N ;
   - mprj_io_dm[69] + NET mprj_io_dm[69]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1603625 ) N ;
   - mprj_io_dm[70] + NET mprj_io_dm[70]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1612825 ) N ;
   - mprj_io_dm[71] + NET mprj_io_dm[71]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1582005 ) N ;
   - mprj_io_holdover[23] + NET mprj_io_holdover[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1578785 ) N ;
   - mprj_io_ib_mode_sel[23] + NET mprj_io_ib_mode_sel[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1563605 ) N ;
   - mprj_io_inp_dis[23] + NET mprj_io_inp_dis[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1597645 ) N ;
   - mprj_io_oeb[23] + NET mprj_io_oeb[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1560385 ) N ;
   - mprj_io_out[23] + NET mprj_io_out[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1576025 ) N ;
   - mprj_io_slow_sel[23] + NET mprj_io_slow_sel[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1622025 ) N ;
   - mprj_io_vtrip_sel[23] + NET mprj_io_vtrip_sel[23]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1566825 ) N ;
   - mprj_io_in[23] + NET mprj_io_in[23]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1631225 ) N ;
   - mprj_io_in_3v3[23] + NET mprj_io_in_3v3[23]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1557625 ) N ;
   - resetb + NET resetb
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -18590 -27915 ) ( 18590 27915 )        + PLACED ( 702155 63630 ) N ;
   - vdda + NET vdda
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met4 ( -480 -1725 ) ( 480 1725 )        + PLACED ( 663480 183340 ) N ;
   - mprj_io[15] + NET mprj_io[15]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 3172470 5123530 ) N ;
   - mprj_io[16] + NET mprj_io[16]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 2663470 5123530 ) N ;
   - mprj_io[17] + NET mprj_io[17]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 2406470 5123530 ) N ;
   - vccd1_pad + NET vccd1_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -33630 -27200 ) ( 33630 27200 )        + PLACED ( 3523530 4575530 ) N ;
   - vdda1_pad + NET vdda1_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 3523530 4129530 ) N ;
   - vdda1_pad2 + NET vdda1_pad2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 3523530 2556530 ) N ;
   - vssa1_pad + NET vssa1_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 2915470 5123530 ) N ;
   - vssa1_pad2 + NET vssa1_pad2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 3523530 2115530 ) N ;
   - vdda1 + NET vdda1
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met4 ( -1725 -480 ) ( 1725 480 )        + PLACED ( 3404660 2299480 ) N ;
   - vssa1 + NET vssa1
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met4 ( -165 -37500 ) ( 165 37500 )        + PLACED ( 3444570 2336500 ) N ;
   - vssd1_pad + NET vssd1_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -33630 -27200 ) ( 33630 27200 )        + PLACED ( 3523530 2336530 ) N ;
   - mprj_analog[7] + NET mprj_analog[7]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 937220 5029175 ) N ;
   - mprj_io[21] + NET mprj_io[21]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 937470 5123530 ) N ;
   - mprj_analog[8] + NET mprj_analog[8]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 680220 5029175 ) N ;
   - mprj_io[22] + NET mprj_io[22]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 680470 5123530 ) N ;
   - mprj_analog[9] + NET mprj_analog[9]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 423220 5029175 ) N ;
   - mprj_io[23] + NET mprj_io[23]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 423470 5123530 ) N ;
   - mprj_analog[10] + NET mprj_analog[10]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -41175 -12500 ) ( 41175 12500 )        + PLACED ( 158825 4813220 ) N ;
   - mprj_io[24] + NET mprj_io[24]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 64465 4813470 ) N ;
   - mprj_analog[6] + NET mprj_analog[6]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -35805 -7840 ) ( 35805 7840 )        + PLACED ( 1238195 4995840 ) N ;
   - mprj_clamp_high[2] + NET mprj_clamp_high[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -12830 ) ( 11950 12830 )        + PLACED ( 1214340 5000830 ) N ;
   - mprj_clamp_low[2] + NET mprj_clamp_low[2]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -1025 ) ( 11950 1025 )        + PLACED ( 1164445 4989025 ) N ;
   - mprj_io[20] + NET mprj_io[20]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 1189470 5123530 ) N ;
   - vccd2_pad + NET vccd2_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -33630 -27200 ) ( 33630 27200 )        + PLACED ( 64465 4597470 ) N ;
   - vdda2_pad + NET vdda2_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 64465 2452470 ) N ;
   - vssa2_pad + NET vssa2_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 64465 4175470 ) N ;
   - vdda2 + NET vdda2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met4 ( -1725 -480 ) ( 1725 480 )        + PLACED ( 183340 2278515 ) N ;
   - vssa2 + NET vssa2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met4 ( -165 -37500 ) ( 165 37500 )        + PLACED ( 143430 2241500 ) N ;
   - vssd2_pad + NET vssd2_pad
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -33630 -27200 ) ( 33630 27200 )        + PLACED ( 64465 2241470 ) N ;
   - mprj_io[18] + NET mprj_io[18]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 1961470 5123530 ) N ;
   - mprj_io[19] + NET mprj_io[19]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30420 -30410 ) ( 30420 30410 )        + PLACED ( 1452470 5123530 ) N ;
   - mprj_io[14] + NET mprj_io[14]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -30410 -30420 ) ( 30410 30420 )        + PLACED ( 3523530 4795530 ) N ;
   - mprj_analog[5] + NET mprj_analog[5]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -35805 -7840 ) ( 35805 7840 )        + PLACED ( 1501195 4995840 ) N ;
   - mprj_clamp_high[1] + NET mprj_clamp_high[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -12830 ) ( 11950 12830 )        + PLACED ( 1477340 5000830 ) N ;
   - mprj_clamp_low[1] + NET mprj_clamp_low[1]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -1025 ) ( 11950 1025 )        + PLACED ( 1427445 4989025 ) N ;
   - mprj_analog[4] + NET mprj_analog[4]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -35805 -7840 ) ( 35805 7840 )        + PLACED ( 2010195 4995840 ) N ;
   - mprj_clamp_high[0] + NET mprj_clamp_high[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -12830 ) ( 11950 12830 )        + PLACED ( 1986340 5000830 ) N ;
   - mprj_clamp_low[0] + NET mprj_clamp_low[0]
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -11950 -1025 ) ( 11950 1025 )        + PLACED ( 1936445 4989025 ) N ;
   - resetb_core_h + NET resetb_core_h
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -365 -165 ) ( 365 165 )        + PLACED ( 708700 199835 ) N ;
   - vccd2 + NET vccd2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -6090 -1880 ) ( 6090 1880 )        + PLACED ( 227470 894390 ) N ;
   - vssd2 + NET vssd2
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -6090 -1880 ) ( 6090 1880 )        + PLACED ( 211370 894390 ) N ;
   - vccd1 + NET vccd1
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -5910 -1740 ) ( 5910 1740 )        + PLACED ( 3376660 675090 ) N ;
   - vssd1 + NET vssd1
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met5 ( -5910 -1740 ) ( 5910 1740 )        + PLACED ( 3360590 675690 ) N ;
   - mprj_analog[0] + NET mprj_analog[0]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -41175 -12500 ) ( 41175 12500 )        + PLACED ( 3429175 4795780 ) N ;
   - mprj_analog[1] + NET mprj_analog[1]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 3172220 5029175 ) N ;
   - mprj_analog[2] + NET mprj_analog[2]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 2663220 5029175 ) N ;
   - mprj_analog[3] + NET mprj_analog[3]
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met3 ( -12500 -41175 ) ( 12500 41175 )        + PLACED ( 2406220 5029175 ) N ;
   - gpio_inenb_core + NET gpio_inenb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2609355 209765 ) N ;
   - flash_csb_oeb_core + NET flash_csb_oeb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 1550615 209765 ) N ;
   - flash_clk_core + NET flash_clk_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 1808975 209765 ) N ;
   - flash_clk_oeb_core + NET flash_clk_oeb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 1824615 209765 ) N ;
   - flash_csb_core + NET flash_csb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 1534975 209765 ) N ;
   - gpio_outenb_core + NET gpio_outenb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2646615 209765 ) N ;
   - gpio_out_core + NET gpio_out_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2630975 209765 ) N ;
   - gpio_mode0_core + NET gpio_mode0_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2603375 209765 ) N ;
   - gpio_in_core + NET gpio_in_core
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2575775 209765 ) N ;
   - flash_io1_oeb_core + NET flash_io1_oeb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2372615 209765 ) N ;
   - flash_io1_ieb_core + NET flash_io1_ieb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2335355 209765 ) N ;
   - flash_io1_do_core + NET flash_io1_do_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2356975 209765 ) N ;
   - flash_io1_di_core + NET flash_io1_di_core
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2301775 209765 ) N ;
   - flash_io0_oeb_core + NET flash_io0_oeb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2098615 209765 ) N ;
   - flash_io0_ieb_core + NET flash_io0_ieb_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2061355 209765 ) N ;
   - flash_io0_do_core + NET flash_io0_do_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2082975 209765 ) N ;
   - flash_io0_di_core + NET flash_io0_di_core
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2027775 209765 ) N ;
   - por + NET por
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 970355 209765 ) N ;
   - clock_core + NET clock_core
     + DIRECTION INOUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 936775 209765 ) N ;
   - gpio_mode1_core + NET gpio_mode1_core
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 2624995 209930 ) N ;
   - mprj_io_one[0] + NET mprj_io_one[0]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 510755 ) N ;
   - mprj_io_one[1] + NET mprj_io_one[1]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 736755 ) N ;
   - mprj_io_one[2] + NET mprj_io_one[2]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 961755 ) N ;
   - mprj_io_one[3] + NET mprj_io_one[3]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1187755 ) N ;
   - mprj_io_one[4] + NET mprj_io_one[4]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1412755 ) N ;
   - mprj_io_one[5] + NET mprj_io_one[5]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1637755 ) N ;
   - mprj_io_one[6] + NET mprj_io_one[6]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 1863755 ) N ;
   - mprj_io_one[7] + NET mprj_io_one[7]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2749755 ) N ;
   - mprj_io_one[8] + NET mprj_io_one[8]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 2975755 ) N ;
   - mprj_io_one[9] + NET mprj_io_one[9]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3200755 ) N ;
   - mprj_io_one[10] + NET mprj_io_one[10]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3426755 ) N ;
   - mprj_io_one[11] + NET mprj_io_one[11]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3651755 ) N ;
   - mprj_io_one[12] + NET mprj_io_one[12]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 3876755 ) N ;
   - mprj_io_one[13] + NET mprj_io_one[13]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 3378235 4322755 ) N ;
   - mprj_io_one[14] + NET mprj_io_one[14]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3991245 ) N ;
   - mprj_io_one[15] + NET mprj_io_one[15]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3775245 ) N ;
   - mprj_io_one[16] + NET mprj_io_one[16]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3559245 ) N ;
   - mprj_io_one[17] + NET mprj_io_one[17]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3343245 ) N ;
   - mprj_io_one[18] + NET mprj_io_one[18]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 3127245 ) N ;
   - mprj_io_one[19] + NET mprj_io_one[19]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2911245 ) N ;
   - mprj_io_one[20] + NET mprj_io_one[20]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2695245 ) N ;
   - mprj_io_one[21] + NET mprj_io_one[21]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 2057245 ) N ;
   - mprj_io_one[22] + NET mprj_io_one[22]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1841245 ) N ;
   - mprj_io_one[23] + NET mprj_io_one[23]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1625245 ) N ;
   - mprj_io_one[24] + NET mprj_io_one[24]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1409245 ) N ;
   - mprj_io_one[25] + NET mprj_io_one[25]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 1193245 ) N ;
   - mprj_io_one[26] + NET mprj_io_one[26]
     + PORT
        + LAYER met2 ( -1200 -140 ) ( 1200 140 )        + PLACED ( 209765 977245 ) N ;
   - porb_h + NET porb_h
     + DIRECTION INPUT
     + USE SIGNAL
     + PORT
        + LAYER met2 ( -140 -1200 ) ( 140 1200 )        + PLACED ( 1541415 209930 ) N ;
   - vccd + NET vccd
     + PORT
        + LAYER met4 ( -2725 -635 ) ( 2725 635 )        + PLACED ( 195240 2278365 ) N ;
   - vddio + NET vddio
     + PORT
        + LAYER met4 ( -1725 -635 ) ( 1725 635 )        + PLACED ( 166390 2278365 ) N ;
   - vssa + NET vssa
     + PORT
        + LAYER met4 ( -37500 -165 ) ( 37500 165 )        + PLACED ( 700500 143430 ) N ;
   - vssd + NET vssd
     + PORT
        + LAYER met4 ( -635 -2325 ) ( 635 2325 )        + PLACED ( 663635 156090 ) N ;
   - vssio + NET vssio
     + PORT
        + LAYER met4 ( -12107.5 -1122.5 ) ( 12107.5 1122.5 )        + PLACED ( 12107.5 2279347.5 ) N ;
END PINS

NONDEFAULTRULES 98 ;
  - met2_width_205
     + LAYER met2 WIDTH 205 ;
  - met4_width_670
     + LAYER met4 WIDTH 670 ;
  - met3_width_545
     + LAYER met3 WIDTH 545 ;
  - met4_width_490
     + LAYER met4 WIDTH 490 ;
  - met4_width_650
     + LAYER met4 WIDTH 650 ;
  - met4_width_480
     + LAYER met4 WIDTH 480 ;
  - met4_width_640
     + LAYER met4 WIDTH 640 ;
  - met4_width_1270
     + LAYER met4 WIDTH 1270 ;
  - met4_width_470
     + LAYER met4 WIDTH 470 ;
  - met3_width_16650
     + LAYER met3 WIDTH 16650 ;
  - met4_width_460
     + LAYER met4 WIDTH 460 ;
  - met4_width_630
     + LAYER met4 WIDTH 630 ;
  - met4_width_620
     + LAYER met4 WIDTH 620 ;
  - met4_width_450
     + LAYER met4 WIDTH 450 ;
  - met3_width_18010
     + LAYER met3 WIDTH 18010 ;
  - met2_width_180
     + LAYER met2 WIDTH 180 ;
  - met4_width_600
     + LAYER met4 WIDTH 600 ;
  - met2_width_330
     + LAYER met2 WIDTH 330 ;
  - met2_width_160
     + LAYER met2 WIDTH 160 ;
  - met3_width_840
     + LAYER met3 WIDTH 840 ;
  - met3_width_16600
     + LAYER met3 WIDTH 16600 ;
  - met3_width_670
     + LAYER met3 WIDTH 670 ;
  - met5_width_62450
     + LAYER met5 WIDTH 62450 ;
  - met2_width_375
     + LAYER met2 WIDTH 375 ;
  - met2_width_320
     + LAYER met2 WIDTH 320 ;
  - met2_width_150
     + LAYER met2 WIDTH 150 ;
  - met3_width_660
     + LAYER met3 WIDTH 660 ;
  - met2_width_195
     + LAYER met2 WIDTH 195 ;
  - met3_width_650
     + LAYER met3 WIDTH 650 ;
  - met2_width_23900
     + LAYER met2 WIDTH 23900 ;
  - met3_width_470
     + LAYER met3 WIDTH 470 ;
  - met2_width_345
     + LAYER met2 WIDTH 345 ;
  - met3_width_800
     + LAYER met3 WIDTH 800 ;
  - met3_width_630
     + LAYER met3 WIDTH 630 ;
  - met5_width_54400
     + LAYER met5 WIDTH 54400 ;
  - met3_width_620
     + LAYER met3 WIDTH 620 ;
  - met4_width_960
     + LAYER met4 WIDTH 960 ;
  - met1_width_190
     + LAYER met1 WIDTH 190 ;
  - met4_width_790
     + LAYER met4 WIDTH 790 ;
  - met5_width_37180
     + LAYER met5 WIDTH 37180 ;
  - met5_width_13000
     + LAYER met5 WIDTH 13000 ;
  - met5_width_60820
     + LAYER met5 WIDTH 60820 ;
  - met4_width_590
     + LAYER met4 WIDTH 590 ;
  - met5_width_2040
     + LAYER met5 WIDTH 2040 ;
  - met4_width_580
     + LAYER met4 WIDTH 580 ;
  - met4_width_740
     + LAYER met4 WIDTH 740 ;
  - met4_width_570
     + LAYER met4 WIDTH 570 ;
  - met3_width_16750
     + LAYER met3 WIDTH 16750 ;
  - met4_width_730
     + LAYER met4 WIDTH 730 ;
  - met3_width_605
     + LAYER met3 WIDTH 605 ;
  - met4_width_560
     + LAYER met4 WIDTH 560 ;
  - met4_width_550
     + LAYER met4 WIDTH 550 ;
  - met4_width_710
     + LAYER met4 WIDTH 710 ;
  - met4_width_540
     + LAYER met4 WIDTH 540 ;
  - met2_width_280
     + LAYER met2 WIDTH 280 ;
  - met3_width_960
     + LAYER met3 WIDTH 960 ;
  - met3_width_16550
     + LAYER met3 WIDTH 16550 ;
  - met4_width_530
     + LAYER met4 WIDTH 530 ;
  - met4_width_700
     + LAYER met4 WIDTH 700 ;
  - met4_width_2245
     + LAYER met4 WIDTH 2245 ;
  - met3_width_16380
     + LAYER met3 WIDTH 16380 ;
  - met3_width_16710
     + LAYER met3 WIDTH 16710 ;
  - met3_width_15680
     + LAYER met3 WIDTH 15680 ;
  - met4_width_520
     + LAYER met4 WIDTH 520 ;
  - met3_width_2040
     + LAYER met3 WIDTH 2040 ;
  - met2_width_260
     + LAYER met2 WIDTH 260 ;
  - met3_width_940
     + LAYER met3 WIDTH 940 ;
  - met3_width_17050
     + LAYER met3 WIDTH 17050 ;
  - met3_width_16190
     + LAYER met3 WIDTH 16190 ;
  - met3_width_590
     + LAYER met3 WIDTH 590 ;
  - met4_width_500
     + LAYER met4 WIDTH 500 ;
  - met4_width_330
     + LAYER met4 WIDTH 330 ;
  - met3_width_1160
     + LAYER met3 WIDTH 1160 ;
  - met2_width_2050
     + LAYER met2 WIDTH 2050 ;
  - met3_width_740
     + LAYER met3 WIDTH 740 ;
  - met3_width_570
     + LAYER met3 WIDTH 570 ;
  - met3_width_17020
     + LAYER met3 WIDTH 17020 ;
  - met2_width_220
     + LAYER met2 WIDTH 220 ;
  - met3_width_730
     + LAYER met3 WIDTH 730 ;
  - met3_width_560
     + LAYER met3 WIDTH 560 ;
  - met2_width_265
     + LAYER met2 WIDTH 265 ;
  - met3_width_25000
     + LAYER met3 WIDTH 25000 ;
  - met3_width_710
     + LAYER met3 WIDTH 710 ;
  - met3_width_595
     + LAYER met3 WIDTH 595 ;
  - met2_width_245
     + LAYER met2 WIDTH 245 ;
  - met3_width_585
     + LAYER met3 WIDTH 585 ;
  - met3_width_700
     + LAYER met3 WIDTH 700 ;
  - met3_width_360
     + LAYER met3 WIDTH 360 ;
  - met3_width_520
     + LAYER met3 WIDTH 520 ;
  - met1_width_260
     + LAYER met1 WIDTH 260 ;
  - met3_width_16880
     + LAYER met3 WIDTH 16880 ;
  - met3_width_350
     + LAYER met3 WIDTH 350 ;
  - met4_width_690
     + LAYER met4 WIDTH 690 ;
  - met3_width_565
     + LAYER met3 WIDTH 565 ;
  - met3_width_510
     + LAYER met3 WIDTH 510 ;
  - met4_width_680
     + LAYER met4 WIDTH 680 ;
  - met3_width_500
     + LAYER met3 WIDTH 500 ;
  - met3_width_16690
     + LAYER met3 WIDTH 16690 ;
END NONDEFAULTRULES

NETS 777 ;
   - vssd2 ( user2_vccd_lvclamp_pad VSSD1 )
       ( user2_vssd_lvclamp_pad VSSD1 )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 211480 892940 ) ( * 2204270 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 2228670 ) ( * 2254540 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 2278940 ) ( * 4585710 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 4609410 ) ( * 4635320 )
      NEW met4 TAPERRULE met4_width_620  ( 205170 4608920 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_650  ( 217685 4586660 ) ( * 4608460 )
      NEW met4 TAPERRULE met4_width_460  ( 205170 4586280 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_490  ( 205265 4586660 ) ( * 4608460 )
      NEW met4  ( 211435 4597560 ) via4_11850_22100 
      NEW met3 TAPERRULE met3_width_650  ( 203620 4608935 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_16550  ( 225635 4586660 ) ( * 4608460 )
      NEW met3 TAPERRULE met3_width_560  ( 203620 4586230 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_2040  ( 204490 4586660 ) ( * 4608460 )
      NEW met3  ( 211435 4597560 ) via3_11850_22100_hx 
      NEW met4 TAPERRULE met4_width_480  ( 205140 2278380 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_450  ( 217695 2255490 ) ( * 2277990 )
      NEW met4 TAPERRULE met4_width_600  ( 205140 2255040 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_550  ( 205265 2255490 ) ( * 2277990 )
      NEW met4  ( 211505 2266740 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_560  ( 204850 2278420 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16650  ( 225795 2255490 ) ( * 2277990 )
      NEW met3 TAPERRULE met3_width_585  ( 204850 2255047.5 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_840  ( 205120 2255490 ) ( * 2277990 )
      NEW met3  ( 211505 2266740 ) via3_11930_22800_hx 
      NEW met4 TAPERRULE met4_width_580  ( 205110 2228160 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_460  ( 217660 2205220 ) ( * 2227720 )
      NEW met4 TAPERRULE met4_width_500  ( 205110 2204820 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_540  ( 205230 2205220 ) ( * 2227720 )
      NEW met4  ( 211465 2216470 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_630  ( 204850 2228185 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16690  ( 225775 2205220 ) ( * 2227720 )
      NEW met3 TAPERRULE met3_width_570  ( 204850 2204785 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_800  ( 205100 2205220 ) ( * 2227720 )
      NEW met3  ( 211465 2216470 ) via3_11930_22800_hx  ;
   - clock_pad/OE_N ( clock_pad OE_N ) ( clock_pad DM[0] )
       ( constant_block_1 one ) ( clock_pad ENABLE_VDDIO )
      + ROUTED met2  ( 1007600 210355 ) via_260_260_hv 
      NEW met2  ( 1007540 210445 ) ( 1007660 * )
      NEW met1 TAPERRULE met1_width_260  ( 964555 210355 ) ( 1007400 * )
      NEW met1  ( 964355 210355 ) via_260_260_hv  ( * 210445 )
       ( 964415 * )
      NEW met1 TAPERRULE met1_width_260  ( 942940 210355 ) ( 964155 * )
      NEW met1  ( 942740 210355 ) via_260_260_hv  ( * 210445 )
       ( 942800 * )
      NEW met1 TAPERRULE met1_width_260  ( 932810 210355 ) ( 942540 * )
      NEW met2  ( 942680 210265 ) ( 942800 * )
      NEW met2  ( 964295 210265 ) ( 964415 * )
      NEW met2  ( 1007540 210265 ) ( 1007660 * )
      NEW met1 TAPERRULE met1_width_260  ( 1007800 210355 ) ( 1013715 * ) via_260_260_hv 
       ( * 210445 ) ( 1013775 * )
      NEW met2 TAPERRULE met2_width_260  ( 1013715 204760 ) ( * 210155 )
      NEW met2  ( 1013635 204620 ) ( 1013795 * )
      NEW met2  ( 1013715 204495 ) via2_300_300_vx 
      NEW met3  ( 1013690 204520 ) ( 1013740 * )
      NEW met3  ( 1014015 204495 ) ( 1015170 * )
      NEW met3  ( 1013690 204470 ) ( 1013740 * )
      NEW met3  ( 1013690 204495 ) ( 1013415 * )
      NEW met2  ( 1013635 204370 ) ( 1013795 * ) ;
   - mprj_io[13] ( mprj_pads.area1_io_pad\[13\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 4319000 ) ( * 4380000 ) ;
   - mprj_pads.area1_io_pad\[13\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[13\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[13\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[13\] ENABLE_INP_H ) ;
   - mprj_io_in[13] ( mprj_pads.area1_io_pad\[13\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4316775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[13\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[13\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[13\] TIE_HI_ESD ) ;
   - mprj_io_one[13] ( mprj_pads.area1_io_pad\[13\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4322755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[13] ( mprj_pads.area1_io_pad\[13\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4325975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[6]
       ( mprj_pads.area1_io_pad\[13\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4329195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[13\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[13\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[40] ( mprj_pads.area1_io_pad\[13\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4335175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[6] ( mprj_pads.area1_io_pad\[13\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4338395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[13] ( mprj_pads.area1_io_pad\[13\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4341155 ) ( 3379365 * ) ;
   - mprj_io_dm[39] ( mprj_pads.area1_io_pad\[13\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4344375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[13]
       ( mprj_pads.area1_io_pad\[13\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4347595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[13] ( mprj_pads.area1_io_pad\[13\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4350355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[13\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[13\] ENABLE_H ) ;
   - mprj_io_analog_sel[13]
       ( mprj_pads.area1_io_pad\[13\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4362775 ) ( 3379365 * ) ;
   - mprj_io_dm[41] ( mprj_pads.area1_io_pad\[13\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4365995 ) ( 3379365 * ) ;
   - mprj_io_holdover[13] ( mprj_pads.area1_io_pad\[13\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4369215 ) ( 3379365 * ) ;
   - mprj_io_out[13] ( mprj_pads.area1_io_pad\[13\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4371975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[13\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[13\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[13] ( mprj_pads.area1_io_pad\[13\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4381175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[13]
       ( mprj_pads.area1_io_pad\[13\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4384395 ) ( 3379365 * ) ;
   - mprj_io_oeb[13] ( mprj_pads.area1_io_pad\[13\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4387615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[13] ( mprj_pads.area1_io_pad\[13\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 4390375 ) ( 3379365 * ) ;
   - vccd1_pad ( user1_vccd_lvclamp_pad VCCD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 3490700 4575530 ) ( 3556360 * ) ;
   - flash_clk ( flash_clk_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 1756000 64215 ) ( 1817000 * ) ;
   - flash_clk_pad/TIE_LO_ESD ( flash_clk_pad TIE_LO_ESD )
       ( flash_clk_pad ENABLE_VSWITCH_H )
       ( flash_clk_pad ENABLE_INP_H )
      + ROUTED met2  ( 1750560 209095 ) via_260_260_hv 
      NEW met2  ( 1750500 209185 ) ( 1750620 * )
      NEW met1 TAPERRULE met1_width_260  ( 1749880 209095 ) ( 1750360 * )
      NEW met2  ( 1750500 209005 ) ( 1750620 * )
      NEW met1 TAPERRULE met1_width_260  ( 1750760 209095 ) ( 1790580 * ) via_260_260_hv 
       ( * 209185 ) ( 1790640 * )
      NEW met2  ( 1790520 209005 ) ( 1790640 * )
      NEW met1 TAPERRULE met1_width_260  ( 1790780 209095 ) ( 1812190 * ) via_260_260_hv 
       ( * 209185 ) ( 1812250 * )
      NEW met2  ( 1812130 209005 ) ( 1812250 * )
      NEW met1 TAPERRULE met1_width_260  ( 1812390 209095 ) ( 1828065 * ) ;
   - flash_clk_pad/IN ( flash_clk_pad IN ) ;
   - flash_clk_pad/HLD_H_N ( flash_clk_pad HLD_H_N )
       ( flash_clk_pad TIE_HI_ESD )
      + ROUTED met2  ( 1797000 209515 ) via_260_260_hv 
      NEW met2  ( 1796940 209605 ) ( 1797060 * )
      NEW met1 TAPERRULE met1_width_260  ( 1757205 209515 ) ( 1796800 * )
      NEW met1  ( 1757005 209515 ) via_260_260_hv  ( * 209605 )
       ( 1757065 * )
      NEW met1 TAPERRULE met1_width_260  ( 1749880 209515 ) ( 1756805 * )
      NEW met2  ( 1756945 209425 ) ( 1757065 * )
      NEW met2  ( 1796940 209425 ) ( 1797060 * )
      NEW met1 TAPERRULE met1_width_260  ( 1797200 209515 ) ( 1828065 * ) ;
   - flash_clk_pad/SLOW ( flash_clk_pad SLOW )
       ( constant_block_3 zero ) ( flash_clk_pad IB_MODE_SEL )
       ( flash_clk_pad VTRIP_SEL ) ( flash_clk_pad HLD_OVR )
       ( flash_clk_pad ANALOG_SEL ) ( flash_clk_pad INP_DIS )
       ( flash_clk_pad ANALOG_POL ) ( flash_clk_pad DM[0] )
       ( flash_clk_pad ANALOG_EN )
      + ROUTED met2  ( 1762970 209935 ) via_260_260_hv 
      NEW met2  ( 1762910 210025 ) ( 1763030 * )
      NEW met1 TAPERRULE met1_width_260  ( 1749880 209935 ) ( 1762770 * )
      NEW met2  ( 1762910 209845 ) ( 1763030 * )
      NEW met1 TAPERRULE met1_width_260  ( 1763170 209935 ) ( 1778130 * ) via_260_260_hv 
       ( * 210025 ) ( 1778190 * )
      NEW met2  ( 1778070 209845 ) ( 1778190 * )
      NEW met1 TAPERRULE met1_width_260  ( 1778330 209935 ) ( 1781360 * ) via_260_260_hv 
       ( * 210025 ) ( 1781420 * )
      NEW met2  ( 1781300 209845 ) ( 1781420 * )
      NEW met1 TAPERRULE met1_width_260  ( 1781560 209935 ) ( 1784575 * ) via_260_260_hv 
       ( * 210025 ) ( 1784635 * )
      NEW met2  ( 1784515 209845 ) ( 1784635 * )
      NEW met1 TAPERRULE met1_width_260  ( 1784775 209935 ) ( 1787350 * ) via_260_260_hv 
       ( * 210025 ) ( 1787410 * )
      NEW met2  ( 1787290 209845 ) ( 1787410 * )
      NEW met1 TAPERRULE met1_width_260  ( 1787550 209935 ) ( 1799770 * ) via_260_260_hv 
       ( * 210025 ) ( 1799830 * )
      NEW met2  ( 1799710 209845 ) ( 1799830 * )
      NEW met1 TAPERRULE met1_width_260  ( 1799970 209935 ) ( 1806215 * ) via_260_260_hv 
       ( * 210025 ) ( 1806275 * )
      NEW met2  ( 1806155 209845 ) ( 1806275 * )
      NEW met1 TAPERRULE met1_width_260  ( 1806415 209935 ) ( 1818165 * ) via_260_260_hv 
       ( * 210025 ) ( 1818225 * )
      NEW met2  ( 1818105 209845 ) ( 1818225 * )
      NEW met1 TAPERRULE met1_width_260  ( 1818365 209935 ) ( 1821390 * ) via_260_260_hv 
       ( * 210025 ) ( 1821450 * )
      NEW met2  ( 1821330 209845 ) ( 1821450 * )
      NEW met1 TAPERRULE met1_width_260  ( 1821590 209935 ) ( 1851770 * ) via_260_260_hv 
       ( * 210025 ) ( 1851830 * )
      NEW met2 TAPERRULE met2_width_260  ( 1851770 204725 ) ( * 209735 )
      NEW met2  ( 1851690 204585 ) ( 1851850 * )
      NEW met2  ( 1851770 204460 ) via2_300_300_vx 
      NEW met3  ( 1850930 204470 ) ( 1851795 * )
      NEW met3  ( 1851745 204485 ) ( 1851795 * )
      NEW met3  ( 1852070 204460 ) ( 1851795 * )
      NEW met3  ( 1851745 204435 ) ( 1851795 * )
      NEW met3  ( 1850930 204470 ) ( 1851470 * )
      NEW met2  ( 1851690 204335 ) ( 1851850 * ) ;
   - flash_clk_pad/PAD_A_ESD_0_H ( flash_clk_pad PAD_A_ESD_0_H ) ;
   - flash_clk_pad/PAD_A_ESD_1_H ( flash_clk_pad PAD_A_ESD_1_H ) ;
   - flash_clk_pad/PAD_A_NOESD_H ( flash_clk_pad PAD_A_NOESD_H ) ;
   - flash_clk_core ( flash_clk_pad OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 1808975 208635 ) ( * 210895 ) ;
   - flash_clk_oeb_core ( flash_clk_pad OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 1824615 208635 ) ( * 210895 ) ;
   - flash_clk_pad/IN_H ( flash_clk_pad IN_H ) ;
   - constant_block_0/zero ( constant_block_0 zero ) ;
   - mprj_io[9] ( mprj_pads.area1_io_pad\[9\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 3197000 ) ( * 3258000 ) ;
   - mprj_pads.area1_io_pad\[9\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[9\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[9\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[9\] ENABLE_INP_H ) ;
   - mprj_io_in[9] ( mprj_pads.area1_io_pad\[9\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3194775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[9\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[9\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[9\] TIE_HI_ESD ) ;
   - mprj_io_one[9] ( mprj_pads.area1_io_pad\[9\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3200755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[9] ( mprj_pads.area1_io_pad\[9\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3203975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[2] ( mprj_pads.area1_io_pad\[9\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3207195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[9\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[9\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[28] ( mprj_pads.area1_io_pad\[9\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3213175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[2] ( mprj_pads.area1_io_pad\[9\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3216395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[9] ( mprj_pads.area1_io_pad\[9\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3219155 ) ( 3379365 * ) ;
   - mprj_io_dm[27] ( mprj_pads.area1_io_pad\[9\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3222375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[9] ( mprj_pads.area1_io_pad\[9\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3225595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[9] ( mprj_pads.area1_io_pad\[9\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3228355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[9\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[9\] ENABLE_H ) ;
   - mprj_io_analog_sel[9] ( mprj_pads.area1_io_pad\[9\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3240775 ) ( 3379365 * ) ;
   - mprj_io_dm[29] ( mprj_pads.area1_io_pad\[9\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3243995 ) ( 3379365 * ) ;
   - mprj_io_holdover[9] ( mprj_pads.area1_io_pad\[9\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3247215 ) ( 3379365 * ) ;
   - mprj_io_out[9] ( mprj_pads.area1_io_pad\[9\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3249975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[9\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[9\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[9] ( mprj_pads.area1_io_pad\[9\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3259175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[9]
       ( mprj_pads.area1_io_pad\[9\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3262395 ) ( 3379365 * ) ;
   - mprj_io_oeb[9] ( mprj_pads.area1_io_pad\[9\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3265615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[9] ( mprj_pads.area1_io_pad\[9\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3268375 ) ( 3379365 * ) ;
   - vssa1_pad ( user1_vssa_hvclamp_pad\[0\] VSSA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 2885850 5123530 ) ( 2945090 * ) ;
   - vdda1 ( user1_corner VDDA ) ( FILLER_147 VDDA )
       ( FILLER_146 VDDA ) ( FILLER_145 VDDA ) ( FILLER_144 VDDA )
       ( FILLER_143 VDDA ) ( FILLER_142 VDDA ) ( FILLER_141 VDDA )
       ( FILLER_140 VDDA ) ( FILLER_139 VDDA ) ( FILLER_138 VDDA )
       ( FILLER_137 VDDA ) ( FILLER_136 VDDA ) ( FILLER_135 VDDA )
       ( user1_analog_pad\[0\] VDDA ) ( FILLER_133 VDDA )
       ( FILLER_132 VDDA ) ( FILLER_131 VDDA ) ( FILLER_130 VDDA )
       ( FILLER_129 VDDA ) ( FILLER_128 VDDA ) ( FILLER_127 VDDA )
       ( FILLER_126 VDDA ) ( FILLER_125 VDDA ) ( FILLER_124 VDDA )
       ( FILLER_123 VDDA ) ( user1_vssa_hvclamp_pad\[0\] VDDA )
       ( FILLER_121 VDDA ) ( FILLER_120 VDDA ) ( FILLER_119 VDDA )
       ( FILLER_118 VDDA ) ( FILLER_117 VDDA ) ( FILLER_116 VDDA )
       ( FILLER_115 VDDA ) ( FILLER_114 VDDA ) ( FILLER_113 VDDA )
       ( FILLER_112 VDDA ) ( FILLER_111 VDDA ) ( FILLER_110 VDDA )
       ( user1_analog_pad\[1\] VDDA ) ( FILLER_108 VDDA )
       ( FILLER_107 VDDA ) ( FILLER_106 VDDA ) ( FILLER_105 VDDA )
       ( FILLER_104 VDDA ) ( FILLER_103 VDDA ) ( FILLER_102 VDDA )
       ( FILLER_101 VDDA ) ( FILLER_100 VDDA ) ( FILLER_99 VDDA )
       ( FILLER_98 VDDA ) ( user1_analog_pad\[2\] VDDA )
       ( FILLER_96 VDDA ) ( FILLER_95 VDDA ) ( FILLER_94 VDDA )
       ( FILLER_93 VDDA ) ( FILLER_92 VDDA ) ( FILLER_91 VDDA )
       ( FILLER_90 VDDA ) ( FILLER_89 VDDA ) ( FILLER_88 VDDA )
       ( FILLER_87 VDDA ) ( FILLER_86 VDDA ) ( FILLER_85 VDDA )
       ( FILLER_84 VDDA ) ( FILLER_83 VDDA ) ( FILLER_82 VDDA )
       ( FILLER_81 VDDA ) ( FILLER_80 VDDA ) ( FILLER_79 VDDA )
       ( sky130_ef_io__com_bus_slice_10um_0 VDDA ) ( FILLER_78 VDDA )
       ( sky130_ef_io__com_bus_slice_5um_1 VDDA )
       ( user1_analog_pad_with_clamp VDDA )
       ( sky130_ef_io__com_bus_slice_5um_0 VDDA ) ( FILLER_SB3 VDDA )
       ( FILLER_786 VDDA ) ( FILLER_785 VDDA ) ( FILLER_784 VDDA )
       ( FILLER_783 VDDA ) ( FILLER_782 VDDA ) ( FILLER_781 VDDA )
       ( FILLER_780 VDDA ) ( FILLER_779 VDDA )
       ( user1_analog_pad\[3\] VDDA ) ( FILLER_776 VDDA )
       ( FILLER_777 VDDA ) ( FILLER_775 VDDA ) ( FILLER_774 VDDA )
       ( FILLER_773 VDDA ) ( FILLER_772 VDDA ) ( FILLER_771 VDDA )
       ( FILLER_770 VDDA ) ( FILLER_769 VDDA )
       ( user1_vccd_lvclamp_pad VDDA ) ( FILLER_767 VDDA )
       ( FILLER_766 VDDA ) ( FILLER_765 VDDA ) ( FILLER_764 VDDA )
       ( FILLER_763 VDDA ) ( FILLER_762 VDDA ) ( FILLER_761 VDDA )
       ( FILLER_760 VDDA ) ( mprj_pads.area1_io_pad\[13\] VDDA )
       ( FILLER_759 VDDA ) ( FILLER_757 VDDA ) ( FILLER_756 VDDA )
       ( FILLER_755 VDDA ) ( FILLER_754 VDDA ) ( FILLER_753 VDDA )
       ( FILLER_752 VDDA ) ( FILLER_751 VDDA )
       ( user1_vdda_hvclamp_pad\[0\] VDDA ) ( FILLER_750 VDDA )
       ( FILLER_748 VDDA ) ( FILLER_747 VDDA ) ( FILLER_746 VDDA )
       ( FILLER_745 VDDA ) ( FILLER_744 VDDA ) ( FILLER_743 VDDA )
       ( FILLER_742 VDDA ) ( FILLER_741 VDDA ) ( FILLER_740 VDDA )
       ( mprj_pads.area1_io_pad\[12\] VDDA ) ( FILLER_738 VDDA )
       ( FILLER_737 VDDA ) ( FILLER_736 VDDA ) ( FILLER_735 VDDA )
       ( FILLER_734 VDDA ) ( FILLER_733 VDDA ) ( FILLER_732 VDDA )
       ( mprj_pads.area1_io_pad\[11\] VDDA ) ( FILLER_731 VDDA )
       ( FILLER_729 VDDA ) ( FILLER_728 VDDA ) ( FILLER_727 VDDA )
       ( FILLER_726 VDDA ) ( FILLER_725 VDDA ) ( FILLER_724 VDDA )
       ( FILLER_723 VDDA ) ( FILLER_722 VDDA )
       ( mprj_pads.area1_io_pad\[10\] VDDA ) ( FILLER_720 VDDA )
       ( FILLER_719 VDDA ) ( FILLER_718 VDDA ) ( FILLER_717 VDDA )
       ( FILLER_716 VDDA ) ( FILLER_715 VDDA ) ( FILLER_714 VDDA )
       ( FILLER_713 VDDA ) ( FILLER_712 VDDA )
       ( mprj_pads.area1_io_pad\[9\] VDDA ) ( FILLER_710 VDDA )
       ( FILLER_709 VDDA ) ( FILLER_708 VDDA ) ( FILLER_707 VDDA )
       ( FILLER_706 VDDA ) ( FILLER_705 VDDA ) ( FILLER_704 VDDA )
       ( FILLER_703 VDDA ) ( mprj_pads.area1_io_pad\[8\] VDDA )
       ( FILLER_701 VDDA ) ( FILLER_700 VDDA ) ( FILLER_699 VDDA )
       ( FILLER_698 VDDA ) ( FILLER_697 VDDA ) ( FILLER_696 VDDA )
       ( FILLER_695 VDDA ) ( FILLER_694 VDDA ) ( FILLER_693 VDDA )
       ( mprj_pads.area1_io_pad\[7\] VDDA ) ( FILLER_691 VDDA )
       ( FILLER_690 VDDA ) ( FILLER_689 VDDA ) ( FILLER_688 VDDA )
       ( FILLER_687 VDDA ) ( FILLER_686 VDDA ) ( FILLER_685 VDDA )
       ( FILLER_684 VDDA ) ( user1_vdda_hvclamp_pad\[1\] VDDA )
       ( FILLER_682 VDDA ) ( FILLER_681 VDDA ) ( FILLER_680 VDDA )
       ( FILLER_679 VDDA ) ( FILLER_678 VDDA ) ( FILLER_677 VDDA )
       ( FILLER_676 VDDA ) ( FILLER_675 VDDA )
       ( user1_vssd_lvclamp_pad VDDA ) ( FILLER_673 VDDA )
       ( FILLER_SB1 VDDA ) ( FILLER_672 VDDA ) ( FILLER_671 VDDA )
       ( FILLER_670 VDDA ) ( FILLER_669 VDDA ) ( FILLER_668 VDDA )
       ( FILLER_667 VDDA ) ( FILLER_666 VDDA ) ( FILLER_665 VDDA )
       ( user1_vssa_hvclamp_pad\[1\] VDDA ) ( FILLER_663 VDDA )
       ( FILLER_662 VDDA ) ( FILLER_661 VDDA ) ( FILLER_660 VDDA )
       ( FILLER_659 VDDA ) ( FILLER_658 VDDA ) ( FILLER_657 VDDA )
       ( FILLER_656 VDDA ) ( mprj_pads.area1_io_pad\[6\] VDDA )
       ( FILLER_654 VDDA ) ( FILLER_653 VDDA ) ( FILLER_652 VDDA )
       ( FILLER_651 VDDA ) ( FILLER_650 VDDA ) ( FILLER_649 VDDA )
       ( FILLER_648 VDDA ) ( FILLER_647 VDDA ) ( FILLER_646 VDDA )
       ( mprj_pads.area1_io_pad\[5\] VDDA ) ( FILLER_644 VDDA )
       ( FILLER_643 VDDA ) ( FILLER_642 VDDA ) ( FILLER_641 VDDA )
       ( FILLER_640 VDDA ) ( FILLER_639 VDDA ) ( FILLER_638 VDDA )
       ( FILLER_637 VDDA ) ( mprj_pads.area1_io_pad\[4\] VDDA )
       ( FILLER_635 VDDA ) ( FILLER_634 VDDA ) ( FILLER_633 VDDA )
       ( FILLER_632 VDDA ) ( FILLER_631 VDDA ) ( FILLER_630 VDDA )
       ( FILLER_629 VDDA ) ( FILLER_628 VDDA )
       ( mprj_pads.area1_io_pad\[3\] VDDA ) ( FILLER_626 VDDA )
       ( FILLER_625 VDDA ) ( FILLER_624 VDDA ) ( FILLER_623 VDDA )
       ( FILLER_622 VDDA ) ( FILLER_621 VDDA ) ( FILLER_620 VDDA )
       ( FILLER_619 VDDA ) ( FILLER_618 VDDA )
       ( mprj_pads.area1_io_pad\[2\] VDDA ) ( FILLER_616 VDDA )
       ( FILLER_615 VDDA ) ( FILLER_614 VDDA ) ( FILLER_613 VDDA )
       ( FILLER_612 VDDA ) ( FILLER_611 VDDA ) ( FILLER_610 VDDA )
       ( FILLER_609 VDDA ) ( mprj_pads.area1_io_pad\[1\] VDDA )
       ( FILLER_607 VDDA ) ( FILLER_606 VDDA ) ( FILLER_605 VDDA )
       ( FILLER_604 VDDA ) ( FILLER_603 VDDA ) ( FILLER_602 VDDA )
       ( FILLER_601 VDDA ) ( FILLER_600 VDDA )
       ( mprj_pads.area1_io_pad\[0\] VDDA ) ( FILLER_599 VDDA )
       ( FILLER_597 VDDA ) ( FILLER_596 VDDA ) ( FILLER_595 VDDA )
       ( FILLER_594 VDDA ) ( FILLER_593 VDDA ) ( FILLER_592 VDDA )
       ( FILLER_591 VDDA ) ( FILLER_590 VDDA )
      + ROUTED met4 TAPERRULE met4_width_960  ( 3403085 2299480 ) ( 3406235 * ) ;
   - vssa1 ( user1_corner VSSA ) ( FILLER_147 VSSA )
       ( FILLER_146 VSSA ) ( FILLER_145 VSSA ) ( FILLER_144 VSSA )
       ( FILLER_143 VSSA ) ( FILLER_142 VSSA ) ( FILLER_141 VSSA )
       ( FILLER_140 VSSA ) ( FILLER_139 VSSA ) ( FILLER_138 VSSA )
       ( FILLER_137 VSSA ) ( FILLER_136 VSSA ) ( FILLER_135 VSSA )
       ( user1_analog_pad\[0\] VSSA ) ( FILLER_133 VSSA )
       ( FILLER_132 VSSA ) ( FILLER_131 VSSA ) ( FILLER_130 VSSA )
       ( FILLER_129 VSSA ) ( FILLER_128 VSSA ) ( FILLER_127 VSSA )
       ( FILLER_126 VSSA ) ( FILLER_125 VSSA ) ( FILLER_124 VSSA )
       ( FILLER_123 VSSA ) ( user1_vssa_hvclamp_pad\[0\] VSSA )
       ( FILLER_121 VSSA ) ( FILLER_120 VSSA ) ( FILLER_119 VSSA )
       ( FILLER_118 VSSA ) ( FILLER_117 VSSA ) ( FILLER_116 VSSA )
       ( FILLER_115 VSSA ) ( FILLER_114 VSSA ) ( FILLER_113 VSSA )
       ( FILLER_112 VSSA ) ( FILLER_111 VSSA ) ( FILLER_110 VSSA )
       ( user1_analog_pad\[1\] VSSA ) ( FILLER_108 VSSA )
       ( FILLER_107 VSSA ) ( FILLER_106 VSSA ) ( FILLER_105 VSSA )
       ( FILLER_104 VSSA ) ( FILLER_103 VSSA ) ( FILLER_102 VSSA )
       ( FILLER_101 VSSA ) ( FILLER_100 VSSA ) ( FILLER_99 VSSA )
       ( FILLER_98 VSSA ) ( user1_analog_pad\[2\] VSSA )
       ( FILLER_96 VSSA ) ( FILLER_95 VSSA ) ( FILLER_94 VSSA )
       ( FILLER_93 VSSA ) ( FILLER_92 VSSA ) ( FILLER_91 VSSA )
       ( FILLER_90 VSSA ) ( FILLER_89 VSSA ) ( FILLER_88 VSSA )
       ( FILLER_87 VSSA ) ( FILLER_86 VSSA ) ( FILLER_85 VSSA )
       ( FILLER_84 VSSA ) ( FILLER_83 VSSA ) ( FILLER_82 VSSA )
       ( FILLER_81 VSSA ) ( FILLER_80 VSSA ) ( FILLER_79 VSSA )
       ( sky130_ef_io__com_bus_slice_10um_0 VSSA ) ( FILLER_78 VSSA )
       ( sky130_ef_io__com_bus_slice_5um_1 VSSA )
       ( user1_analog_pad_with_clamp VSSA )
       ( sky130_ef_io__com_bus_slice_5um_0 VSSA ) ( FILLER_SB3 VSSA )
       ( FILLER_786 VSSA ) ( FILLER_785 VSSA ) ( FILLER_784 VSSA )
       ( FILLER_783 VSSA ) ( FILLER_782 VSSA ) ( FILLER_781 VSSA )
       ( FILLER_780 VSSA ) ( FILLER_779 VSSA )
       ( user1_analog_pad\[3\] VSSA ) ( FILLER_776 VSSA )
       ( FILLER_777 VSSA ) ( FILLER_775 VSSA ) ( FILLER_774 VSSA )
       ( FILLER_773 VSSA ) ( FILLER_772 VSSA ) ( FILLER_771 VSSA )
       ( FILLER_770 VSSA ) ( FILLER_769 VSSA )
       ( user1_vccd_lvclamp_pad VSSA ) ( FILLER_767 VSSA )
       ( FILLER_766 VSSA ) ( FILLER_765 VSSA ) ( FILLER_764 VSSA )
       ( FILLER_763 VSSA ) ( FILLER_762 VSSA ) ( FILLER_761 VSSA )
       ( FILLER_760 VSSA ) ( mprj_pads.area1_io_pad\[13\] VSSA )
       ( FILLER_759 VSSA ) ( FILLER_757 VSSA ) ( FILLER_756 VSSA )
       ( FILLER_755 VSSA ) ( FILLER_754 VSSA ) ( FILLER_753 VSSA )
       ( FILLER_752 VSSA ) ( FILLER_751 VSSA )
       ( user1_vdda_hvclamp_pad\[0\] VSSA ) ( FILLER_750 VSSA )
       ( FILLER_748 VSSA ) ( FILLER_747 VSSA ) ( FILLER_746 VSSA )
       ( FILLER_745 VSSA ) ( FILLER_744 VSSA ) ( FILLER_743 VSSA )
       ( FILLER_742 VSSA ) ( FILLER_741 VSSA ) ( FILLER_740 VSSA )
       ( mprj_pads.area1_io_pad\[12\] VSSA ) ( FILLER_738 VSSA )
       ( FILLER_737 VSSA ) ( FILLER_736 VSSA ) ( FILLER_735 VSSA )
       ( FILLER_734 VSSA ) ( FILLER_733 VSSA ) ( FILLER_732 VSSA )
       ( mprj_pads.area1_io_pad\[11\] VSSA ) ( FILLER_731 VSSA )
       ( FILLER_729 VSSA ) ( FILLER_728 VSSA ) ( FILLER_727 VSSA )
       ( FILLER_726 VSSA ) ( FILLER_725 VSSA ) ( FILLER_724 VSSA )
       ( FILLER_723 VSSA ) ( FILLER_722 VSSA )
       ( mprj_pads.area1_io_pad\[10\] VSSA ) ( FILLER_720 VSSA )
       ( FILLER_719 VSSA ) ( FILLER_718 VSSA ) ( FILLER_717 VSSA )
       ( FILLER_716 VSSA ) ( FILLER_715 VSSA ) ( FILLER_714 VSSA )
       ( FILLER_713 VSSA ) ( FILLER_712 VSSA )
       ( mprj_pads.area1_io_pad\[9\] VSSA ) ( FILLER_710 VSSA )
       ( FILLER_709 VSSA ) ( FILLER_708 VSSA ) ( FILLER_707 VSSA )
       ( FILLER_706 VSSA ) ( FILLER_705 VSSA ) ( FILLER_704 VSSA )
       ( FILLER_703 VSSA ) ( mprj_pads.area1_io_pad\[8\] VSSA )
       ( FILLER_701 VSSA ) ( FILLER_700 VSSA ) ( FILLER_699 VSSA )
       ( FILLER_698 VSSA ) ( FILLER_697 VSSA ) ( FILLER_696 VSSA )
       ( FILLER_695 VSSA ) ( FILLER_694 VSSA ) ( FILLER_693 VSSA )
       ( mprj_pads.area1_io_pad\[7\] VSSA ) ( FILLER_691 VSSA )
       ( FILLER_690 VSSA ) ( FILLER_689 VSSA ) ( FILLER_688 VSSA )
       ( FILLER_687 VSSA ) ( FILLER_686 VSSA ) ( FILLER_685 VSSA )
       ( FILLER_684 VSSA ) ( user1_vdda_hvclamp_pad\[1\] VSSA )
       ( FILLER_682 VSSA ) ( FILLER_681 VSSA ) ( FILLER_680 VSSA )
       ( FILLER_679 VSSA ) ( FILLER_678 VSSA ) ( FILLER_677 VSSA )
       ( FILLER_676 VSSA ) ( FILLER_675 VSSA )
       ( user1_vssd_lvclamp_pad VSSA ) ( FILLER_SB1 VSSA )
       ( FILLER_673 VSSA ) ( FILLER_672 VSSA ) ( FILLER_671 VSSA )
       ( FILLER_670 VSSA ) ( FILLER_669 VSSA ) ( FILLER_668 VSSA )
       ( FILLER_667 VSSA ) ( FILLER_666 VSSA ) ( FILLER_665 VSSA )
       ( user1_vssa_hvclamp_pad\[1\] VSSA ) ( FILLER_663 VSSA )
       ( FILLER_662 VSSA ) ( FILLER_661 VSSA ) ( FILLER_660 VSSA )
       ( FILLER_659 VSSA ) ( FILLER_658 VSSA ) ( FILLER_657 VSSA )
       ( FILLER_656 VSSA ) ( mprj_pads.area1_io_pad\[6\] VSSA )
       ( FILLER_654 VSSA ) ( FILLER_653 VSSA ) ( FILLER_652 VSSA )
       ( FILLER_651 VSSA ) ( FILLER_650 VSSA ) ( FILLER_649 VSSA )
       ( FILLER_648 VSSA ) ( FILLER_647 VSSA ) ( FILLER_646 VSSA )
       ( mprj_pads.area1_io_pad\[5\] VSSA ) ( FILLER_644 VSSA )
       ( FILLER_643 VSSA ) ( FILLER_642 VSSA ) ( FILLER_641 VSSA )
       ( FILLER_640 VSSA ) ( FILLER_639 VSSA ) ( FILLER_638 VSSA )
       ( FILLER_637 VSSA ) ( mprj_pads.area1_io_pad\[4\] VSSA )
       ( FILLER_635 VSSA ) ( FILLER_634 VSSA ) ( FILLER_633 VSSA )
       ( FILLER_632 VSSA ) ( FILLER_631 VSSA ) ( FILLER_630 VSSA )
       ( FILLER_629 VSSA ) ( FILLER_628 VSSA )
       ( mprj_pads.area1_io_pad\[3\] VSSA ) ( FILLER_626 VSSA )
       ( FILLER_625 VSSA ) ( FILLER_624 VSSA ) ( FILLER_623 VSSA )
       ( FILLER_622 VSSA ) ( FILLER_621 VSSA ) ( FILLER_620 VSSA )
       ( FILLER_619 VSSA ) ( FILLER_618 VSSA )
       ( mprj_pads.area1_io_pad\[2\] VSSA ) ( FILLER_616 VSSA )
       ( FILLER_615 VSSA ) ( FILLER_614 VSSA ) ( FILLER_613 VSSA )
       ( FILLER_612 VSSA ) ( FILLER_611 VSSA ) ( FILLER_610 VSSA )
       ( FILLER_609 VSSA ) ( mprj_pads.area1_io_pad\[1\] VSSA )
       ( FILLER_607 VSSA ) ( FILLER_606 VSSA ) ( FILLER_605 VSSA )
       ( FILLER_604 VSSA ) ( FILLER_603 VSSA ) ( FILLER_602 VSSA )
       ( FILLER_601 VSSA ) ( FILLER_600 VSSA )
       ( mprj_pads.area1_io_pad\[0\] VSSA ) ( FILLER_599 VSSA )
       ( FILLER_597 VSSA ) ( FILLER_596 VSSA ) ( FILLER_595 VSSA )
       ( FILLER_594 VSSA ) ( FILLER_593 VSSA ) ( FILLER_592 VSSA )
       ( FILLER_591 VSSA ) ( FILLER_590 VSSA )
      + ROUTED met4 TAPERRULE met4_width_330  ( 3444570 2299150 ) ( * 2373850 ) ;
   - vddio ( FILLER_147 VSWITCH ) ( FILLER_146 VSWITCH )
       ( FILLER_145 VSWITCH ) ( FILLER_144 VSWITCH )
       ( FILLER_143 VSWITCH ) ( FILLER_142 VSWITCH )
       ( FILLER_141 VSWITCH ) ( FILLER_140 VSWITCH )
       ( FILLER_139 VSWITCH ) ( FILLER_138 VSWITCH )
       ( FILLER_137 VSWITCH ) ( FILLER_136 VSWITCH )
       ( FILLER_135 VSWITCH ) ( user1_analog_pad\[0\] VSWITCH )
       ( FILLER_133 VSWITCH ) ( FILLER_132 VSWITCH )
       ( FILLER_131 VSWITCH ) ( FILLER_130 VSWITCH )
       ( FILLER_129 VSWITCH ) ( FILLER_128 VSWITCH )
       ( FILLER_127 VSWITCH ) ( FILLER_126 VSWITCH )
       ( FILLER_125 VSWITCH ) ( FILLER_124 VSWITCH )
       ( FILLER_123 VSWITCH ) ( user1_vssa_hvclamp_pad\[0\] VSWITCH )
       ( FILLER_121 VSWITCH ) ( FILLER_120 VSWITCH )
       ( FILLER_119 VSWITCH ) ( FILLER_118 VSWITCH )
       ( FILLER_117 VSWITCH ) ( FILLER_116 VSWITCH )
       ( FILLER_115 VSWITCH ) ( FILLER_114 VSWITCH )
       ( FILLER_113 VSWITCH ) ( FILLER_112 VSWITCH )
       ( FILLER_111 VSWITCH ) ( FILLER_110 VSWITCH )
       ( user1_analog_pad\[1\] VSWITCH ) ( FILLER_108 VSWITCH )
       ( FILLER_107 VSWITCH ) ( FILLER_106 VSWITCH )
       ( FILLER_105 VSWITCH ) ( FILLER_104 VSWITCH )
       ( FILLER_103 VSWITCH ) ( FILLER_102 VSWITCH )
       ( FILLER_101 VSWITCH ) ( FILLER_100 VSWITCH )
       ( FILLER_99 VSWITCH ) ( FILLER_98 VSWITCH )
       ( user1_analog_pad\[2\] VSWITCH ) ( FILLER_96 VSWITCH )
       ( FILLER_95 VSWITCH ) ( FILLER_94 VSWITCH )
       ( FILLER_93 VSWITCH ) ( FILLER_92 VSWITCH )
       ( FILLER_91 VSWITCH ) ( FILLER_90 VSWITCH )
       ( FILLER_89 VSWITCH ) ( FILLER_88 VSWITCH )
       ( FILLER_87 VSWITCH ) ( FILLER_86 VSWITCH )
       ( FILLER_85 VSWITCH ) ( FILLER_84 VSWITCH )
       ( FILLER_83 VSWITCH ) ( FILLER_82 VSWITCH )
       ( FILLER_81 VSWITCH ) ( FILLER_80 VSWITCH )
       ( FILLER_79 VSWITCH )
       ( sky130_ef_io__com_bus_slice_10um_0 VSWITCH )
       ( FILLER_78 VSWITCH )
       ( sky130_ef_io__com_bus_slice_5um_1 VSWITCH )
       ( user1_analog_pad_with_clamp VSWITCH )
       ( sky130_ef_io__com_bus_slice_5um_0 VSWITCH )
       ( disconnect_vdda_0 VSWITCH ) ( FILLER_SB3 VSWITCH )
       ( FILLER_73 VSWITCH ) ( FILLER_72 VSWITCH )
       ( FILLER_71 VSWITCH ) ( FILLER_70 VSWITCH )
       ( FILLER_69 VSWITCH ) ( FILLER_68 VSWITCH )
       ( mgmt_vssio_hvclamp_pad\[1\] VSWITCH ) ( FILLER_66 VSWITCH )
       ( FILLER_65 VSWITCH ) ( FILLER_64 VSWITCH )
       ( FILLER_63 VSWITCH ) ( FILLER_62 VSWITCH )
       ( FILLER_61 VSWITCH ) ( FILLER_60 VSWITCH )
       ( sky130_ef_io__com_bus_slice_10um_1 VSWITCH )
       ( sky130_ef_io__com_bus_slice_5um_3 VSWITCH )
       ( user2_analog_pad_with_clamp\[0\] VSWITCH )
       ( sky130_ef_io__com_bus_slice_5um_2 VSWITCH )
       ( FILLER_57 VSWITCH ) ( FILLER_56 VSWITCH )
       ( FILLER_55 VSWITCH ) ( FILLER_54 VSWITCH )
       ( FILLER_53 VSWITCH ) ( FILLER_52 VSWITCH )
       ( FILLER_51 VSWITCH ) ( FILLER_50 VSWITCH )
       ( FILLER_49 VSWITCH )
       ( user2_analog_pad_with_clamp\[1\] VSWITCH )
       ( FILLER_47 VSWITCH ) ( FILLER_46 VSWITCH )
       ( FILLER_45 VSWITCH ) ( FILLER_44 VSWITCH )
       ( FILLER_43 VSWITCH ) ( FILLER_42 VSWITCH )
       ( user2_analog_pad\[0\] VSWITCH ) ( FILLER_41 VSWITCH )
       ( FILLER_39 VSWITCH ) ( FILLER_38 VSWITCH )
       ( FILLER_37 VSWITCH ) ( FILLER_36 VSWITCH )
       ( FILLER_35 VSWITCH ) ( FILLER_34 VSWITCH )
       ( FILLER_33 VSWITCH ) ( FILLER_32 VSWITCH )
       ( FILLER_31 VSWITCH ) ( FILLER_30 VSWITCH )
       ( FILLER_29 VSWITCH ) ( user2_analog_pad\[1\] VSWITCH )
       ( FILLER_27 VSWITCH ) ( FILLER_26 VSWITCH )
       ( FILLER_25 VSWITCH ) ( FILLER_24 VSWITCH )
       ( FILLER_23 VSWITCH ) ( FILLER_22 VSWITCH )
       ( FILLER_21 VSWITCH ) ( FILLER_20 VSWITCH )
       ( FILLER_19 VSWITCH ) ( FILLER_18 VSWITCH )
       ( FILLER_17 VSWITCH ) ( user2_analog_pad\[2\] VSWITCH )
       ( FILLER_15 VSWITCH ) ( FILLER_14 VSWITCH )
       ( FILLER_13 VSWITCH ) ( FILLER_12 VSWITCH )
       ( FILLER_11 VSWITCH ) ( FILLER_10 VSWITCH )
       ( FILLER_9 VSWITCH ) ( FILLER_8 VSWITCH ) ( FILLER_7 VSWITCH )
       ( FILLER_6 VSWITCH ) ( FILLER_147 VDDIO ) ( FILLER_5 VSWITCH )
       ( FILLER_146 VDDIO ) ( FILLER_145 VDDIO ) ( FILLER_144 VDDIO )
       ( FILLER_143 VDDIO ) ( FILLER_142 VDDIO ) ( FILLER_141 VDDIO )
       ( FILLER_140 VDDIO ) ( FILLER_139 VDDIO ) ( FILLER_138 VDDIO )
       ( FILLER_137 VDDIO ) ( FILLER_136 VDDIO ) ( FILLER_135 VDDIO )
       ( user1_analog_pad\[0\] VDDIO ) ( FILLER_133 VDDIO )
       ( FILLER_132 VDDIO ) ( FILLER_131 VDDIO ) ( FILLER_130 VDDIO )
       ( FILLER_129 VDDIO ) ( FILLER_128 VDDIO ) ( FILLER_127 VDDIO )
       ( FILLER_126 VDDIO ) ( FILLER_125 VDDIO ) ( FILLER_124 VDDIO )
       ( FILLER_123 VDDIO ) ( user1_vssa_hvclamp_pad\[0\] VDDIO )
       ( FILLER_121 VDDIO ) ( FILLER_120 VDDIO ) ( FILLER_119 VDDIO )
       ( FILLER_118 VDDIO ) ( FILLER_117 VDDIO ) ( FILLER_116 VDDIO )
       ( FILLER_115 VDDIO ) ( FILLER_114 VDDIO ) ( FILLER_113 VDDIO )
       ( FILLER_112 VDDIO ) ( FILLER_111 VDDIO ) ( FILLER_110 VDDIO )
       ( user1_analog_pad\[1\] VDDIO ) ( FILLER_108 VDDIO )
       ( FILLER_107 VDDIO ) ( FILLER_106 VDDIO ) ( FILLER_105 VDDIO )
       ( FILLER_104 VDDIO ) ( FILLER_103 VDDIO ) ( FILLER_102 VDDIO )
       ( FILLER_101 VDDIO ) ( FILLER_100 VDDIO ) ( FILLER_99 VDDIO )
       ( FILLER_98 VDDIO ) ( user1_analog_pad\[2\] VDDIO )
       ( FILLER_96 VDDIO ) ( FILLER_95 VDDIO ) ( FILLER_94 VDDIO )
       ( FILLER_93 VDDIO ) ( FILLER_92 VDDIO ) ( FILLER_91 VDDIO )
       ( FILLER_90 VDDIO ) ( FILLER_89 VDDIO ) ( FILLER_88 VDDIO )
       ( FILLER_87 VDDIO ) ( FILLER_86 VDDIO ) ( FILLER_85 VDDIO )
       ( FILLER_84 VDDIO ) ( FILLER_83 VDDIO ) ( FILLER_82 VDDIO )
       ( FILLER_81 VDDIO ) ( FILLER_80 VDDIO ) ( FILLER_79 VDDIO )
       ( sky130_ef_io__com_bus_slice_10um_0 VDDIO )
       ( FILLER_78 VDDIO ) ( sky130_ef_io__com_bus_slice_5um_1 VDDIO )
       ( user1_analog_pad_with_clamp VDDIO )
       ( sky130_ef_io__com_bus_slice_5um_0 VDDIO )
       ( disconnect_vdda_0 VDDIO ) ( FILLER_SB3 VDDIO )
       ( FILLER_73 VDDIO ) ( FILLER_72 VDDIO ) ( FILLER_71 VDDIO )
       ( FILLER_70 VDDIO ) ( FILLER_69 VDDIO ) ( FILLER_68 VDDIO )
       ( mgmt_vssio_hvclamp_pad\[1\] VDDIO ) ( FILLER_66 VDDIO )
       ( FILLER_65 VDDIO ) ( FILLER_64 VDDIO ) ( FILLER_63 VDDIO )
       ( FILLER_62 VDDIO ) ( FILLER_61 VDDIO ) ( FILLER_60 VDDIO )
       ( sky130_ef_io__com_bus_slice_10um_1 VDDIO )
       ( sky130_ef_io__com_bus_slice_5um_3 VDDIO )
       ( user2_analog_pad_with_clamp\[0\] VDDIO )
       ( sky130_ef_io__com_bus_slice_5um_2 VDDIO ) ( FILLER_57 VDDIO )
       ( FILLER_56 VDDIO ) ( FILLER_55 VDDIO ) ( FILLER_54 VDDIO )
       ( FILLER_53 VDDIO ) ( FILLER_52 VDDIO ) ( FILLER_51 VDDIO )
       ( FILLER_50 VDDIO ) ( FILLER_49 VDDIO )
       ( user2_analog_pad_with_clamp\[1\] VDDIO ) ( FILLER_47 VDDIO )
       ( FILLER_46 VDDIO ) ( FILLER_45 VDDIO ) ( FILLER_44 VDDIO )
       ( FILLER_43 VDDIO ) ( FILLER_42 VDDIO )
       ( user2_analog_pad\[0\] VDDIO ) ( FILLER_41 VDDIO )
       ( FILLER_39 VDDIO ) ( FILLER_38 VDDIO ) ( FILLER_37 VDDIO )
       ( FILLER_36 VDDIO ) ( FILLER_35 VDDIO ) ( FILLER_34 VDDIO )
       ( FILLER_33 VDDIO ) ( FILLER_32 VDDIO ) ( FILLER_31 VDDIO )
       ( FILLER_30 VDDIO ) ( FILLER_29 VDDIO )
       ( user2_analog_pad\[1\] VDDIO ) ( FILLER_27 VDDIO )
       ( FILLER_26 VDDIO ) ( FILLER_25 VDDIO ) ( FILLER_24 VDDIO )
       ( FILLER_23 VDDIO ) ( FILLER_22 VDDIO ) ( FILLER_21 VDDIO )
       ( FILLER_20 VDDIO ) ( FILLER_19 VDDIO ) ( FILLER_18 VDDIO )
       ( FILLER_17 VDDIO ) ( user2_analog_pad\[2\] VDDIO )
       ( FILLER_15 VDDIO ) ( FILLER_14 VDDIO ) ( FILLER_13 VDDIO )
       ( FILLER_12 VDDIO ) ( FILLER_11 VDDIO ) ( FILLER_10 VDDIO )
       ( FILLER_9 VDDIO ) ( FILLER_8 VDDIO ) ( FILLER_7 VDDIO )
       ( FILLER_6 VDDIO ) ( user2_corner VSWITCH ) ( FILLER_5 VDDIO )
       ( FILLER_579 VSWITCH ) ( FILLER_578 VSWITCH )
       ( user2_corner VDDIO ) ( FILLER_579 VDDIO )
       ( FILLER_578 VDDIO ) ( user1_corner VSWITCH )
       ( FILLER_786 VSWITCH ) ( user1_corner VDDIO )
       ( FILLER_786 VDDIO ) ( FILLER_577 VSWITCH )
       ( FILLER_577 VDDIO ) ( FILLER_576 VSWITCH )
       ( FILLER_576 VDDIO ) ( FILLER_785 VSWITCH )
       ( FILLER_785 VDDIO ) ( FILLER_575 VSWITCH )
       ( FILLER_575 VDDIO ) ( FILLER_784 VSWITCH )
       ( FILLER_784 VDDIO ) ( FILLER_574 VSWITCH )
       ( FILLER_574 VDDIO ) ( FILLER_783 VSWITCH )
       ( FILLER_783 VDDIO ) ( FILLER_573 VSWITCH )
       ( FILLER_573 VDDIO ) ( FILLER_782 VSWITCH )
       ( FILLER_782 VDDIO ) ( FILLER_572 VSWITCH )
       ( FILLER_572 VDDIO ) ( FILLER_781 VSWITCH )
       ( FILLER_781 VDDIO ) ( FILLER_571 VSWITCH )
       ( FILLER_571 VDDIO ) ( FILLER_780 VSWITCH )
       ( FILLER_780 VDDIO ) ( FILLER_779 VSWITCH )
       ( FILLER_570 VSWITCH ) ( FILLER_570 VDDIO )
       ( FILLER_779 VDDIO ) ( user2_analog_pad\[3\] VSWITCH )
       ( FILLER_776 VSWITCH ) ( FILLER_776 VDDIO )
       ( FILLER_568 VSWITCH ) ( user2_analog_pad\[3\] VDDIO )
       ( FILLER_568 VDDIO ) ( user1_analog_pad\[3\] VSWITCH )
       ( user1_analog_pad\[3\] VDDIO ) ( FILLER_567 VSWITCH )
       ( FILLER_567 VDDIO ) ( FILLER_777 VSWITCH )
       ( FILLER_777 VDDIO ) ( FILLER_775 VSWITCH )
       ( FILLER_775 VDDIO ) ( FILLER_566 VSWITCH )
       ( FILLER_566 VDDIO ) ( FILLER_774 VSWITCH )
       ( FILLER_774 VDDIO ) ( FILLER_565 VSWITCH )
       ( FILLER_565 VDDIO ) ( FILLER_773 VSWITCH )
       ( FILLER_773 VDDIO ) ( FILLER_564 VSWITCH )
       ( FILLER_564 VDDIO ) ( FILLER_772 VSWITCH )
       ( FILLER_772 VDDIO ) ( FILLER_563 VSWITCH )
       ( FILLER_563 VDDIO ) ( FILLER_771 VSWITCH )
       ( FILLER_771 VDDIO ) ( FILLER_562 VSWITCH )
       ( FILLER_562 VDDIO ) ( FILLER_561 VSWITCH )
       ( FILLER_561 VDDIO ) ( FILLER_770 VSWITCH )
       ( FILLER_770 VDDIO ) ( FILLER_769 VSWITCH )
       ( FILLER_769 VDDIO ) ( user2_vccd_lvclamp_pad VSWITCH )
       ( FILLER_559 VSWITCH ) ( user2_vccd_lvclamp_pad VDDIO )
       ( FILLER_559 VDDIO ) ( FILLER_558 VSWITCH )
       ( FILLER_558 VDDIO ) ( FILLER_557 VSWITCH )
       ( FILLER_557 VDDIO ) ( user1_vccd_lvclamp_pad VSWITCH )
       ( FILLER_767 VSWITCH ) ( user1_vccd_lvclamp_pad VDDIO )
       ( FILLER_767 VDDIO ) ( FILLER_766 VSWITCH )
       ( FILLER_766 VDDIO ) ( FILLER_556 VSWITCH )
       ( FILLER_556 VDDIO ) ( FILLER_765 VSWITCH )
       ( FILLER_765 VDDIO ) ( FILLER_555 VSWITCH )
       ( FILLER_555 VDDIO ) ( FILLER_764 VSWITCH )
       ( FILLER_764 VDDIO ) ( FILLER_554 VSWITCH )
       ( FILLER_554 VDDIO ) ( FILLER_763 VSWITCH )
       ( FILLER_763 VDDIO ) ( FILLER_553 VSWITCH )
       ( FILLER_553 VDDIO ) ( FILLER_762 VSWITCH )
       ( FILLER_762 VDDIO ) ( FILLER_552 VSWITCH )
       ( FILLER_552 VDDIO ) ( FILLER_761 VSWITCH )
       ( FILLER_761 VDDIO ) ( FILLER_551 VSWITCH )
       ( FILLER_551 VDDIO ) ( FILLER_760 VSWITCH )
       ( FILLER_760 VDDIO ) ( mgmt_vddio_hvclamp_pad\[1\] VSWITCH )
       ( FILLER_759 VSWITCH ) ( FILLER_759 VDDIO )
       ( FILLER_549 VSWITCH ) ( mgmt_vddio_hvclamp_pad\[1\] VDDIO )
       ( FILLER_549 VDDIO ) ( FILLER_548 VSWITCH )
       ( FILLER_548 VDDIO ) ( FILLER_547 VSWITCH )
       ( FILLER_547 VDDIO ) ( FILLER_546 VSWITCH )
       ( FILLER_546 VDDIO ) ( mprj_pads.area1_io_pad\[13\] VSWITCH )
       ( FILLER_757 VSWITCH ) ( mprj_pads.area1_io_pad\[13\] VDDIO )
       ( FILLER_757 VDDIO ) ( FILLER_545 VSWITCH )
       ( FILLER_545 VDDIO ) ( FILLER_756 VSWITCH )
       ( FILLER_756 VDDIO ) ( FILLER_544 VSWITCH )
       ( FILLER_544 VDDIO ) ( FILLER_755 VSWITCH )
       ( FILLER_755 VDDIO ) ( FILLER_543 VSWITCH )
       ( FILLER_543 VDDIO ) ( FILLER_754 VSWITCH )
       ( FILLER_754 VDDIO ) ( FILLER_542 VSWITCH )
       ( FILLER_542 VDDIO ) ( FILLER_753 VSWITCH )
       ( FILLER_753 VDDIO ) ( FILLER_541 VSWITCH )
       ( FILLER_541 VDDIO ) ( FILLER_752 VSWITCH )
       ( FILLER_752 VDDIO ) ( FILLER_751 VSWITCH )
       ( FILLER_751 VDDIO ) ( user2_vssa_hvclamp_pad VSWITCH )
       ( FILLER_750 VSWITCH ) ( FILLER_750 VDDIO )
       ( user2_vssa_hvclamp_pad VDDIO ) ( FILLER_539 VSWITCH )
       ( FILLER_538 VSWITCH ) ( FILLER_539 VDDIO )
       ( FILLER_538 VDDIO ) ( FILLER_537 VSWITCH )
       ( FILLER_537 VDDIO ) ( FILLER_536 VSWITCH )
       ( FILLER_536 VDDIO ) ( user1_vdda_hvclamp_pad\[0\] VSWITCH )
       ( FILLER_748 VSWITCH ) ( user1_vdda_hvclamp_pad\[0\] VDDIO )
       ( FILLER_748 VDDIO ) ( FILLER_747 VSWITCH )
       ( FILLER_747 VDDIO ) ( FILLER_535 VSWITCH )
       ( FILLER_535 VDDIO ) ( FILLER_746 VSWITCH )
       ( FILLER_746 VDDIO ) ( FILLER_534 VSWITCH )
       ( FILLER_534 VDDIO ) ( FILLER_745 VSWITCH )
       ( FILLER_745 VDDIO ) ( FILLER_533 VSWITCH )
       ( FILLER_533 VDDIO ) ( FILLER_744 VSWITCH )
       ( FILLER_744 VDDIO ) ( FILLER_532 VSWITCH )
       ( FILLER_532 VDDIO ) ( FILLER_743 VSWITCH )
       ( FILLER_743 VDDIO ) ( FILLER_531 VSWITCH )
       ( FILLER_531 VDDIO ) ( FILLER_742 VSWITCH )
       ( FILLER_742 VDDIO ) ( FILLER_741 VSWITCH )
       ( FILLER_741 VDDIO ) ( FILLER_740 VSWITCH )
       ( FILLER_740 VDDIO ) ( mprj_pads.area2_io_pad\[0\] VSWITCH )
       ( FILLER_529 VSWITCH ) ( mprj_pads.area2_io_pad\[0\] VDDIO )
       ( FILLER_529 VDDIO ) ( FILLER_528 VSWITCH )
       ( FILLER_528 VDDIO ) ( FILLER_527 VSWITCH )
       ( FILLER_527 VDDIO ) ( FILLER_526 VSWITCH )
       ( FILLER_526 VDDIO ) ( mprj_pads.area1_io_pad\[12\] VSWITCH )
       ( mprj_pads.area1_io_pad\[12\] VDDIO ) ( FILLER_525 VSWITCH )
       ( FILLER_525 VDDIO ) ( FILLER_738 VSWITCH )
       ( FILLER_738 VDDIO ) ( FILLER_524 VSWITCH )
       ( FILLER_524 VDDIO ) ( FILLER_737 VSWITCH )
       ( FILLER_737 VDDIO ) ( FILLER_523 VSWITCH )
       ( FILLER_523 VDDIO ) ( FILLER_736 VSWITCH )
       ( FILLER_736 VDDIO ) ( FILLER_522 VSWITCH )
       ( FILLER_522 VDDIO ) ( FILLER_735 VSWITCH )
       ( FILLER_735 VDDIO ) ( FILLER_734 VSWITCH )
       ( FILLER_734 VDDIO ) ( FILLER_521 VSWITCH )
       ( FILLER_521 VDDIO ) ( FILLER_733 VSWITCH )
       ( FILLER_733 VDDIO ) ( FILLER_732 VSWITCH )
       ( FILLER_732 VDDIO ) ( mprj_pads.area2_io_pad\[1\] VSWITCH )
       ( FILLER_731 VSWITCH ) ( FILLER_731 VDDIO )
       ( FILLER_519 VSWITCH ) ( mprj_pads.area2_io_pad\[1\] VDDIO )
       ( FILLER_519 VDDIO ) ( FILLER_518 VSWITCH )
       ( FILLER_518 VDDIO ) ( FILLER_517 VSWITCH )
       ( FILLER_517 VDDIO ) ( FILLER_516 VSWITCH )
       ( FILLER_516 VDDIO ) ( FILLER_515 VSWITCH )
       ( FILLER_515 VDDIO ) ( mprj_pads.area1_io_pad\[11\] VSWITCH )
       ( mprj_pads.area1_io_pad\[11\] VDDIO ) ( FILLER_729 VSWITCH )
       ( FILLER_729 VDDIO ) ( FILLER_514 VSWITCH )
       ( FILLER_514 VDDIO ) ( FILLER_728 VSWITCH )
       ( FILLER_728 VDDIO ) ( FILLER_513 VSWITCH )
       ( FILLER_513 VDDIO ) ( FILLER_727 VSWITCH )
       ( FILLER_727 VDDIO ) ( FILLER_512 VSWITCH )
       ( FILLER_512 VDDIO ) ( FILLER_726 VSWITCH )
       ( FILLER_726 VDDIO ) ( FILLER_511 VSWITCH )
       ( FILLER_511 VDDIO ) ( FILLER_725 VSWITCH )
       ( FILLER_725 VDDIO ) ( FILLER_724 VSWITCH )
       ( FILLER_724 VDDIO ) ( FILLER_723 VSWITCH )
       ( FILLER_723 VDDIO ) ( FILLER_722 VSWITCH )
       ( FILLER_722 VDDIO ) ( mprj_pads.area2_io_pad\[2\] VSWITCH )
       ( FILLER_509 VSWITCH ) ( mprj_pads.area2_io_pad\[2\] VDDIO )
       ( FILLER_509 VDDIO ) ( FILLER_508 VSWITCH )
       ( FILLER_508 VDDIO ) ( FILLER_507 VSWITCH )
       ( FILLER_507 VDDIO ) ( FILLER_506 VSWITCH )
       ( FILLER_506 VDDIO ) ( FILLER_505 VSWITCH )
       ( FILLER_505 VDDIO ) ( mprj_pads.area1_io_pad\[10\] VSWITCH )
       ( FILLER_720 VSWITCH ) ( FILLER_719 VSWITCH )
       ( mprj_pads.area1_io_pad\[10\] VDDIO ) ( FILLER_720 VDDIO )
       ( FILLER_719 VDDIO ) ( FILLER_504 VSWITCH )
       ( FILLER_504 VDDIO ) ( FILLER_718 VSWITCH )
       ( FILLER_718 VDDIO ) ( FILLER_503 VSWITCH )
       ( FILLER_503 VDDIO ) ( FILLER_717 VSWITCH )
       ( FILLER_717 VDDIO ) ( FILLER_502 VSWITCH )
       ( FILLER_502 VDDIO ) ( FILLER_501 VSWITCH )
       ( FILLER_501 VDDIO ) ( FILLER_716 VSWITCH )
       ( FILLER_716 VDDIO ) ( FILLER_715 VSWITCH )
       ( FILLER_715 VDDIO ) ( FILLER_714 VSWITCH )
       ( FILLER_714 VDDIO ) ( FILLER_713 VSWITCH )
       ( FILLER_713 VDDIO ) ( FILLER_712 VSWITCH )
       ( FILLER_712 VDDIO ) ( mprj_pads.area2_io_pad\[3\] VSWITCH )
       ( FILLER_499 VSWITCH ) ( mprj_pads.area2_io_pad\[3\] VDDIO )
       ( FILLER_499 VDDIO ) ( FILLER_498 VSWITCH )
       ( FILLER_498 VDDIO ) ( FILLER_497 VSWITCH )
       ( FILLER_497 VDDIO ) ( FILLER_496 VSWITCH )
       ( FILLER_496 VDDIO ) ( FILLER_495 VSWITCH )
       ( FILLER_495 VDDIO ) ( FILLER_494 VSWITCH )
       ( FILLER_494 VDDIO ) ( mprj_pads.area1_io_pad\[9\] VSWITCH )
       ( mprj_pads.area1_io_pad\[9\] VDDIO ) ( FILLER_710 VSWITCH )
       ( FILLER_710 VDDIO ) ( FILLER_493 VSWITCH )
       ( FILLER_493 VDDIO ) ( FILLER_709 VSWITCH )
       ( FILLER_709 VDDIO ) ( FILLER_492 VSWITCH )
       ( FILLER_492 VDDIO ) ( FILLER_708 VSWITCH )
       ( FILLER_708 VDDIO ) ( FILLER_491 VSWITCH )
       ( FILLER_491 VDDIO ) ( FILLER_707 VSWITCH )
       ( FILLER_707 VDDIO ) ( FILLER_706 VSWITCH )
       ( FILLER_706 VDDIO ) ( FILLER_705 VSWITCH )
       ( FILLER_705 VDDIO ) ( FILLER_704 VSWITCH )
       ( FILLER_704 VDDIO ) ( mprj_pads.area2_io_pad\[4\] VSWITCH )
       ( FILLER_489 VSWITCH ) ( mprj_pads.area2_io_pad\[4\] VDDIO )
       ( FILLER_489 VDDIO ) ( FILLER_488 VSWITCH )
       ( FILLER_488 VDDIO ) ( FILLER_703 VSWITCH )
       ( FILLER_703 VDDIO ) ( FILLER_487 VSWITCH )
       ( FILLER_487 VDDIO ) ( FILLER_486 VSWITCH )
       ( FILLER_486 VDDIO ) ( FILLER_485 VSWITCH )
       ( FILLER_485 VDDIO ) ( FILLER_484 VSWITCH )
       ( FILLER_484 VDDIO ) ( mprj_pads.area1_io_pad\[8\] VSWITCH )
       ( FILLER_701 VSWITCH ) ( mprj_pads.area1_io_pad\[8\] VDDIO )
       ( FILLER_701 VDDIO ) ( FILLER_483 VSWITCH )
       ( FILLER_483 VDDIO ) ( FILLER_700 VSWITCH )
       ( FILLER_700 VDDIO ) ( FILLER_482 VSWITCH )
       ( FILLER_482 VDDIO ) ( FILLER_699 VSWITCH )
       ( FILLER_699 VDDIO ) ( FILLER_481 VSWITCH )
       ( FILLER_481 VDDIO ) ( FILLER_698 VSWITCH )
       ( FILLER_698 VDDIO ) ( FILLER_697 VSWITCH )
       ( FILLER_697 VDDIO ) ( FILLER_696 VSWITCH )
       ( FILLER_696 VDDIO ) ( FILLER_695 VSWITCH )
       ( FILLER_695 VDDIO ) ( FILLER_694 VSWITCH )
       ( FILLER_694 VDDIO ) ( mprj_pads.area2_io_pad\[5\] VSWITCH )
       ( FILLER_479 VSWITCH ) ( FILLER_478 VSWITCH )
       ( mprj_pads.area2_io_pad\[5\] VDDIO ) ( FILLER_479 VDDIO )
       ( FILLER_478 VDDIO ) ( FILLER_477 VSWITCH )
       ( FILLER_477 VDDIO ) ( FILLER_693 VSWITCH )
       ( FILLER_693 VDDIO ) ( FILLER_476 VSWITCH )
       ( FILLER_476 VDDIO ) ( FILLER_475 VSWITCH )
       ( FILLER_475 VDDIO ) ( FILLER_474 VSWITCH )
       ( FILLER_474 VDDIO ) ( FILLER_473 VSWITCH )
       ( FILLER_473 VDDIO ) ( mprj_pads.area1_io_pad\[7\] VSWITCH )
       ( mprj_pads.area1_io_pad\[7\] VDDIO ) ( FILLER_691 VSWITCH )
       ( FILLER_691 VDDIO ) ( FILLER_472 VSWITCH )
       ( FILLER_472 VDDIO ) ( FILLER_690 VSWITCH )
       ( FILLER_690 VDDIO ) ( FILLER_471 VSWITCH )
       ( FILLER_471 VDDIO ) ( FILLER_689 VSWITCH )
       ( FILLER_689 VDDIO ) ( FILLER_688 VSWITCH )
       ( FILLER_688 VDDIO ) ( FILLER_687 VSWITCH )
       ( FILLER_687 VDDIO ) ( FILLER_686 VSWITCH )
       ( FILLER_686 VDDIO ) ( mprj_pads.area2_io_pad\[6\] VSWITCH )
       ( mprj_pads.area2_io_pad\[6\] VDDIO ) ( FILLER_469 VSWITCH )
       ( FILLER_468 VSWITCH ) ( FILLER_469 VDDIO )
       ( FILLER_468 VDDIO ) ( FILLER_685 VSWITCH )
       ( FILLER_685 VDDIO ) ( FILLER_467 VSWITCH )
       ( FILLER_467 VDDIO ) ( FILLER_684 VSWITCH )
       ( FILLER_684 VDDIO ) ( FILLER_466 VSWITCH )
       ( FILLER_466 VDDIO ) ( FILLER_465 VSWITCH )
       ( FILLER_465 VDDIO ) ( FILLER_464 VSWITCH )
       ( FILLER_464 VDDIO ) ( FILLER_463 VSWITCH )
       ( FILLER_463 VDDIO ) ( user1_vdda_hvclamp_pad\[1\] VSWITCH )
       ( FILLER_682 VSWITCH ) ( user1_vdda_hvclamp_pad\[1\] VDDIO )
       ( FILLER_682 VDDIO ) ( FILLER_462 VSWITCH )
       ( FILLER_462 VDDIO ) ( FILLER_681 VSWITCH )
       ( FILLER_681 VDDIO ) ( FILLER_461 VSWITCH )
       ( FILLER_461 VDDIO ) ( FILLER_680 VSWITCH )
       ( FILLER_680 VDDIO ) ( FILLER_679 VSWITCH )
       ( FILLER_679 VDDIO ) ( FILLER_678 VSWITCH )
       ( FILLER_678 VDDIO ) ( FILLER_677 VSWITCH )
       ( FILLER_677 VDDIO ) ( user2_vdda_hvclamp_pad VSWITCH )
       ( FILLER_459 VSWITCH ) ( FILLER_458 VSWITCH )
       ( user2_vdda_hvclamp_pad VDDIO ) ( FILLER_459 VDDIO )
       ( FILLER_458 VDDIO ) ( FILLER_457 VSWITCH )
       ( FILLER_457 VDDIO ) ( FILLER_676 VSWITCH )
       ( FILLER_676 VDDIO ) ( FILLER_675 VSWITCH )
       ( FILLER_675 VDDIO ) ( FILLER_456 VSWITCH )
       ( FILLER_456 VDDIO ) ( FILLER_455 VSWITCH )
       ( FILLER_455 VDDIO ) ( FILLER_454 VSWITCH )
       ( FILLER_454 VDDIO ) ( FILLER_453 VSWITCH )
       ( FILLER_453 VDDIO ) ( user1_vssd_lvclamp_pad VSWITCH )
       ( FILLER_673 VSWITCH ) ( user1_vssd_lvclamp_pad VDDIO )
       ( FILLER_673 VDDIO ) ( FILLER_452 VSWITCH )
       ( FILLER_452 VDDIO ) ( FILLER_672 VSWITCH )
       ( FILLER_672 VDDIO ) ( FILLER_671 VSWITCH )
       ( FILLER_451 VSWITCH ) ( gpio_pad VDDIO ) ( FILLER_451 VDDIO )
       ( FILLER_671 VDDIO ) ( FILLER_670 VSWITCH )
       ( FILLER_670 VDDIO ) ( FILLER_669 VSWITCH )
       ( FILLER_669 VDDIO ) ( FILLER_668 VSWITCH )
       ( FILLER_668 VDDIO ) ( user2_vssd_lvclamp_pad VSWITCH )
       ( FILLER_449 VSWITCH ) ( user2_vssd_lvclamp_pad VDDIO )
       ( FILLER_449 VDDIO ) ( FILLER_667 VSWITCH )
       ( FILLER_667 VDDIO ) ( FILLER_448 VSWITCH )
       ( FILLER_448 VDDIO ) ( FILLER_447 VSWITCH )
       ( FILLER_447 VDDIO ) ( FILLER_666 VSWITCH )
       ( FILLER_666 VDDIO ) ( FILLER_446 VSWITCH )
       ( FILLER_446 VDDIO ) ( FILLER_665 VSWITCH )
       ( FILLER_665 VDDIO ) ( FILLER_445 VSWITCH )
       ( FILLER_445 VDDIO ) ( FILLER_444 VSWITCH )
       ( FILLER_444 VDDIO ) ( FILLER_443 VSWITCH )
       ( FILLER_443 VDDIO ) ( FILLER_442 VSWITCH )
       ( FILLER_442 VDDIO ) ( user1_vssa_hvclamp_pad\[1\] VSWITCH )
       ( FILLER_663 VSWITCH ) ( user1_vssa_hvclamp_pad\[1\] VDDIO )
       ( FILLER_663 VDDIO ) ( FILLER_441 VSWITCH )
       ( FILLER_441 VDDIO ) ( FILLER_662 VSWITCH )
       ( FILLER_662 VDDIO ) ( FILLER_661 VSWITCH )
       ( FILLER_661 VDDIO ) ( FILLER_660 VSWITCH )
       ( FILLER_660 VDDIO ) ( FILLER_659 VSWITCH )
       ( FILLER_659 VDDIO ) ( mprj_pads.area2_io_pad\[7\] VSWITCH )
       ( FILLER_439 VSWITCH ) ( FILLER_438 VSWITCH )
       ( mprj_pads.area2_io_pad\[7\] VDDIO ) ( FILLER_439 VDDIO )
       ( FILLER_438 VDDIO ) ( FILLER_658 VSWITCH )
       ( FILLER_658 VDDIO ) ( FILLER_437 VSWITCH )
       ( FILLER_437 VDDIO ) ( FILLER_657 VSWITCH )
       ( FILLER_657 VDDIO ) ( FILLER_436 VSWITCH )
       ( FILLER_436 VDDIO ) ( FILLER_656 VSWITCH )
       ( FILLER_656 VDDIO ) ( FILLER_435 VSWITCH )
       ( FILLER_435 VDDIO ) ( FILLER_434 VSWITCH )
       ( FILLER_434 VDDIO ) ( FILLER_433 VSWITCH )
       ( FILLER_433 VDDIO ) ( FILLER_432 VSWITCH )
       ( FILLER_432 VDDIO ) ( mprj_pads.area1_io_pad\[6\] VSWITCH )
       ( FILLER_654 VSWITCH ) ( mprj_pads.area1_io_pad\[6\] VDDIO )
       ( FILLER_654 VDDIO ) ( FILLER_431 VSWITCH )
       ( FILLER_431 VDDIO ) ( FILLER_653 VSWITCH )
       ( FILLER_653 VDDIO ) ( FILLER_652 VSWITCH )
       ( FILLER_652 VDDIO ) ( FILLER_651 VSWITCH )
       ( FILLER_651 VDDIO ) ( FILLER_650 VSWITCH )
       ( FILLER_650 VDDIO ) ( mprj_pads.area2_io_pad\[8\] VSWITCH )
       ( mprj_pads.area2_io_pad\[8\] VDDIO ) ( FILLER_649 VSWITCH )
       ( FILLER_649 VDDIO ) ( FILLER_429 VSWITCH )
       ( FILLER_428 VSWITCH ) ( FILLER_429 VDDIO )
       ( FILLER_428 VDDIO ) ( FILLER_427 VSWITCH )
       ( FILLER_427 VDDIO ) ( FILLER_648 VSWITCH )
       ( FILLER_648 VDDIO ) ( FILLER_426 VSWITCH )
       ( FILLER_426 VDDIO ) ( FILLER_647 VSWITCH )
       ( FILLER_647 VDDIO ) ( FILLER_425 VSWITCH )
       ( FILLER_425 VDDIO ) ( FILLER_646 VSWITCH )
       ( FILLER_646 VDDIO ) ( FILLER_424 VSWITCH )
       ( FILLER_424 VDDIO ) ( FILLER_423 VSWITCH )
       ( FILLER_423 VDDIO ) ( FILLER_422 VSWITCH )
       ( FILLER_422 VDDIO ) ( FILLER_421 VSWITCH )
       ( FILLER_421 VDDIO ) ( mprj_pads.area1_io_pad\[5\] VSWITCH )
       ( mprj_pads.area1_io_pad\[5\] VDDIO ) ( FILLER_644 VSWITCH )
       ( FILLER_644 VDDIO ) ( FILLER_643 VSWITCH )
       ( FILLER_643 VDDIO ) ( FILLER_642 VSWITCH )
       ( FILLER_642 VDDIO ) ( FILLER_641 VSWITCH )
       ( FILLER_641 VDDIO ) ( mprj_pads.area2_io_pad\[9\] VSWITCH )
       ( FILLER_419 VSWITCH ) ( mprj_pads.area2_io_pad\[9\] VDDIO )
       ( FILLER_419 VDDIO ) ( FILLER_418 VSWITCH )
       ( FILLER_418 VDDIO ) ( FILLER_640 VSWITCH )
       ( FILLER_640 VDDIO ) ( FILLER_417 VSWITCH )
       ( FILLER_417 VDDIO ) ( FILLER_639 VSWITCH )
       ( FILLER_639 VDDIO ) ( FILLER_416 VSWITCH )
       ( FILLER_416 VDDIO ) ( FILLER_638 VSWITCH )
       ( FILLER_638 VDDIO ) ( FILLER_415 VSWITCH )
       ( FILLER_415 VDDIO ) ( FILLER_637 VSWITCH )
       ( FILLER_637 VDDIO ) ( FILLER_414 VSWITCH )
       ( FILLER_414 VDDIO ) ( FILLER_413 VSWITCH )
       ( FILLER_413 VDDIO ) ( FILLER_412 VSWITCH )
       ( FILLER_412 VDDIO ) ( FILLER_411 VSWITCH )
       ( FILLER_411 VDDIO ) ( mprj_pads.area1_io_pad\[4\] VSWITCH )
       ( mprj_pads.area1_io_pad\[4\] VDDIO ) ( FILLER_635 VSWITCH )
       ( FILLER_635 VDDIO ) ( FILLER_634 VSWITCH )
       ( FILLER_634 VDDIO ) ( FILLER_633 VSWITCH )
       ( FILLER_633 VDDIO ) ( mprj_pads.area2_io_pad\[10\] VSWITCH )
       ( FILLER_409 VSWITCH ) ( mprj_pads.area2_io_pad\[10\] VDDIO )
       ( FILLER_409 VDDIO ) ( FILLER_632 VSWITCH )
       ( FILLER_632 VDDIO ) ( FILLER_408 VSWITCH )
       ( FILLER_408 VDDIO ) ( FILLER_407 VSWITCH )
       ( FILLER_407 VDDIO ) ( FILLER_631 VSWITCH )
       ( FILLER_631 VDDIO ) ( FILLER_406 VSWITCH )
       ( FILLER_406 VDDIO ) ( FILLER_630 VSWITCH )
       ( FILLER_630 VDDIO ) ( FILLER_405 VSWITCH )
       ( FILLER_405 VDDIO ) ( FILLER_629 VSWITCH )
       ( FILLER_629 VDDIO ) ( FILLER_404 VSWITCH )
       ( FILLER_404 VDDIO ) ( FILLER_628 VSWITCH )
       ( FILLER_628 VDDIO ) ( FILLER_403 VSWITCH )
       ( FILLER_403 VDDIO ) ( FILLER_402 VSWITCH )
       ( FILLER_402 VDDIO ) ( FILLER_401 VSWITCH )
       ( FILLER_401 VDDIO ) ( mprj_pads.area1_io_pad\[3\] VSWITCH )
       ( mprj_pads.area1_io_pad\[3\] VDDIO ) ( FILLER_626 VSWITCH )
       ( FILLER_625 VSWITCH ) ( FILLER_626 VDDIO )
       ( FILLER_625 VDDIO ) ( FILLER_624 VSWITCH )
       ( FILLER_624 VDDIO ) ( FILLER_623 VSWITCH )
       ( FILLER_623 VDDIO ) ( mprj_pads.area2_io_pad\[11\] VSWITCH )
       ( FILLER_399 VSWITCH ) ( mprj_pads.area2_io_pad\[11\] VDDIO )
       ( FILLER_399 VDDIO ) ( FILLER_398 VSWITCH )
       ( FILLER_398 VDDIO ) ( FILLER_622 VSWITCH )
       ( FILLER_622 VDDIO ) ( FILLER_397 VSWITCH )
       ( FILLER_397 VDDIO ) ( FILLER_621 VSWITCH )
       ( FILLER_621 VDDIO ) ( FILLER_396 VSWITCH )
       ( FILLER_396 VDDIO ) ( FILLER_620 VSWITCH )
       ( FILLER_620 VDDIO ) ( FILLER_395 VSWITCH )
       ( FILLER_395 VDDIO ) ( FILLER_619 VSWITCH )
       ( FILLER_619 VDDIO ) ( FILLER_394 VSWITCH )
       ( FILLER_394 VDDIO ) ( FILLER_618 VSWITCH )
       ( FILLER_618 VDDIO ) ( FILLER_393 VSWITCH )
       ( FILLER_393 VDDIO ) ( FILLER_392 VSWITCH )
       ( FILLER_392 VDDIO ) ( FILLER_391 VSWITCH )
       ( FILLER_391 VDDIO ) ( mprj_pads.area1_io_pad\[2\] VSWITCH )
       ( FILLER_616 VSWITCH ) ( mprj_pads.area1_io_pad\[2\] VDDIO )
       ( FILLER_616 VDDIO ) ( FILLER_615 VSWITCH )
       ( FILLER_615 VDDIO ) ( FILLER_614 VSWITCH )
       ( FILLER_614 VDDIO ) ( mprj_pads.area2_io_pad\[12\] VSWITCH )
       ( FILLER_389 VSWITCH ) ( FILLER_388 VSWITCH )
       ( mprj_pads.area2_io_pad\[12\] VDDIO ) ( FILLER_389 VDDIO )
       ( FILLER_388 VDDIO ) ( FILLER_387 VSWITCH )
       ( FILLER_387 VDDIO ) ( FILLER_613 VSWITCH )
       ( FILLER_613 VDDIO ) ( FILLER_386 VSWITCH )
       ( FILLER_386 VDDIO ) ( FILLER_612 VSWITCH )
       ( FILLER_612 VDDIO ) ( FILLER_385 VSWITCH )
       ( FILLER_385 VDDIO ) ( FILLER_611 VSWITCH )
       ( FILLER_611 VDDIO ) ( FILLER_384 VSWITCH )
       ( FILLER_384 VDDIO ) ( FILLER_610 VSWITCH )
       ( FILLER_610 VDDIO ) ( FILLER_383 VSWITCH )
       ( FILLER_383 VDDIO ) ( FILLER_609 VSWITCH )
       ( FILLER_609 VDDIO ) ( FILLER_382 VSWITCH )
       ( FILLER_382 VDDIO ) ( FILLER_381 VSWITCH )
       ( FILLER_381 VDDIO ) ( FILLER_380 VSWITCH )
       ( FILLER_380 VDDIO ) ( FILLER_379 VSWITCH )
       ( FILLER_379 VDDIO ) ( mprj_pads.area1_io_pad\[1\] VSWITCH )
       ( FILLER_607 VSWITCH ) ( mprj_pads.area1_io_pad\[1\] VDDIO )
       ( FILLER_607 VDDIO ) ( FILLER_606 VSWITCH )
       ( FILLER_606 VDDIO ) ( FILLER_378 VSWITCH )
       ( FILLER_378 VDDIO ) ( FILLER_605 VSWITCH )
       ( FILLER_605 VDDIO ) ( FILLER_377 VSWITCH )
       ( FILLER_377 VDDIO ) ( FILLER_604 VSWITCH )
       ( FILLER_604 VDDIO ) ( FILLER_376 VSWITCH )
       ( FILLER_376 VDDIO ) ( FILLER_603 VSWITCH )
       ( FILLER_603 VDDIO ) ( FILLER_375 VSWITCH )
       ( FILLER_375 VDDIO ) ( FILLER_602 VSWITCH )
       ( FILLER_602 VDDIO ) ( FILLER_374 VSWITCH )
       ( FILLER_374 VDDIO ) ( FILLER_SB2 VSWITCH )
       ( disconnect_vdda_2 VSWITCH ) ( FILLER_SB2 VDDIO )
       ( disconnect_vdda_2 VDDIO ) ( FILLER_601 VSWITCH )
       ( FILLER_601 VDDIO ) ( FILLER_600 VSWITCH )
       ( FILLER_600 VDDIO ) ( mgmt_vddio_hvclamp_pad\[0\] VSWITCH )
       ( FILLER_599 VSWITCH ) ( FILLER_599 VDDIO )
       ( FILLER_370 VSWITCH ) ( mgmt_vddio_hvclamp_pad\[0\] VDDIO )
       ( FILLER_370 VDDIO ) ( FILLER_369 VSWITCH )
       ( FILLER_369 VDDIO ) ( FILLER_368 VSWITCH )
       ( FILLER_368 VDDIO ) ( FILLER_367 VSWITCH )
       ( FILLER_367 VDDIO ) ( mprj_pads.area1_io_pad\[0\] VSWITCH )
       ( mprj_pads.area1_io_pad\[0\] VDDIO ) ( FILLER_597 VSWITCH )
       ( FILLER_597 VDDIO ) ( FILLER_366 VSWITCH )
       ( FILLER_366 VDDIO ) ( FILLER_596 VSWITCH )
       ( FILLER_596 VDDIO ) ( FILLER_365 VSWITCH )
       ( FILLER_365 VDDIO ) ( FILLER_595 VSWITCH )
       ( FILLER_595 VDDIO ) ( FILLER_364 VSWITCH )
       ( FILLER_364 VDDIO ) ( FILLER_594 VSWITCH )
       ( FILLER_594 VDDIO ) ( FILLER_363 VSWITCH )
       ( FILLER_363 VDDIO ) ( FILLER_593 VSWITCH )
       ( FILLER_593 VDDIO ) ( FILLER_362 VSWITCH )
       ( FILLER_362 VDDIO ) ( FILLER_592 VSWITCH )
       ( FILLER_592 VDDIO ) ( FILLER_591 VSWITCH )
       ( FILLER_591 VDDIO ) ( FILLER_590 VSWITCH )
       ( FILLER_590 VDDIO ) ( disconnect_vdda_1 VSWITCH )
       ( FILLER_SB1 VSWITCH ) ( disconnect_vdda_1 VDDIO )
       ( FILLER_SB1 VDDIO ) ( FILLER_587 VSWITCH )
       ( FILLER_587 VDDIO ) ( mgmt_vccd_lvclamp_pad VSWITCH )
       ( FILLER_360 VSWITCH ) ( mgmt_vccd_lvclamp_pad VDDIO )
       ( FILLER_360 VDDIO ) ( FILLER_359 VSWITCH )
       ( FILLER_359 VDDIO ) ( FILLER_358 VSWITCH )
       ( FILLER_358 VDDIO ) ( FILLER_586 VSWITCH )
       ( FILLER_586 VDDIO ) ( FILLER_357 VSWITCH )
       ( FILLER_357 VDDIO ) ( FILLER_585 VSWITCH )
       ( FILLER_585 VDDIO ) ( FILLER_356 VSWITCH )
       ( FILLER_356 VDDIO ) ( FILLER_584 VSWITCH )
       ( FILLER_584 VDDIO ) ( FILLER_583 VSWITCH )
       ( FILLER_583 VDDIO ) ( FILLER_355 VSWITCH )
       ( FILLER_355 VDDIO ) ( FILLER_582 VSWITCH )
       ( FILLER_582 VDDIO ) ( FILLER_354 VSWITCH )
       ( FILLER_354 VDDIO ) ( FILLER_581 VSWITCH )
       ( FILLER_581 VDDIO ) ( FILLER_353 VSWITCH )
       ( FILLER_353 VDDIO ) ( mgmt_corner\[1\] VSWITCH )
       ( FILLER_352 VSWITCH ) ( FILLER_352 VDDIO )
       ( FILLER_580 VSWITCH ) ( FILLER_580 VDDIO )
       ( FILLER_351 VSWITCH ) ( FILLER_350 VSWITCH )
       ( FILLER_349 VSWITCH ) ( FILLER_348 VSWITCH )
       ( FILLER_347 VSWITCH ) ( FILLER_346 VSWITCH )
       ( bus_tie_72 VSWITCH ) ( bus_tie_71 VSWITCH )
       ( bus_tie_70 VSWITCH ) ( bus_tie_69 VSWITCH )
       ( bus_tie_68 VSWITCH ) ( bus_tie_67 VSWITCH )
       ( FILLER_339 VSWITCH ) ( FILLER_338 VSWITCH )
       ( FILLER_337 VSWITCH ) ( FILLER_336 VSWITCH )
       ( FILLER_335 VSWITCH ) ( mgmt_vdda_hvclamp_pad VSWITCH )
       ( FILLER_333 VSWITCH ) ( FILLER_332 VSWITCH )
       ( FILLER_331 VSWITCH ) ( FILLER_330 VSWITCH )
       ( bus_tie_66 VSWITCH ) ( FILLER_329 VSWITCH )
       ( bus_tie_65 VSWITCH ) ( bus_tie_64 VSWITCH )
       ( bus_tie_63 VSWITCH ) ( bus_tie_62 VSWITCH )
       ( bus_tie_61 VSWITCH ) ( FILLER_322 VSWITCH )
       ( FILLER_321 VSWITCH ) ( FILLER_320 VSWITCH )
       ( FILLER_319 VSWITCH ) ( FILLER_318 VSWITCH )
       ( mgmt_vssio_hvclamp_pad\[0\] VSWITCH ) ( FILLER_316 VSWITCH )
       ( FILLER_315 VSWITCH ) ( FILLER_314 VSWITCH )
       ( FILLER_313 VSWITCH ) ( bus_tie_60 VSWITCH )
       ( FILLER_312 VSWITCH ) ( bus_tie_59 VSWITCH )
       ( bus_tie_58 VSWITCH ) ( bus_tie_57 VSWITCH )
       ( bus_tie_56 VSWITCH ) ( bus_tie_55 VSWITCH )
       ( FILLER_305 VSWITCH ) ( FILLER_304 VSWITCH )
       ( FILLER_303 VSWITCH ) ( FILLER_302 VSWITCH )
       ( FILLER_301 VSWITCH ) ( gpio_pad VSWITCH )
       ( FILLER_299 VSWITCH ) ( FILLER_298 VSWITCH )
       ( FILLER_297 VSWITCH ) ( FILLER_296 VSWITCH )
       ( FILLER_295 VSWITCH ) ( bus_tie_54 VSWITCH )
       ( bus_tie_53 VSWITCH ) ( bus_tie_52 VSWITCH )
       ( bus_tie_51 VSWITCH ) ( bus_tie_50 VSWITCH )
       ( bus_tie_49 VSWITCH ) ( FILLER_288 VSWITCH )
       ( FILLER_287 VSWITCH ) ( FILLER_286 VSWITCH )
       ( FILLER_285 VSWITCH ) ( FILLER_284 VSWITCH )
       ( flash_io1_pad VSWITCH ) ( FILLER_282 VSWITCH )
       ( FILLER_281 VSWITCH ) ( FILLER_280 VSWITCH )
       ( FILLER_279 VSWITCH ) ( bus_tie_48 VSWITCH )
       ( FILLER_278 VSWITCH ) ( bus_tie_47 VSWITCH )
       ( bus_tie_46 VSWITCH ) ( bus_tie_45 VSWITCH )
       ( bus_tie_44 VSWITCH ) ( bus_tie_43 VSWITCH )
       ( FILLER_271 VSWITCH ) ( FILLER_270 VSWITCH )
       ( FILLER_269 VSWITCH ) ( FILLER_268 VSWITCH )
       ( FILLER_267 VSWITCH ) ( flash_io0_pad VSWITCH )
       ( FILLER_265 VSWITCH ) ( FILLER_264 VSWITCH )
       ( FILLER_263 VSWITCH ) ( FILLER_262 VSWITCH )
       ( FILLER_261 VSWITCH ) ( bus_tie_42 VSWITCH )
       ( bus_tie_41 VSWITCH ) ( bus_tie_40 VSWITCH )
       ( bus_tie_39 VSWITCH ) ( bus_tie_38 VSWITCH )
       ( bus_tie_37 VSWITCH ) ( FILLER_254 VSWITCH )
       ( FILLER_253 VSWITCH ) ( FILLER_252 VSWITCH )
       ( FILLER_251 VSWITCH ) ( FILLER_250 VSWITCH )
       ( flash_clk_pad VSWITCH ) ( FILLER_248 VSWITCH )
       ( FILLER_247 VSWITCH ) ( FILLER_246 VSWITCH )
       ( FILLER_245 VSWITCH ) ( bus_tie_36 VSWITCH )
       ( FILLER_244 VSWITCH ) ( bus_tie_35 VSWITCH )
       ( bus_tie_34 VSWITCH ) ( bus_tie_33 VSWITCH )
       ( bus_tie_32 VSWITCH ) ( bus_tie_31 VSWITCH )
       ( FILLER_237 VSWITCH ) ( FILLER_236 VSWITCH )
       ( FILLER_235 VSWITCH ) ( FILLER_234 VSWITCH )
       ( FILLER_233 VSWITCH ) ( flash_csb_pad VSWITCH )
       ( FILLER_231 VSWITCH ) ( FILLER_230 VSWITCH )
       ( FILLER_229 VSWITCH ) ( FILLER_228 VSWITCH )
       ( FILLER_227 VSWITCH ) ( bus_tie_30 VSWITCH )
       ( bus_tie_29 VSWITCH ) ( bus_tie_28 VSWITCH )
       ( bus_tie_27 VSWITCH ) ( bus_tie_26 VSWITCH )
       ( bus_tie_25 VSWITCH ) ( FILLER_220 VSWITCH )
       ( FILLER_219 VSWITCH ) ( FILLER_218 VSWITCH )
       ( FILLER_217 VSWITCH ) ( FILLER_216 VSWITCH )
       ( mgmt_vssd_lvclamp_pad VSWITCH ) ( FILLER_214 VSWITCH )
       ( FILLER_213 VSWITCH ) ( FILLER_212 VSWITCH )
       ( FILLER_211 VSWITCH ) ( bus_tie_24 VSWITCH )
       ( FILLER_210 VSWITCH ) ( bus_tie_23 VSWITCH )
       ( bus_tie_22 VSWITCH ) ( bus_tie_21 VSWITCH )
       ( bus_tie_20 VSWITCH ) ( bus_tie_19 VSWITCH )
       ( FILLER_203 VSWITCH ) ( FILLER_202 VSWITCH )
       ( FILLER_201 VSWITCH ) ( FILLER_200 VSWITCH )
       ( FILLER_199 VSWITCH ) ( clock_pad VSWITCH )
       ( FILLER_197 VSWITCH ) ( FILLER_196 VSWITCH )
       ( FILLER_195 VSWITCH ) ( FILLER_194 VSWITCH )
       ( bus_tie_18 VSWITCH ) ( FILLER_193 VSWITCH )
       ( bus_tie_17 VSWITCH ) ( bus_tie_16 VSWITCH )
       ( bus_tie_15 VSWITCH ) ( bus_tie_14 VSWITCH )
       ( bus_tie_13 VSWITCH ) ( FILLER_186 VSWITCH )
       ( FILLER_185 VSWITCH ) ( FILLER_184 VSWITCH )
       ( FILLER_183 VSWITCH ) ( FILLER_182 VSWITCH )
       ( resetb_pad VSWITCH ) ( FILLER_180 VSWITCH )
       ( FILLER_179 VSWITCH ) ( FILLER_178 VSWITCH )
       ( FILLER_177 VSWITCH ) ( FILLER_176 VSWITCH )
       ( bus_tie_12 VSWITCH ) ( bus_tie_11 VSWITCH )
       ( bus_tie_10 VSWITCH ) ( bus_tie_9 VSWITCH )
       ( bus_tie_8 VSWITCH ) ( bus_tie_7 VSWITCH )
       ( FILLER_169 VSWITCH ) ( FILLER_168 VSWITCH )
       ( FILLER_167 VSWITCH ) ( FILLER_166 VSWITCH )
       ( FILLER_165 VSWITCH ) ( mgmt_vssa_hvclamp_pad VSWITCH )
       ( FILLER_163 VSWITCH ) ( FILLER_162 VSWITCH )
       ( FILLER_161 VSWITCH ) ( FILLER_160 VSWITCH )
       ( bus_tie_6 VSWITCH ) ( FILLER_159 VSWITCH )
       ( bus_tie_5 VSWITCH ) ( bus_tie_4 VSWITCH )
       ( bus_tie_3 VSWITCH ) ( bus_tie_2 VSWITCH )
       ( bus_tie_1 VSWITCH ) ( FILLER_152 VSWITCH )
       ( FILLER_151 VSWITCH ) ( FILLER_150 VSWITCH )
       ( FILLER_149 VSWITCH ) ( mgmt_corner\[0\] VSWITCH )
       ( FILLER_148 VSWITCH ) ( mgmt_corner\[1\] VDDIO )
       ( FILLER_351 VDDIO ) ( FILLER_350 VDDIO ) ( FILLER_349 VDDIO )
       ( FILLER_348 VDDIO ) ( FILLER_347 VDDIO ) ( FILLER_346 VDDIO )
       ( bus_tie_72 VDDIO ) ( bus_tie_71 VDDIO ) ( bus_tie_70 VDDIO )
       ( bus_tie_69 VDDIO ) ( bus_tie_68 VDDIO ) ( bus_tie_67 VDDIO )
       ( FILLER_339 VDDIO ) ( FILLER_338 VDDIO ) ( FILLER_337 VDDIO )
       ( FILLER_336 VDDIO ) ( FILLER_335 VDDIO )
       ( mgmt_vdda_hvclamp_pad VDDIO ) ( FILLER_333 VDDIO )
       ( FILLER_332 VDDIO ) ( FILLER_331 VDDIO ) ( FILLER_330 VDDIO )
       ( bus_tie_66 VDDIO ) ( FILLER_329 VDDIO ) ( bus_tie_65 VDDIO )
       ( bus_tie_64 VDDIO ) ( bus_tie_63 VDDIO ) ( bus_tie_62 VDDIO )
       ( bus_tie_61 VDDIO ) ( FILLER_322 VDDIO ) ( FILLER_321 VDDIO )
       ( FILLER_320 VDDIO ) ( FILLER_319 VDDIO ) ( FILLER_318 VDDIO )
       ( mgmt_vssio_hvclamp_pad\[0\] VDDIO ) ( FILLER_316 VDDIO )
       ( FILLER_315 VDDIO ) ( FILLER_314 VDDIO ) ( FILLER_313 VDDIO )
       ( bus_tie_60 VDDIO ) ( FILLER_312 VDDIO ) ( bus_tie_59 VDDIO )
       ( bus_tie_58 VDDIO ) ( bus_tie_57 VDDIO ) ( bus_tie_56 VDDIO )
       ( bus_tie_55 VDDIO ) ( FILLER_305 VDDIO ) ( FILLER_304 VDDIO )
       ( FILLER_303 VDDIO ) ( FILLER_302 VDDIO ) ( FILLER_301 VDDIO )
       ( clock_pad VDDIO ) ( FILLER_299 VDDIO ) ( FILLER_298 VDDIO )
       ( FILLER_297 VDDIO ) ( FILLER_296 VDDIO ) ( FILLER_295 VDDIO )
       ( bus_tie_54 VDDIO ) ( bus_tie_53 VDDIO ) ( bus_tie_52 VDDIO )
       ( bus_tie_51 VDDIO ) ( bus_tie_50 VDDIO ) ( bus_tie_49 VDDIO )
       ( FILLER_288 VDDIO ) ( FILLER_287 VDDIO ) ( FILLER_286 VDDIO )
       ( FILLER_285 VDDIO ) ( FILLER_284 VDDIO )
       ( flash_io1_pad VDDIO ) ( FILLER_282 VDDIO )
       ( FILLER_281 VDDIO ) ( FILLER_280 VDDIO ) ( FILLER_279 VDDIO )
       ( bus_tie_48 VDDIO ) ( FILLER_278 VDDIO ) ( bus_tie_47 VDDIO )
       ( bus_tie_46 VDDIO ) ( bus_tie_45 VDDIO ) ( bus_tie_44 VDDIO )
       ( bus_tie_43 VDDIO ) ( FILLER_271 VDDIO ) ( FILLER_270 VDDIO )
       ( FILLER_269 VDDIO ) ( FILLER_268 VDDIO ) ( FILLER_267 VDDIO )
       ( flash_io0_pad VDDIO ) ( FILLER_265 VDDIO )
       ( FILLER_264 VDDIO ) ( FILLER_263 VDDIO ) ( FILLER_262 VDDIO )
       ( FILLER_261 VDDIO ) ( bus_tie_42 VDDIO ) ( bus_tie_41 VDDIO )
       ( bus_tie_40 VDDIO ) ( bus_tie_39 VDDIO ) ( bus_tie_38 VDDIO )
       ( bus_tie_37 VDDIO ) ( FILLER_254 VDDIO ) ( FILLER_253 VDDIO )
       ( FILLER_252 VDDIO ) ( FILLER_251 VDDIO ) ( FILLER_250 VDDIO )
       ( flash_clk_pad VDDIO ) ( FILLER_248 VDDIO )
       ( FILLER_247 VDDIO ) ( FILLER_246 VDDIO ) ( FILLER_245 VDDIO )
       ( bus_tie_36 VDDIO ) ( FILLER_244 VDDIO ) ( bus_tie_35 VDDIO )
       ( bus_tie_34 VDDIO ) ( bus_tie_33 VDDIO ) ( bus_tie_32 VDDIO )
       ( bus_tie_31 VDDIO ) ( FILLER_237 VDDIO ) ( FILLER_236 VDDIO )
       ( FILLER_235 VDDIO ) ( FILLER_234 VDDIO ) ( FILLER_233 VDDIO )
       ( flash_csb_pad VDDIO ) ( FILLER_231 VDDIO )
       ( FILLER_230 VDDIO ) ( FILLER_229 VDDIO ) ( FILLER_228 VDDIO )
       ( FILLER_227 VDDIO ) ( bus_tie_30 VDDIO ) ( bus_tie_29 VDDIO )
       ( bus_tie_28 VDDIO ) ( bus_tie_27 VDDIO ) ( bus_tie_26 VDDIO )
       ( bus_tie_25 VDDIO ) ( FILLER_220 VDDIO ) ( FILLER_219 VDDIO )
       ( FILLER_218 VDDIO ) ( FILLER_217 VDDIO ) ( FILLER_216 VDDIO )
       ( mgmt_vssd_lvclamp_pad VDDIO ) ( FILLER_214 VDDIO )
       ( FILLER_213 VDDIO ) ( FILLER_212 VDDIO ) ( FILLER_211 VDDIO )
       ( bus_tie_24 VDDIO ) ( FILLER_210 VDDIO ) ( bus_tie_23 VDDIO )
       ( bus_tie_22 VDDIO ) ( bus_tie_21 VDDIO ) ( bus_tie_20 VDDIO )
       ( bus_tie_19 VDDIO ) ( FILLER_203 VDDIO ) ( FILLER_202 VDDIO )
       ( FILLER_201 VDDIO ) ( FILLER_200 VDDIO ) ( FILLER_199 VDDIO )
       ( bus_tie_9 VDDIO ) ( FILLER_197 VDDIO ) ( FILLER_196 VDDIO )
       ( FILLER_195 VDDIO ) ( FILLER_194 VDDIO ) ( bus_tie_18 VDDIO )
       ( FILLER_193 VDDIO ) ( bus_tie_17 VDDIO ) ( bus_tie_16 VDDIO )
       ( bus_tie_15 VDDIO ) ( bus_tie_14 VDDIO ) ( bus_tie_13 VDDIO )
       ( FILLER_186 VDDIO ) ( FILLER_185 VDDIO ) ( FILLER_184 VDDIO )
       ( FILLER_183 VDDIO ) ( FILLER_182 VDDIO ) ( resetb_pad VDDIO )
       ( FILLER_180 VDDIO ) ( FILLER_179 VDDIO ) ( FILLER_178 VDDIO )
       ( FILLER_177 VDDIO ) ( FILLER_176 VDDIO ) ( bus_tie_12 VDDIO )
       ( bus_tie_11 VDDIO ) ( bus_tie_10 VDDIO ) ( bus_tie_8 VDDIO )
       ( bus_tie_7 VDDIO ) ( bus_tie_6 VDDIO ) ( FILLER_169 VDDIO )
       ( FILLER_168 VDDIO ) ( FILLER_167 VDDIO ) ( FILLER_166 VDDIO )
       ( FILLER_165 VDDIO ) ( mgmt_vssa_hvclamp_pad VDDIO )
       ( FILLER_163 VDDIO ) ( FILLER_162 VDDIO ) ( FILLER_161 VDDIO )
       ( FILLER_160 VDDIO ) ( bus_tie_5 VDDIO ) ( FILLER_159 VDDIO )
       ( bus_tie_4 VDDIO ) ( bus_tie_3 VDDIO ) ( bus_tie_2 VDDIO )
       ( bus_tie_1 VDDIO ) ( FILLER_152 VDDIO ) ( FILLER_151 VDDIO )
       ( FILLER_150 VDDIO ) ( FILLER_149 VDDIO ) ( FILLER_148 VDDIO )
       ( mgmt_corner\[0\] VDDIO )
      + ROUTED met4 TAPERRULE met4_width_1270  ( 164815 2278365 ) ( 167965 * ) ;
   - gpio_pad/VDDIO_Q ( gpio_pad VDDIO_Q ) ( FILLER_147 VDDIO_Q )
       ( FILLER_146 VDDIO_Q ) ( FILLER_145 VDDIO_Q )
       ( FILLER_144 VDDIO_Q ) ( FILLER_143 VDDIO_Q )
       ( FILLER_142 VDDIO_Q ) ( FILLER_141 VDDIO_Q )
       ( FILLER_140 VDDIO_Q ) ( FILLER_139 VDDIO_Q )
       ( FILLER_138 VDDIO_Q ) ( FILLER_137 VDDIO_Q )
       ( FILLER_136 VDDIO_Q ) ( FILLER_135 VDDIO_Q )
       ( user1_analog_pad\[0\] VDDIO_Q ) ( FILLER_133 VDDIO_Q )
       ( FILLER_132 VDDIO_Q ) ( FILLER_131 VDDIO_Q )
       ( FILLER_130 VDDIO_Q ) ( FILLER_129 VDDIO_Q )
       ( FILLER_128 VDDIO_Q ) ( FILLER_127 VDDIO_Q )
       ( FILLER_126 VDDIO_Q ) ( FILLER_125 VDDIO_Q )
       ( FILLER_124 VDDIO_Q ) ( FILLER_123 VDDIO_Q )
       ( user1_vssa_hvclamp_pad\[0\] VDDIO_Q ) ( FILLER_121 VDDIO_Q )
       ( FILLER_120 VDDIO_Q ) ( FILLER_119 VDDIO_Q )
       ( FILLER_118 VDDIO_Q ) ( FILLER_117 VDDIO_Q )
       ( FILLER_116 VDDIO_Q ) ( FILLER_115 VDDIO_Q )
       ( FILLER_114 VDDIO_Q ) ( FILLER_113 VDDIO_Q )
       ( FILLER_112 VDDIO_Q ) ( FILLER_111 VDDIO_Q )
       ( FILLER_110 VDDIO_Q ) ( user1_analog_pad\[1\] VDDIO_Q )
       ( FILLER_108 VDDIO_Q ) ( FILLER_107 VDDIO_Q )
       ( FILLER_106 VDDIO_Q ) ( FILLER_105 VDDIO_Q )
       ( FILLER_104 VDDIO_Q ) ( FILLER_103 VDDIO_Q )
       ( FILLER_102 VDDIO_Q ) ( FILLER_101 VDDIO_Q )
       ( FILLER_100 VDDIO_Q ) ( FILLER_99 VDDIO_Q )
       ( FILLER_98 VDDIO_Q ) ( user1_analog_pad\[2\] VDDIO_Q )
       ( FILLER_96 VDDIO_Q ) ( FILLER_95 VDDIO_Q )
       ( FILLER_94 VDDIO_Q ) ( FILLER_93 VDDIO_Q )
       ( FILLER_92 VDDIO_Q ) ( FILLER_91 VDDIO_Q )
       ( FILLER_90 VDDIO_Q ) ( FILLER_89 VDDIO_Q )
       ( FILLER_88 VDDIO_Q ) ( FILLER_87 VDDIO_Q )
       ( FILLER_86 VDDIO_Q ) ( FILLER_85 VDDIO_Q )
       ( FILLER_84 VDDIO_Q ) ( FILLER_83 VDDIO_Q )
       ( FILLER_82 VDDIO_Q ) ( FILLER_81 VDDIO_Q )
       ( FILLER_80 VDDIO_Q ) ( FILLER_79 VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_10um_0 VDDIO_Q )
       ( FILLER_78 VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_1 VDDIO_Q )
       ( user1_analog_pad_with_clamp VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_0 VDDIO_Q )
       ( disconnect_vdda_0 VDDIO_Q ) ( FILLER_SB3 VDDIO_Q )
       ( FILLER_73 VDDIO_Q ) ( FILLER_72 VDDIO_Q )
       ( FILLER_71 VDDIO_Q ) ( FILLER_70 VDDIO_Q )
       ( FILLER_69 VDDIO_Q ) ( FILLER_68 VDDIO_Q )
       ( mgmt_vssio_hvclamp_pad\[1\] VDDIO_Q ) ( FILLER_66 VDDIO_Q )
       ( FILLER_65 VDDIO_Q ) ( FILLER_64 VDDIO_Q )
       ( FILLER_63 VDDIO_Q ) ( FILLER_62 VDDIO_Q )
       ( FILLER_61 VDDIO_Q ) ( FILLER_60 VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_10um_1 VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_3 VDDIO_Q )
       ( user2_analog_pad_with_clamp\[0\] VDDIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_2 VDDIO_Q )
       ( FILLER_57 VDDIO_Q ) ( FILLER_56 VDDIO_Q )
       ( FILLER_55 VDDIO_Q ) ( FILLER_54 VDDIO_Q )
       ( FILLER_53 VDDIO_Q ) ( FILLER_52 VDDIO_Q )
       ( FILLER_51 VDDIO_Q ) ( FILLER_50 VDDIO_Q )
       ( FILLER_49 VDDIO_Q )
       ( user2_analog_pad_with_clamp\[1\] VDDIO_Q )
       ( FILLER_47 VDDIO_Q ) ( FILLER_46 VDDIO_Q )
       ( FILLER_45 VDDIO_Q ) ( FILLER_44 VDDIO_Q )
       ( FILLER_43 VDDIO_Q ) ( FILLER_42 VDDIO_Q )
       ( user2_analog_pad\[0\] VDDIO_Q ) ( FILLER_41 VDDIO_Q )
       ( FILLER_39 VDDIO_Q ) ( FILLER_38 VDDIO_Q )
       ( FILLER_37 VDDIO_Q ) ( FILLER_36 VDDIO_Q )
       ( FILLER_35 VDDIO_Q ) ( FILLER_34 VDDIO_Q )
       ( FILLER_33 VDDIO_Q ) ( FILLER_32 VDDIO_Q )
       ( FILLER_31 VDDIO_Q ) ( FILLER_30 VDDIO_Q )
       ( FILLER_29 VDDIO_Q ) ( user2_analog_pad\[1\] VDDIO_Q )
       ( FILLER_27 VDDIO_Q ) ( FILLER_26 VDDIO_Q )
       ( FILLER_25 VDDIO_Q ) ( FILLER_24 VDDIO_Q )
       ( FILLER_23 VDDIO_Q ) ( FILLER_22 VDDIO_Q )
       ( FILLER_21 VDDIO_Q ) ( FILLER_20 VDDIO_Q )
       ( FILLER_19 VDDIO_Q ) ( FILLER_18 VDDIO_Q )
       ( FILLER_17 VDDIO_Q ) ( user2_analog_pad\[2\] VDDIO_Q )
       ( FILLER_15 VDDIO_Q ) ( FILLER_14 VDDIO_Q )
       ( FILLER_13 VDDIO_Q ) ( FILLER_12 VDDIO_Q )
       ( FILLER_11 VDDIO_Q ) ( FILLER_10 VDDIO_Q )
       ( FILLER_9 VDDIO_Q ) ( FILLER_8 VDDIO_Q ) ( FILLER_7 VDDIO_Q )
       ( FILLER_6 VDDIO_Q ) ( user2_corner VDDIO_Q )
       ( FILLER_5 VDDIO_Q ) ( FILLER_579 VDDIO_Q )
       ( FILLER_578 VDDIO_Q ) ( user1_corner VDDIO_Q )
       ( FILLER_786 VDDIO_Q ) ( FILLER_577 VDDIO_Q )
       ( FILLER_576 VDDIO_Q ) ( FILLER_785 VDDIO_Q )
       ( FILLER_575 VDDIO_Q ) ( FILLER_784 VDDIO_Q )
       ( FILLER_574 VDDIO_Q ) ( FILLER_783 VDDIO_Q )
       ( FILLER_573 VDDIO_Q ) ( FILLER_782 VDDIO_Q )
       ( FILLER_572 VDDIO_Q ) ( FILLER_781 VDDIO_Q )
       ( FILLER_571 VDDIO_Q ) ( FILLER_780 VDDIO_Q )
       ( FILLER_779 VDDIO_Q ) ( FILLER_570 VDDIO_Q )
       ( user2_analog_pad\[3\] VDDIO_Q ) ( FILLER_776 VDDIO_Q )
       ( FILLER_568 VDDIO_Q ) ( user1_analog_pad\[3\] VDDIO_Q )
       ( FILLER_567 VDDIO_Q ) ( FILLER_777 VDDIO_Q )
       ( FILLER_775 VDDIO_Q ) ( FILLER_566 VDDIO_Q )
       ( FILLER_774 VDDIO_Q ) ( FILLER_565 VDDIO_Q )
       ( FILLER_773 VDDIO_Q ) ( FILLER_564 VDDIO_Q )
       ( FILLER_772 VDDIO_Q ) ( FILLER_563 VDDIO_Q )
       ( FILLER_771 VDDIO_Q ) ( FILLER_562 VDDIO_Q )
       ( FILLER_561 VDDIO_Q ) ( FILLER_770 VDDIO_Q )
       ( FILLER_769 VDDIO_Q ) ( user2_vccd_lvclamp_pad VDDIO_Q )
       ( FILLER_559 VDDIO_Q ) ( FILLER_558 VDDIO_Q )
       ( FILLER_557 VDDIO_Q ) ( user1_vccd_lvclamp_pad VDDIO_Q )
       ( FILLER_767 VDDIO_Q ) ( FILLER_766 VDDIO_Q )
       ( FILLER_556 VDDIO_Q ) ( FILLER_765 VDDIO_Q )
       ( FILLER_555 VDDIO_Q ) ( FILLER_764 VDDIO_Q )
       ( FILLER_554 VDDIO_Q ) ( FILLER_763 VDDIO_Q )
       ( FILLER_553 VDDIO_Q ) ( FILLER_762 VDDIO_Q )
       ( FILLER_552 VDDIO_Q ) ( FILLER_761 VDDIO_Q )
       ( FILLER_551 VDDIO_Q ) ( FILLER_760 VDDIO_Q )
       ( mgmt_vddio_hvclamp_pad\[1\] VDDIO_Q ) ( FILLER_759 VDDIO_Q )
       ( FILLER_549 VDDIO_Q ) ( FILLER_548 VDDIO_Q )
       ( FILLER_547 VDDIO_Q ) ( FILLER_546 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[13\] VDDIO_Q ) ( FILLER_757 VDDIO_Q )
       ( FILLER_545 VDDIO_Q ) ( FILLER_756 VDDIO_Q )
       ( FILLER_544 VDDIO_Q ) ( FILLER_755 VDDIO_Q )
       ( FILLER_543 VDDIO_Q ) ( FILLER_754 VDDIO_Q )
       ( FILLER_542 VDDIO_Q ) ( FILLER_753 VDDIO_Q )
       ( FILLER_541 VDDIO_Q ) ( FILLER_752 VDDIO_Q )
       ( FILLER_751 VDDIO_Q ) ( user2_vssa_hvclamp_pad VDDIO_Q )
       ( FILLER_750 VDDIO_Q ) ( FILLER_539 VDDIO_Q )
       ( FILLER_538 VDDIO_Q ) ( FILLER_537 VDDIO_Q )
       ( FILLER_536 VDDIO_Q ) ( user1_vdda_hvclamp_pad\[0\] VDDIO_Q )
       ( FILLER_748 VDDIO_Q ) ( FILLER_747 VDDIO_Q )
       ( FILLER_535 VDDIO_Q ) ( FILLER_746 VDDIO_Q )
       ( FILLER_534 VDDIO_Q ) ( FILLER_745 VDDIO_Q )
       ( FILLER_533 VDDIO_Q ) ( FILLER_744 VDDIO_Q )
       ( FILLER_532 VDDIO_Q ) ( FILLER_743 VDDIO_Q )
       ( FILLER_531 VDDIO_Q ) ( FILLER_742 VDDIO_Q )
       ( FILLER_741 VDDIO_Q ) ( FILLER_740 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[0\] VDDIO_Q ) ( FILLER_529 VDDIO_Q )
       ( FILLER_528 VDDIO_Q ) ( FILLER_527 VDDIO_Q )
       ( FILLER_526 VDDIO_Q ) ( mprj_pads.area1_io_pad\[12\] VDDIO_Q )
       ( FILLER_525 VDDIO_Q ) ( FILLER_738 VDDIO_Q )
       ( FILLER_524 VDDIO_Q ) ( FILLER_737 VDDIO_Q )
       ( FILLER_523 VDDIO_Q ) ( FILLER_736 VDDIO_Q )
       ( FILLER_522 VDDIO_Q ) ( FILLER_735 VDDIO_Q )
       ( FILLER_734 VDDIO_Q ) ( FILLER_521 VDDIO_Q )
       ( FILLER_733 VDDIO_Q ) ( FILLER_732 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[1\] VDDIO_Q ) ( FILLER_731 VDDIO_Q )
       ( FILLER_519 VDDIO_Q ) ( FILLER_518 VDDIO_Q )
       ( FILLER_517 VDDIO_Q ) ( FILLER_516 VDDIO_Q )
       ( FILLER_515 VDDIO_Q ) ( mprj_pads.area1_io_pad\[11\] VDDIO_Q )
       ( FILLER_729 VDDIO_Q ) ( FILLER_514 VDDIO_Q )
       ( FILLER_728 VDDIO_Q ) ( FILLER_513 VDDIO_Q )
       ( FILLER_727 VDDIO_Q ) ( FILLER_512 VDDIO_Q )
       ( FILLER_726 VDDIO_Q ) ( FILLER_511 VDDIO_Q )
       ( FILLER_725 VDDIO_Q ) ( FILLER_724 VDDIO_Q )
       ( FILLER_723 VDDIO_Q ) ( FILLER_722 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[2\] VDDIO_Q ) ( FILLER_509 VDDIO_Q )
       ( FILLER_508 VDDIO_Q ) ( FILLER_507 VDDIO_Q )
       ( FILLER_506 VDDIO_Q ) ( FILLER_505 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[10\] VDDIO_Q ) ( FILLER_720 VDDIO_Q )
       ( FILLER_719 VDDIO_Q ) ( FILLER_504 VDDIO_Q )
       ( FILLER_718 VDDIO_Q ) ( FILLER_503 VDDIO_Q )
       ( FILLER_717 VDDIO_Q ) ( FILLER_502 VDDIO_Q )
       ( FILLER_501 VDDIO_Q ) ( FILLER_716 VDDIO_Q )
       ( FILLER_715 VDDIO_Q ) ( FILLER_714 VDDIO_Q )
       ( FILLER_713 VDDIO_Q ) ( FILLER_712 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[3\] VDDIO_Q ) ( FILLER_499 VDDIO_Q )
       ( FILLER_498 VDDIO_Q ) ( FILLER_497 VDDIO_Q )
       ( FILLER_496 VDDIO_Q ) ( FILLER_495 VDDIO_Q )
       ( FILLER_494 VDDIO_Q ) ( mprj_pads.area1_io_pad\[9\] VDDIO_Q )
       ( FILLER_710 VDDIO_Q ) ( FILLER_493 VDDIO_Q )
       ( FILLER_709 VDDIO_Q ) ( FILLER_492 VDDIO_Q )
       ( FILLER_708 VDDIO_Q ) ( FILLER_491 VDDIO_Q )
       ( FILLER_707 VDDIO_Q ) ( FILLER_706 VDDIO_Q )
       ( FILLER_705 VDDIO_Q ) ( FILLER_704 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[4\] VDDIO_Q ) ( FILLER_489 VDDIO_Q )
       ( FILLER_488 VDDIO_Q ) ( FILLER_703 VDDIO_Q )
       ( FILLER_487 VDDIO_Q ) ( FILLER_486 VDDIO_Q )
       ( FILLER_485 VDDIO_Q ) ( FILLER_484 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[8\] VDDIO_Q ) ( FILLER_701 VDDIO_Q )
       ( FILLER_483 VDDIO_Q ) ( FILLER_700 VDDIO_Q )
       ( FILLER_482 VDDIO_Q ) ( FILLER_699 VDDIO_Q )
       ( FILLER_481 VDDIO_Q ) ( FILLER_698 VDDIO_Q )
       ( FILLER_697 VDDIO_Q ) ( FILLER_696 VDDIO_Q )
       ( FILLER_695 VDDIO_Q ) ( FILLER_694 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[5\] VDDIO_Q ) ( FILLER_479 VDDIO_Q )
       ( FILLER_478 VDDIO_Q ) ( FILLER_477 VDDIO_Q )
       ( FILLER_693 VDDIO_Q ) ( FILLER_476 VDDIO_Q )
       ( FILLER_475 VDDIO_Q ) ( FILLER_474 VDDIO_Q )
       ( FILLER_473 VDDIO_Q ) ( mprj_pads.area1_io_pad\[7\] VDDIO_Q )
       ( FILLER_691 VDDIO_Q ) ( FILLER_472 VDDIO_Q )
       ( FILLER_690 VDDIO_Q ) ( FILLER_471 VDDIO_Q )
       ( FILLER_689 VDDIO_Q ) ( FILLER_688 VDDIO_Q )
       ( FILLER_687 VDDIO_Q ) ( FILLER_686 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[6\] VDDIO_Q ) ( FILLER_469 VDDIO_Q )
       ( FILLER_468 VDDIO_Q ) ( FILLER_685 VDDIO_Q )
       ( FILLER_467 VDDIO_Q ) ( FILLER_684 VDDIO_Q )
       ( FILLER_466 VDDIO_Q ) ( FILLER_465 VDDIO_Q )
       ( FILLER_464 VDDIO_Q ) ( FILLER_463 VDDIO_Q )
       ( user1_vdda_hvclamp_pad\[1\] VDDIO_Q ) ( FILLER_682 VDDIO_Q )
       ( FILLER_462 VDDIO_Q ) ( FILLER_681 VDDIO_Q )
       ( FILLER_461 VDDIO_Q ) ( FILLER_680 VDDIO_Q )
       ( FILLER_679 VDDIO_Q ) ( FILLER_678 VDDIO_Q )
       ( FILLER_677 VDDIO_Q ) ( user2_vdda_hvclamp_pad VDDIO_Q )
       ( FILLER_459 VDDIO_Q ) ( FILLER_458 VDDIO_Q )
       ( FILLER_457 VDDIO_Q ) ( FILLER_676 VDDIO_Q )
       ( FILLER_675 VDDIO_Q ) ( FILLER_456 VDDIO_Q )
       ( FILLER_455 VDDIO_Q ) ( FILLER_454 VDDIO_Q )
       ( FILLER_453 VDDIO_Q ) ( user1_vssd_lvclamp_pad VDDIO_Q )
       ( FILLER_673 VDDIO_Q ) ( FILLER_452 VDDIO_Q )
       ( FILLER_672 VDDIO_Q ) ( FILLER_671 VDDIO_Q )
       ( FILLER_451 VDDIO_Q ) ( FILLER_670 VDDIO_Q )
       ( FILLER_669 VDDIO_Q ) ( FILLER_668 VDDIO_Q )
       ( user2_vssd_lvclamp_pad VDDIO_Q ) ( FILLER_449 VDDIO_Q )
       ( FILLER_667 VDDIO_Q ) ( FILLER_448 VDDIO_Q )
       ( FILLER_447 VDDIO_Q ) ( FILLER_666 VDDIO_Q )
       ( FILLER_446 VDDIO_Q ) ( FILLER_665 VDDIO_Q )
       ( FILLER_445 VDDIO_Q ) ( FILLER_444 VDDIO_Q )
       ( FILLER_443 VDDIO_Q ) ( FILLER_442 VDDIO_Q )
       ( user1_vssa_hvclamp_pad\[1\] VDDIO_Q ) ( FILLER_663 VDDIO_Q )
       ( FILLER_441 VDDIO_Q ) ( FILLER_662 VDDIO_Q )
       ( FILLER_661 VDDIO_Q ) ( FILLER_660 VDDIO_Q )
       ( FILLER_659 VDDIO_Q ) ( mprj_pads.area2_io_pad\[7\] VDDIO_Q )
       ( FILLER_439 VDDIO_Q ) ( FILLER_438 VDDIO_Q )
       ( FILLER_658 VDDIO_Q ) ( FILLER_437 VDDIO_Q )
       ( FILLER_657 VDDIO_Q ) ( FILLER_436 VDDIO_Q )
       ( FILLER_656 VDDIO_Q ) ( FILLER_435 VDDIO_Q )
       ( FILLER_434 VDDIO_Q ) ( FILLER_433 VDDIO_Q )
       ( FILLER_432 VDDIO_Q ) ( mprj_pads.area1_io_pad\[6\] VDDIO_Q )
       ( FILLER_654 VDDIO_Q ) ( FILLER_431 VDDIO_Q )
       ( FILLER_653 VDDIO_Q ) ( FILLER_652 VDDIO_Q )
       ( FILLER_651 VDDIO_Q ) ( FILLER_650 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[8\] VDDIO_Q ) ( FILLER_649 VDDIO_Q )
       ( FILLER_429 VDDIO_Q ) ( FILLER_428 VDDIO_Q )
       ( FILLER_427 VDDIO_Q ) ( FILLER_648 VDDIO_Q )
       ( FILLER_426 VDDIO_Q ) ( FILLER_647 VDDIO_Q )
       ( FILLER_425 VDDIO_Q ) ( FILLER_646 VDDIO_Q )
       ( FILLER_424 VDDIO_Q ) ( FILLER_423 VDDIO_Q )
       ( FILLER_422 VDDIO_Q ) ( FILLER_421 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[5\] VDDIO_Q ) ( FILLER_644 VDDIO_Q )
       ( FILLER_643 VDDIO_Q ) ( FILLER_642 VDDIO_Q )
       ( FILLER_641 VDDIO_Q ) ( mprj_pads.area2_io_pad\[9\] VDDIO_Q )
       ( FILLER_419 VDDIO_Q ) ( FILLER_418 VDDIO_Q )
       ( FILLER_640 VDDIO_Q ) ( FILLER_417 VDDIO_Q )
       ( FILLER_639 VDDIO_Q ) ( FILLER_416 VDDIO_Q )
       ( FILLER_638 VDDIO_Q ) ( FILLER_415 VDDIO_Q )
       ( FILLER_637 VDDIO_Q ) ( FILLER_414 VDDIO_Q )
       ( FILLER_413 VDDIO_Q ) ( FILLER_412 VDDIO_Q )
       ( FILLER_411 VDDIO_Q ) ( mprj_pads.area1_io_pad\[4\] VDDIO_Q )
       ( FILLER_635 VDDIO_Q ) ( FILLER_634 VDDIO_Q )
       ( FILLER_633 VDDIO_Q ) ( mprj_pads.area2_io_pad\[10\] VDDIO_Q )
       ( FILLER_409 VDDIO_Q ) ( FILLER_632 VDDIO_Q )
       ( FILLER_408 VDDIO_Q ) ( FILLER_407 VDDIO_Q )
       ( FILLER_631 VDDIO_Q ) ( FILLER_406 VDDIO_Q )
       ( FILLER_630 VDDIO_Q ) ( FILLER_405 VDDIO_Q )
       ( FILLER_629 VDDIO_Q ) ( FILLER_404 VDDIO_Q )
       ( FILLER_628 VDDIO_Q ) ( FILLER_403 VDDIO_Q )
       ( FILLER_402 VDDIO_Q ) ( FILLER_401 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[3\] VDDIO_Q ) ( FILLER_626 VDDIO_Q )
       ( FILLER_625 VDDIO_Q ) ( FILLER_624 VDDIO_Q )
       ( FILLER_623 VDDIO_Q ) ( mprj_pads.area2_io_pad\[11\] VDDIO_Q )
       ( FILLER_399 VDDIO_Q ) ( FILLER_398 VDDIO_Q )
       ( FILLER_622 VDDIO_Q ) ( FILLER_397 VDDIO_Q )
       ( FILLER_621 VDDIO_Q ) ( FILLER_396 VDDIO_Q )
       ( FILLER_620 VDDIO_Q ) ( FILLER_395 VDDIO_Q )
       ( FILLER_619 VDDIO_Q ) ( FILLER_394 VDDIO_Q )
       ( FILLER_618 VDDIO_Q ) ( FILLER_393 VDDIO_Q )
       ( FILLER_392 VDDIO_Q ) ( FILLER_391 VDDIO_Q )
       ( mprj_pads.area1_io_pad\[2\] VDDIO_Q ) ( FILLER_616 VDDIO_Q )
       ( FILLER_615 VDDIO_Q ) ( FILLER_614 VDDIO_Q )
       ( mprj_pads.area2_io_pad\[12\] VDDIO_Q ) ( FILLER_389 VDDIO_Q )
       ( FILLER_388 VDDIO_Q ) ( FILLER_387 VDDIO_Q )
       ( FILLER_613 VDDIO_Q ) ( FILLER_386 VDDIO_Q )
       ( FILLER_612 VDDIO_Q ) ( FILLER_385 VDDIO_Q )
       ( FILLER_611 VDDIO_Q ) ( FILLER_384 VDDIO_Q )
       ( FILLER_610 VDDIO_Q ) ( FILLER_383 VDDIO_Q )
       ( FILLER_609 VDDIO_Q ) ( FILLER_382 VDDIO_Q )
       ( FILLER_381 VDDIO_Q ) ( FILLER_380 VDDIO_Q )
       ( FILLER_379 VDDIO_Q ) ( mprj_pads.area1_io_pad\[1\] VDDIO_Q )
       ( FILLER_607 VDDIO_Q ) ( FILLER_606 VDDIO_Q )
       ( FILLER_378 VDDIO_Q ) ( FILLER_605 VDDIO_Q )
       ( FILLER_377 VDDIO_Q ) ( FILLER_604 VDDIO_Q )
       ( FILLER_376 VDDIO_Q ) ( FILLER_603 VDDIO_Q )
       ( FILLER_375 VDDIO_Q ) ( FILLER_602 VDDIO_Q )
       ( FILLER_374 VDDIO_Q ) ( disconnect_vdda_2 VDDIO_Q )
       ( FILLER_SB2 VDDIO_Q ) ( FILLER_601 VDDIO_Q )
       ( FILLER_600 VDDIO_Q ) ( mgmt_vddio_hvclamp_pad\[0\] VDDIO_Q )
       ( FILLER_599 VDDIO_Q ) ( FILLER_370 VDDIO_Q )
       ( FILLER_369 VDDIO_Q ) ( FILLER_368 VDDIO_Q )
       ( FILLER_367 VDDIO_Q ) ( mprj_pads.area1_io_pad\[0\] VDDIO_Q )
       ( FILLER_597 VDDIO_Q ) ( FILLER_366 VDDIO_Q )
       ( FILLER_596 VDDIO_Q ) ( FILLER_365 VDDIO_Q )
       ( FILLER_595 VDDIO_Q ) ( FILLER_364 VDDIO_Q )
       ( FILLER_594 VDDIO_Q ) ( FILLER_363 VDDIO_Q )
       ( FILLER_593 VDDIO_Q ) ( FILLER_362 VDDIO_Q )
       ( FILLER_592 VDDIO_Q ) ( FILLER_591 VDDIO_Q )
       ( FILLER_590 VDDIO_Q ) ( disconnect_vdda_1 VDDIO_Q )
       ( FILLER_SB1 VDDIO_Q ) ( FILLER_587 VDDIO_Q )
       ( mgmt_vccd_lvclamp_pad VDDIO_Q ) ( FILLER_360 VDDIO_Q )
       ( FILLER_359 VDDIO_Q ) ( FILLER_358 VDDIO_Q )
       ( FILLER_586 VDDIO_Q ) ( FILLER_357 VDDIO_Q )
       ( FILLER_585 VDDIO_Q ) ( FILLER_356 VDDIO_Q )
       ( FILLER_584 VDDIO_Q ) ( FILLER_583 VDDIO_Q )
       ( FILLER_355 VDDIO_Q ) ( FILLER_582 VDDIO_Q )
       ( FILLER_354 VDDIO_Q ) ( FILLER_581 VDDIO_Q )
       ( FILLER_353 VDDIO_Q ) ( mgmt_corner\[1\] VDDIO_Q )
       ( FILLER_352 VDDIO_Q ) ( FILLER_580 VDDIO_Q )
       ( FILLER_351 VDDIO_Q ) ( FILLER_350 VDDIO_Q )
       ( FILLER_349 VDDIO_Q ) ( FILLER_348 VDDIO_Q )
       ( FILLER_347 VDDIO_Q ) ( FILLER_346 VDDIO_Q )
       ( bus_tie_72 VDDIO_Q ) ( bus_tie_71 VDDIO_Q )
       ( bus_tie_70 VDDIO_Q ) ( bus_tie_69 VDDIO_Q )
       ( bus_tie_68 VDDIO_Q ) ( bus_tie_67 VDDIO_Q )
       ( FILLER_339 VDDIO_Q ) ( FILLER_338 VDDIO_Q )
       ( FILLER_337 VDDIO_Q ) ( FILLER_336 VDDIO_Q )
       ( FILLER_335 VDDIO_Q ) ( mgmt_vdda_hvclamp_pad VDDIO_Q )
       ( FILLER_333 VDDIO_Q ) ( FILLER_332 VDDIO_Q )
       ( FILLER_331 VDDIO_Q ) ( FILLER_330 VDDIO_Q )
       ( bus_tie_66 VDDIO_Q ) ( FILLER_329 VDDIO_Q )
       ( bus_tie_65 VDDIO_Q ) ( bus_tie_64 VDDIO_Q )
       ( bus_tie_63 VDDIO_Q ) ( bus_tie_62 VDDIO_Q )
       ( bus_tie_61 VDDIO_Q ) ( FILLER_322 VDDIO_Q )
       ( FILLER_321 VDDIO_Q ) ( FILLER_320 VDDIO_Q )
       ( FILLER_319 VDDIO_Q ) ( FILLER_318 VDDIO_Q )
       ( mgmt_vssio_hvclamp_pad\[0\] VDDIO_Q ) ( FILLER_316 VDDIO_Q )
       ( FILLER_315 VDDIO_Q ) ( FILLER_314 VDDIO_Q )
       ( FILLER_313 VDDIO_Q ) ( bus_tie_60 VDDIO_Q )
       ( FILLER_312 VDDIO_Q ) ( bus_tie_59 VDDIO_Q )
       ( bus_tie_58 VDDIO_Q ) ( bus_tie_57 VDDIO_Q )
       ( bus_tie_56 VDDIO_Q ) ( bus_tie_55 VDDIO_Q )
       ( FILLER_305 VDDIO_Q ) ( FILLER_304 VDDIO_Q )
       ( FILLER_303 VDDIO_Q ) ( FILLER_302 VDDIO_Q )
       ( FILLER_301 VDDIO_Q ) ( clock_pad VDDIO_Q )
       ( FILLER_299 VDDIO_Q ) ( FILLER_298 VDDIO_Q )
       ( FILLER_297 VDDIO_Q ) ( FILLER_296 VDDIO_Q )
       ( FILLER_295 VDDIO_Q ) ( bus_tie_54 VDDIO_Q )
       ( bus_tie_53 VDDIO_Q ) ( bus_tie_52 VDDIO_Q )
       ( bus_tie_51 VDDIO_Q ) ( bus_tie_50 VDDIO_Q )
       ( bus_tie_49 VDDIO_Q ) ( FILLER_288 VDDIO_Q )
       ( FILLER_287 VDDIO_Q ) ( FILLER_286 VDDIO_Q )
       ( FILLER_285 VDDIO_Q ) ( FILLER_284 VDDIO_Q )
       ( flash_io1_pad VDDIO_Q ) ( FILLER_282 VDDIO_Q )
       ( FILLER_281 VDDIO_Q ) ( FILLER_280 VDDIO_Q )
       ( FILLER_279 VDDIO_Q ) ( bus_tie_48 VDDIO_Q )
       ( FILLER_278 VDDIO_Q ) ( bus_tie_47 VDDIO_Q )
       ( bus_tie_46 VDDIO_Q ) ( bus_tie_45 VDDIO_Q )
       ( bus_tie_44 VDDIO_Q ) ( bus_tie_43 VDDIO_Q )
       ( FILLER_271 VDDIO_Q ) ( FILLER_270 VDDIO_Q )
       ( FILLER_269 VDDIO_Q ) ( FILLER_268 VDDIO_Q )
       ( FILLER_267 VDDIO_Q ) ( flash_io0_pad VDDIO_Q )
       ( FILLER_265 VDDIO_Q ) ( FILLER_264 VDDIO_Q )
       ( FILLER_263 VDDIO_Q ) ( FILLER_262 VDDIO_Q )
       ( FILLER_261 VDDIO_Q ) ( bus_tie_42 VDDIO_Q )
       ( bus_tie_41 VDDIO_Q ) ( bus_tie_40 VDDIO_Q )
       ( bus_tie_39 VDDIO_Q ) ( bus_tie_38 VDDIO_Q )
       ( bus_tie_37 VDDIO_Q ) ( FILLER_254 VDDIO_Q )
       ( FILLER_253 VDDIO_Q ) ( FILLER_252 VDDIO_Q )
       ( FILLER_251 VDDIO_Q ) ( FILLER_250 VDDIO_Q )
       ( flash_clk_pad VDDIO_Q ) ( FILLER_248 VDDIO_Q )
       ( FILLER_247 VDDIO_Q ) ( FILLER_246 VDDIO_Q )
       ( FILLER_245 VDDIO_Q ) ( bus_tie_36 VDDIO_Q )
       ( FILLER_244 VDDIO_Q ) ( bus_tie_35 VDDIO_Q )
       ( bus_tie_34 VDDIO_Q ) ( bus_tie_33 VDDIO_Q )
       ( bus_tie_32 VDDIO_Q ) ( bus_tie_31 VDDIO_Q )
       ( FILLER_237 VDDIO_Q ) ( FILLER_236 VDDIO_Q )
       ( FILLER_235 VDDIO_Q ) ( FILLER_234 VDDIO_Q )
       ( FILLER_233 VDDIO_Q ) ( flash_csb_pad VDDIO_Q )
       ( FILLER_231 VDDIO_Q ) ( FILLER_230 VDDIO_Q )
       ( FILLER_229 VDDIO_Q ) ( FILLER_228 VDDIO_Q )
       ( FILLER_227 VDDIO_Q ) ( bus_tie_30 VDDIO_Q )
       ( bus_tie_29 VDDIO_Q ) ( bus_tie_28 VDDIO_Q )
       ( bus_tie_27 VDDIO_Q ) ( bus_tie_26 VDDIO_Q )
       ( bus_tie_25 VDDIO_Q ) ( FILLER_220 VDDIO_Q )
       ( FILLER_219 VDDIO_Q ) ( FILLER_218 VDDIO_Q )
       ( FILLER_217 VDDIO_Q ) ( FILLER_216 VDDIO_Q )
       ( mgmt_vssd_lvclamp_pad VDDIO_Q ) ( FILLER_214 VDDIO_Q )
       ( FILLER_213 VDDIO_Q ) ( FILLER_212 VDDIO_Q )
       ( FILLER_211 VDDIO_Q ) ( bus_tie_24 VDDIO_Q )
       ( FILLER_210 VDDIO_Q ) ( bus_tie_23 VDDIO_Q )
       ( bus_tie_22 VDDIO_Q ) ( bus_tie_21 VDDIO_Q )
       ( bus_tie_20 VDDIO_Q ) ( bus_tie_19 VDDIO_Q )
       ( FILLER_203 VDDIO_Q ) ( FILLER_202 VDDIO_Q )
       ( FILLER_201 VDDIO_Q ) ( FILLER_200 VDDIO_Q )
       ( FILLER_199 VDDIO_Q ) ( bus_tie_9 VDDIO_Q )
       ( FILLER_197 VDDIO_Q ) ( FILLER_196 VDDIO_Q )
       ( FILLER_195 VDDIO_Q ) ( FILLER_194 VDDIO_Q )
       ( bus_tie_18 VDDIO_Q ) ( FILLER_193 VDDIO_Q )
       ( bus_tie_17 VDDIO_Q ) ( bus_tie_16 VDDIO_Q )
       ( bus_tie_15 VDDIO_Q ) ( bus_tie_14 VDDIO_Q )
       ( bus_tie_13 VDDIO_Q ) ( FILLER_186 VDDIO_Q )
       ( FILLER_185 VDDIO_Q ) ( FILLER_184 VDDIO_Q )
       ( FILLER_183 VDDIO_Q ) ( FILLER_182 VDDIO_Q )
       ( resetb_pad VDDIO_Q ) ( FILLER_180 VDDIO_Q )
       ( FILLER_179 VDDIO_Q ) ( FILLER_178 VDDIO_Q )
       ( FILLER_177 VDDIO_Q ) ( FILLER_176 VDDIO_Q )
       ( bus_tie_12 VDDIO_Q ) ( bus_tie_11 VDDIO_Q )
       ( bus_tie_10 VDDIO_Q ) ( bus_tie_8 VDDIO_Q )
       ( bus_tie_7 VDDIO_Q ) ( bus_tie_6 VDDIO_Q )
       ( FILLER_169 VDDIO_Q ) ( FILLER_168 VDDIO_Q )
       ( FILLER_167 VDDIO_Q ) ( FILLER_166 VDDIO_Q )
       ( FILLER_165 VDDIO_Q ) ( mgmt_vssa_hvclamp_pad VDDIO_Q )
       ( FILLER_163 VDDIO_Q ) ( FILLER_162 VDDIO_Q )
       ( FILLER_161 VDDIO_Q ) ( FILLER_160 VDDIO_Q )
       ( bus_tie_5 VDDIO_Q ) ( FILLER_159 VDDIO_Q )
       ( bus_tie_4 VDDIO_Q ) ( bus_tie_3 VDDIO_Q )
       ( bus_tie_2 VDDIO_Q ) ( bus_tie_1 VDDIO_Q )
       ( FILLER_152 VDDIO_Q ) ( FILLER_151 VDDIO_Q )
       ( FILLER_150 VDDIO_Q ) ( FILLER_149 VDDIO_Q )
       ( FILLER_148 VDDIO_Q ) ( mgmt_corner\[0\] VDDIO_Q ) ;
   - gpio_pad/VSSIO_Q ( gpio_pad VSSIO_Q ) ( FILLER_147 VSSIO_Q )
       ( FILLER_146 VSSIO_Q ) ( FILLER_145 VSSIO_Q )
       ( FILLER_144 VSSIO_Q ) ( FILLER_143 VSSIO_Q )
       ( FILLER_142 VSSIO_Q ) ( FILLER_141 VSSIO_Q )
       ( FILLER_140 VSSIO_Q ) ( FILLER_139 VSSIO_Q )
       ( FILLER_138 VSSIO_Q ) ( FILLER_137 VSSIO_Q )
       ( FILLER_136 VSSIO_Q ) ( FILLER_135 VSSIO_Q )
       ( user1_analog_pad\[0\] VSSIO_Q ) ( FILLER_133 VSSIO_Q )
       ( FILLER_132 VSSIO_Q ) ( FILLER_131 VSSIO_Q )
       ( FILLER_130 VSSIO_Q ) ( FILLER_129 VSSIO_Q )
       ( FILLER_128 VSSIO_Q ) ( FILLER_127 VSSIO_Q )
       ( FILLER_126 VSSIO_Q ) ( FILLER_125 VSSIO_Q )
       ( FILLER_124 VSSIO_Q ) ( FILLER_123 VSSIO_Q )
       ( user1_vssa_hvclamp_pad\[0\] VSSIO_Q ) ( FILLER_121 VSSIO_Q )
       ( FILLER_120 VSSIO_Q ) ( FILLER_119 VSSIO_Q )
       ( FILLER_118 VSSIO_Q ) ( FILLER_117 VSSIO_Q )
       ( FILLER_116 VSSIO_Q ) ( FILLER_115 VSSIO_Q )
       ( FILLER_114 VSSIO_Q ) ( FILLER_113 VSSIO_Q )
       ( FILLER_112 VSSIO_Q ) ( FILLER_111 VSSIO_Q )
       ( FILLER_110 VSSIO_Q ) ( user1_analog_pad\[1\] VSSIO_Q )
       ( FILLER_108 VSSIO_Q ) ( FILLER_107 VSSIO_Q )
       ( FILLER_106 VSSIO_Q ) ( FILLER_105 VSSIO_Q )
       ( FILLER_104 VSSIO_Q ) ( FILLER_103 VSSIO_Q )
       ( FILLER_102 VSSIO_Q ) ( FILLER_101 VSSIO_Q )
       ( FILLER_100 VSSIO_Q ) ( FILLER_99 VSSIO_Q )
       ( FILLER_98 VSSIO_Q ) ( user1_analog_pad\[2\] VSSIO_Q )
       ( FILLER_96 VSSIO_Q ) ( FILLER_95 VSSIO_Q )
       ( FILLER_94 VSSIO_Q ) ( FILLER_93 VSSIO_Q )
       ( FILLER_92 VSSIO_Q ) ( FILLER_91 VSSIO_Q )
       ( FILLER_90 VSSIO_Q ) ( FILLER_89 VSSIO_Q )
       ( FILLER_88 VSSIO_Q ) ( FILLER_87 VSSIO_Q )
       ( FILLER_86 VSSIO_Q ) ( FILLER_85 VSSIO_Q )
       ( FILLER_84 VSSIO_Q ) ( FILLER_83 VSSIO_Q )
       ( FILLER_82 VSSIO_Q ) ( FILLER_81 VSSIO_Q )
       ( FILLER_80 VSSIO_Q ) ( FILLER_79 VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_10um_0 VSSIO_Q )
       ( FILLER_78 VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_1 VSSIO_Q )
       ( user1_analog_pad_with_clamp VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_0 VSSIO_Q )
       ( disconnect_vdda_0 VSSIO_Q ) ( FILLER_SB3 VSSIO_Q )
       ( FILLER_73 VSSIO_Q ) ( FILLER_72 VSSIO_Q )
       ( FILLER_71 VSSIO_Q ) ( FILLER_70 VSSIO_Q )
       ( FILLER_69 VSSIO_Q ) ( FILLER_68 VSSIO_Q )
       ( mgmt_vssio_hvclamp_pad\[1\] VSSIO_Q ) ( FILLER_66 VSSIO_Q )
       ( FILLER_65 VSSIO_Q ) ( FILLER_64 VSSIO_Q )
       ( FILLER_63 VSSIO_Q ) ( FILLER_62 VSSIO_Q )
       ( FILLER_61 VSSIO_Q ) ( FILLER_60 VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_10um_1 VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_3 VSSIO_Q )
       ( user2_analog_pad_with_clamp\[0\] VSSIO_Q )
       ( sky130_ef_io__com_bus_slice_5um_2 VSSIO_Q )
       ( FILLER_57 VSSIO_Q ) ( FILLER_56 VSSIO_Q )
       ( FILLER_55 VSSIO_Q ) ( FILLER_54 VSSIO_Q )
       ( FILLER_53 VSSIO_Q ) ( FILLER_52 VSSIO_Q )
       ( FILLER_51 VSSIO_Q ) ( FILLER_50 VSSIO_Q )
       ( FILLER_49 VSSIO_Q )
       ( user2_analog_pad_with_clamp\[1\] VSSIO_Q )
       ( FILLER_47 VSSIO_Q ) ( FILLER_46 VSSIO_Q )
       ( FILLER_45 VSSIO_Q ) ( FILLER_44 VSSIO_Q )
       ( FILLER_43 VSSIO_Q ) ( FILLER_42 VSSIO_Q )
       ( user2_analog_pad\[0\] VSSIO_Q ) ( FILLER_41 VSSIO_Q )
       ( FILLER_39 VSSIO_Q ) ( FILLER_38 VSSIO_Q )
       ( FILLER_37 VSSIO_Q ) ( FILLER_36 VSSIO_Q )
       ( FILLER_35 VSSIO_Q ) ( FILLER_34 VSSIO_Q )
       ( FILLER_33 VSSIO_Q ) ( FILLER_32 VSSIO_Q )
       ( FILLER_31 VSSIO_Q ) ( FILLER_30 VSSIO_Q )
       ( FILLER_29 VSSIO_Q ) ( user2_analog_pad\[1\] VSSIO_Q )
       ( FILLER_27 VSSIO_Q ) ( FILLER_26 VSSIO_Q )
       ( FILLER_25 VSSIO_Q ) ( FILLER_24 VSSIO_Q )
       ( FILLER_23 VSSIO_Q ) ( FILLER_22 VSSIO_Q )
       ( FILLER_21 VSSIO_Q ) ( FILLER_20 VSSIO_Q )
       ( FILLER_19 VSSIO_Q ) ( FILLER_18 VSSIO_Q )
       ( FILLER_17 VSSIO_Q ) ( user2_analog_pad\[2\] VSSIO_Q )
       ( FILLER_15 VSSIO_Q ) ( FILLER_14 VSSIO_Q )
       ( FILLER_13 VSSIO_Q ) ( FILLER_12 VSSIO_Q )
       ( FILLER_11 VSSIO_Q ) ( FILLER_10 VSSIO_Q )
       ( FILLER_9 VSSIO_Q ) ( FILLER_8 VSSIO_Q ) ( FILLER_7 VSSIO_Q )
       ( FILLER_6 VSSIO_Q ) ( user2_corner VSSIO_Q )
       ( FILLER_5 VSSIO_Q ) ( FILLER_579 VSSIO_Q )
       ( FILLER_578 VSSIO_Q ) ( user1_corner VSSIO_Q )
       ( FILLER_786 VSSIO_Q ) ( FILLER_577 VSSIO_Q )
       ( FILLER_576 VSSIO_Q ) ( FILLER_785 VSSIO_Q )
       ( FILLER_575 VSSIO_Q ) ( FILLER_784 VSSIO_Q )
       ( FILLER_574 VSSIO_Q ) ( FILLER_783 VSSIO_Q )
       ( FILLER_573 VSSIO_Q ) ( FILLER_782 VSSIO_Q )
       ( FILLER_572 VSSIO_Q ) ( FILLER_781 VSSIO_Q )
       ( FILLER_571 VSSIO_Q ) ( FILLER_780 VSSIO_Q )
       ( FILLER_779 VSSIO_Q ) ( FILLER_570 VSSIO_Q )
       ( user2_analog_pad\[3\] VSSIO_Q ) ( FILLER_776 VSSIO_Q )
       ( FILLER_568 VSSIO_Q ) ( user1_analog_pad\[3\] VSSIO_Q )
       ( FILLER_567 VSSIO_Q ) ( FILLER_777 VSSIO_Q )
       ( FILLER_775 VSSIO_Q ) ( FILLER_566 VSSIO_Q )
       ( FILLER_774 VSSIO_Q ) ( FILLER_565 VSSIO_Q )
       ( FILLER_773 VSSIO_Q ) ( FILLER_564 VSSIO_Q )
       ( FILLER_772 VSSIO_Q ) ( FILLER_563 VSSIO_Q )
       ( FILLER_771 VSSIO_Q ) ( FILLER_562 VSSIO_Q )
       ( FILLER_561 VSSIO_Q ) ( FILLER_770 VSSIO_Q )
       ( FILLER_769 VSSIO_Q ) ( user2_vccd_lvclamp_pad VSSIO_Q )
       ( FILLER_559 VSSIO_Q ) ( FILLER_558 VSSIO_Q )
       ( FILLER_557 VSSIO_Q ) ( user1_vccd_lvclamp_pad VSSIO_Q )
       ( FILLER_767 VSSIO_Q ) ( FILLER_766 VSSIO_Q )
       ( FILLER_556 VSSIO_Q ) ( FILLER_765 VSSIO_Q )
       ( FILLER_555 VSSIO_Q ) ( FILLER_764 VSSIO_Q )
       ( FILLER_554 VSSIO_Q ) ( FILLER_763 VSSIO_Q )
       ( FILLER_553 VSSIO_Q ) ( FILLER_762 VSSIO_Q )
       ( FILLER_552 VSSIO_Q ) ( FILLER_761 VSSIO_Q )
       ( FILLER_551 VSSIO_Q ) ( FILLER_760 VSSIO_Q )
       ( mgmt_vddio_hvclamp_pad\[1\] VSSIO_Q ) ( FILLER_759 VSSIO_Q )
       ( FILLER_549 VSSIO_Q ) ( FILLER_548 VSSIO_Q )
       ( FILLER_547 VSSIO_Q ) ( FILLER_546 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[13\] VSSIO_Q ) ( FILLER_757 VSSIO_Q )
       ( FILLER_545 VSSIO_Q ) ( FILLER_756 VSSIO_Q )
       ( FILLER_544 VSSIO_Q ) ( FILLER_755 VSSIO_Q )
       ( FILLER_543 VSSIO_Q ) ( FILLER_754 VSSIO_Q )
       ( FILLER_542 VSSIO_Q ) ( FILLER_753 VSSIO_Q )
       ( FILLER_541 VSSIO_Q ) ( FILLER_752 VSSIO_Q )
       ( FILLER_751 VSSIO_Q ) ( user2_vssa_hvclamp_pad VSSIO_Q )
       ( FILLER_750 VSSIO_Q ) ( FILLER_539 VSSIO_Q )
       ( FILLER_538 VSSIO_Q ) ( FILLER_537 VSSIO_Q )
       ( FILLER_536 VSSIO_Q ) ( user1_vdda_hvclamp_pad\[0\] VSSIO_Q )
       ( FILLER_748 VSSIO_Q ) ( FILLER_747 VSSIO_Q )
       ( FILLER_535 VSSIO_Q ) ( FILLER_746 VSSIO_Q )
       ( FILLER_534 VSSIO_Q ) ( FILLER_745 VSSIO_Q )
       ( FILLER_533 VSSIO_Q ) ( FILLER_744 VSSIO_Q )
       ( FILLER_532 VSSIO_Q ) ( FILLER_743 VSSIO_Q )
       ( FILLER_531 VSSIO_Q ) ( FILLER_742 VSSIO_Q )
       ( FILLER_741 VSSIO_Q ) ( FILLER_740 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[0\] VSSIO_Q ) ( FILLER_529 VSSIO_Q )
       ( FILLER_528 VSSIO_Q ) ( FILLER_527 VSSIO_Q )
       ( FILLER_526 VSSIO_Q ) ( mprj_pads.area1_io_pad\[12\] VSSIO_Q )
       ( FILLER_525 VSSIO_Q ) ( FILLER_738 VSSIO_Q )
       ( FILLER_524 VSSIO_Q ) ( FILLER_737 VSSIO_Q )
       ( FILLER_523 VSSIO_Q ) ( FILLER_736 VSSIO_Q )
       ( FILLER_522 VSSIO_Q ) ( FILLER_735 VSSIO_Q )
       ( FILLER_734 VSSIO_Q ) ( FILLER_521 VSSIO_Q )
       ( FILLER_733 VSSIO_Q ) ( FILLER_732 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[1\] VSSIO_Q ) ( FILLER_731 VSSIO_Q )
       ( FILLER_519 VSSIO_Q ) ( FILLER_518 VSSIO_Q )
       ( FILLER_517 VSSIO_Q ) ( FILLER_516 VSSIO_Q )
       ( FILLER_515 VSSIO_Q ) ( mprj_pads.area1_io_pad\[11\] VSSIO_Q )
       ( FILLER_729 VSSIO_Q ) ( FILLER_514 VSSIO_Q )
       ( FILLER_728 VSSIO_Q ) ( FILLER_513 VSSIO_Q )
       ( FILLER_727 VSSIO_Q ) ( FILLER_512 VSSIO_Q )
       ( FILLER_726 VSSIO_Q ) ( FILLER_511 VSSIO_Q )
       ( FILLER_725 VSSIO_Q ) ( FILLER_724 VSSIO_Q )
       ( FILLER_723 VSSIO_Q ) ( FILLER_722 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[2\] VSSIO_Q ) ( FILLER_509 VSSIO_Q )
       ( FILLER_508 VSSIO_Q ) ( FILLER_507 VSSIO_Q )
       ( FILLER_506 VSSIO_Q ) ( FILLER_505 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[10\] VSSIO_Q ) ( FILLER_720 VSSIO_Q )
       ( FILLER_719 VSSIO_Q ) ( FILLER_504 VSSIO_Q )
       ( FILLER_718 VSSIO_Q ) ( FILLER_503 VSSIO_Q )
       ( FILLER_717 VSSIO_Q ) ( FILLER_502 VSSIO_Q )
       ( FILLER_501 VSSIO_Q ) ( FILLER_716 VSSIO_Q )
       ( FILLER_715 VSSIO_Q ) ( FILLER_714 VSSIO_Q )
       ( FILLER_713 VSSIO_Q ) ( FILLER_712 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[3\] VSSIO_Q ) ( FILLER_499 VSSIO_Q )
       ( FILLER_498 VSSIO_Q ) ( FILLER_497 VSSIO_Q )
       ( FILLER_496 VSSIO_Q ) ( FILLER_495 VSSIO_Q )
       ( FILLER_494 VSSIO_Q ) ( mprj_pads.area1_io_pad\[9\] VSSIO_Q )
       ( FILLER_710 VSSIO_Q ) ( FILLER_493 VSSIO_Q )
       ( FILLER_709 VSSIO_Q ) ( FILLER_492 VSSIO_Q )
       ( FILLER_708 VSSIO_Q ) ( FILLER_491 VSSIO_Q )
       ( FILLER_707 VSSIO_Q ) ( FILLER_706 VSSIO_Q )
       ( FILLER_705 VSSIO_Q ) ( FILLER_704 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[4\] VSSIO_Q ) ( FILLER_489 VSSIO_Q )
       ( FILLER_488 VSSIO_Q ) ( FILLER_703 VSSIO_Q )
       ( FILLER_487 VSSIO_Q ) ( FILLER_486 VSSIO_Q )
       ( FILLER_485 VSSIO_Q ) ( FILLER_484 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[8\] VSSIO_Q ) ( FILLER_701 VSSIO_Q )
       ( FILLER_483 VSSIO_Q ) ( FILLER_700 VSSIO_Q )
       ( FILLER_482 VSSIO_Q ) ( FILLER_699 VSSIO_Q )
       ( FILLER_481 VSSIO_Q ) ( FILLER_698 VSSIO_Q )
       ( FILLER_697 VSSIO_Q ) ( FILLER_696 VSSIO_Q )
       ( FILLER_695 VSSIO_Q ) ( FILLER_694 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[5\] VSSIO_Q ) ( FILLER_479 VSSIO_Q )
       ( FILLER_478 VSSIO_Q ) ( FILLER_477 VSSIO_Q )
       ( FILLER_693 VSSIO_Q ) ( FILLER_476 VSSIO_Q )
       ( FILLER_475 VSSIO_Q ) ( FILLER_474 VSSIO_Q )
       ( FILLER_473 VSSIO_Q ) ( mprj_pads.area1_io_pad\[7\] VSSIO_Q )
       ( FILLER_691 VSSIO_Q ) ( FILLER_472 VSSIO_Q )
       ( FILLER_690 VSSIO_Q ) ( FILLER_471 VSSIO_Q )
       ( FILLER_689 VSSIO_Q ) ( FILLER_688 VSSIO_Q )
       ( FILLER_687 VSSIO_Q ) ( FILLER_686 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[6\] VSSIO_Q ) ( FILLER_469 VSSIO_Q )
       ( FILLER_468 VSSIO_Q ) ( FILLER_685 VSSIO_Q )
       ( FILLER_467 VSSIO_Q ) ( FILLER_684 VSSIO_Q )
       ( FILLER_466 VSSIO_Q ) ( FILLER_465 VSSIO_Q )
       ( FILLER_464 VSSIO_Q ) ( FILLER_463 VSSIO_Q )
       ( user1_vdda_hvclamp_pad\[1\] VSSIO_Q ) ( FILLER_682 VSSIO_Q )
       ( FILLER_462 VSSIO_Q ) ( FILLER_681 VSSIO_Q )
       ( FILLER_461 VSSIO_Q ) ( FILLER_680 VSSIO_Q )
       ( FILLER_679 VSSIO_Q ) ( FILLER_678 VSSIO_Q )
       ( FILLER_677 VSSIO_Q ) ( user2_vdda_hvclamp_pad VSSIO_Q )
       ( FILLER_459 VSSIO_Q ) ( FILLER_458 VSSIO_Q )
       ( FILLER_457 VSSIO_Q ) ( FILLER_676 VSSIO_Q )
       ( FILLER_675 VSSIO_Q ) ( FILLER_456 VSSIO_Q )
       ( FILLER_455 VSSIO_Q ) ( FILLER_454 VSSIO_Q )
       ( FILLER_453 VSSIO_Q ) ( user1_vssd_lvclamp_pad VSSIO_Q )
       ( FILLER_673 VSSIO_Q ) ( FILLER_452 VSSIO_Q )
       ( FILLER_672 VSSIO_Q ) ( FILLER_671 VSSIO_Q )
       ( FILLER_451 VSSIO_Q ) ( FILLER_670 VSSIO_Q )
       ( FILLER_669 VSSIO_Q ) ( FILLER_668 VSSIO_Q )
       ( user2_vssd_lvclamp_pad VSSIO_Q ) ( FILLER_449 VSSIO_Q )
       ( FILLER_667 VSSIO_Q ) ( FILLER_448 VSSIO_Q )
       ( FILLER_447 VSSIO_Q ) ( FILLER_666 VSSIO_Q )
       ( FILLER_446 VSSIO_Q ) ( FILLER_665 VSSIO_Q )
       ( FILLER_445 VSSIO_Q ) ( FILLER_444 VSSIO_Q )
       ( FILLER_443 VSSIO_Q ) ( FILLER_442 VSSIO_Q )
       ( user1_vssa_hvclamp_pad\[1\] VSSIO_Q ) ( FILLER_663 VSSIO_Q )
       ( FILLER_441 VSSIO_Q ) ( FILLER_662 VSSIO_Q )
       ( FILLER_661 VSSIO_Q ) ( FILLER_660 VSSIO_Q )
       ( FILLER_659 VSSIO_Q ) ( mprj_pads.area2_io_pad\[7\] VSSIO_Q )
       ( FILLER_439 VSSIO_Q ) ( FILLER_438 VSSIO_Q )
       ( FILLER_658 VSSIO_Q ) ( FILLER_437 VSSIO_Q )
       ( FILLER_657 VSSIO_Q ) ( FILLER_436 VSSIO_Q )
       ( FILLER_656 VSSIO_Q ) ( FILLER_435 VSSIO_Q )
       ( FILLER_434 VSSIO_Q ) ( FILLER_433 VSSIO_Q )
       ( FILLER_432 VSSIO_Q ) ( mprj_pads.area1_io_pad\[6\] VSSIO_Q )
       ( FILLER_654 VSSIO_Q ) ( FILLER_431 VSSIO_Q )
       ( FILLER_653 VSSIO_Q ) ( FILLER_652 VSSIO_Q )
       ( FILLER_651 VSSIO_Q ) ( FILLER_650 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[8\] VSSIO_Q ) ( FILLER_649 VSSIO_Q )
       ( FILLER_429 VSSIO_Q ) ( FILLER_428 VSSIO_Q )
       ( FILLER_427 VSSIO_Q ) ( FILLER_648 VSSIO_Q )
       ( FILLER_426 VSSIO_Q ) ( FILLER_647 VSSIO_Q )
       ( FILLER_425 VSSIO_Q ) ( FILLER_646 VSSIO_Q )
       ( FILLER_424 VSSIO_Q ) ( FILLER_423 VSSIO_Q )
       ( FILLER_422 VSSIO_Q ) ( FILLER_421 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[5\] VSSIO_Q ) ( FILLER_644 VSSIO_Q )
       ( FILLER_643 VSSIO_Q ) ( FILLER_642 VSSIO_Q )
       ( FILLER_641 VSSIO_Q ) ( mprj_pads.area2_io_pad\[9\] VSSIO_Q )
       ( FILLER_419 VSSIO_Q ) ( FILLER_418 VSSIO_Q )
       ( FILLER_640 VSSIO_Q ) ( FILLER_417 VSSIO_Q )
       ( FILLER_639 VSSIO_Q ) ( FILLER_416 VSSIO_Q )
       ( FILLER_638 VSSIO_Q ) ( FILLER_415 VSSIO_Q )
       ( FILLER_637 VSSIO_Q ) ( FILLER_414 VSSIO_Q )
       ( FILLER_413 VSSIO_Q ) ( FILLER_412 VSSIO_Q )
       ( FILLER_411 VSSIO_Q ) ( mprj_pads.area1_io_pad\[4\] VSSIO_Q )
       ( FILLER_635 VSSIO_Q ) ( FILLER_634 VSSIO_Q )
       ( FILLER_633 VSSIO_Q ) ( mprj_pads.area2_io_pad\[10\] VSSIO_Q )
       ( FILLER_409 VSSIO_Q ) ( FILLER_632 VSSIO_Q )
       ( FILLER_408 VSSIO_Q ) ( FILLER_407 VSSIO_Q )
       ( FILLER_631 VSSIO_Q ) ( FILLER_406 VSSIO_Q )
       ( FILLER_630 VSSIO_Q ) ( FILLER_405 VSSIO_Q )
       ( FILLER_629 VSSIO_Q ) ( FILLER_404 VSSIO_Q )
       ( FILLER_628 VSSIO_Q ) ( FILLER_403 VSSIO_Q )
       ( FILLER_402 VSSIO_Q ) ( FILLER_401 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[3\] VSSIO_Q ) ( FILLER_626 VSSIO_Q )
       ( FILLER_625 VSSIO_Q ) ( FILLER_624 VSSIO_Q )
       ( FILLER_623 VSSIO_Q ) ( mprj_pads.area2_io_pad\[11\] VSSIO_Q )
       ( FILLER_399 VSSIO_Q ) ( FILLER_398 VSSIO_Q )
       ( FILLER_622 VSSIO_Q ) ( FILLER_397 VSSIO_Q )
       ( FILLER_621 VSSIO_Q ) ( FILLER_396 VSSIO_Q )
       ( FILLER_620 VSSIO_Q ) ( FILLER_395 VSSIO_Q )
       ( FILLER_619 VSSIO_Q ) ( FILLER_394 VSSIO_Q )
       ( FILLER_618 VSSIO_Q ) ( FILLER_393 VSSIO_Q )
       ( FILLER_392 VSSIO_Q ) ( FILLER_391 VSSIO_Q )
       ( mprj_pads.area1_io_pad\[2\] VSSIO_Q ) ( FILLER_616 VSSIO_Q )
       ( FILLER_615 VSSIO_Q ) ( FILLER_614 VSSIO_Q )
       ( mprj_pads.area2_io_pad\[12\] VSSIO_Q ) ( FILLER_389 VSSIO_Q )
       ( FILLER_388 VSSIO_Q ) ( FILLER_387 VSSIO_Q )
       ( FILLER_613 VSSIO_Q ) ( FILLER_386 VSSIO_Q )
       ( FILLER_612 VSSIO_Q ) ( FILLER_385 VSSIO_Q )
       ( FILLER_611 VSSIO_Q ) ( FILLER_384 VSSIO_Q )
       ( FILLER_610 VSSIO_Q ) ( FILLER_383 VSSIO_Q )
       ( FILLER_609 VSSIO_Q ) ( FILLER_382 VSSIO_Q )
       ( FILLER_381 VSSIO_Q ) ( FILLER_380 VSSIO_Q )
       ( FILLER_379 VSSIO_Q ) ( mprj_pads.area1_io_pad\[1\] VSSIO_Q )
       ( FILLER_607 VSSIO_Q ) ( FILLER_606 VSSIO_Q )
       ( FILLER_378 VSSIO_Q ) ( FILLER_605 VSSIO_Q )
       ( FILLER_377 VSSIO_Q ) ( FILLER_604 VSSIO_Q )
       ( FILLER_376 VSSIO_Q ) ( FILLER_603 VSSIO_Q )
       ( FILLER_375 VSSIO_Q ) ( FILLER_602 VSSIO_Q )
       ( FILLER_374 VSSIO_Q ) ( disconnect_vdda_2 VSSIO_Q )
       ( FILLER_SB2 VSSIO_Q ) ( FILLER_601 VSSIO_Q )
       ( FILLER_600 VSSIO_Q ) ( mgmt_vddio_hvclamp_pad\[0\] VSSIO_Q )
       ( FILLER_599 VSSIO_Q ) ( FILLER_370 VSSIO_Q )
       ( FILLER_369 VSSIO_Q ) ( FILLER_368 VSSIO_Q )
       ( FILLER_367 VSSIO_Q ) ( mprj_pads.area1_io_pad\[0\] VSSIO_Q )
       ( FILLER_597 VSSIO_Q ) ( FILLER_366 VSSIO_Q )
       ( FILLER_596 VSSIO_Q ) ( FILLER_365 VSSIO_Q )
       ( FILLER_595 VSSIO_Q ) ( FILLER_364 VSSIO_Q )
       ( FILLER_594 VSSIO_Q ) ( FILLER_363 VSSIO_Q )
       ( FILLER_593 VSSIO_Q ) ( FILLER_362 VSSIO_Q )
       ( FILLER_592 VSSIO_Q ) ( FILLER_591 VSSIO_Q )
       ( FILLER_590 VSSIO_Q ) ( disconnect_vdda_1 VSSIO_Q )
       ( FILLER_SB1 VSSIO_Q ) ( FILLER_587 VSSIO_Q )
       ( mgmt_vccd_lvclamp_pad VSSIO_Q ) ( FILLER_360 VSSIO_Q )
       ( FILLER_359 VSSIO_Q ) ( FILLER_358 VSSIO_Q )
       ( FILLER_586 VSSIO_Q ) ( FILLER_357 VSSIO_Q )
       ( FILLER_585 VSSIO_Q ) ( FILLER_356 VSSIO_Q )
       ( FILLER_584 VSSIO_Q ) ( FILLER_583 VSSIO_Q )
       ( FILLER_355 VSSIO_Q ) ( FILLER_582 VSSIO_Q )
       ( FILLER_354 VSSIO_Q ) ( FILLER_581 VSSIO_Q )
       ( FILLER_353 VSSIO_Q ) ( mgmt_corner\[1\] VSSIO_Q )
       ( FILLER_352 VSSIO_Q ) ( FILLER_580 VSSIO_Q )
       ( FILLER_351 VSSIO_Q ) ( FILLER_350 VSSIO_Q )
       ( FILLER_349 VSSIO_Q ) ( FILLER_348 VSSIO_Q )
       ( FILLER_347 VSSIO_Q ) ( FILLER_346 VSSIO_Q )
       ( bus_tie_72 VSSIO_Q ) ( bus_tie_71 VSSIO_Q )
       ( bus_tie_70 VSSIO_Q ) ( bus_tie_69 VSSIO_Q )
       ( bus_tie_68 VSSIO_Q ) ( bus_tie_67 VSSIO_Q )
       ( FILLER_339 VSSIO_Q ) ( FILLER_338 VSSIO_Q )
       ( FILLER_337 VSSIO_Q ) ( FILLER_336 VSSIO_Q )
       ( FILLER_335 VSSIO_Q ) ( mgmt_vdda_hvclamp_pad VSSIO_Q )
       ( FILLER_333 VSSIO_Q ) ( FILLER_332 VSSIO_Q )
       ( FILLER_331 VSSIO_Q ) ( FILLER_330 VSSIO_Q )
       ( bus_tie_66 VSSIO_Q ) ( FILLER_329 VSSIO_Q )
       ( bus_tie_65 VSSIO_Q ) ( bus_tie_64 VSSIO_Q )
       ( bus_tie_63 VSSIO_Q ) ( bus_tie_62 VSSIO_Q )
       ( bus_tie_61 VSSIO_Q ) ( FILLER_322 VSSIO_Q )
       ( FILLER_321 VSSIO_Q ) ( FILLER_320 VSSIO_Q )
       ( FILLER_319 VSSIO_Q ) ( FILLER_318 VSSIO_Q )
       ( mgmt_vssio_hvclamp_pad\[0\] VSSIO_Q ) ( FILLER_316 VSSIO_Q )
       ( FILLER_315 VSSIO_Q ) ( FILLER_314 VSSIO_Q )
       ( FILLER_313 VSSIO_Q ) ( bus_tie_60 VSSIO_Q )
       ( FILLER_312 VSSIO_Q ) ( bus_tie_59 VSSIO_Q )
       ( bus_tie_58 VSSIO_Q ) ( bus_tie_57 VSSIO_Q )
       ( bus_tie_56 VSSIO_Q ) ( bus_tie_55 VSSIO_Q )
       ( FILLER_305 VSSIO_Q ) ( FILLER_304 VSSIO_Q )
       ( FILLER_303 VSSIO_Q ) ( FILLER_302 VSSIO_Q )
       ( FILLER_301 VSSIO_Q ) ( clock_pad VSSIO_Q )
       ( FILLER_299 VSSIO_Q ) ( FILLER_298 VSSIO_Q )
       ( FILLER_297 VSSIO_Q ) ( FILLER_296 VSSIO_Q )
       ( FILLER_295 VSSIO_Q ) ( bus_tie_54 VSSIO_Q )
       ( bus_tie_53 VSSIO_Q ) ( bus_tie_52 VSSIO_Q )
       ( bus_tie_51 VSSIO_Q ) ( bus_tie_50 VSSIO_Q )
       ( bus_tie_49 VSSIO_Q ) ( FILLER_288 VSSIO_Q )
       ( FILLER_287 VSSIO_Q ) ( FILLER_286 VSSIO_Q )
       ( FILLER_285 VSSIO_Q ) ( FILLER_284 VSSIO_Q )
       ( flash_io1_pad VSSIO_Q ) ( FILLER_282 VSSIO_Q )
       ( FILLER_281 VSSIO_Q ) ( FILLER_280 VSSIO_Q )
       ( FILLER_279 VSSIO_Q ) ( bus_tie_48 VSSIO_Q )
       ( FILLER_278 VSSIO_Q ) ( bus_tie_47 VSSIO_Q )
       ( bus_tie_46 VSSIO_Q ) ( bus_tie_45 VSSIO_Q )
       ( bus_tie_44 VSSIO_Q ) ( bus_tie_43 VSSIO_Q )
       ( FILLER_271 VSSIO_Q ) ( FILLER_270 VSSIO_Q )
       ( FILLER_269 VSSIO_Q ) ( FILLER_268 VSSIO_Q )
       ( FILLER_267 VSSIO_Q ) ( flash_io0_pad VSSIO_Q )
       ( FILLER_265 VSSIO_Q ) ( FILLER_264 VSSIO_Q )
       ( FILLER_263 VSSIO_Q ) ( FILLER_262 VSSIO_Q )
       ( FILLER_261 VSSIO_Q ) ( bus_tie_42 VSSIO_Q )
       ( bus_tie_41 VSSIO_Q ) ( bus_tie_40 VSSIO_Q )
       ( bus_tie_39 VSSIO_Q ) ( bus_tie_38 VSSIO_Q )
       ( bus_tie_37 VSSIO_Q ) ( FILLER_254 VSSIO_Q )
       ( FILLER_253 VSSIO_Q ) ( FILLER_252 VSSIO_Q )
       ( FILLER_251 VSSIO_Q ) ( FILLER_250 VSSIO_Q )
       ( flash_clk_pad VSSIO_Q ) ( FILLER_248 VSSIO_Q )
       ( FILLER_247 VSSIO_Q ) ( FILLER_246 VSSIO_Q )
       ( FILLER_245 VSSIO_Q ) ( bus_tie_36 VSSIO_Q )
       ( FILLER_244 VSSIO_Q ) ( bus_tie_35 VSSIO_Q )
       ( bus_tie_34 VSSIO_Q ) ( bus_tie_33 VSSIO_Q )
       ( bus_tie_32 VSSIO_Q ) ( bus_tie_31 VSSIO_Q )
       ( FILLER_237 VSSIO_Q ) ( FILLER_236 VSSIO_Q )
       ( FILLER_235 VSSIO_Q ) ( FILLER_234 VSSIO_Q )
       ( FILLER_233 VSSIO_Q ) ( flash_csb_pad VSSIO_Q )
       ( FILLER_231 VSSIO_Q ) ( FILLER_230 VSSIO_Q )
       ( FILLER_229 VSSIO_Q ) ( FILLER_228 VSSIO_Q )
       ( FILLER_227 VSSIO_Q ) ( bus_tie_30 VSSIO_Q )
       ( bus_tie_29 VSSIO_Q ) ( bus_tie_28 VSSIO_Q )
       ( bus_tie_27 VSSIO_Q ) ( bus_tie_26 VSSIO_Q )
       ( bus_tie_25 VSSIO_Q ) ( FILLER_220 VSSIO_Q )
       ( FILLER_219 VSSIO_Q ) ( FILLER_218 VSSIO_Q )
       ( FILLER_217 VSSIO_Q ) ( FILLER_216 VSSIO_Q )
       ( mgmt_vssd_lvclamp_pad VSSIO_Q ) ( FILLER_214 VSSIO_Q )
       ( FILLER_213 VSSIO_Q ) ( FILLER_212 VSSIO_Q )
       ( FILLER_211 VSSIO_Q ) ( bus_tie_24 VSSIO_Q )
       ( FILLER_210 VSSIO_Q ) ( bus_tie_23 VSSIO_Q )
       ( bus_tie_22 VSSIO_Q ) ( bus_tie_21 VSSIO_Q )
       ( bus_tie_20 VSSIO_Q ) ( bus_tie_19 VSSIO_Q )
       ( FILLER_203 VSSIO_Q ) ( FILLER_202 VSSIO_Q )
       ( FILLER_201 VSSIO_Q ) ( FILLER_200 VSSIO_Q )
       ( FILLER_199 VSSIO_Q ) ( bus_tie_9 VSSIO_Q )
       ( FILLER_197 VSSIO_Q ) ( FILLER_196 VSSIO_Q )
       ( FILLER_195 VSSIO_Q ) ( FILLER_194 VSSIO_Q )
       ( bus_tie_18 VSSIO_Q ) ( FILLER_193 VSSIO_Q )
       ( bus_tie_17 VSSIO_Q ) ( bus_tie_16 VSSIO_Q )
       ( bus_tie_15 VSSIO_Q ) ( bus_tie_14 VSSIO_Q )
       ( bus_tie_13 VSSIO_Q ) ( FILLER_186 VSSIO_Q )
       ( FILLER_185 VSSIO_Q ) ( FILLER_184 VSSIO_Q )
       ( FILLER_183 VSSIO_Q ) ( FILLER_182 VSSIO_Q )
       ( resetb_pad VSSIO_Q ) ( FILLER_180 VSSIO_Q )
       ( FILLER_179 VSSIO_Q ) ( FILLER_178 VSSIO_Q )
       ( FILLER_177 VSSIO_Q ) ( FILLER_176 VSSIO_Q )
       ( bus_tie_12 VSSIO_Q ) ( bus_tie_11 VSSIO_Q )
       ( bus_tie_10 VSSIO_Q ) ( bus_tie_8 VSSIO_Q )
       ( bus_tie_7 VSSIO_Q ) ( bus_tie_6 VSSIO_Q )
       ( FILLER_169 VSSIO_Q ) ( FILLER_168 VSSIO_Q )
       ( FILLER_167 VSSIO_Q ) ( FILLER_166 VSSIO_Q )
       ( FILLER_165 VSSIO_Q ) ( mgmt_vssa_hvclamp_pad VSSIO_Q )
       ( FILLER_163 VSSIO_Q ) ( FILLER_162 VSSIO_Q )
       ( FILLER_161 VSSIO_Q ) ( FILLER_160 VSSIO_Q )
       ( bus_tie_5 VSSIO_Q ) ( FILLER_159 VSSIO_Q )
       ( bus_tie_4 VSSIO_Q ) ( bus_tie_3 VSSIO_Q )
       ( bus_tie_2 VSSIO_Q ) ( bus_tie_1 VSSIO_Q )
       ( FILLER_152 VSSIO_Q ) ( FILLER_151 VSSIO_Q )
       ( FILLER_150 VSSIO_Q ) ( FILLER_149 VSSIO_Q )
       ( FILLER_148 VSSIO_Q ) ( mgmt_corner\[0\] VSSIO_Q ) ;
   - vssa ( mgmt_vddio_hvclamp_pad\[0\] VSSA ) ( FILLER_370 VSSA )
       ( FILLER_369 VSSA ) ( FILLER_368 VSSA ) ( FILLER_367 VSSA )
       ( FILLER_366 VSSA ) ( FILLER_365 VSSA ) ( FILLER_364 VSSA )
       ( FILLER_363 VSSA ) ( FILLER_362 VSSA ) ( FILLER_587 VSSA )
       ( mgmt_vccd_lvclamp_pad VSSA ) ( FILLER_360 VSSA )
       ( FILLER_359 VSSA ) ( FILLER_358 VSSA ) ( FILLER_586 VSSA )
       ( FILLER_357 VSSA ) ( FILLER_585 VSSA ) ( FILLER_356 VSSA )
       ( FILLER_584 VSSA ) ( FILLER_583 VSSA ) ( FILLER_355 VSSA )
       ( FILLER_582 VSSA ) ( FILLER_354 VSSA ) ( FILLER_581 VSSA )
       ( FILLER_353 VSSA ) ( mgmt_corner\[1\] VSSA )
       ( FILLER_352 VSSA ) ( FILLER_580 VSSA ) ( FILLER_351 VSSA )
       ( FILLER_350 VSSA ) ( FILLER_349 VSSA ) ( FILLER_348 VSSA )
       ( FILLER_347 VSSA ) ( FILLER_346 VSSA ) ( bus_tie_72 VSSA )
       ( bus_tie_71 VSSA ) ( bus_tie_70 VSSA ) ( bus_tie_69 VSSA )
       ( bus_tie_68 VSSA ) ( bus_tie_67 VSSA ) ( FILLER_339 VSSA )
       ( FILLER_338 VSSA ) ( FILLER_337 VSSA ) ( FILLER_336 VSSA )
       ( FILLER_335 VSSA ) ( mgmt_vdda_hvclamp_pad VSSA )
       ( FILLER_333 VSSA ) ( FILLER_332 VSSA ) ( FILLER_331 VSSA )
       ( FILLER_330 VSSA ) ( bus_tie_66 VSSA ) ( FILLER_329 VSSA )
       ( bus_tie_65 VSSA ) ( bus_tie_64 VSSA ) ( bus_tie_63 VSSA )
       ( bus_tie_62 VSSA ) ( bus_tie_61 VSSA ) ( FILLER_322 VSSA )
       ( FILLER_321 VSSA ) ( FILLER_320 VSSA ) ( FILLER_319 VSSA )
       ( FILLER_318 VSSA ) ( mgmt_vssio_hvclamp_pad\[0\] VSSA )
       ( FILLER_316 VSSA ) ( FILLER_315 VSSA ) ( FILLER_314 VSSA )
       ( FILLER_313 VSSA ) ( bus_tie_60 VSSA ) ( FILLER_312 VSSA )
       ( bus_tie_59 VSSA ) ( bus_tie_58 VSSA ) ( bus_tie_57 VSSA )
       ( bus_tie_56 VSSA ) ( bus_tie_55 VSSA ) ( FILLER_305 VSSA )
       ( FILLER_304 VSSA ) ( FILLER_303 VSSA ) ( FILLER_302 VSSA )
       ( FILLER_301 VSSA ) ( gpio_pad VSSA ) ( FILLER_299 VSSA )
       ( FILLER_298 VSSA ) ( FILLER_297 VSSA ) ( FILLER_296 VSSA )
       ( FILLER_295 VSSA ) ( bus_tie_54 VSSA ) ( bus_tie_53 VSSA )
       ( bus_tie_52 VSSA ) ( bus_tie_51 VSSA ) ( bus_tie_50 VSSA )
       ( bus_tie_49 VSSA ) ( FILLER_288 VSSA ) ( FILLER_287 VSSA )
       ( FILLER_286 VSSA ) ( FILLER_285 VSSA ) ( FILLER_284 VSSA )
       ( flash_io1_pad VSSA ) ( FILLER_282 VSSA ) ( FILLER_281 VSSA )
       ( FILLER_280 VSSA ) ( FILLER_279 VSSA ) ( bus_tie_48 VSSA )
       ( FILLER_278 VSSA ) ( bus_tie_47 VSSA ) ( bus_tie_46 VSSA )
       ( bus_tie_45 VSSA ) ( bus_tie_44 VSSA ) ( bus_tie_43 VSSA )
       ( FILLER_271 VSSA ) ( FILLER_270 VSSA ) ( FILLER_269 VSSA )
       ( FILLER_268 VSSA ) ( FILLER_267 VSSA ) ( flash_io0_pad VSSA )
       ( FILLER_265 VSSA ) ( FILLER_264 VSSA ) ( FILLER_263 VSSA )
       ( FILLER_262 VSSA ) ( FILLER_261 VSSA ) ( bus_tie_42 VSSA )
       ( bus_tie_41 VSSA ) ( bus_tie_40 VSSA ) ( bus_tie_39 VSSA )
       ( bus_tie_38 VSSA ) ( bus_tie_37 VSSA ) ( FILLER_254 VSSA )
       ( FILLER_253 VSSA ) ( FILLER_252 VSSA ) ( FILLER_251 VSSA )
       ( FILLER_250 VSSA ) ( flash_clk_pad VSSA ) ( FILLER_248 VSSA )
       ( FILLER_247 VSSA ) ( FILLER_246 VSSA ) ( FILLER_245 VSSA )
       ( bus_tie_36 VSSA ) ( FILLER_244 VSSA ) ( bus_tie_35 VSSA )
       ( bus_tie_34 VSSA ) ( bus_tie_33 VSSA ) ( bus_tie_32 VSSA )
       ( bus_tie_31 VSSA ) ( FILLER_237 VSSA ) ( FILLER_236 VSSA )
       ( FILLER_235 VSSA ) ( FILLER_234 VSSA ) ( FILLER_233 VSSA )
       ( flash_csb_pad VSSA ) ( FILLER_231 VSSA ) ( FILLER_230 VSSA )
       ( FILLER_229 VSSA ) ( FILLER_228 VSSA ) ( FILLER_227 VSSA )
       ( bus_tie_30 VSSA ) ( bus_tie_29 VSSA ) ( bus_tie_28 VSSA )
       ( bus_tie_27 VSSA ) ( bus_tie_26 VSSA ) ( bus_tie_25 VSSA )
       ( FILLER_220 VSSA ) ( FILLER_219 VSSA ) ( FILLER_218 VSSA )
       ( FILLER_217 VSSA ) ( FILLER_216 VSSA )
       ( mgmt_vssd_lvclamp_pad VSSA ) ( FILLER_214 VSSA )
       ( FILLER_213 VSSA ) ( FILLER_212 VSSA ) ( FILLER_211 VSSA )
       ( bus_tie_24 VSSA ) ( FILLER_210 VSSA ) ( bus_tie_23 VSSA )
       ( bus_tie_22 VSSA ) ( bus_tie_21 VSSA ) ( bus_tie_20 VSSA )
       ( bus_tie_19 VSSA ) ( FILLER_203 VSSA ) ( FILLER_202 VSSA )
       ( FILLER_201 VSSA ) ( FILLER_200 VSSA ) ( FILLER_199 VSSA )
       ( clock_pad VSSA ) ( FILLER_197 VSSA ) ( FILLER_196 VSSA )
       ( FILLER_195 VSSA ) ( FILLER_194 VSSA ) ( bus_tie_18 VSSA )
       ( FILLER_193 VSSA ) ( bus_tie_17 VSSA ) ( bus_tie_16 VSSA )
       ( bus_tie_15 VSSA ) ( bus_tie_14 VSSA ) ( bus_tie_13 VSSA )
       ( FILLER_186 VSSA ) ( FILLER_185 VSSA ) ( FILLER_184 VSSA )
       ( FILLER_183 VSSA ) ( FILLER_182 VSSA ) ( resetb_pad VSSA )
       ( FILLER_180 VSSA ) ( bus_tie_9 VSSA ) ( FILLER_179 VSSA )
       ( FILLER_178 VSSA ) ( FILLER_177 VSSA ) ( FILLER_176 VSSA )
       ( bus_tie_12 VSSA ) ( bus_tie_11 VSSA ) ( bus_tie_10 VSSA )
       ( bus_tie_8 VSSA ) ( bus_tie_7 VSSA ) ( bus_tie_6 VSSA )
       ( FILLER_169 VSSA ) ( FILLER_168 VSSA ) ( FILLER_167 VSSA )
       ( FILLER_166 VSSA ) ( FILLER_165 VSSA )
       ( mgmt_vssa_hvclamp_pad VSSA ) ( FILLER_163 VSSA )
       ( FILLER_162 VSSA ) ( FILLER_161 VSSA ) ( FILLER_160 VSSA )
       ( bus_tie_5 VSSA ) ( FILLER_159 VSSA ) ( bus_tie_4 VSSA )
       ( bus_tie_3 VSSA ) ( bus_tie_2 VSSA ) ( bus_tie_1 VSSA )
       ( FILLER_152 VSSA ) ( FILLER_151 VSSA ) ( FILLER_150 VSSA )
       ( FILLER_149 VSSA ) ( FILLER_148 VSSA )
       ( mgmt_corner\[0\] VSSA )
      + ROUTED met4 TAPERRULE met4_width_330  ( 663150 143430 ) ( 737850 * ) ;
   - vssd ( FILLER_147 VSSD ) ( FILLER_146 VSSD ) ( FILLER_145 VSSD )
       ( FILLER_144 VSSD ) ( FILLER_143 VSSD ) ( FILLER_142 VSSD )
       ( FILLER_141 VSSD ) ( FILLER_140 VSSD ) ( FILLER_139 VSSD )
       ( FILLER_138 VSSD ) ( FILLER_137 VSSD ) ( FILLER_136 VSSD )
       ( FILLER_135 VSSD ) ( user1_analog_pad\[0\] VSSD )
       ( FILLER_133 VSSD ) ( FILLER_132 VSSD ) ( FILLER_131 VSSD )
       ( FILLER_130 VSSD ) ( FILLER_129 VSSD ) ( FILLER_128 VSSD )
       ( FILLER_127 VSSD ) ( FILLER_126 VSSD ) ( FILLER_125 VSSD )
       ( FILLER_124 VSSD ) ( FILLER_123 VSSD )
       ( user1_vssa_hvclamp_pad\[0\] VSSD ) ( FILLER_121 VSSD )
       ( FILLER_120 VSSD ) ( FILLER_119 VSSD ) ( FILLER_118 VSSD )
       ( FILLER_117 VSSD ) ( FILLER_116 VSSD ) ( FILLER_115 VSSD )
       ( FILLER_114 VSSD ) ( FILLER_113 VSSD ) ( FILLER_112 VSSD )
       ( FILLER_111 VSSD ) ( FILLER_110 VSSD )
       ( user1_analog_pad\[1\] VSSD ) ( FILLER_108 VSSD )
       ( FILLER_107 VSSD ) ( FILLER_106 VSSD ) ( FILLER_105 VSSD )
       ( FILLER_104 VSSD ) ( FILLER_103 VSSD ) ( FILLER_102 VSSD )
       ( FILLER_101 VSSD ) ( FILLER_100 VSSD ) ( FILLER_99 VSSD )
       ( FILLER_98 VSSD ) ( user1_analog_pad\[2\] VSSD )
       ( FILLER_96 VSSD ) ( FILLER_95 VSSD ) ( FILLER_94 VSSD )
       ( FILLER_93 VSSD ) ( FILLER_92 VSSD ) ( FILLER_91 VSSD )
       ( FILLER_90 VSSD ) ( FILLER_89 VSSD ) ( FILLER_88 VSSD )
       ( FILLER_87 VSSD ) ( FILLER_86 VSSD ) ( FILLER_85 VSSD )
       ( FILLER_84 VSSD ) ( FILLER_83 VSSD ) ( FILLER_82 VSSD )
       ( FILLER_81 VSSD ) ( FILLER_80 VSSD ) ( FILLER_79 VSSD )
       ( sky130_ef_io__com_bus_slice_10um_0 VSSD ) ( FILLER_78 VSSD )
       ( sky130_ef_io__com_bus_slice_5um_1 VSSD )
       ( user1_analog_pad_with_clamp VSSD )
       ( sky130_ef_io__com_bus_slice_5um_0 VSSD )
       ( disconnect_vdda_0 VSSD ) ( FILLER_SB3 VSSD )
       ( FILLER_73 VSSD ) ( FILLER_72 VSSD ) ( FILLER_71 VSSD )
       ( FILLER_70 VSSD ) ( FILLER_69 VSSD ) ( FILLER_68 VSSD )
       ( mgmt_vssio_hvclamp_pad\[1\] VSSD ) ( FILLER_66 VSSD )
       ( FILLER_65 VSSD ) ( FILLER_64 VSSD ) ( FILLER_63 VSSD )
       ( FILLER_62 VSSD ) ( FILLER_61 VSSD ) ( FILLER_60 VSSD )
       ( sky130_ef_io__com_bus_slice_10um_1 VSSD )
       ( sky130_ef_io__com_bus_slice_5um_3 VSSD )
       ( user2_analog_pad_with_clamp\[0\] VSSD )
       ( sky130_ef_io__com_bus_slice_5um_2 VSSD ) ( FILLER_57 VSSD )
       ( FILLER_56 VSSD ) ( FILLER_55 VSSD ) ( FILLER_54 VSSD )
       ( FILLER_53 VSSD ) ( FILLER_52 VSSD ) ( FILLER_51 VSSD )
       ( FILLER_50 VSSD ) ( FILLER_49 VSSD )
       ( user2_analog_pad_with_clamp\[1\] VSSD ) ( FILLER_47 VSSD )
       ( FILLER_46 VSSD ) ( FILLER_45 VSSD ) ( FILLER_44 VSSD )
       ( FILLER_43 VSSD ) ( FILLER_42 VSSD )
       ( user2_analog_pad\[0\] VSSD ) ( FILLER_41 VSSD )
       ( FILLER_39 VSSD ) ( FILLER_38 VSSD ) ( FILLER_37 VSSD )
       ( FILLER_36 VSSD ) ( FILLER_35 VSSD ) ( FILLER_34 VSSD )
       ( FILLER_33 VSSD ) ( FILLER_32 VSSD ) ( FILLER_31 VSSD )
       ( FILLER_30 VSSD ) ( FILLER_29 VSSD )
       ( user2_analog_pad\[1\] VSSD ) ( FILLER_27 VSSD )
       ( FILLER_26 VSSD ) ( FILLER_25 VSSD ) ( FILLER_24 VSSD )
       ( FILLER_23 VSSD ) ( FILLER_22 VSSD ) ( FILLER_21 VSSD )
       ( FILLER_20 VSSD ) ( FILLER_19 VSSD ) ( FILLER_18 VSSD )
       ( FILLER_17 VSSD ) ( user2_analog_pad\[2\] VSSD )
       ( FILLER_15 VSSD ) ( FILLER_14 VSSD ) ( FILLER_13 VSSD )
       ( FILLER_12 VSSD ) ( FILLER_11 VSSD ) ( FILLER_10 VSSD )
       ( FILLER_9 VSSD ) ( FILLER_8 VSSD ) ( FILLER_7 VSSD )
       ( FILLER_6 VSSD ) ( user2_corner VSSD ) ( FILLER_5 VSSD )
       ( FILLER_579 VSSD ) ( FILLER_578 VSSD ) ( user1_corner VSSD )
       ( FILLER_786 VSSD ) ( FILLER_577 VSSD ) ( FILLER_576 VSSD )
       ( FILLER_785 VSSD ) ( FILLER_575 VSSD ) ( FILLER_784 VSSD )
       ( FILLER_574 VSSD ) ( FILLER_783 VSSD ) ( FILLER_573 VSSD )
       ( FILLER_782 VSSD ) ( FILLER_572 VSSD ) ( FILLER_781 VSSD )
       ( FILLER_571 VSSD ) ( FILLER_780 VSSD ) ( FILLER_779 VSSD )
       ( FILLER_570 VSSD ) ( user2_analog_pad\[3\] VSSD )
       ( FILLER_776 VSSD ) ( FILLER_568 VSSD )
       ( user1_analog_pad\[3\] VSSD ) ( FILLER_567 VSSD )
       ( FILLER_777 VSSD ) ( FILLER_775 VSSD ) ( FILLER_566 VSSD )
       ( FILLER_774 VSSD ) ( FILLER_565 VSSD ) ( FILLER_773 VSSD )
       ( FILLER_564 VSSD ) ( FILLER_772 VSSD ) ( FILLER_563 VSSD )
       ( FILLER_771 VSSD ) ( FILLER_562 VSSD ) ( FILLER_561 VSSD )
       ( FILLER_770 VSSD ) ( FILLER_769 VSSD )
       ( user2_vccd_lvclamp_pad VSSD ) ( FILLER_559 VSSD )
       ( FILLER_558 VSSD ) ( FILLER_557 VSSD )
       ( user1_vccd_lvclamp_pad VSSD ) ( FILLER_767 VSSD )
       ( FILLER_766 VSSD ) ( FILLER_556 VSSD ) ( FILLER_765 VSSD )
       ( FILLER_555 VSSD ) ( FILLER_764 VSSD ) ( FILLER_554 VSSD )
       ( FILLER_763 VSSD ) ( FILLER_553 VSSD ) ( FILLER_762 VSSD )
       ( FILLER_552 VSSD ) ( FILLER_761 VSSD ) ( FILLER_551 VSSD )
       ( FILLER_760 VSSD ) ( mgmt_vddio_hvclamp_pad\[1\] VSSD )
       ( FILLER_759 VSSD ) ( FILLER_549 VSSD ) ( FILLER_548 VSSD )
       ( FILLER_547 VSSD ) ( FILLER_546 VSSD )
       ( mprj_pads.area1_io_pad\[13\] VSSD ) ( FILLER_757 VSSD )
       ( FILLER_545 VSSD ) ( FILLER_756 VSSD ) ( FILLER_544 VSSD )
       ( FILLER_755 VSSD ) ( FILLER_543 VSSD ) ( FILLER_754 VSSD )
       ( FILLER_542 VSSD ) ( FILLER_753 VSSD ) ( FILLER_541 VSSD )
       ( FILLER_752 VSSD ) ( FILLER_751 VSSD )
       ( user2_vssa_hvclamp_pad VSSD ) ( FILLER_750 VSSD )
       ( FILLER_539 VSSD ) ( FILLER_538 VSSD ) ( FILLER_537 VSSD )
       ( FILLER_536 VSSD ) ( user1_vdda_hvclamp_pad\[0\] VSSD )
       ( FILLER_748 VSSD ) ( FILLER_747 VSSD ) ( FILLER_535 VSSD )
       ( FILLER_746 VSSD ) ( FILLER_534 VSSD ) ( FILLER_745 VSSD )
       ( FILLER_533 VSSD ) ( FILLER_744 VSSD ) ( FILLER_532 VSSD )
       ( FILLER_743 VSSD ) ( FILLER_531 VSSD ) ( FILLER_742 VSSD )
       ( FILLER_741 VSSD ) ( FILLER_740 VSSD )
       ( mprj_pads.area2_io_pad\[0\] VSSD ) ( FILLER_529 VSSD )
       ( FILLER_528 VSSD ) ( FILLER_527 VSSD ) ( FILLER_526 VSSD )
       ( mprj_pads.area1_io_pad\[12\] VSSD ) ( FILLER_525 VSSD )
       ( FILLER_738 VSSD ) ( FILLER_524 VSSD ) ( FILLER_737 VSSD )
       ( FILLER_523 VSSD ) ( FILLER_736 VSSD ) ( FILLER_522 VSSD )
       ( FILLER_735 VSSD ) ( FILLER_734 VSSD ) ( FILLER_521 VSSD )
       ( FILLER_733 VSSD ) ( FILLER_732 VSSD )
       ( mprj_pads.area2_io_pad\[1\] VSSD ) ( FILLER_731 VSSD )
       ( FILLER_519 VSSD ) ( FILLER_518 VSSD ) ( FILLER_517 VSSD )
       ( FILLER_516 VSSD ) ( FILLER_515 VSSD )
       ( mprj_pads.area1_io_pad\[11\] VSSD ) ( FILLER_729 VSSD )
       ( FILLER_514 VSSD ) ( FILLER_728 VSSD ) ( FILLER_513 VSSD )
       ( FILLER_727 VSSD ) ( FILLER_512 VSSD ) ( FILLER_726 VSSD )
       ( FILLER_511 VSSD ) ( FILLER_725 VSSD ) ( FILLER_724 VSSD )
       ( FILLER_723 VSSD ) ( FILLER_722 VSSD )
       ( mprj_pads.area2_io_pad\[2\] VSSD ) ( FILLER_509 VSSD )
       ( FILLER_508 VSSD ) ( FILLER_507 VSSD ) ( FILLER_506 VSSD )
       ( FILLER_505 VSSD ) ( mprj_pads.area1_io_pad\[10\] VSSD )
       ( FILLER_720 VSSD ) ( FILLER_719 VSSD ) ( FILLER_504 VSSD )
       ( FILLER_718 VSSD ) ( FILLER_503 VSSD ) ( FILLER_717 VSSD )
       ( FILLER_502 VSSD ) ( FILLER_501 VSSD ) ( FILLER_716 VSSD )
       ( FILLER_715 VSSD ) ( FILLER_714 VSSD ) ( FILLER_713 VSSD )
       ( FILLER_712 VSSD ) ( mprj_pads.area2_io_pad\[3\] VSSD )
       ( FILLER_499 VSSD ) ( FILLER_498 VSSD ) ( FILLER_497 VSSD )
       ( FILLER_496 VSSD ) ( FILLER_495 VSSD ) ( FILLER_494 VSSD )
       ( mprj_pads.area1_io_pad\[9\] VSSD ) ( FILLER_710 VSSD )
       ( FILLER_493 VSSD ) ( FILLER_709 VSSD ) ( FILLER_492 VSSD )
       ( FILLER_708 VSSD ) ( FILLER_491 VSSD ) ( FILLER_707 VSSD )
       ( FILLER_706 VSSD ) ( FILLER_705 VSSD ) ( FILLER_704 VSSD )
       ( mprj_pads.area2_io_pad\[4\] VSSD ) ( FILLER_489 VSSD )
       ( FILLER_488 VSSD ) ( FILLER_703 VSSD ) ( FILLER_487 VSSD )
       ( FILLER_486 VSSD ) ( FILLER_485 VSSD ) ( FILLER_484 VSSD )
       ( mprj_pads.area1_io_pad\[8\] VSSD ) ( FILLER_701 VSSD )
       ( FILLER_483 VSSD ) ( FILLER_700 VSSD ) ( FILLER_482 VSSD )
       ( FILLER_699 VSSD ) ( FILLER_481 VSSD ) ( FILLER_698 VSSD )
       ( FILLER_697 VSSD ) ( FILLER_696 VSSD ) ( FILLER_695 VSSD )
       ( FILLER_694 VSSD ) ( mprj_pads.area2_io_pad\[5\] VSSD )
       ( FILLER_479 VSSD ) ( FILLER_478 VSSD ) ( FILLER_477 VSSD )
       ( FILLER_693 VSSD ) ( FILLER_476 VSSD ) ( FILLER_475 VSSD )
       ( FILLER_474 VSSD ) ( FILLER_473 VSSD )
       ( mprj_pads.area1_io_pad\[7\] VSSD ) ( FILLER_691 VSSD )
       ( FILLER_472 VSSD ) ( FILLER_690 VSSD ) ( FILLER_471 VSSD )
       ( FILLER_689 VSSD ) ( FILLER_688 VSSD ) ( FILLER_687 VSSD )
       ( FILLER_686 VSSD ) ( mprj_pads.area2_io_pad\[6\] VSSD )
       ( FILLER_469 VSSD ) ( FILLER_468 VSSD ) ( FILLER_685 VSSD )
       ( FILLER_467 VSSD ) ( FILLER_684 VSSD ) ( FILLER_466 VSSD )
       ( FILLER_465 VSSD ) ( FILLER_464 VSSD ) ( FILLER_463 VSSD )
       ( user1_vdda_hvclamp_pad\[1\] VSSD ) ( FILLER_682 VSSD )
       ( FILLER_462 VSSD ) ( FILLER_681 VSSD ) ( FILLER_461 VSSD )
       ( FILLER_680 VSSD ) ( FILLER_679 VSSD ) ( FILLER_678 VSSD )
       ( FILLER_677 VSSD ) ( user2_vdda_hvclamp_pad VSSD )
       ( FILLER_459 VSSD ) ( FILLER_458 VSSD ) ( FILLER_457 VSSD )
       ( FILLER_676 VSSD ) ( FILLER_675 VSSD ) ( FILLER_456 VSSD )
       ( FILLER_455 VSSD ) ( FILLER_454 VSSD ) ( FILLER_453 VSSD )
       ( user1_vssd_lvclamp_pad VSSD ) ( FILLER_673 VSSD )
       ( FILLER_452 VSSD ) ( FILLER_672 VSSD ) ( FILLER_671 VSSD )
       ( FILLER_451 VSSD ) ( FILLER_670 VSSD ) ( FILLER_669 VSSD )
       ( FILLER_668 VSSD ) ( user2_vssd_lvclamp_pad VSSD )
       ( FILLER_449 VSSD ) ( FILLER_667 VSSD ) ( FILLER_448 VSSD )
       ( FILLER_447 VSSD ) ( FILLER_666 VSSD ) ( FILLER_446 VSSD )
       ( FILLER_665 VSSD ) ( FILLER_445 VSSD ) ( FILLER_444 VSSD )
       ( FILLER_443 VSSD ) ( FILLER_442 VSSD )
       ( user1_vssa_hvclamp_pad\[1\] VSSD ) ( FILLER_663 VSSD )
       ( FILLER_441 VSSD ) ( FILLER_662 VSSD ) ( FILLER_661 VSSD )
       ( FILLER_660 VSSD ) ( FILLER_659 VSSD )
       ( mprj_pads.area2_io_pad\[7\] VSSD ) ( FILLER_439 VSSD )
       ( FILLER_438 VSSD ) ( FILLER_658 VSSD ) ( FILLER_437 VSSD )
       ( FILLER_657 VSSD ) ( FILLER_436 VSSD ) ( FILLER_656 VSSD )
       ( FILLER_435 VSSD ) ( FILLER_434 VSSD ) ( FILLER_433 VSSD )
       ( FILLER_432 VSSD ) ( mprj_pads.area1_io_pad\[6\] VSSD )
       ( FILLER_654 VSSD ) ( FILLER_431 VSSD ) ( FILLER_653 VSSD )
       ( FILLER_652 VSSD ) ( FILLER_651 VSSD ) ( FILLER_650 VSSD )
       ( mprj_pads.area2_io_pad\[8\] VSSD ) ( FILLER_649 VSSD )
       ( FILLER_429 VSSD ) ( FILLER_428 VSSD ) ( FILLER_427 VSSD )
       ( FILLER_648 VSSD ) ( FILLER_426 VSSD ) ( FILLER_647 VSSD )
       ( FILLER_425 VSSD ) ( FILLER_646 VSSD ) ( FILLER_424 VSSD )
       ( FILLER_423 VSSD ) ( FILLER_422 VSSD ) ( FILLER_421 VSSD )
       ( mprj_pads.area1_io_pad\[5\] VSSD ) ( FILLER_644 VSSD )
       ( FILLER_643 VSSD ) ( FILLER_642 VSSD ) ( FILLER_641 VSSD )
       ( mprj_pads.area2_io_pad\[9\] VSSD ) ( FILLER_419 VSSD )
       ( FILLER_418 VSSD ) ( FILLER_640 VSSD ) ( FILLER_417 VSSD )
       ( FILLER_639 VSSD ) ( FILLER_416 VSSD ) ( FILLER_638 VSSD )
       ( FILLER_415 VSSD ) ( FILLER_637 VSSD ) ( FILLER_414 VSSD )
       ( FILLER_413 VSSD ) ( FILLER_412 VSSD ) ( FILLER_411 VSSD )
       ( mprj_pads.area1_io_pad\[4\] VSSD ) ( FILLER_635 VSSD )
       ( FILLER_634 VSSD ) ( FILLER_633 VSSD )
       ( mprj_pads.area2_io_pad\[10\] VSSD ) ( FILLER_409 VSSD )
       ( FILLER_632 VSSD ) ( FILLER_408 VSSD ) ( FILLER_407 VSSD )
       ( FILLER_631 VSSD ) ( FILLER_406 VSSD ) ( FILLER_630 VSSD )
       ( FILLER_405 VSSD ) ( FILLER_629 VSSD ) ( FILLER_404 VSSD )
       ( FILLER_628 VSSD ) ( FILLER_403 VSSD ) ( FILLER_402 VSSD )
       ( FILLER_401 VSSD ) ( mprj_pads.area1_io_pad\[3\] VSSD )
       ( FILLER_626 VSSD ) ( FILLER_625 VSSD ) ( FILLER_624 VSSD )
       ( FILLER_623 VSSD ) ( mprj_pads.area2_io_pad\[11\] VSSD )
       ( FILLER_399 VSSD ) ( FILLER_398 VSSD ) ( FILLER_622 VSSD )
       ( FILLER_397 VSSD ) ( FILLER_621 VSSD ) ( FILLER_396 VSSD )
       ( FILLER_620 VSSD ) ( FILLER_395 VSSD ) ( FILLER_619 VSSD )
       ( FILLER_394 VSSD ) ( FILLER_618 VSSD ) ( FILLER_393 VSSD )
       ( FILLER_392 VSSD ) ( FILLER_391 VSSD )
       ( mprj_pads.area1_io_pad\[2\] VSSD ) ( FILLER_616 VSSD )
       ( FILLER_615 VSSD ) ( FILLER_614 VSSD )
       ( mprj_pads.area2_io_pad\[12\] VSSD ) ( FILLER_389 VSSD )
       ( FILLER_388 VSSD ) ( FILLER_387 VSSD ) ( FILLER_613 VSSD )
       ( FILLER_386 VSSD ) ( FILLER_612 VSSD ) ( FILLER_385 VSSD )
       ( FILLER_611 VSSD ) ( FILLER_384 VSSD ) ( FILLER_610 VSSD )
       ( FILLER_383 VSSD ) ( FILLER_609 VSSD ) ( FILLER_382 VSSD )
       ( FILLER_381 VSSD ) ( FILLER_380 VSSD ) ( FILLER_379 VSSD )
       ( mprj_pads.area1_io_pad\[1\] VSSD ) ( FILLER_607 VSSD )
       ( FILLER_606 VSSD ) ( FILLER_378 VSSD ) ( FILLER_605 VSSD )
       ( FILLER_377 VSSD ) ( FILLER_604 VSSD ) ( FILLER_376 VSSD )
       ( FILLER_603 VSSD ) ( FILLER_375 VSSD ) ( FILLER_602 VSSD )
       ( FILLER_374 VSSD ) ( disconnect_vdda_2 VSSD )
       ( FILLER_SB2 VSSD ) ( FILLER_601 VSSD ) ( FILLER_600 VSSD )
       ( mgmt_vddio_hvclamp_pad\[0\] VSSD ) ( FILLER_599 VSSD )
       ( FILLER_370 VSSD ) ( FILLER_369 VSSD ) ( FILLER_368 VSSD )
       ( FILLER_367 VSSD ) ( mprj_pads.area1_io_pad\[0\] VSSD )
       ( FILLER_597 VSSD ) ( FILLER_366 VSSD ) ( FILLER_596 VSSD )
       ( FILLER_365 VSSD ) ( FILLER_595 VSSD ) ( FILLER_364 VSSD )
       ( FILLER_594 VSSD ) ( FILLER_363 VSSD ) ( FILLER_593 VSSD )
       ( FILLER_362 VSSD ) ( FILLER_592 VSSD ) ( FILLER_591 VSSD )
       ( FILLER_590 VSSD ) ( disconnect_vdda_1 VSSD )
       ( FILLER_SB1 VSSD ) ( FILLER_587 VSSD )
       ( mgmt_vccd_lvclamp_pad VSSD ) ( FILLER_360 VSSD )
       ( FILLER_359 VSSD ) ( FILLER_358 VSSD ) ( FILLER_586 VSSD )
       ( FILLER_357 VSSD ) ( FILLER_585 VSSD ) ( FILLER_356 VSSD )
       ( FILLER_584 VSSD ) ( FILLER_583 VSSD ) ( FILLER_355 VSSD )
       ( FILLER_582 VSSD ) ( FILLER_354 VSSD ) ( FILLER_581 VSSD )
       ( FILLER_353 VSSD ) ( constant_block_6 vssd )
       ( FILLER_352 VSSD ) ( FILLER_580 VSSD )
       ( constant_block_5 vssd ) ( constant_block_4 vssd )
       ( constant_block_3 vssd ) ( constant_block_2 vssd )
       ( constant_block_1 vssd ) ( constant_block_0 vssd )
       ( mgmt_corner\[1\] VSSD ) ( FILLER_351 VSSD )
       ( FILLER_350 VSSD ) ( FILLER_349 VSSD ) ( FILLER_348 VSSD )
       ( FILLER_347 VSSD ) ( FILLER_346 VSSD ) ( bus_tie_72 VSSD )
       ( bus_tie_71 VSSD ) ( bus_tie_70 VSSD ) ( bus_tie_69 VSSD )
       ( bus_tie_68 VSSD ) ( bus_tie_67 VSSD ) ( FILLER_339 VSSD )
       ( FILLER_338 VSSD ) ( FILLER_337 VSSD ) ( FILLER_336 VSSD )
       ( FILLER_335 VSSD ) ( mgmt_vdda_hvclamp_pad VSSD )
       ( FILLER_333 VSSD ) ( FILLER_332 VSSD ) ( FILLER_331 VSSD )
       ( FILLER_330 VSSD ) ( bus_tie_66 VSSD ) ( FILLER_329 VSSD )
       ( bus_tie_65 VSSD ) ( bus_tie_64 VSSD ) ( bus_tie_63 VSSD )
       ( bus_tie_62 VSSD ) ( bus_tie_61 VSSD ) ( FILLER_322 VSSD )
       ( FILLER_321 VSSD ) ( FILLER_320 VSSD ) ( FILLER_319 VSSD )
       ( FILLER_318 VSSD ) ( mgmt_vssio_hvclamp_pad\[0\] VSSD )
       ( FILLER_316 VSSD ) ( FILLER_315 VSSD ) ( FILLER_314 VSSD )
       ( FILLER_313 VSSD ) ( bus_tie_60 VSSD ) ( FILLER_312 VSSD )
       ( bus_tie_59 VSSD ) ( bus_tie_58 VSSD ) ( bus_tie_57 VSSD )
       ( bus_tie_56 VSSD ) ( bus_tie_55 VSSD ) ( FILLER_305 VSSD )
       ( FILLER_304 VSSD ) ( FILLER_303 VSSD ) ( FILLER_302 VSSD )
       ( FILLER_301 VSSD ) ( gpio_pad VSSD ) ( FILLER_299 VSSD )
       ( FILLER_298 VSSD ) ( FILLER_297 VSSD ) ( FILLER_296 VSSD )
       ( FILLER_295 VSSD ) ( bus_tie_54 VSSD ) ( bus_tie_53 VSSD )
       ( bus_tie_52 VSSD ) ( bus_tie_51 VSSD ) ( bus_tie_50 VSSD )
       ( bus_tie_49 VSSD ) ( FILLER_288 VSSD ) ( FILLER_287 VSSD )
       ( FILLER_286 VSSD ) ( FILLER_285 VSSD ) ( FILLER_284 VSSD )
       ( flash_io1_pad VSSD ) ( FILLER_282 VSSD ) ( FILLER_281 VSSD )
       ( FILLER_280 VSSD ) ( FILLER_279 VSSD ) ( bus_tie_48 VSSD )
       ( FILLER_278 VSSD ) ( bus_tie_47 VSSD ) ( bus_tie_46 VSSD )
       ( bus_tie_45 VSSD ) ( bus_tie_44 VSSD ) ( bus_tie_43 VSSD )
       ( FILLER_271 VSSD ) ( FILLER_270 VSSD ) ( FILLER_269 VSSD )
       ( FILLER_268 VSSD ) ( FILLER_267 VSSD ) ( flash_io0_pad VSSD )
       ( FILLER_265 VSSD ) ( FILLER_264 VSSD ) ( FILLER_263 VSSD )
       ( FILLER_262 VSSD ) ( FILLER_261 VSSD ) ( bus_tie_42 VSSD )
       ( bus_tie_41 VSSD ) ( bus_tie_40 VSSD ) ( bus_tie_39 VSSD )
       ( bus_tie_38 VSSD ) ( bus_tie_37 VSSD ) ( FILLER_254 VSSD )
       ( FILLER_253 VSSD ) ( FILLER_252 VSSD ) ( FILLER_251 VSSD )
       ( FILLER_250 VSSD ) ( flash_clk_pad VSSD ) ( FILLER_248 VSSD )
       ( FILLER_247 VSSD ) ( FILLER_246 VSSD ) ( FILLER_245 VSSD )
       ( bus_tie_36 VSSD ) ( FILLER_244 VSSD ) ( bus_tie_35 VSSD )
       ( bus_tie_34 VSSD ) ( bus_tie_33 VSSD ) ( bus_tie_32 VSSD )
       ( bus_tie_31 VSSD ) ( FILLER_237 VSSD ) ( FILLER_236 VSSD )
       ( FILLER_235 VSSD ) ( FILLER_234 VSSD ) ( FILLER_233 VSSD )
       ( flash_csb_pad VSSD ) ( FILLER_231 VSSD ) ( FILLER_230 VSSD )
       ( FILLER_229 VSSD ) ( FILLER_228 VSSD ) ( FILLER_227 VSSD )
       ( bus_tie_30 VSSD ) ( bus_tie_29 VSSD ) ( bus_tie_28 VSSD )
       ( bus_tie_27 VSSD ) ( bus_tie_26 VSSD ) ( bus_tie_25 VSSD )
       ( FILLER_220 VSSD ) ( FILLER_219 VSSD ) ( FILLER_218 VSSD )
       ( FILLER_217 VSSD ) ( FILLER_216 VSSD )
       ( mgmt_vssd_lvclamp_pad VSSD ) ( FILLER_214 VSSD )
       ( FILLER_213 VSSD ) ( FILLER_212 VSSD ) ( FILLER_211 VSSD )
       ( bus_tie_24 VSSD ) ( FILLER_210 VSSD ) ( bus_tie_23 VSSD )
       ( bus_tie_22 VSSD ) ( bus_tie_21 VSSD ) ( bus_tie_20 VSSD )
       ( bus_tie_19 VSSD ) ( FILLER_203 VSSD ) ( FILLER_202 VSSD )
       ( FILLER_201 VSSD ) ( FILLER_200 VSSD ) ( FILLER_199 VSSD )
       ( clock_pad VSSD ) ( FILLER_197 VSSD ) ( FILLER_196 VSSD )
       ( FILLER_195 VSSD ) ( FILLER_194 VSSD ) ( bus_tie_18 VSSD )
       ( FILLER_193 VSSD ) ( bus_tie_17 VSSD ) ( bus_tie_16 VSSD )
       ( bus_tie_15 VSSD ) ( bus_tie_14 VSSD ) ( bus_tie_13 VSSD )
       ( FILLER_186 VSSD ) ( FILLER_185 VSSD ) ( FILLER_184 VSSD )
       ( FILLER_183 VSSD ) ( FILLER_182 VSSD ) ( resetb_pad VSSD )
       ( FILLER_180 VSSD ) ( bus_tie_9 VSSD ) ( FILLER_179 VSSD )
       ( FILLER_178 VSSD ) ( FILLER_177 VSSD ) ( FILLER_176 VSSD )
       ( bus_tie_12 VSSD ) ( bus_tie_11 VSSD ) ( bus_tie_10 VSSD )
       ( bus_tie_8 VSSD ) ( bus_tie_7 VSSD ) ( bus_tie_6 VSSD )
       ( FILLER_169 VSSD ) ( FILLER_168 VSSD ) ( FILLER_167 VSSD )
       ( FILLER_166 VSSD ) ( FILLER_165 VSSD )
       ( mgmt_vssa_hvclamp_pad VSSD ) ( FILLER_163 VSSD )
       ( FILLER_162 VSSD ) ( FILLER_161 VSSD ) ( FILLER_160 VSSD )
       ( bus_tie_5 VSSD ) ( FILLER_159 VSSD ) ( bus_tie_4 VSSD )
       ( bus_tie_3 VSSD ) ( bus_tie_2 VSSD ) ( bus_tie_1 VSSD )
       ( FILLER_152 VSSD ) ( FILLER_151 VSSD ) ( FILLER_150 VSSD )
       ( FILLER_149 VSSD ) ( FILLER_148 VSSD )
       ( mgmt_corner\[0\] VSSD )
      + ROUTED met4 TAPERRULE met4_width_1270  ( 663635 153915 ) ( * 158265 ) ;
   - vdda ( mgmt_vddio_hvclamp_pad\[0\] VDDA ) ( FILLER_370 VDDA )
       ( FILLER_369 VDDA ) ( FILLER_368 VDDA ) ( FILLER_367 VDDA )
       ( FILLER_366 VDDA ) ( FILLER_365 VDDA ) ( FILLER_364 VDDA )
       ( FILLER_363 VDDA ) ( FILLER_362 VDDA ) ( FILLER_587 VDDA )
       ( mgmt_vccd_lvclamp_pad VDDA ) ( FILLER_360 VDDA )
       ( FILLER_359 VDDA ) ( FILLER_358 VDDA ) ( FILLER_586 VDDA )
       ( FILLER_357 VDDA ) ( FILLER_585 VDDA ) ( FILLER_356 VDDA )
       ( FILLER_584 VDDA ) ( FILLER_583 VDDA ) ( FILLER_355 VDDA )
       ( FILLER_582 VDDA ) ( FILLER_354 VDDA ) ( FILLER_581 VDDA )
       ( FILLER_353 VDDA ) ( mgmt_corner\[1\] VDDA )
       ( FILLER_352 VDDA ) ( FILLER_580 VDDA ) ( FILLER_351 VDDA )
       ( FILLER_350 VDDA ) ( FILLER_349 VDDA ) ( FILLER_348 VDDA )
       ( FILLER_347 VDDA ) ( FILLER_346 VDDA ) ( bus_tie_72 VDDA )
       ( bus_tie_71 VDDA ) ( bus_tie_70 VDDA ) ( bus_tie_69 VDDA )
       ( bus_tie_68 VDDA ) ( bus_tie_67 VDDA ) ( FILLER_339 VDDA )
       ( FILLER_338 VDDA ) ( FILLER_337 VDDA ) ( FILLER_336 VDDA )
       ( FILLER_335 VDDA ) ( mgmt_vdda_hvclamp_pad VDDA )
       ( FILLER_333 VDDA ) ( FILLER_332 VDDA ) ( FILLER_331 VDDA )
       ( FILLER_330 VDDA ) ( bus_tie_66 VDDA ) ( FILLER_329 VDDA )
       ( bus_tie_65 VDDA ) ( bus_tie_64 VDDA ) ( bus_tie_63 VDDA )
       ( bus_tie_62 VDDA ) ( bus_tie_61 VDDA ) ( FILLER_322 VDDA )
       ( FILLER_321 VDDA ) ( FILLER_320 VDDA ) ( FILLER_319 VDDA )
       ( FILLER_318 VDDA ) ( mgmt_vssio_hvclamp_pad\[0\] VDDA )
       ( FILLER_316 VDDA ) ( FILLER_315 VDDA ) ( FILLER_314 VDDA )
       ( FILLER_313 VDDA ) ( bus_tie_60 VDDA ) ( FILLER_312 VDDA )
       ( bus_tie_59 VDDA ) ( bus_tie_58 VDDA ) ( bus_tie_57 VDDA )
       ( bus_tie_56 VDDA ) ( bus_tie_55 VDDA ) ( FILLER_305 VDDA )
       ( FILLER_304 VDDA ) ( FILLER_303 VDDA ) ( FILLER_302 VDDA )
       ( FILLER_301 VDDA ) ( gpio_pad VDDA ) ( FILLER_299 VDDA )
       ( FILLER_298 VDDA ) ( FILLER_297 VDDA ) ( FILLER_296 VDDA )
       ( FILLER_295 VDDA ) ( bus_tie_54 VDDA ) ( bus_tie_53 VDDA )
       ( bus_tie_52 VDDA ) ( bus_tie_51 VDDA ) ( bus_tie_50 VDDA )
       ( bus_tie_49 VDDA ) ( FILLER_288 VDDA ) ( FILLER_287 VDDA )
       ( FILLER_286 VDDA ) ( FILLER_285 VDDA ) ( FILLER_284 VDDA )
       ( flash_io1_pad VDDA ) ( FILLER_282 VDDA ) ( FILLER_281 VDDA )
       ( FILLER_280 VDDA ) ( FILLER_279 VDDA ) ( bus_tie_48 VDDA )
       ( FILLER_278 VDDA ) ( bus_tie_47 VDDA ) ( bus_tie_46 VDDA )
       ( bus_tie_45 VDDA ) ( bus_tie_44 VDDA ) ( bus_tie_43 VDDA )
       ( FILLER_271 VDDA ) ( FILLER_270 VDDA ) ( FILLER_269 VDDA )
       ( FILLER_268 VDDA ) ( FILLER_267 VDDA ) ( flash_io0_pad VDDA )
       ( FILLER_265 VDDA ) ( FILLER_264 VDDA ) ( FILLER_263 VDDA )
       ( FILLER_262 VDDA ) ( FILLER_261 VDDA ) ( bus_tie_42 VDDA )
       ( bus_tie_41 VDDA ) ( bus_tie_40 VDDA ) ( bus_tie_39 VDDA )
       ( bus_tie_38 VDDA ) ( bus_tie_37 VDDA ) ( FILLER_254 VDDA )
       ( FILLER_253 VDDA ) ( FILLER_252 VDDA ) ( FILLER_251 VDDA )
       ( FILLER_250 VDDA ) ( flash_clk_pad VDDA ) ( FILLER_248 VDDA )
       ( FILLER_247 VDDA ) ( FILLER_246 VDDA ) ( FILLER_245 VDDA )
       ( bus_tie_36 VDDA ) ( FILLER_244 VDDA ) ( bus_tie_35 VDDA )
       ( bus_tie_34 VDDA ) ( bus_tie_33 VDDA ) ( bus_tie_32 VDDA )
       ( bus_tie_31 VDDA ) ( FILLER_237 VDDA ) ( FILLER_236 VDDA )
       ( FILLER_235 VDDA ) ( FILLER_234 VDDA ) ( FILLER_233 VDDA )
       ( flash_csb_pad VDDA ) ( FILLER_231 VDDA ) ( FILLER_230 VDDA )
       ( FILLER_229 VDDA ) ( FILLER_228 VDDA ) ( FILLER_227 VDDA )
       ( bus_tie_30 VDDA ) ( bus_tie_29 VDDA ) ( bus_tie_28 VDDA )
       ( bus_tie_27 VDDA ) ( bus_tie_26 VDDA ) ( bus_tie_25 VDDA )
       ( FILLER_220 VDDA ) ( FILLER_219 VDDA ) ( FILLER_218 VDDA )
       ( FILLER_217 VDDA ) ( FILLER_216 VDDA )
       ( mgmt_vssd_lvclamp_pad VDDA ) ( FILLER_214 VDDA )
       ( FILLER_213 VDDA ) ( FILLER_212 VDDA ) ( FILLER_211 VDDA )
       ( bus_tie_24 VDDA ) ( FILLER_210 VDDA ) ( bus_tie_23 VDDA )
       ( bus_tie_22 VDDA ) ( bus_tie_21 VDDA ) ( bus_tie_20 VDDA )
       ( bus_tie_19 VDDA ) ( FILLER_203 VDDA ) ( FILLER_202 VDDA )
       ( FILLER_201 VDDA ) ( FILLER_200 VDDA ) ( FILLER_199 VDDA )
       ( clock_pad VDDA ) ( FILLER_197 VDDA ) ( FILLER_196 VDDA )
       ( FILLER_195 VDDA ) ( FILLER_194 VDDA ) ( bus_tie_18 VDDA )
       ( FILLER_193 VDDA ) ( bus_tie_17 VDDA ) ( bus_tie_16 VDDA )
       ( bus_tie_15 VDDA ) ( bus_tie_14 VDDA ) ( bus_tie_13 VDDA )
       ( FILLER_186 VDDA ) ( FILLER_185 VDDA ) ( FILLER_184 VDDA )
       ( FILLER_183 VDDA ) ( FILLER_182 VDDA ) ( resetb_pad VDDA )
       ( FILLER_180 VDDA ) ( bus_tie_9 VDDA ) ( FILLER_179 VDDA )
       ( FILLER_178 VDDA ) ( FILLER_177 VDDA ) ( FILLER_176 VDDA )
       ( bus_tie_12 VDDA ) ( bus_tie_11 VDDA ) ( bus_tie_10 VDDA )
       ( bus_tie_8 VDDA ) ( bus_tie_7 VDDA ) ( bus_tie_6 VDDA )
       ( FILLER_169 VDDA ) ( FILLER_168 VDDA ) ( FILLER_167 VDDA )
       ( FILLER_166 VDDA ) ( FILLER_165 VDDA )
       ( mgmt_vssa_hvclamp_pad VDDA ) ( FILLER_163 VDDA )
       ( FILLER_162 VDDA ) ( FILLER_161 VDDA ) ( FILLER_160 VDDA )
       ( bus_tie_5 VDDA ) ( FILLER_159 VDDA ) ( bus_tie_4 VDDA )
       ( bus_tie_3 VDDA ) ( bus_tie_2 VDDA ) ( bus_tie_1 VDDA )
       ( FILLER_152 VDDA ) ( FILLER_151 VDDA ) ( FILLER_150 VDDA )
       ( FILLER_149 VDDA ) ( FILLER_148 VDDA )
       ( mgmt_corner\[0\] VDDA )
      + ROUTED met4 TAPERRULE met4_width_960  ( 663480 181765 ) ( * 184915 ) ;
   - vccd ( FILLER_147 VCCD ) ( FILLER_146 VCCD ) ( FILLER_145 VCCD )
       ( FILLER_144 VCCD ) ( FILLER_143 VCCD ) ( FILLER_142 VCCD )
       ( FILLER_141 VCCD ) ( FILLER_140 VCCD ) ( FILLER_139 VCCD )
       ( FILLER_138 VCCD ) ( FILLER_137 VCCD ) ( FILLER_136 VCCD )
       ( FILLER_135 VCCD ) ( user1_analog_pad\[0\] VCCD )
       ( FILLER_133 VCCD ) ( FILLER_132 VCCD ) ( FILLER_131 VCCD )
       ( FILLER_130 VCCD ) ( FILLER_129 VCCD ) ( FILLER_128 VCCD )
       ( FILLER_127 VCCD ) ( FILLER_126 VCCD ) ( FILLER_125 VCCD )
       ( FILLER_124 VCCD ) ( FILLER_123 VCCD )
       ( user1_vssa_hvclamp_pad\[0\] VCCD ) ( FILLER_121 VCCD )
       ( FILLER_120 VCCD ) ( FILLER_119 VCCD ) ( FILLER_118 VCCD )
       ( FILLER_117 VCCD ) ( FILLER_116 VCCD ) ( FILLER_115 VCCD )
       ( FILLER_114 VCCD ) ( FILLER_113 VCCD ) ( FILLER_112 VCCD )
       ( FILLER_111 VCCD ) ( FILLER_110 VCCD )
       ( user1_analog_pad\[1\] VCCD ) ( FILLER_108 VCCD )
       ( FILLER_107 VCCD ) ( FILLER_106 VCCD ) ( FILLER_105 VCCD )
       ( FILLER_104 VCCD ) ( FILLER_103 VCCD ) ( FILLER_102 VCCD )
       ( FILLER_101 VCCD ) ( FILLER_100 VCCD ) ( FILLER_99 VCCD )
       ( FILLER_98 VCCD ) ( user1_analog_pad\[2\] VCCD )
       ( FILLER_96 VCCD ) ( FILLER_95 VCCD ) ( FILLER_94 VCCD )
       ( FILLER_93 VCCD ) ( FILLER_92 VCCD ) ( FILLER_91 VCCD )
       ( FILLER_90 VCCD ) ( FILLER_89 VCCD ) ( FILLER_88 VCCD )
       ( FILLER_87 VCCD ) ( FILLER_86 VCCD ) ( FILLER_85 VCCD )
       ( FILLER_84 VCCD ) ( FILLER_83 VCCD ) ( FILLER_82 VCCD )
       ( FILLER_81 VCCD ) ( FILLER_80 VCCD ) ( FILLER_79 VCCD )
       ( sky130_ef_io__com_bus_slice_10um_0 VCCD ) ( FILLER_78 VCCD )
       ( sky130_ef_io__com_bus_slice_5um_1 VCCD )
       ( user1_analog_pad_with_clamp VCCD )
       ( sky130_ef_io__com_bus_slice_5um_0 VCCD )
       ( disconnect_vdda_0 VCCD ) ( FILLER_SB3 VCCD )
       ( FILLER_73 VCCD ) ( FILLER_72 VCCD ) ( FILLER_71 VCCD )
       ( FILLER_70 VCCD ) ( FILLER_69 VCCD ) ( FILLER_68 VCCD )
       ( mgmt_vssio_hvclamp_pad\[1\] VCCD ) ( FILLER_66 VCCD )
       ( FILLER_65 VCCD ) ( FILLER_64 VCCD ) ( FILLER_63 VCCD )
       ( FILLER_62 VCCD ) ( FILLER_61 VCCD ) ( FILLER_60 VCCD )
       ( sky130_ef_io__com_bus_slice_10um_1 VCCD )
       ( sky130_ef_io__com_bus_slice_5um_3 VCCD )
       ( user2_analog_pad_with_clamp\[0\] VCCD )
       ( sky130_ef_io__com_bus_slice_5um_2 VCCD ) ( FILLER_57 VCCD )
       ( FILLER_56 VCCD ) ( FILLER_55 VCCD ) ( FILLER_54 VCCD )
       ( FILLER_53 VCCD ) ( FILLER_52 VCCD ) ( FILLER_51 VCCD )
       ( FILLER_50 VCCD ) ( FILLER_49 VCCD )
       ( user2_analog_pad_with_clamp\[1\] VCCD ) ( FILLER_47 VCCD )
       ( FILLER_46 VCCD ) ( FILLER_45 VCCD ) ( FILLER_44 VCCD )
       ( FILLER_43 VCCD ) ( FILLER_42 VCCD )
       ( user2_analog_pad\[0\] VCCD ) ( FILLER_41 VCCD )
       ( FILLER_39 VCCD ) ( FILLER_38 VCCD ) ( FILLER_37 VCCD )
       ( FILLER_36 VCCD ) ( FILLER_35 VCCD ) ( FILLER_34 VCCD )
       ( FILLER_33 VCCD ) ( FILLER_32 VCCD ) ( FILLER_31 VCCD )
       ( FILLER_30 VCCD ) ( FILLER_29 VCCD )
       ( user2_analog_pad\[1\] VCCD ) ( FILLER_27 VCCD )
       ( FILLER_26 VCCD ) ( FILLER_25 VCCD ) ( FILLER_24 VCCD )
       ( FILLER_23 VCCD ) ( FILLER_22 VCCD ) ( FILLER_21 VCCD )
       ( FILLER_20 VCCD ) ( FILLER_19 VCCD ) ( FILLER_18 VCCD )
       ( FILLER_17 VCCD ) ( user2_analog_pad\[2\] VCCD )
       ( FILLER_15 VCCD ) ( FILLER_14 VCCD ) ( FILLER_13 VCCD )
       ( FILLER_12 VCCD ) ( FILLER_11 VCCD ) ( FILLER_10 VCCD )
       ( FILLER_9 VCCD ) ( FILLER_8 VCCD ) ( FILLER_7 VCCD )
       ( FILLER_6 VCCD ) ( FILLER_147 VCCHIB ) ( FILLER_5 VCCD )
       ( FILLER_146 VCCHIB ) ( FILLER_145 VCCHIB )
       ( FILLER_144 VCCHIB ) ( FILLER_143 VCCHIB )
       ( FILLER_142 VCCHIB ) ( FILLER_141 VCCHIB )
       ( FILLER_140 VCCHIB ) ( FILLER_139 VCCHIB )
       ( FILLER_138 VCCHIB ) ( FILLER_137 VCCHIB )
       ( FILLER_136 VCCHIB ) ( FILLER_135 VCCHIB )
       ( user1_analog_pad\[0\] VCCHIB ) ( FILLER_133 VCCHIB )
       ( FILLER_132 VCCHIB ) ( FILLER_131 VCCHIB )
       ( FILLER_130 VCCHIB ) ( FILLER_129 VCCHIB )
       ( FILLER_128 VCCHIB ) ( FILLER_127 VCCHIB )
       ( FILLER_126 VCCHIB ) ( FILLER_125 VCCHIB )
       ( FILLER_124 VCCHIB ) ( FILLER_123 VCCHIB )
       ( user1_vssa_hvclamp_pad\[0\] VCCHIB ) ( FILLER_121 VCCHIB )
       ( FILLER_120 VCCHIB ) ( FILLER_119 VCCHIB )
       ( FILLER_118 VCCHIB ) ( FILLER_117 VCCHIB )
       ( FILLER_116 VCCHIB ) ( FILLER_115 VCCHIB )
       ( FILLER_114 VCCHIB ) ( FILLER_113 VCCHIB )
       ( FILLER_112 VCCHIB ) ( FILLER_111 VCCHIB )
       ( FILLER_110 VCCHIB ) ( user1_analog_pad\[1\] VCCHIB )
       ( FILLER_108 VCCHIB ) ( FILLER_107 VCCHIB )
       ( FILLER_106 VCCHIB ) ( FILLER_105 VCCHIB )
       ( FILLER_104 VCCHIB ) ( FILLER_103 VCCHIB )
       ( FILLER_102 VCCHIB ) ( FILLER_101 VCCHIB )
       ( FILLER_100 VCCHIB ) ( FILLER_99 VCCHIB ) ( FILLER_98 VCCHIB )
       ( user1_analog_pad\[2\] VCCHIB ) ( FILLER_96 VCCHIB )
       ( FILLER_95 VCCHIB ) ( FILLER_94 VCCHIB ) ( FILLER_93 VCCHIB )
       ( FILLER_92 VCCHIB ) ( FILLER_91 VCCHIB ) ( FILLER_90 VCCHIB )
       ( FILLER_89 VCCHIB ) ( FILLER_88 VCCHIB ) ( FILLER_87 VCCHIB )
       ( FILLER_86 VCCHIB ) ( FILLER_85 VCCHIB ) ( FILLER_84 VCCHIB )
       ( FILLER_83 VCCHIB ) ( FILLER_82 VCCHIB ) ( FILLER_81 VCCHIB )
       ( FILLER_80 VCCHIB ) ( FILLER_79 VCCHIB )
       ( sky130_ef_io__com_bus_slice_10um_0 VCCHIB )
       ( FILLER_78 VCCHIB )
       ( sky130_ef_io__com_bus_slice_5um_1 VCCHIB )
       ( user1_analog_pad_with_clamp VCCHIB )
       ( sky130_ef_io__com_bus_slice_5um_0 VCCHIB )
       ( disconnect_vdda_0 VCCHIB ) ( FILLER_SB3 VCCHIB )
       ( FILLER_73 VCCHIB ) ( FILLER_72 VCCHIB ) ( FILLER_71 VCCHIB )
       ( FILLER_70 VCCHIB ) ( FILLER_69 VCCHIB ) ( FILLER_68 VCCHIB )
       ( mgmt_vssio_hvclamp_pad\[1\] VCCHIB ) ( FILLER_66 VCCHIB )
       ( FILLER_65 VCCHIB ) ( FILLER_64 VCCHIB ) ( FILLER_63 VCCHIB )
       ( FILLER_62 VCCHIB ) ( FILLER_61 VCCHIB ) ( FILLER_60 VCCHIB )
       ( sky130_ef_io__com_bus_slice_10um_1 VCCHIB )
       ( sky130_ef_io__com_bus_slice_5um_3 VCCHIB )
       ( user2_analog_pad_with_clamp\[0\] VCCHIB )
       ( sky130_ef_io__com_bus_slice_5um_2 VCCHIB )
       ( FILLER_57 VCCHIB ) ( FILLER_56 VCCHIB ) ( FILLER_55 VCCHIB )
       ( FILLER_54 VCCHIB ) ( FILLER_53 VCCHIB ) ( FILLER_52 VCCHIB )
       ( FILLER_51 VCCHIB ) ( FILLER_50 VCCHIB ) ( FILLER_49 VCCHIB )
       ( user2_analog_pad_with_clamp\[1\] VCCHIB )
       ( FILLER_47 VCCHIB ) ( FILLER_46 VCCHIB ) ( FILLER_45 VCCHIB )
       ( FILLER_44 VCCHIB ) ( FILLER_43 VCCHIB ) ( FILLER_42 VCCHIB )
       ( user2_analog_pad\[0\] VCCHIB ) ( FILLER_41 VCCHIB )
       ( FILLER_39 VCCHIB ) ( FILLER_38 VCCHIB ) ( FILLER_37 VCCHIB )
       ( FILLER_36 VCCHIB ) ( FILLER_35 VCCHIB ) ( FILLER_34 VCCHIB )
       ( FILLER_33 VCCHIB ) ( FILLER_32 VCCHIB ) ( FILLER_31 VCCHIB )
       ( FILLER_30 VCCHIB ) ( FILLER_29 VCCHIB )
       ( user2_analog_pad\[1\] VCCHIB ) ( FILLER_27 VCCHIB )
       ( FILLER_26 VCCHIB ) ( FILLER_25 VCCHIB ) ( FILLER_24 VCCHIB )
       ( FILLER_23 VCCHIB ) ( FILLER_22 VCCHIB ) ( FILLER_21 VCCHIB )
       ( FILLER_20 VCCHIB ) ( FILLER_19 VCCHIB ) ( FILLER_18 VCCHIB )
       ( FILLER_17 VCCHIB ) ( user2_analog_pad\[2\] VCCHIB )
       ( FILLER_15 VCCHIB ) ( FILLER_14 VCCHIB ) ( FILLER_13 VCCHIB )
       ( FILLER_12 VCCHIB ) ( FILLER_11 VCCHIB ) ( FILLER_10 VCCHIB )
       ( FILLER_9 VCCHIB ) ( FILLER_8 VCCHIB ) ( FILLER_7 VCCHIB )
       ( FILLER_6 VCCHIB ) ( user2_corner VCCHIB ) ( FILLER_5 VCCHIB )
       ( FILLER_579 VCCHIB ) ( FILLER_578 VCCHIB )
       ( user2_corner VCCD ) ( FILLER_579 VCCD ) ( FILLER_578 VCCD )
       ( user1_corner VCCD ) ( FILLER_786 VCCD )
       ( user1_corner VCCHIB ) ( FILLER_786 VCCHIB )
       ( FILLER_577 VCCHIB ) ( FILLER_577 VCCD ) ( FILLER_576 VCCHIB )
       ( FILLER_576 VCCD ) ( FILLER_785 VCCD ) ( FILLER_785 VCCHIB )
       ( FILLER_575 VCCHIB ) ( FILLER_575 VCCD ) ( FILLER_784 VCCD )
       ( FILLER_784 VCCHIB ) ( FILLER_574 VCCHIB ) ( FILLER_574 VCCD )
       ( FILLER_783 VCCD ) ( FILLER_783 VCCHIB ) ( FILLER_573 VCCHIB )
       ( FILLER_573 VCCD ) ( FILLER_782 VCCD ) ( FILLER_782 VCCHIB )
       ( FILLER_572 VCCHIB ) ( FILLER_572 VCCD ) ( FILLER_781 VCCD )
       ( FILLER_781 VCCHIB ) ( FILLER_571 VCCHIB ) ( FILLER_571 VCCD )
       ( FILLER_780 VCCD ) ( FILLER_780 VCCHIB ) ( FILLER_779 VCCD )
       ( FILLER_570 VCCHIB ) ( FILLER_570 VCCD ) ( FILLER_779 VCCHIB )
       ( user2_analog_pad\[3\] VCCHIB ) ( FILLER_776 VCCD )
       ( FILLER_776 VCCHIB ) ( FILLER_568 VCCHIB )
       ( user2_analog_pad\[3\] VCCD ) ( FILLER_568 VCCD )
       ( user1_analog_pad\[3\] VCCD ) ( user1_analog_pad\[3\] VCCHIB )
       ( FILLER_567 VCCHIB ) ( FILLER_567 VCCD ) ( FILLER_777 VCCD )
       ( FILLER_777 VCCHIB ) ( FILLER_775 VCCD ) ( FILLER_775 VCCHIB )
       ( FILLER_566 VCCHIB ) ( FILLER_566 VCCD ) ( FILLER_774 VCCD )
       ( FILLER_774 VCCHIB ) ( FILLER_565 VCCHIB ) ( FILLER_565 VCCD )
       ( FILLER_773 VCCD ) ( FILLER_773 VCCHIB ) ( FILLER_564 VCCHIB )
       ( FILLER_564 VCCD ) ( FILLER_772 VCCD ) ( FILLER_772 VCCHIB )
       ( FILLER_563 VCCHIB ) ( FILLER_563 VCCD ) ( FILLER_771 VCCD )
       ( FILLER_771 VCCHIB ) ( FILLER_562 VCCHIB ) ( FILLER_562 VCCD )
       ( FILLER_561 VCCHIB ) ( FILLER_561 VCCD ) ( FILLER_770 VCCD )
       ( FILLER_770 VCCHIB ) ( FILLER_769 VCCD ) ( FILLER_769 VCCHIB )
       ( user2_vccd_lvclamp_pad VCCHIB ) ( FILLER_559 VCCHIB )
       ( user2_vccd_lvclamp_pad VCCD ) ( FILLER_559 VCCD )
       ( FILLER_558 VCCHIB ) ( FILLER_558 VCCD ) ( FILLER_557 VCCHIB )
       ( FILLER_557 VCCD ) ( user1_vccd_lvclamp_pad VCCD )
       ( FILLER_767 VCCD ) ( user1_vccd_lvclamp_pad VCCHIB )
       ( FILLER_767 VCCHIB ) ( FILLER_766 VCCD ) ( FILLER_766 VCCHIB )
       ( FILLER_556 VCCHIB ) ( FILLER_556 VCCD ) ( FILLER_765 VCCD )
       ( FILLER_765 VCCHIB ) ( FILLER_555 VCCHIB ) ( FILLER_555 VCCD )
       ( FILLER_764 VCCD ) ( FILLER_764 VCCHIB ) ( FILLER_554 VCCHIB )
       ( FILLER_554 VCCD ) ( FILLER_763 VCCD ) ( FILLER_763 VCCHIB )
       ( FILLER_553 VCCHIB ) ( FILLER_553 VCCD ) ( FILLER_762 VCCD )
       ( FILLER_762 VCCHIB ) ( FILLER_552 VCCHIB ) ( FILLER_552 VCCD )
       ( FILLER_761 VCCD ) ( FILLER_761 VCCHIB ) ( FILLER_551 VCCHIB )
       ( FILLER_551 VCCD ) ( FILLER_760 VCCD ) ( FILLER_760 VCCHIB )
       ( mgmt_vddio_hvclamp_pad\[1\] VCCHIB ) ( FILLER_759 VCCD )
       ( FILLER_759 VCCHIB ) ( FILLER_549 VCCHIB )
       ( mgmt_vddio_hvclamp_pad\[1\] VCCD ) ( FILLER_549 VCCD )
       ( FILLER_548 VCCHIB ) ( FILLER_548 VCCD ) ( FILLER_547 VCCHIB )
       ( FILLER_547 VCCD ) ( FILLER_546 VCCHIB ) ( FILLER_546 VCCD )
       ( mprj_pads.area1_io_pad\[13\] VCCD ) ( FILLER_757 VCCD )
       ( mprj_pads.area1_io_pad\[13\] VCCHIB ) ( FILLER_757 VCCHIB )
       ( FILLER_545 VCCHIB ) ( FILLER_545 VCCD ) ( FILLER_756 VCCD )
       ( FILLER_756 VCCHIB ) ( FILLER_544 VCCHIB ) ( FILLER_544 VCCD )
       ( FILLER_755 VCCD ) ( FILLER_755 VCCHIB ) ( FILLER_543 VCCHIB )
       ( FILLER_543 VCCD ) ( FILLER_754 VCCD ) ( FILLER_754 VCCHIB )
       ( FILLER_542 VCCHIB ) ( FILLER_542 VCCD ) ( FILLER_753 VCCD )
       ( FILLER_753 VCCHIB ) ( FILLER_541 VCCHIB ) ( FILLER_541 VCCD )
       ( FILLER_752 VCCD ) ( FILLER_752 VCCHIB ) ( FILLER_751 VCCD )
       ( FILLER_751 VCCHIB ) ( user2_vssa_hvclamp_pad VCCHIB )
       ( FILLER_750 VCCD ) ( FILLER_750 VCCHIB )
       ( user2_vssa_hvclamp_pad VCCD ) ( FILLER_539 VCCHIB )
       ( FILLER_538 VCCHIB ) ( FILLER_539 VCCD ) ( FILLER_538 VCCD )
       ( FILLER_537 VCCHIB ) ( FILLER_537 VCCD ) ( FILLER_536 VCCHIB )
       ( FILLER_536 VCCD ) ( user1_vdda_hvclamp_pad\[0\] VCCD )
       ( FILLER_748 VCCD ) ( user1_vdda_hvclamp_pad\[0\] VCCHIB )
       ( FILLER_748 VCCHIB ) ( FILLER_747 VCCD ) ( FILLER_747 VCCHIB )
       ( FILLER_535 VCCHIB ) ( FILLER_535 VCCD ) ( FILLER_746 VCCD )
       ( FILLER_746 VCCHIB ) ( FILLER_534 VCCHIB ) ( FILLER_534 VCCD )
       ( FILLER_745 VCCD ) ( FILLER_745 VCCHIB ) ( FILLER_533 VCCHIB )
       ( FILLER_533 VCCD ) ( FILLER_744 VCCD ) ( FILLER_744 VCCHIB )
       ( FILLER_532 VCCHIB ) ( FILLER_532 VCCD ) ( FILLER_743 VCCD )
       ( FILLER_743 VCCHIB ) ( FILLER_531 VCCHIB ) ( FILLER_531 VCCD )
       ( FILLER_742 VCCD ) ( FILLER_742 VCCHIB ) ( FILLER_741 VCCD )
       ( FILLER_741 VCCHIB ) ( FILLER_740 VCCD ) ( FILLER_740 VCCHIB )
       ( mprj_pads.area2_io_pad\[0\] VCCHIB ) ( FILLER_529 VCCHIB )
       ( mprj_pads.area2_io_pad\[0\] VCCD ) ( FILLER_529 VCCD )
       ( FILLER_528 VCCHIB ) ( FILLER_528 VCCD ) ( FILLER_527 VCCHIB )
       ( FILLER_527 VCCD ) ( FILLER_526 VCCHIB ) ( FILLER_526 VCCD )
       ( mprj_pads.area1_io_pad\[12\] VCCD )
       ( mprj_pads.area1_io_pad\[12\] VCCHIB ) ( FILLER_525 VCCHIB )
       ( FILLER_525 VCCD ) ( FILLER_738 VCCD ) ( FILLER_738 VCCHIB )
       ( FILLER_524 VCCHIB ) ( FILLER_524 VCCD ) ( FILLER_737 VCCD )
       ( FILLER_737 VCCHIB ) ( FILLER_523 VCCHIB ) ( FILLER_523 VCCD )
       ( FILLER_736 VCCD ) ( FILLER_736 VCCHIB ) ( FILLER_522 VCCHIB )
       ( FILLER_522 VCCD ) ( FILLER_735 VCCD ) ( FILLER_735 VCCHIB )
       ( FILLER_734 VCCD ) ( FILLER_734 VCCHIB ) ( FILLER_521 VCCHIB )
       ( FILLER_521 VCCD ) ( FILLER_733 VCCD ) ( FILLER_733 VCCHIB )
       ( FILLER_732 VCCD ) ( FILLER_732 VCCHIB )
       ( mprj_pads.area2_io_pad\[1\] VCCHIB ) ( FILLER_731 VCCD )
       ( FILLER_731 VCCHIB ) ( FILLER_519 VCCHIB )
       ( mprj_pads.area2_io_pad\[1\] VCCD ) ( FILLER_519 VCCD )
       ( FILLER_518 VCCHIB ) ( FILLER_518 VCCD ) ( FILLER_517 VCCHIB )
       ( FILLER_517 VCCD ) ( FILLER_516 VCCHIB ) ( FILLER_516 VCCD )
       ( FILLER_515 VCCHIB ) ( FILLER_515 VCCD )
       ( mprj_pads.area1_io_pad\[11\] VCCD )
       ( mprj_pads.area1_io_pad\[11\] VCCHIB ) ( FILLER_729 VCCD )
       ( FILLER_729 VCCHIB ) ( FILLER_514 VCCHIB ) ( FILLER_514 VCCD )
       ( FILLER_728 VCCD ) ( FILLER_728 VCCHIB ) ( FILLER_513 VCCHIB )
       ( FILLER_513 VCCD ) ( FILLER_727 VCCD ) ( FILLER_727 VCCHIB )
       ( FILLER_512 VCCHIB ) ( FILLER_512 VCCD ) ( FILLER_726 VCCD )
       ( FILLER_726 VCCHIB ) ( FILLER_511 VCCHIB ) ( FILLER_511 VCCD )
       ( FILLER_725 VCCD ) ( FILLER_725 VCCHIB ) ( FILLER_724 VCCD )
       ( FILLER_724 VCCHIB ) ( FILLER_723 VCCD ) ( FILLER_723 VCCHIB )
       ( FILLER_722 VCCD ) ( FILLER_722 VCCHIB )
       ( mprj_pads.area2_io_pad\[2\] VCCHIB ) ( FILLER_509 VCCHIB )
       ( mprj_pads.area2_io_pad\[2\] VCCD ) ( FILLER_509 VCCD )
       ( FILLER_508 VCCHIB ) ( FILLER_508 VCCD ) ( FILLER_507 VCCHIB )
       ( FILLER_507 VCCD ) ( FILLER_506 VCCHIB ) ( FILLER_506 VCCD )
       ( FILLER_505 VCCHIB ) ( FILLER_505 VCCD )
       ( mprj_pads.area1_io_pad\[10\] VCCD ) ( FILLER_720 VCCD )
       ( FILLER_719 VCCD ) ( mprj_pads.area1_io_pad\[10\] VCCHIB )
       ( FILLER_720 VCCHIB ) ( FILLER_719 VCCHIB )
       ( FILLER_504 VCCHIB ) ( FILLER_504 VCCD ) ( FILLER_718 VCCD )
       ( FILLER_718 VCCHIB ) ( FILLER_503 VCCHIB ) ( FILLER_503 VCCD )
       ( FILLER_717 VCCD ) ( FILLER_717 VCCHIB ) ( FILLER_502 VCCHIB )
       ( FILLER_502 VCCD ) ( FILLER_501 VCCHIB ) ( FILLER_501 VCCD )
       ( FILLER_716 VCCD ) ( FILLER_716 VCCHIB ) ( FILLER_715 VCCD )
       ( FILLER_715 VCCHIB ) ( FILLER_714 VCCD ) ( FILLER_714 VCCHIB )
       ( FILLER_713 VCCD ) ( FILLER_713 VCCHIB ) ( FILLER_712 VCCD )
       ( FILLER_712 VCCHIB ) ( mprj_pads.area2_io_pad\[3\] VCCHIB )
       ( FILLER_499 VCCHIB ) ( mprj_pads.area2_io_pad\[3\] VCCD )
       ( FILLER_499 VCCD ) ( FILLER_498 VCCHIB ) ( FILLER_498 VCCD )
       ( FILLER_497 VCCHIB ) ( FILLER_497 VCCD ) ( FILLER_496 VCCHIB )
       ( FILLER_496 VCCD ) ( FILLER_495 VCCHIB ) ( FILLER_495 VCCD )
       ( FILLER_494 VCCHIB ) ( FILLER_494 VCCD )
       ( mprj_pads.area1_io_pad\[9\] VCCD )
       ( mprj_pads.area1_io_pad\[9\] VCCHIB ) ( FILLER_710 VCCD )
       ( FILLER_710 VCCHIB ) ( FILLER_493 VCCHIB ) ( FILLER_493 VCCD )
       ( FILLER_709 VCCD ) ( FILLER_709 VCCHIB ) ( FILLER_492 VCCHIB )
       ( FILLER_492 VCCD ) ( FILLER_708 VCCD ) ( FILLER_708 VCCHIB )
       ( FILLER_491 VCCHIB ) ( FILLER_491 VCCD ) ( FILLER_707 VCCD )
       ( FILLER_707 VCCHIB ) ( FILLER_706 VCCD ) ( FILLER_706 VCCHIB )
       ( FILLER_705 VCCD ) ( FILLER_705 VCCHIB ) ( FILLER_704 VCCD )
       ( FILLER_704 VCCHIB ) ( mprj_pads.area2_io_pad\[4\] VCCHIB )
       ( FILLER_489 VCCHIB ) ( mprj_pads.area2_io_pad\[4\] VCCD )
       ( FILLER_489 VCCD ) ( FILLER_488 VCCHIB ) ( FILLER_488 VCCD )
       ( FILLER_703 VCCD ) ( FILLER_703 VCCHIB ) ( FILLER_487 VCCHIB )
       ( FILLER_487 VCCD ) ( FILLER_486 VCCHIB ) ( FILLER_486 VCCD )
       ( FILLER_485 VCCHIB ) ( FILLER_485 VCCD ) ( FILLER_484 VCCHIB )
       ( FILLER_484 VCCD ) ( mprj_pads.area1_io_pad\[8\] VCCD )
       ( FILLER_701 VCCD ) ( mprj_pads.area1_io_pad\[8\] VCCHIB )
       ( FILLER_701 VCCHIB ) ( FILLER_483 VCCHIB ) ( FILLER_483 VCCD )
       ( FILLER_700 VCCD ) ( FILLER_700 VCCHIB ) ( FILLER_482 VCCHIB )
       ( FILLER_482 VCCD ) ( FILLER_699 VCCD ) ( FILLER_699 VCCHIB )
       ( FILLER_481 VCCHIB ) ( FILLER_481 VCCD ) ( FILLER_698 VCCD )
       ( FILLER_698 VCCHIB ) ( FILLER_697 VCCD ) ( FILLER_697 VCCHIB )
       ( FILLER_696 VCCD ) ( FILLER_696 VCCHIB ) ( FILLER_695 VCCD )
       ( FILLER_695 VCCHIB ) ( FILLER_694 VCCD ) ( FILLER_694 VCCHIB )
       ( mprj_pads.area2_io_pad\[5\] VCCHIB ) ( FILLER_479 VCCHIB )
       ( FILLER_478 VCCHIB ) ( mprj_pads.area2_io_pad\[5\] VCCD )
       ( FILLER_479 VCCD ) ( FILLER_478 VCCD ) ( FILLER_477 VCCHIB )
       ( FILLER_477 VCCD ) ( FILLER_693 VCCD ) ( FILLER_693 VCCHIB )
       ( FILLER_476 VCCHIB ) ( FILLER_476 VCCD ) ( FILLER_475 VCCHIB )
       ( FILLER_475 VCCD ) ( FILLER_474 VCCHIB ) ( FILLER_474 VCCD )
       ( FILLER_473 VCCHIB ) ( FILLER_473 VCCD )
       ( mprj_pads.area1_io_pad\[7\] VCCD )
       ( mprj_pads.area1_io_pad\[7\] VCCHIB ) ( FILLER_691 VCCD )
       ( FILLER_691 VCCHIB ) ( FILLER_472 VCCHIB ) ( FILLER_472 VCCD )
       ( FILLER_690 VCCD ) ( FILLER_690 VCCHIB ) ( FILLER_471 VCCHIB )
       ( FILLER_471 VCCD ) ( FILLER_689 VCCD ) ( FILLER_689 VCCHIB )
       ( FILLER_688 VCCD ) ( FILLER_688 VCCHIB ) ( FILLER_687 VCCD )
       ( FILLER_687 VCCHIB ) ( FILLER_686 VCCD ) ( FILLER_686 VCCHIB )
       ( mprj_pads.area2_io_pad\[6\] VCCHIB )
       ( mprj_pads.area2_io_pad\[6\] VCCD ) ( FILLER_469 VCCHIB )
       ( FILLER_468 VCCHIB ) ( FILLER_469 VCCD ) ( FILLER_468 VCCD )
       ( FILLER_685 VCCD ) ( FILLER_685 VCCHIB ) ( FILLER_467 VCCHIB )
       ( FILLER_467 VCCD ) ( FILLER_684 VCCD ) ( FILLER_684 VCCHIB )
       ( FILLER_466 VCCHIB ) ( FILLER_466 VCCD ) ( FILLER_465 VCCHIB )
       ( FILLER_465 VCCD ) ( FILLER_464 VCCHIB ) ( FILLER_464 VCCD )
       ( FILLER_463 VCCHIB ) ( FILLER_463 VCCD )
       ( user1_vdda_hvclamp_pad\[1\] VCCD ) ( FILLER_682 VCCD )
       ( user1_vdda_hvclamp_pad\[1\] VCCHIB ) ( FILLER_682 VCCHIB )
       ( FILLER_462 VCCHIB ) ( FILLER_462 VCCD ) ( FILLER_681 VCCD )
       ( FILLER_681 VCCHIB ) ( FILLER_461 VCCHIB ) ( FILLER_461 VCCD )
       ( FILLER_680 VCCD ) ( FILLER_680 VCCHIB ) ( FILLER_679 VCCD )
       ( FILLER_679 VCCHIB ) ( FILLER_678 VCCD ) ( FILLER_678 VCCHIB )
       ( FILLER_677 VCCD ) ( FILLER_677 VCCHIB )
       ( user2_vdda_hvclamp_pad VCCHIB ) ( FILLER_459 VCCHIB )
       ( FILLER_458 VCCHIB ) ( user2_vdda_hvclamp_pad VCCD )
       ( FILLER_459 VCCD ) ( FILLER_458 VCCD ) ( FILLER_457 VCCHIB )
       ( FILLER_457 VCCD ) ( FILLER_676 VCCD ) ( FILLER_676 VCCHIB )
       ( FILLER_675 VCCD ) ( FILLER_675 VCCHIB ) ( FILLER_456 VCCHIB )
       ( FILLER_456 VCCD ) ( FILLER_455 VCCHIB ) ( FILLER_455 VCCD )
       ( FILLER_454 VCCHIB ) ( FILLER_454 VCCD ) ( FILLER_453 VCCHIB )
       ( FILLER_453 VCCD ) ( user1_vssd_lvclamp_pad VCCD )
       ( FILLER_673 VCCD ) ( user1_vssd_lvclamp_pad VCCHIB )
       ( FILLER_673 VCCHIB ) ( FILLER_452 VCCHIB ) ( FILLER_452 VCCD )
       ( FILLER_672 VCCD ) ( FILLER_672 VCCHIB ) ( FILLER_671 VCCD )
       ( FILLER_451 VCCHIB ) ( gpio_pad VCCD ) ( FILLER_451 VCCD )
       ( FILLER_671 VCCHIB ) ( FILLER_670 VCCD ) ( FILLER_670 VCCHIB )
       ( FILLER_669 VCCD ) ( FILLER_669 VCCHIB ) ( FILLER_668 VCCD )
       ( FILLER_668 VCCHIB ) ( user2_vssd_lvclamp_pad VCCHIB )
       ( FILLER_449 VCCHIB ) ( user2_vssd_lvclamp_pad VCCD )
       ( FILLER_449 VCCD ) ( FILLER_667 VCCD ) ( FILLER_667 VCCHIB )
       ( FILLER_448 VCCHIB ) ( FILLER_448 VCCD ) ( FILLER_447 VCCHIB )
       ( FILLER_447 VCCD ) ( FILLER_666 VCCD ) ( FILLER_666 VCCHIB )
       ( FILLER_446 VCCHIB ) ( FILLER_446 VCCD ) ( FILLER_665 VCCD )
       ( FILLER_665 VCCHIB ) ( FILLER_445 VCCHIB ) ( FILLER_445 VCCD )
       ( FILLER_444 VCCHIB ) ( FILLER_444 VCCD ) ( FILLER_443 VCCHIB )
       ( FILLER_443 VCCD ) ( FILLER_442 VCCHIB ) ( FILLER_442 VCCD )
       ( user1_vssa_hvclamp_pad\[1\] VCCD ) ( FILLER_663 VCCD )
       ( user1_vssa_hvclamp_pad\[1\] VCCHIB ) ( FILLER_663 VCCHIB )
       ( FILLER_441 VCCHIB ) ( FILLER_441 VCCD ) ( FILLER_662 VCCD )
       ( FILLER_662 VCCHIB ) ( FILLER_661 VCCD ) ( FILLER_661 VCCHIB )
       ( FILLER_660 VCCD ) ( FILLER_660 VCCHIB ) ( FILLER_659 VCCD )
       ( FILLER_659 VCCHIB ) ( mprj_pads.area2_io_pad\[7\] VCCHIB )
       ( FILLER_439 VCCHIB ) ( FILLER_438 VCCHIB )
       ( mprj_pads.area2_io_pad\[7\] VCCD ) ( FILLER_439 VCCD )
       ( FILLER_438 VCCD ) ( FILLER_658 VCCD ) ( FILLER_658 VCCHIB )
       ( FILLER_437 VCCHIB ) ( FILLER_437 VCCD ) ( FILLER_657 VCCD )
       ( FILLER_657 VCCHIB ) ( FILLER_436 VCCHIB ) ( FILLER_436 VCCD )
       ( FILLER_656 VCCD ) ( FILLER_656 VCCHIB ) ( FILLER_435 VCCHIB )
       ( FILLER_435 VCCD ) ( FILLER_434 VCCHIB ) ( FILLER_434 VCCD )
       ( FILLER_433 VCCHIB ) ( FILLER_433 VCCD ) ( FILLER_432 VCCHIB )
       ( FILLER_432 VCCD ) ( mprj_pads.area1_io_pad\[6\] VCCD )
       ( FILLER_654 VCCD ) ( mprj_pads.area1_io_pad\[6\] VCCHIB )
       ( FILLER_654 VCCHIB ) ( FILLER_431 VCCHIB ) ( FILLER_431 VCCD )
       ( FILLER_653 VCCD ) ( FILLER_653 VCCHIB ) ( FILLER_652 VCCD )
       ( FILLER_652 VCCHIB ) ( FILLER_651 VCCD ) ( FILLER_651 VCCHIB )
       ( FILLER_650 VCCD ) ( FILLER_650 VCCHIB )
       ( mprj_pads.area2_io_pad\[8\] VCCHIB )
       ( mprj_pads.area2_io_pad\[8\] VCCD ) ( FILLER_649 VCCD )
       ( FILLER_649 VCCHIB ) ( FILLER_429 VCCHIB )
       ( FILLER_428 VCCHIB ) ( FILLER_429 VCCD ) ( FILLER_428 VCCD )
       ( FILLER_427 VCCHIB ) ( FILLER_427 VCCD ) ( FILLER_648 VCCD )
       ( FILLER_648 VCCHIB ) ( FILLER_426 VCCHIB ) ( FILLER_426 VCCD )
       ( FILLER_647 VCCD ) ( FILLER_647 VCCHIB ) ( FILLER_425 VCCHIB )
       ( FILLER_425 VCCD ) ( FILLER_646 VCCD ) ( FILLER_646 VCCHIB )
       ( FILLER_424 VCCHIB ) ( FILLER_424 VCCD ) ( FILLER_423 VCCHIB )
       ( FILLER_423 VCCD ) ( FILLER_422 VCCHIB ) ( FILLER_422 VCCD )
       ( FILLER_421 VCCHIB ) ( FILLER_421 VCCD )
       ( mprj_pads.area1_io_pad\[5\] VCCD )
       ( mprj_pads.area1_io_pad\[5\] VCCHIB ) ( FILLER_644 VCCD )
       ( FILLER_644 VCCHIB ) ( FILLER_643 VCCD ) ( FILLER_643 VCCHIB )
       ( FILLER_642 VCCD ) ( FILLER_642 VCCHIB ) ( FILLER_641 VCCD )
       ( FILLER_641 VCCHIB ) ( mprj_pads.area2_io_pad\[9\] VCCHIB )
       ( FILLER_419 VCCHIB ) ( mprj_pads.area2_io_pad\[9\] VCCD )
       ( FILLER_419 VCCD ) ( FILLER_418 VCCHIB ) ( FILLER_418 VCCD )
       ( FILLER_640 VCCD ) ( FILLER_640 VCCHIB ) ( FILLER_417 VCCHIB )
       ( FILLER_417 VCCD ) ( FILLER_639 VCCD ) ( FILLER_639 VCCHIB )
       ( FILLER_416 VCCHIB ) ( FILLER_416 VCCD ) ( FILLER_638 VCCD )
       ( FILLER_638 VCCHIB ) ( FILLER_415 VCCHIB ) ( FILLER_415 VCCD )
       ( FILLER_637 VCCD ) ( FILLER_637 VCCHIB ) ( FILLER_414 VCCHIB )
       ( FILLER_414 VCCD ) ( FILLER_413 VCCHIB ) ( FILLER_413 VCCD )
       ( FILLER_412 VCCHIB ) ( FILLER_412 VCCD ) ( FILLER_411 VCCHIB )
       ( FILLER_411 VCCD ) ( mprj_pads.area1_io_pad\[4\] VCCD )
       ( mprj_pads.area1_io_pad\[4\] VCCHIB ) ( FILLER_635 VCCD )
       ( FILLER_635 VCCHIB ) ( FILLER_634 VCCD ) ( FILLER_634 VCCHIB )
       ( FILLER_633 VCCD ) ( FILLER_633 VCCHIB )
       ( mprj_pads.area2_io_pad\[10\] VCCHIB ) ( FILLER_409 VCCHIB )
       ( mprj_pads.area2_io_pad\[10\] VCCD ) ( FILLER_409 VCCD )
       ( FILLER_632 VCCD ) ( FILLER_632 VCCHIB ) ( FILLER_408 VCCHIB )
       ( FILLER_408 VCCD ) ( FILLER_407 VCCHIB ) ( FILLER_407 VCCD )
       ( FILLER_631 VCCD ) ( FILLER_631 VCCHIB ) ( FILLER_406 VCCHIB )
       ( FILLER_406 VCCD ) ( FILLER_630 VCCD ) ( FILLER_630 VCCHIB )
       ( FILLER_405 VCCHIB ) ( FILLER_405 VCCD ) ( FILLER_629 VCCD )
       ( FILLER_629 VCCHIB ) ( FILLER_404 VCCHIB ) ( FILLER_404 VCCD )
       ( FILLER_628 VCCD ) ( FILLER_628 VCCHIB ) ( FILLER_403 VCCHIB )
       ( FILLER_403 VCCD ) ( FILLER_402 VCCHIB ) ( FILLER_402 VCCD )
       ( FILLER_401 VCCHIB ) ( FILLER_401 VCCD )
       ( mprj_pads.area1_io_pad\[3\] VCCD )
       ( mprj_pads.area1_io_pad\[3\] VCCHIB ) ( FILLER_626 VCCD )
       ( FILLER_625 VCCD ) ( FILLER_626 VCCHIB ) ( FILLER_625 VCCHIB )
       ( FILLER_624 VCCD ) ( FILLER_624 VCCHIB ) ( FILLER_623 VCCD )
       ( FILLER_623 VCCHIB ) ( mprj_pads.area2_io_pad\[11\] VCCHIB )
       ( FILLER_399 VCCHIB ) ( mprj_pads.area2_io_pad\[11\] VCCD )
       ( FILLER_399 VCCD ) ( FILLER_398 VCCHIB ) ( FILLER_398 VCCD )
       ( FILLER_622 VCCD ) ( FILLER_622 VCCHIB ) ( FILLER_397 VCCHIB )
       ( FILLER_397 VCCD ) ( FILLER_621 VCCD ) ( FILLER_621 VCCHIB )
       ( FILLER_396 VCCHIB ) ( FILLER_396 VCCD ) ( FILLER_620 VCCD )
       ( FILLER_620 VCCHIB ) ( FILLER_395 VCCHIB ) ( FILLER_395 VCCD )
       ( FILLER_619 VCCD ) ( FILLER_619 VCCHIB ) ( FILLER_394 VCCHIB )
       ( FILLER_394 VCCD ) ( FILLER_618 VCCD ) ( FILLER_618 VCCHIB )
       ( FILLER_393 VCCHIB ) ( FILLER_393 VCCD ) ( FILLER_392 VCCHIB )
       ( FILLER_392 VCCD ) ( FILLER_391 VCCHIB ) ( FILLER_391 VCCD )
       ( mprj_pads.area1_io_pad\[2\] VCCD ) ( FILLER_616 VCCD )
       ( mprj_pads.area1_io_pad\[2\] VCCHIB ) ( FILLER_616 VCCHIB )
       ( FILLER_615 VCCD ) ( FILLER_615 VCCHIB ) ( FILLER_614 VCCD )
       ( FILLER_614 VCCHIB ) ( mprj_pads.area2_io_pad\[12\] VCCHIB )
       ( FILLER_389 VCCHIB ) ( FILLER_388 VCCHIB )
       ( mprj_pads.area2_io_pad\[12\] VCCD ) ( FILLER_389 VCCD )
       ( FILLER_388 VCCD ) ( FILLER_387 VCCHIB ) ( FILLER_387 VCCD )
       ( FILLER_613 VCCD ) ( FILLER_613 VCCHIB ) ( FILLER_386 VCCHIB )
       ( FILLER_386 VCCD ) ( FILLER_612 VCCD ) ( FILLER_612 VCCHIB )
       ( FILLER_385 VCCHIB ) ( FILLER_385 VCCD ) ( FILLER_611 VCCD )
       ( FILLER_611 VCCHIB ) ( FILLER_384 VCCHIB ) ( FILLER_384 VCCD )
       ( FILLER_610 VCCD ) ( FILLER_610 VCCHIB ) ( FILLER_383 VCCHIB )
       ( FILLER_383 VCCD ) ( FILLER_609 VCCD ) ( FILLER_609 VCCHIB )
       ( FILLER_382 VCCHIB ) ( FILLER_382 VCCD ) ( FILLER_381 VCCHIB )
       ( FILLER_381 VCCD ) ( FILLER_380 VCCHIB ) ( FILLER_380 VCCD )
       ( FILLER_379 VCCHIB ) ( FILLER_379 VCCD )
       ( mprj_pads.area1_io_pad\[1\] VCCD ) ( FILLER_607 VCCD )
       ( mprj_pads.area1_io_pad\[1\] VCCHIB ) ( FILLER_607 VCCHIB )
       ( FILLER_606 VCCD ) ( FILLER_606 VCCHIB ) ( FILLER_378 VCCHIB )
       ( FILLER_378 VCCD ) ( FILLER_605 VCCD ) ( FILLER_605 VCCHIB )
       ( FILLER_377 VCCHIB ) ( FILLER_377 VCCD ) ( FILLER_604 VCCD )
       ( FILLER_604 VCCHIB ) ( FILLER_376 VCCHIB ) ( FILLER_376 VCCD )
       ( FILLER_603 VCCD ) ( FILLER_603 VCCHIB ) ( FILLER_375 VCCHIB )
       ( FILLER_375 VCCD ) ( FILLER_602 VCCD ) ( FILLER_602 VCCHIB )
       ( FILLER_374 VCCHIB ) ( FILLER_374 VCCD ) ( FILLER_SB2 VCCHIB )
       ( disconnect_vdda_2 VCCHIB ) ( FILLER_SB2 VCCD )
       ( disconnect_vdda_2 VCCD ) ( FILLER_601 VCCD )
       ( FILLER_601 VCCHIB ) ( FILLER_600 VCCD ) ( FILLER_600 VCCHIB )
       ( mgmt_vddio_hvclamp_pad\[0\] VCCHIB ) ( FILLER_599 VCCD )
       ( FILLER_599 VCCHIB ) ( FILLER_370 VCCHIB )
       ( mgmt_vddio_hvclamp_pad\[0\] VCCD ) ( FILLER_370 VCCD )
       ( FILLER_369 VCCHIB ) ( FILLER_369 VCCD ) ( FILLER_368 VCCHIB )
       ( FILLER_368 VCCD ) ( FILLER_367 VCCHIB ) ( FILLER_367 VCCD )
       ( mprj_pads.area1_io_pad\[0\] VCCD )
       ( mprj_pads.area1_io_pad\[0\] VCCHIB ) ( FILLER_597 VCCD )
       ( FILLER_597 VCCHIB ) ( FILLER_366 VCCHIB ) ( FILLER_366 VCCD )
       ( FILLER_596 VCCD ) ( FILLER_596 VCCHIB ) ( FILLER_365 VCCHIB )
       ( FILLER_365 VCCD ) ( FILLER_595 VCCD ) ( FILLER_595 VCCHIB )
       ( FILLER_364 VCCHIB ) ( FILLER_364 VCCD ) ( FILLER_594 VCCD )
       ( FILLER_594 VCCHIB ) ( FILLER_363 VCCHIB ) ( FILLER_363 VCCD )
       ( FILLER_593 VCCD ) ( FILLER_593 VCCHIB ) ( FILLER_362 VCCHIB )
       ( FILLER_362 VCCD ) ( FILLER_592 VCCD ) ( FILLER_592 VCCHIB )
       ( FILLER_591 VCCD ) ( FILLER_591 VCCHIB ) ( FILLER_590 VCCD )
       ( FILLER_590 VCCHIB ) ( disconnect_vdda_1 VCCD )
       ( FILLER_SB1 VCCD ) ( disconnect_vdda_1 VCCHIB )
       ( FILLER_SB1 VCCHIB ) ( FILLER_587 VCCD ) ( FILLER_587 VCCHIB )
       ( mgmt_vccd_lvclamp_pad VCCHIB ) ( FILLER_360 VCCHIB )
       ( mgmt_vccd_lvclamp_pad VCCD ) ( FILLER_360 VCCD )
       ( FILLER_359 VCCHIB ) ( FILLER_359 VCCD ) ( FILLER_358 VCCHIB )
       ( FILLER_358 VCCD ) ( FILLER_586 VCCD ) ( FILLER_586 VCCHIB )
       ( FILLER_357 VCCHIB ) ( FILLER_357 VCCD ) ( FILLER_585 VCCD )
       ( FILLER_585 VCCHIB ) ( FILLER_356 VCCHIB ) ( FILLER_356 VCCD )
       ( FILLER_584 VCCD ) ( FILLER_584 VCCHIB ) ( FILLER_583 VCCD )
       ( FILLER_583 VCCHIB ) ( FILLER_355 VCCHIB ) ( FILLER_355 VCCD )
       ( FILLER_582 VCCD ) ( FILLER_582 VCCHIB ) ( FILLER_354 VCCHIB )
       ( FILLER_354 VCCD ) ( FILLER_581 VCCD ) ( FILLER_581 VCCHIB )
       ( FILLER_353 VCCHIB ) ( FILLER_353 VCCD )
       ( constant_block_6 vccd ) ( FILLER_352 VCCHIB )
       ( FILLER_352 VCCD ) ( FILLER_580 VCCD ) ( FILLER_580 VCCHIB )
       ( constant_block_5 vccd ) ( constant_block_4 vccd )
       ( constant_block_3 vccd ) ( constant_block_2 vccd )
       ( constant_block_1 vccd ) ( constant_block_0 vccd )
       ( mgmt_corner\[1\] VCCHIB ) ( FILLER_351 VCCHIB )
       ( FILLER_350 VCCHIB ) ( FILLER_349 VCCHIB )
       ( FILLER_348 VCCHIB ) ( FILLER_347 VCCHIB )
       ( FILLER_346 VCCHIB ) ( FILLER_339 VCCHIB )
       ( FILLER_338 VCCHIB ) ( FILLER_337 VCCHIB )
       ( FILLER_336 VCCHIB ) ( FILLER_335 VCCHIB )
       ( mgmt_vdda_hvclamp_pad VCCHIB ) ( FILLER_333 VCCHIB )
       ( FILLER_332 VCCHIB ) ( FILLER_331 VCCHIB )
       ( FILLER_330 VCCHIB ) ( FILLER_322 VCCHIB )
       ( FILLER_329 VCCHIB ) ( FILLER_321 VCCHIB )
       ( FILLER_320 VCCHIB ) ( FILLER_319 VCCHIB )
       ( FILLER_318 VCCHIB ) ( mgmt_vssio_hvclamp_pad\[0\] VCCHIB )
       ( FILLER_316 VCCHIB ) ( FILLER_315 VCCHIB )
       ( FILLER_314 VCCHIB ) ( FILLER_313 VCCHIB )
       ( FILLER_305 VCCHIB ) ( FILLER_312 VCCHIB )
       ( FILLER_304 VCCHIB ) ( FILLER_303 VCCHIB )
       ( FILLER_302 VCCHIB ) ( FILLER_301 VCCHIB ) ( gpio_pad VCCHIB )
       ( FILLER_299 VCCHIB ) ( FILLER_298 VCCHIB )
       ( FILLER_297 VCCHIB ) ( FILLER_296 VCCHIB )
       ( FILLER_295 VCCHIB ) ( FILLER_288 VCCHIB )
       ( FILLER_287 VCCHIB ) ( FILLER_286 VCCHIB )
       ( FILLER_285 VCCHIB ) ( FILLER_284 VCCHIB )
       ( flash_io1_pad VCCHIB ) ( FILLER_282 VCCHIB )
       ( FILLER_281 VCCHIB ) ( FILLER_280 VCCHIB )
       ( FILLER_279 VCCHIB ) ( FILLER_271 VCCHIB )
       ( FILLER_278 VCCHIB ) ( FILLER_270 VCCHIB )
       ( FILLER_269 VCCHIB ) ( FILLER_268 VCCHIB )
       ( FILLER_267 VCCHIB ) ( flash_io0_pad VCCHIB )
       ( FILLER_265 VCCHIB ) ( FILLER_264 VCCHIB )
       ( FILLER_263 VCCHIB ) ( FILLER_262 VCCHIB )
       ( FILLER_261 VCCHIB ) ( FILLER_254 VCCHIB )
       ( FILLER_253 VCCHIB ) ( FILLER_252 VCCHIB )
       ( FILLER_251 VCCHIB ) ( FILLER_250 VCCHIB )
       ( flash_clk_pad VCCHIB ) ( FILLER_248 VCCHIB )
       ( FILLER_247 VCCHIB ) ( FILLER_246 VCCHIB )
       ( FILLER_245 VCCHIB ) ( FILLER_237 VCCHIB )
       ( FILLER_244 VCCHIB ) ( FILLER_236 VCCHIB )
       ( FILLER_235 VCCHIB ) ( FILLER_234 VCCHIB )
       ( FILLER_233 VCCHIB ) ( flash_csb_pad VCCHIB )
       ( FILLER_231 VCCHIB ) ( FILLER_230 VCCHIB )
       ( FILLER_229 VCCHIB ) ( FILLER_228 VCCHIB )
       ( FILLER_227 VCCHIB ) ( FILLER_220 VCCHIB )
       ( FILLER_219 VCCHIB ) ( FILLER_218 VCCHIB )
       ( FILLER_217 VCCHIB ) ( FILLER_216 VCCHIB )
       ( mgmt_vssd_lvclamp_pad VCCHIB ) ( FILLER_214 VCCHIB )
       ( FILLER_213 VCCHIB ) ( FILLER_212 VCCHIB )
       ( FILLER_211 VCCHIB ) ( FILLER_203 VCCHIB )
       ( FILLER_210 VCCHIB ) ( FILLER_202 VCCHIB )
       ( FILLER_201 VCCHIB ) ( FILLER_200 VCCHIB )
       ( FILLER_199 VCCHIB ) ( clock_pad VCCHIB )
       ( FILLER_197 VCCHIB ) ( FILLER_196 VCCHIB )
       ( FILLER_195 VCCHIB ) ( FILLER_194 VCCHIB )
       ( FILLER_186 VCCHIB ) ( FILLER_193 VCCHIB )
       ( FILLER_185 VCCHIB ) ( FILLER_184 VCCHIB )
       ( FILLER_183 VCCHIB ) ( FILLER_182 VCCHIB )
       ( resetb_pad VCCHIB ) ( FILLER_180 VCCHIB )
       ( FILLER_179 VCCHIB ) ( FILLER_178 VCCHIB )
       ( FILLER_177 VCCHIB ) ( FILLER_176 VCCHIB )
       ( FILLER_169 VCCHIB ) ( FILLER_168 VCCHIB )
       ( FILLER_167 VCCHIB ) ( FILLER_166 VCCHIB )
       ( FILLER_165 VCCHIB ) ( mgmt_vssa_hvclamp_pad VCCHIB )
       ( FILLER_163 VCCHIB ) ( FILLER_162 VCCHIB )
       ( FILLER_161 VCCHIB ) ( FILLER_160 VCCHIB )
       ( mgmt_corner\[1\] VCCD ) ( FILLER_159 VCCHIB )
       ( FILLER_152 VCCHIB ) ( FILLER_151 VCCHIB )
       ( FILLER_150 VCCHIB ) ( FILLER_149 VCCHIB )
       ( mgmt_corner\[0\] VCCHIB ) ( FILLER_148 VCCHIB )
       ( FILLER_351 VCCD ) ( FILLER_350 VCCD ) ( FILLER_349 VCCD )
       ( FILLER_348 VCCD ) ( FILLER_347 VCCD ) ( FILLER_346 VCCD )
       ( bus_tie_72 VCCHIB ) ( bus_tie_72 VCCD ) ( bus_tie_71 VCCHIB )
       ( bus_tie_71 VCCD ) ( bus_tie_70 VCCHIB ) ( bus_tie_70 VCCD )
       ( bus_tie_69 VCCHIB ) ( bus_tie_69 VCCD ) ( bus_tie_68 VCCHIB )
       ( bus_tie_68 VCCD ) ( bus_tie_67 VCCHIB ) ( bus_tie_67 VCCD )
       ( FILLER_339 VCCD ) ( FILLER_338 VCCD ) ( FILLER_337 VCCD )
       ( FILLER_336 VCCD ) ( FILLER_335 VCCD )
       ( mgmt_vdda_hvclamp_pad VCCD ) ( FILLER_333 VCCD )
       ( FILLER_332 VCCD ) ( FILLER_331 VCCD ) ( FILLER_330 VCCD )
       ( bus_tie_66 VCCHIB ) ( FILLER_329 VCCD ) ( bus_tie_66 VCCD )
       ( bus_tie_65 VCCHIB ) ( bus_tie_65 VCCD ) ( bus_tie_64 VCCHIB )
       ( bus_tie_64 VCCD ) ( bus_tie_63 VCCHIB ) ( bus_tie_63 VCCD )
       ( bus_tie_62 VCCHIB ) ( bus_tie_62 VCCD ) ( bus_tie_61 VCCHIB )
       ( bus_tie_61 VCCD ) ( FILLER_322 VCCD ) ( FILLER_321 VCCD )
       ( FILLER_320 VCCD ) ( FILLER_319 VCCD ) ( FILLER_318 VCCD )
       ( mgmt_vssio_hvclamp_pad\[0\] VCCD ) ( FILLER_316 VCCD )
       ( FILLER_315 VCCD ) ( FILLER_314 VCCD ) ( FILLER_313 VCCD )
       ( bus_tie_60 VCCHIB ) ( FILLER_312 VCCD ) ( bus_tie_60 VCCD )
       ( bus_tie_59 VCCHIB ) ( bus_tie_59 VCCD ) ( bus_tie_58 VCCHIB )
       ( bus_tie_58 VCCD ) ( bus_tie_57 VCCHIB ) ( bus_tie_57 VCCD )
       ( bus_tie_56 VCCHIB ) ( bus_tie_56 VCCD ) ( bus_tie_55 VCCHIB )
       ( bus_tie_55 VCCD ) ( FILLER_305 VCCD ) ( FILLER_304 VCCD )
       ( FILLER_303 VCCD ) ( FILLER_302 VCCD ) ( FILLER_301 VCCD )
       ( clock_pad VCCD ) ( FILLER_299 VCCD ) ( FILLER_298 VCCD )
       ( FILLER_297 VCCD ) ( FILLER_296 VCCD ) ( FILLER_295 VCCD )
       ( bus_tie_54 VCCHIB ) ( bus_tie_54 VCCD ) ( bus_tie_53 VCCHIB )
       ( bus_tie_53 VCCD ) ( bus_tie_52 VCCHIB ) ( bus_tie_52 VCCD )
       ( bus_tie_51 VCCHIB ) ( bus_tie_51 VCCD ) ( bus_tie_50 VCCHIB )
       ( bus_tie_50 VCCD ) ( bus_tie_49 VCCHIB ) ( bus_tie_49 VCCD )
       ( FILLER_288 VCCD ) ( FILLER_287 VCCD ) ( FILLER_286 VCCD )
       ( FILLER_285 VCCD ) ( FILLER_284 VCCD ) ( flash_io1_pad VCCD )
       ( FILLER_282 VCCD ) ( FILLER_281 VCCD ) ( FILLER_280 VCCD )
       ( FILLER_279 VCCD ) ( bus_tie_48 VCCHIB ) ( FILLER_278 VCCD )
       ( bus_tie_48 VCCD ) ( bus_tie_47 VCCHIB ) ( bus_tie_47 VCCD )
       ( bus_tie_46 VCCHIB ) ( bus_tie_46 VCCD ) ( bus_tie_45 VCCHIB )
       ( bus_tie_45 VCCD ) ( bus_tie_44 VCCHIB ) ( bus_tie_44 VCCD )
       ( bus_tie_43 VCCHIB ) ( bus_tie_43 VCCD ) ( FILLER_271 VCCD )
       ( FILLER_270 VCCD ) ( FILLER_269 VCCD ) ( FILLER_268 VCCD )
       ( FILLER_267 VCCD ) ( flash_io0_pad VCCD ) ( FILLER_265 VCCD )
       ( FILLER_264 VCCD ) ( FILLER_263 VCCD ) ( FILLER_262 VCCD )
       ( FILLER_261 VCCD ) ( bus_tie_42 VCCHIB ) ( bus_tie_42 VCCD )
       ( bus_tie_41 VCCHIB ) ( bus_tie_41 VCCD ) ( bus_tie_40 VCCHIB )
       ( bus_tie_40 VCCD ) ( bus_tie_39 VCCHIB ) ( bus_tie_39 VCCD )
       ( bus_tie_38 VCCHIB ) ( bus_tie_38 VCCD ) ( bus_tie_37 VCCHIB )
       ( bus_tie_37 VCCD ) ( FILLER_254 VCCD ) ( FILLER_253 VCCD )
       ( FILLER_252 VCCD ) ( FILLER_251 VCCD ) ( FILLER_250 VCCD )
       ( flash_clk_pad VCCD ) ( FILLER_248 VCCD ) ( FILLER_247 VCCD )
       ( FILLER_246 VCCD ) ( FILLER_245 VCCD ) ( bus_tie_36 VCCHIB )
       ( FILLER_244 VCCD ) ( bus_tie_36 VCCD ) ( bus_tie_35 VCCHIB )
       ( bus_tie_35 VCCD ) ( bus_tie_34 VCCHIB ) ( bus_tie_34 VCCD )
       ( bus_tie_33 VCCHIB ) ( bus_tie_33 VCCD ) ( bus_tie_32 VCCHIB )
       ( bus_tie_32 VCCD ) ( bus_tie_31 VCCHIB ) ( bus_tie_31 VCCD )
       ( FILLER_237 VCCD ) ( FILLER_236 VCCD ) ( FILLER_235 VCCD )
       ( FILLER_234 VCCD ) ( FILLER_233 VCCD ) ( flash_csb_pad VCCD )
       ( FILLER_231 VCCD ) ( FILLER_230 VCCD ) ( FILLER_229 VCCD )
       ( FILLER_228 VCCD ) ( FILLER_227 VCCD ) ( bus_tie_30 VCCHIB )
       ( bus_tie_30 VCCD ) ( bus_tie_29 VCCHIB ) ( bus_tie_29 VCCD )
       ( bus_tie_28 VCCHIB ) ( bus_tie_28 VCCD ) ( bus_tie_27 VCCHIB )
       ( bus_tie_27 VCCD ) ( bus_tie_26 VCCHIB ) ( bus_tie_26 VCCD )
       ( bus_tie_25 VCCHIB ) ( bus_tie_25 VCCD ) ( FILLER_220 VCCD )
       ( FILLER_219 VCCD ) ( FILLER_218 VCCD ) ( FILLER_217 VCCD )
       ( FILLER_216 VCCD ) ( mgmt_vssd_lvclamp_pad VCCD )
       ( FILLER_214 VCCD ) ( FILLER_213 VCCD ) ( FILLER_212 VCCD )
       ( FILLER_211 VCCD ) ( bus_tie_24 VCCHIB ) ( FILLER_210 VCCD )
       ( bus_tie_24 VCCD ) ( bus_tie_23 VCCHIB ) ( bus_tie_23 VCCD )
       ( bus_tie_22 VCCHIB ) ( bus_tie_22 VCCD ) ( bus_tie_21 VCCHIB )
       ( bus_tie_21 VCCD ) ( bus_tie_20 VCCHIB ) ( bus_tie_20 VCCD )
       ( bus_tie_19 VCCHIB ) ( bus_tie_19 VCCD ) ( FILLER_203 VCCD )
       ( FILLER_202 VCCD ) ( FILLER_201 VCCD ) ( FILLER_200 VCCD )
       ( FILLER_199 VCCD ) ( bus_tie_9 VCCD ) ( FILLER_197 VCCD )
       ( FILLER_196 VCCD ) ( FILLER_195 VCCD ) ( FILLER_194 VCCD )
       ( bus_tie_18 VCCHIB ) ( FILLER_193 VCCD ) ( bus_tie_18 VCCD )
       ( bus_tie_17 VCCHIB ) ( bus_tie_17 VCCD ) ( bus_tie_16 VCCHIB )
       ( bus_tie_16 VCCD ) ( bus_tie_15 VCCHIB ) ( bus_tie_15 VCCD )
       ( bus_tie_14 VCCHIB ) ( bus_tie_14 VCCD ) ( bus_tie_13 VCCHIB )
       ( bus_tie_13 VCCD ) ( FILLER_186 VCCD ) ( FILLER_185 VCCD )
       ( FILLER_184 VCCD ) ( FILLER_183 VCCD ) ( FILLER_182 VCCD )
       ( resetb_pad VCCD ) ( FILLER_180 VCCD ) ( FILLER_179 VCCD )
       ( FILLER_178 VCCD ) ( FILLER_177 VCCD ) ( FILLER_176 VCCD )
       ( bus_tie_12 VCCHIB ) ( bus_tie_12 VCCD ) ( bus_tie_11 VCCHIB )
       ( bus_tie_11 VCCD ) ( bus_tie_10 VCCHIB ) ( bus_tie_10 VCCD )
       ( bus_tie_9 VCCHIB ) ( bus_tie_8 VCCD ) ( bus_tie_8 VCCHIB )
       ( bus_tie_7 VCCD ) ( bus_tie_7 VCCHIB ) ( bus_tie_6 VCCD )
       ( FILLER_169 VCCD ) ( FILLER_168 VCCD ) ( FILLER_167 VCCD )
       ( FILLER_166 VCCD ) ( FILLER_165 VCCD )
       ( mgmt_vssa_hvclamp_pad VCCD ) ( FILLER_163 VCCD )
       ( FILLER_162 VCCD ) ( FILLER_161 VCCD ) ( FILLER_160 VCCD )
       ( bus_tie_6 VCCHIB ) ( FILLER_159 VCCD ) ( bus_tie_5 VCCD )
       ( bus_tie_5 VCCHIB ) ( bus_tie_4 VCCD ) ( bus_tie_4 VCCHIB )
       ( bus_tie_3 VCCD ) ( bus_tie_3 VCCHIB ) ( bus_tie_2 VCCD )
       ( bus_tie_2 VCCHIB ) ( bus_tie_1 VCCD ) ( bus_tie_1 VCCHIB )
       ( FILLER_152 VCCD ) ( FILLER_151 VCCD ) ( FILLER_150 VCCD )
       ( FILLER_149 VCCD ) ( FILLER_148 VCCD )
       ( mgmt_corner\[0\] VCCD )
      + ROUTED met4 TAPERRULE met4_width_1270  ( 192665 2278365 ) ( 197815 * ) ;
   - gpio_pad/AMUXBUS_A ( gpio_pad AMUXBUS_A )
       ( FILLER_147 AMUXBUS_A ) ( FILLER_146 AMUXBUS_A )
       ( FILLER_145 AMUXBUS_A ) ( FILLER_144 AMUXBUS_A )
       ( FILLER_143 AMUXBUS_A ) ( FILLER_142 AMUXBUS_A )
       ( FILLER_141 AMUXBUS_A ) ( FILLER_140 AMUXBUS_A )
       ( FILLER_139 AMUXBUS_A ) ( FILLER_138 AMUXBUS_A )
       ( FILLER_137 AMUXBUS_A ) ( FILLER_136 AMUXBUS_A )
       ( FILLER_135 AMUXBUS_A ) ( user1_analog_pad\[0\] AMUXBUS_A )
       ( FILLER_133 AMUXBUS_A ) ( FILLER_132 AMUXBUS_A )
       ( FILLER_131 AMUXBUS_A ) ( FILLER_130 AMUXBUS_A )
       ( FILLER_129 AMUXBUS_A ) ( FILLER_128 AMUXBUS_A )
       ( FILLER_127 AMUXBUS_A ) ( FILLER_126 AMUXBUS_A )
       ( FILLER_125 AMUXBUS_A ) ( FILLER_124 AMUXBUS_A )
       ( FILLER_123 AMUXBUS_A )
       ( user1_vssa_hvclamp_pad\[0\] AMUXBUS_A )
       ( FILLER_121 AMUXBUS_A ) ( FILLER_120 AMUXBUS_A )
       ( FILLER_119 AMUXBUS_A ) ( FILLER_118 AMUXBUS_A )
       ( FILLER_117 AMUXBUS_A ) ( FILLER_116 AMUXBUS_A )
       ( FILLER_115 AMUXBUS_A ) ( FILLER_114 AMUXBUS_A )
       ( FILLER_113 AMUXBUS_A ) ( FILLER_112 AMUXBUS_A )
       ( FILLER_111 AMUXBUS_A ) ( FILLER_110 AMUXBUS_A )
       ( user1_analog_pad\[1\] AMUXBUS_A ) ( FILLER_108 AMUXBUS_A )
       ( FILLER_107 AMUXBUS_A ) ( FILLER_106 AMUXBUS_A )
       ( FILLER_105 AMUXBUS_A ) ( FILLER_104 AMUXBUS_A )
       ( FILLER_103 AMUXBUS_A ) ( FILLER_102 AMUXBUS_A )
       ( FILLER_101 AMUXBUS_A ) ( FILLER_100 AMUXBUS_A )
       ( FILLER_99 AMUXBUS_A ) ( FILLER_98 AMUXBUS_A )
       ( user1_analog_pad\[2\] AMUXBUS_A ) ( FILLER_96 AMUXBUS_A )
       ( FILLER_95 AMUXBUS_A ) ( FILLER_94 AMUXBUS_A )
       ( FILLER_93 AMUXBUS_A ) ( FILLER_92 AMUXBUS_A )
       ( FILLER_91 AMUXBUS_A ) ( FILLER_90 AMUXBUS_A )
       ( FILLER_89 AMUXBUS_A ) ( FILLER_88 AMUXBUS_A )
       ( FILLER_87 AMUXBUS_A ) ( FILLER_86 AMUXBUS_A )
       ( FILLER_85 AMUXBUS_A ) ( FILLER_84 AMUXBUS_A )
       ( FILLER_83 AMUXBUS_A ) ( FILLER_82 AMUXBUS_A )
       ( FILLER_81 AMUXBUS_A ) ( FILLER_80 AMUXBUS_A )
       ( FILLER_79 AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_10um_0 AMUXBUS_A )
       ( FILLER_78 AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_5um_1 AMUXBUS_A )
       ( user1_analog_pad_with_clamp AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_5um_0 AMUXBUS_A )
       ( disconnect_vdda_0 AMUXBUS_A ) ( FILLER_SB3 AMUXBUS_A )
       ( FILLER_73 AMUXBUS_A ) ( FILLER_72 AMUXBUS_A )
       ( FILLER_71 AMUXBUS_A ) ( FILLER_70 AMUXBUS_A )
       ( FILLER_69 AMUXBUS_A ) ( FILLER_68 AMUXBUS_A )
       ( mgmt_vssio_hvclamp_pad\[1\] AMUXBUS_A )
       ( FILLER_66 AMUXBUS_A ) ( FILLER_65 AMUXBUS_A )
       ( FILLER_64 AMUXBUS_A ) ( FILLER_63 AMUXBUS_A )
       ( FILLER_62 AMUXBUS_A ) ( FILLER_61 AMUXBUS_A )
       ( FILLER_60 AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_10um_1 AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_5um_3 AMUXBUS_A )
       ( user2_analog_pad_with_clamp\[0\] AMUXBUS_A )
       ( sky130_ef_io__com_bus_slice_5um_2 AMUXBUS_A )
       ( FILLER_57 AMUXBUS_A ) ( FILLER_56 AMUXBUS_A )
       ( FILLER_55 AMUXBUS_A ) ( FILLER_54 AMUXBUS_A )
       ( FILLER_53 AMUXBUS_A ) ( FILLER_52 AMUXBUS_A )
       ( FILLER_51 AMUXBUS_A ) ( FILLER_50 AMUXBUS_A )
       ( FILLER_49 AMUXBUS_A )
       ( user2_analog_pad_with_clamp\[1\] AMUXBUS_A )
       ( FILLER_47 AMUXBUS_A ) ( FILLER_46 AMUXBUS_A )
       ( FILLER_45 AMUXBUS_A ) ( FILLER_44 AMUXBUS_A )
       ( FILLER_43 AMUXBUS_A ) ( FILLER_42 AMUXBUS_A )
       ( user2_analog_pad\[0\] AMUXBUS_A ) ( FILLER_41 AMUXBUS_A )
       ( FILLER_39 AMUXBUS_A ) ( FILLER_38 AMUXBUS_A )
       ( FILLER_37 AMUXBUS_A ) ( FILLER_36 AMUXBUS_A )
       ( FILLER_35 AMUXBUS_A ) ( FILLER_34 AMUXBUS_A )
       ( FILLER_33 AMUXBUS_A ) ( FILLER_32 AMUXBUS_A )
       ( FILLER_31 AMUXBUS_A ) ( FILLER_30 AMUXBUS_A )
       ( FILLER_29 AMUXBUS_A ) ( user2_analog_pad\[1\] AMUXBUS_A )
       ( FILLER_27 AMUXBUS_A ) ( FILLER_26 AMUXBUS_A )
       ( FILLER_25 AMUXBUS_A ) ( FILLER_24 AMUXBUS_A )
       ( FILLER_23 AMUXBUS_A ) ( FILLER_22 AMUXBUS_A )
       ( FILLER_21 AMUXBUS_A ) ( FILLER_20 AMUXBUS_A )
       ( FILLER_19 AMUXBUS_A ) ( FILLER_18 AMUXBUS_A )
       ( FILLER_17 AMUXBUS_A ) ( user2_analog_pad\[2\] AMUXBUS_A )
       ( FILLER_15 AMUXBUS_A ) ( FILLER_14 AMUXBUS_A )
       ( FILLER_13 AMUXBUS_A ) ( FILLER_12 AMUXBUS_A )
       ( FILLER_11 AMUXBUS_A ) ( FILLER_10 AMUXBUS_A )
       ( FILLER_9 AMUXBUS_A ) ( FILLER_8 AMUXBUS_A )
       ( FILLER_7 AMUXBUS_A ) ( FILLER_6 AMUXBUS_A )
       ( user2_corner AMUXBUS_A ) ( FILLER_5 AMUXBUS_A )
       ( FILLER_579 AMUXBUS_A ) ( FILLER_578 AMUXBUS_A )
       ( user1_corner AMUXBUS_A ) ( FILLER_786 AMUXBUS_A )
       ( FILLER_577 AMUXBUS_A ) ( FILLER_576 AMUXBUS_A )
       ( FILLER_785 AMUXBUS_A ) ( FILLER_575 AMUXBUS_A )
       ( FILLER_784 AMUXBUS_A ) ( FILLER_574 AMUXBUS_A )
       ( FILLER_783 AMUXBUS_A ) ( FILLER_573 AMUXBUS_A )
       ( FILLER_782 AMUXBUS_A ) ( FILLER_572 AMUXBUS_A )
       ( FILLER_781 AMUXBUS_A ) ( FILLER_571 AMUXBUS_A )
       ( FILLER_780 AMUXBUS_A ) ( FILLER_779 AMUXBUS_A )
       ( FILLER_570 AMUXBUS_A ) ( user2_analog_pad\[3\] AMUXBUS_A )
       ( FILLER_776 AMUXBUS_A ) ( FILLER_568 AMUXBUS_A )
       ( user1_analog_pad\[3\] AMUXBUS_A ) ( FILLER_567 AMUXBUS_A )
       ( FILLER_777 AMUXBUS_A ) ( FILLER_775 AMUXBUS_A )
       ( FILLER_566 AMUXBUS_A ) ( FILLER_774 AMUXBUS_A )
       ( FILLER_565 AMUXBUS_A ) ( FILLER_773 AMUXBUS_A )
       ( FILLER_564 AMUXBUS_A ) ( FILLER_772 AMUXBUS_A )
       ( FILLER_563 AMUXBUS_A ) ( FILLER_771 AMUXBUS_A )
       ( FILLER_562 AMUXBUS_A ) ( FILLER_561 AMUXBUS_A )
       ( FILLER_770 AMUXBUS_A ) ( FILLER_769 AMUXBUS_A )
       ( user2_vccd_lvclamp_pad AMUXBUS_A ) ( FILLER_559 AMUXBUS_A )
       ( FILLER_558 AMUXBUS_A ) ( FILLER_557 AMUXBUS_A )
       ( user1_vccd_lvclamp_pad AMUXBUS_A ) ( FILLER_767 AMUXBUS_A )
       ( FILLER_766 AMUXBUS_A ) ( FILLER_556 AMUXBUS_A )
       ( FILLER_765 AMUXBUS_A ) ( FILLER_555 AMUXBUS_A )
       ( FILLER_764 AMUXBUS_A ) ( FILLER_554 AMUXBUS_A )
       ( FILLER_763 AMUXBUS_A ) ( FILLER_553 AMUXBUS_A )
       ( FILLER_762 AMUXBUS_A ) ( FILLER_552 AMUXBUS_A )
       ( FILLER_761 AMUXBUS_A ) ( FILLER_551 AMUXBUS_A )
       ( FILLER_760 AMUXBUS_A )
       ( mgmt_vddio_hvclamp_pad\[1\] AMUXBUS_A )
       ( FILLER_759 AMUXBUS_A ) ( FILLER_549 AMUXBUS_A )
       ( FILLER_548 AMUXBUS_A ) ( FILLER_547 AMUXBUS_A )
       ( FILLER_546 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[13\] AMUXBUS_A )
       ( FILLER_757 AMUXBUS_A ) ( FILLER_545 AMUXBUS_A )
       ( FILLER_756 AMUXBUS_A ) ( FILLER_544 AMUXBUS_A )
       ( FILLER_755 AMUXBUS_A ) ( FILLER_543 AMUXBUS_A )
       ( FILLER_754 AMUXBUS_A ) ( FILLER_542 AMUXBUS_A )
       ( FILLER_753 AMUXBUS_A ) ( FILLER_541 AMUXBUS_A )
       ( FILLER_752 AMUXBUS_A ) ( FILLER_751 AMUXBUS_A )
       ( user2_vssa_hvclamp_pad AMUXBUS_A ) ( FILLER_750 AMUXBUS_A )
       ( FILLER_539 AMUXBUS_A ) ( FILLER_538 AMUXBUS_A )
       ( FILLER_537 AMUXBUS_A ) ( FILLER_536 AMUXBUS_A )
       ( user1_vdda_hvclamp_pad\[0\] AMUXBUS_A )
       ( FILLER_748 AMUXBUS_A ) ( FILLER_747 AMUXBUS_A )
       ( FILLER_535 AMUXBUS_A ) ( FILLER_746 AMUXBUS_A )
       ( FILLER_534 AMUXBUS_A ) ( FILLER_745 AMUXBUS_A )
       ( FILLER_533 AMUXBUS_A ) ( FILLER_744 AMUXBUS_A )
       ( FILLER_532 AMUXBUS_A ) ( FILLER_743 AMUXBUS_A )
       ( FILLER_531 AMUXBUS_A ) ( FILLER_742 AMUXBUS_A )
       ( FILLER_741 AMUXBUS_A ) ( FILLER_740 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[0\] AMUXBUS_A )
       ( FILLER_529 AMUXBUS_A ) ( FILLER_528 AMUXBUS_A )
       ( FILLER_527 AMUXBUS_A ) ( FILLER_526 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[12\] AMUXBUS_A )
       ( FILLER_525 AMUXBUS_A ) ( FILLER_738 AMUXBUS_A )
       ( FILLER_524 AMUXBUS_A ) ( FILLER_737 AMUXBUS_A )
       ( FILLER_523 AMUXBUS_A ) ( FILLER_736 AMUXBUS_A )
       ( FILLER_522 AMUXBUS_A ) ( FILLER_735 AMUXBUS_A )
       ( FILLER_734 AMUXBUS_A ) ( FILLER_521 AMUXBUS_A )
       ( FILLER_733 AMUXBUS_A ) ( FILLER_732 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[1\] AMUXBUS_A )
       ( FILLER_731 AMUXBUS_A ) ( FILLER_519 AMUXBUS_A )
       ( FILLER_518 AMUXBUS_A ) ( FILLER_517 AMUXBUS_A )
       ( FILLER_516 AMUXBUS_A ) ( FILLER_515 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[11\] AMUXBUS_A )
       ( FILLER_729 AMUXBUS_A ) ( FILLER_514 AMUXBUS_A )
       ( FILLER_728 AMUXBUS_A ) ( FILLER_513 AMUXBUS_A )
       ( FILLER_727 AMUXBUS_A ) ( FILLER_512 AMUXBUS_A )
       ( FILLER_726 AMUXBUS_A ) ( FILLER_511 AMUXBUS_A )
       ( FILLER_725 AMUXBUS_A ) ( FILLER_724 AMUXBUS_A )
       ( FILLER_723 AMUXBUS_A ) ( FILLER_722 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[2\] AMUXBUS_A )
       ( FILLER_509 AMUXBUS_A ) ( FILLER_508 AMUXBUS_A )
       ( FILLER_507 AMUXBUS_A ) ( FILLER_506 AMUXBUS_A )
       ( FILLER_505 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[10\] AMUXBUS_A )
       ( FILLER_720 AMUXBUS_A ) ( FILLER_719 AMUXBUS_A )
       ( FILLER_504 AMUXBUS_A ) ( FILLER_718 AMUXBUS_A )
       ( FILLER_503 AMUXBUS_A ) ( FILLER_717 AMUXBUS_A )
       ( FILLER_502 AMUXBUS_A ) ( FILLER_501 AMUXBUS_A )
       ( FILLER_716 AMUXBUS_A ) ( FILLER_715 AMUXBUS_A )
       ( FILLER_714 AMUXBUS_A ) ( FILLER_713 AMUXBUS_A )
       ( FILLER_712 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[3\] AMUXBUS_A )
       ( FILLER_499 AMUXBUS_A ) ( FILLER_498 AMUXBUS_A )
       ( FILLER_497 AMUXBUS_A ) ( FILLER_496 AMUXBUS_A )
       ( FILLER_495 AMUXBUS_A ) ( FILLER_494 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[9\] AMUXBUS_A )
       ( FILLER_710 AMUXBUS_A ) ( FILLER_493 AMUXBUS_A )
       ( FILLER_709 AMUXBUS_A ) ( FILLER_492 AMUXBUS_A )
       ( FILLER_708 AMUXBUS_A ) ( FILLER_491 AMUXBUS_A )
       ( FILLER_707 AMUXBUS_A ) ( FILLER_706 AMUXBUS_A )
       ( FILLER_705 AMUXBUS_A ) ( FILLER_704 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[4\] AMUXBUS_A )
       ( FILLER_489 AMUXBUS_A ) ( FILLER_488 AMUXBUS_A )
       ( FILLER_703 AMUXBUS_A ) ( FILLER_487 AMUXBUS_A )
       ( FILLER_486 AMUXBUS_A ) ( FILLER_485 AMUXBUS_A )
       ( FILLER_484 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[8\] AMUXBUS_A )
       ( FILLER_701 AMUXBUS_A ) ( FILLER_483 AMUXBUS_A )
       ( FILLER_700 AMUXBUS_A ) ( FILLER_482 AMUXBUS_A )
       ( FILLER_699 AMUXBUS_A ) ( FILLER_481 AMUXBUS_A )
       ( FILLER_698 AMUXBUS_A ) ( FILLER_697 AMUXBUS_A )
       ( FILLER_696 AMUXBUS_A ) ( FILLER_695 AMUXBUS_A )
       ( FILLER_694 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[5\] AMUXBUS_A )
       ( FILLER_479 AMUXBUS_A ) ( FILLER_478 AMUXBUS_A )
       ( FILLER_477 AMUXBUS_A ) ( FILLER_693 AMUXBUS_A )
       ( FILLER_476 AMUXBUS_A ) ( FILLER_475 AMUXBUS_A )
       ( FILLER_474 AMUXBUS_A ) ( FILLER_473 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[7\] AMUXBUS_A )
       ( FILLER_691 AMUXBUS_A ) ( FILLER_472 AMUXBUS_A )
       ( FILLER_690 AMUXBUS_A ) ( FILLER_471 AMUXBUS_A )
       ( FILLER_689 AMUXBUS_A ) ( FILLER_688 AMUXBUS_A )
       ( FILLER_687 AMUXBUS_A ) ( FILLER_686 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[6\] AMUXBUS_A )
       ( FILLER_469 AMUXBUS_A ) ( FILLER_468 AMUXBUS_A )
       ( FILLER_685 AMUXBUS_A ) ( FILLER_467 AMUXBUS_A )
       ( FILLER_684 AMUXBUS_A ) ( FILLER_466 AMUXBUS_A )
       ( FILLER_465 AMUXBUS_A ) ( FILLER_464 AMUXBUS_A )
       ( FILLER_463 AMUXBUS_A )
       ( user1_vdda_hvclamp_pad\[1\] AMUXBUS_A )
       ( FILLER_682 AMUXBUS_A ) ( FILLER_462 AMUXBUS_A )
       ( FILLER_681 AMUXBUS_A ) ( FILLER_461 AMUXBUS_A )
       ( FILLER_680 AMUXBUS_A ) ( FILLER_679 AMUXBUS_A )
       ( FILLER_678 AMUXBUS_A ) ( FILLER_677 AMUXBUS_A )
       ( user2_vdda_hvclamp_pad AMUXBUS_A ) ( FILLER_459 AMUXBUS_A )
       ( FILLER_458 AMUXBUS_A ) ( FILLER_457 AMUXBUS_A )
       ( FILLER_676 AMUXBUS_A ) ( FILLER_675 AMUXBUS_A )
       ( FILLER_456 AMUXBUS_A ) ( FILLER_455 AMUXBUS_A )
       ( FILLER_454 AMUXBUS_A ) ( FILLER_453 AMUXBUS_A )
       ( user1_vssd_lvclamp_pad AMUXBUS_A ) ( FILLER_673 AMUXBUS_A )
       ( FILLER_452 AMUXBUS_A ) ( FILLER_672 AMUXBUS_A )
       ( FILLER_671 AMUXBUS_A ) ( FILLER_451 AMUXBUS_A )
       ( FILLER_670 AMUXBUS_A ) ( FILLER_669 AMUXBUS_A )
       ( FILLER_668 AMUXBUS_A ) ( user2_vssd_lvclamp_pad AMUXBUS_A )
       ( FILLER_449 AMUXBUS_A ) ( FILLER_667 AMUXBUS_A )
       ( FILLER_448 AMUXBUS_A ) ( FILLER_447 AMUXBUS_A )
       ( FILLER_666 AMUXBUS_A ) ( FILLER_446 AMUXBUS_A )
       ( FILLER_665 AMUXBUS_A ) ( FILLER_445 AMUXBUS_A )
       ( FILLER_444 AMUXBUS_A ) ( FILLER_443 AMUXBUS_A )
       ( FILLER_442 AMUXBUS_A )
       ( user1_vssa_hvclamp_pad\[1\] AMUXBUS_A )
       ( FILLER_663 AMUXBUS_A ) ( FILLER_441 AMUXBUS_A )
       ( FILLER_662 AMUXBUS_A ) ( FILLER_661 AMUXBUS_A )
       ( FILLER_660 AMUXBUS_A ) ( FILLER_659 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[7\] AMUXBUS_A )
       ( FILLER_439 AMUXBUS_A ) ( FILLER_438 AMUXBUS_A )
       ( FILLER_658 AMUXBUS_A ) ( FILLER_437 AMUXBUS_A )
       ( FILLER_657 AMUXBUS_A ) ( FILLER_436 AMUXBUS_A )
       ( FILLER_656 AMUXBUS_A ) ( FILLER_435 AMUXBUS_A )
       ( FILLER_434 AMUXBUS_A ) ( FILLER_433 AMUXBUS_A )
       ( FILLER_432 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[6\] AMUXBUS_A )
       ( FILLER_654 AMUXBUS_A ) ( FILLER_431 AMUXBUS_A )
       ( FILLER_653 AMUXBUS_A ) ( FILLER_652 AMUXBUS_A )
       ( FILLER_651 AMUXBUS_A ) ( FILLER_650 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[8\] AMUXBUS_A )
       ( FILLER_649 AMUXBUS_A ) ( FILLER_429 AMUXBUS_A )
       ( FILLER_428 AMUXBUS_A ) ( FILLER_427 AMUXBUS_A )
       ( FILLER_648 AMUXBUS_A ) ( FILLER_426 AMUXBUS_A )
       ( FILLER_647 AMUXBUS_A ) ( FILLER_425 AMUXBUS_A )
       ( FILLER_646 AMUXBUS_A ) ( FILLER_424 AMUXBUS_A )
       ( FILLER_423 AMUXBUS_A ) ( FILLER_422 AMUXBUS_A )
       ( FILLER_421 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[5\] AMUXBUS_A )
       ( FILLER_644 AMUXBUS_A ) ( FILLER_643 AMUXBUS_A )
       ( FILLER_642 AMUXBUS_A ) ( FILLER_641 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[9\] AMUXBUS_A )
       ( FILLER_419 AMUXBUS_A ) ( FILLER_418 AMUXBUS_A )
       ( FILLER_640 AMUXBUS_A ) ( FILLER_417 AMUXBUS_A )
       ( FILLER_639 AMUXBUS_A ) ( FILLER_416 AMUXBUS_A )
       ( FILLER_638 AMUXBUS_A ) ( FILLER_415 AMUXBUS_A )
       ( FILLER_637 AMUXBUS_A ) ( FILLER_414 AMUXBUS_A )
       ( FILLER_413 AMUXBUS_A ) ( FILLER_412 AMUXBUS_A )
       ( FILLER_411 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[4\] AMUXBUS_A )
       ( FILLER_635 AMUXBUS_A ) ( FILLER_634 AMUXBUS_A )
       ( FILLER_633 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[10\] AMUXBUS_A )
       ( FILLER_409 AMUXBUS_A ) ( FILLER_632 AMUXBUS_A )
       ( FILLER_408 AMUXBUS_A ) ( FILLER_407 AMUXBUS_A )
       ( FILLER_631 AMUXBUS_A ) ( FILLER_406 AMUXBUS_A )
       ( FILLER_630 AMUXBUS_A ) ( FILLER_405 AMUXBUS_A )
       ( FILLER_629 AMUXBUS_A ) ( FILLER_404 AMUXBUS_A )
       ( FILLER_628 AMUXBUS_A ) ( FILLER_403 AMUXBUS_A )
       ( FILLER_402 AMUXBUS_A ) ( FILLER_401 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[3\] AMUXBUS_A )
       ( FILLER_626 AMUXBUS_A ) ( FILLER_625 AMUXBUS_A )
       ( FILLER_624 AMUXBUS_A ) ( FILLER_623 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[11\] AMUXBUS_A )
       ( FILLER_399 AMUXBUS_A ) ( FILLER_398 AMUXBUS_A )
       ( FILLER_622 AMUXBUS_A ) ( FILLER_397 AMUXBUS_A )
       ( FILLER_621 AMUXBUS_A ) ( FILLER_396 AMUXBUS_A )
       ( FILLER_620 AMUXBUS_A ) ( FILLER_395 AMUXBUS_A )
       ( FILLER_619 AMUXBUS_A ) ( FILLER_394 AMUXBUS_A )
       ( FILLER_618 AMUXBUS_A ) ( FILLER_393 AMUXBUS_A )
       ( FILLER_392 AMUXBUS_A ) ( FILLER_391 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[2\] AMUXBUS_A )
       ( FILLER_616 AMUXBUS_A ) ( FILLER_615 AMUXBUS_A )
       ( FILLER_614 AMUXBUS_A )
       ( mprj_pads.area2_io_pad\[12\] AMUXBUS_A )
       ( FILLER_389 AMUXBUS_A ) ( FILLER_388 AMUXBUS_A )
       ( FILLER_387 AMUXBUS_A ) ( FILLER_613 AMUXBUS_A )
       ( FILLER_386 AMUXBUS_A ) ( FILLER_612 AMUXBUS_A )
       ( FILLER_385 AMUXBUS_A ) ( FILLER_611 AMUXBUS_A )
       ( FILLER_384 AMUXBUS_A ) ( FILLER_610 AMUXBUS_A )
       ( FILLER_383 AMUXBUS_A ) ( FILLER_609 AMUXBUS_A )
       ( FILLER_382 AMUXBUS_A ) ( FILLER_381 AMUXBUS_A )
       ( FILLER_380 AMUXBUS_A ) ( FILLER_379 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[1\] AMUXBUS_A )
       ( FILLER_607 AMUXBUS_A ) ( FILLER_606 AMUXBUS_A )
       ( FILLER_378 AMUXBUS_A ) ( FILLER_605 AMUXBUS_A )
       ( FILLER_377 AMUXBUS_A ) ( FILLER_604 AMUXBUS_A )
       ( FILLER_376 AMUXBUS_A ) ( FILLER_603 AMUXBUS_A )
       ( FILLER_375 AMUXBUS_A ) ( FILLER_602 AMUXBUS_A )
       ( FILLER_374 AMUXBUS_A ) ( disconnect_vdda_2 AMUXBUS_A )
       ( FILLER_SB2 AMUXBUS_A ) ( FILLER_601 AMUXBUS_A )
       ( FILLER_600 AMUXBUS_A )
       ( mgmt_vddio_hvclamp_pad\[0\] AMUXBUS_A )
       ( FILLER_599 AMUXBUS_A ) ( FILLER_370 AMUXBUS_A )
       ( FILLER_369 AMUXBUS_A ) ( FILLER_368 AMUXBUS_A )
       ( FILLER_367 AMUXBUS_A )
       ( mprj_pads.area1_io_pad\[0\] AMUXBUS_A )
       ( FILLER_597 AMUXBUS_A ) ( FILLER_366 AMUXBUS_A )
       ( FILLER_596 AMUXBUS_A ) ( FILLER_365 AMUXBUS_A )
       ( FILLER_595 AMUXBUS_A ) ( FILLER_364 AMUXBUS_A )
       ( FILLER_594 AMUXBUS_A ) ( FILLER_363 AMUXBUS_A )
       ( FILLER_593 AMUXBUS_A ) ( FILLER_362 AMUXBUS_A )
       ( FILLER_592 AMUXBUS_A ) ( FILLER_591 AMUXBUS_A )
       ( FILLER_590 AMUXBUS_A ) ( disconnect_vdda_1 AMUXBUS_A )
       ( FILLER_SB1 AMUXBUS_A ) ( FILLER_587 AMUXBUS_A )
       ( mgmt_vccd_lvclamp_pad AMUXBUS_A ) ( FILLER_360 AMUXBUS_A )
       ( FILLER_359 AMUXBUS_A ) ( FILLER_358 AMUXBUS_A )
       ( FILLER_586 AMUXBUS_A ) ( FILLER_357 AMUXBUS_A )
       ( FILLER_585 AMUXBUS_A ) ( FILLER_356 AMUXBUS_A )
       ( FILLER_584 AMUXBUS_A ) ( FILLER_583 AMUXBUS_A )
       ( FILLER_355 AMUXBUS_A ) ( FILLER_582 AMUXBUS_A )
       ( FILLER_354 AMUXBUS_A ) ( FILLER_581 AMUXBUS_A )
       ( FILLER_353 AMUXBUS_A ) ( mgmt_corner\[1\] AMUXBUS_A )
       ( FILLER_352 AMUXBUS_A ) ( FILLER_580 AMUXBUS_A )
       ( FILLER_351 AMUXBUS_A ) ( FILLER_350 AMUXBUS_A )
       ( FILLER_349 AMUXBUS_A ) ( FILLER_348 AMUXBUS_A )
       ( FILLER_347 AMUXBUS_A ) ( FILLER_346 AMUXBUS_A )
       ( bus_tie_72 AMUXBUS_A ) ( bus_tie_71 AMUXBUS_A )
       ( bus_tie_70 AMUXBUS_A ) ( bus_tie_69 AMUXBUS_A )
       ( bus_tie_68 AMUXBUS_A ) ( bus_tie_67 AMUXBUS_A )
       ( FILLER_339 AMUXBUS_A ) ( FILLER_338 AMUXBUS_A )
       ( FILLER_337 AMUXBUS_A ) ( FILLER_336 AMUXBUS_A )
       ( FILLER_335 AMUXBUS_A ) ( mgmt_vdda_hvclamp_pad AMUXBUS_A )
       ( FILLER_333 AMUXBUS_A ) ( FILLER_332 AMUXBUS_A )
       ( FILLER_331 AMUXBUS_A ) ( FILLER_330 AMUXBUS_A )
       ( bus_tie_66 AMUXBUS_A ) ( FILLER_329 AMUXBUS_A )
       ( bus_tie_65 AMUXBUS_A ) ( bus_tie_64 AMUXBUS_A )
       ( bus_tie_63 AMUXBUS_A ) ( bus_tie_62 AMUXBUS_A )
       ( bus_tie_61 AMUXBUS_A ) ( FILLER_322 AMUXBUS_A )
       ( FILLER_321 AMUXBUS_A ) ( FILLER_320 AMUXBUS_A )
       ( FILLER_319 AMUXBUS_A ) ( FILLER_318 AMUXBUS_A )
       ( mgmt_vssio_hvclamp_pad\[0\] AMUXBUS_A )
       ( FILLER_316 AMUXBUS_A ) ( FILLER_315 AMUXBUS_A )
       ( FILLER_314 AMUXBUS_A ) ( FILLER_313 AMUXBUS_A )
       ( bus_tie_60 AMUXBUS_A ) ( FILLER_312 AMUXBUS_A )
       ( bus_tie_59 AMUXBUS_A ) ( bus_tie_58 AMUXBUS_A )
       ( bus_tie_57 AMUXBUS_A ) ( bus_tie_56 AMUXBUS_A )
       ( bus_tie_55 AMUXBUS_A ) ( FILLER_305 AMUXBUS_A )
       ( FILLER_304 AMUXBUS_A ) ( FILLER_303 AMUXBUS_A )
       ( FILLER_302 AMUXBUS_A ) ( FILLER_301 AMUXBUS_A )
       ( clock_pad AMUXBUS_A ) ( FILLER_299 AMUXBUS_A )
       ( FILLER_298 AMUXBUS_A ) ( FILLER_297 AMUXBUS_A )
       ( FILLER_296 AMUXBUS_A ) ( FILLER_295 AMUXBUS_A )
       ( bus_tie_54 AMUXBUS_A ) ( bus_tie_53 AMUXBUS_A )
       ( bus_tie_52 AMUXBUS_A ) ( bus_tie_51 AMUXBUS_A )
       ( bus_tie_50 AMUXBUS_A ) ( bus_tie_49 AMUXBUS_A )
       ( FILLER_288 AMUXBUS_A ) ( FILLER_287 AMUXBUS_A )
       ( FILLER_286 AMUXBUS_A ) ( FILLER_285 AMUXBUS_A )
       ( FILLER_284 AMUXBUS_A ) ( flash_io1_pad AMUXBUS_A )
       ( FILLER_282 AMUXBUS_A ) ( FILLER_281 AMUXBUS_A )
       ( FILLER_280 AMUXBUS_A ) ( FILLER_279 AMUXBUS_A )
       ( bus_tie_48 AMUXBUS_A ) ( FILLER_278 AMUXBUS_A )
       ( bus_tie_47 AMUXBUS_A ) ( bus_tie_46 AMUXBUS_A )
       ( bus_tie_45 AMUXBUS_A ) ( bus_tie_44 AMUXBUS_A )
       ( bus_tie_43 AMUXBUS_A ) ( FILLER_271 AMUXBUS_A )
       ( FILLER_270 AMUXBUS_A ) ( FILLER_269 AMUXBUS_A )
       ( FILLER_268 AMUXBUS_A ) ( FILLER_267 AMUXBUS_A )
       ( flash_io0_pad AMUXBUS_A ) ( FILLER_265 AMUXBUS_A )
       ( FILLER_264 AMUXBUS_A ) ( FILLER_263 AMUXBUS_A )
       ( FILLER_262 AMUXBUS_A ) ( FILLER_261 AMUXBUS_A )
       ( bus_tie_42 AMUXBUS_A ) ( bus_tie_41 AMUXBUS_A )
       ( bus_tie_40 AMUXBUS_A ) ( bus_tie_39 AMUXBUS_A )
       ( bus_tie_38 AMUXBUS_A ) ( bus_tie_37 AMUXBUS_A )
       ( FILLER_254 AMUXBUS_A ) ( FILLER_253 AMUXBUS_A )
       ( FILLER_252 AMUXBUS_A ) ( FILLER_251 AMUXBUS_A )
       ( FILLER_250 AMUXBUS_A ) ( flash_clk_pad AMUXBUS_A )
       ( FILLER_248 AMUXBUS_A ) ( FILLER_247 AMUXBUS_A )
       ( FILLER_246 AMUXBUS_A ) ( FILLER_245 AMUXBUS_A )
       ( bus_tie_36 AMUXBUS_A ) ( FILLER_244 AMUXBUS_A )
       ( bus_tie_35 AMUXBUS_A ) ( bus_tie_34 AMUXBUS_A )
       ( bus_tie_33 AMUXBUS_A ) ( bus_tie_32 AMUXBUS_A )
       ( bus_tie_31 AMUXBUS_A ) ( FILLER_237 AMUXBUS_A )
       ( FILLER_236 AMUXBUS_A ) ( FILLER_235 AMUXBUS_A )
       ( FILLER_234 AMUXBUS_A ) ( FILLER_233 AMUXBUS_A )
       ( flash_csb_pad AMUXBUS_A ) ( FILLER_231 AMUXBUS_A )
       ( FILLER_230 AMUXBUS_A ) ( FILLER_229 AMUXBUS_A )
       ( FILLER_228 AMUXBUS_A ) ( FILLER_227 AMUXBUS_A )
       ( bus_tie_30 AMUXBUS_A ) ( bus_tie_29 AMUXBUS_A )
       ( bus_tie_28 AMUXBUS_A ) ( bus_tie_27 AMUXBUS_A )
       ( bus_tie_26 AMUXBUS_A ) ( bus_tie_25 AMUXBUS_A )
       ( FILLER_220 AMUXBUS_A ) ( FILLER_219 AMUXBUS_A )
       ( FILLER_218 AMUXBUS_A ) ( FILLER_217 AMUXBUS_A )
       ( FILLER_216 AMUXBUS_A ) ( mgmt_vssd_lvclamp_pad AMUXBUS_A )
       ( FILLER_214 AMUXBUS_A ) ( FILLER_213 AMUXBUS_A )
       ( FILLER_212 AMUXBUS_A ) ( FILLER_211 AMUXBUS_A )
       ( bus_tie_24 AMUXBUS_A ) ( FILLER_210 AMUXBUS_A )
       ( bus_tie_23 AMUXBUS_A ) ( bus_tie_22 AMUXBUS_A )
       ( bus_tie_21 AMUXBUS_A ) ( bus_tie_20 AMUXBUS_A )
       ( bus_tie_19 AMUXBUS_A ) ( FILLER_203 AMUXBUS_A )
       ( FILLER_202 AMUXBUS_A ) ( FILLER_201 AMUXBUS_A )
       ( FILLER_200 AMUXBUS_A ) ( FILLER_199 AMUXBUS_A )
       ( bus_tie_9 AMUXBUS_A ) ( FILLER_197 AMUXBUS_A )
       ( FILLER_196 AMUXBUS_A ) ( FILLER_195 AMUXBUS_A )
       ( FILLER_194 AMUXBUS_A ) ( bus_tie_18 AMUXBUS_A )
       ( FILLER_193 AMUXBUS_A ) ( bus_tie_17 AMUXBUS_A )
       ( bus_tie_16 AMUXBUS_A ) ( bus_tie_15 AMUXBUS_A )
       ( bus_tie_14 AMUXBUS_A ) ( bus_tie_13 AMUXBUS_A )
       ( FILLER_186 AMUXBUS_A ) ( FILLER_185 AMUXBUS_A )
       ( FILLER_184 AMUXBUS_A ) ( FILLER_183 AMUXBUS_A )
       ( FILLER_182 AMUXBUS_A ) ( resetb_pad AMUXBUS_A )
       ( FILLER_180 AMUXBUS_A ) ( FILLER_179 AMUXBUS_A )
       ( FILLER_178 AMUXBUS_A ) ( FILLER_177 AMUXBUS_A )
       ( FILLER_176 AMUXBUS_A ) ( bus_tie_12 AMUXBUS_A )
       ( bus_tie_11 AMUXBUS_A ) ( bus_tie_10 AMUXBUS_A )
       ( bus_tie_8 AMUXBUS_A ) ( bus_tie_7 AMUXBUS_A )
       ( bus_tie_6 AMUXBUS_A ) ( FILLER_169 AMUXBUS_A )
       ( FILLER_168 AMUXBUS_A ) ( FILLER_167 AMUXBUS_A )
       ( FILLER_166 AMUXBUS_A ) ( FILLER_165 AMUXBUS_A )
       ( mgmt_vssa_hvclamp_pad AMUXBUS_A ) ( FILLER_163 AMUXBUS_A )
       ( FILLER_162 AMUXBUS_A ) ( FILLER_161 AMUXBUS_A )
       ( FILLER_160 AMUXBUS_A ) ( bus_tie_5 AMUXBUS_A )
       ( FILLER_159 AMUXBUS_A ) ( bus_tie_4 AMUXBUS_A )
       ( bus_tie_3 AMUXBUS_A ) ( bus_tie_2 AMUXBUS_A )
       ( bus_tie_1 AMUXBUS_A ) ( FILLER_152 AMUXBUS_A )
       ( FILLER_151 AMUXBUS_A ) ( FILLER_150 AMUXBUS_A )
       ( FILLER_149 AMUXBUS_A ) ( FILLER_148 AMUXBUS_A )
       ( mgmt_corner\[0\] AMUXBUS_A ) ;
   - gpio_pad/AMUXBUS_B ( gpio_pad AMUXBUS_B )
       ( FILLER_147 AMUXBUS_B ) ( FILLER_146 AMUXBUS_B )
       ( FILLER_145 AMUXBUS_B ) ( FILLER_144 AMUXBUS_B )
       ( FILLER_143 AMUXBUS_B ) ( FILLER_142 AMUXBUS_B )
       ( FILLER_141 AMUXBUS_B ) ( FILLER_140 AMUXBUS_B )
       ( FILLER_139 AMUXBUS_B ) ( FILLER_138 AMUXBUS_B )
       ( FILLER_137 AMUXBUS_B ) ( FILLER_136 AMUXBUS_B )
       ( FILLER_135 AMUXBUS_B ) ( user1_analog_pad\[0\] AMUXBUS_B )
       ( FILLER_133 AMUXBUS_B ) ( FILLER_132 AMUXBUS_B )
       ( FILLER_131 AMUXBUS_B ) ( FILLER_130 AMUXBUS_B )
       ( FILLER_129 AMUXBUS_B ) ( FILLER_128 AMUXBUS_B )
       ( FILLER_127 AMUXBUS_B ) ( FILLER_126 AMUXBUS_B )
       ( FILLER_125 AMUXBUS_B ) ( FILLER_124 AMUXBUS_B )
       ( FILLER_123 AMUXBUS_B )
       ( user1_vssa_hvclamp_pad\[0\] AMUXBUS_B )
       ( FILLER_121 AMUXBUS_B ) ( FILLER_120 AMUXBUS_B )
       ( FILLER_119 AMUXBUS_B ) ( FILLER_118 AMUXBUS_B )
       ( FILLER_117 AMUXBUS_B ) ( FILLER_116 AMUXBUS_B )
       ( FILLER_115 AMUXBUS_B ) ( FILLER_114 AMUXBUS_B )
       ( FILLER_113 AMUXBUS_B ) ( FILLER_112 AMUXBUS_B )
       ( FILLER_111 AMUXBUS_B ) ( FILLER_110 AMUXBUS_B )
       ( user1_analog_pad\[1\] AMUXBUS_B ) ( FILLER_108 AMUXBUS_B )
       ( FILLER_107 AMUXBUS_B ) ( FILLER_106 AMUXBUS_B )
       ( FILLER_105 AMUXBUS_B ) ( FILLER_104 AMUXBUS_B )
       ( FILLER_103 AMUXBUS_B ) ( FILLER_102 AMUXBUS_B )
       ( FILLER_101 AMUXBUS_B ) ( FILLER_100 AMUXBUS_B )
       ( FILLER_99 AMUXBUS_B ) ( FILLER_98 AMUXBUS_B )
       ( user1_analog_pad\[2\] AMUXBUS_B ) ( FILLER_96 AMUXBUS_B )
       ( FILLER_95 AMUXBUS_B ) ( FILLER_94 AMUXBUS_B )
       ( FILLER_93 AMUXBUS_B ) ( FILLER_92 AMUXBUS_B )
       ( FILLER_91 AMUXBUS_B ) ( FILLER_90 AMUXBUS_B )
       ( FILLER_89 AMUXBUS_B ) ( FILLER_88 AMUXBUS_B )
       ( FILLER_87 AMUXBUS_B ) ( FILLER_86 AMUXBUS_B )
       ( FILLER_85 AMUXBUS_B ) ( FILLER_84 AMUXBUS_B )
       ( FILLER_83 AMUXBUS_B ) ( FILLER_82 AMUXBUS_B )
       ( FILLER_81 AMUXBUS_B ) ( FILLER_80 AMUXBUS_B )
       ( FILLER_79 AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_10um_0 AMUXBUS_B )
       ( FILLER_78 AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_5um_1 AMUXBUS_B )
       ( user1_analog_pad_with_clamp AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_5um_0 AMUXBUS_B )
       ( disconnect_vdda_0 AMUXBUS_B ) ( FILLER_SB3 AMUXBUS_B )
       ( FILLER_73 AMUXBUS_B ) ( FILLER_72 AMUXBUS_B )
       ( FILLER_71 AMUXBUS_B ) ( FILLER_70 AMUXBUS_B )
       ( FILLER_69 AMUXBUS_B ) ( FILLER_68 AMUXBUS_B )
       ( mgmt_vssio_hvclamp_pad\[1\] AMUXBUS_B )
       ( FILLER_66 AMUXBUS_B ) ( FILLER_65 AMUXBUS_B )
       ( FILLER_64 AMUXBUS_B ) ( FILLER_63 AMUXBUS_B )
       ( FILLER_62 AMUXBUS_B ) ( FILLER_61 AMUXBUS_B )
       ( FILLER_60 AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_10um_1 AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_5um_3 AMUXBUS_B )
       ( user2_analog_pad_with_clamp\[0\] AMUXBUS_B )
       ( sky130_ef_io__com_bus_slice_5um_2 AMUXBUS_B )
       ( FILLER_57 AMUXBUS_B ) ( FILLER_56 AMUXBUS_B )
       ( FILLER_55 AMUXBUS_B ) ( FILLER_54 AMUXBUS_B )
       ( FILLER_53 AMUXBUS_B ) ( FILLER_52 AMUXBUS_B )
       ( FILLER_51 AMUXBUS_B ) ( FILLER_50 AMUXBUS_B )
       ( FILLER_49 AMUXBUS_B )
       ( user2_analog_pad_with_clamp\[1\] AMUXBUS_B )
       ( FILLER_47 AMUXBUS_B ) ( FILLER_46 AMUXBUS_B )
       ( FILLER_45 AMUXBUS_B ) ( FILLER_44 AMUXBUS_B )
       ( FILLER_43 AMUXBUS_B ) ( FILLER_42 AMUXBUS_B )
       ( user2_analog_pad\[0\] AMUXBUS_B ) ( FILLER_41 AMUXBUS_B )
       ( FILLER_39 AMUXBUS_B ) ( FILLER_38 AMUXBUS_B )
       ( FILLER_37 AMUXBUS_B ) ( FILLER_36 AMUXBUS_B )
       ( FILLER_35 AMUXBUS_B ) ( FILLER_34 AMUXBUS_B )
       ( FILLER_33 AMUXBUS_B ) ( FILLER_32 AMUXBUS_B )
       ( FILLER_31 AMUXBUS_B ) ( FILLER_30 AMUXBUS_B )
       ( FILLER_29 AMUXBUS_B ) ( user2_analog_pad\[1\] AMUXBUS_B )
       ( FILLER_27 AMUXBUS_B ) ( FILLER_26 AMUXBUS_B )
       ( FILLER_25 AMUXBUS_B ) ( FILLER_24 AMUXBUS_B )
       ( FILLER_23 AMUXBUS_B ) ( FILLER_22 AMUXBUS_B )
       ( FILLER_21 AMUXBUS_B ) ( FILLER_20 AMUXBUS_B )
       ( FILLER_19 AMUXBUS_B ) ( FILLER_18 AMUXBUS_B )
       ( FILLER_17 AMUXBUS_B ) ( user2_analog_pad\[2\] AMUXBUS_B )
       ( FILLER_15 AMUXBUS_B ) ( FILLER_14 AMUXBUS_B )
       ( FILLER_13 AMUXBUS_B ) ( FILLER_12 AMUXBUS_B )
       ( FILLER_11 AMUXBUS_B ) ( FILLER_10 AMUXBUS_B )
       ( FILLER_9 AMUXBUS_B ) ( FILLER_8 AMUXBUS_B )
       ( FILLER_7 AMUXBUS_B ) ( FILLER_6 AMUXBUS_B )
       ( user2_corner AMUXBUS_B ) ( FILLER_5 AMUXBUS_B )
       ( FILLER_579 AMUXBUS_B ) ( FILLER_578 AMUXBUS_B )
       ( user1_corner AMUXBUS_B ) ( FILLER_786 AMUXBUS_B )
       ( FILLER_577 AMUXBUS_B ) ( FILLER_576 AMUXBUS_B )
       ( FILLER_785 AMUXBUS_B ) ( FILLER_575 AMUXBUS_B )
       ( FILLER_784 AMUXBUS_B ) ( FILLER_574 AMUXBUS_B )
       ( FILLER_783 AMUXBUS_B ) ( FILLER_573 AMUXBUS_B )
       ( FILLER_782 AMUXBUS_B ) ( FILLER_572 AMUXBUS_B )
       ( FILLER_781 AMUXBUS_B ) ( FILLER_571 AMUXBUS_B )
       ( FILLER_780 AMUXBUS_B ) ( FILLER_779 AMUXBUS_B )
       ( FILLER_570 AMUXBUS_B ) ( user2_analog_pad\[3\] AMUXBUS_B )
       ( FILLER_776 AMUXBUS_B ) ( FILLER_568 AMUXBUS_B )
       ( user1_analog_pad\[3\] AMUXBUS_B ) ( FILLER_567 AMUXBUS_B )
       ( FILLER_777 AMUXBUS_B ) ( FILLER_775 AMUXBUS_B )
       ( FILLER_566 AMUXBUS_B ) ( FILLER_774 AMUXBUS_B )
       ( FILLER_565 AMUXBUS_B ) ( FILLER_773 AMUXBUS_B )
       ( FILLER_564 AMUXBUS_B ) ( FILLER_772 AMUXBUS_B )
       ( FILLER_563 AMUXBUS_B ) ( FILLER_771 AMUXBUS_B )
       ( FILLER_562 AMUXBUS_B ) ( FILLER_561 AMUXBUS_B )
       ( FILLER_770 AMUXBUS_B ) ( FILLER_769 AMUXBUS_B )
       ( user2_vccd_lvclamp_pad AMUXBUS_B ) ( FILLER_559 AMUXBUS_B )
       ( FILLER_558 AMUXBUS_B ) ( FILLER_557 AMUXBUS_B )
       ( user1_vccd_lvclamp_pad AMUXBUS_B ) ( FILLER_767 AMUXBUS_B )
       ( FILLER_766 AMUXBUS_B ) ( FILLER_556 AMUXBUS_B )
       ( FILLER_765 AMUXBUS_B ) ( FILLER_555 AMUXBUS_B )
       ( FILLER_764 AMUXBUS_B ) ( FILLER_554 AMUXBUS_B )
       ( FILLER_763 AMUXBUS_B ) ( FILLER_553 AMUXBUS_B )
       ( FILLER_762 AMUXBUS_B ) ( FILLER_552 AMUXBUS_B )
       ( FILLER_761 AMUXBUS_B ) ( FILLER_551 AMUXBUS_B )
       ( FILLER_760 AMUXBUS_B )
       ( mgmt_vddio_hvclamp_pad\[1\] AMUXBUS_B )
       ( FILLER_759 AMUXBUS_B ) ( FILLER_549 AMUXBUS_B )
       ( FILLER_548 AMUXBUS_B ) ( FILLER_547 AMUXBUS_B )
       ( FILLER_546 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[13\] AMUXBUS_B )
       ( FILLER_757 AMUXBUS_B ) ( FILLER_545 AMUXBUS_B )
       ( FILLER_756 AMUXBUS_B ) ( FILLER_544 AMUXBUS_B )
       ( FILLER_755 AMUXBUS_B ) ( FILLER_543 AMUXBUS_B )
       ( FILLER_754 AMUXBUS_B ) ( FILLER_542 AMUXBUS_B )
       ( FILLER_753 AMUXBUS_B ) ( FILLER_541 AMUXBUS_B )
       ( FILLER_752 AMUXBUS_B ) ( FILLER_751 AMUXBUS_B )
       ( user2_vssa_hvclamp_pad AMUXBUS_B ) ( FILLER_750 AMUXBUS_B )
       ( FILLER_539 AMUXBUS_B ) ( FILLER_538 AMUXBUS_B )
       ( FILLER_537 AMUXBUS_B ) ( FILLER_536 AMUXBUS_B )
       ( user1_vdda_hvclamp_pad\[0\] AMUXBUS_B )
       ( FILLER_748 AMUXBUS_B ) ( FILLER_747 AMUXBUS_B )
       ( FILLER_535 AMUXBUS_B ) ( FILLER_746 AMUXBUS_B )
       ( FILLER_534 AMUXBUS_B ) ( FILLER_745 AMUXBUS_B )
       ( FILLER_533 AMUXBUS_B ) ( FILLER_744 AMUXBUS_B )
       ( FILLER_532 AMUXBUS_B ) ( FILLER_743 AMUXBUS_B )
       ( FILLER_531 AMUXBUS_B ) ( FILLER_742 AMUXBUS_B )
       ( FILLER_741 AMUXBUS_B ) ( FILLER_740 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[0\] AMUXBUS_B )
       ( FILLER_529 AMUXBUS_B ) ( FILLER_528 AMUXBUS_B )
       ( FILLER_527 AMUXBUS_B ) ( FILLER_526 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[12\] AMUXBUS_B )
       ( FILLER_525 AMUXBUS_B ) ( FILLER_738 AMUXBUS_B )
       ( FILLER_524 AMUXBUS_B ) ( FILLER_737 AMUXBUS_B )
       ( FILLER_523 AMUXBUS_B ) ( FILLER_736 AMUXBUS_B )
       ( FILLER_522 AMUXBUS_B ) ( FILLER_735 AMUXBUS_B )
       ( FILLER_734 AMUXBUS_B ) ( FILLER_521 AMUXBUS_B )
       ( FILLER_733 AMUXBUS_B ) ( FILLER_732 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[1\] AMUXBUS_B )
       ( FILLER_731 AMUXBUS_B ) ( FILLER_519 AMUXBUS_B )
       ( FILLER_518 AMUXBUS_B ) ( FILLER_517 AMUXBUS_B )
       ( FILLER_516 AMUXBUS_B ) ( FILLER_515 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[11\] AMUXBUS_B )
       ( FILLER_729 AMUXBUS_B ) ( FILLER_514 AMUXBUS_B )
       ( FILLER_728 AMUXBUS_B ) ( FILLER_513 AMUXBUS_B )
       ( FILLER_727 AMUXBUS_B ) ( FILLER_512 AMUXBUS_B )
       ( FILLER_726 AMUXBUS_B ) ( FILLER_511 AMUXBUS_B )
       ( FILLER_725 AMUXBUS_B ) ( FILLER_724 AMUXBUS_B )
       ( FILLER_723 AMUXBUS_B ) ( FILLER_722 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[2\] AMUXBUS_B )
       ( FILLER_509 AMUXBUS_B ) ( FILLER_508 AMUXBUS_B )
       ( FILLER_507 AMUXBUS_B ) ( FILLER_506 AMUXBUS_B )
       ( FILLER_505 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[10\] AMUXBUS_B )
       ( FILLER_720 AMUXBUS_B ) ( FILLER_719 AMUXBUS_B )
       ( FILLER_504 AMUXBUS_B ) ( FILLER_718 AMUXBUS_B )
       ( FILLER_503 AMUXBUS_B ) ( FILLER_717 AMUXBUS_B )
       ( FILLER_502 AMUXBUS_B ) ( FILLER_501 AMUXBUS_B )
       ( FILLER_716 AMUXBUS_B ) ( FILLER_715 AMUXBUS_B )
       ( FILLER_714 AMUXBUS_B ) ( FILLER_713 AMUXBUS_B )
       ( FILLER_712 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[3\] AMUXBUS_B )
       ( FILLER_499 AMUXBUS_B ) ( FILLER_498 AMUXBUS_B )
       ( FILLER_497 AMUXBUS_B ) ( FILLER_496 AMUXBUS_B )
       ( FILLER_495 AMUXBUS_B ) ( FILLER_494 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[9\] AMUXBUS_B )
       ( FILLER_710 AMUXBUS_B ) ( FILLER_493 AMUXBUS_B )
       ( FILLER_709 AMUXBUS_B ) ( FILLER_492 AMUXBUS_B )
       ( FILLER_708 AMUXBUS_B ) ( FILLER_491 AMUXBUS_B )
       ( FILLER_707 AMUXBUS_B ) ( FILLER_706 AMUXBUS_B )
       ( FILLER_705 AMUXBUS_B ) ( FILLER_704 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[4\] AMUXBUS_B )
       ( FILLER_489 AMUXBUS_B ) ( FILLER_488 AMUXBUS_B )
       ( FILLER_703 AMUXBUS_B ) ( FILLER_487 AMUXBUS_B )
       ( FILLER_486 AMUXBUS_B ) ( FILLER_485 AMUXBUS_B )
       ( FILLER_484 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[8\] AMUXBUS_B )
       ( FILLER_701 AMUXBUS_B ) ( FILLER_483 AMUXBUS_B )
       ( FILLER_700 AMUXBUS_B ) ( FILLER_482 AMUXBUS_B )
       ( FILLER_699 AMUXBUS_B ) ( FILLER_481 AMUXBUS_B )
       ( FILLER_698 AMUXBUS_B ) ( FILLER_697 AMUXBUS_B )
       ( FILLER_696 AMUXBUS_B ) ( FILLER_695 AMUXBUS_B )
       ( FILLER_694 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[5\] AMUXBUS_B )
       ( FILLER_479 AMUXBUS_B ) ( FILLER_478 AMUXBUS_B )
       ( FILLER_477 AMUXBUS_B ) ( FILLER_693 AMUXBUS_B )
       ( FILLER_476 AMUXBUS_B ) ( FILLER_475 AMUXBUS_B )
       ( FILLER_474 AMUXBUS_B ) ( FILLER_473 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[7\] AMUXBUS_B )
       ( FILLER_691 AMUXBUS_B ) ( FILLER_472 AMUXBUS_B )
       ( FILLER_690 AMUXBUS_B ) ( FILLER_471 AMUXBUS_B )
       ( FILLER_689 AMUXBUS_B ) ( FILLER_688 AMUXBUS_B )
       ( FILLER_687 AMUXBUS_B ) ( FILLER_686 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[6\] AMUXBUS_B )
       ( FILLER_469 AMUXBUS_B ) ( FILLER_468 AMUXBUS_B )
       ( FILLER_685 AMUXBUS_B ) ( FILLER_467 AMUXBUS_B )
       ( FILLER_684 AMUXBUS_B ) ( FILLER_466 AMUXBUS_B )
       ( FILLER_465 AMUXBUS_B ) ( FILLER_464 AMUXBUS_B )
       ( FILLER_463 AMUXBUS_B )
       ( user1_vdda_hvclamp_pad\[1\] AMUXBUS_B )
       ( FILLER_682 AMUXBUS_B ) ( FILLER_462 AMUXBUS_B )
       ( FILLER_681 AMUXBUS_B ) ( FILLER_461 AMUXBUS_B )
       ( FILLER_680 AMUXBUS_B ) ( FILLER_679 AMUXBUS_B )
       ( FILLER_678 AMUXBUS_B ) ( FILLER_677 AMUXBUS_B )
       ( user2_vdda_hvclamp_pad AMUXBUS_B ) ( FILLER_459 AMUXBUS_B )
       ( FILLER_458 AMUXBUS_B ) ( FILLER_457 AMUXBUS_B )
       ( FILLER_676 AMUXBUS_B ) ( FILLER_675 AMUXBUS_B )
       ( FILLER_456 AMUXBUS_B ) ( FILLER_455 AMUXBUS_B )
       ( FILLER_454 AMUXBUS_B ) ( FILLER_453 AMUXBUS_B )
       ( user1_vssd_lvclamp_pad AMUXBUS_B ) ( FILLER_673 AMUXBUS_B )
       ( FILLER_452 AMUXBUS_B ) ( FILLER_672 AMUXBUS_B )
       ( FILLER_671 AMUXBUS_B ) ( FILLER_451 AMUXBUS_B )
       ( FILLER_670 AMUXBUS_B ) ( FILLER_669 AMUXBUS_B )
       ( FILLER_668 AMUXBUS_B ) ( user2_vssd_lvclamp_pad AMUXBUS_B )
       ( FILLER_449 AMUXBUS_B ) ( FILLER_667 AMUXBUS_B )
       ( FILLER_448 AMUXBUS_B ) ( FILLER_447 AMUXBUS_B )
       ( FILLER_666 AMUXBUS_B ) ( FILLER_446 AMUXBUS_B )
       ( FILLER_665 AMUXBUS_B ) ( FILLER_445 AMUXBUS_B )
       ( FILLER_444 AMUXBUS_B ) ( FILLER_443 AMUXBUS_B )
       ( FILLER_442 AMUXBUS_B )
       ( user1_vssa_hvclamp_pad\[1\] AMUXBUS_B )
       ( FILLER_663 AMUXBUS_B ) ( FILLER_441 AMUXBUS_B )
       ( FILLER_662 AMUXBUS_B ) ( FILLER_661 AMUXBUS_B )
       ( FILLER_660 AMUXBUS_B ) ( FILLER_659 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[7\] AMUXBUS_B )
       ( FILLER_439 AMUXBUS_B ) ( FILLER_438 AMUXBUS_B )
       ( FILLER_658 AMUXBUS_B ) ( FILLER_437 AMUXBUS_B )
       ( FILLER_657 AMUXBUS_B ) ( FILLER_436 AMUXBUS_B )
       ( FILLER_656 AMUXBUS_B ) ( FILLER_435 AMUXBUS_B )
       ( FILLER_434 AMUXBUS_B ) ( FILLER_433 AMUXBUS_B )
       ( FILLER_432 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[6\] AMUXBUS_B )
       ( FILLER_654 AMUXBUS_B ) ( FILLER_431 AMUXBUS_B )
       ( FILLER_653 AMUXBUS_B ) ( FILLER_652 AMUXBUS_B )
       ( FILLER_651 AMUXBUS_B ) ( FILLER_650 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[8\] AMUXBUS_B )
       ( FILLER_649 AMUXBUS_B ) ( FILLER_429 AMUXBUS_B )
       ( FILLER_428 AMUXBUS_B ) ( FILLER_427 AMUXBUS_B )
       ( FILLER_648 AMUXBUS_B ) ( FILLER_426 AMUXBUS_B )
       ( FILLER_647 AMUXBUS_B ) ( FILLER_425 AMUXBUS_B )
       ( FILLER_646 AMUXBUS_B ) ( FILLER_424 AMUXBUS_B )
       ( FILLER_423 AMUXBUS_B ) ( FILLER_422 AMUXBUS_B )
       ( FILLER_421 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[5\] AMUXBUS_B )
       ( FILLER_644 AMUXBUS_B ) ( FILLER_643 AMUXBUS_B )
       ( FILLER_642 AMUXBUS_B ) ( FILLER_641 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[9\] AMUXBUS_B )
       ( FILLER_419 AMUXBUS_B ) ( FILLER_418 AMUXBUS_B )
       ( FILLER_640 AMUXBUS_B ) ( FILLER_417 AMUXBUS_B )
       ( FILLER_639 AMUXBUS_B ) ( FILLER_416 AMUXBUS_B )
       ( FILLER_638 AMUXBUS_B ) ( FILLER_415 AMUXBUS_B )
       ( FILLER_637 AMUXBUS_B ) ( FILLER_414 AMUXBUS_B )
       ( FILLER_413 AMUXBUS_B ) ( FILLER_412 AMUXBUS_B )
       ( FILLER_411 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[4\] AMUXBUS_B )
       ( FILLER_635 AMUXBUS_B ) ( FILLER_634 AMUXBUS_B )
       ( FILLER_633 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[10\] AMUXBUS_B )
       ( FILLER_409 AMUXBUS_B ) ( FILLER_632 AMUXBUS_B )
       ( FILLER_408 AMUXBUS_B ) ( FILLER_407 AMUXBUS_B )
       ( FILLER_631 AMUXBUS_B ) ( FILLER_406 AMUXBUS_B )
       ( FILLER_630 AMUXBUS_B ) ( FILLER_405 AMUXBUS_B )
       ( FILLER_629 AMUXBUS_B ) ( FILLER_404 AMUXBUS_B )
       ( FILLER_628 AMUXBUS_B ) ( FILLER_403 AMUXBUS_B )
       ( FILLER_402 AMUXBUS_B ) ( FILLER_401 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[3\] AMUXBUS_B )
       ( FILLER_626 AMUXBUS_B ) ( FILLER_625 AMUXBUS_B )
       ( FILLER_624 AMUXBUS_B ) ( FILLER_623 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[11\] AMUXBUS_B )
       ( FILLER_399 AMUXBUS_B ) ( FILLER_398 AMUXBUS_B )
       ( FILLER_622 AMUXBUS_B ) ( FILLER_397 AMUXBUS_B )
       ( FILLER_621 AMUXBUS_B ) ( FILLER_396 AMUXBUS_B )
       ( FILLER_620 AMUXBUS_B ) ( FILLER_395 AMUXBUS_B )
       ( FILLER_619 AMUXBUS_B ) ( FILLER_394 AMUXBUS_B )
       ( FILLER_618 AMUXBUS_B ) ( FILLER_393 AMUXBUS_B )
       ( FILLER_392 AMUXBUS_B ) ( FILLER_391 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[2\] AMUXBUS_B )
       ( FILLER_616 AMUXBUS_B ) ( FILLER_615 AMUXBUS_B )
       ( FILLER_614 AMUXBUS_B )
       ( mprj_pads.area2_io_pad\[12\] AMUXBUS_B )
       ( FILLER_389 AMUXBUS_B ) ( FILLER_388 AMUXBUS_B )
       ( FILLER_387 AMUXBUS_B ) ( FILLER_613 AMUXBUS_B )
       ( FILLER_386 AMUXBUS_B ) ( FILLER_612 AMUXBUS_B )
       ( FILLER_385 AMUXBUS_B ) ( FILLER_611 AMUXBUS_B )
       ( FILLER_384 AMUXBUS_B ) ( FILLER_610 AMUXBUS_B )
       ( FILLER_383 AMUXBUS_B ) ( FILLER_609 AMUXBUS_B )
       ( FILLER_382 AMUXBUS_B ) ( FILLER_381 AMUXBUS_B )
       ( FILLER_380 AMUXBUS_B ) ( FILLER_379 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[1\] AMUXBUS_B )
       ( FILLER_607 AMUXBUS_B ) ( FILLER_606 AMUXBUS_B )
       ( FILLER_378 AMUXBUS_B ) ( FILLER_605 AMUXBUS_B )
       ( FILLER_377 AMUXBUS_B ) ( FILLER_604 AMUXBUS_B )
       ( FILLER_376 AMUXBUS_B ) ( FILLER_603 AMUXBUS_B )
       ( FILLER_375 AMUXBUS_B ) ( FILLER_602 AMUXBUS_B )
       ( FILLER_374 AMUXBUS_B ) ( disconnect_vdda_2 AMUXBUS_B )
       ( FILLER_SB2 AMUXBUS_B ) ( FILLER_601 AMUXBUS_B )
       ( FILLER_600 AMUXBUS_B )
       ( mgmt_vddio_hvclamp_pad\[0\] AMUXBUS_B )
       ( FILLER_599 AMUXBUS_B ) ( FILLER_370 AMUXBUS_B )
       ( FILLER_369 AMUXBUS_B ) ( FILLER_368 AMUXBUS_B )
       ( FILLER_367 AMUXBUS_B )
       ( mprj_pads.area1_io_pad\[0\] AMUXBUS_B )
       ( FILLER_597 AMUXBUS_B ) ( FILLER_366 AMUXBUS_B )
       ( FILLER_596 AMUXBUS_B ) ( FILLER_365 AMUXBUS_B )
       ( FILLER_595 AMUXBUS_B ) ( FILLER_364 AMUXBUS_B )
       ( FILLER_594 AMUXBUS_B ) ( FILLER_363 AMUXBUS_B )
       ( FILLER_593 AMUXBUS_B ) ( FILLER_362 AMUXBUS_B )
       ( FILLER_592 AMUXBUS_B ) ( FILLER_591 AMUXBUS_B )
       ( FILLER_590 AMUXBUS_B ) ( disconnect_vdda_1 AMUXBUS_B )
       ( FILLER_SB1 AMUXBUS_B ) ( FILLER_587 AMUXBUS_B )
       ( mgmt_vccd_lvclamp_pad AMUXBUS_B ) ( FILLER_360 AMUXBUS_B )
       ( FILLER_359 AMUXBUS_B ) ( FILLER_358 AMUXBUS_B )
       ( FILLER_586 AMUXBUS_B ) ( FILLER_357 AMUXBUS_B )
       ( FILLER_585 AMUXBUS_B ) ( FILLER_356 AMUXBUS_B )
       ( FILLER_584 AMUXBUS_B ) ( FILLER_583 AMUXBUS_B )
       ( FILLER_355 AMUXBUS_B ) ( FILLER_582 AMUXBUS_B )
       ( FILLER_354 AMUXBUS_B ) ( FILLER_581 AMUXBUS_B )
       ( FILLER_353 AMUXBUS_B ) ( mgmt_corner\[1\] AMUXBUS_B )
       ( FILLER_352 AMUXBUS_B ) ( FILLER_580 AMUXBUS_B )
       ( FILLER_351 AMUXBUS_B ) ( FILLER_350 AMUXBUS_B )
       ( FILLER_349 AMUXBUS_B ) ( FILLER_348 AMUXBUS_B )
       ( FILLER_347 AMUXBUS_B ) ( FILLER_346 AMUXBUS_B )
       ( bus_tie_72 AMUXBUS_B ) ( bus_tie_71 AMUXBUS_B )
       ( bus_tie_70 AMUXBUS_B ) ( bus_tie_69 AMUXBUS_B )
       ( bus_tie_68 AMUXBUS_B ) ( bus_tie_67 AMUXBUS_B )
       ( FILLER_339 AMUXBUS_B ) ( FILLER_338 AMUXBUS_B )
       ( FILLER_337 AMUXBUS_B ) ( FILLER_336 AMUXBUS_B )
       ( FILLER_335 AMUXBUS_B ) ( mgmt_vdda_hvclamp_pad AMUXBUS_B )
       ( FILLER_333 AMUXBUS_B ) ( FILLER_332 AMUXBUS_B )
       ( FILLER_331 AMUXBUS_B ) ( FILLER_330 AMUXBUS_B )
       ( bus_tie_66 AMUXBUS_B ) ( FILLER_329 AMUXBUS_B )
       ( bus_tie_65 AMUXBUS_B ) ( bus_tie_64 AMUXBUS_B )
       ( bus_tie_63 AMUXBUS_B ) ( bus_tie_62 AMUXBUS_B )
       ( bus_tie_61 AMUXBUS_B ) ( FILLER_322 AMUXBUS_B )
       ( FILLER_321 AMUXBUS_B ) ( FILLER_320 AMUXBUS_B )
       ( FILLER_319 AMUXBUS_B ) ( FILLER_318 AMUXBUS_B )
       ( mgmt_vssio_hvclamp_pad\[0\] AMUXBUS_B )
       ( FILLER_316 AMUXBUS_B ) ( FILLER_315 AMUXBUS_B )
       ( FILLER_314 AMUXBUS_B ) ( FILLER_313 AMUXBUS_B )
       ( bus_tie_60 AMUXBUS_B ) ( FILLER_312 AMUXBUS_B )
       ( bus_tie_59 AMUXBUS_B ) ( bus_tie_58 AMUXBUS_B )
       ( bus_tie_57 AMUXBUS_B ) ( bus_tie_56 AMUXBUS_B )
       ( bus_tie_55 AMUXBUS_B ) ( FILLER_305 AMUXBUS_B )
       ( FILLER_304 AMUXBUS_B ) ( FILLER_303 AMUXBUS_B )
       ( FILLER_302 AMUXBUS_B ) ( FILLER_301 AMUXBUS_B )
       ( clock_pad AMUXBUS_B ) ( FILLER_299 AMUXBUS_B )
       ( FILLER_298 AMUXBUS_B ) ( FILLER_297 AMUXBUS_B )
       ( FILLER_296 AMUXBUS_B ) ( FILLER_295 AMUXBUS_B )
       ( bus_tie_54 AMUXBUS_B ) ( bus_tie_53 AMUXBUS_B )
       ( bus_tie_52 AMUXBUS_B ) ( bus_tie_51 AMUXBUS_B )
       ( bus_tie_50 AMUXBUS_B ) ( bus_tie_49 AMUXBUS_B )
       ( FILLER_288 AMUXBUS_B ) ( FILLER_287 AMUXBUS_B )
       ( FILLER_286 AMUXBUS_B ) ( FILLER_285 AMUXBUS_B )
       ( FILLER_284 AMUXBUS_B ) ( flash_io1_pad AMUXBUS_B )
       ( FILLER_282 AMUXBUS_B ) ( FILLER_281 AMUXBUS_B )
       ( FILLER_280 AMUXBUS_B ) ( FILLER_279 AMUXBUS_B )
       ( bus_tie_48 AMUXBUS_B ) ( FILLER_278 AMUXBUS_B )
       ( bus_tie_47 AMUXBUS_B ) ( bus_tie_46 AMUXBUS_B )
       ( bus_tie_45 AMUXBUS_B ) ( bus_tie_44 AMUXBUS_B )
       ( bus_tie_43 AMUXBUS_B ) ( FILLER_271 AMUXBUS_B )
       ( FILLER_270 AMUXBUS_B ) ( FILLER_269 AMUXBUS_B )
       ( FILLER_268 AMUXBUS_B ) ( FILLER_267 AMUXBUS_B )
       ( flash_io0_pad AMUXBUS_B ) ( FILLER_265 AMUXBUS_B )
       ( FILLER_264 AMUXBUS_B ) ( FILLER_263 AMUXBUS_B )
       ( FILLER_262 AMUXBUS_B ) ( FILLER_261 AMUXBUS_B )
       ( bus_tie_42 AMUXBUS_B ) ( bus_tie_41 AMUXBUS_B )
       ( bus_tie_40 AMUXBUS_B ) ( bus_tie_39 AMUXBUS_B )
       ( bus_tie_38 AMUXBUS_B ) ( bus_tie_37 AMUXBUS_B )
       ( FILLER_254 AMUXBUS_B ) ( FILLER_253 AMUXBUS_B )
       ( FILLER_252 AMUXBUS_B ) ( FILLER_251 AMUXBUS_B )
       ( FILLER_250 AMUXBUS_B ) ( flash_clk_pad AMUXBUS_B )
       ( FILLER_248 AMUXBUS_B ) ( FILLER_247 AMUXBUS_B )
       ( FILLER_246 AMUXBUS_B ) ( FILLER_245 AMUXBUS_B )
       ( bus_tie_36 AMUXBUS_B ) ( FILLER_244 AMUXBUS_B )
       ( bus_tie_35 AMUXBUS_B ) ( bus_tie_34 AMUXBUS_B )
       ( bus_tie_33 AMUXBUS_B ) ( bus_tie_32 AMUXBUS_B )
       ( bus_tie_31 AMUXBUS_B ) ( FILLER_237 AMUXBUS_B )
       ( FILLER_236 AMUXBUS_B ) ( FILLER_235 AMUXBUS_B )
       ( FILLER_234 AMUXBUS_B ) ( FILLER_233 AMUXBUS_B )
       ( flash_csb_pad AMUXBUS_B ) ( FILLER_231 AMUXBUS_B )
       ( FILLER_230 AMUXBUS_B ) ( FILLER_229 AMUXBUS_B )
       ( FILLER_228 AMUXBUS_B ) ( FILLER_227 AMUXBUS_B )
       ( bus_tie_30 AMUXBUS_B ) ( bus_tie_29 AMUXBUS_B )
       ( bus_tie_28 AMUXBUS_B ) ( bus_tie_27 AMUXBUS_B )
       ( bus_tie_26 AMUXBUS_B ) ( bus_tie_25 AMUXBUS_B )
       ( FILLER_220 AMUXBUS_B ) ( FILLER_219 AMUXBUS_B )
       ( FILLER_218 AMUXBUS_B ) ( FILLER_217 AMUXBUS_B )
       ( FILLER_216 AMUXBUS_B ) ( mgmt_vssd_lvclamp_pad AMUXBUS_B )
       ( FILLER_214 AMUXBUS_B ) ( FILLER_213 AMUXBUS_B )
       ( FILLER_212 AMUXBUS_B ) ( FILLER_211 AMUXBUS_B )
       ( bus_tie_24 AMUXBUS_B ) ( FILLER_210 AMUXBUS_B )
       ( bus_tie_23 AMUXBUS_B ) ( bus_tie_22 AMUXBUS_B )
       ( bus_tie_21 AMUXBUS_B ) ( bus_tie_20 AMUXBUS_B )
       ( bus_tie_19 AMUXBUS_B ) ( FILLER_203 AMUXBUS_B )
       ( FILLER_202 AMUXBUS_B ) ( FILLER_201 AMUXBUS_B )
       ( FILLER_200 AMUXBUS_B ) ( FILLER_199 AMUXBUS_B )
       ( bus_tie_9 AMUXBUS_B ) ( FILLER_197 AMUXBUS_B )
       ( FILLER_196 AMUXBUS_B ) ( FILLER_195 AMUXBUS_B )
       ( FILLER_194 AMUXBUS_B ) ( bus_tie_18 AMUXBUS_B )
       ( FILLER_193 AMUXBUS_B ) ( bus_tie_17 AMUXBUS_B )
       ( bus_tie_16 AMUXBUS_B ) ( bus_tie_15 AMUXBUS_B )
       ( bus_tie_14 AMUXBUS_B ) ( bus_tie_13 AMUXBUS_B )
       ( FILLER_186 AMUXBUS_B ) ( FILLER_185 AMUXBUS_B )
       ( FILLER_184 AMUXBUS_B ) ( FILLER_183 AMUXBUS_B )
       ( FILLER_182 AMUXBUS_B ) ( resetb_pad AMUXBUS_B )
       ( FILLER_180 AMUXBUS_B ) ( FILLER_179 AMUXBUS_B )
       ( FILLER_178 AMUXBUS_B ) ( FILLER_177 AMUXBUS_B )
       ( FILLER_176 AMUXBUS_B ) ( bus_tie_12 AMUXBUS_B )
       ( bus_tie_11 AMUXBUS_B ) ( bus_tie_10 AMUXBUS_B )
       ( bus_tie_8 AMUXBUS_B ) ( bus_tie_7 AMUXBUS_B )
       ( bus_tie_6 AMUXBUS_B ) ( FILLER_169 AMUXBUS_B )
       ( FILLER_168 AMUXBUS_B ) ( FILLER_167 AMUXBUS_B )
       ( FILLER_166 AMUXBUS_B ) ( FILLER_165 AMUXBUS_B )
       ( mgmt_vssa_hvclamp_pad AMUXBUS_B ) ( FILLER_163 AMUXBUS_B )
       ( FILLER_162 AMUXBUS_B ) ( FILLER_161 AMUXBUS_B )
       ( FILLER_160 AMUXBUS_B ) ( bus_tie_5 AMUXBUS_B )
       ( FILLER_159 AMUXBUS_B ) ( bus_tie_4 AMUXBUS_B )
       ( bus_tie_3 AMUXBUS_B ) ( bus_tie_2 AMUXBUS_B )
       ( bus_tie_1 AMUXBUS_B ) ( FILLER_152 AMUXBUS_B )
       ( FILLER_151 AMUXBUS_B ) ( FILLER_150 AMUXBUS_B )
       ( FILLER_149 AMUXBUS_B ) ( FILLER_148 AMUXBUS_B )
       ( mgmt_corner\[0\] AMUXBUS_B ) ;
   - mprj_io[34] ( mprj_pads.area2_io_pad\[9\] PAD ) ;
   - mprj_io_in[23] ( mprj_pads.area2_io_pad\[9\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1631225 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[9\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[9\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[9\] TIE_HI_ESD ) ;
   - mprj_io_one[23] ( mprj_pads.area2_io_pad\[9\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1625245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[23] ( mprj_pads.area2_io_pad\[9\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1622025 ) ( 210895 * ) ;
   - mprj_gpio_analog[16]
       ( mprj_pads.area2_io_pad\[9\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1618805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[9\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[9\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[70] ( mprj_pads.area2_io_pad\[9\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1612825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[16] ( mprj_pads.area2_io_pad\[9\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1609605 ) ( 210895 * ) ;
   - mprj_io_analog_en[23] ( mprj_pads.area2_io_pad\[9\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1606845 ) ( 210895 * ) ;
   - mprj_io_dm[69] ( mprj_pads.area2_io_pad\[9\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1603625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[23] ( mprj_pads.area2_io_pad\[9\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1600405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[23] ( mprj_pads.area2_io_pad\[9\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1597645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[9\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[9\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[9\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[9\] ENABLE_VSWITCH_H ) ;
   - mprj_pads.area2_io_pad\[9\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[9\] ENABLE_H ) ;
   - mprj_io_analog_sel[23] ( mprj_pads.area2_io_pad\[9\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1585225 ) ( 210895 * ) ;
   - mprj_io_dm[71] ( mprj_pads.area2_io_pad\[9\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1582005 ) ( 210895 * ) ;
   - mprj_io_holdover[23] ( mprj_pads.area2_io_pad\[9\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1578785 ) ( 210895 * ) ;
   - mprj_io_out[23] ( mprj_pads.area2_io_pad\[9\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1576025 ) ( 210895 * ) ;
   - mprj_io_vtrip_sel[23] ( mprj_pads.area2_io_pad\[9\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1566825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[23]
       ( mprj_pads.area2_io_pad\[9\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1563605 ) ( 210895 * ) ;
   - mprj_io_oeb[23] ( mprj_pads.area2_io_pad\[9\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1560385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[23] ( mprj_pads.area2_io_pad\[9\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1557625 ) ( 210895 * ) ;
   - flash_io0 ( flash_io0_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 2030000 64215 ) ( 2091000 * ) ;
   - flash_io0_pad/TIE_LO_ESD ( flash_io0_pad TIE_LO_ESD )
       ( flash_io0_pad ENABLE_VSWITCH_H )
       ( flash_io0_pad ENABLE_INP_H )
      + ROUTED met2  ( 2024515 209095 ) via_260_260_hv 
      NEW met2  ( 2024455 209185 ) ( 2024575 * )
      NEW met1 TAPERRULE met1_width_260  ( 2023880 209095 ) ( 2024315 * )
      NEW met2  ( 2024455 209005 ) ( 2024575 * )
      NEW met1 TAPERRULE met1_width_260  ( 2024715 209095 ) ( 2064570 * ) via_260_260_hv 
       ( * 209185 ) ( 2064630 * )
      NEW met2  ( 2064510 209005 ) ( 2064630 * )
      NEW met1 TAPERRULE met1_width_260  ( 2064770 209095 ) ( 2086180 * ) via_260_260_hv 
       ( * 209185 ) ( 2086240 * )
      NEW met2  ( 2086120 209005 ) ( 2086240 * )
      NEW met1 TAPERRULE met1_width_260  ( 2086380 209095 ) ( 2102065 * ) ;
   - flash_io0_di_core ( flash_io0_pad IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2027775 208635 ) ( * 210895 ) ;
   - flash_io0_pad/HLD_H_N ( flash_io0_pad HLD_H_N )
       ( flash_io0_pad TIE_HI_ESD )
      + ROUTED met2  ( 2071000 209515 ) via_260_260_hv 
      NEW met2  ( 2070940 209605 ) ( 2071060 * )
      NEW met1 TAPERRULE met1_width_260  ( 2031180 209515 ) ( 2070800 * )
      NEW met1  ( 2030980 209515 ) via_260_260_hv  ( * 209605 )
       ( 2031040 * )
      NEW met1 TAPERRULE met1_width_260  ( 2023880 209515 ) ( 2030780 * )
      NEW met2  ( 2030920 209425 ) ( 2031040 * )
      NEW met2  ( 2070940 209425 ) ( 2071060 * )
      NEW met1 TAPERRULE met1_width_260  ( 2071200 209515 ) ( 2102065 * ) ;
   - flash_io0_pad/SLOW ( flash_io0_pad SLOW )
       ( constant_block_4 zero ) ( flash_io0_pad IB_MODE_SEL )
       ( flash_io0_pad VTRIP_SEL ) ( flash_io0_pad HLD_OVR )
       ( flash_io0_pad ANALOG_SEL ) ( flash_io0_pad ANALOG_POL )
       ( flash_io0_pad ANALOG_EN )
      + ROUTED met2  ( 2036965 209935 ) via_260_260_hv 
      NEW met2  ( 2036905 210025 ) ( 2037025 * )
      NEW met1 TAPERRULE met1_width_260  ( 2023880 209935 ) ( 2036765 * )
      NEW met2  ( 2036905 209845 ) ( 2037025 * )
      NEW met1 TAPERRULE met1_width_260  ( 2037165 209935 ) ( 2052120 * ) via_260_260_hv 
       ( * 210025 ) ( 2052180 * )
      NEW met2  ( 2052060 209845 ) ( 2052180 * )
      NEW met1 TAPERRULE met1_width_260  ( 2052320 209935 ) ( 2058585 * ) via_260_260_hv 
       ( * 210025 ) ( 2058645 * )
      NEW met2  ( 2058525 209845 ) ( 2058645 * )
      NEW met1 TAPERRULE met1_width_260  ( 2058785 209935 ) ( 2073755 * ) via_260_260_hv 
       ( * 210025 ) ( 2073815 * )
      NEW met2  ( 2073695 209845 ) ( 2073815 * )
      NEW met1 TAPERRULE met1_width_260  ( 2073955 209935 ) ( 2080195 * ) via_260_260_hv 
       ( * 210025 ) ( 2080255 * )
      NEW met2  ( 2080135 209845 ) ( 2080255 * )
      NEW met1 TAPERRULE met1_width_260  ( 2080395 209935 ) ( 2092150 * ) via_260_260_hv 
       ( * 210025 ) ( 2092210 * )
      NEW met2  ( 2092090 209845 ) ( 2092210 * )
      NEW met1 TAPERRULE met1_width_260  ( 2092350 209935 ) ( 2095355 * ) via_260_260_hv 
       ( * 210025 ) ( 2095415 * )
      NEW met2  ( 2095295 209845 ) ( 2095415 * )
      NEW met1 TAPERRULE met1_width_260  ( 2095555 209935 ) ( 2126000 * ) via_260_260_hv 
       ( * 210025 ) ( 2126060 * )
      NEW met2 TAPERRULE met2_width_260  ( 2126000 204765 ) ( * 209735 )
      NEW met2  ( 2125920 204625 ) ( 2126080 * )
      NEW met2  ( 2126000 204500 ) via2_300_300_vx 
      NEW met3  ( 2125975 204525 ) ( 2126025 * )
      NEW met3  ( 2124980 204490 ) ( 2126030 * )
      NEW met3  ( 2124980 204490 ) ( 2125700 * )
      NEW met3  ( 2125975 204475 ) ( 2126025 * )
      NEW met2  ( 2125920 204375 ) ( 2126080 * ) ;
   - flash_io0_pad/PAD_A_ESD_0_H ( flash_io0_pad PAD_A_ESD_0_H ) ;
   - flash_io0_pad/PAD_A_ESD_1_H ( flash_io0_pad PAD_A_ESD_1_H ) ;
   - flash_io0_ieb_core ( flash_io0_pad DM[2] )
       ( flash_io0_pad INP_DIS ) ( flash_io0_pad DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2061355 208635 ) ( * 208810 ) ( * 208950 )
       ( * 210895 ) ( * 211035 ) ( * 211380 )
      NEW met2  ( 2061430 211520 ) ( 2061550 * )
      NEW met2  ( 2061490 211610 ) via_260_260_hv 
      NEW met2  ( 2061430 211700 ) ( 2061550 * )
      NEW met1  ( 2061690 211610 ) ( 2077130 * ) via_260_260_hv 
       ( * 211700 ) ( 2077190 * )
      NEW met2  ( 2077070 211520 ) ( 2077190 * )
      NEW met2  ( 2077130 208950 ) ( * 211380 )
      NEW met1  ( 2046510 211610 ) ( 2061290 * )
      NEW met1  ( 2046310 211610 ) via_260_260_hv  ( * 211700 )
       ( 2046370 * )
      NEW met2  ( 2046250 211520 ) ( 2046370 * )
      NEW met2  ( 2046310 208950 ) ( * 211380 ) ;
   - flash_io0_pad/PAD_A_NOESD_H ( flash_io0_pad PAD_A_NOESD_H ) ;
   - flash_io0_oeb_core ( flash_io0_pad OE_N ) ( flash_io0_pad DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2098615 208635 ) ( * 208810 ) ( * 208950 )
       ( * 210895 ) ( * 211035 ) ( * 212010 )
      NEW met2  ( 2098690 212150 ) ( 2098810 * )
      NEW met2  ( 2098750 212240 ) via_260_260_hv 
      NEW met2  ( 2098690 212330 ) ( 2098810 * )
      NEW met1  ( 2055710 212240 ) ( 2098550 * )
      NEW met1  ( 2055510 212240 ) via_260_260_hv  ( * 212330 )
       ( 2055570 * )
      NEW met2  ( 2055450 212150 ) ( 2055570 * )
      NEW met2  ( 2055510 208950 ) ( * 212010 ) ;
   - flash_io0_do_core ( flash_io0_pad OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2082975 208635 ) ( * 210895 ) ;
   - flash_io0_pad/IN_H ( flash_io0_pad IN_H ) ;
   - mprj_io[15] ( user1_analog_pad\[0\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3142850 5123530 ) ( 3202090 * ) ;
   - mprj_analog[1] ( user1_analog_pad\[0\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 3172220 4988150 ) ( * 5070200 ) ;
   - vdda_pad ( mgmt_vdda_hvclamp_pad VDDA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3121910 64465 ) ( 3181150 * ) ;
   - mprj_io[0] ( mprj_pads.area1_io_pad\[0\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 507000 ) ( * 568000 ) ;
   - mprj_pads.area1_io_pad\[0\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[0\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[0\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[0\] ENABLE_INP_H ) ;
   - mprj_io_in[0] ( mprj_pads.area1_io_pad\[0\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 504775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[0\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[0\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[0\] TIE_HI_ESD ) ;
   - mprj_io_one[0] ( mprj_pads.area1_io_pad\[0\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 510755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[0] ( mprj_pads.area1_io_pad\[0\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 513975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[0\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[0\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[0\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[0\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[1] ( mprj_pads.area1_io_pad\[0\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 523175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[0\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[0\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[0] ( mprj_pads.area1_io_pad\[0\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 529155 ) ( 3379365 * ) ;
   - mprj_io_dm[0] ( mprj_pads.area1_io_pad\[0\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 532375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[0] ( mprj_pads.area1_io_pad\[0\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 535595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[0] ( mprj_pads.area1_io_pad\[0\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 538355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[0\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[0\] ENABLE_H ) ;
   - mprj_io_analog_sel[0] ( mprj_pads.area1_io_pad\[0\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 550775 ) ( 3379365 * ) ;
   - mprj_io_dm[2] ( mprj_pads.area1_io_pad\[0\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 553995 ) ( 3379365 * ) ;
   - mprj_io_holdover[0] ( mprj_pads.area1_io_pad\[0\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 557215 ) ( 3379365 * ) ;
   - mprj_io_out[0] ( mprj_pads.area1_io_pad\[0\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 559975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[0] ( mprj_pads.area1_io_pad\[0\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 569175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[0]
       ( mprj_pads.area1_io_pad\[0\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 572395 ) ( 3379365 * ) ;
   - mprj_io_oeb[0] ( mprj_pads.area1_io_pad\[0\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 575615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[0] ( mprj_pads.area1_io_pad\[0\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 578375 ) ( 3379365 * ) ;
   - mprj_io[17] ( user1_analog_pad\[2\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 2376850 5123530 ) ( 2436090 * ) ;
   - mprj_analog[3] ( user1_analog_pad\[2\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 2406220 4988150 ) ( * 5070200 ) ;
   - mprj_io[25] ( mprj_pads.area2_io_pad\[0\] PAD ) ;
   - mprj_io_in[14] ( mprj_pads.area2_io_pad\[0\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3997225 ) ( 210895 * ) ;
   - mprj_io_one[14] ( mprj_pads.area2_io_pad\[0\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3991245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[14] ( mprj_pads.area2_io_pad\[0\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3988025 ) ( 210895 * ) ;
   - mprj_gpio_analog[7] ( mprj_pads.area2_io_pad\[0\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3984805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[0\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[0\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[43] ( mprj_pads.area2_io_pad\[0\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3978825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[7] ( mprj_pads.area2_io_pad\[0\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3975605 ) ( 210895 * ) ;
   - mprj_io_analog_en[14] ( mprj_pads.area2_io_pad\[0\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3972845 ) ( 210895 * ) ;
   - mprj_io_dm[42] ( mprj_pads.area2_io_pad\[0\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3969625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[14] ( mprj_pads.area2_io_pad\[0\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3966405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[14] ( mprj_pads.area2_io_pad\[0\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3963645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[0\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[0\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[0\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[0\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[0\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[14] ( mprj_pads.area2_io_pad\[0\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3951225 ) ( 210895 * ) ;
   - mprj_io_dm[44] ( mprj_pads.area2_io_pad\[0\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3948005 ) ( 210895 * ) ;
   - mprj_io_holdover[14] ( mprj_pads.area2_io_pad\[0\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3944785 ) ( 210895 * ) ;
   - mprj_io_out[14] ( mprj_pads.area2_io_pad\[0\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3942025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[0\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[0\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[0\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[0\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[14] ( mprj_pads.area2_io_pad\[0\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3932825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[14]
       ( mprj_pads.area2_io_pad\[0\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3929605 ) ( 210895 * ) ;
   - mprj_io_oeb[14] ( mprj_pads.area2_io_pad\[0\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3926385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[14] ( mprj_pads.area2_io_pad\[0\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3923625 ) ( 210895 * ) ;
   - mprj_io[35] ( mprj_pads.area2_io_pad\[10\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 211480 2278940 ) ( * 4585710 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 4609410 ) ( * 4635320 )
      NEW met4 TAPERRULE met4_width_620  ( 205170 4608920 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_650  ( 217685 4586660 ) ( * 4608460 )
      NEW met4 TAPERRULE met4_width_460  ( 205170 4586280 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_490  ( 205265 4586660 ) ( * 4608460 )
      NEW met4  ( 211435 4597560 ) via4_11850_22100 
      NEW met3 TAPERRULE met3_width_650  ( 203620 4608935 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_16550  ( 225635 4586660 ) ( * 4608460 )
      NEW met3 TAPERRULE met3_width_560  ( 203620 4586230 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_2040  ( 204490 4586660 ) ( * 4608460 )
      NEW met3  ( 211435 4597560 ) via3_11850_22100_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 2228670 ) ( * 2254540 )
      NEW met4 TAPERRULE met4_width_480  ( 205140 2278380 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_450  ( 217695 2255490 ) ( * 2277990 )
      NEW met4 TAPERRULE met4_width_600  ( 205140 2255040 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_550  ( 205265 2255490 ) ( * 2277990 )
      NEW met4  ( 211505 2266740 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_560  ( 204850 2278420 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16650  ( 225795 2255490 ) ( * 2277990 )
      NEW met3 TAPERRULE met3_width_585  ( 204850 2255047.5 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_840  ( 205120 2255490 ) ( * 2277990 )
      NEW met3  ( 211505 2266740 ) via3_11930_22800_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 892940 ) ( * 2204270 )
      NEW met4 TAPERRULE met4_width_580  ( 205110 2228160 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_460  ( 217660 2205220 ) ( * 2227720 )
      NEW met4 TAPERRULE met4_width_500  ( 205110 2204820 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_540  ( 205230 2205220 ) ( * 2227720 )
      NEW met4  ( 211465 2216470 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_630  ( 204850 2228185 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16690  ( 225775 2205220 ) ( * 2227720 )
      NEW met3 TAPERRULE met3_width_570  ( 204850 2204785 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_800  ( 205100 2205220 ) ( * 2227720 )
      NEW met3  ( 211465 2216470 ) via3_11930_22800_hx  ;
   - mprj_io_in[24] ( mprj_pads.area2_io_pad\[10\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1415225 ) ( 210895 * ) ;
   - mprj_io_one[24] ( mprj_pads.area2_io_pad\[10\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1409245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[24] ( mprj_pads.area2_io_pad\[10\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1406025 ) ( 210895 * ) ;
   - mprj_gpio_analog[17]
       ( mprj_pads.area2_io_pad\[10\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1402805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[10\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[10\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[73] ( mprj_pads.area2_io_pad\[10\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1396825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[17]
       ( mprj_pads.area2_io_pad\[10\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1393605 ) ( 210895 * ) ;
   - mprj_io_analog_en[24] ( mprj_pads.area2_io_pad\[10\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1390845 ) ( 210895 * ) ;
   - mprj_io_dm[72] ( mprj_pads.area2_io_pad\[10\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1387625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[24]
       ( mprj_pads.area2_io_pad\[10\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1384405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[24] ( mprj_pads.area2_io_pad\[10\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1381645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[10\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[10\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[10\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[10\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[10\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[24]
       ( mprj_pads.area2_io_pad\[10\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1369225 ) ( 210895 * ) ;
   - mprj_io_dm[74] ( mprj_pads.area2_io_pad\[10\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1366005 ) ( 210895 * ) ;
   - mprj_io_holdover[24] ( mprj_pads.area2_io_pad\[10\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1362785 ) ( 210895 * ) ;
   - mprj_io_out[24] ( mprj_pads.area2_io_pad\[10\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1360025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[10\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[10\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[10\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[10\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[24] ( mprj_pads.area2_io_pad\[10\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1350825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[24]
       ( mprj_pads.area2_io_pad\[10\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1347605 ) ( 210895 * ) ;
   - mprj_io_oeb[24] ( mprj_pads.area2_io_pad\[10\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1344385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[24] ( mprj_pads.area2_io_pad\[10\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1341625 ) ( 210895 * ) ;
   - vdda1_pad2 ( user1_vdda_hvclamp_pad\[1\] VDDA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3523530 2526910 ) ( * 2586150 ) ;
   - mprj_io[19] ( user2_analog_pad_with_clamp\[0\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 1422850 5123530 ) ( 1482090 * ) ;
   - mprj_analog[5] ( user2_analog_pad_with_clamp\[0\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_15680  ( 1465540 4995840 ) ( 1536850 * ) ;
   - mprj_clamp_high[1] ( user2_analog_pad_with_clamp\[0\] DRN_HVC )
      + ROUTED met2 TAPERRULE met2_width_23900  ( 1477340 4988070 ) ( * 5013590 ) ;
   - mprj_clamp_low[1]
       ( user2_analog_pad_with_clamp\[0\] SRC_BDY_HVC )
      + ROUTED met2 TAPERRULE met2_width_2050  ( 1415565 4989025 ) ( 1439325 * ) ;
   - mprj_io[2] ( mprj_pads.area1_io_pad\[2\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 958000 ) ( * 1019000 ) ;
   - mprj_pads.area1_io_pad\[2\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[2\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[2\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[2\] ENABLE_INP_H ) ;
   - mprj_io_in[2] ( mprj_pads.area1_io_pad\[2\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 955775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[2\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[2\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[2\] TIE_HI_ESD ) ;
   - mprj_io_one[2] ( mprj_pads.area1_io_pad\[2\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 961755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[2] ( mprj_pads.area1_io_pad\[2\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 964975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[2\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[2\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[2\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[2\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[7] ( mprj_pads.area1_io_pad\[2\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 974175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[2\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[2\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[2] ( mprj_pads.area1_io_pad\[2\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 980155 ) ( 3379365 * ) ;
   - mprj_io_dm[6] ( mprj_pads.area1_io_pad\[2\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 983375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[2] ( mprj_pads.area1_io_pad\[2\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 986595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[2] ( mprj_pads.area1_io_pad\[2\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 989355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[2\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[2\] ENABLE_H ) ;
   - mprj_io_analog_sel[2] ( mprj_pads.area1_io_pad\[2\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1001775 ) ( 3379365 * ) ;
   - mprj_io_dm[8] ( mprj_pads.area1_io_pad\[2\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1004995 ) ( 3379365 * ) ;
   - mprj_io_holdover[2] ( mprj_pads.area1_io_pad\[2\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1008215 ) ( 3379365 * ) ;
   - mprj_io_out[2] ( mprj_pads.area1_io_pad\[2\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1010975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[2] ( mprj_pads.area1_io_pad\[2\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1020175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[2]
       ( mprj_pads.area1_io_pad\[2\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1023395 ) ( 3379365 * ) ;
   - mprj_io_oeb[2] ( mprj_pads.area1_io_pad\[2\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1026615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[2] ( mprj_pads.area1_io_pad\[2\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1029375 ) ( 3379365 * ) ;
   - vssa2_pad ( user2_vssa_hvclamp_pad VSSA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 64465 4145850 ) ( * 4205090 ) ;
   - mprj_io[27] ( mprj_pads.area2_io_pad\[2\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[16] ( mprj_pads.area2_io_pad\[2\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3565225 ) ( 210895 * ) ;
   - mprj_io_one[16] ( mprj_pads.area2_io_pad\[2\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3559245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[16] ( mprj_pads.area2_io_pad\[2\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3556025 ) ( 210895 * ) ;
   - mprj_gpio_analog[9] ( mprj_pads.area2_io_pad\[2\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3552805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[2\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[2\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[49] ( mprj_pads.area2_io_pad\[2\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3546825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[9] ( mprj_pads.area2_io_pad\[2\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3543605 ) ( 210895 * ) ;
   - mprj_io_analog_en[16] ( mprj_pads.area2_io_pad\[2\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3540845 ) ( 210895 * ) ;
   - mprj_io_dm[48] ( mprj_pads.area2_io_pad\[2\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3537625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[16] ( mprj_pads.area2_io_pad\[2\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3534405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[16] ( mprj_pads.area2_io_pad\[2\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3531645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[2\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[2\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[2\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[2\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[2\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[16] ( mprj_pads.area2_io_pad\[2\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3519225 ) ( 210895 * ) ;
   - mprj_io_dm[50] ( mprj_pads.area2_io_pad\[2\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3516005 ) ( 210895 * ) ;
   - mprj_io_holdover[16] ( mprj_pads.area2_io_pad\[2\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3512785 ) ( 210895 * ) ;
   - mprj_io_out[16] ( mprj_pads.area2_io_pad\[2\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3510025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[2\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[2\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[2\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[2\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[16] ( mprj_pads.area2_io_pad\[2\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3500825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[16]
       ( mprj_pads.area2_io_pad\[2\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3497605 ) ( 210895 * ) ;
   - mprj_io_oeb[16] ( mprj_pads.area2_io_pad\[2\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3494385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[16] ( mprj_pads.area2_io_pad\[2\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3491625 ) ( 210895 * ) ;
   - vssio_pad ( mgmt_vssio_hvclamp_pad\[0\] VSSIO_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 2852910 64465 ) ( 2912150 * ) ;
   - mprj_io[37] ( mprj_pads.area2_io_pad\[12\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 211480 2278940 ) ( * 4585710 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 4609410 ) ( * 4635320 )
      NEW met4 TAPERRULE met4_width_620  ( 205170 4608920 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_650  ( 217685 4586660 ) ( * 4608460 )
      NEW met4 TAPERRULE met4_width_460  ( 205170 4586280 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_490  ( 205265 4586660 ) ( * 4608460 )
      NEW met4  ( 211435 4597560 ) via4_11850_22100 
      NEW met3 TAPERRULE met3_width_650  ( 203620 4608935 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_16550  ( 225635 4586660 ) ( * 4608460 )
      NEW met3 TAPERRULE met3_width_560  ( 203620 4586230 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_2040  ( 204490 4586660 ) ( * 4608460 )
      NEW met3  ( 211435 4597560 ) via3_11850_22100_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 2228670 ) ( * 2254540 )
      NEW met4 TAPERRULE met4_width_480  ( 205140 2278380 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_450  ( 217695 2255490 ) ( * 2277990 )
      NEW met4 TAPERRULE met4_width_600  ( 205140 2255040 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_550  ( 205265 2255490 ) ( * 2277990 )
      NEW met4  ( 211505 2266740 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_560  ( 204850 2278420 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16650  ( 225795 2255490 ) ( * 2277990 )
      NEW met3 TAPERRULE met3_width_585  ( 204850 2255047.5 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_840  ( 205120 2255490 ) ( * 2277990 )
      NEW met3  ( 211505 2266740 ) via3_11930_22800_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 892940 ) ( * 2204270 )
      NEW met4 TAPERRULE met4_width_580  ( 205110 2228160 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_460  ( 217660 2205220 ) ( * 2227720 )
      NEW met4 TAPERRULE met4_width_500  ( 205110 2204820 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_540  ( 205230 2205220 ) ( * 2227720 )
      NEW met4  ( 211465 2216470 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_630  ( 204850 2228185 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16690  ( 225775 2205220 ) ( * 2227720 )
      NEW met3 TAPERRULE met3_width_570  ( 204850 2204785 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_800  ( 205100 2205220 ) ( * 2227720 )
      NEW met3  ( 211465 2216470 ) via3_11930_22800_hx  ;
   - mprj_io_in[26] ( mprj_pads.area2_io_pad\[12\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 983225 ) ( 210895 * ) ;
   - mprj_io_one[26] ( mprj_pads.area2_io_pad\[12\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 977245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[26] ( mprj_pads.area2_io_pad\[12\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 974025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[12\]/PAD_A_ESD_0_H
       ( mprj_pads.area2_io_pad\[12\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area2_io_pad\[12\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[12\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[79] ( mprj_pads.area2_io_pad\[12\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 964825 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[12\]/PAD_A_NOESD_H
       ( mprj_pads.area2_io_pad\[12\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[26] ( mprj_pads.area2_io_pad\[12\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 958845 ) ( 210895 * ) ;
   - mprj_io_dm[78] ( mprj_pads.area2_io_pad\[12\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 955625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[26]
       ( mprj_pads.area2_io_pad\[12\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 952405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[26] ( mprj_pads.area2_io_pad\[12\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 949645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[12\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[12\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[12\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[12\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[12\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[26]
       ( mprj_pads.area2_io_pad\[12\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 937225 ) ( 210895 * ) ;
   - mprj_io_dm[80] ( mprj_pads.area2_io_pad\[12\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 934005 ) ( 210895 * ) ;
   - mprj_io_holdover[26] ( mprj_pads.area2_io_pad\[12\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 930785 ) ( 210895 * ) ;
   - mprj_io_out[26] ( mprj_pads.area2_io_pad\[12\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 928025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[12\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[12\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[12\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[12\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[26] ( mprj_pads.area2_io_pad\[12\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 918825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[26]
       ( mprj_pads.area2_io_pad\[12\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 915605 ) ( 210895 * ) ;
   - mprj_io_oeb[26] ( mprj_pads.area2_io_pad\[12\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 912385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[26] ( mprj_pads.area2_io_pad\[12\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 909625 ) ( 210895 * ) ;
   - vssd2_pad ( user2_vssd_lvclamp_pad VSSD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 31635 2241470 ) ( 97295 * ) ;
   - vccd2 ( user2_vccd_lvclamp_pad VCCD1 )
       ( user2_vssd_lvclamp_pad VCCD1 )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 227480 892940 ) ( * 2229720 )
      NEW met5 TAPERRULE met5_width_13000  ( 227480 2253470 ) ( * 4560370 )
      NEW met5 TAPERRULE met5_width_13000  ( 227480 4584730 ) ( * 4610520 )
      NEW met5 TAPERRULE met5_width_2040  ( 221780 4635100 ) ( 233180 * )
      NEW met4 TAPERRULE met4_width_640  ( 221100 4634400 ) ( 233790 * )
      NEW met4 TAPERRULE met4_width_570  ( 233655 4611470 ) ( * 4633930 )
      NEW met4 TAPERRULE met4_width_490  ( 221100 4611075 ) ( 233790 * )
      NEW met4 TAPERRULE met4_width_530  ( 221215 4611470 ) ( * 4633930 )
      NEW met4  ( 227425 4622700 ) via4_11890_22760 
      NEW met3 TAPERRULE met3_width_620  ( 203620 4634390 ) ( 233960 * )
      NEW met3 TAPERRULE met3_width_740  ( 233740 4611470 ) ( * 4633930 )
      NEW met3 TAPERRULE met3_width_565  ( 203620 4611037.5 ) ( 233960 * )
      NEW met3 TAPERRULE met3_width_18010  ( 212475 4611470 ) ( * 4633930 )
      NEW met3  ( 227425 4622700 ) via3_11890_22760_hx 
      NEW met4 TAPERRULE met4_width_550  ( 221140 4584205 ) ( 233830 * )
      NEW met4 TAPERRULE met4_width_520  ( 233720 4561320 ) ( * 4583780 )
      NEW met4 TAPERRULE met4_width_580  ( 221140 4560880 ) ( 233830 * )
      NEW met4 TAPERRULE met4_width_580  ( 221280 4561320 ) ( * 4583780 )
      NEW met4  ( 227515 4572550 ) via4_11890_22760 
      NEW met3 TAPERRULE met3_width_570  ( 205530 4584215 ) ( 233960 * )
      NEW met3 TAPERRULE met3_width_650  ( 233785 4561320 ) ( * 4583780 )
      NEW met3 TAPERRULE met3_width_670  ( 205530 4560835 ) ( 233960 * )
      NEW met3 TAPERRULE met3_width_16190  ( 213475 4561320 ) ( * 4583780 )
      NEW met3  ( 227515 4572550 ) via3_11890_22760_hx 
      NEW met4 TAPERRULE met4_width_560  ( 221100 2252950 ) ( 233830 * )
      NEW met4 TAPERRULE met4_width_700  ( 233630 2230670 ) ( * 2252520 )
      NEW met4 TAPERRULE met4_width_470  ( 221100 2230285 ) ( 233830 * )
      NEW met4 TAPERRULE met4_width_500  ( 221200 2230670 ) ( * 2252520 )
      NEW met4  ( 227365 2241595 ) via4_11830_22150 
      NEW met3 TAPERRULE met3_width_585  ( 204850 2252962.5 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_840  ( 233700 2230670 ) ( * 2252520 )
      NEW met3 TAPERRULE met3_width_520  ( 204850 2230260 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16750  ( 213075 2230670 ) ( * 2252520 )
      NEW met3  ( 227365 2241595 ) via3_11830_22150_hx  ;
   - mprj_io[4] ( mprj_pads.area1_io_pad\[4\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 1409000 ) ( * 1470000 ) ;
   - mprj_pads.area1_io_pad\[4\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[4\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[4\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[4\] ENABLE_INP_H ) ;
   - mprj_io_in[4] ( mprj_pads.area1_io_pad\[4\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1406775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[4\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[4\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[4\] TIE_HI_ESD ) ;
   - mprj_io_one[4] ( mprj_pads.area1_io_pad\[4\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1412755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[4] ( mprj_pads.area1_io_pad\[4\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1415975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[4\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[4\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[4\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[4\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[13] ( mprj_pads.area1_io_pad\[4\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1425175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[4\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[4\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[4] ( mprj_pads.area1_io_pad\[4\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1431155 ) ( 3379365 * ) ;
   - mprj_io_dm[12] ( mprj_pads.area1_io_pad\[4\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1434375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[4] ( mprj_pads.area1_io_pad\[4\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1437595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[4] ( mprj_pads.area1_io_pad\[4\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1440355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[4\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[4\] ENABLE_H ) ;
   - mprj_io_analog_sel[4] ( mprj_pads.area1_io_pad\[4\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1452775 ) ( 3379365 * ) ;
   - mprj_io_dm[14] ( mprj_pads.area1_io_pad\[4\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1455995 ) ( 3379365 * ) ;
   - mprj_io_holdover[4] ( mprj_pads.area1_io_pad\[4\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1459215 ) ( 3379365 * ) ;
   - mprj_io_out[4] ( mprj_pads.area1_io_pad\[4\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1461975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[4] ( mprj_pads.area1_io_pad\[4\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1471175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[4]
       ( mprj_pads.area1_io_pad\[4\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1474395 ) ( 3379365 * ) ;
   - mprj_io_oeb[4] ( mprj_pads.area1_io_pad\[4\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1477615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[4] ( mprj_pads.area1_io_pad\[4\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1480375 ) ( 3379365 * ) ;
   - mprj_io[18] ( user1_analog_pad_with_clamp P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 1931850 5123530 ) ( 1991090 * ) ;
   - mprj_analog[4] ( user1_analog_pad_with_clamp P_CORE )
      + ROUTED met3 TAPERRULE met3_width_15680  ( 1974540 4995840 ) ( 2045850 * ) ;
   - mprj_clamp_high[0] ( user1_analog_pad_with_clamp DRN_HVC )
      + ROUTED met2 TAPERRULE met2_width_23900  ( 1986340 4988070 ) ( * 5013590 ) ;
   - mprj_clamp_low[0] ( user1_analog_pad_with_clamp SRC_BDY_HVC )
      + ROUTED met2 TAPERRULE met2_width_2050  ( 1924565 4989025 ) ( 1948325 * ) ;
   - mprj_io[29] ( mprj_pads.area2_io_pad\[4\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[18] ( mprj_pads.area2_io_pad\[4\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3133225 ) ( 210895 * ) ;
   - mprj_io_one[18] ( mprj_pads.area2_io_pad\[4\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3127245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[18] ( mprj_pads.area2_io_pad\[4\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3124025 ) ( 210895 * ) ;
   - mprj_gpio_analog[11]
       ( mprj_pads.area2_io_pad\[4\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3120805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[4\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[4\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[55] ( mprj_pads.area2_io_pad\[4\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3114825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[11] ( mprj_pads.area2_io_pad\[4\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3111605 ) ( 210895 * ) ;
   - mprj_io_analog_en[18] ( mprj_pads.area2_io_pad\[4\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3108845 ) ( 210895 * ) ;
   - mprj_io_dm[54] ( mprj_pads.area2_io_pad\[4\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3105625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[18] ( mprj_pads.area2_io_pad\[4\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3102405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[18] ( mprj_pads.area2_io_pad\[4\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3099645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[4\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[4\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[4\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[4\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[4\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[18] ( mprj_pads.area2_io_pad\[4\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3087225 ) ( 210895 * ) ;
   - mprj_io_dm[56] ( mprj_pads.area2_io_pad\[4\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3084005 ) ( 210895 * ) ;
   - mprj_io_holdover[18] ( mprj_pads.area2_io_pad\[4\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3080785 ) ( 210895 * ) ;
   - mprj_io_out[18] ( mprj_pads.area2_io_pad\[4\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3078025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[4\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[4\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[4\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[4\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[18] ( mprj_pads.area2_io_pad\[4\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3068825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[18]
       ( mprj_pads.area2_io_pad\[4\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3065605 ) ( 210895 * ) ;
   - mprj_io_oeb[18] ( mprj_pads.area2_io_pad\[4\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3062385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[18] ( mprj_pads.area2_io_pad\[4\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3059625 ) ( 210895 * ) ;
   - vddio_pad2 ( mgmt_vddio_hvclamp_pad\[1\] VDDIO_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 64465 4356850 ) ( * 4416090 ) ;
   - flash_io1 ( flash_io1_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 2304000 64215 ) ( 2365000 * ) ;
   - flash_io1_pad/TIE_LO_ESD ( flash_io1_pad TIE_LO_ESD )
       ( flash_io1_pad ENABLE_VSWITCH_H )
       ( flash_io1_pad ENABLE_INP_H )
      + ROUTED met2  ( 2298520 209095 ) via_260_260_hv 
      NEW met2  ( 2298460 209185 ) ( 2298580 * )
      NEW met1 TAPERRULE met1_width_260  ( 2297880 209095 ) ( 2298320 * )
      NEW met2  ( 2298460 209005 ) ( 2298580 * )
      NEW met1 TAPERRULE met1_width_260  ( 2298720 209095 ) ( 2338550 * ) via_260_260_hv 
       ( * 209185 ) ( 2338610 * )
      NEW met2  ( 2338490 209005 ) ( 2338610 * )
      NEW met1 TAPERRULE met1_width_260  ( 2338750 209095 ) ( 2360180 * ) via_260_260_hv 
       ( * 209185 ) ( 2360240 * )
      NEW met2  ( 2360120 209005 ) ( 2360240 * )
      NEW met1 TAPERRULE met1_width_260  ( 2360380 209095 ) ( 2376065 * ) ;
   - flash_io1_di_core ( flash_io1_pad IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2301775 208635 ) ( * 210895 ) ;
   - flash_io1_pad/HLD_H_N ( flash_io1_pad HLD_H_N )
       ( flash_io1_pad TIE_HI_ESD )
      + ROUTED met2  ( 2344965 209515 ) via_260_260_hv 
      NEW met2  ( 2344905 209605 ) ( 2345025 * )
      NEW met1 TAPERRULE met1_width_260  ( 2305185 209515 ) ( 2344765 * )
      NEW met1  ( 2304985 209515 ) via_260_260_hv  ( * 209605 )
       ( 2305045 * )
      NEW met1 TAPERRULE met1_width_260  ( 2297880 209515 ) ( 2304785 * )
      NEW met2  ( 2304925 209425 ) ( 2305045 * )
      NEW met2  ( 2344905 209425 ) ( 2345025 * )
      NEW met1 TAPERRULE met1_width_260  ( 2345165 209515 ) ( 2376065 * ) ;
   - flash_io1_pad/SLOW ( flash_io1_pad SLOW )
       ( constant_block_5 zero ) ( flash_io1_pad IB_MODE_SEL )
       ( flash_io1_pad VTRIP_SEL ) ( flash_io1_pad HLD_OVR )
       ( flash_io1_pad ANALOG_SEL ) ( flash_io1_pad ANALOG_POL )
       ( flash_io1_pad ANALOG_EN )
      + ROUTED met2  ( 2310940 209935 ) via_260_260_hv 
      NEW met2  ( 2310880 210025 ) ( 2311000 * )
      NEW met1 TAPERRULE met1_width_260  ( 2297880 209935 ) ( 2310740 * )
      NEW met2  ( 2310880 209845 ) ( 2311000 * )
      NEW met1 TAPERRULE met1_width_260  ( 2311140 209935 ) ( 2326135 * ) via_260_260_hv 
       ( * 210025 ) ( 2326195 * )
      NEW met2  ( 2326075 209845 ) ( 2326195 * )
      NEW met1 TAPERRULE met1_width_260  ( 2326335 209935 ) ( 2332570 * ) via_260_260_hv 
       ( * 210025 ) ( 2332630 * )
      NEW met2  ( 2332510 209845 ) ( 2332630 * )
      NEW met1 TAPERRULE met1_width_260  ( 2332770 209935 ) ( 2347740 * ) via_260_260_hv 
       ( * 210025 ) ( 2347800 * )
      NEW met2  ( 2347680 209845 ) ( 2347800 * )
      NEW met1 TAPERRULE met1_width_260  ( 2347940 209935 ) ( 2354180 * ) via_260_260_hv 
       ( * 210025 ) ( 2354240 * )
      NEW met2  ( 2354120 209845 ) ( 2354240 * )
      NEW met1 TAPERRULE met1_width_260  ( 2354380 209935 ) ( 2366135 * ) via_260_260_hv 
       ( * 210025 ) ( 2366195 * )
      NEW met2  ( 2366075 209845 ) ( 2366195 * )
      NEW met1 TAPERRULE met1_width_260  ( 2366335 209935 ) ( 2369375 * ) via_260_260_hv 
       ( * 210025 ) ( 2369435 * )
      NEW met2  ( 2369315 209845 ) ( 2369435 * )
      NEW met1 TAPERRULE met1_width_260  ( 2369575 209935 ) ( 2399910 * ) via_260_260_hv 
       ( * 210025 ) ( 2399970 * )
      NEW met2 TAPERRULE met2_width_260  ( 2399910 204775 ) ( * 209735 )
      NEW met2  ( 2399830 204635 ) ( 2399990 * )
      NEW met2  ( 2399910 204510 ) via2_300_300_vx 
      NEW met3  ( 2398980 204530 ) ( 2399940 * )
      NEW met3  ( 2399885 204535 ) ( 2399935 * )
      NEW met3  ( 2399885 204485 ) ( 2399935 * )
      NEW met3  ( 2398980 204530 ) ( 2399610 * )
      NEW met2  ( 2399830 204385 ) ( 2399990 * ) ;
   - flash_io1_pad/PAD_A_ESD_0_H ( flash_io1_pad PAD_A_ESD_0_H ) ;
   - flash_io1_pad/PAD_A_ESD_1_H ( flash_io1_pad PAD_A_ESD_1_H ) ;
   - flash_io1_pad/PAD_A_NOESD_H ( flash_io1_pad PAD_A_NOESD_H ) ;
   - flash_io1_oeb_core ( flash_io1_pad OE_N ) ( flash_io1_pad DM[0] )
      + ROUTED met2 TAPERRULE met2_width_245  ( 2372545 208687.5 ) ( 2372685 * )
      NEW met2 TAPERRULE met2_width_375  ( 2372567.5 208880 ) ( * 210895 ) ( * 211035 )
       ( * 212060 )
      NEW met2  ( 2372390 212200 ) ( 2372510 * )
      NEW met2  ( 2372450 212290 ) via_260_260_hv 
      NEW met2  ( 2372390 212380 ) ( 2372510 * )
      NEW met1  ( 2329410 212290 ) ( 2372250 * )
      NEW met1  ( 2329210 212290 ) via_260_260_hv  ( * 212380 )
       ( 2329270 * )
      NEW met2  ( 2329150 212200 ) ( 2329270 * )
      NEW met2  ( 2329210 209020 ) ( * 212060 )
      NEW met2  ( 2329210 208880 ) ( 2329305 * ) ;
   - flash_io1_ieb_core ( flash_io1_pad DM[2] )
       ( flash_io1_pad DM[1] ) ( flash_io1_pad INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2335355 208635 ) ( * 210895 ) ( * 211035 )
       ( * 211550 ) via_260_260_hv 
      NEW met2  ( 2335300 211640 ) ( 2335420 * )
      NEW met1  ( 2335560 211550 ) ( 2350995 * ) via_260_260_hv 
       ( * 211640 ) ( 2351055 * )
      NEW met2 TAPERRULE met2_width_260  ( 2350995 210755 ) ( * 211350 )
      NEW met1  ( 2320380 211550 ) ( 2335160 * )
      NEW met1  ( 2320180 211550 ) via_260_260_hv  ( * 211640 )
       ( 2320240 * )
      NEW met2 TAPERRULE met2_width_260  ( 2320180 210750 ) ( * 211350 ) ;
   - flash_io1_do_core ( flash_io1_pad OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2356975 208635 ) ( * 210895 ) ;
   - flash_io1_pad/IN_H ( flash_io1_pad IN_H ) ;
   - mprj_io[10] ( mprj_pads.area1_io_pad\[10\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 3423000 ) ( * 3484000 ) ;
   - mprj_pads.area1_io_pad\[10\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[10\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[10\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[10\] ENABLE_INP_H ) ;
   - mprj_io_in[10] ( mprj_pads.area1_io_pad\[10\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3420775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[10\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[10\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[10\] TIE_HI_ESD ) ;
   - mprj_io_one[10] ( mprj_pads.area1_io_pad\[10\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3426755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[10] ( mprj_pads.area1_io_pad\[10\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3429975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[3]
       ( mprj_pads.area1_io_pad\[10\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3433195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[10\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[10\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[31] ( mprj_pads.area1_io_pad\[10\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3439175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[3] ( mprj_pads.area1_io_pad\[10\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3442395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[10] ( mprj_pads.area1_io_pad\[10\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3445155 ) ( 3379365 * ) ;
   - mprj_io_dm[30] ( mprj_pads.area1_io_pad\[10\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3448375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[10]
       ( mprj_pads.area1_io_pad\[10\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3451595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[10] ( mprj_pads.area1_io_pad\[10\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3454355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[10\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[10\] ENABLE_H ) ;
   - mprj_io_analog_sel[10]
       ( mprj_pads.area1_io_pad\[10\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3466775 ) ( 3379365 * ) ;
   - mprj_io_dm[32] ( mprj_pads.area1_io_pad\[10\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3469995 ) ( 3379365 * ) ;
   - mprj_io_holdover[10] ( mprj_pads.area1_io_pad\[10\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3473215 ) ( 3379365 * ) ;
   - mprj_io_out[10] ( mprj_pads.area1_io_pad\[10\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3475975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[10\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[10\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[10] ( mprj_pads.area1_io_pad\[10\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3485175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[10]
       ( mprj_pads.area1_io_pad\[10\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3488395 ) ( 3379365 * ) ;
   - mprj_io_oeb[10] ( mprj_pads.area1_io_pad\[10\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3491615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[10] ( mprj_pads.area1_io_pad\[10\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3494375 ) ( 3379365 * ) ;
   - mprj_io[6] ( mprj_pads.area1_io_pad\[6\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 1860000 ) ( * 1921000 ) ;
   - mprj_pads.area1_io_pad\[6\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[6\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[6\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[6\] ENABLE_INP_H ) ;
   - mprj_io_in[6] ( mprj_pads.area1_io_pad\[6\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1857775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[6\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[6\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[6\] TIE_HI_ESD ) ;
   - mprj_io_one[6] ( mprj_pads.area1_io_pad\[6\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1863755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[6] ( mprj_pads.area1_io_pad\[6\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1866975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[6\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[6\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[6\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[6\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[19] ( mprj_pads.area1_io_pad\[6\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1876175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[6\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[6\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[6] ( mprj_pads.area1_io_pad\[6\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1882155 ) ( 3379365 * ) ;
   - mprj_io_dm[18] ( mprj_pads.area1_io_pad\[6\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1885375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[6] ( mprj_pads.area1_io_pad\[6\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1888595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[6] ( mprj_pads.area1_io_pad\[6\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1891355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[6\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[6\] ENABLE_H ) ;
   - mprj_io_analog_sel[6] ( mprj_pads.area1_io_pad\[6\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1903775 ) ( 3379365 * ) ;
   - mprj_io_dm[20] ( mprj_pads.area1_io_pad\[6\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1906995 ) ( 3379365 * ) ;
   - mprj_io_holdover[6] ( mprj_pads.area1_io_pad\[6\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1910215 ) ( 3379365 * ) ;
   - mprj_io_out[6] ( mprj_pads.area1_io_pad\[6\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1912975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[6] ( mprj_pads.area1_io_pad\[6\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1922175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[6]
       ( mprj_pads.area1_io_pad\[6\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1925395 ) ( 3379365 * ) ;
   - mprj_io_oeb[6] ( mprj_pads.area1_io_pad\[6\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1928615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[6] ( mprj_pads.area1_io_pad\[6\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1931375 ) ( 3379365 * ) ;
   - mprj_io[22] ( user2_analog_pad\[1\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 650850 5123530 ) ( 710090 * ) ;
   - mprj_analog[8] ( user2_analog_pad\[1\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 680220 4988150 ) ( * 5070200 ) ;
   - flash_csb ( flash_csb_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 1482000 64215 ) ( 1543000 * ) ;
   - flash_csb_pad/TIE_LO_ESD ( flash_csb_pad TIE_LO_ESD )
       ( flash_csb_pad ENABLE_VSWITCH_H )
       ( flash_csb_pad ENABLE_INP_H )
      + ROUTED met2  ( 1476545 209095 ) via_260_260_hv 
      NEW met2  ( 1476485 209185 ) ( 1476605 * )
      NEW met1 TAPERRULE met1_width_260  ( 1475880 209095 ) ( 1476345 * )
      NEW met2  ( 1476485 209005 ) ( 1476605 * )
      NEW met1 TAPERRULE met1_width_260  ( 1476745 209095 ) ( 1516580 * ) via_260_260_hv 
       ( * 209185 ) ( 1516640 * )
      NEW met2  ( 1516520 209005 ) ( 1516640 * )
      NEW met1 TAPERRULE met1_width_260  ( 1516780 209095 ) ( 1538210 * ) via_260_260_hv 
       ( * 209185 ) ( 1538270 * )
      NEW met2  ( 1538150 209005 ) ( 1538270 * )
      NEW met1 TAPERRULE met1_width_260  ( 1538410 209095 ) ( 1554065 * ) ;
   - flash_csb_pad/IN ( flash_csb_pad IN ) ;
   - flash_csb_pad/HLD_H_N ( flash_csb_pad HLD_H_N )
       ( flash_csb_pad TIE_HI_ESD )
      + ROUTED met2  ( 1523015 209515 ) via_260_260_hv 
      NEW met2  ( 1522955 209605 ) ( 1523075 * )
      NEW met1 TAPERRULE met1_width_260  ( 1483210 209515 ) ( 1522815 * )
      NEW met1  ( 1483010 209515 ) via_260_260_hv  ( * 209605 )
       ( 1483070 * )
      NEW met1 TAPERRULE met1_width_260  ( 1475880 209515 ) ( 1482810 * )
      NEW met2  ( 1482950 209425 ) ( 1483070 * )
      NEW met2  ( 1522955 209425 ) ( 1523075 * )
      NEW met1 TAPERRULE met1_width_260  ( 1523215 209515 ) ( 1554065 * ) ;
   - flash_csb_pad/SLOW ( flash_csb_pad SLOW )
       ( constant_block_2 zero ) ( flash_csb_pad IB_MODE_SEL )
       ( flash_csb_pad VTRIP_SEL ) ( flash_csb_pad HLD_OVR )
       ( flash_csb_pad ANALOG_SEL ) ( flash_csb_pad INP_DIS )
       ( flash_csb_pad ANALOG_POL ) ( flash_csb_pad DM[0] )
       ( flash_csb_pad ANALOG_EN )
      + ROUTED met2  ( 1488970 209935 ) via_260_260_hv 
      NEW met2  ( 1488910 210025 ) ( 1489030 * )
      NEW met1 TAPERRULE met1_width_260  ( 1475880 209935 ) ( 1488770 * )
      NEW met2  ( 1488910 209845 ) ( 1489030 * )
      NEW met1 TAPERRULE met1_width_260  ( 1489170 209935 ) ( 1504150 * ) via_260_260_hv 
       ( * 210025 ) ( 1504210 * )
      NEW met2  ( 1504090 209845 ) ( 1504210 * )
      NEW met1 TAPERRULE met1_width_260  ( 1504350 209935 ) ( 1507385 * ) via_260_260_hv 
       ( * 210025 ) ( 1507445 * )
      NEW met2  ( 1507325 209845 ) ( 1507445 * )
      NEW met1 TAPERRULE met1_width_260  ( 1507585 209935 ) ( 1510600 * ) via_260_260_hv 
       ( * 210025 ) ( 1510660 * )
      NEW met2  ( 1510540 209845 ) ( 1510660 * )
      NEW met1 TAPERRULE met1_width_260  ( 1510800 209935 ) ( 1513345 * ) via_260_260_hv 
      NEW met2 TAPERRULE met2_width_280  ( 1513355 210135 ) ( * 210490 )
      NEW met2 TAPERRULE met2_width_205  ( 1513285 209702.5 ) ( 1513425 * )
      NEW met1 TAPERRULE met1_width_260  ( 1513545 209935 ) ( 1525795 * ) via_260_260_hv 
       ( * 210025 ) ( 1525855 * )
      NEW met2  ( 1525735 209845 ) ( 1525855 * )
      NEW met1 TAPERRULE met1_width_260  ( 1525995 209935 ) ( 1532220 * ) via_260_260_hv 
       ( * 210025 ) ( 1532280 * )
      NEW met2  ( 1532160 209845 ) ( 1532280 * )
      NEW met1 TAPERRULE met1_width_260  ( 1532420 209935 ) ( 1544175 * ) via_260_260_hv 
       ( * 210025 ) ( 1544235 * )
      NEW met2  ( 1544115 209845 ) ( 1544235 * )
      NEW met1 TAPERRULE met1_width_260  ( 1544375 209935 ) ( 1547390 * ) via_260_260_hv 
       ( * 210025 ) ( 1547450 * )
      NEW met2  ( 1547330 209845 ) ( 1547450 * )
      NEW met1 TAPERRULE met1_width_260  ( 1547590 209935 ) ( 1577810 * ) via_260_260_hv 
       ( * 210025 ) ( 1577870 * )
      NEW met2 TAPERRULE met2_width_260  ( 1577810 204755 ) ( * 209735 )
      NEW met2  ( 1577730 204615 ) ( 1577890 * )
      NEW met2  ( 1577810 204490 ) via2_300_300_vx 
      NEW met3  ( 1577785 204515 ) ( 1577835 * )
      NEW met3  ( 1577060 204480 ) ( 1577850 * )
      NEW met3  ( 1577060 204480 ) ( 1577510 * )
      NEW met3  ( 1577785 204465 ) ( 1577835 * )
      NEW met2  ( 1577730 204365 ) ( 1577890 * ) ;
   - flash_csb_pad/PAD_A_ESD_0_H ( flash_csb_pad PAD_A_ESD_0_H ) ;
   - flash_csb_pad/PAD_A_ESD_1_H ( flash_csb_pad PAD_A_ESD_1_H ) ;
   - flash_csb_pad/PAD_A_NOESD_H ( flash_csb_pad PAD_A_NOESD_H ) ;
   - flash_csb_core ( flash_csb_pad OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 1534975 208635 ) ( * 210895 ) ;
   - flash_csb_oeb_core ( flash_csb_pad OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 1550615 208635 ) ( * 210895 ) ;
   - flash_csb_pad/IN_H ( flash_csb_pad IN_H ) ;
   - mprj_io[31] ( mprj_pads.area2_io_pad\[6\] PAD ) ;
   - mprj_io_in[20] ( mprj_pads.area2_io_pad\[6\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2701225 ) ( 210895 * ) ;
   - mprj_io_one[20] ( mprj_pads.area2_io_pad\[6\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2695245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[20] ( mprj_pads.area2_io_pad\[6\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2692025 ) ( 210895 * ) ;
   - mprj_gpio_analog[13]
       ( mprj_pads.area2_io_pad\[6\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2688805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[6\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[6\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[61] ( mprj_pads.area2_io_pad\[6\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2682825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[13] ( mprj_pads.area2_io_pad\[6\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2679605 ) ( 210895 * ) ;
   - mprj_io_analog_en[20] ( mprj_pads.area2_io_pad\[6\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2676845 ) ( 210895 * ) ;
   - mprj_io_dm[60] ( mprj_pads.area2_io_pad\[6\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2673625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[20] ( mprj_pads.area2_io_pad\[6\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2670405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[20] ( mprj_pads.area2_io_pad\[6\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2667645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[6\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[6\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[6\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[6\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[6\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[20] ( mprj_pads.area2_io_pad\[6\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2655225 ) ( 210895 * ) ;
   - mprj_io_dm[62] ( mprj_pads.area2_io_pad\[6\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2652005 ) ( 210895 * ) ;
   - mprj_io_holdover[20] ( mprj_pads.area2_io_pad\[6\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2648785 ) ( 210895 * ) ;
   - mprj_io_out[20] ( mprj_pads.area2_io_pad\[6\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2646025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[6\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[6\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[6\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[6\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[20] ( mprj_pads.area2_io_pad\[6\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2636825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[20]
       ( mprj_pads.area2_io_pad\[6\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2633605 ) ( 210895 * ) ;
   - mprj_io_oeb[20] ( mprj_pads.area2_io_pad\[6\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2630385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[20] ( mprj_pads.area2_io_pad\[6\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2627625 ) ( 210895 * ) ;
   - mprj_io[12] ( mprj_pads.area1_io_pad\[12\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 3873000 ) ( * 3934000 ) ;
   - mprj_pads.area1_io_pad\[12\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[12\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[12\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[12\] ENABLE_INP_H ) ;
   - mprj_io_in[12] ( mprj_pads.area1_io_pad\[12\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3870775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[12\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[12\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[12\] TIE_HI_ESD ) ;
   - mprj_io_one[12] ( mprj_pads.area1_io_pad\[12\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3876755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[12] ( mprj_pads.area1_io_pad\[12\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3879975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[5]
       ( mprj_pads.area1_io_pad\[12\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3883195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[12\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[12\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[37] ( mprj_pads.area1_io_pad\[12\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3889175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[5] ( mprj_pads.area1_io_pad\[12\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3892395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[12] ( mprj_pads.area1_io_pad\[12\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3895155 ) ( 3379365 * ) ;
   - mprj_io_dm[36] ( mprj_pads.area1_io_pad\[12\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3898375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[12]
       ( mprj_pads.area1_io_pad\[12\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3901595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[12] ( mprj_pads.area1_io_pad\[12\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3904355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[12\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[12\] ENABLE_H ) ;
   - mprj_io_analog_sel[12]
       ( mprj_pads.area1_io_pad\[12\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3916775 ) ( 3379365 * ) ;
   - mprj_io_dm[38] ( mprj_pads.area1_io_pad\[12\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3919995 ) ( 3379365 * ) ;
   - mprj_io_holdover[12] ( mprj_pads.area1_io_pad\[12\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3923215 ) ( 3379365 * ) ;
   - mprj_io_out[12] ( mprj_pads.area1_io_pad\[12\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3925975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[12\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[12\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[12] ( mprj_pads.area1_io_pad\[12\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3935175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[12]
       ( mprj_pads.area1_io_pad\[12\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3938395 ) ( 3379365 * ) ;
   - mprj_io_oeb[12] ( mprj_pads.area1_io_pad\[12\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3941615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[12] ( mprj_pads.area1_io_pad\[12\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3944375 ) ( 3379365 * ) ;
   - resetb ( resetb_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_37180  ( 702155 36515 ) ( * 90745 ) ;
   - xresloop ( resetb_pad PAD_A_ESD_H ) ( resetb_pad TIE_WEAK_HI_H )
      + ROUTED met3  ( 665620 199850 ) ( * 200420 )
      NEW met3 ( 665620 200720 ) ( 719900 * )
      NEW met3  ( 719900 199850 ) ( * 200420 ) ;
   - resetb_core_h ( resetb_pad XRES_H_N )
      + ROUTED met2 TAPERRULE met2_width_330  ( 708405 199835 ) ( 708995 * ) ;
   - constant_block_0/one ( constant_block_0 one )
       ( resetb_pad ENABLE_VDDIO )
      + ROUTED met3  ( 729275 204500 ) ( 741110 * )
      NEW met3  ( 729275 204515 ) ( 729305 * )
      NEW met3  ( 729580 204500 ) ( 741110 * )
      NEW met3  ( 729275 204500 ) ( 741110 * )
      NEW met2  ( 729210 204580 ) ( 729370 * )
      NEW met2  ( 729220 204615 ) ( 729370 * )
      NEW met2  ( 729210 204365 ) ( 729370 * )
      NEW met2  ( 729290 204500 ) via2_280_280_vx 
      NEW met2 TAPERRULE met2_width_180  ( 729350 200520 ) ( * 204225 )
      NEW met2  ( 729335 200300 ) via2_300_300_hx 
      NEW met3  ( 729310 200370 ) ( 729360 * )
      NEW met3  ( 729635 200300 ) ( 729360 * )
      NEW met3 TAPERRULE met3_width_350  ( 729335 199840 ) ( * 200000 )
      NEW met3 ( 729310 200300 ) ( 729035 * )
      NEW met3  ( 729275 204485 ) ( 729305 * ) ;
   - xres_vss_loop ( resetb_pad PULLUP_H ) ( resetb_pad FILT_IN_H )
       ( resetb_pad EN_VDDIO_SIG_H ) ( resetb_pad TIE_LO_ESD )
       ( resetb_pad DISABLE_PULLUP_H )
      + ROUTED met2  ( 705110 200275 ) via_260_260_hv 
      NEW met2  ( 705050 200365 ) ( 705170 * )
      NEW met2 TAPERRULE met2_width_260  ( 705110 199800 ) ( * 200075 )
      NEW met1 TAPERRULE met1_width_190  ( 705310 200275 ) ( 710090 * ) via_260_260_hv 
       ( * 200365 ) ( 710150 * )
      NEW met2 TAPERRULE met2_width_320  ( 710090 199840 ) ( * 200075 )
      NEW met1 TAPERRULE met1_width_190  ( 710290 200275 ) ( 715470 * ) via_260_260_hv 
       ( * 200365 ) ( 715530 * )
      NEW met2 TAPERRULE met2_width_260  ( 715470 199830 ) ( * 200075 )
      NEW met1 TAPERRULE met1_width_190  ( 715670 200275 ) ( 717315 * ) via_560_260_hv 
       ( * 200365 ) ( 717525 * )
      NEW met3  ( 717160 200105 ) ( 717470 * )
      NEW met3  ( 717185 200115 ) ( 717445 * )
      NEW met3  ( 717160 199890 ) ( 717470 * )
      NEW met3  ( 717315 200090 ) via2_560_280_hx 
      NEW met1 TAPERRULE met1_width_190  ( 717665 200275 ) ( 723145 * ) via_260_260_hv 
       ( * 200365 ) ( 723205 * )
      NEW met2 TAPERRULE met2_width_260  ( 723145 199800 ) ( * 200075 ) ;
   - resetb_pad/TIE_HI_ESD ( resetb_pad TIE_HI_ESD ) ;
   - porb_h ( mprj_pads.area2_io_pad\[0\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[1\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[2\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[3\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[4\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[5\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[6\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[7\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[6\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[8\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[5\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[9\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[4\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[10\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[3\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[11\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[2\] ENABLE_VDDA_H )
       ( mprj_pads.area2_io_pad\[12\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[1\] ENABLE_VDDA_H )
       ( mprj_pads.area1_io_pad\[0\] ENABLE_VDDA_H )
       ( gpio_pad ENABLE_VDDA_H ) ( gpio_pad ENABLE_H )
       ( flash_io1_pad ENABLE_VDDA_H ) ( flash_io1_pad ENABLE_H )
       ( flash_io0_pad ENABLE_VDDA_H ) ( flash_io0_pad ENABLE_H )
       ( flash_clk_pad ENABLE_VDDA_H ) ( flash_clk_pad ENABLE_H )
       ( flash_csb_pad ENABLE_H ) ( clock_pad ENABLE_VDDA_H )
       ( clock_pad ENABLE_H ) ( flash_csb_pad ENABLE_VDDA_H )
       ( resetb_pad ENABLE_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 1541415 208800 ) ( * 210075 )
      NEW met2 TAPERRULE met2_width_280  ( 1540395 210285 ) ( 1541485 * )
      NEW met2 TAPERRULE met2_width_220  ( 1540395 210535 ) ( 1540535 * )
      NEW met2  ( 1540395 210950 ) ( 1540535 * )
      NEW met1 TAPERRULE met1_width_260  ( 1519975 210775 ) ( 1540460 * ) via_260_260_hv 
      NEW met1 TAPERRULE met1_width_260  ( 1540660 210775 ) ( 1793790 * ) via_260_260_hv 
       ( * 210910 ) ( 1793865 * )
      NEW met2 TAPERRULE met2_width_180  ( 1793725 210555 ) ( 1793865 * )
      NEW met1 TAPERRULE met1_width_260  ( 1793990 210775 ) ( 1815395 * ) via_260_260_hv 
       ( * 210865 ) ( 1815485 * )
      NEW met2  ( 1815345 210910 ) ( 1815485 * )
      NEW met2  ( 1815335 210685 ) ( 1815485 * )
      NEW met2 TAPERRULE met2_width_150  ( 1815345 210540 ) ( 1815485 * )
      NEW met1 TAPERRULE met1_width_260  ( 1815595 210775 ) ( 2067750 * ) via_260_260_hv 
       ( * 210865 ) ( 2067865 * )
      NEW met2  ( 2067725 210910 ) ( 2067865 * )
      NEW met2  ( 2067690 210685 ) ( 2067865 * )
      NEW met2 TAPERRULE met2_width_160  ( 2067725 210535 ) ( 2067865 * )
      NEW met1 TAPERRULE met1_width_260  ( 2067950 210775 ) ( 2089420 * ) via_260_260_hv 
      NEW met2  ( 2089345 210890 ) ( 2089485 * )
      NEW met2 TAPERRULE met2_width_180  ( 2089345 210555 ) ( 2089485 * )
      NEW met1 TAPERRULE met1_width_260  ( 2089620 210775 ) ( 2341780 * ) via_260_260_hv 
       ( * 210865 ) ( 2341865 * )
      NEW met2  ( 2341725 210935 ) ( 2341865 * )
      NEW met2  ( 2341720 210685 ) ( 2341865 * )
      NEW met2 TAPERRULE met2_width_160  ( 2341725 210535 ) ( 2341865 * )
      NEW met1 TAPERRULE met1_width_260  ( 2341980 210775 ) ( 2363410 * ) via_260_260_hv 
       ( * 210885 ) ( 2363485 * )
      NEW met2 TAPERRULE met2_width_205  ( 2363345 210542.5 ) ( 2363485 * )
      NEW met1 TAPERRULE met1_width_260  ( 2363610 210775 ) ( 2615760 * ) via_260_260_hv 
       ( * 210865 ) ( 2615865 * )
      NEW met2  ( 2615725 210965 ) ( 2615865 * )
      NEW met2  ( 2615700 210685 ) ( 2615865 * )
      NEW met2 TAPERRULE met2_width_195  ( 2615725 210517.5 ) ( 2615865 * )
      NEW met1 TAPERRULE met1_width_260  ( 2615960 210775 ) ( 2637415 * ) via_260_260_hv 
      NEW met2  ( 2637345 210955 ) ( 2637485 * )
      NEW met2 TAPERRULE met2_width_265  ( 2637345 210512.5 ) ( 2637485 * )
      NEW met1 TAPERRULE met1_width_260  ( 2637615 210775 ) ( 3378600 * )
      NEW met1 TAPERRULE met1_width_260  ( 3378540 210975 ) ( * 1852890 )
      NEW met1  ( 1519775 210775 ) via_260_260_hv  ( * 210865 )
       ( 1519865 * )
      NEW met2  ( 1519725 210910 ) ( 1519865 * )
      NEW met2  ( 1519715 210685 ) ( 1519865 * )
      NEW met1 TAPERRULE met1_width_260  ( 998595 210775 ) ( 1519575 * )
      NEW met1  ( 998395 210775 ) via_260_260_hv  ( * 210865 )
       ( 998485 * )
      NEW met2  ( 998345 210925 ) ( 998485 * )
      NEW met2  ( 998335 210685 ) ( 998485 * )
      NEW met1 TAPERRULE met1_width_260  ( 976970 210775 ) ( 998195 * )
      NEW met1  ( 976770 210775 ) via_260_260_hv  ( * 210865 )
       ( 976865 * )
      NEW met2  ( 976725 210920 ) ( 976865 * )
      NEW met2  ( 976710 210685 ) ( 976865 * )
      NEW met1 TAPERRULE met1_width_260  ( 726105 210775 ) ( 976570 * )
      NEW met1  ( 725605 210775 ) via_860_260_hv  ( * 210865 )
       ( 725965 * )
      NEW met1 TAPERRULE met1_width_260  ( 209400 210775 ) ( 725105 * )
      NEW met1 TAPERRULE met1_width_260  ( 209460 210975 ) ( * 3923860 )
      NEW met2  ( 725245 210685 ) ( 725965 * )
      NEW met2 TAPERRULE met2_width_150  ( 725605 199800 ) ( * 210545 )
      NEW met2 TAPERRULE met2_width_150  ( 976725 210540 ) ( 976865 * )
      NEW met2 TAPERRULE met2_width_150  ( 998345 210540 ) ( 998485 * )
      NEW met2 TAPERRULE met2_width_150  ( 1519725 210540 ) ( 1519865 * )
      NEW met2 TAPERRULE met2_width_280  ( 1541415 210495 ) ( * 211060 ) ;
   - resetb_pad/INP_SEL_H ( resetb_pad INP_SEL_H ) ;
   - mprj_io[8] ( mprj_pads.area1_io_pad\[8\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 2972000 ) ( * 3033000 ) ;
   - mprj_pads.area1_io_pad\[8\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[8\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[8\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[8\] ENABLE_INP_H ) ;
   - mprj_io_in[8] ( mprj_pads.area1_io_pad\[8\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2969775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[8\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[8\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[8\] TIE_HI_ESD ) ;
   - mprj_io_one[8] ( mprj_pads.area1_io_pad\[8\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2975755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[8] ( mprj_pads.area1_io_pad\[8\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2978975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[1] ( mprj_pads.area1_io_pad\[8\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2982195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[8\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[8\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[25] ( mprj_pads.area1_io_pad\[8\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2988175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[1] ( mprj_pads.area1_io_pad\[8\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2991395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[8] ( mprj_pads.area1_io_pad\[8\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2994155 ) ( 3379365 * ) ;
   - mprj_io_dm[24] ( mprj_pads.area1_io_pad\[8\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2997375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[8] ( mprj_pads.area1_io_pad\[8\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3000595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[8] ( mprj_pads.area1_io_pad\[8\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3003355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[8\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[8\] ENABLE_H ) ;
   - mprj_io_analog_sel[8] ( mprj_pads.area1_io_pad\[8\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3015775 ) ( 3379365 * ) ;
   - mprj_io_dm[26] ( mprj_pads.area1_io_pad\[8\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3018995 ) ( 3379365 * ) ;
   - mprj_io_holdover[8] ( mprj_pads.area1_io_pad\[8\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3022215 ) ( 3379365 * ) ;
   - mprj_io_out[8] ( mprj_pads.area1_io_pad\[8\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3024975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[8\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[8\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[8] ( mprj_pads.area1_io_pad\[8\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3034175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[8]
       ( mprj_pads.area1_io_pad\[8\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3037395 ) ( 3379365 * ) ;
   - mprj_io_oeb[8] ( mprj_pads.area1_io_pad\[8\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3040615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[8] ( mprj_pads.area1_io_pad\[8\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3043375 ) ( 3379365 * ) ;
   - mprj_io[24] ( user2_analog_pad\[3\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 64465 4783850 ) ( * 4843090 ) ;
   - mprj_analog[10] ( user2_analog_pad\[3\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 117800 4813220 ) ( 199850 * ) ;
   - mprj_io[33] ( mprj_pads.area2_io_pad\[8\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[22] ( mprj_pads.area2_io_pad\[8\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1847225 ) ( 210895 * ) ;
   - mprj_io_one[22] ( mprj_pads.area2_io_pad\[8\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1841245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[22] ( mprj_pads.area2_io_pad\[8\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1838025 ) ( 210895 * ) ;
   - mprj_gpio_analog[15]
       ( mprj_pads.area2_io_pad\[8\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1834805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[8\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[8\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[67] ( mprj_pads.area2_io_pad\[8\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1828825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[15] ( mprj_pads.area2_io_pad\[8\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1825605 ) ( 210895 * ) ;
   - mprj_io_analog_en[22] ( mprj_pads.area2_io_pad\[8\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1822845 ) ( 210895 * ) ;
   - mprj_io_dm[66] ( mprj_pads.area2_io_pad\[8\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1819625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[22] ( mprj_pads.area2_io_pad\[8\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1816405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[22] ( mprj_pads.area2_io_pad\[8\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1813645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[8\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[8\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[8\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[8\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[8\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[22] ( mprj_pads.area2_io_pad\[8\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1801225 ) ( 210895 * ) ;
   - mprj_io_dm[68] ( mprj_pads.area2_io_pad\[8\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1798005 ) ( 210895 * ) ;
   - mprj_io_holdover[22] ( mprj_pads.area2_io_pad\[8\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1794785 ) ( 210895 * ) ;
   - mprj_io_out[22] ( mprj_pads.area2_io_pad\[8\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1792025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[8\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[8\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[8\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[8\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[22] ( mprj_pads.area2_io_pad\[8\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1782825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[22]
       ( mprj_pads.area2_io_pad\[8\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1779605 ) ( 210895 * ) ;
   - mprj_io_oeb[22] ( mprj_pads.area2_io_pad\[8\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1776385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[22] ( mprj_pads.area2_io_pad\[8\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1773625 ) ( 210895 * ) ;
   - vssa1_pad2 ( user1_vssa_hvclamp_pad\[1\] VSSA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3523530 2085910 ) ( * 2145150 ) ;
   - vssa_pad ( mgmt_vssa_hvclamp_pad VSSA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 401910 64465 ) ( 461150 * ) ;
   - mprj_io[16] ( user1_analog_pad\[1\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 2633850 5123530 ) ( 2693090 * ) ;
   - mprj_analog[2] ( user1_analog_pad\[1\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 2663220 4988150 ) ( * 5070200 ) ;
   - vccd2_pad ( user2_vccd_lvclamp_pad VCCD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 31635 4597470 ) ( 97295 * ) ;
   - vssio ( FILLER_147 VSSIO ) ( FILLER_146 VSSIO )
       ( FILLER_145 VSSIO ) ( FILLER_144 VSSIO ) ( FILLER_143 VSSIO )
       ( FILLER_142 VSSIO ) ( FILLER_141 VSSIO ) ( FILLER_140 VSSIO )
       ( FILLER_139 VSSIO ) ( FILLER_138 VSSIO ) ( FILLER_137 VSSIO )
       ( FILLER_136 VSSIO ) ( FILLER_135 VSSIO )
       ( user1_analog_pad\[0\] VSSIO ) ( FILLER_133 VSSIO )
       ( FILLER_132 VSSIO ) ( FILLER_131 VSSIO ) ( FILLER_130 VSSIO )
       ( FILLER_129 VSSIO ) ( FILLER_128 VSSIO ) ( FILLER_127 VSSIO )
       ( FILLER_126 VSSIO ) ( FILLER_125 VSSIO ) ( FILLER_124 VSSIO )
       ( FILLER_123 VSSIO ) ( user1_vssa_hvclamp_pad\[0\] VSSIO )
       ( FILLER_121 VSSIO ) ( FILLER_120 VSSIO ) ( FILLER_119 VSSIO )
       ( FILLER_118 VSSIO ) ( FILLER_117 VSSIO ) ( FILLER_116 VSSIO )
       ( FILLER_115 VSSIO ) ( FILLER_114 VSSIO ) ( FILLER_113 VSSIO )
       ( FILLER_112 VSSIO ) ( FILLER_111 VSSIO ) ( FILLER_110 VSSIO )
       ( user1_analog_pad\[1\] VSSIO ) ( FILLER_108 VSSIO )
       ( FILLER_107 VSSIO ) ( FILLER_106 VSSIO ) ( FILLER_105 VSSIO )
       ( FILLER_104 VSSIO ) ( FILLER_103 VSSIO ) ( FILLER_102 VSSIO )
       ( FILLER_101 VSSIO ) ( FILLER_100 VSSIO ) ( FILLER_99 VSSIO )
       ( FILLER_98 VSSIO ) ( user1_analog_pad\[2\] VSSIO )
       ( FILLER_96 VSSIO ) ( FILLER_95 VSSIO ) ( FILLER_94 VSSIO )
       ( FILLER_93 VSSIO ) ( FILLER_92 VSSIO ) ( FILLER_91 VSSIO )
       ( FILLER_90 VSSIO ) ( FILLER_89 VSSIO ) ( FILLER_88 VSSIO )
       ( FILLER_87 VSSIO ) ( FILLER_86 VSSIO ) ( FILLER_85 VSSIO )
       ( FILLER_84 VSSIO ) ( FILLER_83 VSSIO ) ( FILLER_82 VSSIO )
       ( FILLER_81 VSSIO ) ( FILLER_80 VSSIO ) ( FILLER_79 VSSIO )
       ( sky130_ef_io__com_bus_slice_10um_0 VSSIO )
       ( FILLER_78 VSSIO ) ( sky130_ef_io__com_bus_slice_5um_1 VSSIO )
       ( user1_analog_pad_with_clamp VSSIO )
       ( sky130_ef_io__com_bus_slice_5um_0 VSSIO )
       ( disconnect_vdda_0 VSSIO ) ( FILLER_SB3 VSSIO )
       ( FILLER_73 VSSIO ) ( FILLER_72 VSSIO ) ( FILLER_71 VSSIO )
       ( FILLER_70 VSSIO ) ( FILLER_69 VSSIO ) ( FILLER_68 VSSIO )
       ( mgmt_vssio_hvclamp_pad\[1\] VSSIO ) ( FILLER_66 VSSIO )
       ( FILLER_65 VSSIO ) ( FILLER_64 VSSIO ) ( FILLER_63 VSSIO )
       ( FILLER_62 VSSIO ) ( FILLER_61 VSSIO ) ( FILLER_60 VSSIO )
       ( sky130_ef_io__com_bus_slice_10um_1 VSSIO )
       ( sky130_ef_io__com_bus_slice_5um_3 VSSIO )
       ( user2_analog_pad_with_clamp\[0\] VSSIO )
       ( sky130_ef_io__com_bus_slice_5um_2 VSSIO ) ( FILLER_57 VSSIO )
       ( FILLER_56 VSSIO ) ( FILLER_55 VSSIO ) ( FILLER_54 VSSIO )
       ( FILLER_53 VSSIO ) ( FILLER_52 VSSIO ) ( FILLER_51 VSSIO )
       ( FILLER_50 VSSIO ) ( FILLER_49 VSSIO )
       ( user2_analog_pad_with_clamp\[1\] VSSIO ) ( FILLER_47 VSSIO )
       ( FILLER_46 VSSIO ) ( FILLER_45 VSSIO ) ( FILLER_44 VSSIO )
       ( FILLER_43 VSSIO ) ( FILLER_42 VSSIO )
       ( user2_analog_pad\[0\] VSSIO ) ( FILLER_41 VSSIO )
       ( FILLER_39 VSSIO ) ( FILLER_38 VSSIO ) ( FILLER_37 VSSIO )
       ( FILLER_36 VSSIO ) ( FILLER_35 VSSIO ) ( FILLER_34 VSSIO )
       ( FILLER_33 VSSIO ) ( FILLER_32 VSSIO ) ( FILLER_31 VSSIO )
       ( FILLER_30 VSSIO ) ( FILLER_29 VSSIO )
       ( user2_analog_pad\[1\] VSSIO ) ( FILLER_27 VSSIO )
       ( FILLER_26 VSSIO ) ( FILLER_25 VSSIO ) ( FILLER_24 VSSIO )
       ( FILLER_23 VSSIO ) ( FILLER_22 VSSIO ) ( FILLER_21 VSSIO )
       ( FILLER_20 VSSIO ) ( FILLER_19 VSSIO ) ( FILLER_18 VSSIO )
       ( FILLER_17 VSSIO ) ( user2_analog_pad\[2\] VSSIO )
       ( FILLER_15 VSSIO ) ( FILLER_14 VSSIO ) ( FILLER_13 VSSIO )
       ( FILLER_12 VSSIO ) ( FILLER_11 VSSIO ) ( FILLER_10 VSSIO )
       ( FILLER_9 VSSIO ) ( FILLER_8 VSSIO ) ( FILLER_7 VSSIO )
       ( FILLER_6 VSSIO ) ( user2_corner VSSIO ) ( FILLER_5 VSSIO )
       ( FILLER_579 VSSIO ) ( FILLER_578 VSSIO )
       ( user1_corner VSSIO ) ( FILLER_786 VSSIO )
       ( FILLER_577 VSSIO ) ( FILLER_576 VSSIO ) ( FILLER_785 VSSIO )
       ( FILLER_575 VSSIO ) ( FILLER_784 VSSIO ) ( FILLER_574 VSSIO )
       ( FILLER_783 VSSIO ) ( FILLER_573 VSSIO ) ( FILLER_782 VSSIO )
       ( FILLER_572 VSSIO ) ( FILLER_781 VSSIO ) ( FILLER_571 VSSIO )
       ( FILLER_780 VSSIO ) ( FILLER_779 VSSIO ) ( FILLER_570 VSSIO )
       ( user2_analog_pad\[3\] VSSIO ) ( FILLER_776 VSSIO )
       ( FILLER_568 VSSIO ) ( user1_analog_pad\[3\] VSSIO )
       ( FILLER_567 VSSIO ) ( FILLER_777 VSSIO ) ( FILLER_775 VSSIO )
       ( FILLER_566 VSSIO ) ( FILLER_774 VSSIO ) ( FILLER_565 VSSIO )
       ( FILLER_773 VSSIO ) ( FILLER_564 VSSIO ) ( FILLER_772 VSSIO )
       ( FILLER_563 VSSIO ) ( FILLER_771 VSSIO ) ( FILLER_562 VSSIO )
       ( FILLER_561 VSSIO ) ( FILLER_770 VSSIO ) ( FILLER_769 VSSIO )
       ( user2_vccd_lvclamp_pad VSSIO ) ( FILLER_559 VSSIO )
       ( FILLER_558 VSSIO ) ( FILLER_557 VSSIO )
       ( user1_vccd_lvclamp_pad VSSIO ) ( FILLER_767 VSSIO )
       ( FILLER_766 VSSIO ) ( FILLER_556 VSSIO ) ( FILLER_765 VSSIO )
       ( FILLER_555 VSSIO ) ( FILLER_764 VSSIO ) ( FILLER_554 VSSIO )
       ( FILLER_763 VSSIO ) ( FILLER_553 VSSIO ) ( FILLER_762 VSSIO )
       ( FILLER_552 VSSIO ) ( FILLER_761 VSSIO ) ( FILLER_551 VSSIO )
       ( FILLER_760 VSSIO ) ( mgmt_vddio_hvclamp_pad\[1\] VSSIO )
       ( FILLER_759 VSSIO ) ( FILLER_549 VSSIO ) ( FILLER_548 VSSIO )
       ( FILLER_547 VSSIO ) ( FILLER_546 VSSIO )
       ( mprj_pads.area1_io_pad\[13\] VSSIO ) ( FILLER_757 VSSIO )
       ( FILLER_545 VSSIO ) ( FILLER_756 VSSIO ) ( FILLER_544 VSSIO )
       ( FILLER_755 VSSIO ) ( FILLER_543 VSSIO ) ( FILLER_754 VSSIO )
       ( FILLER_542 VSSIO ) ( FILLER_753 VSSIO ) ( FILLER_541 VSSIO )
       ( FILLER_752 VSSIO ) ( FILLER_751 VSSIO )
       ( user2_vssa_hvclamp_pad VSSIO ) ( FILLER_750 VSSIO )
       ( FILLER_539 VSSIO ) ( FILLER_538 VSSIO ) ( FILLER_537 VSSIO )
       ( FILLER_536 VSSIO ) ( user1_vdda_hvclamp_pad\[0\] VSSIO )
       ( FILLER_748 VSSIO ) ( FILLER_747 VSSIO ) ( FILLER_535 VSSIO )
       ( FILLER_746 VSSIO ) ( FILLER_534 VSSIO ) ( FILLER_745 VSSIO )
       ( FILLER_533 VSSIO ) ( FILLER_744 VSSIO ) ( FILLER_532 VSSIO )
       ( FILLER_743 VSSIO ) ( FILLER_531 VSSIO ) ( FILLER_742 VSSIO )
       ( FILLER_741 VSSIO ) ( FILLER_740 VSSIO )
       ( mprj_pads.area2_io_pad\[0\] VSSIO ) ( FILLER_529 VSSIO )
       ( FILLER_528 VSSIO ) ( FILLER_527 VSSIO ) ( FILLER_526 VSSIO )
       ( mprj_pads.area1_io_pad\[12\] VSSIO ) ( FILLER_525 VSSIO )
       ( FILLER_738 VSSIO ) ( FILLER_524 VSSIO ) ( FILLER_737 VSSIO )
       ( FILLER_523 VSSIO ) ( FILLER_736 VSSIO ) ( FILLER_522 VSSIO )
       ( FILLER_735 VSSIO ) ( FILLER_734 VSSIO ) ( FILLER_521 VSSIO )
       ( FILLER_733 VSSIO ) ( FILLER_732 VSSIO )
       ( mprj_pads.area2_io_pad\[1\] VSSIO ) ( FILLER_731 VSSIO )
       ( FILLER_519 VSSIO ) ( FILLER_518 VSSIO ) ( FILLER_517 VSSIO )
       ( FILLER_516 VSSIO ) ( FILLER_515 VSSIO )
       ( mprj_pads.area1_io_pad\[11\] VSSIO ) ( FILLER_729 VSSIO )
       ( FILLER_514 VSSIO ) ( FILLER_728 VSSIO ) ( FILLER_513 VSSIO )
       ( FILLER_727 VSSIO ) ( FILLER_512 VSSIO ) ( FILLER_726 VSSIO )
       ( FILLER_511 VSSIO ) ( FILLER_725 VSSIO ) ( FILLER_724 VSSIO )
       ( FILLER_723 VSSIO ) ( FILLER_722 VSSIO )
       ( mprj_pads.area2_io_pad\[2\] VSSIO ) ( FILLER_509 VSSIO )
       ( FILLER_508 VSSIO ) ( FILLER_507 VSSIO ) ( FILLER_506 VSSIO )
       ( FILLER_505 VSSIO ) ( mprj_pads.area1_io_pad\[10\] VSSIO )
       ( FILLER_720 VSSIO ) ( FILLER_719 VSSIO ) ( FILLER_504 VSSIO )
       ( FILLER_718 VSSIO ) ( FILLER_503 VSSIO ) ( FILLER_717 VSSIO )
       ( FILLER_502 VSSIO ) ( FILLER_501 VSSIO ) ( FILLER_716 VSSIO )
       ( FILLER_715 VSSIO ) ( FILLER_714 VSSIO ) ( FILLER_713 VSSIO )
       ( FILLER_712 VSSIO ) ( mprj_pads.area2_io_pad\[3\] VSSIO )
       ( FILLER_499 VSSIO ) ( FILLER_498 VSSIO ) ( FILLER_497 VSSIO )
       ( FILLER_496 VSSIO ) ( FILLER_495 VSSIO ) ( FILLER_494 VSSIO )
       ( mprj_pads.area1_io_pad\[9\] VSSIO ) ( FILLER_710 VSSIO )
       ( FILLER_493 VSSIO ) ( FILLER_709 VSSIO ) ( FILLER_492 VSSIO )
       ( FILLER_708 VSSIO ) ( FILLER_491 VSSIO ) ( FILLER_707 VSSIO )
       ( FILLER_706 VSSIO ) ( FILLER_705 VSSIO ) ( FILLER_704 VSSIO )
       ( mprj_pads.area2_io_pad\[4\] VSSIO ) ( FILLER_489 VSSIO )
       ( FILLER_488 VSSIO ) ( FILLER_703 VSSIO ) ( FILLER_487 VSSIO )
       ( FILLER_486 VSSIO ) ( FILLER_485 VSSIO ) ( FILLER_484 VSSIO )
       ( mprj_pads.area1_io_pad\[8\] VSSIO ) ( FILLER_701 VSSIO )
       ( FILLER_483 VSSIO ) ( FILLER_700 VSSIO ) ( FILLER_482 VSSIO )
       ( FILLER_699 VSSIO ) ( FILLER_481 VSSIO ) ( FILLER_698 VSSIO )
       ( FILLER_697 VSSIO ) ( FILLER_696 VSSIO ) ( FILLER_695 VSSIO )
       ( FILLER_694 VSSIO ) ( mprj_pads.area2_io_pad\[5\] VSSIO )
       ( FILLER_479 VSSIO ) ( FILLER_478 VSSIO ) ( FILLER_477 VSSIO )
       ( FILLER_693 VSSIO ) ( FILLER_476 VSSIO ) ( FILLER_475 VSSIO )
       ( FILLER_474 VSSIO ) ( FILLER_473 VSSIO )
       ( mprj_pads.area1_io_pad\[7\] VSSIO ) ( FILLER_691 VSSIO )
       ( FILLER_472 VSSIO ) ( FILLER_690 VSSIO ) ( FILLER_471 VSSIO )
       ( FILLER_689 VSSIO ) ( FILLER_688 VSSIO ) ( FILLER_687 VSSIO )
       ( FILLER_686 VSSIO ) ( mprj_pads.area2_io_pad\[6\] VSSIO )
       ( FILLER_469 VSSIO ) ( FILLER_468 VSSIO ) ( FILLER_685 VSSIO )
       ( FILLER_467 VSSIO ) ( FILLER_684 VSSIO ) ( FILLER_466 VSSIO )
       ( FILLER_465 VSSIO ) ( FILLER_464 VSSIO ) ( FILLER_463 VSSIO )
       ( user1_vdda_hvclamp_pad\[1\] VSSIO ) ( FILLER_682 VSSIO )
       ( FILLER_462 VSSIO ) ( FILLER_681 VSSIO ) ( FILLER_461 VSSIO )
       ( FILLER_680 VSSIO ) ( FILLER_679 VSSIO ) ( FILLER_678 VSSIO )
       ( FILLER_677 VSSIO ) ( user2_vdda_hvclamp_pad VSSIO )
       ( FILLER_459 VSSIO ) ( FILLER_458 VSSIO ) ( FILLER_457 VSSIO )
       ( FILLER_676 VSSIO ) ( FILLER_675 VSSIO ) ( FILLER_456 VSSIO )
       ( FILLER_455 VSSIO ) ( FILLER_454 VSSIO ) ( FILLER_453 VSSIO )
       ( user1_vssd_lvclamp_pad VSSIO ) ( FILLER_673 VSSIO )
       ( FILLER_452 VSSIO ) ( FILLER_672 VSSIO ) ( FILLER_671 VSSIO )
       ( FILLER_451 VSSIO ) ( gpio_pad VSSIO ) ( FILLER_670 VSSIO )
       ( FILLER_669 VSSIO ) ( FILLER_668 VSSIO )
       ( user2_vssd_lvclamp_pad VSSIO ) ( FILLER_449 VSSIO )
       ( FILLER_667 VSSIO ) ( FILLER_448 VSSIO ) ( FILLER_447 VSSIO )
       ( FILLER_666 VSSIO ) ( FILLER_446 VSSIO ) ( FILLER_665 VSSIO )
       ( FILLER_445 VSSIO ) ( FILLER_444 VSSIO ) ( FILLER_443 VSSIO )
       ( FILLER_442 VSSIO ) ( user1_vssa_hvclamp_pad\[1\] VSSIO )
       ( FILLER_663 VSSIO ) ( FILLER_441 VSSIO ) ( FILLER_662 VSSIO )
       ( FILLER_661 VSSIO ) ( FILLER_660 VSSIO ) ( FILLER_659 VSSIO )
       ( mprj_pads.area2_io_pad\[7\] VSSIO ) ( FILLER_439 VSSIO )
       ( FILLER_438 VSSIO ) ( FILLER_658 VSSIO ) ( FILLER_437 VSSIO )
       ( FILLER_657 VSSIO ) ( FILLER_436 VSSIO ) ( FILLER_656 VSSIO )
       ( FILLER_435 VSSIO ) ( FILLER_434 VSSIO ) ( FILLER_433 VSSIO )
       ( FILLER_432 VSSIO ) ( mprj_pads.area1_io_pad\[6\] VSSIO )
       ( FILLER_654 VSSIO ) ( FILLER_431 VSSIO ) ( FILLER_653 VSSIO )
       ( FILLER_652 VSSIO ) ( FILLER_651 VSSIO ) ( FILLER_650 VSSIO )
       ( mprj_pads.area2_io_pad\[8\] VSSIO ) ( FILLER_649 VSSIO )
       ( FILLER_429 VSSIO ) ( FILLER_428 VSSIO ) ( FILLER_427 VSSIO )
       ( FILLER_648 VSSIO ) ( FILLER_426 VSSIO ) ( FILLER_647 VSSIO )
       ( FILLER_425 VSSIO ) ( FILLER_646 VSSIO ) ( FILLER_424 VSSIO )
       ( FILLER_423 VSSIO ) ( FILLER_422 VSSIO ) ( FILLER_421 VSSIO )
       ( mprj_pads.area1_io_pad\[5\] VSSIO ) ( FILLER_644 VSSIO )
       ( FILLER_643 VSSIO ) ( FILLER_642 VSSIO ) ( FILLER_641 VSSIO )
       ( mprj_pads.area2_io_pad\[9\] VSSIO ) ( FILLER_419 VSSIO )
       ( FILLER_418 VSSIO ) ( FILLER_640 VSSIO ) ( FILLER_417 VSSIO )
       ( FILLER_639 VSSIO ) ( FILLER_416 VSSIO ) ( FILLER_638 VSSIO )
       ( FILLER_415 VSSIO ) ( FILLER_637 VSSIO ) ( FILLER_414 VSSIO )
       ( FILLER_413 VSSIO ) ( FILLER_412 VSSIO ) ( FILLER_411 VSSIO )
       ( mprj_pads.area1_io_pad\[4\] VSSIO ) ( FILLER_635 VSSIO )
       ( FILLER_634 VSSIO ) ( FILLER_633 VSSIO )
       ( mprj_pads.area2_io_pad\[10\] VSSIO ) ( FILLER_409 VSSIO )
       ( FILLER_632 VSSIO ) ( FILLER_408 VSSIO ) ( FILLER_407 VSSIO )
       ( FILLER_631 VSSIO ) ( FILLER_406 VSSIO ) ( FILLER_630 VSSIO )
       ( FILLER_405 VSSIO ) ( FILLER_629 VSSIO ) ( FILLER_404 VSSIO )
       ( FILLER_628 VSSIO ) ( FILLER_403 VSSIO ) ( FILLER_402 VSSIO )
       ( FILLER_401 VSSIO ) ( mprj_pads.area1_io_pad\[3\] VSSIO )
       ( FILLER_626 VSSIO ) ( FILLER_625 VSSIO ) ( FILLER_624 VSSIO )
       ( FILLER_623 VSSIO ) ( mprj_pads.area2_io_pad\[11\] VSSIO )
       ( FILLER_399 VSSIO ) ( FILLER_398 VSSIO ) ( FILLER_622 VSSIO )
       ( FILLER_397 VSSIO ) ( FILLER_621 VSSIO ) ( FILLER_396 VSSIO )
       ( FILLER_620 VSSIO ) ( FILLER_395 VSSIO ) ( FILLER_619 VSSIO )
       ( FILLER_394 VSSIO ) ( FILLER_618 VSSIO ) ( FILLER_393 VSSIO )
       ( FILLER_392 VSSIO ) ( FILLER_391 VSSIO )
       ( mprj_pads.area1_io_pad\[2\] VSSIO ) ( FILLER_616 VSSIO )
       ( FILLER_615 VSSIO ) ( FILLER_614 VSSIO )
       ( mprj_pads.area2_io_pad\[12\] VSSIO ) ( FILLER_389 VSSIO )
       ( FILLER_388 VSSIO ) ( FILLER_387 VSSIO ) ( FILLER_613 VSSIO )
       ( FILLER_386 VSSIO ) ( FILLER_612 VSSIO ) ( FILLER_385 VSSIO )
       ( FILLER_611 VSSIO ) ( FILLER_384 VSSIO ) ( FILLER_610 VSSIO )
       ( FILLER_383 VSSIO ) ( FILLER_609 VSSIO ) ( FILLER_382 VSSIO )
       ( FILLER_381 VSSIO ) ( FILLER_380 VSSIO ) ( FILLER_379 VSSIO )
       ( mprj_pads.area1_io_pad\[1\] VSSIO ) ( FILLER_607 VSSIO )
       ( FILLER_606 VSSIO ) ( FILLER_378 VSSIO ) ( FILLER_605 VSSIO )
       ( FILLER_377 VSSIO ) ( FILLER_604 VSSIO ) ( FILLER_376 VSSIO )
       ( FILLER_603 VSSIO ) ( FILLER_375 VSSIO ) ( FILLER_602 VSSIO )
       ( FILLER_374 VSSIO ) ( disconnect_vdda_2 VSSIO )
       ( FILLER_SB2 VSSIO ) ( FILLER_601 VSSIO ) ( FILLER_600 VSSIO )
       ( mgmt_vddio_hvclamp_pad\[0\] VSSIO ) ( FILLER_599 VSSIO )
       ( FILLER_370 VSSIO ) ( FILLER_369 VSSIO ) ( FILLER_368 VSSIO )
       ( FILLER_367 VSSIO ) ( mprj_pads.area1_io_pad\[0\] VSSIO )
       ( FILLER_597 VSSIO ) ( FILLER_366 VSSIO ) ( FILLER_596 VSSIO )
       ( FILLER_365 VSSIO ) ( FILLER_595 VSSIO ) ( FILLER_364 VSSIO )
       ( FILLER_594 VSSIO ) ( FILLER_363 VSSIO ) ( FILLER_593 VSSIO )
       ( FILLER_362 VSSIO ) ( FILLER_592 VSSIO ) ( FILLER_591 VSSIO )
       ( FILLER_590 VSSIO ) ( disconnect_vdda_1 VSSIO )
       ( FILLER_SB1 VSSIO ) ( FILLER_587 VSSIO )
       ( mgmt_vccd_lvclamp_pad VSSIO ) ( FILLER_360 VSSIO )
       ( FILLER_359 VSSIO ) ( FILLER_358 VSSIO ) ( FILLER_586 VSSIO )
       ( FILLER_357 VSSIO ) ( FILLER_585 VSSIO ) ( FILLER_356 VSSIO )
       ( FILLER_584 VSSIO ) ( FILLER_583 VSSIO ) ( FILLER_355 VSSIO )
       ( FILLER_582 VSSIO ) ( FILLER_354 VSSIO ) ( FILLER_581 VSSIO )
       ( FILLER_353 VSSIO ) ( mgmt_corner\[1\] VSSIO )
       ( FILLER_352 VSSIO ) ( FILLER_580 VSSIO ) ( FILLER_351 VSSIO )
       ( FILLER_350 VSSIO ) ( FILLER_349 VSSIO ) ( FILLER_348 VSSIO )
       ( FILLER_347 VSSIO ) ( FILLER_346 VSSIO ) ( bus_tie_72 VSSIO )
       ( bus_tie_71 VSSIO ) ( bus_tie_70 VSSIO ) ( bus_tie_69 VSSIO )
       ( bus_tie_68 VSSIO ) ( bus_tie_67 VSSIO ) ( FILLER_339 VSSIO )
       ( FILLER_338 VSSIO ) ( FILLER_337 VSSIO ) ( FILLER_336 VSSIO )
       ( FILLER_335 VSSIO ) ( mgmt_vdda_hvclamp_pad VSSIO )
       ( FILLER_333 VSSIO ) ( FILLER_332 VSSIO ) ( FILLER_331 VSSIO )
       ( FILLER_330 VSSIO ) ( bus_tie_66 VSSIO ) ( FILLER_329 VSSIO )
       ( bus_tie_65 VSSIO ) ( bus_tie_64 VSSIO ) ( bus_tie_63 VSSIO )
       ( bus_tie_62 VSSIO ) ( bus_tie_61 VSSIO ) ( FILLER_322 VSSIO )
       ( FILLER_321 VSSIO ) ( FILLER_320 VSSIO ) ( FILLER_319 VSSIO )
       ( FILLER_318 VSSIO ) ( mgmt_vssio_hvclamp_pad\[0\] VSSIO )
       ( FILLER_316 VSSIO ) ( FILLER_315 VSSIO ) ( FILLER_314 VSSIO )
       ( FILLER_313 VSSIO ) ( bus_tie_60 VSSIO ) ( FILLER_312 VSSIO )
       ( bus_tie_59 VSSIO ) ( bus_tie_58 VSSIO ) ( bus_tie_57 VSSIO )
       ( bus_tie_56 VSSIO ) ( bus_tie_55 VSSIO ) ( FILLER_305 VSSIO )
       ( FILLER_304 VSSIO ) ( FILLER_303 VSSIO ) ( FILLER_302 VSSIO )
       ( FILLER_301 VSSIO ) ( clock_pad VSSIO ) ( FILLER_299 VSSIO )
       ( FILLER_298 VSSIO ) ( FILLER_297 VSSIO ) ( FILLER_296 VSSIO )
       ( FILLER_295 VSSIO ) ( bus_tie_54 VSSIO ) ( bus_tie_53 VSSIO )
       ( bus_tie_52 VSSIO ) ( bus_tie_51 VSSIO ) ( bus_tie_50 VSSIO )
       ( bus_tie_49 VSSIO ) ( FILLER_288 VSSIO ) ( FILLER_287 VSSIO )
       ( FILLER_286 VSSIO ) ( FILLER_285 VSSIO ) ( FILLER_284 VSSIO )
       ( flash_io1_pad VSSIO ) ( FILLER_282 VSSIO )
       ( FILLER_281 VSSIO ) ( FILLER_280 VSSIO ) ( FILLER_279 VSSIO )
       ( bus_tie_48 VSSIO ) ( FILLER_278 VSSIO ) ( bus_tie_47 VSSIO )
       ( bus_tie_46 VSSIO ) ( bus_tie_45 VSSIO ) ( bus_tie_44 VSSIO )
       ( bus_tie_43 VSSIO ) ( FILLER_271 VSSIO ) ( FILLER_270 VSSIO )
       ( FILLER_269 VSSIO ) ( FILLER_268 VSSIO ) ( FILLER_267 VSSIO )
       ( flash_io0_pad VSSIO ) ( FILLER_265 VSSIO )
       ( FILLER_264 VSSIO ) ( FILLER_263 VSSIO ) ( FILLER_262 VSSIO )
       ( FILLER_261 VSSIO ) ( bus_tie_42 VSSIO ) ( bus_tie_41 VSSIO )
       ( bus_tie_40 VSSIO ) ( bus_tie_39 VSSIO ) ( bus_tie_38 VSSIO )
       ( bus_tie_37 VSSIO ) ( FILLER_254 VSSIO ) ( FILLER_253 VSSIO )
       ( FILLER_252 VSSIO ) ( FILLER_251 VSSIO ) ( FILLER_250 VSSIO )
       ( flash_clk_pad VSSIO ) ( FILLER_248 VSSIO )
       ( FILLER_247 VSSIO ) ( FILLER_246 VSSIO ) ( FILLER_245 VSSIO )
       ( bus_tie_36 VSSIO ) ( FILLER_244 VSSIO ) ( bus_tie_35 VSSIO )
       ( bus_tie_34 VSSIO ) ( bus_tie_33 VSSIO ) ( bus_tie_32 VSSIO )
       ( bus_tie_31 VSSIO ) ( FILLER_237 VSSIO ) ( FILLER_236 VSSIO )
       ( FILLER_235 VSSIO ) ( FILLER_234 VSSIO ) ( FILLER_233 VSSIO )
       ( flash_csb_pad VSSIO ) ( FILLER_231 VSSIO )
       ( FILLER_230 VSSIO ) ( FILLER_229 VSSIO ) ( FILLER_228 VSSIO )
       ( FILLER_227 VSSIO ) ( bus_tie_30 VSSIO ) ( bus_tie_29 VSSIO )
       ( bus_tie_28 VSSIO ) ( bus_tie_27 VSSIO ) ( bus_tie_26 VSSIO )
       ( bus_tie_25 VSSIO ) ( FILLER_220 VSSIO ) ( FILLER_219 VSSIO )
       ( FILLER_218 VSSIO ) ( FILLER_217 VSSIO ) ( FILLER_216 VSSIO )
       ( mgmt_vssd_lvclamp_pad VSSIO ) ( FILLER_214 VSSIO )
       ( FILLER_213 VSSIO ) ( FILLER_212 VSSIO ) ( FILLER_211 VSSIO )
       ( bus_tie_24 VSSIO ) ( FILLER_210 VSSIO ) ( bus_tie_23 VSSIO )
       ( bus_tie_22 VSSIO ) ( bus_tie_21 VSSIO ) ( bus_tie_20 VSSIO )
       ( bus_tie_19 VSSIO ) ( FILLER_203 VSSIO ) ( FILLER_202 VSSIO )
       ( FILLER_201 VSSIO ) ( FILLER_200 VSSIO ) ( FILLER_199 VSSIO )
       ( bus_tie_9 VSSIO ) ( FILLER_197 VSSIO )
       ( mgmt_vssa_hvclamp_pad VSSIO ) ( mgmt_corner\[0\] VSSIO )
       ( FILLER_163 VSSIO ) ( FILLER_162 VSSIO ) ( FILLER_161 VSSIO )
       ( FILLER_160 VSSIO ) ( bus_tie_6 VSSIO ) ( FILLER_159 VSSIO )
       ( bus_tie_5 VSSIO ) ( bus_tie_4 VSSIO ) ( bus_tie_3 VSSIO )
       ( bus_tie_2 VSSIO ) ( bus_tie_1 VSSIO ) ( FILLER_152 VSSIO )
       ( FILLER_151 VSSIO ) ( FILLER_150 VSSIO ) ( FILLER_149 VSSIO )
       ( FILLER_148 VSSIO ) ( FILLER_196 VSSIO ) ( FILLER_195 VSSIO )
       ( FILLER_194 VSSIO ) ( bus_tie_18 VSSIO ) ( FILLER_193 VSSIO )
       ( bus_tie_17 VSSIO ) ( bus_tie_16 VSSIO ) ( bus_tie_15 VSSIO )
       ( bus_tie_14 VSSIO ) ( bus_tie_13 VSSIO ) ( FILLER_186 VSSIO )
       ( FILLER_185 VSSIO ) ( FILLER_184 VSSIO ) ( FILLER_183 VSSIO )
       ( FILLER_182 VSSIO ) ( resetb_pad VSSIO ) ( FILLER_180 VSSIO )
       ( FILLER_179 VSSIO ) ( FILLER_178 VSSIO ) ( FILLER_177 VSSIO )
       ( FILLER_176 VSSIO ) ( bus_tie_12 VSSIO ) ( bus_tie_11 VSSIO )
       ( bus_tie_10 VSSIO ) ( bus_tie_8 VSSIO ) ( bus_tie_7 VSSIO )
       ( FILLER_169 VSSIO ) ( FILLER_168 VSSIO ) ( FILLER_167 VSSIO )
       ( FILLER_166 VSSIO ) ( FILLER_165 VSSIO )
      + ROUTED met4 TAPERRULE met4_width_2245  ( 150 2279347.5 ) ( 24065 * ) ;
   - vssd_pad ( mgmt_vssd_lvclamp_pad VSSD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 1243530 31635 ) ( * 97295 ) ;
   - vdda1_pad ( user1_vdda_hvclamp_pad\[0\] VDDA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3523530 4099910 ) ( * 4159150 ) ;
   - gpio ( gpio_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 2578000 64215 ) ( 2639000 * ) ;
   - gpio_pad/TIE_LO_ESD ( gpio_pad TIE_LO_ESD )
       ( gpio_pad ENABLE_VSWITCH_H ) ( gpio_pad ENABLE_INP_H )
      + ROUTED met2  ( 2572565 209095 ) via_260_260_hv 
      NEW met2  ( 2572505 209185 ) ( 2572625 * )
      NEW met1 TAPERRULE met1_width_260  ( 2571880 209095 ) ( 2572365 * )
      NEW met2  ( 2572505 209005 ) ( 2572625 * )
      NEW met1 TAPERRULE met1_width_260  ( 2572765 209095 ) ( 2612560 * ) via_260_260_hv 
       ( * 209185 ) ( 2612620 * )
      NEW met2  ( 2612500 209005 ) ( 2612620 * )
      NEW met1 TAPERRULE met1_width_260  ( 2612760 209095 ) ( 2634180 * ) via_260_260_hv 
       ( * 209185 ) ( 2634240 * )
      NEW met2  ( 2634120 209005 ) ( 2634240 * )
      NEW met1 TAPERRULE met1_width_260  ( 2634380 209095 ) ( 2650065 * ) ;
   - gpio_in_core ( gpio_pad IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2575775 208635 ) ( * 210895 ) ;
   - gpio_pad/HLD_H_N ( gpio_pad HLD_H_N ) ( gpio_pad TIE_HI_ESD )
      + ROUTED met2  ( 2618995 209515 ) via_260_260_hv 
      NEW met2  ( 2618935 209605 ) ( 2619055 * )
      NEW met1 TAPERRULE met1_width_260  ( 2579190 209515 ) ( 2618795 * )
      NEW met1  ( 2578990 209515 ) via_260_260_hv  ( * 209605 )
       ( 2579050 * )
      NEW met1 TAPERRULE met1_width_260  ( 2571880 209515 ) ( 2578790 * )
      NEW met2  ( 2578930 209425 ) ( 2579050 * )
      NEW met2  ( 2618935 209425 ) ( 2619055 * )
      NEW met1 TAPERRULE met1_width_260  ( 2619195 209515 ) ( 2650065 * ) ;
   - gpio_pad/SLOW ( gpio_pad SLOW ) ( constant_block_6 zero )
       ( gpio_pad IB_MODE_SEL ) ( gpio_pad VTRIP_SEL )
       ( gpio_pad HLD_OVR ) ( gpio_pad ANALOG_SEL )
       ( gpio_pad ANALOG_POL ) ( gpio_pad ANALOG_EN )
      + ROUTED met2  ( 2584975 209935 ) via_260_260_hv 
      NEW met2  ( 2584915 210025 ) ( 2585035 * )
      NEW met1 TAPERRULE met1_width_260  ( 2571880 209935 ) ( 2584775 * )
      NEW met2  ( 2584915 209845 ) ( 2585035 * )
      NEW met1 TAPERRULE met1_width_260  ( 2585175 209935 ) ( 2600150 * ) via_260_260_hv 
       ( * 210025 ) ( 2600210 * )
      NEW met2  ( 2600090 209845 ) ( 2600210 * )
      NEW met1 TAPERRULE met1_width_260  ( 2600350 209935 ) ( 2606595 * ) via_260_260_hv 
       ( * 210025 ) ( 2606655 * )
      NEW met2  ( 2606535 209845 ) ( 2606655 * )
      NEW met1 TAPERRULE met1_width_260  ( 2606795 209935 ) ( 2621770 * ) via_260_260_hv 
       ( * 210025 ) ( 2621830 * )
      NEW met2  ( 2621710 209845 ) ( 2621830 * )
      NEW met1 TAPERRULE met1_width_260  ( 2621970 209935 ) ( 2628205 * ) via_260_260_hv 
       ( * 210025 ) ( 2628265 * )
      NEW met2  ( 2628145 209845 ) ( 2628265 * )
      NEW met1 TAPERRULE met1_width_260  ( 2628405 209935 ) ( 2640175 * ) via_260_260_hv 
       ( * 210025 ) ( 2640235 * )
      NEW met2  ( 2640115 209845 ) ( 2640235 * )
      NEW met1 TAPERRULE met1_width_260  ( 2640375 209935 ) ( 2643390 * ) via_260_260_hv 
       ( * 210025 ) ( 2643450 * )
      NEW met2  ( 2643330 209845 ) ( 2643450 * )
      NEW met1 TAPERRULE met1_width_260  ( 2643590 209935 ) ( 2673930 * ) via_260_260_vh 
      NEW met1  ( 2673870 210025 ) ( 2673990 * )
      NEW met2 TAPERRULE met2_width_260  ( 2673930 204755 ) ( * 209735 )
      NEW met2  ( 2673850 204615 ) ( 2674010 * )
      NEW met2  ( 2673930 204490 ) via2_300_300_vx 
      NEW met3  ( 2673905 204515 ) ( 2673955 * )
      NEW met3  ( 2673030 204470 ) ( 2673960 * )
      NEW met3  ( 2673030 204470 ) ( 2673630 * )
      NEW met3  ( 2673905 204465 ) ( 2673955 * )
      NEW met2  ( 2673850 204365 ) ( 2674010 * )
      NEW met1  ( 2673870 209845 ) ( 2673990 * ) ;
   - gpio_pad/PAD_A_ESD_0_H ( gpio_pad PAD_A_ESD_0_H ) ;
   - gpio_pad/PAD_A_ESD_1_H ( gpio_pad PAD_A_ESD_1_H ) ;
   - gpio_mode1_core ( gpio_pad DM[2] ) ( gpio_pad DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2624995 208800 ) ( * 211060 ) ( * 211200 )
       ( * 211380 )
      NEW met2  ( 2624930 211520 ) ( 2625050 * )
      NEW met2  ( 2624990 211610 ) via_260_260_hv 
      NEW met2  ( 2624930 211700 ) ( 2625050 * )
      NEW met1  ( 2594370 211610 ) ( 2624790 * )
      NEW met1  ( 2594170 211610 ) via_260_260_hv  ( * 211700 )
       ( 2594230 * )
      NEW met2  ( 2594110 211520 ) ( 2594230 * )
      NEW met2  ( 2594170 208950 ) ( * 211380 ) ;
   - gpio_pad/PAD_A_NOESD_H ( gpio_pad PAD_A_NOESD_H ) ;
   - gpio_mode0_core ( gpio_pad DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2603375 208635 ) ( * 210895 ) ;
   - gpio_inenb_core ( gpio_pad INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2609355 208635 ) ( * 210895 ) ;
   - gpio_out_core ( gpio_pad OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2630975 208635 ) ( * 210895 ) ;
   - gpio_outenb_core ( gpio_pad OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 2646615 208635 ) ( * 210895 ) ;
   - gpio_pad/IN_H ( gpio_pad IN_H ) ;
   - vssd1_pad ( user1_vssd_lvclamp_pad VSSD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 3490700 2336530 ) ( 3556360 * ) ;
   - vssd1 ( user1_vccd_lvclamp_pad VSSD1 )
       ( user1_vssd_lvclamp_pad VSSD1 )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3360600 673680 ) ( * 2299230 )
      NEW met5 TAPERRULE met5_width_13000  ( 3360600 2323450 ) ( * 2349170 )
      NEW met5 TAPERRULE met5_width_13000  ( 3360600 2373790 ) ( * 4563640 )
      NEW met5 TAPERRULE met5_width_13000  ( 3360600 4587190 ) ( * 4612730 )
      NEW met4 TAPERRULE met4_width_620  ( 3354240 4586700 ) ( 3366960 * )
      NEW met4 TAPERRULE met4_width_680  ( 3366770 4564590 ) ( * 4586240 )
      NEW met4 TAPERRULE met4_width_680  ( 3354240 4564100 ) ( 3366960 * )
      NEW met4 TAPERRULE met4_width_650  ( 3354415 4564590 ) ( * 4586240 )
      NEW met4  ( 3360585 4575415 ) via4_11690_21950 
      NEW met3 TAPERRULE met3_width_660  ( 3353950 4586720 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16380  ( 3374620 4564590 ) ( * 4586240 )
      NEW met3 TAPERRULE met3_width_700  ( 3353950 4564090 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_940  ( 3354270 4564590 ) ( * 4586240 )
      NEW met3  ( 3360585 4575415 ) via3_11690_21950_hx 
      NEW met4 TAPERRULE met4_width_530  ( 3354200 2373255 ) ( 3366930 * )
      NEW met4 TAPERRULE met4_width_690  ( 3366735 2350120 ) ( * 2372840 )
      NEW met4 TAPERRULE met4_width_470  ( 3354200 2349735 ) ( 3366930 * )
      NEW met4 TAPERRULE met4_width_550  ( 3354325 2350120 ) ( * 2372840 )
      NEW met4  ( 3360495 2361480 ) via4_11790_23020 
      NEW met3 TAPERRULE met3_width_510  ( 3353790 2373245 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_16710  ( 3374745 2350120 ) ( * 2372840 )
      NEW met3 TAPERRULE met3_width_470  ( 3353790 2349735 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_960  ( 3354120 2350120 ) ( * 2372840 )
      NEW met3  ( 3360495 2361480 ) via3_11790_23020_hx 
      NEW met4 TAPERRULE met4_width_670  ( 3354240 2322985 ) ( 3366950 * )
      NEW met4 TAPERRULE met4_width_600  ( 3366800 2300180 ) ( * 2322500 )
      NEW met4 TAPERRULE met4_width_730  ( 3354240 2299665 ) ( 3366950 * )
      NEW met4 TAPERRULE met4_width_710  ( 3354445 2300180 ) ( * 2322500 )
      NEW met4  ( 3360650 2311340 ) via4_11700_22620 
      NEW met3 TAPERRULE met3_width_595  ( 3353790 2322947.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_16600  ( 3374800 2300180 ) ( * 2322500 )
      NEW met3 TAPERRULE met3_width_730  ( 3353790 2299665 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_1160  ( 3354220 2300180 ) ( * 2322500 )
      NEW met3  ( 3360650 2311340 ) via3_11700_22620_hx  ;
   - vccd1 ( user1_vccd_lvclamp_pad VCCD1 )
       ( user1_vssd_lvclamp_pad VCCD1 )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io[1] ( mprj_pads.area1_io_pad\[1\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 733000 ) ( * 794000 ) ;
   - mprj_pads.area1_io_pad\[1\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[1\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[1\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[1\] ENABLE_INP_H ) ;
   - mprj_io_in[1] ( mprj_pads.area1_io_pad\[1\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 730775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[1\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[1\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[1\] TIE_HI_ESD ) ;
   - mprj_io_one[1] ( mprj_pads.area1_io_pad\[1\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 736755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[1] ( mprj_pads.area1_io_pad\[1\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 739975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[1\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[1\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[1\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[1\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[4] ( mprj_pads.area1_io_pad\[1\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 749175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[1\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[1\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[1] ( mprj_pads.area1_io_pad\[1\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 755155 ) ( 3379365 * ) ;
   - mprj_io_dm[3] ( mprj_pads.area1_io_pad\[1\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 758375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[1] ( mprj_pads.area1_io_pad\[1\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 761595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[1] ( mprj_pads.area1_io_pad\[1\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 764355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[1\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[1\] ENABLE_H ) ;
   - mprj_io_analog_sel[1] ( mprj_pads.area1_io_pad\[1\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 776775 ) ( 3379365 * ) ;
   - mprj_io_dm[5] ( mprj_pads.area1_io_pad\[1\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 779995 ) ( 3379365 * ) ;
   - mprj_io_holdover[1] ( mprj_pads.area1_io_pad\[1\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 783215 ) ( 3379365 * ) ;
   - mprj_io_out[1] ( mprj_pads.area1_io_pad\[1\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 785975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[1] ( mprj_pads.area1_io_pad\[1\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 795175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[1]
       ( mprj_pads.area1_io_pad\[1\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 798395 ) ( 3379365 * ) ;
   - mprj_io_oeb[1] ( mprj_pads.area1_io_pad\[1\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 801615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[1] ( mprj_pads.area1_io_pad\[1\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 804375 ) ( 3379365 * ) ;
   - mprj_io[14] ( user1_analog_pad\[3\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 3523530 4765910 ) ( * 4825150 ) ;
   - mprj_analog[0] ( user1_analog_pad\[3\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 3388150 4795780 ) ( 3470200 * ) ;
   - mprj_io[26] ( mprj_pads.area2_io_pad\[1\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[15] ( mprj_pads.area2_io_pad\[1\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3781225 ) ( 210895 * ) ;
   - mprj_io_one[15] ( mprj_pads.area2_io_pad\[1\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3775245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[15] ( mprj_pads.area2_io_pad\[1\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3772025 ) ( 210895 * ) ;
   - mprj_gpio_analog[8] ( mprj_pads.area2_io_pad\[1\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3768805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[1\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[1\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[46] ( mprj_pads.area2_io_pad\[1\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3762825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[8] ( mprj_pads.area2_io_pad\[1\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3759605 ) ( 210895 * ) ;
   - mprj_io_analog_en[15] ( mprj_pads.area2_io_pad\[1\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3756845 ) ( 210895 * ) ;
   - mprj_io_dm[45] ( mprj_pads.area2_io_pad\[1\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3753625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[15] ( mprj_pads.area2_io_pad\[1\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3750405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[15] ( mprj_pads.area2_io_pad\[1\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3747645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[1\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[1\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[1\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[1\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[1\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[15] ( mprj_pads.area2_io_pad\[1\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3735225 ) ( 210895 * ) ;
   - mprj_io_dm[47] ( mprj_pads.area2_io_pad\[1\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3732005 ) ( 210895 * ) ;
   - mprj_io_holdover[15] ( mprj_pads.area2_io_pad\[1\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3728785 ) ( 210895 * ) ;
   - mprj_io_out[15] ( mprj_pads.area2_io_pad\[1\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3726025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[1\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[1\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[1\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[1\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[15] ( mprj_pads.area2_io_pad\[1\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3716825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[15]
       ( mprj_pads.area2_io_pad\[1\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3713605 ) ( 210895 * ) ;
   - mprj_io_oeb[15] ( mprj_pads.area2_io_pad\[1\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3710385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[15] ( mprj_pads.area2_io_pad\[1\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3707625 ) ( 210895 * ) ;
   - mprj_io[36] ( mprj_pads.area2_io_pad\[11\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 211480 2278940 ) ( * 4585710 )
      NEW met5 TAPERRULE met5_width_13000  ( 211480 4609410 ) ( * 4635320 )
      NEW met4 TAPERRULE met4_width_620  ( 205170 4608920 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_650  ( 217685 4586660 ) ( * 4608460 )
      NEW met4 TAPERRULE met4_width_460  ( 205170 4586280 ) ( 217860 * )
      NEW met4 TAPERRULE met4_width_490  ( 205265 4586660 ) ( * 4608460 )
      NEW met4  ( 211435 4597560 ) via4_11850_22100 
      NEW met3 TAPERRULE met3_width_650  ( 203620 4608935 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_16550  ( 225635 4586660 ) ( * 4608460 )
      NEW met3 TAPERRULE met3_width_560  ( 203620 4586230 ) ( 233760 * )
      NEW met3 TAPERRULE met3_width_2040  ( 204490 4586660 ) ( * 4608460 )
      NEW met3  ( 211435 4597560 ) via3_11850_22100_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 2228670 ) ( * 2254540 )
      NEW met4 TAPERRULE met4_width_480  ( 205140 2278380 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_450  ( 217695 2255490 ) ( * 2277990 )
      NEW met4 TAPERRULE met4_width_600  ( 205140 2255040 ) ( 217770 * )
      NEW met4 TAPERRULE met4_width_550  ( 205265 2255490 ) ( * 2277990 )
      NEW met4  ( 211505 2266740 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_560  ( 204850 2278420 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16650  ( 225795 2255490 ) ( * 2277990 )
      NEW met3 TAPERRULE met3_width_585  ( 204850 2255047.5 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_840  ( 205120 2255490 ) ( * 2277990 )
      NEW met3  ( 211505 2266740 ) via3_11930_22800_hx 
      NEW met5 TAPERRULE met5_width_13000  ( 211480 892940 ) ( * 2204270 )
      NEW met4 TAPERRULE met4_width_580  ( 205110 2228160 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_460  ( 217660 2205220 ) ( * 2227720 )
      NEW met4 TAPERRULE met4_width_500  ( 205110 2204820 ) ( 217740 * )
      NEW met4 TAPERRULE met4_width_540  ( 205230 2205220 ) ( * 2227720 )
      NEW met4  ( 211465 2216470 ) via4_11930_22800 
      NEW met3 TAPERRULE met3_width_630  ( 204850 2228185 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_16690  ( 225775 2205220 ) ( * 2227720 )
      NEW met3 TAPERRULE met3_width_570  ( 204850 2204785 ) ( 233970 * )
      NEW met3 TAPERRULE met3_width_800  ( 205100 2205220 ) ( * 2227720 )
      NEW met3  ( 211465 2216470 ) via3_11930_22800_hx  ;
   - mprj_io_in[25] ( mprj_pads.area2_io_pad\[11\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1199225 ) ( 210895 * ) ;
   - mprj_io_one[25] ( mprj_pads.area2_io_pad\[11\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1193245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[25] ( mprj_pads.area2_io_pad\[11\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1190025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[11\]/PAD_A_ESD_0_H
       ( mprj_pads.area2_io_pad\[11\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area2_io_pad\[11\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[11\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[76] ( mprj_pads.area2_io_pad\[11\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1180825 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[11\]/PAD_A_NOESD_H
       ( mprj_pads.area2_io_pad\[11\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[25] ( mprj_pads.area2_io_pad\[11\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1174845 ) ( 210895 * ) ;
   - mprj_io_dm[75] ( mprj_pads.area2_io_pad\[11\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1171625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[25]
       ( mprj_pads.area2_io_pad\[11\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1168405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[25] ( mprj_pads.area2_io_pad\[11\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1165645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[11\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[11\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[11\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[11\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[11\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[25]
       ( mprj_pads.area2_io_pad\[11\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1153225 ) ( 210895 * ) ;
   - mprj_io_dm[77] ( mprj_pads.area2_io_pad\[11\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1150005 ) ( 210895 * ) ;
   - mprj_io_holdover[25] ( mprj_pads.area2_io_pad\[11\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1146785 ) ( 210895 * ) ;
   - mprj_io_out[25] ( mprj_pads.area2_io_pad\[11\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1144025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[11\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[11\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[11\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[11\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[25] ( mprj_pads.area2_io_pad\[11\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1134825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[25]
       ( mprj_pads.area2_io_pad\[11\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1131605 ) ( 210895 * ) ;
   - mprj_io_oeb[25] ( mprj_pads.area2_io_pad\[11\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1128385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[25] ( mprj_pads.area2_io_pad\[11\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1125625 ) ( 210895 * ) ;
   - mprj_io[20] ( user2_analog_pad_with_clamp\[1\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 1159850 5123530 ) ( 1219090 * ) ;
   - mprj_analog[6] ( user2_analog_pad_with_clamp\[1\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_15680  ( 1202540 4995840 ) ( 1273850 * ) ;
   - mprj_clamp_high[2] ( user2_analog_pad_with_clamp\[1\] DRN_HVC )
      + ROUTED met2 TAPERRULE met2_width_23900  ( 1214340 4988070 ) ( * 5013590 ) ;
   - mprj_clamp_low[2]
       ( user2_analog_pad_with_clamp\[1\] SRC_BDY_HVC )
      + ROUTED met2 TAPERRULE met2_width_2050  ( 1152565 4989025 ) ( 1176325 * ) ;
   - vdda2_pad ( user2_vdda_hvclamp_pad VDDA_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 64465 2422850 ) ( * 2482090 ) ;
   - mprj_io[3] ( mprj_pads.area1_io_pad\[3\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 1184000 ) ( * 1245000 ) ;
   - mprj_pads.area1_io_pad\[3\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[3\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[3\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[3\] ENABLE_INP_H ) ;
   - mprj_io_in[3] ( mprj_pads.area1_io_pad\[3\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1181775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[3\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[3\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[3\] TIE_HI_ESD ) ;
   - mprj_io_one[3] ( mprj_pads.area1_io_pad\[3\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1187755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[3] ( mprj_pads.area1_io_pad\[3\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1190975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[3\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[3\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[3\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[3\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[10] ( mprj_pads.area1_io_pad\[3\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1200175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[3\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[3\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[3] ( mprj_pads.area1_io_pad\[3\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1206155 ) ( 3379365 * ) ;
   - mprj_io_dm[9] ( mprj_pads.area1_io_pad\[3\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1209375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[3] ( mprj_pads.area1_io_pad\[3\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1212595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[3] ( mprj_pads.area1_io_pad\[3\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1215355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[3\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[3\] ENABLE_H ) ;
   - mprj_io_analog_sel[3] ( mprj_pads.area1_io_pad\[3\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1227775 ) ( 3379365 * ) ;
   - mprj_io_dm[11] ( mprj_pads.area1_io_pad\[3\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1230995 ) ( 3379365 * ) ;
   - mprj_io_holdover[3] ( mprj_pads.area1_io_pad\[3\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1234215 ) ( 3379365 * ) ;
   - mprj_io_out[3] ( mprj_pads.area1_io_pad\[3\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1236975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[3] ( mprj_pads.area1_io_pad\[3\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1246175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[3]
       ( mprj_pads.area1_io_pad\[3\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1249395 ) ( 3379365 * ) ;
   - mprj_io_oeb[3] ( mprj_pads.area1_io_pad\[3\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1252615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[3] ( mprj_pads.area1_io_pad\[3\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1255375 ) ( 3379365 * ) ;
   - vdda2 ( FILLER_73 VDDA ) ( FILLER_72 VDDA ) ( FILLER_71 VDDA )
       ( FILLER_70 VDDA ) ( FILLER_69 VDDA ) ( FILLER_68 VDDA )
       ( mgmt_vssio_hvclamp_pad\[1\] VDDA ) ( FILLER_66 VDDA )
       ( FILLER_65 VDDA ) ( FILLER_64 VDDA ) ( FILLER_63 VDDA )
       ( FILLER_62 VDDA ) ( FILLER_61 VDDA ) ( FILLER_60 VDDA )
       ( sky130_ef_io__com_bus_slice_10um_1 VDDA )
       ( sky130_ef_io__com_bus_slice_5um_3 VDDA )
       ( user2_analog_pad_with_clamp\[0\] VDDA )
       ( sky130_ef_io__com_bus_slice_5um_2 VDDA ) ( FILLER_57 VDDA )
       ( FILLER_56 VDDA ) ( FILLER_55 VDDA ) ( FILLER_54 VDDA )
       ( FILLER_53 VDDA ) ( FILLER_52 VDDA ) ( FILLER_51 VDDA )
       ( FILLER_50 VDDA ) ( FILLER_49 VDDA )
       ( user2_analog_pad_with_clamp\[1\] VDDA ) ( FILLER_47 VDDA )
       ( FILLER_46 VDDA ) ( FILLER_45 VDDA ) ( FILLER_44 VDDA )
       ( FILLER_43 VDDA ) ( FILLER_42 VDDA )
       ( user2_analog_pad\[0\] VDDA ) ( FILLER_41 VDDA )
       ( FILLER_39 VDDA ) ( FILLER_38 VDDA ) ( FILLER_37 VDDA )
       ( FILLER_36 VDDA ) ( FILLER_35 VDDA ) ( FILLER_34 VDDA )
       ( FILLER_33 VDDA ) ( FILLER_32 VDDA ) ( FILLER_31 VDDA )
       ( FILLER_30 VDDA ) ( FILLER_29 VDDA )
       ( user2_analog_pad\[1\] VDDA ) ( FILLER_27 VDDA )
       ( FILLER_26 VDDA ) ( FILLER_25 VDDA ) ( FILLER_24 VDDA )
       ( FILLER_23 VDDA ) ( FILLER_22 VDDA ) ( FILLER_21 VDDA )
       ( FILLER_20 VDDA ) ( FILLER_19 VDDA ) ( FILLER_18 VDDA )
       ( FILLER_17 VDDA ) ( user2_analog_pad\[2\] VDDA )
       ( FILLER_15 VDDA ) ( FILLER_14 VDDA ) ( FILLER_13 VDDA )
       ( FILLER_12 VDDA ) ( FILLER_11 VDDA ) ( FILLER_10 VDDA )
       ( FILLER_9 VDDA ) ( FILLER_8 VDDA ) ( FILLER_7 VDDA )
       ( FILLER_6 VDDA ) ( user2_corner VDDA ) ( FILLER_5 VDDA )
       ( FILLER_579 VDDA ) ( FILLER_578 VDDA ) ( FILLER_577 VDDA )
       ( FILLER_576 VDDA ) ( FILLER_575 VDDA ) ( FILLER_574 VDDA )
       ( FILLER_573 VDDA ) ( FILLER_572 VDDA ) ( FILLER_571 VDDA )
       ( user2_analog_pad\[3\] VDDA ) ( FILLER_570 VDDA )
       ( FILLER_568 VDDA ) ( FILLER_567 VDDA ) ( FILLER_566 VDDA )
       ( FILLER_565 VDDA ) ( FILLER_564 VDDA ) ( FILLER_563 VDDA )
       ( FILLER_562 VDDA ) ( FILLER_561 VDDA )
       ( user2_vccd_lvclamp_pad VDDA ) ( FILLER_559 VDDA )
       ( FILLER_558 VDDA ) ( FILLER_557 VDDA ) ( FILLER_556 VDDA )
       ( FILLER_555 VDDA ) ( FILLER_554 VDDA ) ( FILLER_553 VDDA )
       ( FILLER_552 VDDA ) ( FILLER_551 VDDA )
       ( mgmt_vddio_hvclamp_pad\[1\] VDDA ) ( FILLER_549 VDDA )
       ( FILLER_548 VDDA ) ( FILLER_547 VDDA ) ( FILLER_546 VDDA )
       ( FILLER_545 VDDA ) ( FILLER_544 VDDA ) ( FILLER_543 VDDA )
       ( FILLER_542 VDDA ) ( FILLER_541 VDDA )
       ( user2_vssa_hvclamp_pad VDDA ) ( FILLER_539 VDDA )
       ( FILLER_538 VDDA ) ( FILLER_537 VDDA ) ( FILLER_536 VDDA )
       ( FILLER_535 VDDA ) ( FILLER_534 VDDA ) ( FILLER_533 VDDA )
       ( FILLER_532 VDDA ) ( FILLER_531 VDDA )
       ( mprj_pads.area2_io_pad\[0\] VDDA ) ( FILLER_529 VDDA )
       ( FILLER_528 VDDA ) ( FILLER_527 VDDA ) ( FILLER_526 VDDA )
       ( FILLER_525 VDDA ) ( FILLER_524 VDDA ) ( FILLER_523 VDDA )
       ( FILLER_522 VDDA ) ( FILLER_521 VDDA )
       ( mprj_pads.area2_io_pad\[1\] VDDA ) ( FILLER_519 VDDA )
       ( FILLER_518 VDDA ) ( FILLER_517 VDDA ) ( FILLER_516 VDDA )
       ( FILLER_515 VDDA ) ( FILLER_514 VDDA ) ( FILLER_513 VDDA )
       ( FILLER_512 VDDA ) ( FILLER_511 VDDA )
       ( mprj_pads.area2_io_pad\[2\] VDDA ) ( FILLER_509 VDDA )
       ( FILLER_508 VDDA ) ( FILLER_507 VDDA ) ( FILLER_506 VDDA )
       ( FILLER_505 VDDA ) ( FILLER_504 VDDA ) ( FILLER_503 VDDA )
       ( FILLER_502 VDDA ) ( FILLER_501 VDDA )
       ( mprj_pads.area2_io_pad\[3\] VDDA ) ( FILLER_499 VDDA )
       ( FILLER_498 VDDA ) ( FILLER_497 VDDA ) ( FILLER_496 VDDA )
       ( FILLER_495 VDDA ) ( FILLER_494 VDDA ) ( FILLER_493 VDDA )
       ( FILLER_492 VDDA ) ( FILLER_491 VDDA )
       ( mprj_pads.area2_io_pad\[4\] VDDA ) ( FILLER_489 VDDA )
       ( FILLER_488 VDDA ) ( FILLER_487 VDDA ) ( FILLER_486 VDDA )
       ( FILLER_485 VDDA ) ( FILLER_484 VDDA ) ( FILLER_483 VDDA )
       ( FILLER_482 VDDA ) ( FILLER_481 VDDA )
       ( mprj_pads.area2_io_pad\[5\] VDDA ) ( FILLER_479 VDDA )
       ( FILLER_478 VDDA ) ( FILLER_477 VDDA ) ( FILLER_476 VDDA )
       ( FILLER_475 VDDA ) ( FILLER_474 VDDA ) ( FILLER_473 VDDA )
       ( FILLER_472 VDDA ) ( FILLER_471 VDDA )
       ( mprj_pads.area2_io_pad\[6\] VDDA ) ( FILLER_469 VDDA )
       ( FILLER_468 VDDA ) ( FILLER_467 VDDA ) ( FILLER_466 VDDA )
       ( FILLER_465 VDDA ) ( FILLER_464 VDDA ) ( FILLER_463 VDDA )
       ( FILLER_462 VDDA ) ( FILLER_461 VDDA )
       ( user2_vdda_hvclamp_pad VDDA ) ( FILLER_459 VDDA )
       ( FILLER_458 VDDA ) ( FILLER_457 VDDA ) ( FILLER_456 VDDA )
       ( FILLER_455 VDDA ) ( FILLER_454 VDDA ) ( FILLER_453 VDDA )
       ( FILLER_452 VDDA ) ( user2_vssd_lvclamp_pad VDDA )
       ( FILLER_SB2 VDDA ) ( FILLER_451 VDDA ) ( FILLER_449 VDDA )
       ( FILLER_448 VDDA ) ( FILLER_447 VDDA ) ( FILLER_446 VDDA )
       ( FILLER_445 VDDA ) ( FILLER_444 VDDA ) ( FILLER_443 VDDA )
       ( FILLER_442 VDDA ) ( FILLER_441 VDDA )
       ( mprj_pads.area2_io_pad\[7\] VDDA ) ( FILLER_439 VDDA )
       ( FILLER_438 VDDA ) ( FILLER_437 VDDA ) ( FILLER_436 VDDA )
       ( FILLER_435 VDDA ) ( FILLER_434 VDDA ) ( FILLER_433 VDDA )
       ( FILLER_432 VDDA ) ( FILLER_431 VDDA )
       ( mprj_pads.area2_io_pad\[8\] VDDA ) ( FILLER_429 VDDA )
       ( FILLER_428 VDDA ) ( FILLER_427 VDDA ) ( FILLER_426 VDDA )
       ( FILLER_425 VDDA ) ( FILLER_424 VDDA ) ( FILLER_423 VDDA )
       ( FILLER_422 VDDA ) ( FILLER_421 VDDA )
       ( mprj_pads.area2_io_pad\[9\] VDDA ) ( FILLER_419 VDDA )
       ( FILLER_418 VDDA ) ( FILLER_417 VDDA ) ( FILLER_416 VDDA )
       ( FILLER_415 VDDA ) ( FILLER_414 VDDA ) ( FILLER_413 VDDA )
       ( FILLER_412 VDDA ) ( FILLER_411 VDDA )
       ( mprj_pads.area2_io_pad\[10\] VDDA ) ( FILLER_409 VDDA )
       ( FILLER_408 VDDA ) ( FILLER_407 VDDA ) ( FILLER_406 VDDA )
       ( FILLER_405 VDDA ) ( FILLER_404 VDDA ) ( FILLER_403 VDDA )
       ( FILLER_402 VDDA ) ( FILLER_401 VDDA )
       ( mprj_pads.area2_io_pad\[11\] VDDA ) ( FILLER_399 VDDA )
       ( FILLER_398 VDDA ) ( FILLER_397 VDDA ) ( FILLER_396 VDDA )
       ( FILLER_395 VDDA ) ( FILLER_394 VDDA ) ( FILLER_393 VDDA )
       ( FILLER_392 VDDA ) ( FILLER_391 VDDA )
       ( mprj_pads.area2_io_pad\[12\] VDDA ) ( FILLER_389 VDDA )
       ( FILLER_388 VDDA ) ( FILLER_387 VDDA ) ( FILLER_386 VDDA )
       ( FILLER_385 VDDA ) ( FILLER_384 VDDA ) ( FILLER_383 VDDA )
       ( FILLER_382 VDDA ) ( FILLER_381 VDDA ) ( FILLER_380 VDDA )
       ( FILLER_379 VDDA ) ( FILLER_378 VDDA ) ( FILLER_377 VDDA )
       ( FILLER_376 VDDA ) ( FILLER_375 VDDA ) ( FILLER_374 VDDA )
      + ROUTED met4 TAPERRULE met4_width_960  ( 181765 2278515 ) ( 184915 * ) ;
   - vssa2 ( FILLER_73 VSSA ) ( FILLER_72 VSSA ) ( FILLER_71 VSSA )
       ( FILLER_70 VSSA ) ( FILLER_69 VSSA ) ( FILLER_68 VSSA )
       ( mgmt_vssio_hvclamp_pad\[1\] VSSA ) ( FILLER_66 VSSA )
       ( FILLER_65 VSSA ) ( FILLER_64 VSSA ) ( FILLER_63 VSSA )
       ( FILLER_62 VSSA ) ( FILLER_61 VSSA ) ( FILLER_60 VSSA )
       ( sky130_ef_io__com_bus_slice_10um_1 VSSA )
       ( sky130_ef_io__com_bus_slice_5um_3 VSSA )
       ( user2_analog_pad_with_clamp\[0\] VSSA )
       ( sky130_ef_io__com_bus_slice_5um_2 VSSA ) ( FILLER_57 VSSA )
       ( FILLER_56 VSSA ) ( FILLER_55 VSSA ) ( FILLER_54 VSSA )
       ( FILLER_53 VSSA ) ( FILLER_52 VSSA ) ( FILLER_51 VSSA )
       ( FILLER_50 VSSA ) ( FILLER_49 VSSA )
       ( user2_analog_pad_with_clamp\[1\] VSSA ) ( FILLER_47 VSSA )
       ( FILLER_46 VSSA ) ( FILLER_45 VSSA ) ( FILLER_44 VSSA )
       ( FILLER_43 VSSA ) ( FILLER_42 VSSA )
       ( user2_analog_pad\[0\] VSSA ) ( FILLER_41 VSSA )
       ( FILLER_39 VSSA ) ( FILLER_38 VSSA ) ( FILLER_37 VSSA )
       ( FILLER_36 VSSA ) ( FILLER_35 VSSA ) ( FILLER_34 VSSA )
       ( FILLER_33 VSSA ) ( FILLER_32 VSSA ) ( FILLER_31 VSSA )
       ( FILLER_30 VSSA ) ( FILLER_29 VSSA )
       ( user2_analog_pad\[1\] VSSA ) ( FILLER_27 VSSA )
       ( FILLER_26 VSSA ) ( FILLER_25 VSSA ) ( FILLER_24 VSSA )
       ( FILLER_23 VSSA ) ( FILLER_22 VSSA ) ( FILLER_21 VSSA )
       ( FILLER_20 VSSA ) ( FILLER_19 VSSA ) ( FILLER_18 VSSA )
       ( FILLER_17 VSSA ) ( user2_analog_pad\[2\] VSSA )
       ( FILLER_15 VSSA ) ( FILLER_14 VSSA ) ( FILLER_13 VSSA )
       ( FILLER_12 VSSA ) ( FILLER_11 VSSA ) ( FILLER_10 VSSA )
       ( FILLER_9 VSSA ) ( FILLER_8 VSSA ) ( FILLER_7 VSSA )
       ( FILLER_6 VSSA ) ( user2_corner VSSA ) ( FILLER_5 VSSA )
       ( FILLER_579 VSSA ) ( FILLER_578 VSSA ) ( FILLER_577 VSSA )
       ( FILLER_576 VSSA ) ( FILLER_575 VSSA ) ( FILLER_574 VSSA )
       ( FILLER_573 VSSA ) ( FILLER_572 VSSA ) ( FILLER_571 VSSA )
       ( user2_analog_pad\[3\] VSSA ) ( FILLER_570 VSSA )
       ( FILLER_568 VSSA ) ( FILLER_567 VSSA ) ( FILLER_566 VSSA )
       ( FILLER_565 VSSA ) ( FILLER_564 VSSA ) ( FILLER_563 VSSA )
       ( FILLER_562 VSSA ) ( FILLER_561 VSSA )
       ( user2_vccd_lvclamp_pad VSSA ) ( FILLER_559 VSSA )
       ( FILLER_558 VSSA ) ( FILLER_557 VSSA ) ( FILLER_556 VSSA )
       ( FILLER_555 VSSA ) ( FILLER_554 VSSA ) ( FILLER_553 VSSA )
       ( FILLER_552 VSSA ) ( FILLER_551 VSSA )
       ( mgmt_vddio_hvclamp_pad\[1\] VSSA ) ( FILLER_549 VSSA )
       ( FILLER_548 VSSA ) ( FILLER_547 VSSA ) ( FILLER_546 VSSA )
       ( FILLER_545 VSSA ) ( FILLER_544 VSSA ) ( FILLER_543 VSSA )
       ( FILLER_542 VSSA ) ( FILLER_541 VSSA )
       ( user2_vssa_hvclamp_pad VSSA ) ( FILLER_539 VSSA )
       ( FILLER_538 VSSA ) ( FILLER_537 VSSA ) ( FILLER_536 VSSA )
       ( FILLER_535 VSSA ) ( FILLER_534 VSSA ) ( FILLER_533 VSSA )
       ( FILLER_532 VSSA ) ( FILLER_531 VSSA )
       ( mprj_pads.area2_io_pad\[0\] VSSA ) ( FILLER_529 VSSA )
       ( FILLER_528 VSSA ) ( FILLER_527 VSSA ) ( FILLER_526 VSSA )
       ( FILLER_525 VSSA ) ( FILLER_524 VSSA ) ( FILLER_523 VSSA )
       ( FILLER_522 VSSA ) ( FILLER_521 VSSA )
       ( mprj_pads.area2_io_pad\[1\] VSSA ) ( FILLER_519 VSSA )
       ( FILLER_518 VSSA ) ( FILLER_517 VSSA ) ( FILLER_516 VSSA )
       ( FILLER_515 VSSA ) ( FILLER_514 VSSA ) ( FILLER_513 VSSA )
       ( FILLER_512 VSSA ) ( FILLER_511 VSSA )
       ( mprj_pads.area2_io_pad\[2\] VSSA ) ( FILLER_509 VSSA )
       ( FILLER_508 VSSA ) ( FILLER_507 VSSA ) ( FILLER_506 VSSA )
       ( FILLER_505 VSSA ) ( FILLER_504 VSSA ) ( FILLER_503 VSSA )
       ( FILLER_502 VSSA ) ( FILLER_501 VSSA )
       ( mprj_pads.area2_io_pad\[3\] VSSA ) ( FILLER_499 VSSA )
       ( FILLER_498 VSSA ) ( FILLER_497 VSSA ) ( FILLER_496 VSSA )
       ( FILLER_495 VSSA ) ( FILLER_494 VSSA ) ( FILLER_493 VSSA )
       ( FILLER_492 VSSA ) ( FILLER_491 VSSA )
       ( mprj_pads.area2_io_pad\[4\] VSSA ) ( FILLER_489 VSSA )
       ( FILLER_488 VSSA ) ( FILLER_487 VSSA ) ( FILLER_486 VSSA )
       ( FILLER_485 VSSA ) ( FILLER_484 VSSA ) ( FILLER_483 VSSA )
       ( FILLER_482 VSSA ) ( FILLER_481 VSSA )
       ( mprj_pads.area2_io_pad\[5\] VSSA ) ( FILLER_479 VSSA )
       ( FILLER_478 VSSA ) ( FILLER_477 VSSA ) ( FILLER_476 VSSA )
       ( FILLER_475 VSSA ) ( FILLER_474 VSSA ) ( FILLER_473 VSSA )
       ( FILLER_472 VSSA ) ( FILLER_471 VSSA )
       ( mprj_pads.area2_io_pad\[6\] VSSA ) ( FILLER_469 VSSA )
       ( FILLER_468 VSSA ) ( FILLER_467 VSSA ) ( FILLER_466 VSSA )
       ( FILLER_465 VSSA ) ( FILLER_464 VSSA ) ( FILLER_463 VSSA )
       ( FILLER_462 VSSA ) ( FILLER_461 VSSA )
       ( user2_vdda_hvclamp_pad VSSA ) ( FILLER_459 VSSA )
       ( FILLER_458 VSSA ) ( FILLER_457 VSSA ) ( FILLER_456 VSSA )
       ( FILLER_455 VSSA ) ( FILLER_454 VSSA ) ( FILLER_453 VSSA )
       ( FILLER_452 VSSA ) ( FILLER_451 VSSA )
       ( user2_vssd_lvclamp_pad VSSA ) ( FILLER_449 VSSA )
       ( FILLER_SB2 VSSA ) ( FILLER_448 VSSA ) ( FILLER_447 VSSA )
       ( FILLER_446 VSSA ) ( FILLER_445 VSSA ) ( FILLER_444 VSSA )
       ( FILLER_443 VSSA ) ( FILLER_442 VSSA ) ( FILLER_441 VSSA )
       ( mprj_pads.area2_io_pad\[7\] VSSA ) ( FILLER_439 VSSA )
       ( FILLER_438 VSSA ) ( FILLER_437 VSSA ) ( FILLER_436 VSSA )
       ( FILLER_435 VSSA ) ( FILLER_434 VSSA ) ( FILLER_433 VSSA )
       ( FILLER_432 VSSA ) ( FILLER_431 VSSA )
       ( mprj_pads.area2_io_pad\[8\] VSSA ) ( FILLER_429 VSSA )
       ( FILLER_428 VSSA ) ( FILLER_427 VSSA ) ( FILLER_426 VSSA )
       ( FILLER_425 VSSA ) ( FILLER_424 VSSA ) ( FILLER_423 VSSA )
       ( FILLER_422 VSSA ) ( FILLER_421 VSSA )
       ( mprj_pads.area2_io_pad\[9\] VSSA ) ( FILLER_419 VSSA )
       ( FILLER_418 VSSA ) ( FILLER_417 VSSA ) ( FILLER_416 VSSA )
       ( FILLER_415 VSSA ) ( FILLER_414 VSSA ) ( FILLER_413 VSSA )
       ( FILLER_412 VSSA ) ( FILLER_411 VSSA )
       ( mprj_pads.area2_io_pad\[10\] VSSA ) ( FILLER_409 VSSA )
       ( FILLER_408 VSSA ) ( FILLER_407 VSSA ) ( FILLER_406 VSSA )
       ( FILLER_405 VSSA ) ( FILLER_404 VSSA ) ( FILLER_403 VSSA )
       ( FILLER_402 VSSA ) ( FILLER_401 VSSA )
       ( mprj_pads.area2_io_pad\[11\] VSSA ) ( FILLER_399 VSSA )
       ( FILLER_398 VSSA ) ( FILLER_397 VSSA ) ( FILLER_396 VSSA )
       ( FILLER_395 VSSA ) ( FILLER_394 VSSA ) ( FILLER_393 VSSA )
       ( FILLER_392 VSSA ) ( FILLER_391 VSSA )
       ( mprj_pads.area2_io_pad\[12\] VSSA ) ( FILLER_389 VSSA )
       ( FILLER_388 VSSA ) ( FILLER_387 VSSA ) ( FILLER_386 VSSA )
       ( FILLER_385 VSSA ) ( FILLER_384 VSSA ) ( FILLER_383 VSSA )
       ( FILLER_382 VSSA ) ( FILLER_381 VSSA ) ( FILLER_380 VSSA )
       ( FILLER_379 VSSA ) ( FILLER_378 VSSA ) ( FILLER_377 VSSA )
       ( FILLER_376 VSSA ) ( FILLER_375 VSSA ) ( FILLER_374 VSSA )
      + ROUTED met4 TAPERRULE met4_width_330  ( 143430 2204150 ) ( * 2278850 ) ;
   - mprj_io[28] ( mprj_pads.area2_io_pad\[3\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[17] ( mprj_pads.area2_io_pad\[3\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3349225 ) ( 210895 * ) ;
   - mprj_io_one[17] ( mprj_pads.area2_io_pad\[3\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3343245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[17] ( mprj_pads.area2_io_pad\[3\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3340025 ) ( 210895 * ) ;
   - mprj_gpio_analog[10]
       ( mprj_pads.area2_io_pad\[3\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3336805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[3\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[3\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[52] ( mprj_pads.area2_io_pad\[3\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3330825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[10] ( mprj_pads.area2_io_pad\[3\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3327605 ) ( 210895 * ) ;
   - mprj_io_analog_en[17] ( mprj_pads.area2_io_pad\[3\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3324845 ) ( 210895 * ) ;
   - mprj_io_dm[51] ( mprj_pads.area2_io_pad\[3\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3321625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[17] ( mprj_pads.area2_io_pad\[3\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3318405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[17] ( mprj_pads.area2_io_pad\[3\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3315645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[3\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[3\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[3\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[3\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[3\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[17] ( mprj_pads.area2_io_pad\[3\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3303225 ) ( 210895 * ) ;
   - mprj_io_dm[53] ( mprj_pads.area2_io_pad\[3\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3300005 ) ( 210895 * ) ;
   - mprj_io_holdover[17] ( mprj_pads.area2_io_pad\[3\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3296785 ) ( 210895 * ) ;
   - mprj_io_out[17] ( mprj_pads.area2_io_pad\[3\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3294025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[3\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[3\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[3\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[3\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[17] ( mprj_pads.area2_io_pad\[3\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3284825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[17]
       ( mprj_pads.area2_io_pad\[3\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3281605 ) ( 210895 * ) ;
   - mprj_io_oeb[17] ( mprj_pads.area2_io_pad\[3\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3278385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[17] ( mprj_pads.area2_io_pad\[3\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 3275625 ) ( 210895 * ) ;
   - vssio_pad2 ( mgmt_vssio_hvclamp_pad\[1\] VSSIO_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 1674850 5123530 ) ( 1734090 * ) ;
   - vddio_pad ( mgmt_vddio_hvclamp_pad\[0\] VDDIO_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 64465 558850 ) ( * 618090 ) ;
   - constant_block_6/one ( constant_block_6 one )
       ( gpio_pad ENABLE_VDDIO )
      + ROUTED met3  ( 2653015 204495 ) ( 2659130 * )
      NEW met3  ( 2652690 204520 ) ( 2652740 * )
      NEW met2  ( 2652635 204620 ) ( 2652795 * )
      NEW met2 TAPERRULE met2_width_260  ( 2652715 204760 ) ( * 210155 )
      NEW met1 TAPERRULE met1_width_260  ( 2581930 210355 ) ( 2652715 * ) via_260_260_hv 
       ( * 210445 ) ( 2652775 * )
      NEW met2  ( 2581730 210355 ) via_260_260_hv 
      NEW met2  ( 2581670 210445 ) ( 2581790 * )
      NEW met1 TAPERRULE met1_width_260  ( 2571880 210355 ) ( 2581530 * )
      NEW met2  ( 2581670 210265 ) ( 2581790 * )
      NEW met2  ( 2652715 204495 ) via2_300_300_vx 
      NEW met2  ( 2652635 204370 ) ( 2652795 * )
      NEW met3  ( 2652690 204470 ) ( 2652740 * )
      NEW met3  ( 2652690 204495 ) ( 2652415 * ) ;
   - mprj_io[5] ( mprj_pads.area1_io_pad\[5\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 1634000 ) ( * 1695000 ) ;
   - mprj_pads.area1_io_pad\[5\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[5\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[5\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[5\] ENABLE_INP_H ) ;
   - mprj_io_in[5] ( mprj_pads.area1_io_pad\[5\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1631775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[5\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[5\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[5\] TIE_HI_ESD ) ;
   - mprj_io_one[5] ( mprj_pads.area1_io_pad\[5\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1637755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[5] ( mprj_pads.area1_io_pad\[5\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1640975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[5\]/PAD_A_ESD_0_H
       ( mprj_pads.area1_io_pad\[5\] PAD_A_ESD_0_H ) ;
   - mprj_pads.area1_io_pad\[5\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[5\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[16] ( mprj_pads.area1_io_pad\[5\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1650175 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[5\]/PAD_A_NOESD_H
       ( mprj_pads.area1_io_pad\[5\] PAD_A_NOESD_H ) ;
   - mprj_io_analog_en[5] ( mprj_pads.area1_io_pad\[5\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1656155 ) ( 3379365 * ) ;
   - mprj_io_dm[15] ( mprj_pads.area1_io_pad\[5\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1659375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[5] ( mprj_pads.area1_io_pad\[5\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1662595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[5] ( mprj_pads.area1_io_pad\[5\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1665355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[5\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[5\] ENABLE_H ) ;
   - mprj_io_analog_sel[5] ( mprj_pads.area1_io_pad\[5\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1677775 ) ( 3379365 * ) ;
   - mprj_io_dm[17] ( mprj_pads.area1_io_pad\[5\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1680995 ) ( 3379365 * ) ;
   - mprj_io_holdover[5] ( mprj_pads.area1_io_pad\[5\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1684215 ) ( 3379365 * ) ;
   - mprj_io_out[5] ( mprj_pads.area1_io_pad\[5\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1686975 ) ( 3379365 * ) ;
   - mprj_io_vtrip_sel[5] ( mprj_pads.area1_io_pad\[5\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1696175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[5]
       ( mprj_pads.area1_io_pad\[5\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1699395 ) ( 3379365 * ) ;
   - mprj_io_oeb[5] ( mprj_pads.area1_io_pad\[5\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1702615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[5] ( mprj_pads.area1_io_pad\[5\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 1705375 ) ( 3379365 * ) ;
   - mprj_io[21] ( user2_analog_pad\[0\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 907850 5123530 ) ( 967090 * ) ;
   - mprj_analog[7] ( user2_analog_pad\[0\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 937220 4988150 ) ( * 5070200 ) ;
   - mprj_io[30] ( mprj_pads.area2_io_pad\[5\] PAD )
      + ROUTED met5 TAPERRULE met5_width_13000  ( 3376600 673680 ) ( * 2324550 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 2348180 ) ( * 4538130 )
      NEW met5 TAPERRULE met5_width_13000  ( 3376600 4562500 ) ( * 4588410 )
      NEW met5  ( 3370900 4612730 ) ( 3382300 * )
      NEW met4 TAPERRULE met4_width_600  ( 3370200 4612280 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_790  ( 3382705 4589360 ) ( * 4611830 )
      NEW met4 TAPERRULE met4_width_740  ( 3370200 4588840 ) ( 3382950 * )
      NEW met4 TAPERRULE met4_width_630  ( 3370365 4589360 ) ( * 4611830 )
      NEW met4  ( 3376495 4600595 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_520  ( 3353950 4612240 ) ( 3382660 * )
      NEW met3  ( 3353950 4612360 ) ( 3382055 * )
      NEW met3 TAPERRULE met3_width_500  ( 3382560 4589360 ) ( * 4611830 )
      NEW met3 TAPERRULE met3_width_710  ( 3353950 4588855 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_16880  ( 3362240 4589360 ) ( * 4611830 )
      NEW met3  ( 3376495 4600595 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_690  ( 3370280 4562045 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_730  ( 3382815 4539080 ) ( * 4561550 )
      NEW met4 TAPERRULE met4_width_650  ( 3370280 4538605 ) ( 3383030 * )
      NEW met4 TAPERRULE met4_width_690  ( 3370475 4539080 ) ( * 4561550 )
      NEW met4  ( 3376635 4550315 ) via4_11630_22770 
      NEW met3 TAPERRULE met3_width_545  ( 3353950 4561972.5 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_360  ( 3382630 4539080 ) ( * 4561550 )
      NEW met3 TAPERRULE met3_width_630  ( 3353950 4538615 ) ( 3382660 * )
      NEW met3 TAPERRULE met3_width_17020  ( 3362310 4539080 ) ( * 4561550 )
      NEW met3  ( 3376635 4550315 ) via3_11630_22770_hx 
      NEW met4 TAPERRULE met4_width_620  ( 3370250 2347690 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_630  ( 3382825 2325500 ) ( * 2347230 )
      NEW met4 TAPERRULE met4_width_630  ( 3370250 2325035 ) ( 3382990 * )
      NEW met4 TAPERRULE met4_width_590  ( 3370395 2325500 ) ( * 2347230 )
      NEW met4  ( 3376600 2336365 ) via4_11820_22030 
      NEW met3 TAPERRULE met3_width_620  ( 3353790 2347690 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_590  ( 3382805 2325500 ) ( * 2347230 )
      NEW met3 TAPERRULE met3_width_605  ( 3353790 2325047.5 ) ( 3382950 * )
      NEW met3 TAPERRULE met3_width_17050  ( 3362165 2325500 ) ( * 2347230 )
      NEW met3  ( 3376600 2336365 ) via3_11820_22030_hx  ;
   - mprj_io_in[19] ( mprj_pads.area2_io_pad\[5\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2917225 ) ( 210895 * ) ;
   - mprj_io_one[19] ( mprj_pads.area2_io_pad\[5\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2911245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[19] ( mprj_pads.area2_io_pad\[5\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2908025 ) ( 210895 * ) ;
   - mprj_gpio_analog[12]
       ( mprj_pads.area2_io_pad\[5\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2904805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[5\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[5\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[58] ( mprj_pads.area2_io_pad\[5\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2898825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[12] ( mprj_pads.area2_io_pad\[5\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2895605 ) ( 210895 * ) ;
   - mprj_io_analog_en[19] ( mprj_pads.area2_io_pad\[5\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2892845 ) ( 210895 * ) ;
   - mprj_io_dm[57] ( mprj_pads.area2_io_pad\[5\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2889625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[19] ( mprj_pads.area2_io_pad\[5\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2886405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[19] ( mprj_pads.area2_io_pad\[5\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2883645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[5\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[5\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[5\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[5\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[5\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[19] ( mprj_pads.area2_io_pad\[5\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2871225 ) ( 210895 * ) ;
   - mprj_io_dm[59] ( mprj_pads.area2_io_pad\[5\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2868005 ) ( 210895 * ) ;
   - mprj_io_holdover[19] ( mprj_pads.area2_io_pad\[5\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2864785 ) ( 210895 * ) ;
   - mprj_io_out[19] ( mprj_pads.area2_io_pad\[5\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2862025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[5\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[5\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[5\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[5\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[19] ( mprj_pads.area2_io_pad\[5\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2852825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[19]
       ( mprj_pads.area2_io_pad\[5\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2849605 ) ( 210895 * ) ;
   - mprj_io_oeb[19] ( mprj_pads.area2_io_pad\[5\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2846385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[19] ( mprj_pads.area2_io_pad\[5\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2843625 ) ( 210895 * ) ;
   - constant_block_5/one ( constant_block_5 one )
       ( flash_io1_pad ENABLE_VDDIO )
      + ROUTED met3  ( 2379015 204495 ) ( 2385125 * )
      NEW met3  ( 2378690 204520 ) ( 2378740 * )
      NEW met2  ( 2378635 204620 ) ( 2378795 * )
      NEW met2 TAPERRULE met2_width_260  ( 2378715 204760 ) ( * 210155 )
      NEW met1 TAPERRULE met1_width_260  ( 2307950 210355 ) ( 2378715 * ) via_260_260_hv 
       ( * 210445 ) ( 2378775 * )
      NEW met2  ( 2307750 210355 ) via_260_260_hv 
      NEW met2  ( 2307690 210445 ) ( 2307810 * )
      NEW met1 TAPERRULE met1_width_260  ( 2297880 210355 ) ( 2307550 * )
      NEW met2  ( 2307690 210265 ) ( 2307810 * )
      NEW met2  ( 2378715 204495 ) via2_300_300_vx 
      NEW met2  ( 2378635 204370 ) ( 2378795 * )
      NEW met3  ( 2378690 204470 ) ( 2378740 * )
      NEW met3  ( 2378690 204495 ) ( 2378415 * ) ;
   - constant_block_4/one ( constant_block_4 one )
       ( flash_io0_pad ENABLE_VDDIO )
      + ROUTED met3  ( 2105015 204495 ) ( 2111160 * )
      NEW met3  ( 2104690 204520 ) ( 2104740 * )
      NEW met2  ( 2104635 204620 ) ( 2104795 * )
      NEW met2 TAPERRULE met2_width_260  ( 2104715 204760 ) ( * 210155 )
      NEW met1 TAPERRULE met1_width_260  ( 2033925 210355 ) ( 2104715 * ) via_260_260_hv 
       ( * 210445 ) ( 2104775 * )
      NEW met2  ( 2033725 210355 ) via_260_260_hv 
      NEW met2  ( 2033665 210445 ) ( 2033785 * )
      NEW met1 TAPERRULE met1_width_260  ( 2023880 210355 ) ( 2033525 * )
      NEW met2  ( 2033665 210265 ) ( 2033785 * )
      NEW met2  ( 2104715 204495 ) via2_300_300_vx 
      NEW met2  ( 2104635 204370 ) ( 2104795 * )
      NEW met3  ( 2104690 204470 ) ( 2104740 * )
      NEW met3  ( 2104690 204495 ) ( 2104415 * ) ;
   - mprj_io[11] ( mprj_pads.area1_io_pad\[11\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 3648000 ) ( * 3709000 ) ;
   - mprj_pads.area1_io_pad\[11\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[11\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[11\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[11\] ENABLE_INP_H ) ;
   - mprj_io_in[11] ( mprj_pads.area1_io_pad\[11\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3645775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[11\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[11\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[11\] TIE_HI_ESD ) ;
   - mprj_io_one[11] ( mprj_pads.area1_io_pad\[11\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3651755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[11] ( mprj_pads.area1_io_pad\[11\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3654975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[4]
       ( mprj_pads.area1_io_pad\[11\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3658195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[11\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[11\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[34] ( mprj_pads.area1_io_pad\[11\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3664175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[4] ( mprj_pads.area1_io_pad\[11\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3667395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[11] ( mprj_pads.area1_io_pad\[11\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3670155 ) ( 3379365 * ) ;
   - mprj_io_dm[33] ( mprj_pads.area1_io_pad\[11\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3673375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[11]
       ( mprj_pads.area1_io_pad\[11\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3676595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[11] ( mprj_pads.area1_io_pad\[11\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3679355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[11\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[11\] ENABLE_H ) ;
   - mprj_io_analog_sel[11]
       ( mprj_pads.area1_io_pad\[11\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3691775 ) ( 3379365 * ) ;
   - mprj_io_dm[35] ( mprj_pads.area1_io_pad\[11\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3694995 ) ( 3379365 * ) ;
   - mprj_io_holdover[11] ( mprj_pads.area1_io_pad\[11\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3698215 ) ( 3379365 * ) ;
   - mprj_io_out[11] ( mprj_pads.area1_io_pad\[11\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3700975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[11\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[11\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[11] ( mprj_pads.area1_io_pad\[11\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3710175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[11]
       ( mprj_pads.area1_io_pad\[11\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3713395 ) ( 3379365 * ) ;
   - mprj_io_oeb[11] ( mprj_pads.area1_io_pad\[11\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3716615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[11] ( mprj_pads.area1_io_pad\[11\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 3719375 ) ( 3379365 * ) ;
   - flash_clk_pad/DM[2] ( flash_clk_pad DM[2] )
       ( flash_clk_pad DM[1] ) ( constant_block_3 one )
       ( flash_clk_pad ENABLE_VDDIO )
      + ROUTED met2  ( 1802980 210355 ) via_260_260_hv 
      NEW met2  ( 1802920 210445 ) ( 1803040 * )
      NEW met1 TAPERRULE met1_width_260  ( 1772360 210355 ) ( 1802780 * )
      NEW met1  ( 1772160 210355 ) via_260_260_hv  ( * 210445 )
       ( 1772220 * )
      NEW met1 TAPERRULE met1_width_260  ( 1759955 210355 ) ( 1771960 * )
      NEW met1  ( 1759755 210355 ) via_260_260_hv  ( * 210445 )
       ( 1759815 * )
      NEW met1 TAPERRULE met1_width_260  ( 1749880 210355 ) ( 1759555 * )
      NEW met2  ( 1759695 210265 ) ( 1759815 * )
      NEW met2  ( 1772100 210265 ) ( 1772220 * )
      NEW met2  ( 1802920 210265 ) ( 1803040 * )
      NEW met1 TAPERRULE met1_width_260  ( 1803180 210355 ) ( 1830715 * ) via_260_260_hv 
       ( * 210445 ) ( 1830775 * )
      NEW met2 TAPERRULE met2_width_260  ( 1830715 204760 ) ( * 210155 )
      NEW met2  ( 1830635 204620 ) ( 1830795 * )
      NEW met2  ( 1830715 204495 ) via2_300_300_vx 
      NEW met3  ( 1830690 204520 ) ( 1830740 * )
      NEW met3  ( 1831015 204495 ) ( 1837270 * )
      NEW met3  ( 1830690 204470 ) ( 1830740 * )
      NEW met3  ( 1830690 204495 ) ( 1830415 * )
      NEW met2  ( 1830635 204370 ) ( 1830795 * ) ;
   - mprj_io[7] ( mprj_pads.area1_io_pad\[7\] PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 3523785 2746000 ) ( * 2807000 ) ;
   - mprj_pads.area1_io_pad\[7\]/TIE_LO_ESD
       ( mprj_pads.area1_io_pad\[7\] TIE_LO_ESD )
       ( mprj_pads.area1_io_pad\[7\] ENABLE_VSWITCH_H )
       ( mprj_pads.area1_io_pad\[7\] ENABLE_INP_H ) ;
   - mprj_io_in[7] ( mprj_pads.area1_io_pad\[7\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2743775 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[7\]/HLD_H_N
       ( mprj_pads.area1_io_pad\[7\] HLD_H_N )
       ( mprj_pads.area1_io_pad\[7\] TIE_HI_ESD ) ;
   - mprj_io_one[7] ( mprj_pads.area1_io_pad\[7\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2749755 ) ( 3379365 * ) ;
   - mprj_io_slow_sel[7] ( mprj_pads.area1_io_pad\[7\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2752975 ) ( 3379365 * ) ;
   - mprj_gpio_analog[0] ( mprj_pads.area1_io_pad\[7\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2756195 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[7\]/PAD_A_ESD_1_H
       ( mprj_pads.area1_io_pad\[7\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[22] ( mprj_pads.area1_io_pad\[7\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2762175 ) ( 3379365 * ) ;
   - mprj_gpio_noesd[0] ( mprj_pads.area1_io_pad\[7\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2765395 ) ( 3379365 * ) ;
   - mprj_io_analog_en[7] ( mprj_pads.area1_io_pad\[7\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2768155 ) ( 3379365 * ) ;
   - mprj_io_dm[21] ( mprj_pads.area1_io_pad\[7\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2771375 ) ( 3379365 * ) ;
   - mprj_io_analog_pol[7] ( mprj_pads.area1_io_pad\[7\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2774595 ) ( 3379365 * ) ;
   - mprj_io_inp_dis[7] ( mprj_pads.area1_io_pad\[7\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2777355 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[7\]/ENABLE_H
       ( mprj_pads.area1_io_pad\[7\] ENABLE_H ) ;
   - mprj_io_analog_sel[7] ( mprj_pads.area1_io_pad\[7\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2789775 ) ( 3379365 * ) ;
   - mprj_io_dm[23] ( mprj_pads.area1_io_pad\[7\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2792995 ) ( 3379365 * ) ;
   - mprj_io_holdover[7] ( mprj_pads.area1_io_pad\[7\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2796215 ) ( 3379365 * ) ;
   - mprj_io_out[7] ( mprj_pads.area1_io_pad\[7\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2798975 ) ( 3379365 * ) ;
   - mprj_pads.area1_io_pad\[7\]/ENABLE_VDDA_H
       ( mprj_pads.area1_io_pad\[7\] ENABLE_VDDA_H ) ;
   - mprj_io_vtrip_sel[7] ( mprj_pads.area1_io_pad\[7\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2808175 ) ( 3379365 * ) ;
   - mprj_io_ib_mode_sel[7]
       ( mprj_pads.area1_io_pad\[7\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2811395 ) ( 3379365 * ) ;
   - mprj_io_oeb[7] ( mprj_pads.area1_io_pad\[7\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2814615 ) ( 3379365 * ) ;
   - mprj_io_in_3v3[7] ( mprj_pads.area1_io_pad\[7\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 3377105 2817375 ) ( 3379365 * ) ;
   - mprj_io[23] ( user2_analog_pad\[2\] P_PAD )
      + ROUTED met5 TAPERRULE met5_width_60820  ( 393850 5123530 ) ( 453090 * ) ;
   - mprj_analog[9] ( user2_analog_pad\[2\] P_CORE )
      + ROUTED met3 TAPERRULE met3_width_25000  ( 423220 4988150 ) ( * 5070200 ) ;
   - flash_csb_pad/DM[2] ( flash_csb_pad DM[2] )
       ( flash_csb_pad DM[1] ) ( constant_block_2 one )
       ( flash_csb_pad ENABLE_VDDIO )
      + ROUTED met2  ( 1529000 210355 ) via_260_260_hv 
      NEW met2  ( 1528940 210445 ) ( 1529060 * )
      NEW met1 TAPERRULE met1_width_260  ( 1498365 210355 ) ( 1528800 * )
      NEW met1  ( 1498165 210355 ) via_260_260_hv  ( * 210445 )
       ( 1498225 * )
      NEW met1 TAPERRULE met1_width_260  ( 1485955 210355 ) ( 1497965 * )
      NEW met1  ( 1485755 210355 ) via_260_260_hv  ( * 210445 )
       ( 1485815 * )
      NEW met1 TAPERRULE met1_width_260  ( 1475880 210355 ) ( 1485555 * )
      NEW met2  ( 1485695 210265 ) ( 1485815 * )
      NEW met2  ( 1498105 210265 ) ( 1498225 * )
      NEW met2  ( 1528940 210265 ) ( 1529060 * )
      NEW met1 TAPERRULE met1_width_260  ( 1529200 210355 ) ( 1556715 * ) via_260_260_hv 
       ( * 210445 ) ( 1556775 * )
      NEW met2 TAPERRULE met2_width_260  ( 1556715 204760 ) ( * 210155 )
      NEW met2  ( 1556635 204620 ) ( 1556795 * )
      NEW met2  ( 1556715 204495 ) via2_300_300_vx 
      NEW met3  ( 1556690 204520 ) ( 1556740 * )
      NEW met3  ( 1557015 204495 ) ( 1563270 * )
      NEW met3  ( 1556690 204470 ) ( 1556740 * )
      NEW met3  ( 1556690 204495 ) ( 1556415 * )
      NEW met2  ( 1556635 204370 ) ( 1556795 * ) ;
   - mprj_io[32] ( mprj_pads.area2_io_pad\[7\] PAD ) ;
   - mprj_io_in[21] ( mprj_pads.area2_io_pad\[7\] IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2063225 ) ( 210895 * ) ;
   - mprj_io_one[21] ( mprj_pads.area2_io_pad\[7\] ENABLE_VDDIO )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2057245 ) ( 210895 * ) ;
   - mprj_io_slow_sel[21] ( mprj_pads.area2_io_pad\[7\] SLOW )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2054025 ) ( 210895 * ) ;
   - mprj_gpio_analog[14]
       ( mprj_pads.area2_io_pad\[7\] PAD_A_ESD_0_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2050805 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[7\]/PAD_A_ESD_1_H
       ( mprj_pads.area2_io_pad\[7\] PAD_A_ESD_1_H ) ;
   - mprj_io_dm[64] ( mprj_pads.area2_io_pad\[7\] DM[1] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2044825 ) ( 210895 * ) ;
   - mprj_gpio_noesd[14] ( mprj_pads.area2_io_pad\[7\] PAD_A_NOESD_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2041605 ) ( 210895 * ) ;
   - mprj_io_analog_en[21] ( mprj_pads.area2_io_pad\[7\] ANALOG_EN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2038845 ) ( 210895 * ) ;
   - mprj_io_dm[63] ( mprj_pads.area2_io_pad\[7\] DM[0] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2035625 ) ( 210895 * ) ;
   - mprj_io_analog_pol[21] ( mprj_pads.area2_io_pad\[7\] ANALOG_POL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2032405 ) ( 210895 * ) ;
   - mprj_io_inp_dis[21] ( mprj_pads.area2_io_pad\[7\] INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2029645 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[7\]/ENABLE_H
       ( mprj_pads.area2_io_pad\[7\] ENABLE_H ) ;
   - mprj_pads.area2_io_pad\[7\]/HLD_H_N
       ( mprj_pads.area2_io_pad\[7\] HLD_H_N )
       ( mprj_pads.area2_io_pad\[7\] TIE_HI_ESD ) ;
   - mprj_io_analog_sel[21] ( mprj_pads.area2_io_pad\[7\] ANALOG_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2017225 ) ( 210895 * ) ;
   - mprj_io_dm[65] ( mprj_pads.area2_io_pad\[7\] DM[2] )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2014005 ) ( 210895 * ) ;
   - mprj_io_holdover[21] ( mprj_pads.area2_io_pad\[7\] HLD_OVR )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2010785 ) ( 210895 * ) ;
   - mprj_io_out[21] ( mprj_pads.area2_io_pad\[7\] OUT )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 2008025 ) ( 210895 * ) ;
   - mprj_pads.area2_io_pad\[7\]/TIE_LO_ESD
       ( mprj_pads.area2_io_pad\[7\] TIE_LO_ESD )
       ( mprj_pads.area2_io_pad\[7\] ENABLE_INP_H )
       ( mprj_pads.area2_io_pad\[7\] ENABLE_VSWITCH_H ) ;
   - mprj_io_vtrip_sel[21] ( mprj_pads.area2_io_pad\[7\] VTRIP_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1998825 ) ( 210895 * ) ;
   - mprj_io_ib_mode_sel[21]
       ( mprj_pads.area2_io_pad\[7\] IB_MODE_SEL )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1995605 ) ( 210895 * ) ;
   - mprj_io_oeb[21] ( mprj_pads.area2_io_pad\[7\] OE_N )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1992385 ) ( 210895 * ) ;
   - mprj_io_in_3v3[21] ( mprj_pads.area2_io_pad\[7\] IN_H )
      + ROUTED met2 TAPERRULE met2_width_280  ( 208635 1989625 ) ( 210895 * ) ;
   - vccd_pad ( mgmt_vccd_lvclamp_pad VCCD_PAD )
      + ROUTED met5 TAPERRULE met5_width_54400  ( 31635 377470 ) ( 97295 * ) ;
   - clock ( clock_pad PAD )
      + ROUTED met5 TAPERRULE met5_width_62450  ( 939000 64215 ) ( 1000000 * ) ;
   - clock_pad/TIE_LO_ESD ( clock_pad TIE_LO_ESD )
       ( clock_pad ENABLE_VSWITCH_H ) ( clock_pad ENABLE_INP_H )
      + ROUTED met2  ( 933545 209095 ) via_260_260_hv 
      NEW met2  ( 933485 209185 ) ( 933605 * )
      NEW met1 TAPERRULE met1_width_260  ( 932810 209095 ) ( 933345 * )
      NEW met2  ( 933485 209005 ) ( 933605 * )
      NEW met1 TAPERRULE met1_width_260  ( 933745 209095 ) ( 973570 * ) via_260_260_hv 
       ( * 209185 ) ( 973630 * )
      NEW met2  ( 973510 209005 ) ( 973630 * )
      NEW met1 TAPERRULE met1_width_260  ( 973770 209095 ) ( 995190 * ) via_260_260_hv 
       ( * 209185 ) ( 995250 * )
      NEW met2  ( 995130 209005 ) ( 995250 * )
      NEW met1 TAPERRULE met1_width_260  ( 995390 209095 ) ( 1010740 * ) ;
   - clock_core ( clock_pad IN )
      + ROUTED met2 TAPERRULE met2_width_280  ( 936775 208635 ) ( * 210895 ) ;
   - clock_pad/HLD_H_N ( clock_pad HLD_H_N ) ( clock_pad TIE_HI_ESD )
      + ROUTED met2  ( 979995 209515 ) via_260_260_hv 
      NEW met2  ( 979935 209605 ) ( 980055 * )
      NEW met1 TAPERRULE met1_width_260  ( 940170 209515 ) ( 979795 * )
      NEW met1  ( 939970 209515 ) via_260_260_hv  ( * 209605 )
       ( 940030 * )
      NEW met1 TAPERRULE met1_width_260  ( 932810 209515 ) ( 939770 * )
      NEW met2  ( 939910 209425 ) ( 940030 * )
      NEW met2  ( 979935 209425 ) ( 980055 * )
      NEW met1 TAPERRULE met1_width_260  ( 980195 209515 ) ( 1010740 * ) ;
   - clock_pad/OUT ( clock_pad OUT ) ( constant_block_1 zero )
       ( clock_pad IB_MODE_SEL ) ( clock_pad VTRIP_SEL )
       ( clock_pad SLOW ) ( clock_pad HLD_OVR ) ( clock_pad DM[2] )
       ( clock_pad ANALOG_SEL ) ( clock_pad ANALOG_POL )
       ( clock_pad ANALOG_EN ) ( clock_pad DM[1] )
      + ROUTED met2  ( 991970 209935 ) via_260_260_hv 
      NEW met2  ( 991910 210025 ) ( 992030 * )
      NEW met1 TAPERRULE met1_width_260  ( 989395 209935 ) ( 991770 * )
      NEW met1  ( 989195 209935 ) via_260_260_hv  ( * 210025 )
       ( 989255 * )
      NEW met1 TAPERRULE met1_width_260  ( 986180 209935 ) ( 988995 * )
      NEW met1  ( 985980 209935 ) via_260_260_hv  ( * 210025 )
       ( 986040 * )
      NEW met1 TAPERRULE met1_width_260  ( 982970 209935 ) ( 985780 * )
      NEW met1  ( 982770 209935 ) via_260_260_hv  ( * 210025 )
       ( 982830 * )
      NEW met1 TAPERRULE met1_width_260  ( 967775 209935 ) ( 982570 * )
      NEW met1  ( 967575 209935 ) via_260_260_hv  ( * 210025 )
       ( 967635 * )
      NEW met1 TAPERRULE met1_width_260  ( 961340 209935 ) ( 967375 * )
      NEW met1  ( 961140 209935 ) via_260_260_hv  ( * 210025 )
       ( 961200 * )
      NEW met1 TAPERRULE met1_width_260  ( 955345 209935 ) ( 960940 * )
      NEW met1  ( 955145 209935 ) via_260_260_hv  ( * 210025 )
       ( 955205 * )
      NEW met1 TAPERRULE met1_width_260  ( 946145 209935 ) ( 954945 * )
      NEW met1  ( 945945 209935 ) via_260_260_hv  ( * 210025 )
       ( 946005 * )
      NEW met1 TAPERRULE met1_width_260  ( 932810 209935 ) ( 945745 * )
      NEW met2  ( 945885 209845 ) ( 946005 * )
      NEW met2  ( 955085 209845 ) ( 955205 * )
      NEW met2  ( 961080 209845 ) ( 961200 * )
      NEW met2  ( 967515 209845 ) ( 967635 * )
      NEW met2  ( 982710 209845 ) ( 982830 * )
      NEW met2  ( 985920 209845 ) ( 986040 * )
      NEW met2  ( 989135 209845 ) ( 989255 * )
      NEW met2  ( 991910 209845 ) ( 992030 * )
      NEW met1 TAPERRULE met1_width_260  ( 992170 209935 ) ( 1001160 * ) via_260_260_hv 
       ( * 210025 ) ( 1001220 * )
      NEW met2  ( 1001100 209845 ) ( 1001220 * )
      NEW met1 TAPERRULE met1_width_260  ( 1001360 209935 ) ( 1004415 * ) via_260_260_hv 
       ( * 210025 ) ( 1004475 * )
      NEW met2  ( 1004355 209845 ) ( 1004475 * )
      NEW met1 TAPERRULE met1_width_260  ( 1004615 209935 ) ( 1029760 * ) via_260_260_hv 
       ( * 210025 ) ( 1029820 * )
      NEW met2 TAPERRULE met2_width_260  ( 1029760 204705 ) ( * 209735 )
      NEW met2  ( 1029680 204565 ) ( 1029840 * )
      NEW met2  ( 1029760 204440 ) via2_300_300_vx 
      NEW met3  ( 1028970 204460 ) ( 1029790 * )
      NEW met3  ( 1029735 204465 ) ( 1029785 * )
      NEW met3  ( 1029735 204415 ) ( 1029785 * )
      NEW met3  ( 1028970 204460 ) ( 1029460 * )
      NEW met2  ( 1029680 204315 ) ( 1029840 * ) ;
   - clock_pad/PAD_A_ESD_0_H ( clock_pad PAD_A_ESD_0_H ) ;
   - clock_pad/PAD_A_ESD_1_H ( clock_pad PAD_A_ESD_1_H ) ;
   - clock_pad/PAD_A_NOESD_H ( clock_pad PAD_A_NOESD_H ) ;
   - por ( clock_pad INP_DIS )
      + ROUTED met2 TAPERRULE met2_width_280  ( 970355 208635 ) ( * 210895 ) ;
   - clock_pad/IN_H ( clock_pad IN_H ) ;
END NETS

END DESIGN

