VERSION 5.8 ;
DIVIDERCHAR "/" ;
BUSBITCHARS "[]" ;
DESIGN gpio_control_block ;
UNITS DISTANCE MICRONS 1000 ;
DIEAREA ( 0 0 ) ( 170000 65000 ) ;
ROW ROW_1_2 unithd 15180 8160 FS DO 74 BY 1 STEP 460 0 ;
ROW ROW_2_2 unithd 15180 10880 N DO 74 BY 1 STEP 460 0 ;
ROW ROW_3_2 unithd 15180 13600 FS DO 74 BY 1 STEP 460 0 ;
ROW ROW_4_2 unithd 15180 16320 N DO 74 BY 1 STEP 460 0 ;
ROW ROW_5_2 unithd 15180 19040 FS DO 74 BY 1 STEP 460 0 ;
ROW ROW_6_2 unithd 15180 21760 N DO 74 BY 1 STEP 460 0 ;
ROW ROW_7_2 unithd 15180 24480 FS DO 74 BY 1 STEP 460 0 ;
ROW ROW_8 unithd 4600 27200 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_9 unithd 4600 29920 FS DO 97 BY 1 STEP 460 0 ;
ROW ROW_10 unithd 4600 32640 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_11 unithd 4600 35360 FS DO 97 BY 1 STEP 460 0 ;
ROW ROW_12 unithd 4600 38080 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_13 unithd 4600 40800 FS DO 97 BY 1 STEP 460 0 ;
ROW ROW_14 unithd 4600 43520 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_15 unithd 4600 46240 FS DO 97 BY 1 STEP 460 0 ;
ROW ROW_16 unithd 4600 48960 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_17 unithd 4600 51680 FS DO 97 BY 1 STEP 460 0 ;
ROW ROW_18 unithd 4600 54400 N DO 97 BY 1 STEP 460 0 ;
ROW ROW_0_2 unithd 15180 5440 N DO 74 BY 1 STEP 460 0 ;
TRACKS X 230 DO 370 STEP 460 LAYER li1 ;
TRACKS Y 170 DO 191 STEP 340 LAYER li1 ;
TRACKS X 170 DO 500 STEP 340 LAYER met1 ;
TRACKS Y 170 DO 191 STEP 340 LAYER met1 ;
TRACKS X 230 DO 370 STEP 460 LAYER met2 ;
TRACKS Y 230 DO 141 STEP 460 LAYER met2 ;
TRACKS X 340 DO 250 STEP 680 LAYER met3 ;
TRACKS Y 340 DO 96 STEP 680 LAYER met3 ;
TRACKS X 460 DO 185 STEP 920 LAYER met4 ;
TRACKS Y 460 DO 71 STEP 920 LAYER met4 ;
TRACKS X 1700 DO 50 STEP 3400 LAYER met5 ;
TRACKS Y 1700 DO 19 STEP 3400 LAYER met5 ;
GCELLGRID X 0 DO 24 STEP 6900 ;
GCELLGRID Y 0 DO 9 STEP 6900 ;
VIAS 5 ;
    - via2_3_1600_480_1_5_320_320 + VIARULE M1M2_PR + CUTSIZE 150 150  + LAYERS met1 via met2  + CUTSPACING 170 170  + ENCLOSURE 85 165 55 85  + ROWCOL 1 5  ;
    - via3_4_1600_480_1_4_400_400 + VIARULE M2M3_PR + CUTSIZE 200 200  + LAYERS met2 via2 met3  + CUTSPACING 200 200  + ENCLOSURE 40 85 65 65  + ROWCOL 1 4  ;
    - via4_5_1600_480_1_4_400_400 + VIARULE M3M4_PR + CUTSIZE 200 200  + LAYERS met3 via3 met4  + CUTSPACING 200 200  + ENCLOSURE 90 60 100 65  + ROWCOL 1 4  ;
    - via5_6_1600_1600_1_1_1600_1600 + VIARULE M4M5_PR + CUTSIZE 800 800  + LAYERS met4 via4 met5  + CUTSPACING 800 800  + ENCLOSURE 400 190 310 400  ;
    - via5_6_1400_1600_1_1_1600_1600 + VIARULE M4M5_PR + CUTSIZE 800 800  + LAYERS met4 via4 met5  + CUTSPACING 800 800  + ENCLOSURE 300 400 310 400  ;
END VIAS
COMPONENTS 301 ;
    - ANTENNA__058__A sky130_fd_sc_hd__diode_2 + PLACED ( 46920 8160 ) S ;
    - ANTENNA__061__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 41400 27200 ) FN ;
    - ANTENNA__062__B sky130_fd_sc_hd__diode_2 + PLACED ( 46920 43520 ) N ;
    - ANTENNA__063__A2 sky130_fd_sc_hd__diode_2 + PLACED ( 46920 16320 ) N ;
    - ANTENNA__064__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 43700 8160 ) S ;
    - ANTENNA__064__C sky130_fd_sc_hd__diode_2 + PLACED ( 46920 5440 ) FN ;
    - ANTENNA__065__A0 sky130_fd_sc_hd__diode_2 + PLACED ( 46000 8160 ) S ;
    - ANTENNA__066__A0 sky130_fd_sc_hd__diode_2 + PLACED ( 46920 19040 ) S ;
    - ANTENNA__067__A sky130_fd_sc_hd__diode_2 + PLACED ( 36340 54400 ) FN ;
    - ANTENNA__067__B sky130_fd_sc_hd__diode_2 + PLACED ( 33120 54400 ) N ;
    - ANTENNA__068__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 34040 54400 ) FN ;
    - ANTENNA__068__B sky130_fd_sc_hd__diode_2 + PLACED ( 30820 54400 ) N ;
    - ANTENNA__069__A sky130_fd_sc_hd__diode_2 + PLACED ( 12420 43520 ) N ;
    - ANTENNA__069__B sky130_fd_sc_hd__diode_2 + PLACED ( 11500 43520 ) N ;
    - ANTENNA__070__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 26220 48960 ) N ;
    - ANTENNA__070__B sky130_fd_sc_hd__diode_2 + PLACED ( 23000 54400 ) N ;
    - ANTENNA__071__A sky130_fd_sc_hd__diode_2 + PLACED ( 45080 19040 ) FS ;
    - ANTENNA__071__B sky130_fd_sc_hd__diode_2 + PLACED ( 42320 27200 ) FN ;
    - ANTENNA__072__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 46920 35360 ) FS ;
    - ANTENNA__072__B sky130_fd_sc_hd__diode_2 + PLACED ( 12880 35360 ) S ;
    - ANTENNA__073__A sky130_fd_sc_hd__diode_2 + PLACED ( 46920 48960 ) N ;
    - ANTENNA__073__B sky130_fd_sc_hd__diode_2 + PLACED ( 46000 43520 ) N ;
    - ANTENNA__074__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 46920 21760 ) N ;
    - ANTENNA__074__B sky130_fd_sc_hd__diode_2 + PLACED ( 46920 38080 ) FN ;
    - ANTENNA__075__A sky130_fd_sc_hd__diode_2 + PLACED ( 17940 43520 ) N ;
    - ANTENNA__075__B sky130_fd_sc_hd__diode_2 + PLACED ( 13340 43520 ) N ;
    - ANTENNA__076__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 21160 43520 ) N ;
    - ANTENNA__076__B sky130_fd_sc_hd__diode_2 + PLACED ( 13340 38080 ) N ;
    - ANTENNA__077__A sky130_fd_sc_hd__diode_2 + PLACED ( 6900 27200 ) FN ;
    - ANTENNA__077__B sky130_fd_sc_hd__diode_2 + PLACED ( 10580 29920 ) S ;
    - ANTENNA__078__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 15640 38080 ) N ;
    - ANTENNA__078__B sky130_fd_sc_hd__diode_2 + PLACED ( 11960 35360 ) FS ;
    - ANTENNA__079__A sky130_fd_sc_hd__diode_2 + PLACED ( 31740 54400 ) FN ;
    - ANTENNA__079__B sky130_fd_sc_hd__diode_2 + PLACED ( 25760 54400 ) N ;
    - ANTENNA__080__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 23920 54400 ) FN ;
    - ANTENNA__080__B sky130_fd_sc_hd__diode_2 + PLACED ( 18860 54400 ) N ;
    - ANTENNA__081__A sky130_fd_sc_hd__diode_2 + PLACED ( 42780 8160 ) FS ;
    - ANTENNA__081__B sky130_fd_sc_hd__diode_2 + PLACED ( 39560 8160 ) S ;
    - ANTENNA__082__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 41400 8160 ) FS ;
    - ANTENNA__082__B sky130_fd_sc_hd__diode_2 + PLACED ( 36340 8160 ) S ;
    - ANTENNA__083__A sky130_fd_sc_hd__diode_2 + PLACED ( 41400 13600 ) FS ;
    - ANTENNA__083__B sky130_fd_sc_hd__diode_2 + PLACED ( 42320 13600 ) S ;
    - ANTENNA__084__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 40020 13600 ) FS ;
    - ANTENNA__084__B sky130_fd_sc_hd__diode_2 + PLACED ( 39100 13600 ) S ;
    - ANTENNA__085__A sky130_fd_sc_hd__diode_2 + PLACED ( 41400 54400 ) FN ;
    - ANTENNA__085__B sky130_fd_sc_hd__diode_2 + PLACED ( 46000 54400 ) FN ;
    - ANTENNA__086__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 42320 54400 ) FN ;
    - ANTENNA__086__B sky130_fd_sc_hd__diode_2 + PLACED ( 40020 54400 ) N ;
    - ANTENNA__087__A sky130_fd_sc_hd__diode_2 + PLACED ( 16560 10880 ) N ;
    - ANTENNA__087__B sky130_fd_sc_hd__diode_2 + PLACED ( 26680 5440 ) FN ;
    - ANTENNA__088__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 25760 5440 ) FN ;
    - ANTENNA__088__B sky130_fd_sc_hd__diode_2 + PLACED ( 16560 19040 ) FS ;
    - ANTENNA__089__A sky130_fd_sc_hd__diode_2 + PLACED ( 27140 10880 ) N ;
    - ANTENNA__089__B sky130_fd_sc_hd__diode_2 + PLACED ( 16560 13600 ) S ;
    - ANTENNA__090__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 31740 10880 ) N ;
    - ANTENNA__090__B sky130_fd_sc_hd__diode_2 + PLACED ( 25300 10880 ) FN ;
    - ANTENNA__091__A sky130_fd_sc_hd__diode_2 + PLACED ( 35880 10880 ) N ;
    - ANTENNA__091__B sky130_fd_sc_hd__diode_2 + PLACED ( 32660 10880 ) FN ;
    - ANTENNA__092__A_N sky130_fd_sc_hd__diode_2 + PLACED ( 33580 10880 ) N ;
    - ANTENNA__092__B sky130_fd_sc_hd__diode_2 + PLACED ( 29440 8160 ) S ;
    - ANTENNA__118__D sky130_fd_sc_hd__diode_2 + PLACED ( 41860 43520 ) FN ;
    - ANTENNA__118__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 29440 46240 ) FS ;
    - ANTENNA__119__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 17940 54400 ) FN ;
    - ANTENNA__120__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 16560 54400 ) FN ;
    - ANTENNA__121__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 14260 43520 ) N ;
    - ANTENNA__122__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 11500 29920 ) FS ;
    - ANTENNA__123__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 9660 29920 ) FS ;
    - ANTENNA__124__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 26220 10880 ) N ;
    - ANTENNA__125__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 30360 19040 ) FS ;
    - ANTENNA__126__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 40480 27200 ) N ;
    - ANTENNA__127__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 46920 29920 ) FS ;
    - ANTENNA__128__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 40020 24480 ) FS ;
    - ANTENNA__129__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 46000 19040 ) FS ;
    - ANTENNA__130__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 46000 48960 ) N ;
    - ANTENNA__131__RESET_B sky130_fd_sc_hd__diode_2 + PLACED ( 37720 54400 ) FN ;
    - ANTENNA__132__A sky130_fd_sc_hd__diode_2 + PLACED ( 46920 54400 ) FN ;
    - ANTENNA__135__A sky130_fd_sc_hd__diode_2 + PLACED ( 46920 10880 ) N ;
    - ANTENNA_clkbuf_0_serial_clock_A sky130_fd_sc_hd__diode_2 + PLACED ( 16560 38080 ) FN ;
    - ANTENNA_clkbuf_0_serial_load_A sky130_fd_sc_hd__diode_2 + PLACED ( 40480 29920 ) S ;
    - FILLER_0_50 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 27600 5440 ) N ;
    - FILLER_0_52 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 28520 5440 ) N ;
    - FILLER_0_64 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 34040 5440 ) N ;
    - FILLER_0_76 sky130_fd_sc_hd__decap_3 + SOURCE DIST + PLACED ( 39560 5440 ) N ;
    - FILLER_0_80 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 41400 5440 ) N ;
    - FILLER_10_27 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 17020 32640 ) N ;
    - FILLER_10_3 sky130_fd_sc_hd__decap_3 + SOURCE DIST + PLACED ( 5980 32640 ) N ;
    - FILLER_10_44 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 24840 32640 ) N ;
    - FILLER_10_76 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 39560 32640 ) N ;
    - FILLER_11_15 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 11500 35360 ) FS ;
    - FILLER_11_3 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 5980 35360 ) FS ;
    - FILLER_11_48 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 26680 35360 ) FS ;
    - FILLER_12_15 sky130_fd_sc_hd__decap_4 + SOURCE DIST + PLACED ( 11500 38080 ) N ;
    - FILLER_12_3 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 5980 38080 ) N ;
    - FILLER_13_3 sky130_fd_sc_hd__decap_3 + SOURCE DIST + PLACED ( 5980 40800 ) FS ;
    - FILLER_13_35 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 20700 40800 ) FS ;
    - FILLER_14_3 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 5980 43520 ) N ;
    - FILLER_14_38 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 22080 43520 ) N ;
    - FILLER_14_83 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 42780 43520 ) N ;
    - FILLER_14_85 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 43700 43520 ) N ;
    - FILLER_15_3 sky130_fd_sc_hd__fill_2 + SOURCE DIST + PLACED ( 5980 46240 ) FS ;
    - FILLER_15_65 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 34500 46240 ) FS ;
    - FILLER_16_3 sky130_fd_sc_hd__decap_4 + SOURCE DIST + PLACED ( 5980 48960 ) N ;
    - FILLER_17_11 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 9660 51680 ) FS ;
    - FILLER_17_3 sky130_fd_sc_hd__decap_8 + SOURCE DIST + PLACED ( 5980 51680 ) FS ;
    - FILLER_17_72 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 37720 51680 ) FS ;
    - FILLER_18_15 sky130_fd_sc_hd__decap_6 + SOURCE DIST + PLACED ( 11500 54400 ) N ;
    - FILLER_18_24 sky130_fd_sc_hd__fill_2 + SOURCE DIST + PLACED ( 15640 54400 ) N ;
    - FILLER_18_3 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 5980 54400 ) N ;
    - FILLER_18_44 sky130_fd_sc_hd__fill_2 + SOURCE DIST + PLACED ( 24840 54400 ) N ;
    - FILLER_18_48 sky130_fd_sc_hd__decap_4 + SOURCE DIST + PLACED ( 26680 54400 ) N ;
    - FILLER_18_52 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 28520 54400 ) N ;
    - FILLER_18_61 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 32660 54400 ) N ;
    - FILLER_18_66 sky130_fd_sc_hd__decap_3 + SOURCE DIST + PLACED ( 34960 54400 ) N ;
    - FILLER_18_71 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 37260 54400 ) N ;
    - FILLER_18_79 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 40940 54400 ) N ;
    - FILLER_18_85 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 43700 54400 ) N ;
    - FILLER_1_56 sky130_fd_sc_hd__decap_12 + SOURCE DIST + PLACED ( 30360 8160 ) FS ;
    - FILLER_1_68 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 35880 8160 ) FS ;
    - FILLER_1_71 sky130_fd_sc_hd__decap_4 + SOURCE DIST + PLACED ( 37260 8160 ) FS ;
    - FILLER_1_75 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 39100 8160 ) FS ;
    - FILLER_1_78 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 40480 8160 ) FS ;
    - FILLER_1_82 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 42320 8160 ) FS ;
    - FILLER_2_40 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 23000 10880 ) N ;
    - FILLER_2_44 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 24840 10880 ) N ;
    - FILLER_2_70 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 36800 10880 ) N ;
    - FILLER_2_83 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 42780 10880 ) N ;
    - FILLER_3_39 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 22540 13600 ) FS ;
    - FILLER_3_93 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 47380 13600 ) FS ;
    - FILLER_6_50 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 27600 21760 ) N ;
    - FILLER_6_60 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 32200 21760 ) N ;
    - FILLER_7_76 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 39560 24480 ) FS ;
    - FILLER_7_93 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 47380 24480 ) FS ;
    - FILLER_8_29 sky130_fd_sc_hd__fill_1 + SOURCE DIST + PLACED ( 17940 27200 ) N ;
    - FILLER_8_3 sky130_fd_sc_hd__fill_2 + SOURCE DIST + PLACED ( 5980 27200 ) N ;
    - FILLER_9_3 sky130_fd_sc_hd__decap_8 + SOURCE DIST + PLACED ( 5980 29920 ) FS ;
    - PHY_0 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 5440 ) N ;
    - PHY_1 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 5440 ) FN ;
    - PHY_10 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 19040 ) FS ;
    - PHY_11 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 19040 ) S ;
    - PHY_12 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 21760 ) N ;
    - PHY_13 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 21760 ) FN ;
    - PHY_14 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 24480 ) FS ;
    - PHY_15 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 24480 ) S ;
    - PHY_16 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 27200 ) N ;
    - PHY_17 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 27200 ) FN ;
    - PHY_18 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 29920 ) FS ;
    - PHY_19 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 29920 ) S ;
    - PHY_2 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 8160 ) FS ;
    - PHY_20 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 32640 ) N ;
    - PHY_21 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 32640 ) FN ;
    - PHY_22 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 35360 ) FS ;
    - PHY_23 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 35360 ) S ;
    - PHY_24 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 38080 ) N ;
    - PHY_25 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 38080 ) FN ;
    - PHY_26 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 40800 ) FS ;
    - PHY_27 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 40800 ) S ;
    - PHY_28 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 43520 ) N ;
    - PHY_29 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 43520 ) FN ;
    - PHY_3 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 8160 ) S ;
    - PHY_30 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 46240 ) FS ;
    - PHY_31 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 46240 ) S ;
    - PHY_32 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 48960 ) N ;
    - PHY_33 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 48960 ) FN ;
    - PHY_34 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 51680 ) FS ;
    - PHY_35 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 51680 ) S ;
    - PHY_36 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 4600 54400 ) N ;
    - PHY_37 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 54400 ) FN ;
    - PHY_4 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 10880 ) N ;
    - PHY_5 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 10880 ) FN ;
    - PHY_6 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 13600 ) FS ;
    - PHY_7 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 13600 ) S ;
    - PHY_8 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 15180 16320 ) N ;
    - PHY_9 sky130_fd_sc_hd__decap_3 + SOURCE DIST + FIXED ( 47840 16320 ) FN ;
    - TAP_38 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 28060 5440 ) N ;
    - TAP_39 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 40940 5440 ) N ;
    - TAP_40 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 40940 8160 ) FS ;
    - TAP_41 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 28060 10880 ) N ;
    - TAP_42 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 40940 13600 ) FS ;
    - TAP_43 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 28060 16320 ) N ;
    - TAP_44 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 40940 19040 ) FS ;
    - TAP_45 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 28060 21760 ) N ;
    - TAP_46 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 40940 24480 ) FS ;
    - TAP_47 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 27200 ) N ;
    - TAP_48 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 27200 ) N ;
    - TAP_49 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 27200 ) N ;
    - TAP_50 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 29920 ) FS ;
    - TAP_51 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 32640 ) N ;
    - TAP_52 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 32640 ) N ;
    - TAP_53 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 35360 ) FS ;
    - TAP_54 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 38080 ) N ;
    - TAP_55 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 38080 ) N ;
    - TAP_56 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 40800 ) FS ;
    - TAP_57 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 43520 ) N ;
    - TAP_58 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 43520 ) N ;
    - TAP_59 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 46240 ) FS ;
    - TAP_60 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 48960 ) N ;
    - TAP_61 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 48960 ) N ;
    - TAP_62 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 51680 ) FS ;
    - TAP_63 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 17480 54400 ) N ;
    - TAP_64 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 30360 54400 ) N ;
    - TAP_65 sky130_fd_sc_hd__tapvpwrvgnd_1 + SOURCE DIST + FIXED ( 43240 54400 ) N ;
    - _058_ sky130_fd_sc_hd__inv_2 + PLACED ( 45540 21760 ) FN ;
    - _059__1 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 28980 54400 ) FN ;
    - _060__14 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 38640 54400 ) FN ;
    - _061_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 40020 32640 ) N ;
    - _062_ sky130_fd_sc_hd__and2b_2 + PLACED ( 43700 38080 ) FN ;
    - _063_ sky130_fd_sc_hd__a31o_2 + PLACED ( 43700 29920 ) S ;
    - _064_ sky130_fd_sc_hd__and3b_2 + PLACED ( 43240 10880 ) N ;
    - _065_ sky130_fd_sc_hd__mux2_1 + PLACED ( 43240 13600 ) S ;
    - _066_ sky130_fd_sc_hd__mux2_1 + PLACED ( 43700 32640 ) FN ;
    - _067_ sky130_fd_sc_hd__or2_2 + PLACED ( 34040 51680 ) FS ;
    - _068_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 30820 51680 ) FS ;
    - _069_ sky130_fd_sc_hd__or2_2 + PLACED ( 15180 43520 ) N ;
    - _070_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 23000 48960 ) FN ;
    - _071_ sky130_fd_sc_hd__or2_2 + PLACED ( 41400 29920 ) S ;
    - _072_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 27140 35360 ) FS ;
    - _073_ sky130_fd_sc_hd__or2_2 + PLACED ( 43700 40800 ) S ;
    - _074_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 43700 35360 ) S ;
    - _075_ sky130_fd_sc_hd__or2_2 + PLACED ( 18860 43520 ) N ;
    - _076_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 17940 38080 ) FN ;
    - _077_ sky130_fd_sc_hd__or2_2 + PLACED ( 18400 27200 ) N ;
    - _078_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 21620 32640 ) FN ;
    - _079_ sky130_fd_sc_hd__or2_2 + PLACED ( 26680 51680 ) FS ;
    - _080_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 19780 54400 ) N ;
    - _081_ sky130_fd_sc_hd__or2_2 + PLACED ( 40480 10880 ) N ;
    - _082_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 37260 10880 ) N ;
    - _083_ sky130_fd_sc_hd__or2_2 + PLACED ( 45080 24480 ) FS ;
    - _084_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 35880 13600 ) FS ;
    - _085_ sky130_fd_sc_hd__or2_2 + PLACED ( 43700 48960 ) FN ;
    - _086_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 40020 48960 ) FN ;
    - _087_ sky130_fd_sc_hd__or2_2 + PLACED ( 20700 10880 ) N ;
    - _088_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 17480 10880 ) N ;
    - _089_ sky130_fd_sc_hd__or2_2 + PLACED ( 25760 16320 ) N ;
    - _090_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 28520 16320 ) FN ;
    - _091_ sky130_fd_sc_hd__or2_2 + PLACED ( 31740 16320 ) FN ;
    - _092_ sky130_fd_sc_hd__nand2b_2 + PLACED ( 28520 10880 ) FN ;
    - _093__2 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 14260 54400 ) FN ;
    - _094__3 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 38180 32640 ) FN ;
    - _095__4 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 28980 51680 ) FS ;
    - _096__5 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 14260 38080 ) FN ;
    - _097__6 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 12420 29920 ) S ;
    - _098__7 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 21620 48960 ) FN ;
    - _099__8 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 34500 10880 ) N ;
    - _100__9 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 31280 19040 ) FS ;
    - _101__10 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 36340 51680 ) S ;
    - _102__11 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 21160 13600 ) S ;
    - _103__12 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 26220 21760 ) FN ;
    - _104__13 sky130_fd_sc_hd__inv_2 + SOURCE TIMING + PLACED ( 23460 10880 ) FN ;
    - _105_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 27140 48960 ) N ;
    - _106_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 13800 51680 ) FS ;
    - _107_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 25300 32640 ) N ;
    - _108_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 30360 38080 ) N ;
    - _109_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 13800 35360 ) FS ;
    - _110_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 13800 29920 ) FS ;
    - _111_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 16560 46240 ) FS ;
    - _112_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 34040 16320 ) N ;
    - _113_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 32660 21760 ) N ;
    - _114_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 34960 46240 ) FS ;
    - _115_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 16560 8160 ) FS ;
    - _116_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 17480 19040 ) FS ;
    - _117_ sky130_fd_sc_hd__dfbbn_2 + PLACED ( 23000 13600 ) FS ;
    - _118_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 22540 43520 ) FN ;
    - _119_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 7820 48960 ) N ;
    - _120_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 6900 46240 ) S ;
    - _121_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 7360 40800 ) FS ;
    - _122_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 7360 32640 ) N ;
    - _123_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 7820 27200 ) N ;
    - _124_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 16560 21760 ) N ;
    - _125_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 16560 24480 ) FS ;
    - _126_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 20700 27200 ) N ;
    - _127_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 30820 29920 ) FS ;
    - _128_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 30820 27200 ) N ;
    - _129_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 29900 24480 ) FS ;
    - _130_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 32200 43520 ) N ;
    - _131_ sky130_fd_sc_hd__dfrtp_2 + PLACED ( 38180 51680 ) FS ;
    - _132_ sky130_fd_sc_hd__buf_2 + PLACED ( 46000 40800 ) FS ;
    - _133_ sky130_fd_sc_hd__buf_2 + PLACED ( 44160 43520 ) N ;
    - _134_ sky130_fd_sc_hd__buf_2 + PLACED ( 44160 54400 ) N ;
    - _135_ sky130_fd_sc_hd__ebufn_2 + PLACED ( 43700 27200 ) N ;
    - clkbuf_0_serial_clock sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 21160 38080 ) FN ;
    - clkbuf_0_serial_load sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 30820 35360 ) S ;
    - clkbuf_1_0__f_serial_clock sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 16560 16320 ) FN ;
    - clkbuf_1_0__f_serial_load sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 16560 5440 ) FN ;
    - clkbuf_1_1__f_serial_clock sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 30820 40800 ) FS ;
    - clkbuf_1_1__f_serial_load sky130_fd_sc_hd__clkbuf_16 + SOURCE TIMING + PLACED ( 21160 40800 ) S ;
    - const_source sky130_fd_sc_hd__conb_1 + PLACED ( 44620 8160 ) S ;
    - gpio_in_buf sky130_fd_sc_hd__einvp_8 + PLACED ( 32660 19040 ) FS ;
    - gpio_logic_high gpio_logic_high + FIXED ( 5980 8400 ) N ;
    - hold1 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 40020 40800 ) S ;
    - hold10 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 26220 24480 ) S ;
    - hold11 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 28520 21760 ) FN ;
    - hold12 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 17480 13600 ) FS ;
    - hold13 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 41400 24480 ) S ;
    - hold2 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 40020 35360 ) S ;
    - hold3 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 10120 51680 ) FS ;
    - hold4 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 17020 40800 ) S ;
    - hold5 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 17940 48960 ) FN ;
    - hold6 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 30820 46240 ) S ;
    - hold7 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 26680 29920 ) S ;
    - hold8 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 41400 19040 ) S ;
    - hold9 sky130_fd_sc_hd__dlygate4sd3_1 + SOURCE TIMING + PLACED ( 17940 32640 ) FN ;
END COMPONENTS
PINS 47 ;
    - gpio_defaults[0] + NET gpio_defaults[0] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 4830 63000 ) N ;
    - gpio_defaults[10] + NET gpio_defaults[10] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 27830 63000 ) N ;
    - gpio_defaults[11] + NET gpio_defaults[11] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 30130 63000 ) N ;
    - gpio_defaults[12] + NET gpio_defaults[12] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 32430 63000 ) N ;
    - gpio_defaults[1] + NET gpio_defaults[1] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 7130 63000 ) N ;
    - gpio_defaults[2] + NET gpio_defaults[2] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 9430 63000 ) N ;
    - gpio_defaults[3] + NET gpio_defaults[3] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 11730 63000 ) N ;
    - gpio_defaults[4] + NET gpio_defaults[4] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 14030 63000 ) N ;
    - gpio_defaults[5] + NET gpio_defaults[5] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 16330 63000 ) N ;
    - gpio_defaults[6] + NET gpio_defaults[6] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 18630 63000 ) N ;
    - gpio_defaults[7] + NET gpio_defaults[7] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 20930 63000 ) N ;
    - gpio_defaults[8] + NET gpio_defaults[8] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 23230 63000 ) N ;
    - gpio_defaults[9] + NET gpio_defaults[9] + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met2 ( -140 -2000 ) ( 140 2000 )
        + PLACED ( 25530 63000 ) N ;
    - mgmt_gpio_in + NET mgmt_gpio_in + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 4420 ) N ;
    - mgmt_gpio_oeb + NET mgmt_gpio_oeb + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 8500 ) N ;
    - mgmt_gpio_out + NET mgmt_gpio_out + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 10540 ) N ;
    - one + NET one + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 6460 ) N ;
    - pad_gpio_ana_en + NET pad_gpio_ana_en + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 12580 ) N ;
    - pad_gpio_ana_pol + NET pad_gpio_ana_pol + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 14620 ) N ;
    - pad_gpio_ana_sel + NET pad_gpio_ana_sel + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 16660 ) N ;
    - pad_gpio_dm[0] + NET pad_gpio_dm[0] + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 18700 ) N ;
    - pad_gpio_dm[1] + NET pad_gpio_dm[1] + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 20740 ) N ;
    - pad_gpio_dm[2] + NET pad_gpio_dm[2] + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 22780 ) N ;
    - pad_gpio_holdover + NET pad_gpio_holdover + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 24820 ) N ;
    - pad_gpio_ib_mode_sel + NET pad_gpio_ib_mode_sel + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 26860 ) N ;
    - pad_gpio_in + NET pad_gpio_in + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 28900 ) N ;
    - pad_gpio_inenb + NET pad_gpio_inenb + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 30940 ) N ;
    - pad_gpio_out + NET pad_gpio_out + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 32980 ) N ;
    - pad_gpio_outenb + NET pad_gpio_outenb + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 35020 ) N ;
    - pad_gpio_slow_sel + NET pad_gpio_slow_sel + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 37060 ) N ;
    - pad_gpio_vtrip_sel + NET pad_gpio_vtrip_sel + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 39100 ) N ;
    - resetn + NET resetn + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 41140 ) N ;
    - resetn_out + NET resetn_out + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 43180 ) N ;
    - serial_clock + NET serial_clock + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 45220 ) N ;
    - serial_clock_out + NET serial_clock_out + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 47260 ) N ;
    - serial_data_in + NET serial_data_in + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 49300 ) N ;
    - serial_data_out + NET serial_data_out + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 51340 ) N ;
    - serial_load + NET serial_load + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 53380 ) N ;
    - serial_load_out + NET serial_load_out + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 55420 ) N ;
    - user_gpio_in + NET user_gpio_in + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 57460 ) N ;
    - user_gpio_oeb + NET user_gpio_oeb + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 59500 ) N ;
    - user_gpio_out + NET user_gpio_out + DIRECTION INPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 61540 ) N ;
    - vccd + NET vccd + SPECIAL + DIRECTION INOUT + USE POWER
      + PORT
        + LAYER met5 ( -22550 -800 ) ( 22550 800 )
        + LAYER met5 ( -22550 -17700 ) ( 22550 -16100 )
        + LAYER met5 ( -22550 -34600 ) ( 22550 -33000 )
        + LAYER met4 ( 10890 -35300 ) ( 12490 16860 )
        + LAYER met4 ( -14110 -35300 ) ( -12510 16860 )
        + FIXED ( 26910 40500 ) N ;
    - vccd1 + NET vccd1 + SPECIAL + DIRECTION INOUT + USE POWER
      + PORT
        + LAYER met5 ( -22550 -800 ) ( 22550 800 )
        + LAYER met5 ( -22550 -17700 ) ( 22550 -16100 )
        + LAYER met5 ( -22550 -34600 ) ( 22550 -33000 )
        + LAYER met4 ( 15890 -40540 ) ( 17490 11620 )
        + LAYER met4 ( -9110 -40540 ) ( -7510 11620 )
        + FIXED ( 26910 45740 ) N ;
    - vssd + NET vssd + SPECIAL + DIRECTION INOUT + USE GROUND
      + PORT
        + LAYER met5 ( -22550 -800 ) ( 22550 800 )
        + LAYER met5 ( -22550 -17700 ) ( 22550 -16100 )
        + LAYER met5 ( -22550 -34600 ) ( 22550 -33000 )
        + LAYER met4 ( -1610 -43750 ) ( -10 8410 )
        + FIXED ( 26910 48950 ) N ;
    - vssd1 + NET vssd1 + SPECIAL + DIRECTION INOUT + USE GROUND
      + PORT
        + LAYER met5 ( -22550 -800 ) ( 22550 800 )
        + LAYER met5 ( -22550 -17700 ) ( 22550 -16100 )
        + LAYER met5 ( -22550 -34600 ) ( 22550 -33000 )
        + LAYER met4 ( 3390 -48990 ) ( 4990 3170 )
        + FIXED ( 26910 54190 ) N ;
    - zero + NET zero + DIRECTION OUTPUT + USE SIGNAL
      + PORT
        + LAYER met3 ( -50000 -300 ) ( 50000 300 )
        + PLACED ( 120000 2380 ) N ;
END PINS
BLOCKAGES 9 ;
    - LAYER li1 RECT ( 0 0 ) ( 16795 30025 ) ;
    - LAYER li1 RECT ( 0 29965 ) ( 4265 65069 ) ;
    - LAYER li1 RECT ( 4215 57405 ) ( 49815 64930 ) ;
    - LAYER li1 RECT ( 16830 0 ) ( 49410 5240 ) ;
    - LAYER li1 RECT ( 49000 0 ) ( 169810 64845 ) ;
    - LAYER met5 RECT ( 67000 0 ) ( 170000 65000 ) ;
    - LAYER met4 RECT ( 67000 0 ) ( 170000 65000 ) ;
    - LAYER met2 RECT ( 120000 0 ) ( 170000 65000 ) ;
    - LAYER met1 RECT ( 120000 0 ) ( 170000 65000 ) ;
END BLOCKAGES
SPECIALNETS 4 ;
    - vccd ( PIN vccd ) ( gpio_in_buf VPB ) ( const_source VPB ) ( _135_ VPB ) ( _134_ VPB ) ( _133_ VPB ) ( _132_ VPB )
      ( _131_ VPB ) ( _130_ VPB ) ( _129_ VPB ) ( _128_ VPB ) ( _127_ VPB ) ( _126_ VPB ) ( _125_ VPB ) ( _124_ VPB )
      ( _123_ VPB ) ( _122_ VPB ) ( _121_ VPB ) ( _120_ VPB ) ( _119_ VPB ) ( _118_ VPB ) ( _117_ VPB ) ( _116_ VPB )
      ( _115_ VPB ) ( _114_ VPB ) ( _113_ VPB ) ( _112_ VPB ) ( _111_ VPB ) ( _110_ VPB ) ( _109_ VPB ) ( _108_ VPB )
      ( _107_ VPB ) ( _106_ VPB ) ( _105_ VPB ) ( _092_ VPB ) ( _091_ VPB ) ( _090_ VPB ) ( _089_ VPB ) ( _088_ VPB )
      ( _087_ VPB ) ( _086_ VPB ) ( _085_ VPB ) ( _084_ VPB ) ( _083_ VPB ) ( _082_ VPB ) ( _081_ VPB ) ( _080_ VPB )
      ( _079_ VPB ) ( _078_ VPB ) ( _077_ VPB ) ( _076_ VPB ) ( _075_ VPB ) ( _074_ VPB ) ( _073_ VPB ) ( _072_ VPB )
      ( _071_ VPB ) ( _070_ VPB ) ( _069_ VPB ) ( _068_ VPB ) ( _067_ VPB ) ( _066_ VPB ) ( _065_ VPB ) ( _064_ VPB )
      ( _063_ VPB ) ( _062_ VPB ) ( _061_ VPB ) ( _058_ VPB ) ( PHY_9 VPB ) ( PHY_8 VPB ) ( PHY_7 VPB ) ( PHY_6 VPB )
      ( PHY_5 VPB ) ( PHY_4 VPB ) ( PHY_37 VPB ) ( PHY_36 VPB ) ( PHY_35 VPB ) ( PHY_34 VPB ) ( PHY_33 VPB ) ( PHY_32 VPB )
      ( PHY_31 VPB ) ( PHY_30 VPB ) ( PHY_3 VPB ) ( PHY_29 VPB ) ( PHY_28 VPB ) ( PHY_27 VPB ) ( PHY_26 VPB ) ( PHY_25 VPB )
      ( PHY_24 VPB ) ( PHY_23 VPB ) ( PHY_22 VPB ) ( PHY_21 VPB ) ( PHY_20 VPB ) ( PHY_2 VPB ) ( PHY_19 VPB ) ( PHY_18 VPB )
      ( PHY_17 VPB ) ( PHY_16 VPB ) ( PHY_15 VPB ) ( PHY_14 VPB ) ( PHY_13 VPB ) ( PHY_12 VPB ) ( PHY_11 VPB ) ( PHY_10 VPB )
      ( PHY_1 VPB ) ( PHY_0 VPB ) ( gpio_in_buf VPWR ) ( const_source VPWR ) ( _135_ VPWR ) ( _134_ VPWR ) ( _133_ VPWR ) ( _132_ VPWR )
      ( _131_ VPWR ) ( _130_ VPWR ) ( _129_ VPWR ) ( _128_ VPWR ) ( _127_ VPWR ) ( _126_ VPWR ) ( _125_ VPWR ) ( _124_ VPWR )
      ( _123_ VPWR ) ( _122_ VPWR ) ( _121_ VPWR ) ( _120_ VPWR ) ( _119_ VPWR ) ( _118_ VPWR ) ( _117_ VPWR ) ( _116_ VPWR )
      ( _115_ VPWR ) ( _114_ VPWR ) ( _113_ VPWR ) ( _112_ VPWR ) ( _111_ VPWR ) ( _110_ VPWR ) ( _109_ VPWR ) ( _108_ VPWR )
      ( _107_ VPWR ) ( _106_ VPWR ) ( _105_ VPWR ) ( _092_ VPWR ) ( _091_ VPWR ) ( _090_ VPWR ) ( _089_ VPWR ) ( _088_ VPWR )
      ( _087_ VPWR ) ( _086_ VPWR ) ( _085_ VPWR ) ( _084_ VPWR ) ( _083_ VPWR ) ( _082_ VPWR ) ( _081_ VPWR ) ( _080_ VPWR )
      ( _079_ VPWR ) ( _078_ VPWR ) ( _077_ VPWR ) ( _076_ VPWR ) ( _075_ VPWR ) ( _074_ VPWR ) ( _073_ VPWR ) ( _072_ VPWR )
      ( _071_ VPWR ) ( _070_ VPWR ) ( _069_ VPWR ) ( _068_ VPWR ) ( _067_ VPWR ) ( _066_ VPWR ) ( _065_ VPWR ) ( _064_ VPWR )
      ( _063_ VPWR ) ( _062_ VPWR ) ( _061_ VPWR ) ( _058_ VPWR ) ( TAP_65 VPWR ) ( TAP_64 VPWR ) ( TAP_63 VPWR ) ( TAP_62 VPWR )
      ( TAP_61 VPWR ) ( TAP_60 VPWR ) ( TAP_59 VPWR ) ( TAP_58 VPWR ) ( TAP_57 VPWR ) ( TAP_56 VPWR ) ( TAP_55 VPWR ) ( TAP_54 VPWR )
      ( TAP_53 VPWR ) ( TAP_52 VPWR ) ( TAP_51 VPWR ) ( TAP_50 VPWR ) ( TAP_49 VPWR ) ( TAP_48 VPWR ) ( TAP_47 VPWR ) ( TAP_46 VPWR )
      ( TAP_45 VPWR ) ( TAP_44 VPWR ) ( TAP_43 VPWR ) ( TAP_42 VPWR ) ( TAP_41 VPWR ) ( TAP_40 VPWR ) ( TAP_39 VPWR ) ( TAP_38 VPWR )
      ( PHY_9 VPWR ) ( PHY_8 VPWR ) ( PHY_7 VPWR ) ( PHY_6 VPWR ) ( PHY_5 VPWR ) ( PHY_4 VPWR ) ( PHY_37 VPWR ) ( PHY_36 VPWR )
      ( PHY_35 VPWR ) ( PHY_34 VPWR ) ( PHY_33 VPWR ) ( PHY_32 VPWR ) ( PHY_31 VPWR ) ( PHY_30 VPWR ) ( PHY_3 VPWR ) ( PHY_29 VPWR )
      ( PHY_28 VPWR ) ( PHY_27 VPWR ) ( PHY_26 VPWR ) ( PHY_25 VPWR ) ( PHY_24 VPWR ) ( PHY_23 VPWR ) ( PHY_22 VPWR ) ( PHY_21 VPWR )
      ( PHY_20 VPWR ) ( PHY_2 VPWR ) ( PHY_19 VPWR ) ( PHY_18 VPWR ) ( PHY_17 VPWR ) ( PHY_16 VPWR ) ( PHY_15 VPWR ) ( PHY_14 VPWR )
      ( PHY_13 VPWR ) ( PHY_12 VPWR ) ( PHY_11 VPWR ) ( PHY_10 VPWR ) ( PHY_1 VPWR ) ( PHY_0 VPWR ) + USE POWER
      + ROUTED met4 0 + SHAPE STRIPE ( 13600 23600 ) via5_6_1600_1600_1_1_1600_1600
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 24480 ) ( 49220 24480 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 19040 ) ( 49220 19040 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 13600 ) ( 49220 13600 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 8160 ) ( 49220 8160 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 57120 ) ( 49220 57120 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 51680 ) ( 49220 51680 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 46240 ) ( 49220 46240 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 40800 ) ( 49220 40800 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 35360 ) ( 49220 35360 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 29920 ) ( 49220 29920 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 40500 ) ( 49460 40500 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 23600 ) ( 49460 23600 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 6700 ) ( 49460 6700 )
      NEW met4 1600 + SHAPE STRIPE ( 38600 5200 ) ( 38600 57360 )
      NEW met4 1600 + SHAPE STRIPE ( 13600 5200 ) ( 13600 57360 )
      NEW met4 0 + SHAPE STRIPE ( 38600 40500 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 38600 23600 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 38600 6700 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 13600 40500 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 13600 23600 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 13600 6700 ) via5_6_1600_1600_1_1_1600_1600
      NEW met3 330 + SHAPE STRIPE ( 37810 57120 ) ( 39390 57120 )
      NEW met3 0 + SHAPE STRIPE ( 38600 57120 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 57120 ) ( 39370 57120 )
      NEW met2 0 + SHAPE STRIPE ( 38600 57120 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 57120 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 51680 ) ( 39390 51680 )
      NEW met3 0 + SHAPE STRIPE ( 38600 51680 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 51680 ) ( 39370 51680 )
      NEW met2 0 + SHAPE STRIPE ( 38600 51680 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 51680 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 46240 ) ( 39390 46240 )
      NEW met3 0 + SHAPE STRIPE ( 38600 46240 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 46240 ) ( 39370 46240 )
      NEW met2 0 + SHAPE STRIPE ( 38600 46240 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 46240 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 40800 ) ( 39390 40800 )
      NEW met3 0 + SHAPE STRIPE ( 38600 40800 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 40800 ) ( 39370 40800 )
      NEW met2 0 + SHAPE STRIPE ( 38600 40800 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 40800 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 35360 ) ( 39390 35360 )
      NEW met3 0 + SHAPE STRIPE ( 38600 35360 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 35360 ) ( 39370 35360 )
      NEW met2 0 + SHAPE STRIPE ( 38600 35360 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 35360 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 29920 ) ( 39390 29920 )
      NEW met3 0 + SHAPE STRIPE ( 38600 29920 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 29920 ) ( 39370 29920 )
      NEW met2 0 + SHAPE STRIPE ( 38600 29920 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 29920 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 24480 ) ( 39390 24480 )
      NEW met3 0 + SHAPE STRIPE ( 38600 24480 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 24480 ) ( 39370 24480 )
      NEW met2 0 + SHAPE STRIPE ( 38600 24480 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 24480 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 19040 ) ( 39390 19040 )
      NEW met3 0 + SHAPE STRIPE ( 38600 19040 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 19040 ) ( 39370 19040 )
      NEW met2 0 + SHAPE STRIPE ( 38600 19040 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 19040 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 13600 ) ( 39390 13600 )
      NEW met3 0 + SHAPE STRIPE ( 38600 13600 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 13600 ) ( 39370 13600 )
      NEW met2 0 + SHAPE STRIPE ( 38600 13600 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 13600 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 37810 8160 ) ( 39390 8160 )
      NEW met3 0 + SHAPE STRIPE ( 38600 8160 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 37830 8160 ) ( 39370 8160 )
      NEW met2 0 + SHAPE STRIPE ( 38600 8160 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 38600 8160 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 57120 ) ( 14390 57120 )
      NEW met3 0 + SHAPE STRIPE ( 13600 57120 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 57120 ) ( 14370 57120 )
      NEW met2 0 + SHAPE STRIPE ( 13600 57120 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 57120 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 51680 ) ( 14390 51680 )
      NEW met3 0 + SHAPE STRIPE ( 13600 51680 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 51680 ) ( 14370 51680 )
      NEW met2 0 + SHAPE STRIPE ( 13600 51680 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 51680 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 46240 ) ( 14390 46240 )
      NEW met3 0 + SHAPE STRIPE ( 13600 46240 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 46240 ) ( 14370 46240 )
      NEW met2 0 + SHAPE STRIPE ( 13600 46240 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 46240 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 40800 ) ( 14390 40800 )
      NEW met3 0 + SHAPE STRIPE ( 13600 40800 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 40800 ) ( 14370 40800 )
      NEW met2 0 + SHAPE STRIPE ( 13600 40800 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 40800 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 35360 ) ( 14390 35360 )
      NEW met3 0 + SHAPE STRIPE ( 13600 35360 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 35360 ) ( 14370 35360 )
      NEW met2 0 + SHAPE STRIPE ( 13600 35360 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 35360 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 12810 29920 ) ( 14390 29920 )
      NEW met3 0 + SHAPE STRIPE ( 13600 29920 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 12830 29920 ) ( 14370 29920 )
      NEW met2 0 + SHAPE STRIPE ( 13600 29920 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 13600 29920 ) via2_3_1600_480_1_5_320_320 ;
    - vccd1 ( PIN vccd1 ) ( * vccd1 ) + USE POWER
      + ROUTED met4 0 + SHAPE STRIPE ( 6980 11940 ) via5_6_1400_1600_1_1_1600_1600
      NEW met5 1600 + SHAPE STRIPE ( 4360 45740 ) ( 49460 45740 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 28840 ) ( 49460 28840 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 11940 ) ( 49460 11940 )
      NEW met4 1600 + SHAPE STRIPE ( 43600 5200 ) ( 43600 57360 )
      NEW met4 1600 + SHAPE STRIPE ( 18600 5200 ) ( 18600 57360 )
      NEW met4 0 + SHAPE STRIPE ( 43600 45740 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 43600 28840 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 43600 11940 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 18600 45740 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 18600 28840 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 18600 11940 ) via5_6_1600_1600_1_1_1600_1600 ;
    - vssd ( PIN vssd ) ( gpio_in_buf VNB ) ( const_source VNB ) ( _135_ VNB ) ( _134_ VNB ) ( _133_ VNB ) ( _132_ VNB )
      ( _131_ VNB ) ( _130_ VNB ) ( _129_ VNB ) ( _128_ VNB ) ( _127_ VNB ) ( _126_ VNB ) ( _125_ VNB ) ( _124_ VNB )
      ( _123_ VNB ) ( _122_ VNB ) ( _121_ VNB ) ( _120_ VNB ) ( _119_ VNB ) ( _118_ VNB ) ( _117_ VNB ) ( _116_ VNB )
      ( _115_ VNB ) ( _114_ VNB ) ( _113_ VNB ) ( _112_ VNB ) ( _111_ VNB ) ( _110_ VNB ) ( _109_ VNB ) ( _108_ VNB )
      ( _107_ VNB ) ( _106_ VNB ) ( _105_ VNB ) ( _092_ VNB ) ( _091_ VNB ) ( _090_ VNB ) ( _089_ VNB ) ( _088_ VNB )
      ( _087_ VNB ) ( _086_ VNB ) ( _085_ VNB ) ( _084_ VNB ) ( _083_ VNB ) ( _082_ VNB ) ( _081_ VNB ) ( _080_ VNB )
      ( _079_ VNB ) ( _078_ VNB ) ( _077_ VNB ) ( _076_ VNB ) ( _075_ VNB ) ( _074_ VNB ) ( _073_ VNB ) ( _072_ VNB )
      ( _071_ VNB ) ( _070_ VNB ) ( _069_ VNB ) ( _068_ VNB ) ( _067_ VNB ) ( _066_ VNB ) ( _065_ VNB ) ( _064_ VNB )
      ( _063_ VNB ) ( _062_ VNB ) ( _061_ VNB ) ( _058_ VNB ) ( PHY_9 VNB ) ( PHY_8 VNB ) ( PHY_7 VNB ) ( PHY_6 VNB )
      ( PHY_5 VNB ) ( PHY_4 VNB ) ( PHY_37 VNB ) ( PHY_36 VNB ) ( PHY_35 VNB ) ( PHY_34 VNB ) ( PHY_33 VNB ) ( PHY_32 VNB )
      ( PHY_31 VNB ) ( PHY_30 VNB ) ( PHY_3 VNB ) ( PHY_29 VNB ) ( PHY_28 VNB ) ( PHY_27 VNB ) ( PHY_26 VNB ) ( PHY_25 VNB )
      ( PHY_24 VNB ) ( PHY_23 VNB ) ( PHY_22 VNB ) ( PHY_21 VNB ) ( PHY_20 VNB ) ( PHY_2 VNB ) ( PHY_19 VNB ) ( PHY_18 VNB )
      ( PHY_17 VNB ) ( PHY_16 VNB ) ( PHY_15 VNB ) ( PHY_14 VNB ) ( PHY_13 VNB ) ( PHY_12 VNB ) ( PHY_11 VNB ) ( PHY_10 VNB )
      ( PHY_1 VNB ) ( PHY_0 VNB ) ( gpio_in_buf VGND ) ( const_source VGND ) ( _135_ VGND ) ( _134_ VGND ) ( _133_ VGND ) ( _132_ VGND )
      ( _131_ VGND ) ( _130_ VGND ) ( _129_ VGND ) ( _128_ VGND ) ( _127_ VGND ) ( _126_ VGND ) ( _125_ VGND ) ( _124_ VGND )
      ( _123_ VGND ) ( _122_ VGND ) ( _121_ VGND ) ( _120_ VGND ) ( _119_ VGND ) ( _118_ VGND ) ( _117_ VGND ) ( _116_ VGND )
      ( _115_ VGND ) ( _114_ VGND ) ( _113_ VGND ) ( _112_ VGND ) ( _111_ VGND ) ( _110_ VGND ) ( _109_ VGND ) ( _108_ VGND )
      ( _107_ VGND ) ( _106_ VGND ) ( _105_ VGND ) ( _092_ VGND ) ( _091_ VGND ) ( _090_ VGND ) ( _089_ VGND ) ( _088_ VGND )
      ( _087_ VGND ) ( _086_ VGND ) ( _085_ VGND ) ( _084_ VGND ) ( _083_ VGND ) ( _082_ VGND ) ( _081_ VGND ) ( _080_ VGND )
      ( _079_ VGND ) ( _078_ VGND ) ( _077_ VGND ) ( _076_ VGND ) ( _075_ VGND ) ( _074_ VGND ) ( _073_ VGND ) ( _072_ VGND )
      ( _071_ VGND ) ( _070_ VGND ) ( _069_ VGND ) ( _068_ VGND ) ( _067_ VGND ) ( _066_ VGND ) ( _065_ VGND ) ( _064_ VGND )
      ( _063_ VGND ) ( _062_ VGND ) ( _061_ VGND ) ( _058_ VGND ) ( TAP_65 VGND ) ( TAP_64 VGND ) ( TAP_63 VGND ) ( TAP_62 VGND )
      ( TAP_61 VGND ) ( TAP_60 VGND ) ( TAP_59 VGND ) ( TAP_58 VGND ) ( TAP_57 VGND ) ( TAP_56 VGND ) ( TAP_55 VGND ) ( TAP_54 VGND )
      ( TAP_53 VGND ) ( TAP_52 VGND ) ( TAP_51 VGND ) ( TAP_50 VGND ) ( TAP_49 VGND ) ( TAP_48 VGND ) ( TAP_47 VGND ) ( TAP_46 VGND )
      ( TAP_45 VGND ) ( TAP_44 VGND ) ( TAP_43 VGND ) ( TAP_42 VGND ) ( TAP_41 VGND ) ( TAP_40 VGND ) ( TAP_39 VGND ) ( TAP_38 VGND )
      ( PHY_9 VGND ) ( PHY_8 VGND ) ( PHY_7 VGND ) ( PHY_6 VGND ) ( PHY_5 VGND ) ( PHY_4 VGND ) ( PHY_37 VGND ) ( PHY_36 VGND )
      ( PHY_35 VGND ) ( PHY_34 VGND ) ( PHY_33 VGND ) ( PHY_32 VGND ) ( PHY_31 VGND ) ( PHY_30 VGND ) ( PHY_3 VGND ) ( PHY_29 VGND )
      ( PHY_28 VGND ) ( PHY_27 VGND ) ( PHY_26 VGND ) ( PHY_25 VGND ) ( PHY_24 VGND ) ( PHY_23 VGND ) ( PHY_22 VGND ) ( PHY_21 VGND )
      ( PHY_20 VGND ) ( PHY_2 VGND ) ( PHY_19 VGND ) ( PHY_18 VGND ) ( PHY_17 VGND ) ( PHY_16 VGND ) ( PHY_15 VGND ) ( PHY_14 VGND )
      ( PHY_13 VGND ) ( PHY_12 VGND ) ( PHY_11 VGND ) ( PHY_10 VGND ) ( PHY_1 VGND ) ( PHY_0 VGND ) + USE GROUND
      + ROUTED met1 480 + SHAPE FOLLOWPIN ( 15180 21760 ) ( 49220 21760 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 16320 ) ( 49220 16320 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 10880 ) ( 49220 10880 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 15180 5440 ) ( 49220 5440 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 54400 ) ( 49220 54400 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 48960 ) ( 49220 48960 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 43520 ) ( 49220 43520 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 38080 ) ( 49220 38080 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 32640 ) ( 49220 32640 )
      NEW met1 480 + SHAPE FOLLOWPIN ( 4600 27200 ) ( 49220 27200 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 48950 ) ( 49460 48950 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 32050 ) ( 49460 32050 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 15150 ) ( 49460 15150 )
      NEW met4 1600 + SHAPE STRIPE ( 26100 5200 ) ( 26100 57360 )
      NEW met4 0 + SHAPE STRIPE ( 26100 48950 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 26100 32050 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 26100 15150 ) via5_6_1600_1600_1_1_1600_1600
      NEW met3 330 + SHAPE STRIPE ( 25310 54400 ) ( 26890 54400 )
      NEW met3 0 + SHAPE STRIPE ( 26100 54400 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 54400 ) ( 26870 54400 )
      NEW met2 0 + SHAPE STRIPE ( 26100 54400 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 54400 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 48960 ) ( 26890 48960 )
      NEW met3 0 + SHAPE STRIPE ( 26100 48960 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 48960 ) ( 26870 48960 )
      NEW met2 0 + SHAPE STRIPE ( 26100 48960 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 48960 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 43520 ) ( 26890 43520 )
      NEW met3 0 + SHAPE STRIPE ( 26100 43520 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 43520 ) ( 26870 43520 )
      NEW met2 0 + SHAPE STRIPE ( 26100 43520 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 43520 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 38080 ) ( 26890 38080 )
      NEW met3 0 + SHAPE STRIPE ( 26100 38080 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 38080 ) ( 26870 38080 )
      NEW met2 0 + SHAPE STRIPE ( 26100 38080 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 38080 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 32640 ) ( 26890 32640 )
      NEW met3 0 + SHAPE STRIPE ( 26100 32640 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 32640 ) ( 26870 32640 )
      NEW met2 0 + SHAPE STRIPE ( 26100 32640 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 32640 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 27200 ) ( 26890 27200 )
      NEW met3 0 + SHAPE STRIPE ( 26100 27200 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 27200 ) ( 26870 27200 )
      NEW met2 0 + SHAPE STRIPE ( 26100 27200 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 27200 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 21760 ) ( 26890 21760 )
      NEW met3 0 + SHAPE STRIPE ( 26100 21760 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 21760 ) ( 26870 21760 )
      NEW met2 0 + SHAPE STRIPE ( 26100 21760 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 21760 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 16320 ) ( 26890 16320 )
      NEW met3 0 + SHAPE STRIPE ( 26100 16320 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 16320 ) ( 26870 16320 )
      NEW met2 0 + SHAPE STRIPE ( 26100 16320 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 16320 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 10880 ) ( 26890 10880 )
      NEW met3 0 + SHAPE STRIPE ( 26100 10880 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 10880 ) ( 26870 10880 )
      NEW met2 0 + SHAPE STRIPE ( 26100 10880 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 10880 ) via2_3_1600_480_1_5_320_320
      NEW met3 330 + SHAPE STRIPE ( 25310 5440 ) ( 26890 5440 )
      NEW met3 0 + SHAPE STRIPE ( 26100 5440 ) via4_5_1600_480_1_4_400_400
      NEW met2 370 + SHAPE STRIPE ( 25330 5440 ) ( 26870 5440 )
      NEW met2 0 + SHAPE STRIPE ( 26100 5440 ) via3_4_1600_480_1_4_400_400
      NEW met1 0 + SHAPE STRIPE ( 26100 5440 ) via2_3_1600_480_1_5_320_320 ;
    - vssd1 ( PIN vssd1 ) ( * vssd1 ) + USE GROUND
      + ROUTED met4 0 + SHAPE STRIPE ( 10680 20390 ) via5_6_1400_1600_1_1_1600_1600
      NEW met5 1600 + SHAPE STRIPE ( 4360 54190 ) ( 49460 54190 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 37290 ) ( 49460 37290 )
      NEW met5 1600 + SHAPE STRIPE ( 4360 20390 ) ( 49460 20390 )
      NEW met4 1600 + SHAPE STRIPE ( 31100 5200 ) ( 31100 57360 )
      NEW met4 0 + SHAPE STRIPE ( 31100 54190 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 31100 37290 ) via5_6_1600_1600_1_1_1600_1600
      NEW met4 0 + SHAPE STRIPE ( 31100 20390 ) via5_6_1600_1600_1_1_1600_1600 ;
END SPECIALNETS
NETS 136 ;
    - _000_ ( _112_ Q_N ) ( _065_ A1 ) + USE SIGNAL
      + ROUTED met2 ( 44850 15810 ) ( * 16830 )
      NEW met1 ( 44390 16830 ) ( 44850 * )
      NEW li1 ( 44850 15810 ) L1M1_PR
      NEW met1 ( 44850 15810 ) M1M2_PR
      NEW met1 ( 44850 16830 ) M1M2_PR
      NEW li1 ( 44390 16830 ) L1M1_PR
      NEW met1 ( 44850 15810 ) RECT ( -355 -70 0 70 )  ;
    - _001_ ( gpio_in_buf A ) ( _058_ Y ) + USE SIGNAL
      + ROUTED met1 ( 40710 20570 ) ( 46230 * )
      NEW met2 ( 46230 20570 ) ( * 22270 )
      NEW li1 ( 40710 20570 ) L1M1_PR
      NEW met1 ( 46230 20570 ) M1M2_PR
      NEW li1 ( 46230 22270 ) L1M1_PR
      NEW met1 ( 46230 22270 ) M1M2_PR
      NEW met1 ( 46230 22270 ) RECT ( -355 -70 0 70 )  ;
    - _002_ ( _105_ RESET_B ) ( _067_ X ) + USE SIGNAL
      + ROUTED met1 ( 35650 50150 ) ( 36570 * )
      NEW met2 ( 35650 50150 ) ( * 52190 )
      NEW li1 ( 36570 50150 ) L1M1_PR
      NEW met1 ( 35650 50150 ) M1M2_PR
      NEW li1 ( 35650 52190 ) L1M1_PR
      NEW met1 ( 35650 52190 ) M1M2_PR
      NEW met1 ( 35650 52190 ) RECT ( -355 -70 0 70 )  ;
    - _003_ ( _105_ SET_B ) ( _068_ Y ) + USE SIGNAL
      + ROUTED met2 ( 31970 49810 ) ( * 52190 )
      NEW li1 ( 31970 52190 ) L1M1_PR
      NEW met1 ( 31970 52190 ) M1M2_PR
      NEW met1 ( 31970 49810 ) M1M2_PR
      NEW met1 ( 31970 52190 ) RECT ( -355 -70 0 70 )  ;
    - _004_ ( _106_ RESET_B ) ( _069_ X ) + USE SIGNAL
      + ROUTED met1 ( 17250 45390 ) ( 21850 * )
      NEW met2 ( 21850 45390 ) ( * 53210 )
      NEW met1 ( 21850 53210 ) ( 23230 * )
      NEW li1 ( 17250 45390 ) L1M1_PR
      NEW met1 ( 21850 45390 ) M1M2_PR
      NEW met1 ( 21850 53210 ) M1M2_PR
      NEW li1 ( 23230 53210 ) L1M1_PR ;
    - _005_ ( _106_ SET_B ) ( _070_ Y ) + USE SIGNAL
      + ROUTED met1 ( 22770 51170 ) ( 23690 * )
      NEW met2 ( 22770 51170 ) ( * 53550 )
      NEW met1 ( 21390 53550 0 ) ( 22770 * )
      NEW li1 ( 23690 51170 ) L1M1_PR
      NEW met1 ( 22770 51170 ) M1M2_PR
      NEW met1 ( 22770 53550 ) M1M2_PR ;
    - _006_ ( _107_ RESET_B ) ( _071_ X ) + USE SIGNAL
      + ROUTED met1 ( 38870 31790 ) ( 41630 * )
      NEW met1 ( 38870 31790 ) ( * 32130 )
      NEW met1 ( 37030 32130 ) ( 38870 * )
      NEW met2 ( 37030 32130 ) ( * 33830 )
      NEW met1 ( 34730 33830 ) ( 37030 * )
      NEW li1 ( 41630 31790 ) L1M1_PR
      NEW met1 ( 37030 32130 ) M1M2_PR
      NEW met1 ( 37030 33830 ) M1M2_PR
      NEW li1 ( 34730 33830 ) L1M1_PR ;
    - _007_ ( _107_ SET_B ) ( _072_ Y ) + USE SIGNAL
      + ROUTED met2 ( 29670 33490 ) ( * 35870 )
      NEW li1 ( 29670 35870 ) L1M1_PR
      NEW met1 ( 29670 35870 ) M1M2_PR
      NEW met1 ( 29670 33490 ) M1M2_PR
      NEW met1 ( 29670 35870 ) RECT ( -355 -70 0 70 )  ;
    - _008_ ( _108_ RESET_B ) ( _073_ X ) + USE SIGNAL
      + ROUTED met1 ( 39790 39270 ) ( * 39610 )
      NEW met1 ( 39790 39610 ) ( 43930 * )
      NEW met2 ( 43930 39610 ) ( * 41650 )
      NEW li1 ( 39790 39270 ) L1M1_PR
      NEW met1 ( 43930 39610 ) M1M2_PR
      NEW li1 ( 43930 41650 ) L1M1_PR
      NEW met1 ( 43930 41650 ) M1M2_PR
      NEW met1 ( 43930 41650 ) RECT ( -355 -70 0 70 )  ;
    - _009_ ( _108_ SET_B ) ( _074_ Y ) + USE SIGNAL
      + ROUTED met1 ( 37950 38930 0 ) ( 40250 * )
      NEW met2 ( 40250 37230 ) ( * 38930 )
      NEW met1 ( 40250 37230 ) ( 45310 * )
      NEW met1 ( 40250 38930 ) M1M2_PR
      NEW met1 ( 40250 37230 ) M1M2_PR
      NEW li1 ( 45310 37230 ) L1M1_PR ;
    - _010_ ( _109_ RESET_B ) ( _075_ X ) + USE SIGNAL
      + ROUTED met1 ( 20930 36890 ) ( 23230 * )
      NEW met2 ( 20930 36890 ) ( * 45730 )
      NEW met1 ( 20470 45730 ) ( 20930 * )
      NEW li1 ( 23230 36890 ) L1M1_PR
      NEW met1 ( 20930 36890 ) M1M2_PR
      NEW met1 ( 20930 45730 ) M1M2_PR
      NEW li1 ( 20470 45730 ) L1M1_PR ;
    - _011_ ( _109_ SET_B ) ( _076_ Y ) + USE SIGNAL
      + ROUTED met2 ( 19550 37230 ) ( * 38930 )
      NEW li1 ( 19550 38930 ) L1M1_PR
      NEW met1 ( 19550 38930 ) M1M2_PR
      NEW met1 ( 19550 37230 ) M1M2_PR
      NEW met1 ( 19550 38930 ) RECT ( -355 -70 0 70 )  ;
    - _012_ ( _110_ RESET_B ) ( _077_ X ) + USE SIGNAL
      + ROUTED met1 ( 20010 29410 ) ( 23230 * )
      NEW met2 ( 23230 29410 ) ( * 31450 )
      NEW li1 ( 20010 29410 ) L1M1_PR
      NEW met1 ( 23230 29410 ) M1M2_PR
      NEW li1 ( 23230 31450 ) L1M1_PR
      NEW met1 ( 23230 31450 ) M1M2_PR
      NEW met1 ( 23230 31450 ) RECT ( -355 -70 0 70 )  ;
    - _013_ ( _110_ SET_B ) ( _078_ Y ) + USE SIGNAL
      + ROUTED met2 ( 21390 31790 ) ( * 33490 )
      NEW met1 ( 21390 33490 ) ( 23230 * )
      NEW met1 ( 21390 31790 ) M1M2_PR_MR
      NEW met1 ( 21390 33490 ) M1M2_PR
      NEW li1 ( 23230 33490 ) L1M1_PR ;
    - _014_ ( _111_ RESET_B ) ( _079_ X ) + USE SIGNAL
      + ROUTED met1 ( 25990 47770 ) ( 28290 * )
      NEW met2 ( 28290 47770 ) ( * 52190 )
      NEW li1 ( 25990 47770 ) L1M1_PR
      NEW met1 ( 28290 47770 ) M1M2_PR
      NEW li1 ( 28290 52190 ) L1M1_PR
      NEW met1 ( 28290 52190 ) M1M2_PR
      NEW met1 ( 28290 52190 ) RECT ( -355 -70 0 70 )  ;
    - _015_ ( _111_ SET_B ) ( _080_ Y ) + USE SIGNAL
      + ROUTED met2 ( 21390 48110 ) ( * 55250 )
      NEW li1 ( 21390 55250 ) L1M1_PR
      NEW met1 ( 21390 55250 ) M1M2_PR
      NEW met1 ( 21390 48110 ) M1M2_PR
      NEW met1 ( 21390 55250 ) RECT ( -355 -70 0 70 )  ;
    - _016_ ( _112_ RESET_B ) ( _081_ X ) + USE SIGNAL
      + ROUTED met1 ( 42550 17510 ) ( 43470 * )
      NEW met2 ( 42550 12750 ) ( * 17510 )
      NEW li1 ( 42550 12750 ) L1M1_PR
      NEW met1 ( 42550 12750 ) M1M2_PR
      NEW met1 ( 42550 17510 ) M1M2_PR
      NEW li1 ( 43470 17510 ) L1M1_PR
      NEW met1 ( 42550 12750 ) RECT ( -355 -70 0 70 )  ;
    - _017_ ( _112_ SET_B ) ( _082_ Y ) + USE SIGNAL
      + ROUTED met2 ( 39790 13090 ) ( * 17170 )
      NEW li1 ( 39790 13090 ) L1M1_PR
      NEW met1 ( 39790 13090 ) M1M2_PR
      NEW met1 ( 39790 17170 ) M1M2_PR
      NEW met1 ( 39790 13090 ) RECT ( -355 -70 0 70 )  ;
    - _018_ ( _113_ RESET_B ) ( _083_ X ) + USE SIGNAL
      + ROUTED met2 ( 42090 22950 ) ( * 24990 )
      NEW met1 ( 42090 24990 ) ( 46690 * )
      NEW li1 ( 42090 22950 ) L1M1_PR
      NEW met1 ( 42090 22950 ) M1M2_PR
      NEW met1 ( 42090 24990 ) M1M2_PR
      NEW li1 ( 46690 24990 ) L1M1_PR
      NEW met1 ( 42090 22950 ) RECT ( -355 -70 0 70 )  ;
    - _019_ ( _113_ SET_B ) ( _084_ Y ) + USE SIGNAL
      + ROUTED met2 ( 37490 15470 ) ( * 22610 )
      NEW li1 ( 37490 15470 ) L1M1_PR
      NEW met1 ( 37490 15470 ) M1M2_PR
      NEW met1 ( 37490 22610 ) M1M2_PR
      NEW met1 ( 37490 15470 ) RECT ( -355 -70 0 70 )  ;
    - _020_ ( _114_ RESET_B ) ( _085_ X ) + USE SIGNAL
      + ROUTED met2 ( 44390 47770 ) ( * 49810 )
      NEW met1 ( 43930 49810 ) ( 44390 * )
      NEW li1 ( 44390 47770 ) L1M1_PR
      NEW met1 ( 44390 47770 ) M1M2_PR
      NEW met1 ( 44390 49810 ) M1M2_PR
      NEW li1 ( 43930 49810 ) L1M1_PR
      NEW met1 ( 44390 47770 ) RECT ( -355 -70 0 70 )  ;
    - _021_ ( _114_ SET_B ) ( _086_ Y ) + USE SIGNAL
      + ROUTED met2 ( 41630 48110 ) ( * 49810 )
      NEW met1 ( 41630 48110 ) M1M2_PR
      NEW li1 ( 41630 49810 ) L1M1_PR
      NEW met1 ( 41630 49810 ) M1M2_PR
      NEW met1 ( 41630 49810 ) RECT ( -355 -70 0 70 )  ;
    - _022_ ( _115_ RESET_B ) ( _087_ X ) + USE SIGNAL
      + ROUTED met1 ( 25070 9690 ) ( 25990 * )
      NEW met2 ( 25070 9690 ) ( * 11730 )
      NEW met1 ( 22770 11730 ) ( 25070 * )
      NEW li1 ( 25990 9690 ) L1M1_PR
      NEW met1 ( 25070 9690 ) M1M2_PR
      NEW met1 ( 25070 11730 ) M1M2_PR
      NEW li1 ( 22770 11730 ) L1M1_PR ;
    - _023_ ( _115_ SET_B ) ( _088_ Y ) + USE SIGNAL
      + ROUTED met1 ( 19090 11730 ) ( 20470 * )
      NEW met2 ( 20470 10030 ) ( * 11730 )
      NEW li1 ( 19090 11730 ) L1M1_PR
      NEW met1 ( 20470 11730 ) M1M2_PR
      NEW met1 ( 20470 10030 ) M1M2_PR ;
    - _024_ ( _116_ RESET_B ) ( _089_ X ) + USE SIGNAL
      + ROUTED met1 ( 26910 18530 ) ( 27370 * )
      NEW met2 ( 26910 18530 ) ( * 20570 )
      NEW li1 ( 27370 18530 ) L1M1_PR
      NEW met1 ( 26910 18530 ) M1M2_PR
      NEW li1 ( 26910 20570 ) L1M1_PR
      NEW met1 ( 26910 20570 ) M1M2_PR
      NEW met1 ( 26910 20570 ) RECT ( -355 -70 0 70 )  ;
    - _025_ ( _116_ SET_B ) ( _090_ Y ) + USE SIGNAL
      + ROUTED met2 ( 29210 18530 ) ( * 20910 )
      NEW met1 ( 25070 20910 0 ) ( 29210 * )
      NEW li1 ( 29210 18530 ) L1M1_PR
      NEW met1 ( 29210 18530 ) M1M2_PR
      NEW met1 ( 29210 20910 ) M1M2_PR
      NEW met1 ( 29210 18530 ) RECT ( -355 -70 0 70 )  ;
    - _026_ ( _117_ RESET_B ) ( _091_ X ) + USE SIGNAL
      + ROUTED met2 ( 32430 15130 ) ( * 17170 )
      NEW met1 ( 31970 17170 ) ( 32430 * )
      NEW li1 ( 32430 15130 ) L1M1_PR
      NEW met1 ( 32430 15130 ) M1M2_PR
      NEW met1 ( 32430 17170 ) M1M2_PR
      NEW li1 ( 31970 17170 ) L1M1_PR
      NEW met1 ( 32430 15130 ) RECT ( -355 -70 0 70 )  ;
    - _027_ ( _117_ SET_B ) ( _092_ Y ) + USE SIGNAL
      + ROUTED met2 ( 30590 13090 ) ( * 15470 )
      NEW li1 ( 30590 13090 ) L1M1_PR
      NEW met1 ( 30590 13090 ) M1M2_PR
      NEW met1 ( 30590 15470 ) M1M2_PR_MR
      NEW met1 ( 30590 13090 ) RECT ( -355 -70 0 70 )  ;
    - _042_ ( _063_ B1 ) ( _062_ X ) + USE SIGNAL
      + ROUTED met1 ( 43930 31790 ) ( 44390 * )
      NEW met2 ( 44390 31790 ) ( * 38590 )
      NEW li1 ( 43930 31790 ) L1M1_PR
      NEW met1 ( 44390 31790 ) M1M2_PR
      NEW li1 ( 44390 38590 ) L1M1_PR
      NEW met1 ( 44390 38590 ) M1M2_PR
      NEW met1 ( 44390 38590 ) RECT ( -355 -70 0 70 )  ;
    - _043_ ( _065_ S ) ( _064_ X ) + USE SIGNAL
      + ROUTED met1 ( 44390 14790 ) ( 46230 * )
      NEW met2 ( 46230 13090 ) ( * 14790 )
      NEW li1 ( 46230 13090 ) L1M1_PR
      NEW met1 ( 46230 13090 ) M1M2_PR
      NEW li1 ( 44390 14790 ) L1M1_PR
      NEW met1 ( 46230 14790 ) M1M2_PR
      NEW met1 ( 46230 13090 ) RECT ( -355 -70 0 70 )  ;
    - _044_ ( _066_ A1 ) ( _065_ X ) + USE SIGNAL
      + ROUTED met1 ( 45310 15810 ) ( 47150 * )
      NEW met2 ( 45310 15810 ) ( * 33150 )
      NEW li1 ( 47150 15810 ) L1M1_PR
      NEW met1 ( 45310 15810 ) M1M2_PR
      NEW li1 ( 45310 33150 ) L1M1_PR
      NEW met1 ( 45310 33150 ) M1M2_PR
      NEW met1 ( 45310 33150 ) RECT ( -355 -70 0 70 )  ;
    - _045_ ( _135_ TE_B ) ( _061_ Y ) + USE SIGNAL
      + ROUTED met2 ( 44850 28050 ) ( * 33490 )
      NEW met1 ( 41630 33490 ) ( 44850 * )
      NEW li1 ( 44850 28050 ) L1M1_PR
      NEW met1 ( 44850 28050 ) M1M2_PR
      NEW met1 ( 44850 33490 ) M1M2_PR
      NEW li1 ( 41630 33490 ) L1M1_PR
      NEW met1 ( 44850 28050 ) RECT ( 0 -70 355 70 )  ;
    - _046_ ( _116_ Q_N ) + USE SIGNAL ;
    - _047_ ( _115_ Q_N ) + USE SIGNAL ;
    - _048_ ( _114_ Q_N ) + USE SIGNAL ;
    - _049_ ( _113_ Q_N ) + USE SIGNAL ;
    - _050_ ( _111_ Q_N ) + USE SIGNAL ;
    - _051_ ( _110_ Q_N ) + USE SIGNAL ;
    - _052_ ( _109_ Q_N ) + USE SIGNAL ;
    - _053_ ( _108_ Q_N ) + USE SIGNAL ;
    - _054_ ( _107_ Q_N ) + USE SIGNAL ;
    - _055_ ( _106_ Q_N ) + USE SIGNAL ;
    - _056_ ( _105_ Q_N ) + USE SIGNAL ;
    - _057_ ( _117_ Q_N ) + USE SIGNAL ;
    - clknet_0_serial_clock ( clkbuf_1_1__f_serial_clock A ) ( clkbuf_1_0__f_serial_clock A ) ( clkbuf_0_serial_clock X ) + USE CLOCK
      + ROUTED met1 ( 23690 39950 ) ( 24150 * )
      NEW met2 ( 24150 17510 ) ( * 39950 )
      NEW met1 ( 24150 17510 ) ( 25530 * )
      NEW met1 ( 24150 42670 ) ( 31050 * )
      NEW met2 ( 24150 39950 ) ( * 42670 )
      NEW li1 ( 23690 39950 ) L1M1_PR
      NEW met1 ( 24150 39950 ) M1M2_PR
      NEW met1 ( 24150 17510 ) M1M2_PR
      NEW li1 ( 25530 17510 ) L1M1_PR
      NEW li1 ( 31050 42670 ) L1M1_PR
      NEW met1 ( 24150 42670 ) M1M2_PR ;
    - clknet_0_serial_load ( clkbuf_1_1__f_serial_load A ) ( clkbuf_1_0__f_serial_load A ) ( clkbuf_0_serial_load X ) + USE CLOCK
      + ROUTED met1 ( 25530 6630 ) ( 31050 * )
      NEW met1 ( 30130 42330 ) ( 30590 * )
      NEW met2 ( 30590 41820 ) ( * 42330 )
      NEW met2 ( 30590 41820 ) ( 31050 * )
      NEW met2 ( 31050 36550 ) ( * 41820 )
      NEW met2 ( 31050 6630 ) ( * 36550 )
      NEW met1 ( 31050 6630 ) M1M2_PR
      NEW li1 ( 25530 6630 ) L1M1_PR
      NEW li1 ( 31050 36550 ) L1M1_PR
      NEW met1 ( 31050 36550 ) M1M2_PR
      NEW li1 ( 30130 42330 ) L1M1_PR
      NEW met1 ( 30590 42330 ) M1M2_PR
      NEW met1 ( 31050 36550 ) RECT ( -355 -70 0 70 )  ;
    - clknet_1_0__leaf_serial_clock ( _119_ CLK ) ( _120_ CLK ) ( _121_ CLK ) ( _122_ CLK ) ( _123_ CLK ) ( _124_ CLK ) ( _125_ CLK )
      ( _126_ CLK ) ( clkbuf_1_0__f_serial_clock X ) + USE CLOCK
      + ROUTED met1 ( 7590 50150 ) ( 8050 * )
      NEW met1 ( 7590 48450 ) ( 13570 * )
      NEW met2 ( 7590 34170 ) ( * 42330 )
      NEW met1 ( 7590 28730 ) ( 8050 * )
      NEW met2 ( 7590 28730 ) ( * 34170 )
      NEW met1 ( 7590 26010 ) ( 16790 * )
      NEW met2 ( 7590 26010 ) ( * 28730 )
      NEW met2 ( 16790 23290 ) ( * 26010 )
      NEW met1 ( 16790 28390 ) ( 20930 * )
      NEW met2 ( 16790 26010 ) ( * 28390 )
      NEW met1 ( 16790 17850 ) ( 17250 * )
      NEW met2 ( 16790 17850 ) ( * 23290 )
      NEW met1 ( 13570 48110 ) ( 16330 * )
      NEW met1 ( 16330 47770 ) ( * 48110 )
      NEW met2 ( 7590 42330 ) ( * 50150 )
      NEW met1 ( 13570 48110 ) ( * 48450 )
      NEW li1 ( 8050 50150 ) L1M1_PR
      NEW met1 ( 7590 50150 ) M1M2_PR
      NEW met1 ( 7590 48450 ) M1M2_PR
      NEW li1 ( 7590 42330 ) L1M1_PR
      NEW met1 ( 7590 42330 ) M1M2_PR
      NEW li1 ( 7590 34170 ) L1M1_PR
      NEW met1 ( 7590 34170 ) M1M2_PR
      NEW li1 ( 8050 28730 ) L1M1_PR
      NEW met1 ( 7590 28730 ) M1M2_PR
      NEW li1 ( 16790 26010 ) L1M1_PR
      NEW met1 ( 7590 26010 ) M1M2_PR
      NEW li1 ( 16790 23290 ) L1M1_PR
      NEW met1 ( 16790 23290 ) M1M2_PR
      NEW met1 ( 16790 26010 ) M1M2_PR
      NEW li1 ( 20930 28390 ) L1M1_PR
      NEW met1 ( 16790 28390 ) M1M2_PR
      NEW li1 ( 17250 17850 ) L1M1_PR
      NEW met1 ( 16790 17850 ) M1M2_PR
      NEW li1 ( 16330 47770 ) L1M1_PR
      NEW met2 ( 7590 48450 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 7590 42330 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 7590 34170 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 16790 23290 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 16790 26010 ) RECT ( -595 -70 0 70 )  ;
    - clknet_1_0__leaf_serial_load ( _097__6 A ) ( _099__8 A ) ( _100__9 A ) ( _102__11 A ) ( _103__12 A ) ( _104__13 A ) ( clkbuf_1_0__f_serial_load X ) + USE CLOCK
      + ROUTED met1 ( 34270 11390 ) ( * 12070 )
      NEW met1 ( 26450 11390 ) ( 34270 * )
      NEW met1 ( 26450 11390 ) ( * 12070 )
      NEW met1 ( 24610 12070 ) ( 26450 * )
      NEW met1 ( 19090 5950 ) ( 24610 * )
      NEW met2 ( 24610 5950 ) ( * 12070 )
      NEW met1 ( 34270 12070 ) ( 34730 * )
      NEW met1 ( 25070 22950 ) ( 27370 * )
      NEW met2 ( 25070 22950 ) ( * 30430 )
      NEW met1 ( 14490 30430 ) ( 25070 * )
      NEW met1 ( 14490 30430 ) ( * 31450 )
      NEW met1 ( 27370 20570 ) ( 31510 * )
      NEW met2 ( 27370 20570 ) ( * 22950 )
      NEW met1 ( 22310 15130 ) ( 24610 * )
      NEW met2 ( 24610 15130 ) ( * 15300 )
      NEW met2 ( 24610 15300 ) ( 25070 * )
      NEW met2 ( 25070 15300 ) ( * 22950 )
      NEW met1 ( 13570 31450 ) ( 14490 * )
      NEW met2 ( 24610 12070 ) ( * 15130 )
      NEW li1 ( 13570 31450 ) L1M1_PR
      NEW li1 ( 24610 12070 ) L1M1_PR
      NEW met1 ( 24610 12070 ) M1M2_PR
      NEW li1 ( 19090 5950 ) L1M1_PR
      NEW met1 ( 24610 5950 ) M1M2_PR
      NEW li1 ( 34730 12070 ) L1M1_PR
      NEW li1 ( 27370 22950 ) L1M1_PR
      NEW met1 ( 25070 22950 ) M1M2_PR
      NEW met1 ( 25070 30430 ) M1M2_PR
      NEW li1 ( 31510 20570 ) L1M1_PR
      NEW met1 ( 27370 20570 ) M1M2_PR
      NEW met1 ( 27370 22950 ) M1M2_PR
      NEW li1 ( 22310 15130 ) L1M1_PR
      NEW met1 ( 24610 15130 ) M1M2_PR
      NEW met1 ( 24610 12070 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 27370 22950 ) RECT ( -595 -70 0 70 )  ;
    - clknet_1_1__leaf_serial_clock ( _118_ CLK ) ( _127_ CLK ) ( _128_ CLK ) ( _129_ CLK ) ( _130_ CLK ) ( _133_ A ) ( _060__14 A )
      ( clkbuf_1_1__f_serial_clock X ) + USE CLOCK
      + ROUTED met1 ( 34270 43010 ) ( 37490 * )
      NEW met2 ( 34270 43010 ) ( * 55590 )
      NEW met1 ( 34270 55590 ) ( 39790 * )
      NEW met1 ( 32430 45050 ) ( 34270 * )
      NEW met1 ( 31970 45050 ) ( 32430 * )
      NEW met1 ( 44390 44710 ) ( * 45050 )
      NEW met1 ( 34270 45050 ) ( 44390 * )
      NEW met1 ( 31050 31450 ) ( * 31790 )
      NEW met1 ( 31050 31790 ) ( 33810 * )
      NEW met2 ( 33810 31790 ) ( * 39780 )
      NEW met2 ( 33810 39780 ) ( 34270 * )
      NEW met2 ( 34270 39780 ) ( * 43010 )
      NEW met1 ( 30590 28730 ) ( 31050 * )
      NEW met2 ( 30590 28730 ) ( * 31450 )
      NEW met1 ( 30590 31450 ) ( 31050 * )
      NEW met2 ( 30130 26010 ) ( * 28220 )
      NEW met2 ( 30130 28220 ) ( 30590 * )
      NEW met2 ( 30590 28220 ) ( * 28730 )
      NEW li1 ( 37490 43010 ) L1M1_PR
      NEW met1 ( 34270 43010 ) M1M2_PR
      NEW met1 ( 34270 55590 ) M1M2_PR
      NEW li1 ( 39790 55590 ) L1M1_PR
      NEW li1 ( 32430 45050 ) L1M1_PR
      NEW met1 ( 34270 45050 ) M1M2_PR
      NEW li1 ( 31970 45050 ) L1M1_PR
      NEW li1 ( 44390 44710 ) L1M1_PR
      NEW li1 ( 31050 31450 ) L1M1_PR
      NEW met1 ( 33810 31790 ) M1M2_PR
      NEW li1 ( 31050 28730 ) L1M1_PR
      NEW met1 ( 30590 28730 ) M1M2_PR
      NEW met1 ( 30590 31450 ) M1M2_PR
      NEW li1 ( 30130 26010 ) L1M1_PR
      NEW met1 ( 30130 26010 ) M1M2_PR
      NEW met2 ( 34270 45050 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 30130 26010 ) RECT ( -355 -70 0 70 )  ;
    - clknet_1_1__leaf_serial_load ( _134_ A ) ( _059__1 A ) ( _093__2 A ) ( _094__3 A ) ( _095__4 A ) ( _096__5 A ) ( _098__7 A )
      ( _101__10 A ) ( clkbuf_1_1__f_serial_load X ) + USE CLOCK
      + ROUTED met2 ( 37490 33830 ) ( * 53210 )
      NEW met1 ( 37490 33830 ) ( 39330 * )
      NEW met1 ( 44390 55250 ) ( * 55590 )
      NEW met1 ( 37490 55250 ) ( 44390 * )
      NEW met2 ( 37490 53210 ) ( * 55250 )
      NEW met1 ( 30130 55250 ) ( * 55590 )
      NEW met1 ( 30130 55250 ) ( 37490 * )
      NEW met1 ( 29210 53210 ) ( * 53550 )
      NEW met1 ( 29210 53550 ) ( 37490 * )
      NEW met1 ( 37490 53210 ) ( * 53550 )
      NEW met2 ( 23690 43010 ) ( * 53550 )
      NEW met1 ( 23690 53550 ) ( 29210 * )
      NEW met1 ( 22770 50150 ) ( 23690 * )
      NEW met1 ( 15410 39270 ) ( * 39610 )
      NEW met1 ( 15410 39610 ) ( 23230 * )
      NEW met2 ( 23230 39610 ) ( * 39780 )
      NEW met2 ( 23230 39780 ) ( 23690 * )
      NEW met2 ( 23690 39780 ) ( * 43010 )
      NEW met1 ( 15410 55590 ) ( * 55930 )
      NEW met1 ( 15410 55930 ) ( 23690 * )
      NEW met2 ( 23690 53550 ) ( * 55930 )
      NEW li1 ( 37490 53210 ) L1M1_PR
      NEW met1 ( 37490 53210 ) M1M2_PR
      NEW met1 ( 37490 33830 ) M1M2_PR
      NEW li1 ( 39330 33830 ) L1M1_PR
      NEW li1 ( 44390 55590 ) L1M1_PR
      NEW met1 ( 37490 55250 ) M1M2_PR
      NEW li1 ( 30130 55590 ) L1M1_PR
      NEW li1 ( 29210 53210 ) L1M1_PR
      NEW li1 ( 23690 43010 ) L1M1_PR
      NEW met1 ( 23690 43010 ) M1M2_PR
      NEW met1 ( 23690 53550 ) M1M2_PR
      NEW li1 ( 22770 50150 ) L1M1_PR
      NEW met1 ( 23690 50150 ) M1M2_PR
      NEW li1 ( 15410 39270 ) L1M1_PR
      NEW met1 ( 23230 39610 ) M1M2_PR
      NEW li1 ( 15410 55590 ) L1M1_PR
      NEW met1 ( 23690 55930 ) M1M2_PR
      NEW met1 ( 37490 53210 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 23690 43010 ) RECT ( -355 -70 0 70 ) 
      NEW met2 ( 23690 50150 ) RECT ( -70 -485 70 0 )  ;
    - gpio_defaults[0] ( PIN gpio_defaults[0] ) ( ANTENNA__067__B DIODE ) ( ANTENNA__068__B DIODE ) ( _068_ B ) ( _067_ B ) + USE SIGNAL
      + ROUTED met2 ( 6210 56270 ) ( * 61540 )
      NEW met2 ( 4830 61540 0 ) ( 6210 * )
      NEW met1 ( 31050 56270 ) ( 33350 * )
      NEW met2 ( 32890 53210 ) ( * 56270 )
      NEW met1 ( 32890 53210 ) ( 34270 * )
      NEW met1 ( 6210 56270 ) ( 31050 * )
      NEW met1 ( 6210 56270 ) M1M2_PR
      NEW li1 ( 31050 56270 ) L1M1_PR
      NEW li1 ( 33350 56270 ) L1M1_PR
      NEW li1 ( 32890 53210 ) L1M1_PR
      NEW met1 ( 32890 53210 ) M1M2_PR
      NEW met1 ( 32890 56270 ) M1M2_PR
      NEW li1 ( 34270 53210 ) L1M1_PR
      NEW met1 ( 32890 53210 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 32890 56270 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[10] ( PIN gpio_defaults[10] ) ( ANTENNA__081__B DIODE ) ( ANTENNA__082__B DIODE ) ( _082_ B ) ( _081_ B ) + USE SIGNAL
      + ROUTED met1 ( 36570 10030 ) ( 39790 * )
      NEW met2 ( 39330 10030 ) ( * 12070 )
      NEW met1 ( 39330 12070 ) ( 40710 * )
      NEW met1 ( 31510 10030 ) ( 36570 * )
      NEW met1 ( 27830 55930 ) ( 31510 * )
      NEW met2 ( 27830 55930 ) ( * 61540 0 )
      NEW met2 ( 31510 10030 ) ( * 55930 )
      NEW met1 ( 31510 10030 ) M1M2_PR
      NEW li1 ( 36570 10030 ) L1M1_PR
      NEW li1 ( 39790 10030 ) L1M1_PR
      NEW li1 ( 39330 12070 ) L1M1_PR
      NEW met1 ( 39330 12070 ) M1M2_PR
      NEW met1 ( 39330 10030 ) M1M2_PR
      NEW li1 ( 40710 12070 ) L1M1_PR
      NEW met1 ( 31510 55930 ) M1M2_PR
      NEW met1 ( 27830 55930 ) M1M2_PR
      NEW met1 ( 39330 12070 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 39330 10030 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[11] ( PIN gpio_defaults[11] ) ( ANTENNA__083__B DIODE ) ( ANTENNA__084__B DIODE ) ( _084_ B ) ( _083_ B ) + USE SIGNAL
      + ROUTED met1 ( 42550 26350 ) ( 45310 * )
      NEW met2 ( 42550 26350 ) ( * 41650 )
      NEW met1 ( 32430 41650 ) ( 42550 * )
      NEW met1 ( 39790 15810 ) ( 42090 * )
      NEW met2 ( 42090 15810 ) ( * 18020 )
      NEW met2 ( 42090 18020 ) ( 42550 * )
      NEW met2 ( 42550 18020 ) ( * 26350 )
      NEW met1 ( 42090 15810 ) ( 42550 * )
      NEW met1 ( 38870 15130 ) ( * 15810 )
      NEW met1 ( 38870 15810 ) ( 39790 * )
      NEW met1 ( 30130 53890 ) ( 32430 * )
      NEW met2 ( 30130 53890 ) ( * 61540 0 )
      NEW met2 ( 32430 41650 ) ( * 53890 )
      NEW li1 ( 45310 26350 ) L1M1_PR
      NEW met1 ( 42550 26350 ) M1M2_PR
      NEW met1 ( 42550 41650 ) M1M2_PR
      NEW met1 ( 32430 41650 ) M1M2_PR
      NEW li1 ( 39790 15810 ) L1M1_PR
      NEW met1 ( 42090 15810 ) M1M2_PR
      NEW li1 ( 42550 15810 ) L1M1_PR
      NEW li1 ( 38870 15130 ) L1M1_PR
      NEW met1 ( 32430 53890 ) M1M2_PR
      NEW met1 ( 30130 53890 ) M1M2_PR ;
    - gpio_defaults[12] ( PIN gpio_defaults[12] ) ( ANTENNA__085__B DIODE ) ( ANTENNA__086__B DIODE ) ( _086_ B ) ( _085_ B ) + USE SIGNAL
      + ROUTED met1 ( 32430 56610 ) ( 40250 * )
      NEW met2 ( 32430 56610 ) ( * 61540 0 )
      NEW met1 ( 40250 56610 ) ( 46230 * )
      NEW met2 ( 40710 50150 ) ( * 56610 )
      NEW met1 ( 45770 50150 ) ( * 50490 )
      NEW met1 ( 40710 50490 ) ( 45770 * )
      NEW met1 ( 40710 50150 ) ( * 50490 )
      NEW li1 ( 40250 56610 ) L1M1_PR
      NEW met1 ( 32430 56610 ) M1M2_PR
      NEW li1 ( 46230 56610 ) L1M1_PR
      NEW li1 ( 40710 50150 ) L1M1_PR
      NEW met1 ( 40710 50150 ) M1M2_PR
      NEW met1 ( 40710 56610 ) M1M2_PR
      NEW li1 ( 45770 50150 ) L1M1_PR
      NEW met1 ( 40710 50150 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 40710 56610 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[1] ( PIN gpio_defaults[1] ) ( ANTENNA__079__B DIODE ) ( ANTENNA__080__B DIODE ) ( _080_ B ) ( _079_ B ) + USE SIGNAL
      + ROUTED met2 ( 8970 56610 ) ( * 61540 )
      NEW met2 ( 7130 61540 0 ) ( 8970 * )
      NEW met2 ( 21850 55590 ) ( * 56610 )
      NEW met1 ( 19090 56610 ) ( 21850 * )
      NEW met1 ( 21850 55590 ) ( 25990 * )
      NEW met1 ( 25070 53210 ) ( 26910 * )
      NEW met2 ( 25070 53210 ) ( * 55590 )
      NEW met1 ( 8970 56610 ) ( 19090 * )
      NEW met1 ( 8970 56610 ) M1M2_PR
      NEW li1 ( 19090 56610 ) L1M1_PR
      NEW li1 ( 21850 55590 ) L1M1_PR
      NEW met1 ( 21850 55590 ) M1M2_PR
      NEW met1 ( 21850 56610 ) M1M2_PR
      NEW li1 ( 25990 55590 ) L1M1_PR
      NEW li1 ( 26910 53210 ) L1M1_PR
      NEW met1 ( 25070 53210 ) M1M2_PR
      NEW met1 ( 25070 55590 ) M1M2_PR
      NEW met1 ( 21850 55590 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 25070 55590 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[2] ( PIN gpio_defaults[2] ) ( ANTENNA__069__B DIODE ) ( ANTENNA__070__B DIODE ) ( _070_ B ) ( _069_ B ) + USE SIGNAL
      + ROUTED met2 ( 9430 48620 ) ( 9890 * )
      NEW met2 ( 9430 48620 ) ( * 61540 0 )
      NEW met1 ( 23230 50490 ) ( 24150 * )
      NEW met2 ( 23230 50490 ) ( * 54910 )
      NEW met3 ( 9890 47940 ) ( 23230 * )
      NEW met1 ( 9890 45730 ) ( 11730 * )
      NEW met2 ( 9890 45730 ) ( * 47940 )
      NEW met1 ( 15410 44370 ) ( 15870 * )
      NEW met2 ( 15870 44370 ) ( * 47940 )
      NEW met2 ( 9890 47940 ) ( * 48620 )
      NEW met2 ( 23230 47940 ) ( * 50490 )
      NEW li1 ( 24150 50490 ) L1M1_PR
      NEW met1 ( 23230 50490 ) M1M2_PR
      NEW li1 ( 23230 54910 ) L1M1_PR
      NEW met1 ( 23230 54910 ) M1M2_PR
      NEW met2 ( 9890 47940 ) M2M3_PR
      NEW met2 ( 23230 47940 ) M2M3_PR
      NEW li1 ( 11730 45730 ) L1M1_PR
      NEW met1 ( 9890 45730 ) M1M2_PR
      NEW li1 ( 15410 44370 ) L1M1_PR
      NEW met1 ( 15870 44370 ) M1M2_PR
      NEW met2 ( 15870 47940 ) M2M3_PR
      NEW met1 ( 23230 54910 ) RECT ( -355 -70 0 70 ) 
      NEW met3 ( 15870 47940 ) RECT ( -800 -150 0 150 )  ;
    - gpio_defaults[3] ( PIN gpio_defaults[3] ) ( ANTENNA__075__B DIODE ) ( ANTENNA__076__B DIODE ) ( _076_ B ) ( _075_ B ) + USE SIGNAL
      + ROUTED met2 ( 12190 45730 ) ( * 61540 )
      NEW met2 ( 11730 61540 0 ) ( 12190 * )
      NEW met1 ( 14030 40290 ) ( 14950 * )
      NEW met2 ( 14950 40290 ) ( * 45730 )
      NEW met1 ( 14030 45730 ) ( 14950 * )
      NEW met1 ( 18170 44710 ) ( 19090 * )
      NEW met2 ( 18170 44710 ) ( * 45730 )
      NEW met1 ( 14950 45730 ) ( 18170 * )
      NEW met2 ( 18170 39270 ) ( * 44710 )
      NEW met1 ( 12190 45730 ) ( 14030 * )
      NEW met1 ( 12190 45730 ) M1M2_PR
      NEW li1 ( 14030 45730 ) L1M1_PR
      NEW li1 ( 14030 40290 ) L1M1_PR
      NEW met1 ( 14950 40290 ) M1M2_PR
      NEW met1 ( 14950 45730 ) M1M2_PR
      NEW li1 ( 19090 44710 ) L1M1_PR
      NEW met1 ( 18170 44710 ) M1M2_PR
      NEW met1 ( 18170 45730 ) M1M2_PR
      NEW li1 ( 18170 39270 ) L1M1_PR
      NEW met1 ( 18170 39270 ) M1M2_PR
      NEW met1 ( 18170 39270 ) RECT ( -355 -70 0 70 )  ;
    - gpio_defaults[4] ( PIN gpio_defaults[4] ) ( ANTENNA__077__B DIODE ) ( ANTENNA__078__B DIODE ) ( _078_ B ) ( _077_ B ) + USE SIGNAL
      + ROUTED met2 ( 15410 32130 ) ( * 37570 )
      NEW met1 ( 15410 33830 ) ( 21850 * )
      NEW met1 ( 18630 28050 ) ( 19090 * )
      NEW met2 ( 19090 28050 ) ( * 33830 )
      NEW met1 ( 11270 32130 ) ( 15410 * )
      NEW met1 ( 12650 37570 ) ( 15410 * )
      NEW met2 ( 14030 58140 ) ( 15410 * )
      NEW met2 ( 14030 58140 ) ( * 61540 0 )
      NEW met2 ( 15410 37570 ) ( * 58140 )
      NEW li1 ( 11270 32130 ) L1M1_PR
      NEW li1 ( 12650 37570 ) L1M1_PR
      NEW met1 ( 15410 37570 ) M1M2_PR
      NEW met1 ( 15410 32130 ) M1M2_PR
      NEW li1 ( 21850 33830 ) L1M1_PR
      NEW met1 ( 15410 33830 ) M1M2_PR
      NEW li1 ( 18630 28050 ) L1M1_PR
      NEW met1 ( 19090 28050 ) M1M2_PR
      NEW met1 ( 19090 33830 ) M1M2_PR
      NEW met2 ( 15410 33830 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 19090 33830 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[5] ( PIN gpio_defaults[5] ) ( ANTENNA__087__B DIODE ) ( ANTENNA__088__B DIODE ) ( _088_ B ) ( _087_ B ) + USE SIGNAL
      + ROUTED met1 ( 18630 12070 ) ( 20010 * )
      NEW met1 ( 18630 11730 ) ( * 12070 )
      NEW met1 ( 16330 11730 ) ( 18630 * )
      NEW met1 ( 20010 12070 ) ( 20930 * )
      NEW met1 ( 20930 7650 ) ( 26910 * )
      NEW met2 ( 20930 7650 ) ( * 12070 )
      NEW met1 ( 16330 20570 ) ( 16790 * )
      NEW met2 ( 16330 20570 ) ( * 61540 0 )
      NEW met2 ( 16330 11730 ) ( * 20570 )
      NEW li1 ( 20010 12070 ) L1M1_PR
      NEW met1 ( 16330 11730 ) M1M2_PR
      NEW li1 ( 20930 12070 ) L1M1_PR
      NEW li1 ( 26910 7650 ) L1M1_PR
      NEW met1 ( 20930 7650 ) M1M2_PR
      NEW met1 ( 20930 12070 ) M1M2_PR
      NEW li1 ( 16790 20570 ) L1M1_PR
      NEW met1 ( 16330 20570 ) M1M2_PR
      NEW met1 ( 20930 12070 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[6] ( PIN gpio_defaults[6] ) ( ANTENNA__089__B DIODE ) ( ANTENNA__090__B DIODE ) ( _090_ B ) ( _089_ B ) + USE SIGNAL
      + ROUTED met1 ( 22310 12750 ) ( 25530 * )
      NEW met1 ( 17250 15470 ) ( 22310 * )
      NEW met1 ( 22310 15470 ) ( * 15810 )
      NEW met2 ( 22310 15810 ) ( * 41650 )
      NEW met1 ( 19090 41650 ) ( 22310 * )
      NEW met2 ( 19090 41650 ) ( * 49980 )
      NEW met2 ( 18630 49980 ) ( 19090 * )
      NEW met2 ( 18630 49980 ) ( * 61540 0 )
      NEW met1 ( 22310 17170 ) ( 25990 * )
      NEW met1 ( 25990 17510 ) ( 28750 * )
      NEW met1 ( 25990 17170 ) ( * 17510 )
      NEW met2 ( 22310 12750 ) ( * 15810 )
      NEW li1 ( 25530 12750 ) L1M1_PR
      NEW met1 ( 22310 12750 ) M1M2_PR
      NEW li1 ( 17250 15470 ) L1M1_PR
      NEW met1 ( 22310 15810 ) M1M2_PR
      NEW met1 ( 22310 41650 ) M1M2_PR
      NEW met1 ( 19090 41650 ) M1M2_PR
      NEW li1 ( 25990 17170 ) L1M1_PR
      NEW met1 ( 22310 17170 ) M1M2_PR
      NEW li1 ( 28750 17510 ) L1M1_PR
      NEW met2 ( 22310 17170 ) RECT ( -70 -485 70 0 )  ;
    - gpio_defaults[7] ( PIN gpio_defaults[7] ) ( ANTENNA__091__B DIODE ) ( ANTENNA__092__B DIODE ) ( _092_ B ) ( _091_ B ) + USE SIGNAL
      + ROUTED met1 ( 33350 13090 ) ( 33810 * )
      NEW met1 ( 29670 11730 ) ( * 12070 )
      NEW met1 ( 29670 11730 ) ( 33810 * )
      NEW met2 ( 33810 11730 ) ( * 13090 )
      NEW met2 ( 30130 10030 ) ( * 11730 )
      NEW met2 ( 33810 13090 ) ( * 13800 )
      NEW met1 ( 33350 17510 ) ( 33810 * )
      NEW met2 ( 33350 17510 ) ( * 46750 )
      NEW met1 ( 22310 46750 ) ( 33350 * )
      NEW met2 ( 33350 13800 ) ( 33810 * )
      NEW met2 ( 33350 13800 ) ( * 17510 )
      NEW met2 ( 20930 61540 0 ) ( 22310 * )
      NEW met2 ( 22310 46750 ) ( * 61540 )
      NEW li1 ( 33350 13090 ) L1M1_PR
      NEW met1 ( 33810 13090 ) M1M2_PR
      NEW li1 ( 29670 12070 ) L1M1_PR
      NEW met1 ( 33810 11730 ) M1M2_PR
      NEW li1 ( 30130 10030 ) L1M1_PR
      NEW met1 ( 30130 10030 ) M1M2_PR
      NEW met1 ( 30130 11730 ) M1M2_PR
      NEW li1 ( 33810 17510 ) L1M1_PR
      NEW met1 ( 33350 17510 ) M1M2_PR
      NEW met1 ( 33350 46750 ) M1M2_PR
      NEW met1 ( 22310 46750 ) M1M2_PR
      NEW met1 ( 30130 10030 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 30130 11730 ) RECT ( -595 -70 0 70 )  ;
    - gpio_defaults[8] ( PIN gpio_defaults[8] ) ( ANTENNA__071__B DIODE ) ( ANTENNA__072__B DIODE ) ( _072_ B ) ( _071_ B ) + USE SIGNAL
      + ROUTED met2 ( 23230 56780 ) ( 24150 * )
      NEW met2 ( 23230 56780 ) ( * 61540 0 )
      NEW met1 ( 43010 31450 ) ( 43470 * )
      NEW met2 ( 43010 29410 ) ( * 31450 )
      NEW met1 ( 30130 36890 ) ( 41630 * )
      NEW met2 ( 41630 31110 ) ( * 36890 )
      NEW met1 ( 41630 31110 ) ( 43470 * )
      NEW met1 ( 43470 31110 ) ( * 31450 )
      NEW met1 ( 13570 35870 ) ( 25530 * )
      NEW met1 ( 25530 35870 ) ( * 36550 )
      NEW met1 ( 25530 36550 ) ( 30130 * )
      NEW met1 ( 30130 36550 ) ( * 36890 )
      NEW met2 ( 24150 43180 ) ( 25070 * )
      NEW met2 ( 25070 36550 ) ( * 43180 )
      NEW met1 ( 25070 36550 ) ( 25530 * )
      NEW met2 ( 24150 43180 ) ( * 56780 )
      NEW li1 ( 43470 31450 ) L1M1_PR
      NEW met1 ( 43010 31450 ) M1M2_PR
      NEW li1 ( 43010 29410 ) L1M1_PR
      NEW met1 ( 43010 29410 ) M1M2_PR
      NEW li1 ( 30130 36890 ) L1M1_PR
      NEW met1 ( 41630 36890 ) M1M2_PR
      NEW met1 ( 41630 31110 ) M1M2_PR
      NEW li1 ( 13570 35870 ) L1M1_PR
      NEW met1 ( 25070 36550 ) M1M2_PR
      NEW met1 ( 43010 29410 ) RECT ( -355 -70 0 70 )  ;
    - gpio_defaults[9] ( PIN gpio_defaults[9] ) ( ANTENNA__073__B DIODE ) ( ANTENNA__074__B DIODE ) ( _074_ B ) ( _073_ B ) + USE SIGNAL
      + ROUTED met1 ( 33810 42670 ) ( 45770 * )
      NEW met1 ( 33810 42670 ) ( * 43010 )
      NEW met1 ( 27370 43010 ) ( 33810 * )
      NEW met2 ( 46690 42670 ) ( * 44030 )
      NEW met1 ( 45770 42670 ) ( 46690 * )
      NEW met1 ( 46690 40290 ) ( 47150 * )
      NEW met2 ( 46690 40290 ) ( * 42670 )
      NEW met1 ( 44850 36550 ) ( 46690 * )
      NEW met2 ( 46690 36550 ) ( * 40290 )
      NEW met2 ( 25530 54910 ) ( 27370 * )
      NEW met2 ( 25530 54910 ) ( * 61540 0 )
      NEW met2 ( 27370 43010 ) ( * 54910 )
      NEW li1 ( 45770 42670 ) L1M1_PR
      NEW met1 ( 27370 43010 ) M1M2_PR
      NEW li1 ( 46690 44030 ) L1M1_PR
      NEW met1 ( 46690 44030 ) M1M2_PR
      NEW met1 ( 46690 42670 ) M1M2_PR
      NEW li1 ( 47150 40290 ) L1M1_PR
      NEW met1 ( 46690 40290 ) M1M2_PR
      NEW li1 ( 44850 36550 ) L1M1_PR
      NEW met1 ( 46690 36550 ) M1M2_PR
      NEW met1 ( 46690 44030 ) RECT ( -355 -70 0 70 )  ;
    - gpio_logic1 ( gpio_logic_high gpio_logic1 ) ( gpio_in_buf TE ) + USE SIGNAL
      + ROUTED met2 ( 13570 17000 ) ( * 19890 )
      NEW met3 ( 12420 17000 0 ) ( 13570 * )
      NEW met1 ( 18170 19550 ) ( * 19890 )
      NEW met1 ( 18170 19550 ) ( 24150 * )
      NEW met1 ( 24150 19550 ) ( * 19890 )
      NEW met1 ( 24150 19890 ) ( 32890 * )
      NEW met1 ( 32890 19890 ) ( * 20230 )
      NEW met1 ( 13570 19890 ) ( 18170 * )
      NEW met1 ( 13570 19890 ) M1M2_PR
      NEW met2 ( 13570 17000 ) M2M3_PR
      NEW li1 ( 32890 20230 ) L1M1_PR ;
    - gpio_outenb ( _111_ Q ) ( _063_ A1 ) ( _061_ B ) + USE SIGNAL
      + ROUTED met2 ( 42090 34170 ) ( * 46750 )
      NEW met1 ( 35650 46750 ) ( 42090 * )
      NEW met1 ( 35650 46750 ) ( * 47090 )
      NEW met1 ( 28810 47090 ) ( 35650 * )
      NEW met1 ( 42090 32130 ) ( 44850 * )
      NEW met2 ( 42090 32130 ) ( * 34170 )
      NEW li1 ( 42090 34170 ) L1M1_PR
      NEW met1 ( 42090 34170 ) M1M2_PR
      NEW met1 ( 42090 46750 ) M1M2_PR
      NEW li1 ( 28810 47090 ) L1M1_PR
      NEW li1 ( 44850 32130 ) L1M1_PR
      NEW met1 ( 42090 32130 ) M1M2_PR
      NEW met1 ( 42090 34170 ) RECT ( -355 -70 0 70 )  ;
    - mgmt_ena ( _105_ Q ) ( _066_ S ) ( _063_ A3 ) ( _062_ A_N ) + USE SIGNAL
      + ROUTED met1 ( 45770 39610 ) ( 46690 * )
      NEW met2 ( 45770 39610 ) ( * 49470 )
      NEW met1 ( 39390 49470 ) ( 45770 * )
      NEW met1 ( 44850 34170 ) ( 45770 * )
      NEW met2 ( 45770 34170 ) ( * 39610 )
      NEW met2 ( 45770 31790 ) ( * 34170 )
      NEW li1 ( 46690 39610 ) L1M1_PR
      NEW met1 ( 45770 39610 ) M1M2_PR
      NEW met1 ( 45770 49470 ) M1M2_PR
      NEW li1 ( 39390 49470 ) L1M1_PR
      NEW li1 ( 44850 34170 ) L1M1_PR
      NEW met1 ( 45770 34170 ) M1M2_PR
      NEW li1 ( 45770 31790 ) L1M1_PR
      NEW met1 ( 45770 31790 ) M1M2_PR
      NEW met1 ( 45770 31790 ) RECT ( -355 -70 0 70 )  ;
    - mgmt_gpio_in ( PIN mgmt_gpio_in ) ( _135_ Z ) + USE SIGNAL
      + ROUTED met3 ( 47610 4420 ) ( 70380 * 0 )
      NEW met2 ( 47610 4420 ) ( * 28050 )
      NEW met2 ( 47610 4420 ) M2M3_PR
      NEW li1 ( 47610 28050 ) L1M1_PR
      NEW met1 ( 47610 28050 ) M1M2_PR
      NEW met1 ( 47610 28050 ) RECT ( -355 -70 0 70 )  ;
    - mgmt_gpio_oeb ( PIN mgmt_gpio_oeb ) ( ANTENNA__063__A2 DIODE ) ( ANTENNA__064__C DIODE ) ( _064_ C ) ( _063_ A2 ) + USE SIGNAL
      + ROUTED met1 ( 47610 7650 ) ( 48070 * )
      NEW met2 ( 48070 7650 ) ( * 8500 )
      NEW met3 ( 48070 8500 ) ( 70380 * 0 )
      NEW met1 ( 45540 11730 ) ( 48070 * )
      NEW met2 ( 48070 8500 ) ( * 11730 )
      NEW met2 ( 47150 18530 ) ( * 32130 )
      NEW met1 ( 45310 32130 ) ( 47150 * )
      NEW met1 ( 47150 18530 ) ( 48070 * )
      NEW met2 ( 48070 11730 ) ( * 18530 )
      NEW li1 ( 47610 7650 ) L1M1_PR
      NEW met1 ( 48070 7650 ) M1M2_PR
      NEW met2 ( 48070 8500 ) M2M3_PR
      NEW li1 ( 45540 11730 ) L1M1_PR
      NEW met1 ( 48070 11730 ) M1M2_PR
      NEW li1 ( 47150 18530 ) L1M1_PR
      NEW met1 ( 47150 18530 ) M1M2_PR
      NEW met1 ( 47150 32130 ) M1M2_PR
      NEW li1 ( 45310 32130 ) L1M1_PR
      NEW met1 ( 48070 18530 ) M1M2_PR
      NEW met1 ( 47150 18530 ) RECT ( -355 -70 0 70 )  ;
    - mgmt_gpio_out ( PIN mgmt_gpio_out ) ( ANTENNA__065__A0 DIODE ) ( _065_ A0 ) + USE SIGNAL
      + ROUTED met2 ( 46690 10370 ) ( * 10540 )
      NEW met3 ( 46690 10540 ) ( 70380 * 0 )
      NEW met1 ( 45310 15130 ) ( 46690 * )
      NEW met2 ( 46690 10540 ) ( * 15130 )
      NEW li1 ( 46690 10370 ) L1M1_PR
      NEW met1 ( 46690 10370 ) M1M2_PR
      NEW met2 ( 46690 10540 ) M2M3_PR
      NEW met1 ( 46690 15130 ) M1M2_PR
      NEW li1 ( 45310 15130 ) L1M1_PR
      NEW met1 ( 46690 10370 ) RECT ( -355 -70 0 70 )  ;
    - net1 ( _105_ CLK_N ) ( _059__1 Y ) + USE CLOCK
      + ROUTED met1 ( 27370 50490 ) ( 27830 * )
      NEW met2 ( 27830 50490 ) ( * 54910 )
      NEW met1 ( 27830 54910 ) ( 29670 * )
      NEW li1 ( 27370 50490 ) L1M1_PR
      NEW met1 ( 27830 50490 ) M1M2_PR
      NEW met1 ( 27830 54910 ) M1M2_PR
      NEW li1 ( 29670 54910 ) L1M1_PR ;
    - net10 ( _114_ CLK_N ) ( _101__10 Y ) + USE CLOCK
      + ROUTED met1 ( 35190 47770 ) ( 36110 * )
      NEW met2 ( 36110 47770 ) ( * 52190 )
      NEW met1 ( 36110 52190 ) ( 37030 * )
      NEW li1 ( 35190 47770 ) L1M1_PR
      NEW met1 ( 36110 47770 ) M1M2_PR
      NEW met1 ( 36110 52190 ) M1M2_PR
      NEW li1 ( 37030 52190 ) L1M1_PR ;
    - net11 ( _115_ CLK_N ) ( _102__11 Y ) + USE CLOCK
      + ROUTED met1 ( 16790 9690 ) ( * 10370 )
      NEW met1 ( 16790 10370 ) ( 21850 * )
      NEW met2 ( 21850 10370 ) ( * 14110 )
      NEW li1 ( 16790 9690 ) L1M1_PR
      NEW met1 ( 21850 10370 ) M1M2_PR
      NEW li1 ( 21850 14110 ) L1M1_PR
      NEW met1 ( 21850 14110 ) M1M2_PR
      NEW met1 ( 21850 14110 ) RECT ( -355 -70 0 70 )  ;
    - net12 ( _116_ CLK_N ) ( _103__12 Y ) + USE CLOCK
      + ROUTED met1 ( 17710 20570 ) ( 20010 * )
      NEW met1 ( 20010 20230 ) ( * 20570 )
      NEW met1 ( 20010 20230 ) ( 20930 * )
      NEW met2 ( 20930 20230 ) ( * 23290 )
      NEW met1 ( 20930 23290 ) ( 26910 * )
      NEW li1 ( 17710 20570 ) L1M1_PR
      NEW met1 ( 20930 20230 ) M1M2_PR
      NEW met1 ( 20930 23290 ) M1M2_PR
      NEW li1 ( 26910 23290 ) L1M1_PR ;
    - net13 ( _117_ CLK_N ) ( _104__13 Y ) + USE CLOCK
      + ROUTED met1 ( 23230 13090 ) ( 24150 * )
      NEW met2 ( 23230 13090 ) ( * 14790 )
      NEW li1 ( 24150 13090 ) L1M1_PR
      NEW met1 ( 23230 13090 ) M1M2_PR
      NEW li1 ( 23230 14790 ) L1M1_PR
      NEW met1 ( 23230 14790 ) M1M2_PR
      NEW met1 ( 23230 14790 ) RECT ( -355 -70 0 70 )  ;
    - net14 ( _131_ CLK ) ( _060__14 Y ) + USE CLOCK
      + ROUTED met2 ( 38410 53210 ) ( * 54910 )
      NEW met1 ( 38410 54910 ) ( 39330 * )
      NEW li1 ( 38410 53210 ) L1M1_PR
      NEW met1 ( 38410 53210 ) M1M2_PR
      NEW met1 ( 38410 54910 ) M1M2_PR
      NEW li1 ( 39330 54910 ) L1M1_PR
      NEW met1 ( 38410 53210 ) RECT ( -355 -70 0 70 )  ;
    - net15 ( _114_ D ) ( hold1 X ) + USE SIGNAL
      + ROUTED met2 ( 40250 43010 ) ( * 47430 )
      NEW met1 ( 37030 47430 ) ( 40250 * )
      NEW li1 ( 40250 43010 ) L1M1_PR
      NEW met1 ( 40250 43010 ) M1M2_PR
      NEW met1 ( 40250 47430 ) M1M2_PR
      NEW li1 ( 37030 47430 ) L1M1_PR
      NEW met1 ( 40250 43010 ) RECT ( -355 -70 0 70 )  ;
    - net16 ( _128_ D ) ( _108_ D ) ( hold2 X ) + USE SIGNAL
      + ROUTED met2 ( 32430 28730 ) ( * 39270 )
      NEW met1 ( 32430 35870 ) ( 40250 * )
      NEW li1 ( 32430 39270 ) L1M1_PR
      NEW met1 ( 32430 39270 ) M1M2_PR
      NEW li1 ( 32430 28730 ) L1M1_PR
      NEW met1 ( 32430 28730 ) M1M2_PR
      NEW li1 ( 40250 35870 ) L1M1_PR
      NEW met1 ( 32430 35870 ) M1M2_PR
      NEW met1 ( 32430 39270 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 32430 28730 ) RECT ( -355 -70 0 70 ) 
      NEW met2 ( 32430 35870 ) RECT ( -70 -485 70 0 )  ;
    - net17 ( _121_ D ) ( _106_ D ) ( hold3 X ) + USE SIGNAL
      + ROUTED met1 ( 8970 52190 ) ( 13570 * )
      NEW met2 ( 8970 42670 ) ( * 52190 )
      NEW met1 ( 13570 52190 ) ( * 52870 )
      NEW met1 ( 13570 52870 ) ( 15870 * )
      NEW li1 ( 13570 52190 ) L1M1_PR
      NEW met1 ( 8970 52190 ) M1M2_PR
      NEW li1 ( 8970 42670 ) L1M1_PR
      NEW met1 ( 8970 42670 ) M1M2_PR
      NEW li1 ( 15870 52870 ) L1M1_PR
      NEW met1 ( 8970 42670 ) RECT ( -355 -70 0 70 )  ;
    - net18 ( _122_ D ) ( _109_ D ) ( hold4 X ) + USE SIGNAL
      + ROUTED met2 ( 15870 36890 ) ( * 41310 )
      NEW met1 ( 15870 41310 ) ( 17250 * )
      NEW met2 ( 15870 34850 ) ( * 36890 )
      NEW met1 ( 8905 34850 ) ( 15870 * )
      NEW li1 ( 8905 34850 ) L1M1_PR
      NEW li1 ( 15870 36890 ) L1M1_PR
      NEW met1 ( 15870 36890 ) M1M2_PR
      NEW met1 ( 15870 41310 ) M1M2_PR
      NEW li1 ( 17250 41310 ) L1M1_PR
      NEW met1 ( 15870 34850 ) M1M2_PR
      NEW met1 ( 15870 36890 ) RECT ( -355 -70 0 70 )  ;
    - net19 ( _120_ D ) ( _111_ D ) ( hold5 X ) + USE SIGNAL
      + ROUTED met2 ( 18630 47430 ) ( * 49470 )
      NEW met1 ( 18170 49470 ) ( 18630 * )
      NEW met1 ( 14950 47430 ) ( 18630 * )
      NEW li1 ( 18630 47430 ) L1M1_PR
      NEW met1 ( 18630 47430 ) M1M2_PR
      NEW met1 ( 18630 49470 ) M1M2_PR
      NEW li1 ( 18170 49470 ) L1M1_PR
      NEW li1 ( 14950 47430 ) L1M1_PR
      NEW met1 ( 18630 47430 ) RECT ( -355 -70 0 70 )  ;
    - net2 ( _106_ CLK_N ) ( _093__2 Y ) + USE CLOCK
      + ROUTED met1 ( 14030 53210 ) ( 14950 * )
      NEW met2 ( 14950 53210 ) ( * 54910 )
      NEW li1 ( 14030 53210 ) L1M1_PR
      NEW met1 ( 14950 53210 ) M1M2_PR
      NEW li1 ( 14950 54910 ) L1M1_PR
      NEW met1 ( 14950 54910 ) M1M2_PR
      NEW met1 ( 14950 54910 ) RECT ( -355 -70 0 70 )  ;
    - net20 ( _119_ D ) ( _105_ D ) ( hold6 X ) + USE SIGNAL
      + ROUTED met1 ( 25990 50150 ) ( 29210 * )
      NEW met1 ( 25990 49810 ) ( * 50150 )
      NEW met1 ( 16330 49810 ) ( 25990 * )
      NEW met1 ( 16330 49810 ) ( * 50490 )
      NEW met1 ( 29210 48450 ) ( 31050 * )
      NEW met2 ( 29210 48450 ) ( * 50150 )
      NEW met1 ( 9430 50490 ) ( 16330 * )
      NEW li1 ( 9430 50490 ) L1M1_PR
      NEW li1 ( 29210 50150 ) L1M1_PR
      NEW li1 ( 31050 48450 ) L1M1_PR
      NEW met1 ( 29210 48450 ) M1M2_PR
      NEW met1 ( 29210 50150 ) M1M2_PR
      NEW met1 ( 29210 50150 ) RECT ( -595 -70 0 70 )  ;
    - net21 ( _127_ D ) ( _107_ D ) ( hold7 X ) + USE SIGNAL
      + ROUTED met1 ( 26910 31450 ) ( 30130 * )
      NEW met1 ( 30130 31110 ) ( * 31450 )
      NEW met1 ( 30130 31110 ) ( 32430 * )
      NEW met2 ( 27370 31450 ) ( * 33830 )
      NEW li1 ( 26910 31450 ) L1M1_PR
      NEW li1 ( 32430 31110 ) L1M1_PR
      NEW li1 ( 27370 33830 ) L1M1_PR
      NEW met1 ( 27370 33830 ) M1M2_PR
      NEW met1 ( 27370 31450 ) M1M2_PR
      NEW met1 ( 27370 33830 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 27370 31450 ) RECT ( -595 -70 0 70 )  ;
    - net22 ( _129_ D ) ( _112_ D ) ( hold8 X ) + USE SIGNAL
      + ROUTED met1 ( 34730 17850 ) ( 36110 * )
      NEW met2 ( 34730 17850 ) ( * 25670 )
      NEW met1 ( 31510 25670 ) ( 34730 * )
      NEW met1 ( 34730 20230 ) ( 41630 * )
      NEW li1 ( 36110 17850 ) L1M1_PR
      NEW met1 ( 34730 17850 ) M1M2_PR
      NEW met1 ( 34730 25670 ) M1M2_PR
      NEW li1 ( 31510 25670 ) L1M1_PR
      NEW li1 ( 41630 20230 ) L1M1_PR
      NEW met1 ( 34730 20230 ) M1M2_PR
      NEW met2 ( 34730 20230 ) RECT ( -70 -485 70 0 )  ;
    - net23 ( _123_ D ) ( _110_ D ) ( hold9 X ) + USE SIGNAL
      + ROUTED met2 ( 15870 31450 ) ( * 33150 )
      NEW met1 ( 15870 33150 ) ( 18170 * )
      NEW met2 ( 15870 29410 ) ( * 31450 )
      NEW met1 ( 9365 29410 ) ( 15870 * )
      NEW li1 ( 9365 29410 ) L1M1_PR
      NEW li1 ( 15870 31450 ) L1M1_PR
      NEW met1 ( 15870 31450 ) M1M2_PR
      NEW met1 ( 15870 33150 ) M1M2_PR
      NEW li1 ( 18170 33150 ) L1M1_PR
      NEW met1 ( 15870 29410 ) M1M2_PR
      NEW met1 ( 15870 31450 ) RECT ( -355 -70 0 70 )  ;
    - net24 ( _125_ D ) ( _116_ D ) ( hold10 X ) + USE SIGNAL
      + ROUTED met1 ( 18170 26350 ) ( * 26690 )
      NEW met1 ( 18170 26690 ) ( 26450 * )
      NEW met2 ( 19550 20230 ) ( * 26690 )
      NEW li1 ( 18170 26350 ) L1M1_PR
      NEW li1 ( 26450 26690 ) L1M1_PR
      NEW li1 ( 19550 20230 ) L1M1_PR
      NEW met1 ( 19550 20230 ) M1M2_PR
      NEW met1 ( 19550 26690 ) M1M2_PR
      NEW met1 ( 19550 20230 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 19550 26690 ) RECT ( -595 -70 0 70 )  ;
    - net25 ( _126_ D ) ( _117_ D ) ( hold11 X ) + USE SIGNAL
      + ROUTED met2 ( 28750 23970 ) ( * 28730 )
      NEW met1 ( 22310 28730 ) ( 28750 * )
      NEW met1 ( 25070 14790 ) ( 28290 * )
      NEW met2 ( 28290 14790 ) ( * 15300 )
      NEW met2 ( 28290 15300 ) ( 28750 * )
      NEW met2 ( 28750 15300 ) ( * 23970 )
      NEW li1 ( 28750 23970 ) L1M1_PR
      NEW met1 ( 28750 23970 ) M1M2_PR
      NEW met1 ( 28750 28730 ) M1M2_PR
      NEW li1 ( 22310 28730 ) L1M1_PR
      NEW li1 ( 25070 14790 ) L1M1_PR
      NEW met1 ( 28290 14790 ) M1M2_PR
      NEW met1 ( 28750 23970 ) RECT ( -355 -70 0 70 )  ;
    - net26 ( _124_ D ) ( _115_ D ) ( hold12 X ) + USE SIGNAL
      + ROUTED met1 ( 18630 9350 ) ( 21390 * )
      NEW met1 ( 20930 15810 ) ( 21850 * )
      NEW met2 ( 21850 15810 ) ( * 22270 )
      NEW met1 ( 18170 22270 ) ( 21850 * )
      NEW met1 ( 18170 22270 ) ( * 22610 )
      NEW met2 ( 21390 15300 ) ( 21850 * )
      NEW met2 ( 21850 15300 ) ( * 15810 )
      NEW met2 ( 21390 9350 ) ( * 15300 )
      NEW li1 ( 18630 9350 ) L1M1_PR
      NEW met1 ( 21390 9350 ) M1M2_PR
      NEW li1 ( 20930 15810 ) L1M1_PR
      NEW met1 ( 21850 15810 ) M1M2_PR
      NEW met1 ( 21850 22270 ) M1M2_PR
      NEW li1 ( 18170 22610 ) L1M1_PR ;
    - net27 ( _130_ D ) ( _113_ D ) ( hold13 X ) + USE SIGNAL
      + ROUTED met1 ( 34730 22950 ) ( 35190 * )
      NEW met2 ( 35190 22950 ) ( * 44370 )
      NEW met1 ( 33810 44370 ) ( 35190 * )
      NEW met1 ( 35190 26690 ) ( 41630 * )
      NEW li1 ( 34730 22950 ) L1M1_PR
      NEW met1 ( 35190 22950 ) M1M2_PR
      NEW met1 ( 35190 44370 ) M1M2_PR
      NEW li1 ( 33810 44370 ) L1M1_PR
      NEW li1 ( 41630 26690 ) L1M1_PR
      NEW met1 ( 35190 26690 ) M1M2_PR
      NEW met2 ( 35190 26690 ) RECT ( -70 -485 70 0 )  ;
    - net3 ( _107_ CLK_N ) ( _094__3 Y ) + USE CLOCK
      + ROUTED met1 ( 25530 33150 ) ( * 33830 )
      NEW met1 ( 25530 33150 ) ( 33350 * )
      NEW met1 ( 33350 33150 ) ( * 33490 )
      NEW met1 ( 33350 33490 ) ( 38870 * )
      NEW li1 ( 25530 33830 ) L1M1_PR
      NEW li1 ( 38870 33490 ) L1M1_PR ;
    - net4 ( _108_ CLK_N ) ( _095__4 Y ) + USE CLOCK
      + ROUTED met1 ( 29670 39610 ) ( 30590 * )
      NEW met2 ( 29670 39610 ) ( * 52190 )
      NEW li1 ( 30590 39610 ) L1M1_PR
      NEW met1 ( 29670 39610 ) M1M2_PR
      NEW li1 ( 29670 52190 ) L1M1_PR
      NEW met1 ( 29670 52190 ) M1M2_PR
      NEW met1 ( 29670 52190 ) RECT ( -355 -70 0 70 )  ;
    - net5 ( _109_ CLK_N ) ( _096__5 Y ) + USE CLOCK
      + ROUTED met1 ( 14030 36890 ) ( 14950 * )
      NEW met2 ( 14950 36890 ) ( * 38590 )
      NEW li1 ( 14030 36890 ) L1M1_PR
      NEW met1 ( 14950 36890 ) M1M2_PR
      NEW li1 ( 14950 38590 ) L1M1_PR
      NEW met1 ( 14950 38590 ) M1M2_PR
      NEW met1 ( 14950 38590 ) RECT ( -355 -70 0 70 )  ;
    - net6 ( _110_ CLK_N ) ( _097__6 Y ) + USE CLOCK
      + ROUTED met1 ( 13110 31110 ) ( 14030 * )
      NEW li1 ( 13110 31110 ) L1M1_PR
      NEW li1 ( 14030 31110 ) L1M1_PR ;
    - net7 ( _111_ CLK_N ) ( _098__7 Y ) + USE CLOCK
      + ROUTED met1 ( 16790 47770 ) ( 19090 * )
      NEW met1 ( 19090 47430 ) ( * 47770 )
      NEW met1 ( 19090 47430 ) ( 20930 * )
      NEW met2 ( 20930 47430 ) ( * 49470 )
      NEW met1 ( 20930 49470 ) ( 22310 * )
      NEW li1 ( 16790 47770 ) L1M1_PR
      NEW met1 ( 20930 47430 ) M1M2_PR
      NEW met1 ( 20930 49470 ) M1M2_PR
      NEW li1 ( 22310 49470 ) L1M1_PR ;
    - net8 ( _112_ CLK_N ) ( _099__8 Y ) + USE CLOCK
      + ROUTED met1 ( 34270 17510 ) ( 35190 * )
      NEW met2 ( 35190 13090 ) ( * 17510 )
      NEW li1 ( 35190 13090 ) L1M1_PR
      NEW met1 ( 35190 13090 ) M1M2_PR
      NEW met1 ( 35190 17510 ) M1M2_PR
      NEW li1 ( 34270 17510 ) L1M1_PR
      NEW met1 ( 35190 13090 ) RECT ( -355 -70 0 70 )  ;
    - net9 ( _113_ CLK_N ) ( _100__9 Y ) + USE CLOCK
      + ROUTED met1 ( 31970 21250 ) ( 32890 * )
      NEW met2 ( 32890 21250 ) ( * 22950 )
      NEW li1 ( 31970 21250 ) L1M1_PR
      NEW met1 ( 32890 21250 ) M1M2_PR
      NEW li1 ( 32890 22950 ) L1M1_PR
      NEW met1 ( 32890 22950 ) M1M2_PR
      NEW met1 ( 32890 22950 ) RECT ( -355 -70 0 70 )  ;
    - one ( PIN one ) ( const_source HI ) + USE SIGNAL
      + ROUTED met2 ( 45770 6460 ) ( * 9350 )
      NEW met3 ( 45770 6460 ) ( 70380 * 0 )
      NEW li1 ( 45770 9350 ) L1M1_PR
      NEW met1 ( 45770 9350 ) M1M2_PR
      NEW met2 ( 45770 6460 ) M2M3_PR
      NEW met1 ( 45770 9350 ) RECT ( -355 -70 0 70 )  ;
    - pad_gpio_ana_en ( PIN pad_gpio_ana_en ) ( _115_ Q ) + USE SIGNAL
      + ROUTED met2 ( 34270 10370 ) ( * 11900 )
      NEW met1 ( 28810 10370 ) ( 34270 * )
      NEW met3 ( 34270 11900 ) ( 34500 * )
      NEW met3 ( 34500 11900 ) ( * 12580 )
      NEW met3 ( 34500 12580 ) ( 70380 * 0 )
      NEW met2 ( 34270 11900 ) M2M3_PR
      NEW met1 ( 34270 10370 ) M1M2_PR
      NEW li1 ( 28810 10370 ) L1M1_PR ;
    - pad_gpio_ana_pol ( PIN pad_gpio_ana_pol ) ( _117_ Q ) + USE SIGNAL
      + ROUTED met2 ( 41170 14450 ) ( * 14620 )
      NEW met1 ( 35250 14450 ) ( 41170 * )
      NEW met3 ( 41170 14620 ) ( 70380 * 0 )
      NEW met2 ( 41170 14620 ) M2M3_PR
      NEW met1 ( 41170 14450 ) M1M2_PR
      NEW li1 ( 35250 14450 ) L1M1_PR ;
    - pad_gpio_ana_sel ( PIN pad_gpio_ana_sel ) ( _116_ Q ) + USE SIGNAL
      + ROUTED met2 ( 29670 16660 ) ( * 19550 )
      NEW met1 ( 29670 19550 ) ( 29710 * )
      NEW met3 ( 29670 16660 ) ( 70380 * 0 )
      NEW met2 ( 29670 16660 ) M2M3_PR
      NEW met1 ( 29670 19550 ) M1M2_PR
      NEW li1 ( 29710 19550 ) L1M1_PR
      NEW met1 ( 29670 19550 ) RECT ( -315 -70 0 70 )  ;
    - pad_gpio_dm[0] ( PIN pad_gpio_dm[0] ) ( _112_ Q ) + USE SIGNAL
      + ROUTED met2 ( 83030 16830 ) ( * 18700 )
      NEW met3 ( 83030 18700 ) ( 83260 * 0 )
      NEW met1 ( 82800 16830 ) ( 83030 * )
      NEW met1 ( 82800 16830 ) ( * 17170 )
      NEW met1 ( 46290 17170 ) ( 82800 * )
      NEW met1 ( 83030 16830 ) M1M2_PR
      NEW met2 ( 83030 18700 ) M2M3_PR
      NEW li1 ( 46290 17170 ) L1M1_PR ;
    - pad_gpio_dm[1] ( PIN pad_gpio_dm[1] ) ( _113_ Q ) ( _064_ B ) + USE SIGNAL
      + ROUTED met2 ( 45310 13090 ) ( * 13800 )
      NEW met1 ( 44850 22270 ) ( 44890 * )
      NEW met2 ( 44850 20740 ) ( * 22270 )
      NEW met2 ( 44390 13800 ) ( 45310 * )
      NEW met2 ( 44390 13800 ) ( * 17340 )
      NEW met2 ( 44390 17340 ) ( 44850 * )
      NEW met2 ( 44850 17340 ) ( * 20740 )
      NEW met3 ( 44850 20740 ) ( 70380 * 0 )
      NEW li1 ( 45310 13090 ) L1M1_PR
      NEW met1 ( 45310 13090 ) M1M2_PR
      NEW li1 ( 44890 22270 ) L1M1_PR
      NEW met1 ( 44850 22270 ) M1M2_PR
      NEW met2 ( 44850 20740 ) M2M3_PR
      NEW met1 ( 45310 13090 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 44890 22270 ) RECT ( 0 -70 315 70 )  ;
    - pad_gpio_dm[2] ( PIN pad_gpio_dm[2] ) ( ANTENNA__064__A_N DIODE ) ( _114_ Q ) ( _064_ A_N ) + USE SIGNAL
      + ROUTED met1 ( 43470 10370 ) ( 43930 * )
      NEW met2 ( 43470 10370 ) ( * 12070 )
      NEW met1 ( 43470 46750 ) ( 47190 * )
      NEW met2 ( 43470 12070 ) ( * 46750 )
      NEW met3 ( 43470 22780 ) ( 70380 * 0 )
      NEW li1 ( 43470 12070 ) L1M1_PR
      NEW met1 ( 43470 12070 ) M1M2_PR
      NEW li1 ( 43930 10370 ) L1M1_PR
      NEW met1 ( 43470 10370 ) M1M2_PR
      NEW met1 ( 43470 46750 ) M1M2_PR
      NEW li1 ( 47190 46750 ) L1M1_PR
      NEW met2 ( 43470 22780 ) M2M3_PR
      NEW met1 ( 43470 12070 ) RECT ( -355 -70 0 70 ) 
      NEW met2 ( 43470 22780 ) RECT ( -70 -485 70 0 )  ;
    - pad_gpio_holdover ( PIN pad_gpio_holdover ) ( _106_ Q ) + USE SIGNAL
      + ROUTED met3 ( 62100 24820 ) ( 70380 * 0 )
      NEW met3 ( 62100 24820 ) ( * 25500 )
      NEW met3 ( 22770 25500 ) ( 62100 * )
      NEW met2 ( 22770 25500 ) ( * 48450 )
      NEW met1 ( 22770 48450 ) ( 24610 * )
      NEW met2 ( 24610 48450 ) ( * 52190 )
      NEW met1 ( 24610 52190 ) ( 26030 * )
      NEW met2 ( 22770 25500 ) M2M3_PR
      NEW met1 ( 22770 48450 ) M1M2_PR
      NEW met1 ( 24610 48450 ) M1M2_PR
      NEW met1 ( 24610 52190 ) M1M2_PR
      NEW li1 ( 26030 52190 ) L1M1_PR ;
    - pad_gpio_ib_mode_sel ( PIN pad_gpio_ib_mode_sel ) ( _110_ Q ) + USE SIGNAL
      + ROUTED met2 ( 27370 26860 ) ( * 30430 )
      NEW met1 ( 26050 30430 ) ( 27370 * )
      NEW met3 ( 27370 26860 ) ( 70380 * 0 )
      NEW met2 ( 27370 26860 ) M2M3_PR
      NEW met1 ( 27370 30430 ) M1M2_PR
      NEW li1 ( 26050 30430 ) L1M1_PR ;
    - pad_gpio_in ( PIN pad_gpio_in ) ( ANTENNA__058__A DIODE ) ( ANTENNA__135__A DIODE ) ( _135_ A ) ( _058_ A ) + USE SIGNAL
      + ROUTED met1 ( 45770 12750 ) ( 47150 * )
      NEW met1 ( 45770 10030 ) ( 47150 * )
      NEW met2 ( 45770 10030 ) ( * 12750 )
      NEW met1 ( 44390 27710 ) ( * 28050 )
      NEW met1 ( 44390 27710 ) ( 45770 * )
      NEW met2 ( 45770 27710 ) ( * 28900 )
      NEW met1 ( 45770 22950 ) ( 46690 * )
      NEW met2 ( 45770 22950 ) ( * 27710 )
      NEW met2 ( 45770 15300 ) ( 46230 * )
      NEW met2 ( 46230 15300 ) ( * 15980 )
      NEW met2 ( 46230 15980 ) ( 46690 * )
      NEW met2 ( 46690 15980 ) ( * 22950 )
      NEW met2 ( 45770 12750 ) ( * 15300 )
      NEW met3 ( 45770 28900 ) ( 70380 * 0 )
      NEW li1 ( 47150 12750 ) L1M1_PR
      NEW met1 ( 45770 12750 ) M1M2_PR
      NEW li1 ( 47150 10030 ) L1M1_PR
      NEW met1 ( 45770 10030 ) M1M2_PR
      NEW li1 ( 44390 28050 ) L1M1_PR
      NEW met1 ( 45770 27710 ) M1M2_PR
      NEW met2 ( 45770 28900 ) M2M3_PR
      NEW li1 ( 46690 22950 ) L1M1_PR
      NEW met1 ( 45770 22950 ) M1M2_PR
      NEW met1 ( 46690 22950 ) M1M2_PR
      NEW met1 ( 46690 22950 ) RECT ( -595 -70 0 70 )  ;
    - pad_gpio_inenb ( PIN pad_gpio_inenb ) ( ANTENNA__061__A_N DIODE ) ( _109_ Q ) ( _061_ A_N ) + USE SIGNAL
      + ROUTED met2 ( 83030 27710 ) ( * 30940 )
      NEW met3 ( 83030 30940 ) ( 83260 * 0 )
      NEW met1 ( 62100 27710 ) ( 83030 * )
      NEW met1 ( 42090 29070 ) ( 62100 * )
      NEW met1 ( 62100 27710 ) ( * 29070 )
      NEW met2 ( 40710 29070 ) ( * 33830 )
      NEW met1 ( 40710 29070 ) ( 42090 * )
      NEW met1 ( 26050 36210 ) ( 31970 * )
      NEW met2 ( 31970 34510 ) ( * 36210 )
      NEW met1 ( 31970 34510 ) ( 34730 * )
      NEW met1 ( 34730 34170 ) ( * 34510 )
      NEW met1 ( 34730 34170 ) ( 40710 * )
      NEW met1 ( 40710 33830 ) ( * 34170 )
      NEW met1 ( 83030 27710 ) M1M2_PR
      NEW met2 ( 83030 30940 ) M2M3_PR
      NEW li1 ( 42090 29070 ) L1M1_PR
      NEW li1 ( 40710 33830 ) L1M1_PR
      NEW met1 ( 40710 33830 ) M1M2_PR
      NEW met1 ( 40710 29070 ) M1M2_PR
      NEW li1 ( 26050 36210 ) L1M1_PR
      NEW met1 ( 31970 36210 ) M1M2_PR
      NEW met1 ( 31970 34510 ) M1M2_PR
      NEW met1 ( 40710 33830 ) RECT ( -355 -70 0 70 )  ;
    - pad_gpio_out ( PIN pad_gpio_out ) ( _066_ X ) + USE SIGNAL
      + ROUTED met2 ( 83030 32130 ) ( * 32980 )
      NEW met3 ( 83030 32980 ) ( 83260 * 0 )
      NEW met1 ( 82800 32130 ) ( 83030 * )
      NEW met1 ( 82800 32130 ) ( * 33150 )
      NEW met1 ( 47610 33150 ) ( 82800 * )
      NEW met1 ( 83030 32130 ) M1M2_PR
      NEW met2 ( 83030 32980 ) M2M3_PR
      NEW li1 ( 47610 33150 ) L1M1_PR ;
    - pad_gpio_outenb ( PIN pad_gpio_outenb ) ( _063_ X ) + USE SIGNAL
      + ROUTED met3 ( 97060 35020 0 ) ( 97290 * )
      NEW met2 ( 97290 30770 ) ( * 35020 )
      NEW met1 ( 46690 30770 ) ( 97290 * )
      NEW met1 ( 97290 30770 ) M1M2_PR
      NEW met2 ( 97290 35020 ) M2M3_PR
      NEW li1 ( 46690 30770 ) L1M1_PR ;
    - pad_gpio_slow_sel ( PIN pad_gpio_slow_sel ) ( _107_ Q ) + USE SIGNAL
      + ROUTED met2 ( 41170 33150 ) ( * 37060 )
      NEW met1 ( 37550 33150 ) ( 41170 * )
      NEW met3 ( 41170 37060 ) ( 70380 * 0 )
      NEW met2 ( 41170 37060 ) M2M3_PR
      NEW met1 ( 41170 33150 ) M1M2_PR
      NEW li1 ( 37550 33150 ) L1M1_PR ;
    - pad_gpio_vtrip_sel ( PIN pad_gpio_vtrip_sel ) ( _108_ Q ) + USE SIGNAL
      + ROUTED met2 ( 83030 38590 ) ( * 39100 )
      NEW met3 ( 83030 39100 ) ( 83260 * 0 )
      NEW met1 ( 62790 38590 ) ( * 38930 )
      NEW met1 ( 62790 38590 ) ( 83030 * )
      NEW met1 ( 42610 38930 ) ( 62790 * )
      NEW met1 ( 83030 38590 ) M1M2_PR
      NEW met2 ( 83030 39100 ) M2M3_PR
      NEW li1 ( 42610 38930 ) L1M1_PR ;
    - resetn ( PIN resetn ) ( ANTENNA__086__A_N DIODE ) ( ANTENNA__074__A_N DIODE ) ( ANTENNA__073__A DIODE ) ( ANTENNA__132__A DIODE ) ( ANTENNA__071__A DIODE ) ( ANTENNA__130__RESET_B DIODE )
      ( ANTENNA__085__A DIODE ) ( ANTENNA__131__RESET_B DIODE ) ( ANTENNA__067__A DIODE ) ( ANTENNA__118__RESET_B DIODE ) ( ANTENNA__072__A_N DIODE ) ( ANTENNA__079__A DIODE ) ( ANTENNA__068__A_N DIODE ) ( ANTENNA__119__RESET_B DIODE )
      ( ANTENNA__070__A_N DIODE ) ( ANTENNA__080__A_N DIODE ) ( ANTENNA__069__A DIODE ) ( ANTENNA__120__RESET_B DIODE ) ( ANTENNA__122__RESET_B DIODE ) ( ANTENNA__077__A DIODE ) ( ANTENNA__076__A_N DIODE ) ( ANTENNA__075__A DIODE )
      ( ANTENNA__121__RESET_B DIODE ) ( ANTENNA__123__RESET_B DIODE ) ( ANTENNA__129__RESET_B DIODE ) ( ANTENNA__083__A DIODE ) ( ANTENNA__128__RESET_B DIODE ) ( ANTENNA__084__A_N DIODE ) ( ANTENNA__081__A DIODE ) ( ANTENNA__091__A DIODE )
      ( ANTENNA__082__A_N DIODE ) ( ANTENNA__078__A_N DIODE ) ( ANTENNA__126__RESET_B DIODE ) ( ANTENNA__127__RESET_B DIODE ) ( ANTENNA__089__A DIODE ) ( ANTENNA__125__RESET_B DIODE ) ( ANTENNA__092__A_N DIODE ) ( ANTENNA__087__A DIODE )
      ( ANTENNA__088__A_N DIODE ) ( ANTENNA__124__RESET_B DIODE ) ( ANTENNA__090__A_N DIODE ) ( _090_ A_N ) ( _124_ RESET_B ) ( _088_ A_N ) ( _087_ A ) ( _092_ A_N )
      ( _125_ RESET_B ) ( _089_ A ) ( _127_ RESET_B ) ( _126_ RESET_B ) ( _078_ A_N ) ( _082_ A_N ) ( _091_ A ) ( _081_ A )
      ( _084_ A_N ) ( _128_ RESET_B ) ( _083_ A ) ( _129_ RESET_B ) ( _123_ RESET_B ) ( _121_ RESET_B ) ( _075_ A ) ( _076_ A_N )
      ( _077_ A ) ( _122_ RESET_B ) ( _120_ RESET_B ) ( _069_ A ) ( _080_ A_N ) ( _070_ A_N ) ( _119_ RESET_B ) ( _068_ A_N )
      ( _079_ A ) ( _072_ A_N ) ( _118_ RESET_B ) ( _067_ A ) ( _131_ RESET_B ) ( _085_ A ) ( _130_ RESET_B ) ( _071_ A )
      ( _132_ A ) ( _073_ A ) ( _074_ A_N ) ( _086_ A_N ) + USE SIGNAL
      + ROUTED met1 ( 46690 49470 ) ( 47150 * )
      NEW met1 ( 44850 49810 ) ( 46690 * )
      NEW met1 ( 46690 49470 ) ( * 49810 )
      NEW met1 ( 42550 50150 ) ( 44850 * )
      NEW met1 ( 44850 49810 ) ( * 50150 )
      NEW met1 ( 45310 53210 0 ) ( 47150 * )
      NEW met2 ( 47150 49470 ) ( * 53210 )
      NEW met1 ( 35190 52870 ) ( * 53210 )
      NEW met1 ( 35190 52870 ) ( 45310 * )
      NEW met1 ( 45310 52870 ) ( * 53210 0 )
      NEW met2 ( 36570 52870 ) ( * 54910 )
      NEW met1 ( 36570 54910 ) ( 37950 * )
      NEW met1 ( 34730 54910 ) ( 36570 * )
      NEW met1 ( 36570 55930 ) ( 41630 * )
      NEW met2 ( 36570 54910 ) ( * 55930 )
      NEW met1 ( 41630 55930 ) ( 42550 * )
      NEW met1 ( 42550 55930 ) ( 47150 * )
      NEW met1 ( 32430 54910 ) ( 34730 * )
      NEW met1 ( 31510 52870 ) ( * 53210 )
      NEW met1 ( 31510 52870 ) ( 35190 * )
      NEW met1 ( 30130 52190 ) ( 30590 * )
      NEW met1 ( 30590 52190 ) ( * 52530 )
      NEW met1 ( 30590 52530 ) ( 31510 * )
      NEW met1 ( 31510 52530 ) ( * 52870 )
      NEW met1 ( 27830 52870 ) ( * 53210 )
      NEW met1 ( 27830 52870 ) ( 31510 * )
      NEW met1 ( 26910 51170 ) ( 30130 * )
      NEW met1 ( 25530 50150 ) ( * 50490 )
      NEW met1 ( 25530 50490 ) ( 26910 * )
      NEW met1 ( 26910 50490 ) ( * 51170 )
      NEW met1 ( 24610 55250 ) ( 28290 * )
      NEW met2 ( 28290 52870 ) ( * 55250 )
      NEW met1 ( 18630 54910 ) ( * 55250 )
      NEW met1 ( 18630 54910 ) ( 22310 * )
      NEW met1 ( 22310 54910 ) ( * 55250 )
      NEW met1 ( 22310 55250 ) ( 24610 * )
      NEW met1 ( 17250 55250 ) ( 18630 * )
      NEW met1 ( 20470 54910 ) ( * 55590 )
      NEW met1 ( 46230 42330 ) ( 47150 * )
      NEW met1 ( 44850 42330 ) ( 46230 * )
      NEW met2 ( 47150 37570 ) ( * 42330 )
      NEW met1 ( 46230 36890 ) ( 47150 * )
      NEW met1 ( 47150 36890 ) ( * 37570 )
      NEW met2 ( 47610 32130 ) ( * 37570 )
      NEW met2 ( 47150 37570 ) ( 47610 * )
      NEW met1 ( 42090 31450 ) ( 42550 * )
      NEW met2 ( 42090 31450 ) ( * 31620 )
      NEW met3 ( 42090 31620 ) ( 47610 * )
      NEW met2 ( 47610 31620 ) ( * 32130 )
      NEW met1 ( 39790 44370 0 ) ( 43930 * )
      NEW met2 ( 43930 42330 ) ( * 44370 )
      NEW met1 ( 43930 42330 ) ( 44850 * )
      NEW met1 ( 37950 31450 0 ) ( 42090 * )
      NEW met2 ( 41170 29410 ) ( * 31450 )
      NEW met1 ( 38410 28050 0 ) ( 41170 * )
      NEW met2 ( 41170 28050 ) ( * 29410 )
      NEW met1 ( 40710 26350 ) ( 41170 * )
      NEW met2 ( 41170 26350 ) ( * 28050 )
      NEW met1 ( 41170 26010 ) ( 46230 * )
      NEW met1 ( 41170 26010 ) ( * 26350 )
      NEW met1 ( 37490 26350 0 ) ( 40710 * )
      NEW met1 ( 46230 23970 ) ( 47150 * )
      NEW met2 ( 46230 23970 ) ( * 26010 )
      NEW met1 ( 43930 21250 ) ( 45310 * )
      NEW met2 ( 43930 21250 ) ( * 26010 )
      NEW met1 ( 45310 21250 ) ( 46230 * )
      NEW met1 ( 40710 15470 ) ( 43930 * )
      NEW met2 ( 43930 15470 ) ( * 21250 )
      NEW met1 ( 36570 12750 ) ( * 13090 )
      NEW met1 ( 36570 12750 ) ( 40710 * )
      NEW met2 ( 40710 12750 ) ( * 15470 )
      NEW met1 ( 37950 12070 ) ( * 12750 )
      NEW met1 ( 34270 12750 ) ( 36570 * )
      NEW met1 ( 32430 12750 ) ( 34270 * )
      NEW met2 ( 32890 12750 ) ( * 17170 )
      NEW met1 ( 31050 17510 ) ( 32890 * )
      NEW met1 ( 32890 17170 ) ( * 17510 )
      NEW met1 ( 31050 12070 ) ( 32430 * )
      NEW met1 ( 32430 12070 ) ( * 12750 )
      NEW met1 ( 31050 19550 ) ( 32890 * )
      NEW met2 ( 32890 17170 ) ( * 19550 )
      NEW met1 ( 41630 11730 ) ( * 12410 )
      NEW met1 ( 40710 12410 ) ( 41630 * )
      NEW met1 ( 40710 12410 ) ( * 12750 )
      NEW met2 ( 41630 10370 ) ( * 11730 )
      NEW met1 ( 41630 10370 ) ( 43010 * )
      NEW met1 ( 27830 12410 ) ( 31050 * )
      NEW met1 ( 31050 12070 ) ( * 12410 )
      NEW met1 ( 28290 28050 0 ) ( 32430 * )
      NEW met1 ( 32430 27710 ) ( * 28050 )
      NEW met1 ( 32430 27710 ) ( 38870 * )
      NEW met1 ( 38870 27710 ) ( * 28050 )
      NEW met1 ( 26910 12410 ) ( 27830 * )
      NEW met1 ( 26910 17170 ) ( 31050 * )
      NEW met1 ( 31050 17170 ) ( * 17510 )
      NEW met1 ( 32890 15130 ) ( 36420 * )
      NEW met1 ( 24150 22610 0 ) ( 27830 * )
      NEW met2 ( 27830 17170 ) ( * 22610 )
      NEW met1 ( 24150 26350 0 ) ( 24610 * )
      NEW met2 ( 24610 22610 ) ( * 26350 )
      NEW met1 ( 21850 12070 ) ( * 12410 )
      NEW met1 ( 21850 12410 ) ( 26910 * )
      NEW met1 ( 20470 39270 ) ( 24610 * )
      NEW met2 ( 24610 26350 ) ( * 39270 )
      NEW met1 ( 19550 28050 ) ( 24610 * 0 )
      NEW met1 ( 18170 12070 ) ( * 12410 )
      NEW met1 ( 18170 12410 ) ( 21850 * )
      NEW met1 ( 17250 12410 ) ( 18170 * )
      NEW met1 ( 16330 38930 ) ( 18630 * )
      NEW met1 ( 18630 38930 ) ( * 39270 )
      NEW met1 ( 18630 39270 ) ( 20470 * )
      NEW met1 ( 15410 28050 0 ) ( 18170 * )
      NEW met1 ( 18170 27710 ) ( * 28050 )
      NEW met1 ( 18170 27710 ) ( 19550 * )
      NEW met1 ( 19550 27710 ) ( * 28050 )
      NEW met1 ( 14950 33490 0 ) ( 16790 * )
      NEW met2 ( 16790 33490 ) ( * 38930 )
      NEW met1 ( 26450 7310 ) ( 27370 * )
      NEW met2 ( 27370 7310 ) ( * 12410 )
      NEW met2 ( 12190 31790 ) ( * 33150 )
      NEW met1 ( 12190 33150 ) ( 15410 * )
      NEW met1 ( 15410 33150 ) ( * 33490 )
      NEW met1 ( 10350 31790 ) ( 12190 * )
      NEW met1 ( 7590 29410 ) ( 8050 * )
      NEW met2 ( 8050 29410 ) ( * 31790 )
      NEW met1 ( 8050 31790 ) ( 10350 * )
      NEW met1 ( 28290 44370 0 ) ( 30130 * )
      NEW met2 ( 30130 44370 ) ( * 48110 )
      NEW met1 ( 21850 44030 ) ( 28750 * )
      NEW met1 ( 28750 44030 ) ( * 44370 )
      NEW met1 ( 20010 44710 ) ( 21850 * )
      NEW met1 ( 21850 44030 ) ( * 44710 )
      NEW met1 ( 18630 44370 ) ( 20010 * )
      NEW met1 ( 20010 44370 ) ( * 44710 )
      NEW met1 ( 16330 44370 ) ( * 44710 )
      NEW met1 ( 16330 44370 ) ( 18630 * )
      NEW met1 ( 14950 44710 ) ( 16330 * )
      NEW met2 ( 14490 42330 ) ( * 44710 )
      NEW met1 ( 14490 44710 ) ( 14950 * )
      NEW met1 ( 13110 44710 ) ( 14490 * )
      NEW met2 ( 11730 44710 ) ( * 48110 )
      NEW met1 ( 11730 44710 ) ( 13110 * )
      NEW met1 ( 27830 36890 ) ( 28290 * )
      NEW met2 ( 28290 36890 ) ( * 44370 )
      NEW met1 ( 24150 33830 ) ( * 34170 )
      NEW met1 ( 24150 34170 ) ( 28290 * )
      NEW met2 ( 28290 34170 ) ( * 36890 )
      NEW met2 ( 11730 48110 ) ( * 49810 )
      NEW met2 ( 30130 48110 ) ( * 52190 )
      NEW met2 ( 47150 42330 ) ( * 49470 )
      NEW met3 ( 47150 41140 ) ( 70380 * 0 )
      NEW met1 ( 11730 49810 ) M1M2_PR
      NEW li1 ( 47150 49470 ) L1M1_PR
      NEW met1 ( 47150 49470 ) M1M2_PR
      NEW li1 ( 46690 49470 ) L1M1_PR
      NEW li1 ( 44850 49810 ) L1M1_PR
      NEW li1 ( 42550 50150 ) L1M1_PR
      NEW met1 ( 47150 53210 ) M1M2_PR
      NEW li1 ( 35190 53210 ) L1M1_PR
      NEW li1 ( 36570 54910 ) L1M1_PR
      NEW met1 ( 36570 54910 ) M1M2_PR
      NEW met1 ( 36570 52870 ) M1M2_PR
      NEW li1 ( 37950 54910 ) L1M1_PR
      NEW li1 ( 34730 54910 ) L1M1_PR
      NEW li1 ( 41630 55930 ) L1M1_PR
      NEW met1 ( 36570 55930 ) M1M2_PR
      NEW li1 ( 42550 55930 ) L1M1_PR
      NEW li1 ( 47150 55930 ) L1M1_PR
      NEW li1 ( 32430 54910 ) L1M1_PR
      NEW li1 ( 31510 53210 ) L1M1_PR
      NEW met1 ( 30130 52190 ) M1M2_PR
      NEW li1 ( 27830 53210 ) L1M1_PR
      NEW li1 ( 26910 51170 ) L1M1_PR
      NEW met1 ( 30130 51170 ) M1M2_PR
      NEW li1 ( 25530 50150 ) L1M1_PR
      NEW li1 ( 24610 55250 ) L1M1_PR
      NEW met1 ( 28290 55250 ) M1M2_PR
      NEW met1 ( 28290 52870 ) M1M2_PR
      NEW li1 ( 18630 55250 ) L1M1_PR
      NEW li1 ( 17250 55250 ) L1M1_PR
      NEW li1 ( 20470 55590 ) L1M1_PR
      NEW li1 ( 46230 42330 ) L1M1_PR
      NEW met1 ( 47150 42330 ) M1M2_PR
      NEW li1 ( 44850 42330 ) L1M1_PR
      NEW li1 ( 47150 37570 ) L1M1_PR
      NEW met1 ( 47150 37570 ) M1M2_PR
      NEW li1 ( 46230 36890 ) L1M1_PR
      NEW met2 ( 47150 41140 ) M2M3_PR
      NEW li1 ( 47610 32130 ) L1M1_PR
      NEW met1 ( 47610 32130 ) M1M2_PR
      NEW li1 ( 42550 31450 ) L1M1_PR
      NEW met1 ( 42090 31450 ) M1M2_PR
      NEW met2 ( 42090 31620 ) M2M3_PR
      NEW met2 ( 47610 31620 ) M2M3_PR
      NEW met1 ( 43930 44370 ) M1M2_PR
      NEW met1 ( 43930 42330 ) M1M2_PR
      NEW li1 ( 41170 29410 ) L1M1_PR
      NEW met1 ( 41170 29410 ) M1M2_PR
      NEW met1 ( 41170 31450 ) M1M2_PR
      NEW met1 ( 41170 28050 ) M1M2_PR
      NEW li1 ( 40710 26350 ) L1M1_PR
      NEW met1 ( 41170 26350 ) M1M2_PR
      NEW li1 ( 46230 26010 ) L1M1_PR
      NEW li1 ( 47150 23970 ) L1M1_PR
      NEW met1 ( 46230 23970 ) M1M2_PR
      NEW met1 ( 46230 26010 ) M1M2_PR
      NEW li1 ( 45310 21250 ) L1M1_PR
      NEW met1 ( 43930 21250 ) M1M2_PR
      NEW met1 ( 43930 26010 ) M1M2_PR
      NEW li1 ( 46230 21250 ) L1M1_PR
      NEW li1 ( 40710 15470 ) L1M1_PR
      NEW met1 ( 43930 15470 ) M1M2_PR
      NEW li1 ( 41630 15470 ) L1M1_PR
      NEW li1 ( 36570 13090 ) L1M1_PR
      NEW met1 ( 40710 12750 ) M1M2_PR
      NEW met1 ( 40710 15470 ) M1M2_PR
      NEW li1 ( 37950 12070 ) L1M1_PR
      NEW li1 ( 34270 12750 ) L1M1_PR
      NEW li1 ( 32430 12750 ) L1M1_PR
      NEW li1 ( 32890 17170 ) L1M1_PR
      NEW met1 ( 32890 17170 ) M1M2_PR
      NEW met1 ( 32890 12750 ) M1M2_PR
      NEW li1 ( 31050 17510 ) L1M1_PR
      NEW li1 ( 31050 12070 ) L1M1_PR
      NEW li1 ( 31050 19550 ) L1M1_PR
      NEW met1 ( 32890 19550 ) M1M2_PR
      NEW li1 ( 41630 11730 ) L1M1_PR
      NEW li1 ( 41630 10370 ) L1M1_PR
      NEW met1 ( 41630 10370 ) M1M2_PR
      NEW met1 ( 41630 11730 ) M1M2_PR
      NEW li1 ( 43010 10370 ) L1M1_PR
      NEW li1 ( 27830 12410 ) L1M1_PR
      NEW li1 ( 26910 12410 ) L1M1_PR
      NEW li1 ( 26910 17170 ) L1M1_PR
      NEW li1 ( 36420 15130 ) L1M1_PR
      NEW met1 ( 32890 15130 ) M1M2_PR
      NEW met1 ( 27830 22610 ) M1M2_PR
      NEW met1 ( 27830 17170 ) M1M2_PR
      NEW met1 ( 24610 26350 ) M1M2_PR
      NEW met1 ( 24610 22610 ) M1M2_PR
      NEW li1 ( 21850 12070 ) L1M1_PR
      NEW li1 ( 20470 39270 ) L1M1_PR
      NEW met1 ( 24610 39270 ) M1M2_PR
      NEW li1 ( 19550 28050 ) L1M1_PR
      NEW met1 ( 24610 28050 ) M1M2_PR
      NEW li1 ( 18170 12070 ) L1M1_PR
      NEW li1 ( 17250 12410 ) L1M1_PR
      NEW li1 ( 16330 38930 ) L1M1_PR
      NEW met1 ( 16790 33490 ) M1M2_PR
      NEW met1 ( 16790 38930 ) M1M2_PR
      NEW li1 ( 26450 7310 ) L1M1_PR
      NEW met1 ( 27370 7310 ) M1M2_PR
      NEW met1 ( 27370 12410 ) M1M2_PR
      NEW li1 ( 12190 31790 ) L1M1_PR
      NEW met1 ( 12190 31790 ) M1M2_PR
      NEW met1 ( 12190 33150 ) M1M2_PR
      NEW li1 ( 10350 31790 ) L1M1_PR
      NEW li1 ( 7590 29410 ) L1M1_PR
      NEW met1 ( 8050 29410 ) M1M2_PR
      NEW met1 ( 8050 31790 ) M1M2_PR
      NEW li1 ( 30130 48110 ) L1M1_PR
      NEW met1 ( 30130 48110 ) M1M2_PR
      NEW met1 ( 30130 44370 ) M1M2_PR
      NEW li1 ( 21850 44030 ) L1M1_PR
      NEW li1 ( 20010 44710 ) L1M1_PR
      NEW li1 ( 18630 44370 ) L1M1_PR
      NEW li1 ( 16330 44710 ) L1M1_PR
      NEW li1 ( 14950 44710 ) L1M1_PR
      NEW met1 ( 14490 42330 ) M1M2_PR
      NEW met1 ( 14490 44710 ) M1M2_PR
      NEW li1 ( 13110 44710 ) L1M1_PR
      NEW met1 ( 11730 48110 ) M1M2_PR
      NEW met1 ( 11730 44710 ) M1M2_PR
      NEW li1 ( 27830 36890 ) L1M1_PR
      NEW met1 ( 28290 36890 ) M1M2_PR
      NEW met1 ( 28290 44370 ) M1M2_PR
      NEW li1 ( 24150 33830 ) L1M1_PR
      NEW met1 ( 28290 34170 ) M1M2_PR
      NEW met1 ( 47150 49470 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 36570 54910 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 36570 52870 ) RECT ( -595 -70 0 70 ) 
      NEW met2 ( 30130 51170 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 28290 52870 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 47150 37570 ) RECT ( -355 -70 0 70 ) 
      NEW met2 ( 47150 41140 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 47610 32130 ) RECT ( 0 -70 355 70 ) 
      NEW met1 ( 41170 29410 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 41170 31450 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 46230 26010 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 43930 26010 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 41630 15470 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 40710 15470 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 32890 17170 ) RECT ( 0 -70 355 70 ) 
      NEW met1 ( 32890 12750 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 41630 10370 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 41630 11730 ) RECT ( -595 -70 0 70 ) 
      NEW met2 ( 32890 15130 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 27830 17170 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 24610 22610 ) RECT ( -595 -70 0 70 ) 
      NEW met2 ( 24610 28050 ) RECT ( -70 -485 70 0 ) 
      NEW met1 ( 16790 38930 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 27370 12410 ) RECT ( -595 -70 0 70 ) 
      NEW met1 ( 12190 31790 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 30130 48110 ) RECT ( -355 -70 0 70 )  ;
    - resetn_out ( PIN resetn_out ) ( _132_ X ) + USE SIGNAL
      + ROUTED met2 ( 83030 41650 ) ( * 43180 )
      NEW met3 ( 83030 43180 ) ( 83260 * 0 )
      NEW met1 ( 47150 41650 ) ( 83030 * )
      NEW met1 ( 83030 41650 ) M1M2_PR
      NEW met2 ( 83030 43180 ) M2M3_PR
      NEW li1 ( 47150 41650 ) L1M1_PR ;
    - serial_clock ( PIN serial_clock ) ( ANTENNA_clkbuf_0_serial_clock_A DIODE ) ( clkbuf_0_serial_clock A ) + USE CLOCK
      + ROUTED met2 ( 83490 38930 ) ( * 45220 )
      NEW met3 ( 83260 45220 0 ) ( 83490 * )
      NEW met1 ( 82800 38930 ) ( 83490 * )
      NEW met1 ( 82800 38930 ) ( * 39270 )
      NEW met1 ( 30130 38930 ) ( * 39270 )
      NEW met1 ( 30130 39270 ) ( 31050 * )
      NEW met1 ( 31050 39270 ) ( * 40290 )
      NEW met1 ( 31050 40290 ) ( 44390 * )
      NEW met1 ( 44390 39270 ) ( * 40290 )
      NEW met1 ( 17250 40290 ) ( 31050 * )
      NEW met1 ( 44390 39270 ) ( 82800 * )
      NEW met1 ( 83490 38930 ) M1M2_PR
      NEW met2 ( 83490 45220 ) M2M3_PR
      NEW li1 ( 30130 38930 ) L1M1_PR
      NEW li1 ( 17250 40290 ) L1M1_PR ;
    - serial_clock_out ( PIN serial_clock_out ) ( _133_ X ) + USE CLOCK
      + ROUTED met2 ( 83030 44030 ) ( * 47260 )
      NEW met3 ( 83030 47260 ) ( 83260 * 0 )
      NEW met1 ( 82800 44030 ) ( 83030 * )
      NEW met1 ( 82800 44030 ) ( * 44370 )
      NEW met1 ( 45310 44030 ) ( * 44370 )
      NEW met1 ( 45310 44370 ) ( 82800 * )
      NEW met1 ( 83030 44030 ) M1M2_PR
      NEW met2 ( 83030 47260 ) M2M3_PR
      NEW li1 ( 45310 44030 ) L1M1_PR ;
    - serial_data_in ( PIN serial_data_in ) ( ANTENNA__118__D DIODE ) ( _118_ D ) + USE SIGNAL
      + ROUTED met2 ( 83950 45050 ) ( * 49300 )
      NEW met3 ( 83950 49300 ) ( 84180 * 0 )
      NEW met1 ( 82800 45050 ) ( 83950 * )
      NEW met1 ( 82800 45050 ) ( * 45390 )
      NEW met1 ( 30590 44030 ) ( * 44370 )
      NEW met1 ( 30590 44030 ) ( 44850 * )
      NEW met1 ( 44850 44030 ) ( * 45390 )
      NEW met1 ( 42550 45390 ) ( 82800 * )
      NEW met1 ( 83950 45050 ) M1M2_PR
      NEW met2 ( 83950 49300 ) M2M3_PR
      NEW li1 ( 42550 45390 ) L1M1_PR
      NEW li1 ( 30590 44370 ) L1M1_PR ;
    - serial_data_out ( PIN serial_data_out ) ( _131_ Q ) + USE SIGNAL
      + ROUTED met2 ( 83030 51340 ) ( * 52190 )
      NEW met3 ( 83030 51340 ) ( 83260 * 0 )
      NEW met1 ( 47150 52190 ) ( 83030 * )
      NEW met1 ( 83030 52190 ) M1M2_PR
      NEW met2 ( 83030 51340 ) M2M3_PR
      NEW li1 ( 47150 52190 ) L1M1_PR ;
    - serial_load ( PIN serial_load ) ( ANTENNA_clkbuf_0_serial_load_A DIODE ) ( clkbuf_0_serial_load A ) + USE CLOCK
      + ROUTED met2 ( 39790 37230 ) ( * 53380 )
      NEW met1 ( 39790 32130 ) ( 40710 * )
      NEW met2 ( 39790 32130 ) ( * 37230 )
      NEW met3 ( 39790 53380 ) ( 70380 * 0 )
      NEW li1 ( 39790 37230 ) L1M1_PR
      NEW met1 ( 39790 37230 ) M1M2_PR
      NEW met2 ( 39790 53380 ) M2M3_PR
      NEW li1 ( 40710 32130 ) L1M1_PR
      NEW met1 ( 39790 32130 ) M1M2_PR
      NEW met1 ( 39790 37230 ) RECT ( -355 -70 0 70 )  ;
    - serial_load_out ( PIN serial_load_out ) ( _134_ X ) + USE CLOCK
      + ROUTED met2 ( 83030 55250 ) ( * 55420 )
      NEW met3 ( 83030 55420 ) ( 83260 * 0 )
      NEW met1 ( 45310 54910 ) ( * 55250 )
      NEW met1 ( 45310 55250 ) ( 83030 * )
      NEW met1 ( 83030 55250 ) M1M2_PR
      NEW met2 ( 83030 55420 ) M2M3_PR
      NEW li1 ( 45310 54910 ) L1M1_PR ;
    - shift_register\[0\] ( hold6 A ) ( _118_ Q ) + USE SIGNAL
      + ROUTED met1 ( 23230 45730 ) ( 33810 * )
      NEW met2 ( 33810 45730 ) ( * 47430 )
      NEW li1 ( 23230 45730 ) L1M1_PR
      NEW met1 ( 33810 45730 ) M1M2_PR
      NEW li1 ( 33810 47430 ) L1M1_PR
      NEW met1 ( 33810 47430 ) M1M2_PR
      NEW met1 ( 33810 47430 ) RECT ( -355 -70 0 70 )  ;
    - shift_register\[10\] ( hold8 A ) ( _128_ Q ) + USE SIGNAL
      + ROUTED met2 ( 44390 20230 ) ( * 28730 )
      NEW met1 ( 39790 28730 ) ( 44390 * )
      NEW li1 ( 44390 20230 ) L1M1_PR
      NEW met1 ( 44390 20230 ) M1M2_PR
      NEW met1 ( 44390 28730 ) M1M2_PR
      NEW li1 ( 39790 28730 ) L1M1_PR
      NEW met1 ( 44390 20230 ) RECT ( -355 -70 0 70 )  ;
    - shift_register\[11\] ( hold13 A ) ( _129_ Q ) + USE SIGNAL
      + ROUTED met1 ( 38870 25670 ) ( 44390 * )
      NEW li1 ( 44390 25670 ) L1M1_PR
      NEW li1 ( 38870 25670 ) L1M1_PR ;
    - shift_register\[12\] ( hold1 A ) ( _131_ D ) ( _130_ Q ) + USE SIGNAL
      + ROUTED met2 ( 41170 45730 ) ( * 53550 )
      NEW met1 ( 39790 53550 ) ( 41170 * )
      NEW met1 ( 41170 42330 ) ( 43010 * )
      NEW met2 ( 41170 42330 ) ( * 45730 )
      NEW li1 ( 41170 45730 ) L1M1_PR
      NEW met1 ( 41170 45730 ) M1M2_PR
      NEW met1 ( 41170 53550 ) M1M2_PR
      NEW li1 ( 39790 53550 ) L1M1_PR
      NEW li1 ( 43010 42330 ) L1M1_PR
      NEW met1 ( 41170 42330 ) M1M2_PR
      NEW met1 ( 41170 45730 ) RECT ( -355 -70 0 70 )  ;
    - shift_register\[1\] ( hold5 A ) ( _119_ Q ) + USE SIGNAL
      + ROUTED met1 ( 16790 50490 ) ( 20930 * )
      NEW li1 ( 20930 50490 ) L1M1_PR
      NEW li1 ( 16790 50490 ) L1M1_PR ;
    - shift_register\[2\] ( hold3 A ) ( _120_ Q ) + USE SIGNAL
      + ROUTED met1 ( 7590 47430 ) ( 8050 * )
      NEW met2 ( 8050 47430 ) ( * 52870 )
      NEW met1 ( 8050 52870 ) ( 10350 * )
      NEW li1 ( 7590 47430 ) L1M1_PR
      NEW met1 ( 8050 47430 ) M1M2_PR
      NEW met1 ( 8050 52870 ) M1M2_PR
      NEW li1 ( 10350 52870 ) L1M1_PR ;
    - shift_register\[3\] ( hold4 A ) ( _121_ Q ) + USE SIGNAL
      + ROUTED met1 ( 16330 41990 ) ( 20010 * )
      NEW li1 ( 20010 41990 ) L1M1_PR
      NEW li1 ( 16330 41990 ) L1M1_PR ;
    - shift_register\[4\] ( hold9 A ) ( _122_ Q ) + USE SIGNAL
      + ROUTED met1 ( 16330 34170 ) ( 20930 * )
      NEW li1 ( 20930 34170 ) L1M1_PR
      NEW li1 ( 16330 34170 ) L1M1_PR ;
    - shift_register\[5\] ( hold12 A ) ( _123_ Q ) + USE SIGNAL
      + ROUTED met1 ( 17250 14790 ) ( 18170 * )
      NEW met2 ( 17250 14790 ) ( * 27710 )
      NEW met1 ( 16790 27710 ) ( 17250 * )
      NEW li1 ( 18170 14790 ) L1M1_PR
      NEW met1 ( 17250 14790 ) M1M2_PR
      NEW met1 ( 17250 27710 ) M1M2_PR
      NEW li1 ( 16790 27710 ) L1M1_PR ;
    - shift_register\[6\] ( hold10 A ) ( _124_ Q ) + USE SIGNAL
      + ROUTED met1 ( 25530 22270 ) ( 25990 * )
      NEW met2 ( 25990 22270 ) ( * 25670 )
      NEW met1 ( 25990 25670 ) ( 29210 * )
      NEW li1 ( 25530 22270 ) L1M1_PR
      NEW met1 ( 25990 22270 ) M1M2_PR
      NEW met1 ( 25990 25670 ) M1M2_PR
      NEW li1 ( 29210 25670 ) L1M1_PR ;
    - shift_register\[7\] ( hold11 A ) ( _125_ Q ) + USE SIGNAL
      + ROUTED met1 ( 31510 23290 ) ( * 23630 )
      NEW met1 ( 25530 23630 ) ( 31510 * )
      NEW met2 ( 25530 23630 ) ( * 24990 )
      NEW li1 ( 31510 23290 ) L1M1_PR
      NEW met1 ( 25530 23630 ) M1M2_PR
      NEW li1 ( 25530 24990 ) L1M1_PR
      NEW met1 ( 25530 24990 ) M1M2_PR
      NEW met1 ( 25530 24990 ) RECT ( -355 -70 0 70 )  ;
    - shift_register\[8\] ( hold7 A ) ( _126_ Q ) + USE SIGNAL
      + ROUTED met2 ( 29670 29410 ) ( * 31110 )
      NEW li1 ( 29670 29410 ) L1M1_PR
      NEW met1 ( 29670 29410 ) M1M2_PR
      NEW li1 ( 29670 31110 ) L1M1_PR
      NEW met1 ( 29670 31110 ) M1M2_PR
      NEW met1 ( 29670 29410 ) RECT ( -355 -70 0 70 ) 
      NEW met1 ( 29670 31110 ) RECT ( -355 -70 0 70 )  ;
    - shift_register\[9\] ( hold2 A ) ( _127_ Q ) + USE SIGNAL
      + ROUTED met1 ( 39790 31110 ) ( 40250 * )
      NEW met2 ( 40250 31110 ) ( * 33490 )
      NEW met1 ( 40250 33490 ) ( 41170 * )
      NEW met1 ( 41170 33490 ) ( * 33830 )
      NEW met1 ( 41170 33830 ) ( 43010 * )
      NEW met2 ( 43010 33830 ) ( * 36550 )
      NEW li1 ( 39790 31110 ) L1M1_PR
      NEW met1 ( 40250 31110 ) M1M2_PR
      NEW met1 ( 40250 33490 ) M1M2_PR
      NEW met1 ( 43010 33830 ) M1M2_PR
      NEW li1 ( 43010 36550 ) L1M1_PR
      NEW met1 ( 43010 36550 ) M1M2_PR
      NEW met1 ( 43010 36550 ) RECT ( -355 -70 0 70 )  ;
    - user_gpio_in ( PIN user_gpio_in ) ( gpio_in_buf Z ) + USE SIGNAL
      + ROUTED met2 ( 83490 28050 ) ( * 34500 )
      NEW met2 ( 83490 34500 ) ( 84410 * )
      NEW met2 ( 84410 34500 ) ( * 57460 )
      NEW met3 ( 84180 57460 0 ) ( 84410 * )
      NEW met2 ( 69230 19890 ) ( * 28050 )
      NEW met1 ( 69230 28050 ) ( 83490 * )
      NEW met1 ( 40250 19890 ) ( 69230 * )
      NEW met1 ( 83490 28050 ) M1M2_PR
      NEW met2 ( 84410 57460 ) M2M3_PR
      NEW met1 ( 69230 28050 ) M1M2_PR
      NEW met1 ( 69230 19890 ) M1M2_PR
      NEW li1 ( 40250 19890 ) L1M1_PR ;
    - user_gpio_oeb ( PIN user_gpio_oeb ) ( ANTENNA__062__B DIODE ) ( _062_ B ) + USE SIGNAL
      + ROUTED met2 ( 47610 45730 ) ( * 59500 )
      NEW met1 ( 45310 39950 ) ( 47610 * )
      NEW met2 ( 47610 39950 ) ( * 45730 )
      NEW met3 ( 47610 59500 ) ( 70380 * 0 )
      NEW li1 ( 47610 45730 ) L1M1_PR
      NEW met1 ( 47610 45730 ) M1M2_PR
      NEW met2 ( 47610 59500 ) M2M3_PR
      NEW li1 ( 45310 39950 ) L1M1_PR
      NEW met1 ( 47610 39950 ) M1M2_PR
      NEW met1 ( 47610 45730 ) RECT ( -355 -70 0 70 )  ;
    - user_gpio_out ( PIN user_gpio_out ) ( ANTENNA__066__A0 DIODE ) ( _066_ A0 ) + USE SIGNAL
      + ROUTED met1 ( 45770 33490 ) ( 46230 * )
      NEW met2 ( 46230 33490 ) ( * 61540 )
      NEW met1 ( 47610 20570 ) ( 48070 * )
      NEW met2 ( 48070 20570 ) ( * 33490 )
      NEW met1 ( 46230 33490 ) ( 48070 * )
      NEW met3 ( 46230 61540 ) ( 70380 * 0 )
      NEW li1 ( 45770 33490 ) L1M1_PR
      NEW met1 ( 46230 33490 ) M1M2_PR
      NEW met2 ( 46230 61540 ) M2M3_PR
      NEW li1 ( 47610 20570 ) L1M1_PR
      NEW met1 ( 48070 20570 ) M1M2_PR
      NEW met1 ( 48070 33490 ) M1M2_PR ;
    - zero ( PIN zero ) ( const_source LO ) + USE SIGNAL
      + ROUTED met2 ( 44850 2380 ) ( * 8670 )
      NEW met3 ( 44850 2380 ) ( 70380 * 0 )
      NEW li1 ( 44850 8670 ) L1M1_PR
      NEW met1 ( 44850 8670 ) M1M2_PR
      NEW met2 ( 44850 2380 ) M2M3_PR
      NEW met1 ( 44850 8670 ) RECT ( -355 -70 0 70 )  ;
END NETS
END DESIGN
