Summary of Key Periphery Rules
==============================

.. csv-table:: Table F3a: Front end layers (Low Voltage Devices)
   :file: summary/table-f3a-font-end-low-voltage.csv
   :header-rows: 1
   :stub-columns: 1

.. csv-table:: Table F3b: Front end layers (High Voltage Devices)
   :file: summary/table-f3b-font-end-high-voltage.csv
   :header-rows: 1
   :stub-columns: 1

Manual merge means that features below min. space should be manually merged by drawing.

.. csv-table:: Table F3c: Back end layers for S8D* flow
   :file: summary/table-f3c-back-end-high-S8Dx.csv
   :header-rows: 1
   :stub-columns: 1

.. csv-table:: Table F3d: Back end layers for S8T* flow
   :file: summary/table-f3d-back-end-high-S8Tx.csv
   :header-rows: 1
   :stub-columns: 1

.. csv-table:: Table F4: Connectivity of Drawn and Mask Layers [#f1]_
   :file: summary/table-f4-connectivity-of-drawn-and-mask.csv
   :header-rows: 1
   :stub-columns: 1

.. include:: summary/table-f4-key.rst

.. csv-table:: Table F5: Device Connectivity Table
   :file: summary/table-f5-device-connectivity.csv
   :header-rows: 1
   :stub-columns: 1
