(module Cherry_MX_Matias (layer F.Cu) (tedit 5A2BA8FB)
  (tags switch)
  (fp_text reference REF** (at 3.2 -0.05 90) (layer B.SilkS)
    (effects (font (thickness 0.3048)) (justify mirror))
  )
  (fp_text value SW_MX (at 0 3.45) (layer B.Fab) hide
    (effects (font (thickness 0.3048)) (justify mirror))
  )
  (fp_line (start 7 7) (end -7 7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 -7) (layer B.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 -7) (end 7 -7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 -7) (end 7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 7) (end -7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 -7) (layer F.SilkS) (width 0.15))
  (pad "" np_thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -2.5 -3.683) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.5 -4) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (model cherry_mx1.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
