(module TC2030-NL_SMALL (layer F.Cu) (tedit 4FBCCECC)
  (descr "Tag-Connect TC2030-NL footprint by carloscuev@gmail.com")
  (tags "Tag-Connect TC2030-NL")
  (clearance 0.127)
  (attr virtual)
  (fp_text reference TC2030-NL (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_text value VAL (at 0 2.667) (layer F.SilkS) hide
    (effects (font (size 0.75692 0.75692) (thickness 0.127)))
  )
  (fp_line (start 2.6035 1.905) (end -2.0828 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.6035 -1.905) (end -2.0828 -1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.2639 0.7239) (end -2.0828 1.905) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.2639 -0.7239) (end -2.0828 -1.905) (layer F.SilkS) (width 0.127))
  (fp_arc (start -2.54 0) (end -3.2639 0.7239) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.556 -0.9525) (end 3.556 0.9525) (layer F.SilkS) (width 0.127))
  (fp_arc (start 2.6035 0.9525) (end 3.556 0.9525) (angle 90) (layer F.SilkS) (width 0.127))
  (fp_arc (start 2.6035 -0.9525) (end 2.6035 -1.905) (angle 90) (layer F.SilkS) (width 0.127))
  (pad 1 connect circle (at -1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 2 connect circle (at -1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 3 connect circle (at 0 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 4 connect circle (at 0 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 5 connect circle (at 1.27 0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad 6 connect circle (at 1.27 -0.635) (size 0.78486 0.78486) (layers F.Cu F.Mask))
  (pad "" np_thru_hole circle (at -2.54 0) (size 0.98806 0.98806) (drill 0.98806) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 2.54 -1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 2.54 1.016) (size 0.98552 0.98552) (drill 0.98552) (layers *.Cu *.Mask F.SilkS))
)
