EESchema-DOCLIB  Version 2.0
#
$CMP MCP1700
D 250mA Low Quiscent Current LDO, 3.0V output, SOT-23
K regulator linear ldo
F http://ww1.microchip.com/downloads/en/DeviceDoc/20001826C.pdf
$ENDCMP
#
$CMP MIC5216-3.3BM5
D 300mA low dropout linear regulator, shutdown pin, 1.5V fixed positive output, SOT-23-5 package
K linear regulator ldo fixed positive
F http://www.diodes.com/_files/datasheets/AP131.pdf
$ENDCMP
#
$CMP MIC5219-3.3
D 500mA LDO fixed output voltage 3.3V ultra-low-noise, SOT-23-5
K linear low dropout Regulator fixed ultra-low-noise
F http://ww1.microchip.com/downloads/en/DeviceDoc/mic5216.pdf
$ENDCMP
#
$CMP MIC550X
D Single 300mA LDO
K voltage regulator, LDO
F http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf
$ENDCMP
#
$CMP TPS6102x
D Synchronous Boost Converter
K TPS61020, TPS61024, TPS61025, TPS61026, TPS61027, TPS61028, TPS61029
$ENDCMP
#
$CMP TPS6107x
K TPS61070, TPS61071, TPS61072, TPS61073
$ENDCMP
#
#End Doc Library
