(module MX_Matias_KailhLP_NoSilk (layer F.Cu) (tedit 5AA342CB)
  (tags switch)
  (fp_text reference REF** (at 3.2 0 90) (layer Cmts.User)
    (effects (font (thickness 0.3048)))
  )
  (fp_text value key_switch (at 0.01 2.76) (layer F.SilkS) hide
    (effects (font (thickness 0.15)))
  )
  (fp_line (start -7 -7) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask)
    (zone_connect 0))
  (pad "" np_thru_hole circle (at -5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
    (zone_connect 0))
  (pad 1 thru_hole circle (at -2.5 -3.683) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 thru_hole oval (at -3.81 -2.54 311) (size 2.5 4.1) (drill 1.5 (offset 0 -0.8)) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask)
    (zone_connect 0))
  (pad "" np_thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
    (zone_connect 0))
  (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 2 thru_hole oval (at 2.5 -4 358) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 smd oval (at -3.18 -3.09 311) (size 2.5 4.1) (layers F.Cu F.Mask))
  (pad 1 smd oval (at -3.18 -3.09 311) (size 2.5 4.1) (layers B.Cu F.Mask))
  (pad 2 smd oval (at 2.52 -4.54 358) (size 2.5 3.6) (layers B.Cu F.Mask))
  (pad 2 smd oval (at 2.52 -4.54 358) (size 2.5 3.6) (layers F.Cu F.Mask))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask)
    (zone_connect 0))
  (pad 1 thru_hole circle (at 0 -5.9 311) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 thru_hole circle (at -5 -3.8 311) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
    (zone_connect 2))
  (model ../../../../code/keyboard_pcb/kicad_common/packages3d/switch_mx.packages3d/cherry_mx_blue_pcb.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
