diff --exclude=.svn -uNr crlcore/etc.soc/CMakeLists.txt crlcore/etc/CMakeLists.txt
--- crlcore/etc.soc/CMakeLists.txt	2010-05-27 13:37:15.000000000 +0200
+++ crlcore/etc/CMakeLists.txt	2010-05-27 13:37:57.000000000 +0200
@@ -1,7 +1,4 @@
  install ( FILES   environment.alliance.xml     DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
  install ( FILES   technology.symbolic.xml      DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
- install ( FILES   technology.cmos130.s2r.xml   DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
- install ( FILES   technology.cmos65.s2r.xml    DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
- install ( FILES   technology.freePDK45.s2r.xml DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
  install ( FILES   technology.fake.s2r.xml      DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
  install ( FILES   display.xml                  DESTINATION ${SYS_CONF_DIR}/coriolis2 ) 
diff --exclude=.svn -uNr crlcore/etc.soc/environment.alliance.xml crlcore/etc/environment.alliance.xml
--- crlcore/etc.soc/environment.alliance.xml	2010-05-22 11:00:46.000000000 +0200
+++ crlcore/etc/environment.alliance.xml	2010-05-27 13:38:57.000000000 +0200
@@ -1,18 +1,18 @@
 <?xml version="1.0"?>
 <environment>
-  <variable name="CELL_TOP" value="/opt/alliance-5.0"/>
+  <variable name="CELL_TOP" value="/usr/share/alliance"/>
   <technologies>
     <hurricane>
-      <config>${CORIOLIS_TOP}/etc/coriolis2/technology.symbolic.xml</config>
+      <config>/etc/coriolis2/technology.symbolic.xml</config>
     </hurricane>
     <real>
-      <config>${CORIOLIS_TOP}/etc/coriolis2/technology.cmos130.s2r.xml</config>
+      <config>/etc/coriolis2/technology.fake.s2r.xml</config>
     </real>
     <lef>
-      <config>${CORIOLIS_TOP}/etc/coriolis2/cmos.lef</config>
+      <config>/etc/coriolis2/cmos.lef</config>
     </lef>
     <display>
-      <config>${CORIOLIS_TOP}/etc/coriolis2/display.xml</config>
+      <config>/etc/coriolis2/display.xml</config>
     </display>
   </technologies>
   <libraries>
diff --exclude=.svn -uNr crlcore/etc.soc/technology.cmos130.s2r.xml crlcore/etc/technology.cmos130.s2r.xml
--- crlcore/etc.soc/technology.cmos130.s2r.xml	2010-05-27 13:35:07.000000000 +0200
+++ crlcore/etc/technology.cmos130.s2r.xml	1970-01-01 01:00:00.000000000 +0100
@@ -1,29 +0,0 @@
-<?xml version="1.0"?>
-<technology>
-  <real>
-    <name>hcmos9</name>
-    <grid value="0.005" unit="micron"/>
-    <gridsperlambda value="24"/>
-    <layers>
-      <!-- Non routing layers -->
-      <processlayer symbolic="nWell"    real="NWELL"    gdsII="3" />
-      <processlayer symbolic="nImplant" real="NPLUS"    gdsII="26"/>
-      <processlayer symbolic="pImplant" real="PPLUS"    gdsII="25"/>
-      <processlayer symbolic="active"   real="ACTIVE"   gdsII="6" />
-      <processlayer symbolic="poly"     real="POLY"     gdsII="17"/>
-      <!-- Routing layers -->
-      <processlayer symbolic="cut0"     real="CONTACT"  gdsII="30"/>
-      <processlayer symbolic="metal1"   real="METAL1"   gdsII="31"/>
-      <processlayer symbolic="cut1"     real="VIA1"     gdsII="51"/>
-      <processlayer symbolic="metal2"   real="METAL2"   gdsII="32"/>
-      <processlayer symbolic="cut2"     real="VIA2"     gdsII="52"/>
-      <processlayer symbolic="metal3"   real="METAL3"   gdsII="33"/>
-      <processlayer symbolic="cut3"     real="VIA3"     gdsII="53"/>
-      <processlayer symbolic="metal4"   real="METAL4"   gdsII="34"/>
-      <processlayer symbolic="cut4"     real="VIA4"     gdsII="54"/>
-      <processlayer symbolic="metal5"   real="METAL5"   gdsII="35"/>
-      <processlayer symbolic="cut5"     real="VIA5"     gdsII="55"/>
-      <processlayer symbolic="metal6"   real="METAL6"   gdsII="36"/>
-    </layers>
-  </real>
-</technology>
diff --exclude=.svn -uNr crlcore/etc.soc/technology.cmos65.s2r.xml crlcore/etc/technology.cmos65.s2r.xml
--- crlcore/etc.soc/technology.cmos65.s2r.xml	2010-05-27 13:35:07.000000000 +0200
+++ crlcore/etc/technology.cmos65.s2r.xml	1970-01-01 01:00:00.000000000 +0100
@@ -1,29 +0,0 @@
-<?xml version="1.0"?>
-<technology>
-  <real>
-    <name>cmos065</name>
-    <grid value="0.005" unit="micron"/>
-    <gridsperlambda value="24"/>
-    <layers>
-      <!-- Non routing layers -->
-      <processlayer symbolic="nWell"    real="NW"    gdsII="3" />
-      <processlayer symbolic="nImplant" real="NP"    gdsII="26"/>
-      <processlayer symbolic="pImplant" real="PP"    gdsII="25"/>
-      <processlayer symbolic="active"   real="OD"    gdsII="6" />
-      <processlayer symbolic="poly"     real="PO"    gdsII="17"/>
-      <!-- Routing layers -->
-      <processlayer symbolic="cut0"     real="CO"    gdsII="30"/>
-      <processlayer symbolic="metal1"   real="M1"    gdsII="31"/>
-      <processlayer symbolic="cut1"     real="VIA1X" gdsII="51"/>
-      <processlayer symbolic="metal2"   real="M2X"   gdsII="32"/>
-      <processlayer symbolic="cut2"     real="VIA2X" gdsII="52"/>
-      <processlayer symbolic="metal3"   real="M3X"   gdsII="33"/>
-      <processlayer symbolic="cut3"     real="VIA3X" gdsII="53"/>
-      <processlayer symbolic="metal4"   real="M4X"   gdsII="34"/>
-      <processlayer symbolic="cut4"     real="VIA4X" gdsII="54"/>
-      <processlayer symbolic="metal5"   real="M5X"   gdsII="35"/>
-      <processlayer symbolic="cut5"     real="VIA5X" gdsII="55"/>
-      <processlayer symbolic="metal6"   real="M6X"   gdsII="36"/>
-    </layers>
-  </real>
-</technology>
diff --exclude=.svn -uNr crlcore/etc.soc/technology.freePDK45.s2r.xml crlcore/etc/technology.freePDK45.s2r.xml
--- crlcore/etc.soc/technology.freePDK45.s2r.xml	2010-04-23 15:26:06.000000000 +0200
+++ crlcore/etc/technology.freePDK45.s2r.xml	1970-01-01 01:00:00.000000000 +0100
@@ -1,29 +0,0 @@
-<?xml version="1.0"?>
-<technology>
-  <real>
-    <name>freePDK45</name>
-    <grid value="0.0025" unit="micron"/>
-    <gridsperlambda value="24"/>
-    <layers>
-      <!-- Non routing layers -->
-      <processlayer symbolic="nWell"    real="NW"    gdsII="3" />
-      <processlayer symbolic="nImplant" real="NP"    gdsII="26"/>
-      <processlayer symbolic="pImplant" real="PP"    gdsII="25"/>
-      <processlayer symbolic="active"   real="OD"    gdsII="6" />
-      <processlayer symbolic="poly"     real="PO"    gdsII="17"/>
-      <!-- Routing layers -->
-      <processlayer symbolic="cut0"     real="CO"    gdsII="30"/>
-      <processlayer symbolic="metal1"   real="M1"    gdsII="31"/>
-      <processlayer symbolic="cut1"     real="VIA1X" gdsII="51"/>
-      <processlayer symbolic="metal2"   real="M2X"   gdsII="32"/>
-      <processlayer symbolic="cut2"     real="VIA2X" gdsII="52"/>
-      <processlayer symbolic="metal3"   real="M3X"   gdsII="33"/>
-      <processlayer symbolic="cut3"     real="VIA3X" gdsII="53"/>
-      <processlayer symbolic="metal4"   real="M4X"   gdsII="34"/>
-      <processlayer symbolic="cut4"     real="VIA4X" gdsII="54"/>
-      <processlayer symbolic="metal5"   real="M5X"   gdsII="35"/>
-      <processlayer symbolic="cut5"     real="VIA5X" gdsII="55"/>
-      <processlayer symbolic="metal6"   real="M6X"   gdsII="36"/>
-    </layers>
-  </real>
-</technology>
--- unicorn/src/CgtMain.cpp.soc	2010-05-27 18:22:37.000000000 +0200
+++ unicorn/src/CgtMain.cpp	2010-05-27 18:23:02.000000000 +0200
@@ -83,7 +83,7 @@
     float         edgeCapacity;
     float         expandStep;
     unsigned long eventsLimit;
-    unsigned int  traceLevel;
+  //unsigned int  traceLevel;
     bool          verbose1;
     bool          verbose2;
     bool          info;
@@ -99,9 +99,9 @@
     poptions::options_description options ("Command line arguments & options");
     options.add_options()
       ( "help,h"           , "Print this help." )
-      ( "trace-level,l"    , poptions::value<unsigned int>(&traceLevel)->default_value(1000)
-                           , "Set the level of trace, trace messages with a level superior to "
-                             "<arg> will be printed on <stderr>." )
+      // ( "trace-level,l"    , poptions::value<unsigned int>(&traceLevel)->default_value(1000)
+      //                      , "Set the level of trace, trace messages with a level superior to "
+      //                        "<arg> will be printed on <stderr>." )
       ( "verbose,v"        , poptions::bool_switch(&verbose1)->default_value(false)
                            , "First level of verbosity.")
       ( "very-verbose,V"   , poptions::bool_switch(&verbose2)->default_value(false)
@@ -152,7 +152,7 @@
     if ( info     ) mstream::enable ( mstream::Info ); 
     if ( logMode  ) tty::disable ();
 
-    ltracelevel ( traceLevel );
+  //ltracelevel ( traceLevel );
 
     dbo_ptr<DataBase>          db ( DataBase::create() );
     dbo_ptr<AllianceFramework> af ( AllianceFramework::create() );
