ENTITY tie_x0 IS
PORT (
  vdd	 : in  BIT;
  vss	 : in  BIT
);
END tie_x0;

ARCHITECTURE behaviour_data_flow OF tie_x0 IS

BEGIN
  ASSERT (vdd and not (vss))
  REPORT "power supply is missing on tie_x0"
  SEVERITY WARNING;
END;
